{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["Instructions","RailroadCostProgram","DetailedParameters","BatchCostProgram","BatchOutput","URCSInputs","RailroadUnitCostXML","Railroads","STCCs","ECodeTable"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":596,"comments":5,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":15,"n_cols":2,"rows_kept":15,"cut":false,"hidden":false,"merged":[[3,0,3,1]]}
["Surface Transportation Board - Railroad Cost Program - Instructions"]
[null,"Version 2017.1"]
["Overview"]
["This is a Microsoft Excel version of the Surface Transportation Board's URCS Phase III Railroad Cost Program.  This replaces the Visual Basic version of the program that needed to be installed on a user's computer.\n\nThis Excel version of the program can be run one of two ways.  First, the RailroadCostProgram worksheet of the workbook can be used to calculate the variable cost of a shipment by directly inputting the URCS input parameters.  Second, the BatchCostProgram worksheet of the workbook can be used to calculate the variable costs of series of shipments by running a macro.  The BatchCostProgram is designed to support evidence filed before the STB."]
[]
["Worksheet Name","Description"]
["RailroadCostProgram","This worksheet is used to input the mandatory parameters used by the URCS Phase III program, which are highlighted in yellow.  A description of each field pops up when each field is selected.  Some fields have drop-down lists that the user can select from.  The variable costs of the shipment are automatically calculated.\n\nThis worksheet can be used to calculate the variable cost of a single segment by only entering values in the \"ORR\" column.  If only costing one segment, enter the distance traveled by any other railroads in the TRR Distance field so that Loss & Damage can be allocated appropriately.\n\nFor multi-carrier shipments, the originating railroad should go in the \"ORR\" column, the terminating railroad should to in the \"TRR\" column, and any intermediate railroads should go in the \"JRR\" columns (i.e., junction railroads).\n\nThis worksheet can be printed out as the URCS Standard Output Report."]
["Detailed Parameters","This worksheet can be used to override certain values in the RailroadCostProgram worksheet.  The user should input any override values into the cells highlighted in yellow.  The detailed parameters allow for \"What If\" scenarios to be evaluated."]
["BatchCostProgram","This worksheet is used to define the inputs needed for calculating the costs of many segments at one time.  The user should input values into the columns highlighted in yellow (columns A-N).  To cost the records, press the \"Run Batch Program\" button.  The results are stored in the BatchOutput worksheet.\n\nSince the BatchCostProgram is designed to support evidence filed before the STB, only a limited number of detailed parameter options are available.  Those are the circuity and the TOFC Plan.\n\nAny records whose inputs were invalid will have #N/A in one or more of columns P through AC.  Use the AutoFilter feature to find those records."]
["BatchOutput","This worksheet contains the results of running the BatchCostProgram.  Any records that were unable to be costed will have #N/A in column PN, which is the total variable cost (L700).  Use the AutoFilter feature to find those records."]
["URCSInputs","This worksheet contains various URCS input values.  It acts as a reference for various codes expected by the Phase III program."]
["RailroadUnitCostXML","This worksheet contains the unit costs for various years that were previously stored in the Railroad Unit Cost files, which were in an XML format."]
["Railroads","This worksheet contains the various URCS Class I railroad codes.  It also contains a list of all railroads listed in previous waybill samples and the regions to which they are assigned."]
["STCCs","This worksheet contains the translation of 5-digit STCC codes into their URCS commodity group."]
["ECodeTable","This worksheet contains the translations of the URCS Phase II reference ID (e.g., E1L101C1=Gross Ton Mile (GTM) OPR Expense)."]

{"sheet":"RailroadCostProgram","index":1,"n_rows":504,"n_cols":11,"rows_kept":504,"cut":false,"hidden":false,"merged":[]}
["Surface Transportation Board - Railroad Cost Program",null,null,2021,"Unit Cost Year"]
[]
[{"$f":"\"Using \"&TEXT(CostYear,\"0000\")&\" Unit Costs\"","v":"Using 2021 Unit Costs"},null,null,1,2,3,4,5,{"$f":"Version","v":"Version 2017.1"}]
["LINE","DESCRIPTION","SOURCE","ORR","JRR1","JRR2","JRR3","TRR","Total","Information"]
["RR","Railroad","[User]","WEST"]
["DIS","Distance","[User]",1000,null,null,null,null,{"$f":"SUM($D6:$H6)","v":1000}]
["SG","Segment Type","[User]","OT",{"$f":"IF(ISBLANK(RR),\"\",\"RD\")","v":""},{"$f":"IF(ISBLANK(RR),\"\",\"RD\")","v":""},{"$f":"IF(ISBLANK(RR),\"\",\"RD\")","v":""}]
["FC","Freight Car Type","[User]","Covered Hopper Cars",null,null,null,null,null,"Car Type Index=",{"$f":"VLOOKUP($D$8,URCSInputs!$L$3:$M$19,2,FALSE)","v":6}]
["NC",{"$f":"IF(SZ<>\"Intermodal\",\"Number of Cars\",\"Number of TCUs\")","v":"Number of Cars"},"[User]",1]
["OWN","Car Ownership","[User]","Railroad"]
["WT",{"$f":"IF(SZ<>\"Intermodal\",\"Weight per Car (tons)\",\"Weight per TCU (tons)\")","v":"Weight per Car (tons)"},"[User]",80]
["COM","Commodity","[User]","0113 Grains",null,null,null,null,null,"Commodity Index=",{"$f":"VLOOKUP(COM,URCSInputs!$Q$3:$R$84,2,FALSE)","v":2}]
["SZ","Shipment Size","[User]","Single"]
["REV","Revenue","[User]"]
[null,null,{"$f":"IF(AND($D$7=\"OT\",$H$6>0),\"CAUTION:  The ORR Segment Type should not be 'OT' if a TRR Distance is specified.\",IF(AND(OR($D$7=\"OD\",$D$7=\"RD\",$D$7=\"RT\",$D$7=\"IR\"),$H$6=0),\"CAUTION:  The Loss & Damage expense will not be allocated properly unless the distance traveled by all other railroads is specified as the TRR distance.\",IF(AND(FC=\"Flat Cars TOFC/COFC\",SZ<>\"Intermodal\"),\"CAUTION:  TOFC Flatcars usually move in Intermodal service.\",IF(AND(SZ=\"Intermodal\",NOT(OR(FC=\"Flat Cars TOFC/COFC\",FC=\"Flat Cars-General Service\",FC=\"Flat Cars-Other\"))),\"CAUTION:  Intermodal usually moves in TOFC Flatcars, General Service Flatcars, or Other Flatcars.\",\"\"))))","v":""}]
[null,null,"VARIABLE COST SUMMARY",null,null,null,null,{"$f":"IF(REV=0,\"\",\"RVC RATIO:\")","v":""},{"$f":"IF(REV=0,\"\",REV/$I$21)","v":""}]
[null,null,"Category",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[null,null,"Variable Costs",{"$f":"IF(ISBLANK(RR),\"\",SUM(D$370:D$464))","v":2128.6531378838113},{"$f":"IF(ISBLANK(RR),\"\",SUM(E$370:E$464))","v":""},{"$f":"IF(ISBLANK(RR),\"\",SUM(F$370:F$464))","v":""},{"$f":"IF(ISBLANK(RR),\"\",SUM(G$370:G$464))","v":""},{"$f":"IF(ISBLANK(RR),\"\",SUM(H$370:H$464))","v":""},{"$f":"SUM(D18:H18)","v":2128.6531378838113}]
[null,null,"Loss & Damage",{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":1.3588848083408001},{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":""},{"$f":"SUM(D19:H19)","v":1.3588848083408001}]
[null,null,"Ex Parte Adjustment (i.e., Make Whole)",{"$f":"IF(ISBLANK(RR),\"\",Line587)","v":462.87460510785456},{"$f":"IF(ISBLANK(RR),\"\",Line587)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line587)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line587)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line587)","v":""},{"$f":"SUM(D20:H20)","v":462.87460510785456}]
[null,null,"Total Variable Costs",{"$f":"IF(ISBLANK(RR),\"\",SUM(D$18:D$20))","v":2592.8866278000069},"","","","",{"$f":"SUM(D21:H21)","v":2592.8866278000069}]
[]
["HDR","Train Mileage","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[101,"Short line miles","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,DIS))","v":1000},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,DIS))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,DIS))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,DIS))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,DIS))","v":""},{"$f":"SUM(D24:H24)","v":1000}]
[102,"Circuity factor",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C\"&IF(INDEX(SG,1)=\"OT\",\"5\",\"6\")","v":"E2L106C5"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_Circuity,D$3)),INDEX(User_Circuity,D$3),AdjustL102*VLOOKUP(RR&\"-\"&$C25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_Circuity,E$3)),INDEX(User_Circuity,E$3),AdjustL102*VLOOKUP(RR&\"-\"&$C25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_Circuity,F$3)),INDEX(User_Circuity,F$3),AdjustL102*VLOOKUP(RR&\"-\"&$C25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_Circuity,G$3)),INDEX(User_Circuity,G$3),AdjustL102*VLOOKUP(RR&\"-\"&$C25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_Circuity,H$3)),INDEX(User_Circuity,H$3),AdjustL102*VLOOKUP(RR&\"-\"&$C25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C25&\"=\"&VLOOKUP($C25,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C5=Local circuity, HOPPER - COVERED"}]
[103,"Actual miles including circuity","L101*L102",{"$f":"IF(ISBLANK(RR),\"\",Line101*Line102)","v":1000},{"$f":"IF(ISBLANK(RR),\"\",Line101*Line102)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line101*Line102)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line101*Line102)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line101*Line102)","v":""},{"$f":"SUM(D26:H26)","v":1000}]
[104,"Actual unit train miles including circuity","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,Line101*Line102))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,Line101*Line102))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,Line101*Line102))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,Line101*Line102))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,Line101*Line102))","v":""},{"$f":"SUM(D27:H27)","v":0}]
[105,"E/L ratio, this car",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C\"&IF(OWN=\"Railroad\",\"2\",\"3\")","v":"E2L106C2"},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_ELRatio,D$3)),INDEX(User_ELRatio,D$3),AdjustL105*VLOOKUP(RR&\"-\"&$C28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":1.9769228108307599},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_ELRatio,E$3)),INDEX(User_ELRatio,E$3),AdjustL105*VLOOKUP(RR&\"-\"&$C28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_ELRatio,F$3)),INDEX(User_ELRatio,F$3),AdjustL105*VLOOKUP(RR&\"-\"&$C28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_ELRatio,G$3)),INDEX(User_ELRatio,G$3),AdjustL105*VLOOKUP(RR&\"-\"&$C28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_ELRatio,H$3)),INDEX(User_ELRatio,H$3),AdjustL105*VLOOKUP(RR&\"-\"&$C28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C28&\"=\"&VLOOKUP($C28,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C2=E/L Ratio, Railroad-Owned, HOPPER - COVERED"}]
[106,"Estimated way train miles including circuity",{"$f":"\"(E2L201C1/E2L118C4)*(\"&$C$25&\"/E2L118C7)*L250\"","v":"(E2L201C1/E2L118C4)*(E2L106C5/E2L118C7)*L250"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,D$480))","v":15.902153970978807},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,E$480))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,F$480))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,G$480))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,H$480))","v":""},null,"See Special Calculations area below, after L703"]
[107,"Estimated through train miles including circuity","L103-L106",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line103-Line106))","v":984.09784602902118},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line103-Line106))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line103-Line106))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line103-Line106))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line103-Line106))","v":""}]
[108,"Total unit train miles including empty return","L104*L105",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,Line104*Line105))","v":0},{"$f":"IF(ISBLANK(E$5),\"\",IF(SZ<>\"Unit\",0,E27*E28))","v":""},{"$f":"IF(ISBLANK(F$5),\"\",IF(SZ<>\"Unit\",0,F27*F28))","v":""},{"$f":"IF(ISBLANK(G$5),\"\",IF(SZ<>\"Unit\",0,G27*G28))","v":""},{"$f":"IF(ISBLANK(H$5),\"\",IF(SZ<>\"Unit\",0,H27*H28))","v":""},{"$f":"SUM(D31:H31)","v":0}]
[109,"Total way train miles including empty return","L105*L106",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line106))","v":31.437330926570954},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line106))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line106))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line106))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line106))","v":""},{"$f":"SUM(D32:H32)","v":31.437330926570954}]
[110,"Total through train miles including empty return","L105*L107",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line107))","v":1945.4854799041889},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line107))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line107))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line107))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,Line105*Line107))","v":""},{"$f":"SUM(D33:H33)","v":1945.4854799041889}]
[111,"Total train miles including empty return","L103*L105",{"$f":"IF(ISBLANK(RR),\"\",Line103*Line105)","v":1976.92281083076},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line105)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line105)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line105)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line105)","v":""},{"$f":"SUM(D34:H34)","v":1976.92281083076}]
["HDR","Car Mile Costs (Other than Clerical)","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[201,"Number of freight cars","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",NC,0))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",NC,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",NC,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",NC,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",NC,0))","v":""}]
[202,"TCUs per flat car","E2L202C1",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,1,IF(ISNUMBER(User_TCUsPerFlatcar),User_TCUsPerFlatcar,TCUsPerFlatcarDefault))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,1,IF(ISNUMBER(User_TCUsPerFlatcar),User_TCUsPerFlatcar,TCUsPerFlatcarDefault))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,1,IF(ISNUMBER(User_TCUsPerFlatcar),User_TCUsPerFlatcar,TCUsPerFlatcarDefault))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,1,IF(ISNUMBER(User_TCUsPerFlatcar),User_TCUsPerFlatcar,TCUsPerFlatcarDefault))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,1,IF(ISNUMBER(User_TCUsPerFlatcar),User_TCUsPerFlatcar,TCUsPerFlatcarDefault))))","v":""},null,{"$f":"$C37&\"=\"&VLOOKUP($C37,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L202C1=Average TCUs Per Flat Car"}]
[203,"Number of TCUs","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUs),User_TCUs,NC)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUs),User_TCUs,NC)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUs),User_TCUs,NC)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUs),User_TCUs,NC)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUs),User_TCUs,NC)))","v":""}]
[204,"Number of flat cars","L203/L202",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",Line203/Line202,0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",Line203/Line202,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",Line203/Line202,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",Line203/Line202,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",Line203/Line202,0))","v":""}]
[205,"Car miles including empty return","L111*L201; TOFC:L111*L204",{"$f":"IF(ISBLANK(D$5),\"\",IF(SZ<>\"Intermodal\",Line111*Line201,IF(User_TOFCPlanCode=4,0,Line111*Line204)))","v":1976.92281083076},{"$f":"IF(ISBLANK(E$5),\"\",IF(SZ<>\"Intermodal\",Line111*Line201,IF(User_TOFCPlanCode=4,0,Line111*Line204)))","v":""},{"$f":"IF(ISBLANK(F$5),\"\",IF(SZ<>\"Intermodal\",Line111*Line201,IF(User_TOFCPlanCode=4,0,Line111*Line204)))","v":""},{"$f":"IF(ISBLANK(G$5),\"\",IF(SZ<>\"Intermodal\",Line111*Line201,IF(User_TOFCPlanCode=4,0,Line111*Line204)))","v":""},{"$f":"IF(ISBLANK(H$5),\"\",IF(SZ<>\"Intermodal\",Line111*Line201,IF(User_TOFCPlanCode=4,0,Line111*Line204)))","v":""},{"$f":"SUM(D40:H40)","v":1976.92281083076}]
[206,"UC per CM-OPR","E1L102C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C41,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C41,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C41,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C41,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C41,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C41&\"=\"&VLOOKUP($C41,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L102C1=Car Mile (CM) - Other Than Clerical, OPR Expense"}]
[207,"VC-CM Other-OPR","L205*L206",{"$f":"IF(ISBLANK(RR),\"\",Line205*Line206)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line206)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line206)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line206)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line206)","v":""},{"$f":"SUM(D42:H42)","v":0}]
[208,"UC per CM-DRL","E1L102C2",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C43,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C43,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C43,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C43,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C43,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C43&\"=\"&VLOOKUP($C43,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L102C2=Car Mile (CM) - Other Than Clerical, DRL Expense"}]
[209,"VC-CM Other-DRL","L205*L208",{"$f":"IF(ISBLANK(RR),\"\",Line205*Line208)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line208)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line208)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line208)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line208)","v":""},{"$f":"SUM(D44:H44)","v":0}]
[210,"UC per CM-ROI","E1L102C3",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C45,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C45,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C45,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C45,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C45,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C45&\"=\"&VLOOKUP($C45,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L102C3=Car Mile (CM) - Other Than Clerical, ROI Expense"}]
[211,"VC-CM Other-ROI","L205*L210",{"$f":"IF(ISBLANK(RR),\"\",Line205*Line210)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line210)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line210)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line210)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line210)","v":""},{"$f":"SUM(D46:H46)","v":0}]
["HDR","Gross Ton Mile Costs","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[212,"Tare weight (tons) this car type",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C1\"","v":"E2L106C1"},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(User_FreightCarTareWeight),User_FreightCarTareWeight,VLOOKUP(RR&\"-\"&$C48,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":30.9},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(User_FreightCarTareWeight),User_FreightCarTareWeight,VLOOKUP(RR&\"-\"&$C48,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(User_FreightCarTareWeight),User_FreightCarTareWeight,VLOOKUP(RR&\"-\"&$C48,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(User_FreightCarTareWeight),User_FreightCarTareWeight,VLOOKUP(RR&\"-\"&$C48,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(User_FreightCarTareWeight),User_FreightCarTareWeight,VLOOKUP(RR&\"-\"&$C48,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C48&\"=\"&VLOOKUP($C48,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C1=Average Tare Weight, HOPPER - COVERED"}]
[213,"Freight car tare ton mileage","L111*L201*L212; TOFC:L111*L204*L212",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line111*Line201*Line212,Line111*Line204*Line212))","v":61086.914854670482},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line111*Line201*Line212,Line111*Line204*Line212))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line111*Line201*Line212,Line111*Line204*Line212))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line111*Line201*Line212,Line111*Line204*Line212))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line111*Line201*Line212,Line111*Line204*Line212))","v":""},{"$f":"SUM(D49:H49)","v":61086.914854670482}]
[214,"Tare weight (tons) of one TCU",{"$f":"IF(User_TCURefrigFlag=\"Y\",\"E2L203C1\",\"E2L204C1\")","v":"E2L204C1"},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,13.9,IF(ISNUMBER(User_TCUTareWeight),User_TCUTareWeight,TCUTareWeightDefault))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,13.9,IF(ISNUMBER(User_TCUTareWeight),User_TCUTareWeight,TCUTareWeightDefault))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,13.9,IF(ISNUMBER(User_TCUTareWeight),User_TCUTareWeight,TCUTareWeightDefault))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,13.9,IF(ISNUMBER(User_TCUTareWeight),User_TCUTareWeight,TCUTareWeightDefault))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(User_TOFCPlanCode=4,13.9,IF(ISNUMBER(User_TCUTareWeight),User_TCUTareWeight,TCUTareWeightDefault))))","v":""},null,{"$f":"$C50&\"=\"&VLOOKUP($C50,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L204C1=Average Tare Weight - Non-Refrigerated TCU"}]
[215,"E/L ratio - TCU","E2L207C1",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUELRatio),User_TCUELRatio,TCUELRatioDefault)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUELRatio),User_TCUELRatio,TCUELRatioDefault)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUELRatio),User_TCUELRatio,TCUELRatioDefault)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUELRatio),User_TCUELRatio,TCUELRatioDefault)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUELRatio),User_TCUELRatio,TCUELRatioDefault)))","v":""},null,{"$f":"$C51&\"=\"&VLOOKUP($C51,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L207C1=L/E Ratio - Refrigerated/Non-Refrigerated - TCU"}]
[216,"TCU tare ton mileage","L103*L203*L214*L215",{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line214*Line215)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line214*Line215)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line214*Line215)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line214*Line215)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line214*Line215)","v":""},{"$f":"SUM(D52:H52)","v":0}]
[217,"Weight of shipment (tons)","[User]",{"$f":"IF(ISBLANK(RR),\"\",NC*WT)","v":80},{"$f":"IF(ISBLANK(RR),\"\",NC*WT)","v":""},{"$f":"IF(ISBLANK(RR),\"\",NC*WT)","v":""},{"$f":"IF(ISBLANK(RR),\"\",NC*WT)","v":""},{"$f":"IF(ISBLANK(RR),\"\",NC*WT)","v":""}]
[218,"Shipment net ton miles","L103*L217",{"$f":"IF(ISBLANK(RR),\"\",Line103*Line217)","v":80000},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line217)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line217)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line217)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line217)","v":""},{"$f":"SUM(D54:H54)","v":80000}]
[219,"Gross ton miles","L213+L216+L218",{"$f":"IF(ISBLANK(RR),\"\",Line213+Line216+Line218)","v":141086.91485467047},{"$f":"IF(ISBLANK(RR),\"\",Line213+Line216+Line218)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line213+Line216+Line218)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line213+Line216+Line218)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line213+Line216+Line218)","v":""},{"$f":"SUM(D55:H55)","v":141086.91485467047}]
[220,"UC per GTM-OPR","E1L101C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":2.3218368538080402E-3},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C56&\"=\"&VLOOKUP($C56,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L101C1=Gross Ton Mile (GTM), OPR Expense"}]
[221,"VC-GTM-OPR","L219*L220",{"$f":"IF(ISBLANK(RR),\"\",Line219*Line220)","v":327.58079849965094},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line220)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line220)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line220)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line220)","v":""},{"$f":"SUM(D57:H57)","v":327.58079849965094}]
[222,"UC per GTM-DRL","E1L101C2",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1.0304982814394201E-3},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C58&\"=\"&VLOOKUP($C58,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L101C2=Gross Ton Mile (GTM), DRL Expense"}]
[223,"VC-GTM-DRL","L219*L222",{"$f":"IF(ISBLANK(RR),\"\",Line219*Line222)","v":145.3898232913277},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line222)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line222)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line222)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line222)","v":""},{"$f":"SUM(D59:H59)","v":145.3898232913277}]
[224,"UC per GTM-ROI","E1L101C3",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C60,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":2.1317564600293899E-3},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C60,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C60,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C60,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C60,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C60&\"=\"&VLOOKUP($C60,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L101C3=Gross Ton Mile (GTM), ROI Expense"}]
[225,"VC-GTM-ROI","L219*L224",{"$f":"IF(ISBLANK(RR),\"\",Line219*Line224)","v":300.76294216706026},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line224)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line224)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line224)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line219*Line224)","v":""},{"$f":"SUM(D61:H61)","v":300.76294216706026}]
["HDR","Locomotive Unit Miles","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[226,"Average loco units/Unit train","E2L208C1",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L226,D$3)),INDEX(User_L226,D$3),VLOOKUP(RR&\"-\"&$C63,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":3.3800302893865402},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L226,E$3)),INDEX(User_L226,E$3),VLOOKUP(RR&\"-\"&$C63,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L226,F$3)),INDEX(User_L226,F$3),VLOOKUP(RR&\"-\"&$C63,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L226,G$3)),INDEX(User_L226,G$3),VLOOKUP(RR&\"-\"&$C63,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L226,H$3)),INDEX(User_L226,H$3),VLOOKUP(RR&\"-\"&$C63,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C63&\"=\"&VLOOKUP($C63,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L208C1=Average Locomotive Units - Unit Train"}]
[227,"Average loco units/Way train","E2L209C1",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L227,D$3)),INDEX(User_L227,D$3),VLOOKUP(RR&\"-\"&$C64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":2.0571275181762698},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L227,E$3)),INDEX(User_L227,E$3),VLOOKUP(RR&\"-\"&$C64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L227,F$3)),INDEX(User_L227,F$3),VLOOKUP(RR&\"-\"&$C64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L227,G$3)),INDEX(User_L227,G$3),VLOOKUP(RR&\"-\"&$C64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L227,H$3)),INDEX(User_L227,H$3),VLOOKUP(RR&\"-\"&$C64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C64&\"=\"&VLOOKUP($C64,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L209C1=Average Locomotive Units - Way Train"}]
[228,"Average loco units/Through train","E2L210C1",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L228,D$3)),INDEX(User_L228,D$3),VLOOKUP(RR&\"-\"&$C65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":3.31597647188162},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L228,E$3)),INDEX(User_L228,E$3),VLOOKUP(RR&\"-\"&$C65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L228,F$3)),INDEX(User_L228,F$3),VLOOKUP(RR&\"-\"&$C65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L228,G$3)),INDEX(User_L228,G$3),VLOOKUP(RR&\"-\"&$C65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L228,H$3)),INDEX(User_L228,H$3),VLOOKUP(RR&\"-\"&$C65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C65&\"=\"&VLOOKUP($C65,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L210C1=Average Locomotive Units - Through Train"}]
[229,"Unit train loco unit miles","L108*L226",{"$f":"IF(ISBLANK(RR),\"\",Line108*Line226)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line108*Line226)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line108*Line226)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line108*Line226)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line108*Line226)","v":""}]
[230,"Way train loco unit miles","L109*L227",{"$f":"IF(ISBLANK(RR),\"\",Line109*Line227)","v":64.670598547062994},{"$f":"IF(ISBLANK(RR),\"\",Line109*Line227)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line109*Line227)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line109*Line227)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line109*Line227)","v":""}]
[231,"Through train loco unit miles","L110*L228",{"$f":"IF(ISBLANK(RR),\"\",Line110*Line228)","v":6451.1840777496127},{"$f":"IF(ISBLANK(RR),\"\",Line110*Line228)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line110*Line228)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line110*Line228)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line110*Line228)","v":""}]
[232,"Avg trailing gross tons-Unit round trip","E2L211C1*L105",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L232,D$3)),INDEX(User_L232,D$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C69,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":20109.14742859266},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L232,E$3)),INDEX(User_L232,E$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C69,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L232,F$3)),INDEX(User_L232,F$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C69,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L232,G$3)),INDEX(User_L232,G$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C69,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L232,H$3)),INDEX(User_L232,H$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C69,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"LEFT($C69,8)&\"=\"&VLOOKUP(LEFT($C69,8),ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L211C1=Average Gross Tons - Unit Train"}]
[233,"Avg trailing gross tons-Way round trip","E2L212C1*L105",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L233,D$3)),INDEX(User_L233,D$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C70,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":5229.6360278061547},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L233,E$3)),INDEX(User_L233,E$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C70,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L233,F$3)),INDEX(User_L233,F$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C70,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L233,G$3)),INDEX(User_L233,G$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C70,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L233,H$3)),INDEX(User_L233,H$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C70,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"LEFT($C70,8)&\"=\"&VLOOKUP(LEFT($C70,8),ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L212C1=Average Gross Tons - Way Train"}]
[234,"Avg trailing gross tons-Through round trip","E2L213C1*L105",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L234,D$3)),INDEX(User_L234,D$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C71,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":14737.997599254424},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L234,E$3)),INDEX(User_L234,E$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C71,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L234,F$3)),INDEX(User_L234,F$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C71,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L234,G$3)),INDEX(User_L234,G$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C71,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L234,H$3)),INDEX(User_L234,H$3),Line105*VLOOKUP(RR&\"-\"&LEFT($C71,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"LEFT($C71,8)&\"=\"&VLOOKUP(LEFT($C71,8),ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L213C1=Average Gross Tons - Through Train"}]
[235,"Gross tons - cars & contents","(L105*L201*L212)+L217; TOFC:(L105*L204*L212)+(L203*L214*L215)+L217",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",(Line105*Line201*Line212)+Line217,(Line105*Line204*Line212)+(Line203*Line214*Line215)+Line217))","v":141.08691485467048},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",(Line105*Line201*Line212)+Line217,(Line105*Line204*Line212)+(Line203*Line214*Line215)+Line217))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",(Line105*Line201*Line212)+Line217,(Line105*Line204*Line212)+(Line203*Line214*Line215)+Line217))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",(Line105*Line201*Line212)+Line217,(Line105*Line204*Line212)+(Line203*Line214*Line215)+Line217))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",(Line105*Line201*Line212)+Line217,(Line105*Line204*Line212)+(Line203*Line214*Line215)+Line217))","v":""},{"$f":"SUM(D72:H72)","v":141.08691485467048}]
[236,"Percent of Unit train tonnage","L235/L232",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",Line235/Line232,0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",Line235/Line232,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",Line235/Line232,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",Line235/Line232,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",Line235/Line232,0))","v":""}]
[237,"Percent of Way train tonnage","L235/L233",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line233,0))","v":2.6978343063361675E-2},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line233,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line233,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line233,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line233,0))","v":""}]
[238,"Percent of Through train tonnage","L235/L234",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line234,0))","v":9.5730043314573403E-3},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line234,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line234,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line234,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",Line235/Line234,0))","v":""}]
[239,"Unit train LUM (alloc)","L229*L236",{"$f":"IF(ISBLANK(RR),\"\",Line229*Line236)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line229*Line236)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line229*Line236)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line229*Line236)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line229*Line236)","v":""}]
[240,"Way train LUM (alloc)","L230*L237",{"$f":"IF(ISBLANK(RR),\"\",Line230*Line237)","v":1.7447055937156046},{"$f":"IF(ISBLANK(RR),\"\",Line230*Line237)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line230*Line237)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line230*Line237)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line230*Line237)","v":""}]
[241,"Thru train LUM (alloc)","L231*L238",{"$f":"IF(ISBLANK(RR),\"\",Line231*Line238)","v":61.757213119325669},{"$f":"IF(ISBLANK(RR),\"\",Line231*Line238)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line231*Line238)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line231*Line238)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line231*Line238)","v":""}]
[242,"Total shipment LUM (allocated)","L239+L240+L241",{"$f":"IF(ISBLANK(RR),\"\",Line239+Line240+Line241)","v":63.501918713041277},{"$f":"IF(ISBLANK(RR),\"\",Line239+Line240+Line241)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line239+Line240+Line241)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line239+Line240+Line241)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line239+Line240+Line241)","v":""},{"$f":"SUM(D79:H79)","v":63.501918713041277}]
[243,"UC per LUM-OPR","E1L105C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C80,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":4.7579488438892099},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C80,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C80,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C80,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C80,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C80&\"=\"&VLOOKUP($C80,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L105C1=Locomotive Unit Mile (LUM), OPR Expense"}]
[244,"VC-LUM-OPR","L242*L243",{"$f":"IF(ISBLANK(RR),\"\",Line242*Line243)","v":302.13888072546132},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line243)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line243)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line243)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line243)","v":""},{"$f":"SUM(D81:H81)","v":302.13888072546132}]
[245,"UC per LUM-DRL","E1L105C2",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C82,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0.84062305220072797},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C82,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C82,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C82,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C82,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C82&\"=\"&VLOOKUP($C82,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L105C2=Locomotive Unit Mile (LUM), DRL Expense"}]
[246,"VC-LUM-DRL","L242*L245",{"$f":"IF(ISBLANK(RR),\"\",Line242*Line245)","v":53.381176729159279},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line245)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line245)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line245)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line245)","v":""},{"$f":"SUM(D83:H83)","v":53.381176729159279}]
[247,"UC per LUM-ROI","E1L105C3",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C84,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0.81566752566563605},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C84,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C84,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C84,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C84,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C84&\"=\"&VLOOKUP($C84,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L105C3=Locomotive Unit Mile (LUM), ROI Expense"}]
[248,"VC-LUM-ROI","L242*L247",{"$f":"IF(ISBLANK(RR),\"\",Line242*Line247)","v":51.796452911686728},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line247)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line247)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line247)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line242*Line247)","v":""},{"$f":"SUM(D85:H85)","v":51.796452911686728}]
["HDR","Carload and Clerical Costs","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[250,"Shipment origination/termination","Originate=1; Terminate=1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A87,URCSSegmentsHeaders,0),FALSE))","v":2},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A87,URCSSegmentsHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A87,URCSSegmentsHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A87,URCSSegmentsHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A87,URCSSegmentsHeaders,0),FALSE))","v":""}]
[251,"Carloads orig/term (TOFC)","L204*L250",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line204*Line250))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line204*Line250))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line204*Line250))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line204*Line250))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line204*Line250))","v":""}]
[252,"Carloads orig/term (Non-TOFC)","L201*L250",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,Line201*Line250))","v":2},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,Line201*Line250))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,Line201*Line250))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,Line201*Line250))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,Line201*Line250))","v":""}]
[253,"Carloads handled (TOFC)","L204",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line204)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line204)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line204)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line204)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line204)))","v":""}]
[254,"Carloads handled (Non-TOFC)","L201",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line201)))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line201)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line201)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line201)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Intermodal\",0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line201)))","v":""}]
[255,"UC per CM Cler-OPR","E1L110C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C92,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C92,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C92,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C92,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C92,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C92&\"=\"&VLOOKUP($C92,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L110C1=Car Mile (CM) - Clerical, OPR Expense"}]
[256,"VC-CM Cler-OPR","L205*L255",{"$f":"IF(ISBLANK(RR),\"\",Line205*Line255)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line255)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line255)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line255)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line205*Line255)","v":""},{"$f":"SUM(D93:H93)","v":0}]
[257,"UC per CLOT Cler-OPR","E1L109C1",{"$f":"IF(ISBLANK(RR),\"\",AdjustL257*VLOOKUP(RR&\"-\"&$C94,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":6.92833589137242},{"$f":"IF(ISBLANK(RR),\"\",AdjustL257*VLOOKUP(RR&\"-\"&$C94,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",AdjustL257*VLOOKUP(RR&\"-\"&$C94,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",AdjustL257*VLOOKUP(RR&\"-\"&$C94,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",AdjustL257*VLOOKUP(RR&\"-\"&$C94,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C94&\"=\"&VLOOKUP($C94,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L109C1=CLOT (Carloads Orig Or Term) - Clerical, OPR Expense"}]
[258,"VC-CLOT Cler-OPR","L252*L257; TOFC:L251*L257",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line252*Line257,Line251*Line257))","v":13.85667178274484},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line252*Line257,Line251*Line257))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line252*Line257,Line251*Line257))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line252*Line257,Line251*Line257))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line252*Line257,Line251*Line257))","v":""},{"$f":"SUM(D95:H95)","v":13.85667178274484}]
[259,"UC per CLOR Cler-OPR","E1L107C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C96,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C96,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C96,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C96,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C96,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C96&\"=\"&VLOOKUP($C96,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L107C1=CLOR (Carloads Handled) - Clerical, OPR Expense"}]
[260,"VC-CLOR Cler-OPR","L254*L259",{"$f":"IF(ISBLANK(RR),\"\",Line254*Line259)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line259)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line259)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line259)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line259)","v":""},{"$f":"SUM(D97:H97)","v":0}]
[261,"UC per CLOT Other-OPR","E1L108C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C98,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C98,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C98,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C98,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C98,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C98&\"=\"&VLOOKUP($C98,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L108C1=CLOT (Carloads Orig Or Term) - Other, OPR Expense"}]
[262,"VC-CLOT Other-OPR","L252*L261",{"$f":"IF(ISBLANK(RR),\"\",Line252*Line261)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line252*Line261)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line252*Line261)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line252*Line261)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line252*Line261)","v":""},{"$f":"SUM(D99:H99)","v":0}]
[263,"UC per CLOR Other-OPR","E1L106C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C100,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1.6930165994223101},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C100,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C100,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C100,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C100,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C100&\"=\"&VLOOKUP($C100,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L106C1=CLOR (Carloads Handled) - Other, OPR Expense"}]
[264,"VC-CLOR Other-OPR","L254*L263; TOFC:L253*L257",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line254*Line263,Line253*Line263))","v":1.6930165994223101},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line254*Line263,Line253*Line263))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line254*Line263,Line253*Line263))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line254*Line263,Line253*Line263))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",Line254*Line263,Line253*Line263))","v":""},{"$f":"SUM(D101:H101)","v":1.6930165994223101}]
[265,"UC per CLOR Other-DRL","E1L106C2",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C102,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C102,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C102,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C102,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C102,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C102&\"=\"&VLOOKUP($C102,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L106C2=CLOR (Carloads Handled) - Other, DRL Expense"}]
[266,"VC-CLOR Other-DRL","L254*L265",{"$f":"IF(ISBLANK(RR),\"\",Line254*Line265)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line265)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line265)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line265)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line265)","v":""},{"$f":"SUM(D103:H103)","v":0}]
[267,"UC per CLOR Other-ROI","E1L106C3",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C104,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C104,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C104,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C104,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C104,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C104&\"=\"&VLOOKUP($C104,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L106C3=CLOR (Carloads Handled) - Other, ROI Expense"}]
[268,"VC-CLOR Other-ROI","L254*L267",{"$f":"IF(ISBLANK(RR),\"\",Line254*Line267)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line267)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line267)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line267)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line254*Line267)","v":""},{"$f":"SUM(D105:H105)","v":0}]
["HDR","Train Mile Costs - Crew Wage Expense","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[269,"Shipment share-Unit train miles","L108",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L269,D$3)),INDEX(User_L269,D$3),Line108)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L269,E$3)),INDEX(User_L269,E$3),Line108)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L269,F$3)),INDEX(User_L269,F$3),Line108)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L269,G$3)),INDEX(User_L269,G$3),Line108)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L269,H$3)),INDEX(User_L269,H$3),Line108)))","v":""}]
[270,"Shipment share-Way train miles","L109*L237",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L270,D$3)),INDEX(User_L270,D$3),Line109*Line237)))","v":0.84812709873346093},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L270,E$3)),INDEX(User_L270,E$3),Line109*Line237)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L270,F$3)),INDEX(User_L270,F$3),Line109*Line237)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L270,G$3)),INDEX(User_L270,G$3),Line109*Line237)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L270,H$3)),INDEX(User_L270,H$3),Line109*Line237)))","v":""}]
[271,"Shipment share-Thru train miles","L110*L238",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L271,D$3)),INDEX(User_L271,D$3),Line110*Line238)))","v":18.624140925910162},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L271,E$3)),INDEX(User_L271,E$3),Line110*Line238)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L271,F$3)),INDEX(User_L271,F$3),Line110*Line238)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L271,G$3)),INDEX(User_L271,G$3),Line110*Line238)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L271,H$3)),INDEX(User_L271,H$3),Line110*Line238)))","v":""}]
[272,"Total train miles (allocated)","L269+L270+L271",{"$f":"IF(ISBLANK(RR),\"\",Line269+Line270+Line271)","v":19.472268024643622},{"$f":"IF(ISBLANK(RR),\"\",Line269+Line270+Line271)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line269+Line270+Line271)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line269+Line270+Line271)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line269+Line270+Line271)","v":""},{"$f":"SUM(D110:H110)","v":19.472268024643622}]
[273,"Actual crew wage/train mile-Unit","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L273,D$3)),INDEX(User_L273,D$3),0)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L273,E$3)),INDEX(User_L273,E$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L273,F$3)),INDEX(User_L273,F$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L273,G$3)),INDEX(User_L273,G$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",0,IF(ISNUMBER(INDEX(User_L273,H$3)),INDEX(User_L273,H$3),0)))","v":""}]
[274,"Actual crew wage/train mile-Way","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L274,D$3)),INDEX(User_L274,D$3),0)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L274,E$3)),INDEX(User_L274,E$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L274,F$3)),INDEX(User_L274,F$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L274,G$3)),INDEX(User_L274,G$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L274,H$3)),INDEX(User_L274,H$3),0)))","v":""}]
[275,"Actual crew wage/train mile-Thru","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L275,D$3)),INDEX(User_L275,D$3),0)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L275,E$3)),INDEX(User_L275,E$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L275,F$3)),INDEX(User_L275,F$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L275,G$3)),INDEX(User_L275,G$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ=\"Unit\",0,IF(ISNUMBER(INDEX(User_L275,H$3)),INDEX(User_L275,H$3),0)))","v":""}]
[276,"Average/wages per train mile","E2L218C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C114,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":8.8760010513333292},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C114,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C114,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C114,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C114,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C114&\"=\"&VLOOKUP($C114,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L218C1=Average Crew Wages (Assigned To TM-Crew)"}]
[277,"Crew wages adj. ratio-Unit train","L273/L276",{"$f":"IF(ISBLANK(RR),\"\",IF(Line273=0,1,Line273/Line276))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(Line273=0,1,Line273/Line276))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line273=0,1,Line273/Line276))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line273=0,1,Line273/Line276))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line273=0,1,Line273/Line276))","v":""}]
[278,"Crew wages adj. ratio-Way train","L274/L276",{"$f":"IF(ISBLANK(RR),\"\",IF(Line274=0,1,Line274/Line276))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(Line274=0,1,Line274/Line276))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line274=0,1,Line274/Line276))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line274=0,1,Line274/Line276))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line274=0,1,Line274/Line276))","v":""}]
[279,"Crew wages adj. ratio-Thru train","L275/L276",{"$f":"IF(ISBLANK(RR),\"\",IF(Line275=0,1,Line275/Line276))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(Line275=0,1,Line275/Line276))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line275=0,1,Line275/Line276))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line275=0,1,Line275/Line276))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line275=0,1,Line275/Line276))","v":""}]
[280,"UC per TM Crew-OPR","E1L104C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C118,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":11.361180154585099},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C118,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C118,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C118,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C118,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C118&\"=\"&VLOOKUP($C118,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L104C1=Train Mile (TM) - Crew, OPR Expense"}]
[281,"VC-TM Crew-OPR-Unit train","L269*L277*L280",{"$f":"IF(ISBLANK(RR),\"\",Line269*Line277*Line280)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line269*Line277*Line280)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line269*Line277*Line280)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line269*Line277*Line280)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line269*Line277*Line280)","v":""}]
[282,"VC-TM Crew-OPR-Way train","L270*L278*L280",{"$f":"IF(ISBLANK(RR),\"\",Line270*Line278*Line280)","v":9.6357247626964337},{"$f":"IF(ISBLANK(RR),\"\",Line270*Line278*Line280)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line270*Line278*Line280)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line270*Line278*Line280)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line270*Line278*Line280)","v":""}]
[283,"VC-TM Crew-OPR-Thru train","L271*L279*L280",{"$f":"IF(ISBLANK(RR),\"\",Line271*Line279*Line280)","v":211.5922202836467},{"$f":"IF(ISBLANK(RR),\"\",Line271*Line279*Line280)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line271*Line279*Line280)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line271*Line279*Line280)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line271*Line279*Line280)","v":""}]
[284,"Total VC-TM Crew-OPR","L281+L282+L283",{"$f":"IF(ISBLANK(RR),\"\",Line281+Line282+Line283)","v":221.22794504634314},{"$f":"IF(ISBLANK(RR),\"\",Line281+Line282+Line283)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line281+Line282+Line283)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line281+Line282+Line283)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line281+Line282+Line283)","v":""},{"$f":"SUM(D122:H122)","v":221.22794504634314}]
["HDR","Train Mile Costs - Other Expenses","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[285,"UC per TM Other-OPR","E1L103C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C124,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":0.63688697269414296},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C124,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C124,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C124,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C124,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C124&\"=\"&VLOOKUP($C124,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L103C1=Train Mile (TM) - Other Than Crew, OPR Expense"}]
[286,"VC-TM Other-OPR","L272*L285",{"$f":"IF(ISBLANK(RR),\"\",Line272*Line285)","v":12.401633833704235},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line285)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line285)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line285)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line285)","v":""},{"$f":"SUM(D125:H125)","v":12.401633833704235}]
[287,"UC per TM Other-DRL","E1L103C2",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C126,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":-3.4287390173140699E-4},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C126,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C126,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C126,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C126,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C126&\"=\"&VLOOKUP($C126,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L103C2=Train Mile (TM) - Other Than Crew, DRL Expense"}]
[288,"VC-TM Other-DRL","L272*L287",{"$f":"IF(ISBLANK(RR),\"\",Line272*Line287)","v":-6.6765325131692759E-3},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line287)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line287)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line287)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line287)","v":""},{"$f":"SUM(D127:H127)","v":-6.6765325131692759E-3}]
[289,"UC per TM Other-ROI","E1L103C3",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C128,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1.77341275904486E-3},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C128,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C128,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C128,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C128,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C128&\"=\"&VLOOKUP($C128,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L103C3=Train Mile (TM) - Other Than Crew, ROI Expense"}]
[290,"VC-TM Other-ROI","L272*L289",{"$f":"IF(ISBLANK(RR),\"\",Line272*Line289)","v":3.4532368562444252E-2},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line289)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line289)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line289)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line272*Line289)","v":""},{"$f":"SUM(D129:H129)","v":3.4532368562444252E-2}]
["HDR","Industry, Interchange and Inter & Intratrain Switching","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[301,"SEM per Industry switch event",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C25\"","v":"E2L106C25"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L301,D$3)),INDEX(User_L301,D$3),AdjustL301*VLOOKUP(RR&\"-\"&$C131,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":4.3365301515291002},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L301,E$3)),INDEX(User_L301,E$3),AdjustL301*VLOOKUP(RR&\"-\"&$C131,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L301,F$3)),INDEX(User_L301,F$3),AdjustL301*VLOOKUP(RR&\"-\"&$C131,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L301,G$3)),INDEX(User_L301,G$3),AdjustL301*VLOOKUP(RR&\"-\"&$C131,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L301,H$3)),INDEX(User_L301,H$3),AdjustL301*VLOOKUP(RR&\"-\"&$C131,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C131&\"=\"&VLOOKUP($C131,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C25=SEMs per Industry Switch, HOPPER - COVERED"}]
[302,"SEM per Interchange switch event",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C26\"","v":"E2L106C26"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L302,D$3)),INDEX(User_L302,D$3),AdjustL302*VLOOKUP(RR&\"-\"&$C132,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":2.3850915833410098},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L302,E$3)),INDEX(User_L302,E$3),AdjustL302*VLOOKUP(RR&\"-\"&$C132,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L302,F$3)),INDEX(User_L302,F$3),AdjustL302*VLOOKUP(RR&\"-\"&$C132,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L302,G$3)),INDEX(User_L302,G$3),AdjustL302*VLOOKUP(RR&\"-\"&$C132,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L302,H$3)),INDEX(User_L302,H$3),AdjustL302*VLOOKUP(RR&\"-\"&$C132,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C132&\"=\"&VLOOKUP($C132,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C26=SEMs per Interchange Switch, HOPPER - COVERED"}]
[303,"SEM per I&I train switch event",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C29\"","v":"E2L106C29"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L303,D$3)),INDEX(User_L303,D$3),AdjustL303*VLOOKUP(RR&\"-\"&$C133,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":1.0841325378822799},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L303,E$3)),INDEX(User_L303,E$3),AdjustL303*VLOOKUP(RR&\"-\"&$C133,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L303,F$3)),INDEX(User_L303,F$3),AdjustL303*VLOOKUP(RR&\"-\"&$C133,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L303,G$3)),INDEX(User_L303,G$3),AdjustL303*VLOOKUP(RR&\"-\"&$C133,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L303,H$3)),INDEX(User_L303,H$3),AdjustL303*VLOOKUP(RR&\"-\"&$C133,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C133&\"=\"&VLOOKUP($C133,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C29=SEMs per I&I Switch, HOPPER - COVERED"}]
[304,"Spotted-Pulled Ratio this car",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C8\"","v":"E2L106C8"},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L304,D$3)),INDEX(User_L304,D$3),VLOOKUP(RR&\"-\"&$C134,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":2},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L304,E$3)),INDEX(User_L304,E$3),VLOOKUP(RR&\"-\"&$C134,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L304,F$3)),INDEX(User_L304,F$3),VLOOKUP(RR&\"-\"&$C134,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L304,G$3)),INDEX(User_L304,G$3),VLOOKUP(RR&\"-\"&$C134,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L304,H$3)),INDEX(User_L304,H$3),VLOOKUP(RR&\"-\"&$C134,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C134&\"=\"&VLOOKUP($C134,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C8=Spotted-to-Pulled Ratio, HOPPER - COVERED"}]
[305,"Industry switch events","L252*L304; TOFC:L251*L304",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L305,D$3)),INDEX(User_L305,D$3),IF(SZ<>\"Intermodal\",Line252*Line304,Line251*Line304)))","v":4},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L305,E$3)),INDEX(User_L305,E$3),IF(SZ<>\"Intermodal\",Line252*Line304,Line251*Line304)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L305,F$3)),INDEX(User_L305,F$3),IF(SZ<>\"Intermodal\",Line252*Line304,Line251*Line304)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L305,G$3)),INDEX(User_L305,G$3),IF(SZ<>\"Intermodal\",Line252*Line304,Line251*Line304)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L305,H$3)),INDEX(User_L305,H$3),IF(SZ<>\"Intermodal\",Line252*Line304,Line251*Line304)))","v":""}]
[306,"Avg miles bet. Interchange event",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C24\"","v":"E2L106C24"},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C136,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1900.4198779763999},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C136,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C136,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C136,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C136,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C136&\"=\"&VLOOKUP($C136,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C24=Average Miles between Interchange Switches, HOPPER - COVERED"}]
[307,"Number of interchange events","Receive=1; Deliver=1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A137,URCSSegmentsHeaders,0),FALSE))","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A137,URCSSegmentsHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A137,URCSSegmentsHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A137,URCSSegmentsHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(SG,URCSSegments,MATCH(\"L\"&$A137,URCSSegmentsHeaders,0),FALSE))","v":""}]
[308,"Number of cars interchanged","L105*L201*L307; TOFC:L105*L204*L307",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L308,D$3)),INDEX(User_L308,D$3),IF(SZ<>\"Intermodal\",Line105*Line201*Line307,Line105*Line204*Line307)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L308,E$3)),INDEX(User_L308,E$3),IF(SZ<>\"Intermodal\",Line105*Line201*Line307,Line105*Line204*Line307)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L308,F$3)),INDEX(User_L308,F$3),IF(SZ<>\"Intermodal\",Line105*Line201*Line307,Line105*Line204*Line307)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L308,G$3)),INDEX(User_L308,G$3),IF(SZ<>\"Intermodal\",Line105*Line201*Line307,Line105*Line204*Line307)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L308,H$3)),INDEX(User_L308,H$3),IF(SZ<>\"Intermodal\",Line105*Line201*Line307,Line105*Line204*Line307)))","v":""}]
[309,"Avg miles between I&I sw event",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C23\"","v":"E2L106C23"},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L309,D$3)),INDEX(User_L309,D$3),VLOOKUP(RR&\"-\"&$C139,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":200},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L309,E$3)),INDEX(User_L309,E$3),VLOOKUP(RR&\"-\"&$C139,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L309,F$3)),INDEX(User_L309,F$3),VLOOKUP(RR&\"-\"&$C139,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L309,G$3)),INDEX(User_L309,G$3),VLOOKUP(RR&\"-\"&$C139,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L309,H$3)),INDEX(User_L309,H$3),VLOOKUP(RR&\"-\"&$C139,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C139&\"=\"&VLOOKUP($C139,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C23=Average Miles between I&I Switches, HOPPER - COVERED"}]
[310,"Cars given I&I switch","L205/L309",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L310,D$3)),INDEX(User_L310,D$3),Line205/Line309))","v":9.8846140541538006},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L310,E$3)),INDEX(User_L310,E$3),Line205/Line309))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L310,F$3)),INDEX(User_L310,F$3),Line205/Line309))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L310,G$3)),INDEX(User_L310,G$3),Line205/Line309))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L310,H$3)),INDEX(User_L310,H$3),Line205/Line309))","v":""}]
[311,"Total SEM-Industry","L301*L305",{"$f":"IF(ISBLANK(RR),\"\",Line301*Line305)","v":17.346120606116401},{"$f":"IF(ISBLANK(RR),\"\",Line301*Line305)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line301*Line305)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line301*Line305)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line301*Line305)","v":""}]
[312,"Total SEM-Interchange","L302*L308",{"$f":"IF(ISBLANK(RR),\"\",Line302*Line308)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line302*Line308)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line302*Line308)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line302*Line308)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line302*Line308)","v":""}]
[313,"Total SEM-I&I train","L303*L310",{"$f":"IF(ISBLANK(RR),\"\",Line303*Line310)","v":10.716231720516612},{"$f":"IF(ISBLANK(RR),\"\",Line303*Line310)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line303*Line310)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line303*Line310)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line303*Line310)","v":""}]
[314,"Total SEM","L311+L312+L313",{"$f":"IF(ISBLANK(RR),\"\",Line311+Line312+Line313)","v":28.062352326633011},{"$f":"IF(ISBLANK(RR),\"\",Line311+Line312+Line313)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line311+Line312+Line313)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line311+Line312+Line313)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line311+Line312+Line313)","v":""},{"$f":"SUM(D144:H144)","v":28.062352326633011}]
[315,"UC per SEM-OPR","E1L111C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C145,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":6.0228035161016402},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C145,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C145,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C145,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C145,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C145&\"=\"&VLOOKUP($C145,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L111C1=Switch Engine Minutes (SEM), OPR Expense"}]
[316,"VC-SEM-OPR","L314*L315",{"$f":"IF(ISBLANK(RR),\"\",Line314*Line315)","v":169.01403426292833},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line315)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line315)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line315)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line315)","v":""},{"$f":"SUM(D146:H146)","v":169.01403426292833}]
[317,"UC per SEM-DRL","E1L111C2",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C147,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1.65613308535255},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C147,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C147,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C147,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C147,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C147&\"=\"&VLOOKUP($C147,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L111C2=Switch Engine Minutes (SEM), DRL Expense"}]
[318,"VC-SEM-DRL","L314*L317",{"$f":"IF(ISBLANK(RR),\"\",Line314*Line317)","v":46.47499014095704},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line317)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line317)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line317)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line317)","v":""},{"$f":"SUM(D148:H148)","v":46.47499014095704}]
[319,"UC per SEM-ROI","E1L111C3",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C149,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":5.0243142132773198},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C149,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C149,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C149,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C149,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C149&\"=\"&VLOOKUP($C149,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L111C3=Switch Engine Minutes (SEM), ROI Expense"}]
[320,"VC-SEM-ROI","L314*L319",{"$f":"IF(ISBLANK(RR),\"\",Line314*Line319)","v":140.99407565269809},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line319)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line319)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line319)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line314*Line319)","v":""},{"$f":"SUM(D150:H150)","v":140.99407565269809}]
["HDR","Intraterminal and Interterminal Switching","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[321,"Cars-Intraterm switching","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L321,D$3)),INDEX(User_L321,D$3),NC)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L321,E$3)),INDEX(User_L321,E$3),NC)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L321,F$3)),INDEX(User_L321,F$3),NC)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L321,G$3)),INDEX(User_L321,G$3),NC)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L321,H$3)),INDEX(User_L321,H$3),NC)))","v":""}]
[322,"Cars-Interterm switching","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L322,D$3)),INDEX(User_L322,D$3),NC)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L322,E$3)),INDEX(User_L322,E$3),NC)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L322,F$3)),INDEX(User_L322,F$3),NC)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L322,G$3)),INDEX(User_L322,G$3),NC)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L322,H$3)),INDEX(User_L322,H$3),NC)))","v":""}]
[323,"Cars-Intraterminal switching including empty","L304*L321",{"$f":"IF(ISBLANK(RR),\"\",Line304*Line321)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line304*Line321)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line304*Line321)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line304*Line321)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line304*Line321)","v":""}]
[324,"Cars-Interterminal switching including empty","L304*L322",{"$f":"IF(ISBLANK(RR),\"\",Line304*Line322)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line304*Line322)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line304*Line322)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line304*Line322)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line304*Line322)","v":""}]
[325,"SEM per Intraterminal switch",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C27\"","v":"E2L106C27"},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L325,D$3)),INDEX(User_L325,D$3),AdjustL325*VLOOKUP(RR&\"-\"&$C156,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L325,E$3)),INDEX(User_L325,E$3),AdjustL325*VLOOKUP(RR&\"-\"&$C156,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L325,F$3)),INDEX(User_L325,F$3),AdjustL325*VLOOKUP(RR&\"-\"&$C156,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L325,G$3)),INDEX(User_L325,G$3),AdjustL325*VLOOKUP(RR&\"-\"&$C156,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L325,H$3)),INDEX(User_L325,H$3),AdjustL325*VLOOKUP(RR&\"-\"&$C156,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C156&\"=\"&VLOOKUP($C156,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C27=SEMs per Intraterminal Switch, HOPPER - COVERED"}]
[326,"SEM per Interterminal switch",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C28\"","v":"E2L106C28"},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L326,D$3)),INDEX(User_L326,D$3),AdjustL326*VLOOKUP(RR&\"-\"&$C157,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L326,E$3)),INDEX(User_L326,E$3),AdjustL326*VLOOKUP(RR&\"-\"&$C157,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L326,F$3)),INDEX(User_L326,F$3),AdjustL326*VLOOKUP(RR&\"-\"&$C157,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L326,G$3)),INDEX(User_L326,G$3),AdjustL326*VLOOKUP(RR&\"-\"&$C157,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L326,H$3)),INDEX(User_L326,H$3),AdjustL326*VLOOKUP(RR&\"-\"&$C157,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C157&\"=\"&VLOOKUP($C157,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C28=SEMs per Interterminal Switch, HOPPER - COVERED"}]
[327,"Total SEM Intraterm","L323*L325",{"$f":"IF(ISBLANK(RR),\"\",Line323*Line325)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line323*Line325)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line323*Line325)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line323*Line325)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line323*Line325)","v":""}]
[328,"Total SEM Interterm","L324*L326",{"$f":"IF(ISBLANK(RR),\"\",Line324*Line326)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line324*Line326)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line324*Line326)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line324*Line326)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line324*Line326)","v":""}]
[329,"VC-Intraterm-SEM-OPR","L315*L327",{"$f":"IF(ISBLANK(RR),\"\",Line315*Line327)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line315*Line327)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line315*Line327)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line315*Line327)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line315*Line327)","v":""},{"$f":"SUM(D160:H160)","v":0}]
[330,"VC-Intraterm-SEM-DRL","L317*L327",{"$f":"IF(ISBLANK(RR),\"\",Line317*Line327)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line317*Line327)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line317*Line327)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line317*Line327)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line317*Line327)","v":""},0]
[331,"VC-Intraterm-SEM-ROI","L319*L327",{"$f":"IF(ISBLANK(RR),\"\",Line319*Line327)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line319*Line327)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line319*Line327)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line319*Line327)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line319*Line327)","v":""},0]
[332,"VC-Interterm-SEM-OPR","L315*L328",{"$f":"IF(ISBLANK(RR),\"\",Line315*Line328)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line315*Line328)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line315*Line328)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line315*Line328)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line315*Line328)","v":""},0]
[333,"VC-Interterm-SEM-DRL","L317*L328",{"$f":"IF(ISBLANK(RR),\"\",Line317*Line328)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line317*Line328)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line317*Line328)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line317*Line328)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line317*Line328)","v":""},0]
[334,"VC-Interterm-SEM-ROI","L319*L328",{"$f":"IF(ISBLANK(RR),\"\",Line319*Line328)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line319*Line328)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line319*Line328)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line319*Line328)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line319*Line328)","v":""},0]
["HDR","Private Line Car Rentals","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[401,"Total car miles","L205",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,Line205))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,Line205))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,Line205))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,Line205))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,Line205))","v":""}]
[402,"Rental cost per car mile","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,D$3)),INDEX(User_L402,D$3),0)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,E$3)),INDEX(User_L402,E$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,F$3)),INDEX(User_L402,F$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,G$3)),INDEX(User_L402,G$3),0)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,H$3)),INDEX(User_L402,H$3),0)))","v":""}]
[403,"General overhead ratio","E2L219C1",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,D$3)),INDEX(User_OverheadRatio,D$3),VLOOKUP(RR&\"-\"&$C169,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":1.07001626723413},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,E$3)),INDEX(User_OverheadRatio,E$3),VLOOKUP(RR&\"-\"&$C169,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,F$3)),INDEX(User_OverheadRatio,F$3),VLOOKUP(RR&\"-\"&$C169,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,G$3)),INDEX(User_OverheadRatio,G$3),VLOOKUP(RR&\"-\"&$C169,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,H$3)),INDEX(User_OverheadRatio,H$3),VLOOKUP(RR&\"-\"&$C169,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C169&\"=\"&VLOOKUP($C169,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L219C1=General Overhead Ratio"}]
[404,"UC per CM-rental",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C13\"","v":"E1L206C13"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,D$3)),0,VLOOKUP(RR&\"-\"&$C170,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,E$3)),0,VLOOKUP(RR&\"-\"&$C170,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,F$3)),0,VLOOKUP(RR&\"-\"&$C170,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,G$3)),0,VLOOKUP(RR&\"-\"&$C170,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,H$3)),0,VLOOKUP(RR&\"-\"&$C170,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C170&\"=\"&VLOOKUP($C170,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C13=CM(R), DRL Expense, Privately-Owned, HOPPER - COVERED"}]
[405,"VC-CM-rental","if L402=0:L401*L404; else:L401*L402*L403",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,D$3)),Line401*Line402*Line403,Line401*Line404)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,E$3)),Line401*Line402*Line403,Line401*Line404)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,F$3)),Line401*Line402*Line403,Line401*Line404)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,G$3)),Line401*Line402*Line403,Line401*Line404)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",0,IF(ISNUMBER(INDEX(User_L402,H$3)),Line401*Line402*Line403,Line401*Line404)))","v":""},{"$f":"SUM(D171:H171)","v":0}]
["HDR","Railroad Owned Cars - Mileage Costs","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[406,"Total car miles","L205",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",Line205,0))","v":1976.92281083076},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",Line205,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",Line205,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",Line205,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN=\"Railroad\",Line205,0))","v":""}]
[407,"Actual charge per car mile","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,D$3)),INDEX(User_L407,D$3),0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,E$3)),INDEX(User_L407,E$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,F$3)),INDEX(User_L407,F$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,G$3)),INDEX(User_L407,G$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,H$3)),INDEX(User_L407,H$3),0))","v":""}]
[408,"General overhead ratio","E2L219C1",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,D$3)),INDEX(User_OverheadRatio,D$3),VLOOKUP(RR&\"-\"&$C175,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":1.07001626723413},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,E$3)),INDEX(User_OverheadRatio,E$3),VLOOKUP(RR&\"-\"&$C175,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,F$3)),INDEX(User_OverheadRatio,F$3),VLOOKUP(RR&\"-\"&$C175,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,G$3)),INDEX(User_OverheadRatio,G$3),VLOOKUP(RR&\"-\"&$C175,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_OverheadRatio,H$3)),INDEX(User_OverheadRatio,H$3),VLOOKUP(RR&\"-\"&$C175,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C175&\"=\"&VLOOKUP($C175,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L219C1=General Overhead Ratio"}]
[409,"VC-CM-Total","L406*L407*L408; L409 used only if L407 used",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,D$3)),Line406*Line407*Line408,0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,E$3)),Line406*Line407*Line408,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,F$3)),Line406*Line407*Line408,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,G$3)),Line406*Line407*Line408,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L407,H$3)),Line406*Line407*Line408,0))","v":""},{"$f":"SUM(D176:H176)","v":0}]
[410,"UC per CM(R)-OPR",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C1\"","v":"E1L206C1"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,D$3)),0,VLOOKUP(RR&\"-\"&$C177,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":3.3299107981417601E-2},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,E$3)),0,VLOOKUP(RR&\"-\"&$C177,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,F$3)),0,VLOOKUP(RR&\"-\"&$C177,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,G$3)),0,VLOOKUP(RR&\"-\"&$C177,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,H$3)),0,VLOOKUP(RR&\"-\"&$C177,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C177&\"=\"&VLOOKUP($C177,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C1=CM(R), OPR Expense, Railroad-Owned, HOPPER - COVERED"}]
[411,"VC-CM(R)-OPR","L406*L410",{"$f":"IF(ISBLANK(RR),\"\",Line406*Line410)","v":65.829766148781076},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line410)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line410)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line410)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line410)","v":""},{"$f":"SUM(D178:H178)","v":65.829766148781076}]
[412,"UC per CM(R)-DRL",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C2\"","v":"E1L206C2"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,D$3)),0,VLOOKUP(RR&\"-\"&$C179,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":-9.4949203518043801E-4},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,E$3)),0,VLOOKUP(RR&\"-\"&$C179,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,F$3)),0,VLOOKUP(RR&\"-\"&$C179,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,G$3)),0,VLOOKUP(RR&\"-\"&$C179,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,H$3)),0,VLOOKUP(RR&\"-\"&$C179,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C179&\"=\"&VLOOKUP($C179,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C2=CM(R), DRL Expense, Railroad-Owned, HOPPER - COVERED"}]
[413,"VC-CM(R)-DRL","L406*L412",{"$f":"IF(ISBLANK(RR),\"\",Line406*Line412)","v":-1.8770724630503304},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line412)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line412)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line412)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line412)","v":""},{"$f":"SUM(D180:H180)","v":-1.8770724630503304}]
[414,"UC per CM(R)-ROI",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C3\"","v":"E1L206C3"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,D$3)),0,VLOOKUP(RR&\"-\"&$C181,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":2.3750125261897698E-2},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,E$3)),0,VLOOKUP(RR&\"-\"&$C181,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,F$3)),0,VLOOKUP(RR&\"-\"&$C181,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,G$3)),0,VLOOKUP(RR&\"-\"&$C181,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,H$3)),0,VLOOKUP(RR&\"-\"&$C181,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C181&\"=\"&VLOOKUP($C181,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C3=CM(R), ROI Expense, Railroad-Owned, HOPPER - COVERED"}]
[415,"VC-CM(R)-ROI","L406*L414",{"$f":"IF(ISBLANK(RR),\"\",Line406*Line414)","v":46.952164390333436},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line414)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line414)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line414)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line414)","v":""},{"$f":"SUM(D182:H182)","v":46.952164390333436}]
[416,"Industry switch event (L&E)","L305",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line305))","v":4},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line305))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line305))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line305))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line305))","v":""}]
[417,"Interchange swt event (L&E)","L308",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line308))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line308))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line308))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line308))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line308))","v":""}]
[418,"I&I train swt event (L&E)","L310",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line310))","v":9.8846140541538006},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line310))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line310))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line310))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,Line310))","v":""}]
[419,"CM(Y)/Industry switch (L-E)",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C17\"","v":"E2L106C17"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L419,D$3)),INDEX(User_L419,D$3),AdjustL419*VLOOKUP(RR&\"-\"&$C186,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":4},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L419,E$3)),INDEX(User_L419,E$3),AdjustL419*VLOOKUP(RR&\"-\"&$C186,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L419,F$3)),INDEX(User_L419,F$3),AdjustL419*VLOOKUP(RR&\"-\"&$C186,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L419,G$3)),INDEX(User_L419,G$3),AdjustL419*VLOOKUP(RR&\"-\"&$C186,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L419,H$3)),INDEX(User_L419,H$3),AdjustL419*VLOOKUP(RR&\"-\"&$C186,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},null,{"$f":"$C186&\"=\"&VLOOKUP($C186,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C17=CM per Industry Switch, HOPPER - COVERED"}]
[420,"CM(Y)/Interchange switch (L-E)",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C18\"","v":"E2L106C18"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L420,D$3)),INDEX(User_L420,D$3),AdjustL420*VLOOKUP(RR&\"-\"&$C187,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":2.75},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L420,E$3)),INDEX(User_L420,E$3),AdjustL420*VLOOKUP(RR&\"-\"&$C187,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L420,F$3)),INDEX(User_L420,F$3),AdjustL420*VLOOKUP(RR&\"-\"&$C187,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L420,G$3)),INDEX(User_L420,G$3),AdjustL420*VLOOKUP(RR&\"-\"&$C187,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L420,H$3)),INDEX(User_L420,H$3),AdjustL420*VLOOKUP(RR&\"-\"&$C187,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},null,{"$f":"$C187&\"=\"&VLOOKUP($C187,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C18=CM per Interchange Switch, HOPPER - COVERED"}]
[421,"CM(Y)/I&I train switch (L-E)",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C21\"","v":"E2L106C21"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L421,D$3)),INDEX(User_L421,D$3),AdjustL421*VLOOKUP(RR&\"-\"&$C188,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L421,E$3)),INDEX(User_L421,E$3),AdjustL421*VLOOKUP(RR&\"-\"&$C188,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L421,F$3)),INDEX(User_L421,F$3),AdjustL421*VLOOKUP(RR&\"-\"&$C188,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L421,G$3)),INDEX(User_L421,G$3),AdjustL421*VLOOKUP(RR&\"-\"&$C188,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L421,H$3)),INDEX(User_L421,H$3),AdjustL421*VLOOKUP(RR&\"-\"&$C188,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},null,{"$f":"$C188&\"=\"&VLOOKUP($C188,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C21=CM per I&I Switch, HOPPER - COVERED"}]
[422,"CM(Y)-Industry","L416*L419",{"$f":"IF(ISBLANK(RR),\"\",Line416*Line419)","v":16},{"$f":"IF(ISBLANK(RR),\"\",Line416*Line419)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line416*Line419)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line416*Line419)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line416*Line419)","v":""}]
[423,"CM(Y)-Interchange","L417*L420",{"$f":"IF(ISBLANK(RR),\"\",Line417*Line420)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line417*Line420)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line417*Line420)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line417*Line420)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line417*Line420)","v":""}]
[424,"CM(Y)-I&I train","L418*L421",{"$f":"IF(ISBLANK(RR),\"\",Line418*Line421)","v":9.8846140541538006},{"$f":"IF(ISBLANK(RR),\"\",Line418*Line421)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line418*Line421)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line418*Line421)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line418*Line421)","v":""}]
[425,"CM(Y)-Total","L422+L423+L424",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line422+Line423+Line424)))","v":25.884614054153801},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line422+Line423+Line424)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line422+Line423+Line424)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line422+Line423+Line424)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,Line422+Line423+Line424)))","v":""}]
[426,"UC per CM(Y)-OPR",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C4\"","v":"E1L206C4"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,D$3)),0,VLOOKUP(RR&\"-\"&$C193,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":8.6577680751685995E-2},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,E$3)),0,VLOOKUP(RR&\"-\"&$C193,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,F$3)),0,VLOOKUP(RR&\"-\"&$C193,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,G$3)),0,VLOOKUP(RR&\"-\"&$C193,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,H$3)),0,VLOOKUP(RR&\"-\"&$C193,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C193&\"=\"&VLOOKUP($C193,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C4=CM(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED"}]
[427,"VC-CM(Y)-OPR","L425*L426",{"$f":"IF(ISBLANK(RR),\"\",Line425*Line426)","v":2.2410298519611325},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line426)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line426)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line426)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line426)","v":""},{"$f":"SUM(D194:H194)","v":2.2410298519611325}]
[428,"UC per CM(Y)-DRL",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C5\"","v":"E1L206C5"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,D$3)),0,VLOOKUP(RR&\"-\"&$C195,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":-2.4686792914691098E-3},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,E$3)),0,VLOOKUP(RR&\"-\"&$C195,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,F$3)),0,VLOOKUP(RR&\"-\"&$C195,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,G$3)),0,VLOOKUP(RR&\"-\"&$C195,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,H$3)),0,VLOOKUP(RR&\"-\"&$C195,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C195&\"=\"&VLOOKUP($C195,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C5=CM(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED"}]
[429,"VC-CM(Y)-DRL","L425*L428",{"$f":"IF(ISBLANK(RR),\"\",Line425*Line428)","v":-6.3900810683159767E-2},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line428)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line428)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line428)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line428)","v":""},{"$f":"SUM(D196:H196)","v":-6.3900810683159767E-2}]
[430,"UC per CM(Y)-ROI",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C6\"","v":"E1L206C6"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,D$3)),0,VLOOKUP(RR&\"-\"&$C197,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":6.1750325680933901E-2},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,E$3)),0,VLOOKUP(RR&\"-\"&$C197,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,F$3)),0,VLOOKUP(RR&\"-\"&$C197,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,G$3)),0,VLOOKUP(RR&\"-\"&$C197,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L407,H$3)),0,VLOOKUP(RR&\"-\"&$C197,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C197&\"=\"&VLOOKUP($C197,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C6=CM(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED"}]
[431,"VC-CM(Y)-ROI","L425*L430",{"$f":"IF(ISBLANK(RR),\"\",Line425*Line430)","v":1.5983833479692759},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line430)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line430)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line430)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line425*Line430)","v":""},{"$f":"SUM(D198:H198)","v":1.5983833479692759}]
["HDR","Railroad Owned Cars - Time Costs","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[432,"Actual charge per day","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,D$3)),INDEX(User_L432,D$3),0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,E$3)),INDEX(User_L432,E$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,F$3)),INDEX(User_L432,F$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,G$3)),INDEX(User_L432,G$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,H$3)),INDEX(User_L432,H$3),0))","v":""}]
[433,"Total car days","L436+L451",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,D$3)),Line436+Line451,0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,E$3)),Line436+Line451,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,F$3)),Line436+Line451,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,G$3)),Line436+Line451,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,H$3)),Line436+Line451,0))","v":""}]
[434,"VC-CD-Total","L408*L432*L433; L434 used only if L432 used",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,D$3)),Line408*Line432*Line433,0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,E$3)),Line408*Line432*Line433,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,F$3)),Line408*Line432*Line433,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,G$3)),Line408*Line432*Line433,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L432,H$3)),Line408*Line432*Line433,0))","v":""}]
[435,"Average CM(R)/CD(R)",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C22\"","v":"E2L106C22"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L435,D$3)),INDEX(User_L435,D$3),VLOOKUP(RR&\"-\"&$C203,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":473.48660392642898},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L435,E$3)),INDEX(User_L435,E$3),VLOOKUP(RR&\"-\"&$C203,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L435,F$3)),INDEX(User_L435,F$3),VLOOKUP(RR&\"-\"&$C203,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L435,G$3)),INDEX(User_L435,G$3),VLOOKUP(RR&\"-\"&$C203,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L435,H$3)),INDEX(User_L435,H$3),VLOOKUP(RR&\"-\"&$C203,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C203&\"=\"&VLOOKUP($C203,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C22=Average CM per CD, Railroad-Owned, HOPPER - COVERED"}]
[436,"Car days-running","L406/L435",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L436,D$3)),INDEX(User_L436,D$3),Line406/Line435)))","v":4.1752454967827077},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L436,E$3)),INDEX(User_L436,E$3),Line406/Line435)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L436,F$3)),INDEX(User_L436,F$3),Line406/Line435)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L436,G$3)),INDEX(User_L436,G$3),Line406/Line435)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L436,H$3)),INDEX(User_L436,H$3),Line406/Line435)))","v":""}]
[437,"UC per CD(R)-OPR",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C7\"","v":"E1L206C7"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,D$3)),0,VLOOKUP(RR&\"-\"&$C205,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":4.1926106668546304},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,E$3)),0,VLOOKUP(RR&\"-\"&$C205,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,F$3)),0,VLOOKUP(RR&\"-\"&$C205,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,G$3)),0,VLOOKUP(RR&\"-\"&$C205,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,H$3)),0,VLOOKUP(RR&\"-\"&$C205,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C205&\"=\"&VLOOKUP($C205,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C7=CD(R), OPR Expense, Railroad-Owned, HOPPER - COVERED"}]
[438,"VC-CD(R)-OPR","L436*L437",{"$f":"IF(ISBLANK(RR),\"\",Line436*Line437)","v":17.505178806547942},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line437)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line437)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line437)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line437)","v":""},{"$f":"SUM(D206:H206)","v":17.505178806547942}]
[439,"UC per CD(R)-DRL",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C8\"","v":"E1L206C8"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,D$3)),0,VLOOKUP(RR&\"-\"&$C207,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":4.1847974112718003},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,E$3)),0,VLOOKUP(RR&\"-\"&$C207,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,F$3)),0,VLOOKUP(RR&\"-\"&$C207,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,G$3)),0,VLOOKUP(RR&\"-\"&$C207,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,H$3)),0,VLOOKUP(RR&\"-\"&$C207,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C207&\"=\"&VLOOKUP($C207,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C8=CD(R), DRL Expense, Railroad-Owned, HOPPER - COVERED"}]
[440,"VC-CD(R)-DRL","L436*L439",{"$f":"IF(ISBLANK(RR),\"\",Line436*Line439)","v":17.472556546360519},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line439)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line439)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line439)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line439)","v":""},{"$f":"SUM(D208:H208)","v":17.472556546360519}]
[441,"UC per CD(R)-ROI",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C9\"","v":"E1L206C9"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,D$3)),0,VLOOKUP(RR&\"-\"&$C209,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":4.3929953638335997},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,E$3)),0,VLOOKUP(RR&\"-\"&$C209,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,F$3)),0,VLOOKUP(RR&\"-\"&$C209,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,G$3)),0,VLOOKUP(RR&\"-\"&$C209,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,H$3)),0,VLOOKUP(RR&\"-\"&$C209,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C209&\"=\"&VLOOKUP($C209,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C9=CD(R), ROI Expense, Railroad-Owned, HOPPER - COVERED"}]
[442,"VC-CD(R)-ROI","L436*L441",{"$f":"IF(ISBLANK(RR),\"\",Line436*Line441)","v":18.341834110233549},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line441)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line441)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line441)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line441)","v":""},{"$f":"SUM(D210:H210)","v":18.341834110233549}]
[443,"CD(Y)/Industry switch (L or E)",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C9\"","v":"E2L106C9"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L443,D$3)),INDEX(User_L443,D$3),AdjustL443*VLOOKUP(RR&\"-\"&$C211,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L443,E$3)),INDEX(User_L443,E$3),AdjustL443*VLOOKUP(RR&\"-\"&$C211,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L443,F$3)),INDEX(User_L443,F$3),AdjustL443*VLOOKUP(RR&\"-\"&$C211,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L443,G$3)),INDEX(User_L443,G$3),AdjustL443*VLOOKUP(RR&\"-\"&$C211,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L443,H$3)),INDEX(User_L443,H$3),AdjustL443*VLOOKUP(RR&\"-\"&$C211,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},null,{"$f":"$C211&\"=\"&VLOOKUP($C211,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C9=CD per Industry Switch, HOPPER - COVERED"}]
[444,"CD(Y)/Interchange swt (L or E)",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C10\"","v":"E2L106C10"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L444,D$3)),INDEX(User_L444,D$3),AdjustL444*VLOOKUP(RR&\"-\"&$C212,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":0.5},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L444,E$3)),INDEX(User_L444,E$3),AdjustL444*VLOOKUP(RR&\"-\"&$C212,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L444,F$3)),INDEX(User_L444,F$3),AdjustL444*VLOOKUP(RR&\"-\"&$C212,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L444,G$3)),INDEX(User_L444,G$3),AdjustL444*VLOOKUP(RR&\"-\"&$C212,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L444,H$3)),INDEX(User_L444,H$3),AdjustL444*VLOOKUP(RR&\"-\"&$C212,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},null,{"$f":"$C212&\"=\"&VLOOKUP($C212,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C10=CD per Interchange Switch, HOPPER - COVERED"}]
[445,"CD(Y)/I&I train switch (L or E)",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C13\"","v":"E2L106C13"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L445,D$3)),INDEX(User_L445,D$3),AdjustL445*VLOOKUP(RR&\"-\"&$C213,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":0.5},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L445,E$3)),INDEX(User_L445,E$3),AdjustL445*VLOOKUP(RR&\"-\"&$C213,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L445,F$3)),INDEX(User_L445,F$3),AdjustL445*VLOOKUP(RR&\"-\"&$C213,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L445,G$3)),INDEX(User_L445,G$3),AdjustL445*VLOOKUP(RR&\"-\"&$C213,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L445,H$3)),INDEX(User_L445,H$3),AdjustL445*VLOOKUP(RR&\"-\"&$C213,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},null,{"$f":"$C213&\"=\"&VLOOKUP($C213,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C13=CD per I&I Switch, HOPPER - COVERED"}]
[446,"CD(Y)-Industry(L&E)","L416*L443",{"$f":"IF(ISBLANK(RR),\"\",Line416*Line443)","v":4},{"$f":"IF(ISBLANK(RR),\"\",Line416*Line443)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line416*Line443)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line416*Line443)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line416*Line443)","v":""}]
[447,"CD(Y)-Interchange(L&E)","L417*L444",{"$f":"IF(ISBLANK(RR),\"\",Line417*Line444)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line417*Line444)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line417*Line444)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line417*Line444)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line417*Line444)","v":""}]
[448,"CD(Y)-I&I train(L&E)","L418*L445",{"$f":"IF(ISBLANK(RR),\"\",Line418*Line445)","v":4.9423070270769003},{"$f":"IF(ISBLANK(RR),\"\",Line418*Line445)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line418*Line445)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line418*Line445)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line418*Line445)","v":""}]
[449,"CD(Y)-per Loading & Unloading for Industry switch",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C14\"","v":"E2L106C14"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L449,D$3)),INDEX(User_L449,D$3),AdjustL449*VLOOKUP(RR&\"-\"&$C217,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":2},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L449,E$3)),INDEX(User_L449,E$3),AdjustL449*VLOOKUP(RR&\"-\"&$C217,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L449,F$3)),INDEX(User_L449,F$3),AdjustL449*VLOOKUP(RR&\"-\"&$C217,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L449,G$3)),INDEX(User_L449,G$3),AdjustL449*VLOOKUP(RR&\"-\"&$C217,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(ISNUMBER(INDEX(User_L449,H$3)),INDEX(User_L449,H$3),AdjustL449*VLOOKUP(RR&\"-\"&$C217,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))))","v":""},null,{"$f":"$C217&\"=\"&VLOOKUP($C217,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C14=CD per Load & Unload Industry Switch, HOPPER - COVERED"}]
[450,"CD(Y)-L&UL","L252*L449; TOFC:L251*L449",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(SZ<>\"Intermodal\",Line252*Line449,Line251*Line449)))","v":4},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(SZ<>\"Intermodal\",Line252*Line449,Line251*Line449)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(SZ<>\"Intermodal\",Line252*Line449,Line251*Line449)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(SZ<>\"Intermodal\",Line252*Line449,Line251*Line449)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SG=\"IA\",SG=\"IR\"),0,IF(SZ<>\"Intermodal\",Line252*Line449,Line251*Line449)))","v":""}]
[451,"CD(Y) Total","L446+L447+L448+L450",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(INDEX(User_L451,D$3)),INDEX(User_L451,D$3),Line446+Line447+Line448+Line450)))","v":12.9423070270769},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(INDEX(User_L451,E$3)),INDEX(User_L451,E$3),Line446+Line447+Line448+Line450)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(INDEX(User_L451,F$3)),INDEX(User_L451,F$3),Line446+Line447+Line448+Line450)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(INDEX(User_L451,G$3)),INDEX(User_L451,G$3),Line446+Line447+Line448+Line450)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,IF(ISNUMBER(INDEX(User_L451,H$3)),INDEX(User_L451,H$3),Line446+Line447+Line448+Line450)))","v":""}]
[452,"UC per CD(Y)-OPR",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C10\"","v":"E1L206C10"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,D$3)),0,VLOOKUP(RR&\"-\"&$C220,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":4.1926106668546304},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,E$3)),0,VLOOKUP(RR&\"-\"&$C220,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,F$3)),0,VLOOKUP(RR&\"-\"&$C220,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,G$3)),0,VLOOKUP(RR&\"-\"&$C220,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,H$3)),0,VLOOKUP(RR&\"-\"&$C220,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C220&\"=\"&VLOOKUP($C220,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C10=CD(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED"}]
[453,"VC-CD(Y)-OPR","L451*L452",{"$f":"IF(ISBLANK(RR),\"\",Line451*Line452)","v":54.262054495430249},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line452)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line452)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line452)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line452)","v":""},{"$f":"SUM(D221:H221)","v":54.262054495430249}]
[454,"UC per CD(Y)-DRL",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C11\"","v":"E1L206C11"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,D$3)),0,VLOOKUP(RR&\"-\"&$C222,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":4.1847974112718003},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,E$3)),0,VLOOKUP(RR&\"-\"&$C222,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,F$3)),0,VLOOKUP(RR&\"-\"&$C222,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,G$3)),0,VLOOKUP(RR&\"-\"&$C222,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,H$3)),0,VLOOKUP(RR&\"-\"&$C222,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C222&\"=\"&VLOOKUP($C222,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C11=CD(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED"}]
[455,"VC-CD(Y)-DRL","L451*L454",{"$f":"IF(ISBLANK(RR),\"\",Line451*Line454)","v":54.160932942796244},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line454)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line454)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line454)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line454)","v":""},{"$f":"SUM(D223:H223)","v":54.160932942796244}]
[456,"UC per CD(Y)-ROI",{"$f":"\"E1L2\"&TEXT(CarIndex,\"00\")&\"C12\"","v":"E1L206C12"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,D$3)),0,VLOOKUP(RR&\"-\"&$C224,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":4.3929953638335997},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,E$3)),0,VLOOKUP(RR&\"-\"&$C224,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,F$3)),0,VLOOKUP(RR&\"-\"&$C224,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,G$3)),0,VLOOKUP(RR&\"-\"&$C224,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(ISNUMBER(INDEX(User_L432,H$3)),0,VLOOKUP(RR&\"-\"&$C224,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C224&\"=\"&VLOOKUP($C224,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L206C12=CD(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED"}]
[457,"VC-CD(Y)-ROI","L451*L456",{"$f":"IF(ISBLANK(RR),\"\",Line451*Line456)","v":56.855494767259842},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line456)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line456)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line456)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line451*Line456)","v":""},{"$f":"SUM(D225:H225)","v":56.855494767259842}]
["HDR","Railroad Owned Cars - Accessorial Services","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[458,"UC per CM(R)-OPR","E1L219C1",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C227,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C227,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C227,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C227,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C227,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C227&\"=\"&VLOOKUP($C227,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C1=CM(R), OPR Expense, Railroad-Owned, ACCESSORIAL"}]
[459,"VC-CM(R)-OPR","L406*L458",{"$f":"IF(ISBLANK(RR),\"\",Line406*Line458)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line458)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line458)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line458)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line458)","v":""},{"$f":"SUM(D228:H228)","v":0}]
[460,"UC per CM(R)-DRL","E1L219C2",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C229,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":8.4837359774947495E-4},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C229,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C229,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C229,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C229,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C229&\"=\"&VLOOKUP($C229,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C2=CM(R), DRL Expense, Railroad-Owned, ACCESSORIAL"}]
[461,"VC-CM(R)-DRL","L406*L460",{"$f":"IF(ISBLANK(RR),\"\",Line406*Line460)","v":1.6771691174974965},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line460)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line460)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line460)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line460)","v":""},{"$f":"SUM(D230:H230)","v":1.6771691174974965}]
[462,"UC per CM(R)-ROI","E1L219C3",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C231,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":9.1879146870481895E-4},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C231,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C231,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C231,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C231,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C231&\"=\"&VLOOKUP($C231,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C3=CM(R), ROI Expense, Railroad-Owned, ACCESSORIAL"}]
[463,"VC-CM(R)-ROI","L406*L462",{"$f":"IF(ISBLANK(RR),\"\",Line406*Line462)","v":1.816379812879253},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line462)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line462)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line462)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line406*Line462)","v":""},{"$f":"SUM(D232:H232)","v":1.816379812879253}]
[464,"UC per CM(Y)-OPR","E1L219C4",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C233,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C233,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C233,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C233,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C233,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C233&\"=\"&VLOOKUP($C233,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C4=CM(Y), OPR Expense, Railroad-Owned, ACCESSORIAL"}]
[465,"VC-CM(Y)-OPR","L425*L464; if IA:L484*L464; if IR:L485*L464",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line464,IF(SG=\"IA\",Line484*Line464,Line485*Line464)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line464,IF(SG=\"IA\",Line484*Line464,Line485*Line464)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line464,IF(SG=\"IA\",Line484*Line464,Line485*Line464)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line464,IF(SG=\"IA\",Line484*Line464,Line485*Line464)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line464,IF(SG=\"IA\",Line484*Line464,Line485*Line464)))","v":""},{"$f":"SUM(D234:H234)","v":0}]
[466,"UC per CM(Y)-DRL","E1L219C5",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C235,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":2.2057713541486302E-3},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C235,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C235,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C235,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C235,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C235&\"=\"&VLOOKUP($C235,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C5=CM(Y), DRL Expense, Railroad-Owned, ACCESSORIAL"}]
[467,"VC-CM(Y)-DRL","L425*L466; if IA:L484*L466; if IR:L485*L466",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line466,IF(SG=\"IA\",Line484*Line466,Line485*Line466)))","v":5.7095540193845495E-2},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line466,IF(SG=\"IA\",Line484*Line466,Line485*Line466)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line466,IF(SG=\"IA\",Line484*Line466,Line485*Line466)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line466,IF(SG=\"IA\",Line484*Line466,Line485*Line466)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line466,IF(SG=\"IA\",Line484*Line466,Line485*Line466)))","v":""},{"$f":"SUM(D236:H236)","v":5.7095540193845495E-2}]
[468,"UC per CM(Y)-ROI","E1L219C6",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C237,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":2.3888578186325301E-3},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C237,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C237,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C237,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C237,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C237&\"=\"&VLOOKUP($C237,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C6=CM(Y), ROI Expense, Railroad-Owned, ACCESSORIAL"}]
[469,"VC-CM(Y)-ROI","L425*L468; if IA:L484*L468; if IR:L485*L468",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line468,IF(SG=\"IA\",Line484*Line468,Line485*Line468)))","v":6.183466266555078E-2},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line468,IF(SG=\"IA\",Line484*Line468,Line485*Line468)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line468,IF(SG=\"IA\",Line484*Line468,Line485*Line468)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line468,IF(SG=\"IA\",Line484*Line468,Line485*Line468)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line425*Line468,IF(SG=\"IA\",Line484*Line468,Line485*Line468)))","v":""},{"$f":"SUM(D238:H238)","v":6.183466266555078E-2}]
[470,"UC per CD(R)-OPR","E1L219C7",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C239,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C239,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C239,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C239,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C239,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C239&\"=\"&VLOOKUP($C239,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C7=CD(R), OPR Expense, Railroad-Owned, ACCESSORIAL"}]
[471,"VC-CD(R)-OPR","L436*L470",{"$f":"IF(ISBLANK(RR),\"\",Line436*Line470)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line470)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line470)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line470)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line470)","v":""},{"$f":"SUM(D240:H240)","v":0}]
[472,"UC per CD(R)-DRL","E1L219C8",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C241,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0.14149790856257899},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C241,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C241,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C241,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C241,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C241&\"=\"&VLOOKUP($C241,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C8=CD(R), DRL Expense, Railroad-Owned, ACCESSORIAL"}]
[473,"VC-CD(R)-DRL","L436*L472",{"$f":"IF(ISBLANK(RR),\"\",Line436*Line472)","v":0.59078850553007922},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line472)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line472)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line472)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line472)","v":""},{"$f":"SUM(D242:H242)","v":0.59078850553007922}]
[474,"UC per CD(R)-ROI","E1L219C9",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C243,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0.15188159942736401},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C243,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C243,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C243,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C243,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C243&\"=\"&VLOOKUP($C243,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C9=CD(R), ROI Expense, Railroad-Owned, ACCESSORIAL"}]
[475,"VC-CD(R)-ROI","L436*L474",{"$f":"IF(ISBLANK(RR),\"\",Line436*Line474)","v":0.63414296405325665},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line474)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line474)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line474)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line436*Line474)","v":""},{"$f":"SUM(D244:H244)","v":0.63414296405325665}]
[476,"UC per CD(Y)-OPR","E1L219C10",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C245,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C245,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C245,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C245,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C245,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C245&\"=\"&VLOOKUP($C245,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C10=CD(Y), OPR Expense, Railroad-Owned, ACCESSORIAL"}]
[477,"VC-CD(Y)-OPR","L451*L476; if IA:L496*L476; if IR:L497*L476",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line476,IF(SG=\"IA\",Line496*Line476,Line497*Line476)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line476,IF(SG=\"IA\",Line496*Line476,Line497*Line476)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line476,IF(SG=\"IA\",Line496*Line476,Line497*Line476)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line476,IF(SG=\"IA\",Line496*Line476,Line497*Line476)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line476,IF(SG=\"IA\",Line496*Line476,Line497*Line476)))","v":""},{"$f":"SUM(D246:H246)","v":0}]
[478,"UC per CD(Y)-DRL","E1L219C11",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C247,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0.14149790856257899},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C247,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C247,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C247,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C247,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C247&\"=\"&VLOOKUP($C247,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C11=CD(Y), DRL Expense, Railroad-Owned, ACCESSORIAL"}]
[479,"VC-CD(Y)-DRL","L451*L478; if IA:L496*L478; if IR:L497*L478",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line478,IF(SG=\"IA\",Line496*Line478,Line497*Line478)))","v":1.8313093763061508},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line478,IF(SG=\"IA\",Line496*Line478,Line497*Line478)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line478,IF(SG=\"IA\",Line496*Line478,Line497*Line478)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line478,IF(SG=\"IA\",Line496*Line478,Line497*Line478)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line478,IF(SG=\"IA\",Line496*Line478,Line497*Line478)))","v":""},{"$f":"SUM(D248:H248)","v":1.8313093763061508}]
[480,"UC per CD(Y)-ROI","E1L219C12",{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C249,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0.15188159942736401},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C249,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C249,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C249,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(User_Accessorial_Flag=\"N\",0,VLOOKUP(RR&\"-\"&$C249,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},null,{"$f":"$C249&\"=\"&VLOOKUP($C249,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L219C12=CD(Y), ROI Expense, Railroad-Owned, ACCESSORIAL"}]
[481,"VC-CD(Y)-ROI","L451*L480; if IA:L496*L480; if IR:L497*L480",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line480,IF(SG=\"IA\",Line496*Line480,Line497*Line480)))","v":1.9656982915524521},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line480,IF(SG=\"IA\",Line496*Line480,Line497*Line480)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line480,IF(SG=\"IA\",Line496*Line480,Line497*Line480)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line480,IF(SG=\"IA\",Line496*Line480,Line497*Line480)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SG<>\"IA\",SG<>\"IR\"),Line451*Line480,IF(SG=\"IA\",Line496*Line480,Line497*Line480)))","v":""},{"$f":"SUM(D250:H250)","v":1.9656982915524521}]
["HDR","Railroad Owned Cars - Intra & Interterminal Switching","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[482,"CM(Y) per Intraterminal event",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C19\"","v":"E2L106C19"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L482,D$3)),INDEX(User_L482,D$3),VLOOKUP(RR&\"-\"&$C252,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L482,E$3)),INDEX(User_L482,E$3),VLOOKUP(RR&\"-\"&$C252,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L482,F$3)),INDEX(User_L482,F$3),VLOOKUP(RR&\"-\"&$C252,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L482,G$3)),INDEX(User_L482,G$3),VLOOKUP(RR&\"-\"&$C252,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L482,H$3)),INDEX(User_L482,H$3),VLOOKUP(RR&\"-\"&$C252,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},null,{"$f":"$C252&\"=\"&VLOOKUP($C252,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C19=CM per Intraterminal Switch, HOPPER - COVERED"}]
[483,"CM(Y) per Interterminal event",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C20\"","v":"E2L106C20"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L483,D$3)),INDEX(User_L483,D$3),VLOOKUP(RR&\"-\"&$C253,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L483,E$3)),INDEX(User_L483,E$3),VLOOKUP(RR&\"-\"&$C253,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L483,F$3)),INDEX(User_L483,F$3),VLOOKUP(RR&\"-\"&$C253,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L483,G$3)),INDEX(User_L483,G$3),VLOOKUP(RR&\"-\"&$C253,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L483,H$3)),INDEX(User_L483,H$3),VLOOKUP(RR&\"-\"&$C253,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},null,{"$f":"$C253&\"=\"&VLOOKUP($C253,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C20=CM per Interterminal Switch, HOPPER - COVERED"}]
[484,"Total CM(Y) Intraterminal","L323*L482",{"$f":"IF(ISBLANK(RR),\"\",Line323*Line482)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line323*Line482)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line323*Line482)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line323*Line482)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line323*Line482)","v":""}]
[485,"Total CM(Y) Interterminal","L324*L483",{"$f":"IF(ISBLANK(RR),\"\",Line324*Line483)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line324*Line483)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line324*Line483)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line324*Line483)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line324*Line483)","v":""}]
[486,"VC-Intraterm-CM(Y)-OPR","L426*L484",{"$f":"IF(ISBLANK(RR),\"\",Line426*Line484)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line426*Line484)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line426*Line484)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line426*Line484)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line426*Line484)","v":""},{"$f":"SUM(D256:H256)","v":0}]
[487,"VC-Intraterm-CM(Y)-DRL","L428*L484",{"$f":"IF(ISBLANK(RR),\"\",Line428*Line484)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line428*Line484)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line428*Line484)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line428*Line484)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line428*Line484)","v":""},0]
[488,"VC-Intraterm-CM(Y)-ROI","L430*L484",{"$f":"IF(ISBLANK(RR),\"\",Line430*Line484)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line430*Line484)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line430*Line484)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line430*Line484)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line430*Line484)","v":""},0]
[489,"VC-Interterm-CM(Y)-OPR","L426*L485",{"$f":"IF(ISBLANK(RR),\"\",Line426*Line485)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line426*Line485)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line426*Line485)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line426*Line485)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line426*Line485)","v":""},0]
[490,"VC-Interterm-CM(Y)-DRL","L428*L485",{"$f":"IF(ISBLANK(RR),\"\",Line428*Line485)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line428*Line485)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line428*Line485)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line428*Line485)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line428*Line485)","v":""},0]
[491,"VC-Interterm-CM(Y)-ROI","L430*L485",{"$f":"IF(ISBLANK(RR),\"\",Line430*Line485)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line430*Line485)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line430*Line485)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line430*Line485)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line430*Line485)","v":""},0]
[492,"CD(Y) per Intraterminal switch",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C11\"","v":"E2L106C11"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L492,D$3)),INDEX(User_L492,D$3),VLOOKUP(RR&\"-\"&$C262,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L492,E$3)),INDEX(User_L492,E$3),VLOOKUP(RR&\"-\"&$C262,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L492,F$3)),INDEX(User_L492,F$3),VLOOKUP(RR&\"-\"&$C262,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L492,G$3)),INDEX(User_L492,G$3),VLOOKUP(RR&\"-\"&$C262,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L492,H$3)),INDEX(User_L492,H$3),VLOOKUP(RR&\"-\"&$C262,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},null,{"$f":"$C262&\"=\"&VLOOKUP($C262,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C11=CD per Intraterminal Switch, HOPPER - COVERED"}]
[493,"CD(Y)-L&UL-Intraterminal",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C15\"","v":"E2L106C15"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L493,D$3)),INDEX(User_L493,D$3),VLOOKUP(RR&\"-\"&$C263,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L493,E$3)),INDEX(User_L493,E$3),VLOOKUP(RR&\"-\"&$C263,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L493,F$3)),INDEX(User_L493,F$3),VLOOKUP(RR&\"-\"&$C263,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L493,G$3)),INDEX(User_L493,G$3),VLOOKUP(RR&\"-\"&$C263,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IA\",0,IF(ISNUMBER(INDEX(User_L493,H$3)),INDEX(User_L493,H$3),VLOOKUP(RR&\"-\"&$C263,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},null,{"$f":"$C263&\"=\"&VLOOKUP($C263,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C15=CD per Load & Unload Intraterminal Switch, HOPPER - COVERED"}]
[494,"CD(Y) per Interterminal switch",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C12\"","v":"E2L106C12"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L494,D$3)),INDEX(User_L494,D$3),VLOOKUP(RR&\"-\"&$C264,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L494,E$3)),INDEX(User_L494,E$3),VLOOKUP(RR&\"-\"&$C264,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L494,F$3)),INDEX(User_L494,F$3),VLOOKUP(RR&\"-\"&$C264,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L494,G$3)),INDEX(User_L494,G$3),VLOOKUP(RR&\"-\"&$C264,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L494,H$3)),INDEX(User_L494,H$3),VLOOKUP(RR&\"-\"&$C264,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},null,{"$f":"$C264&\"=\"&VLOOKUP($C264,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C12=CD per Interterminal Switch, HOPPER - COVERED"}]
[495,"CD(Y)-L&UL-Interterminal",{"$f":"\"E2L1\"&TEXT(CarIndex,\"00\")&\"C16\"","v":"E2L106C16"},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L495,D$3)),INDEX(User_L495,D$3),VLOOKUP(RR&\"-\"&$C265,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L495,E$3)),INDEX(User_L495,E$3),VLOOKUP(RR&\"-\"&$C265,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L495,F$3)),INDEX(User_L495,F$3),VLOOKUP(RR&\"-\"&$C265,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L495,G$3)),INDEX(User_L495,G$3),VLOOKUP(RR&\"-\"&$C265,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OWN<>\"Railroad\",0,IF(SG<>\"IR\",0,IF(ISNUMBER(INDEX(User_L495,H$3)),INDEX(User_L495,H$3),VLOOKUP(RR&\"-\"&$C265,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))))","v":""},null,{"$f":"$C265&\"=\"&VLOOKUP($C265,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L106C16=CD per Load & Unload Interterminal Switch, HOPPER - COVERED"}]
[496,"Total CD(Y) Intraterminal","(L323*L492)+(L321*L493)",{"$f":"IF(ISBLANK(RR),\"\",(Line323*Line492)+(Line321*Line493))","v":0},{"$f":"IF(ISBLANK(RR),\"\",(Line323*Line492)+(Line321*Line493))","v":""},{"$f":"IF(ISBLANK(RR),\"\",(Line323*Line492)+(Line321*Line493))","v":""},{"$f":"IF(ISBLANK(RR),\"\",(Line323*Line492)+(Line321*Line493))","v":""},{"$f":"IF(ISBLANK(RR),\"\",(Line323*Line492)+(Line321*Line493))","v":""}]
[497,"Total CD(Y) Interterminal","(L324*L494)+(L322*L495)",{"$f":"IF(ISBLANK(RR),\"\",(Line324*Line494)+(Line322*Line495))","v":0},{"$f":"IF(ISBLANK(RR),\"\",(Line324*Line494)+(Line322*Line495))","v":""},{"$f":"IF(ISBLANK(RR),\"\",(Line324*Line494)+(Line322*Line495))","v":""},{"$f":"IF(ISBLANK(RR),\"\",(Line324*Line494)+(Line322*Line495))","v":""},{"$f":"IF(ISBLANK(RR),\"\",(Line324*Line494)+(Line322*Line495))","v":""}]
[498,"VC-Intraterm-CD(Y)-OPR","L452*L496",{"$f":"IF(ISBLANK(RR),\"\",Line452*Line496)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line452*Line496)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line452*Line496)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line452*Line496)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line452*Line496)","v":""},{"$f":"SUM(D268:H268)","v":0}]
[499,"VC-Intraterm-CD(Y)-DRL","L454*L496",{"$f":"IF(ISBLANK(RR),\"\",Line454*Line496)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line454*Line496)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line454*Line496)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line454*Line496)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line454*Line496)","v":""},0]
["499A","VC-Intraterm-CD(Y)-ROI","L456*L496",{"$f":"IF(ISBLANK(RR),\"\",Line456*Line496)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line456*Line496)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line456*Line496)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line456*Line496)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line456*Line496)","v":""},0]
["499B","VC-Interterm-CD(Y)-OPR","L452*L497",{"$f":"IF(ISBLANK(RR),\"\",Line452*Line497)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line452*Line497)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line452*Line497)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line452*Line497)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line452*Line497)","v":""},0]
["499C","VC-Interterm-CD(Y)-DRL","L454*L497",{"$f":"IF(ISBLANK(RR),\"\",Line454*Line497)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line454*Line497)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line454*Line497)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line454*Line497)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line454*Line497)","v":""},0]
["499D","VC-Interterm-CD(Y)-ROI","L456*L497",{"$f":"IF(ISBLANK(RR),\"\",Line456*Line497)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line456*Line497)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line456*Line497)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line456*Line497)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line456*Line497)","v":""},0]
["HDR","Lake Transfer Services","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[501,"Lake transfer ton miles","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L501,D$3)),INDEX(User_L501,D$3),0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L501,E$3)),INDEX(User_L501,E$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L501,F$3)),INDEX(User_L501,F$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L501,G$3)),INDEX(User_L501,G$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L501,H$3)),INDEX(User_L501,H$3),0))","v":""}]
[502,"UC per TM Lake-OPR","E1L112C1",{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C276,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C276,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C276,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C276,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C276,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C276&\"=\"&VLOOKUP($C276,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L112C1=Ton Miles In Lake Transfer Service, OPR Expense"}]
[503,"VC-TM Lake-OPR","L501*L502",{"$f":"IF(ISBLANK(RR),\"\",Line501*Line502)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line502)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line502)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line502)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line502)","v":""},{"$f":"SUM(D277:H277)","v":0}]
[504,"UC per TM Lake-DRL","E1L112C2",{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C278,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C278,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C278,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C278,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C278,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C278&\"=\"&VLOOKUP($C278,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L112C2=Ton Miles In Lake Transfer Service, DRL Expense"}]
[505,"VC-TM Lake-DRL","L501*L504",{"$f":"IF(ISBLANK(RR),\"\",Line501*Line504)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line504)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line504)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line504)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line504)","v":""},{"$f":"SUM(D279:H279)","v":0}]
[506,"UC per TM Lake-ROI","E1L112C3",{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C280,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C280,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C280,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C280,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line501=0,0,VLOOKUP(RR&\"-\"&$C280,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C280&\"=\"&VLOOKUP($C280,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L112C3=Ton Miles In Lake Transfer Service, ROI Expense"}]
[507,"VC-TM Lake-ROI","L501*L506",{"$f":"IF(ISBLANK(RR),\"\",Line501*Line506)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line506)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line506)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line506)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line501*Line506)","v":""},{"$f":"SUM(D281:H281)","v":0}]
["HDR","Coal Terminals","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[508,"Coal terminal tons","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L508,D$3)),INDEX(User_L508,D$3),0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L508,E$3)),INDEX(User_L508,E$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L508,F$3)),INDEX(User_L508,F$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L508,G$3)),INDEX(User_L508,G$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L508,H$3)),INDEX(User_L508,H$3),0))","v":""}]
[509,"UC per Ton Coal-OPR","E1L113C1",{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C284,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C284,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C284,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C284,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C284,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C284&\"=\"&VLOOKUP($C284,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L113C1=Tons Handled at Coal Terminals, OPR Expense"}]
[510,"VC-Ton Coal-OPR","L508*L509",{"$f":"IF(ISBLANK(RR),\"\",Line508*Line509)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line509)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line509)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line509)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line509)","v":""},{"$f":"SUM(D285:H285)","v":0}]
[511,"UC per Ton coal-DRL","E1L113C2",{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C286,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C286,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C286,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C286,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C286,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C286&\"=\"&VLOOKUP($C286,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L113C2=Tons Handled at Coal Terminals, DRL Expense"}]
[512,"VC-Ton Coal-DRL","L508*L511",{"$f":"IF(ISBLANK(RR),\"\",Line508*Line511)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line511)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line511)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line511)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line511)","v":""},{"$f":"SUM(D287:H287)","v":0}]
[513,"UC per Ton Coal-ROI","E1L113C3",{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C288,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C288,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C288,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C288,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line508=0,0,VLOOKUP(RR&\"-\"&$C288,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C288&\"=\"&VLOOKUP($C288,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L113C3=Tons Handled at Coal Terminals, ROI Expense"}]
[514,"VC-Ton Coal-ROI","L508*L513",{"$f":"IF(ISBLANK(RR),\"\",Line508*Line513)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line513)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line513)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line513)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line508*Line513)","v":""},{"$f":"SUM(D289:H289)","v":0}]
["HDR","Ore Terminals","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[515,"Ore terminal tons","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L515,D$3)),INDEX(User_L515,D$3),0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L515,E$3)),INDEX(User_L515,E$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L515,F$3)),INDEX(User_L515,F$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L515,G$3)),INDEX(User_L515,G$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L515,H$3)),INDEX(User_L515,H$3),0))","v":""}]
[516,"UC per Ton Ore-OPR","E1L114C1",{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C292,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C292,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C292,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C292,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C292,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C292&\"=\"&VLOOKUP($C292,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L114C1=Tons Handled at Ore Terminals, OPR Expense"}]
[517,"VC-Ton Ore-OPR","L515*L516",{"$f":"IF(ISBLANK(RR),\"\",Line515*Line516)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line516)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line516)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line516)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line516)","v":""},{"$f":"SUM(D293:H293)","v":0}]
[518,"UC per Ton Ore-DRL","E1L114C2",{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C294,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C294,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C294,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C294,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C294,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C294&\"=\"&VLOOKUP($C294,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L114C2=Tons Handled at Ore Terminals, DRL Expense"}]
[519,"VC-Ton Ore-DRL","L515*L518",{"$f":"IF(ISBLANK(RR),\"\",Line515*Line518)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line518)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line518)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line518)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line518)","v":""},{"$f":"SUM(D295:H295)","v":0}]
[520,"UC per Ton Ore-ROI","E1L114C3",{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C296,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C296,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C296,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C296,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line515=0,0,VLOOKUP(RR&\"-\"&$C296,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C296&\"=\"&VLOOKUP($C296,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L114C3=Tons Handled at Ore Terminals, ROI Expense"}]
[521,"VC-Ton Ore-ROI","L515*L520",{"$f":"IF(ISBLANK(RR),\"\",Line515*Line520)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line520)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line520)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line520)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line515*Line520)","v":""},{"$f":"SUM(D297:H297)","v":0}]
["HDR","Other Marine Terminals","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[522,"Marine terminal tons","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L522,D$3)),INDEX(User_L522,D$3),0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L522,E$3)),INDEX(User_L522,E$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L522,F$3)),INDEX(User_L522,F$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L522,G$3)),INDEX(User_L522,G$3),0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(ISNUMBER(INDEX(User_L522,H$3)),INDEX(User_L522,H$3),0))","v":""}]
[523,"UC per Ton Marine-OPR","E1L115C1",{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C300,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C300,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C300,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C300,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C300,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C300&\"=\"&VLOOKUP($C300,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L115C1=Tons Handled at Other Marine Terminals, OPR Expense"}]
[524,"VC-Ton Marine-OPR","L522*L523",{"$f":"IF(ISBLANK(RR),\"\",Line522*Line523)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line523)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line523)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line523)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line523)","v":""},{"$f":"SUM(D301:H301)","v":0}]
[525,"UC per Ton Marine-DRL","E1L115C2",{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C302,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C302,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C302,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C302,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C302,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C302&\"=\"&VLOOKUP($C302,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L115C2=Tons Handled at Other Marine Terminals, DRL Expense"}]
[526,"VC-Ton Marine-DRL","L522*L525",{"$f":"IF(ISBLANK(RR),\"\",Line522*Line525)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line525)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line525)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line525)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line525)","v":""},{"$f":"SUM(D303:H303)","v":0}]
[527,"UC per Ton Marine-ROI","E1L115C3",{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C304,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C304,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C304,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C304,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line522=0,0,VLOOKUP(RR&\"-\"&$C304,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C304&\"=\"&VLOOKUP($C304,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L115C3=Tons Handled at Other Marine Terminals, ROI Expense"}]
[528,"VC-Ton Marine-ROI","L522*L527",{"$f":"IF(ISBLANK(RR),\"\",Line522*Line527)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line527)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line527)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line527)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line522*Line527)","v":""},{"$f":"SUM(D305:H305)","v":0}]
["HDR","Motor Vehicle Units Loaded and Unloaded","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[529,"MVUs handled","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex<>12,0,IF(ISNUMBER(User_MVUs),User_MVUs*Line250,(WT/2)*NC*Line250)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex<>12,0,IF(ISNUMBER(User_MVUs),User_MVUs*Line250,(WT/2)*NC*Line250)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex<>12,0,IF(ISNUMBER(User_MVUs),User_MVUs*Line250,(WT/2)*NC*Line250)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex<>12,0,IF(ISNUMBER(User_MVUs),User_MVUs*Line250,(WT/2)*NC*Line250)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex<>12,0,IF(ISNUMBER(User_MVUs),User_MVUs*Line250,(WT/2)*NC*Line250)))","v":""}]
[530,"UC per MVU","E1L121C1",{"$f":"IF(ISBLANK(RR),\"\",IF(Line529=0,0,VLOOKUP(RR&\"-\"&$C308,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line529=0,0,VLOOKUP(RR&\"-\"&$C308,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line529=0,0,VLOOKUP(RR&\"-\"&$C308,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line529=0,0,VLOOKUP(RR&\"-\"&$C308,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line529=0,0,VLOOKUP(RR&\"-\"&$C308,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C308&\"=\"&VLOOKUP($C308,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L121C1=MVUs Loaded And Unloaded (L&UL), OPR Expense"}]
[531,"VC-MVUs L&UL","L529*L530",{"$f":"IF(ISBLANK(RR),\"\",Line529*Line530)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line529*Line530)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line529*Line530)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line529*Line530)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line529*Line530)","v":""},{"$f":"SUM(D309:H309)","v":0}]
["HDR","Refrigerated Car Protective Service","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[532,"Loaded car miles","L103*L201",{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex=9,Line103*Line201,0))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex=9,Line103*Line201,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex=9,Line103*Line201,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex=9,Line103*Line201,0))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(CarIndex=9,Line103*Line201,0))","v":""}]
[533,"UC per car mile","E1L116C1",{"$f":"IF(ISBLANK(RR),\"\",IF(Line532=0,0,VLOOKUP(RR&\"-\"&$C312,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(Line532=0,0,VLOOKUP(RR&\"-\"&$C312,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line532=0,0,VLOOKUP(RR&\"-\"&$C312,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line532=0,0,VLOOKUP(RR&\"-\"&$C312,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(Line532=0,0,VLOOKUP(RR&\"-\"&$C312,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C312&\"=\"&VLOOKUP($C312,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L116C1=Refrigerated Car Miles, OPR Expense"}]
[534,"VC-Refer-Protect","L532*L533",{"$f":"IF(ISBLANK(RR),\"\",Line532*Line533)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line532*Line533)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line532*Line533)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line532*Line533)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line532*Line533)","v":""},{"$f":"SUM(D313:H313)","v":0}]
["HDR","Loss And Damage Claim Payments","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[535,"Weight of shipment (tons)","L217",{"$f":"IF(ISBLANK(RR),\"\",Line217)","v":80},{"$f":"IF(ISBLANK(RR),\"\",Line217)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line217)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line217)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line217)","v":""}]
[536,"UC per ton",{"$f":"\"E1L3\"&TEXT(CommodIndex,\"00\")&\"C1\"","v":"E1L302C1"},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C316,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1.6986060104260001E-2},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C316,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C316,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C316,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C316,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C316&\"=\"&VLOOKUP($C316,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L302C1=L&D Expense, GRAIN"}]
[537,"Loss & damage claim expense","(% of total miles)*L535*L536",{"$f":"IF(ISBLANK(RR),\"\",(DIS/TotalDistance)*Line535*Line536)","v":1.3588848083408001},{"$f":"IF(ISBLANK(RR),\"\",(DIS/TotalDistance)*Line535*Line536)","v":""},{"$f":"IF(ISBLANK(RR),\"\",(DIS/TotalDistance)*Line535*Line536)","v":""},{"$f":"IF(ISBLANK(RR),\"\",(DIS/TotalDistance)*Line535*Line536)","v":""},{"$f":"IF(ISBLANK(RR),\"\",(DIS/TotalDistance)*Line535*Line536)","v":""},{"$f":"SUM(D317:H317)","v":1.3588848083408001}]
["HDR","TCU's Loading and Unloading (Tie and Untie)","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[540,"TCUs in shipment","L203",{"$f":"IF(ISBLANK(RR),\"\",Line203)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line203)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line203)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line203)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line203)","v":""}]
[541,"Total TCUs loaded & unloaded","L540*L250",{"$f":"IF(ISBLANK(RR),\"\",Line540*Line250)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line540*Line250)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line540*Line250)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line540*Line250)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line540*Line250)","v":""}]
[542,"UC per TCU L&UL-OPR","E1L120C1",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C321,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C321,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C321,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C321,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C321,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C321&\"=\"&VLOOKUP($C321,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L120C1=TCUs Loaded And Unloaded (L&UL), OPR Expense"}]
[543,"VC-TCU L&UL-OPR","L541*L542",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line542))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line542))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line542))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line542))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line542))","v":""},{"$f":"SUM(D322:H322)","v":0}]
[544,"UC per TCU L&UL-DRL","E1L120C2",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C323,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C323,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C323,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C323,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C323,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C323&\"=\"&VLOOKUP($C323,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L120C2=TCUs Loaded And Unloaded (L&UL), DRL Expense"}]
[545,"VC-TCU L&UL-DRL","L541*L544",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line544))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line544))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line544))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line544))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line544))","v":""},{"$f":"SUM(D324:H324)","v":0}]
[546,"UC per TCU L&UL-ROI","E1L120C3",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C325,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C325,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C325,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C325,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C325,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C325&\"=\"&VLOOKUP($C325,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L120C3=TCUs Loaded And Unloaded (L&UL), ROI Expense"}]
[547,"VC-TCU L&UL-ROI","L541*L546",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line546))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line546))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line546))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line546))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,Line541*Line546))","v":""},{"$f":"SUM(D326:H326)","v":0}]
["HDR","TCU Ownership and Protective Service","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[548,"Line haul mileage","L103*L203*L215",{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line215)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line215)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line215)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line215)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103*Line203*Line215)","v":""}]
[549,"Line haul TCU days","L548/E2L205C1",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line548/IF(ISNUMBER(User_TCULineHaulMiles),User_TCULineHaulMiles,TCULineHaulMilesDefault)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line548/IF(ISNUMBER(User_TCULineHaulMiles),User_TCULineHaulMiles,TCULineHaulMilesDefault)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line548/IF(ISNUMBER(User_TCULineHaulMiles),User_TCULineHaulMiles,TCULineHaulMilesDefault)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line548/IF(ISNUMBER(User_TCULineHaulMiles),User_TCULineHaulMiles,TCULineHaulMilesDefault)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,Line548/IF(ISNUMBER(User_TCULineHaulMiles),User_TCULineHaulMiles,TCULineHaulMilesDefault)))","v":""},null,{"$f":"RIGHT($C329,8)&\"=\"&VLOOKUP(RIGHT($C329,8),ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L205C1=Linehaul Miles Per TCU Day"}]
[550,"Days origin/destination per TCU","E2L206C1",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUDays),User_TCUDays,TCUDaysDefault)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUDays),User_TCUDays,TCUDaysDefault)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUDays),User_TCUDays,TCUDaysDefault)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUDays),User_TCUDays,TCUDaysDefault)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISNUMBER(User_TCUDays),User_TCUDays,TCUDaysDefault)))","v":""},null,{"$f":"$C330&\"=\"&VLOOKUP($C330,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L206C1=TCU Days Per Orig Or Term Event"}]
[551,"Total TCU days O&T","L203*L250*L550",{"$f":"IF(ISBLANK(RR),\"\",Line203*Line250*Line550)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line203*Line250*Line550)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line203*Line250*Line550)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line203*Line250*Line550)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line203*Line250*Line550)","v":""}]
[552,"Total TCU days","L549+L551",{"$f":"IF(ISBLANK(RR),\"\",Line549+Line551)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line549+Line551)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line549+Line551)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line549+Line551)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line549+Line551)","v":""}]
[553,"UC Ref TCU day-OPR","E1L118C1",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C333,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C333,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C333,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C333,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C333,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C333&\"=\"&VLOOKUP($C333,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L118C1=Refrigerated TCU Days, OPR Expense"}]
[554,"VC-Ref TCU-OPR","L552*L553",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line553)","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line553)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line553)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line553)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line553)","v":""},{"$f":"SUM(D334:H334)","v":0}]
[555,"UC Ref TCU day-DRL","E1L118C2",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C335,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C335,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C335,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C335,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C335,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C335&\"=\"&VLOOKUP($C335,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L118C2=Refrigerated TCU Days, DRL Expense"}]
[556,"VC-Ref TCU-DRL","L552*L555",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line555)","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line555)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line555)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line555)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line555)","v":""},{"$f":"SUM(D336:H336)","v":0}]
[557,"UC Ref TCU day-ROI","E1L118C3",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C337,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C337,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C337,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C337,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C337,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C337&\"=\"&VLOOKUP($C337,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L118C3=Refrigerated TCU Days, ROI Expense"}]
[558,"VC-Ref TCU-ROI","L552*L557",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line557)","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line557)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line557)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line557)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line557)","v":""},{"$f":"SUM(D338:H338)","v":0}]
[559,"UC Ref TCU-Protect-OPR","E1L117C1",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C339,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C339,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C339,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C339,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag<>\"Y\"),0,VLOOKUP(RR&\"-\"&$C339,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C339&\"=\"&VLOOKUP($C339,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L117C1=Protective Service Reefer TCU Days, OPR Expense"}]
[560,"VC-Ref TCU-Protect-OPR","L552*L559",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line559)","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line559)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line559)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line559)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line559)","v":""},{"$f":"SUM(D340:H340)","v":0}]
[561,"UC TCU Non-Ref-OPR","E1L119C1",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C341,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C341,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C341,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C341,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C341,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C341&\"=\"&VLOOKUP($C341,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L119C1=Other (Non-Refrigerated) TCU Days, OPR Expense"}]
[562,"VC-TCU Non-Ref-OPR","L552*L561",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line561)","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line561)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line561)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line561)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line561)","v":""},{"$f":"SUM(D342:H342)","v":0}]
[563,"UC TCU Non-Ref-DRL","E1L119C2",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C343,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C343,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C343,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C343,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C343,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C343&\"=\"&VLOOKUP($C343,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L119C2=Other (Non-Refrigerated) TCU Days, DRL Expense"}]
[564,"VC-TCU Non-Ref-DRL","L552*L563",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line563)","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line563)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line563)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line563)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line563)","v":""},{"$f":"SUM(D344:H344)","v":0}]
[565,"UC TCU Non-Ref-ROI","E1L119C3",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C345,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C345,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C345,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C345,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ<>\"Intermodal\",User_TCURefrigFlag=\"Y\"),0,VLOOKUP(RR&\"-\"&$C345,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C345&\"=\"&VLOOKUP($C345,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L119C3=Other (Non-Refrigerated) TCU Days, ROI Expense"}]
[566,"VC-TCU Non-Ref-ROI","L552*L565",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line565)","v":0},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line565)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line565)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line565)","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(Line569,URCSTOFCPlans,MATCH(\"O&PS\",URCSTOFCPlansHeaders,0),FALSE)*Line552*Line565)","v":""},{"$f":"SUM(D346:H346)","v":0}]
["HDR","TCU Pickup and Delivery","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[569,"Intermodal Plan","[User]",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISBLANK(User_TOFCPlanCode),TOFCPlanCodeDefault,IF(ISNUMBER(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCPlans,1,FALSE),IF(ISTEXT(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCServiceCodes,3,FALSE))))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISBLANK(User_TOFCPlanCode),TOFCPlanCodeDefault,IF(ISNUMBER(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCPlans,1,FALSE),IF(ISTEXT(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCServiceCodes,3,FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISBLANK(User_TOFCPlanCode),TOFCPlanCodeDefault,IF(ISNUMBER(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCPlans,1,FALSE),IF(ISTEXT(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCServiceCodes,3,FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISBLANK(User_TOFCPlanCode),TOFCPlanCodeDefault,IF(ISNUMBER(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCPlans,1,FALSE),IF(ISTEXT(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCServiceCodes,3,FALSE))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,IF(ISBLANK(User_TOFCPlanCode),TOFCPlanCodeDefault,IF(ISNUMBER(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCPlans,1,FALSE),IF(ISTEXT(User_TOFCPlanCode),VLOOKUP(User_TOFCPlanCode,URCSTOFCServiceCodes,3,FALSE))))))","v":""}]
[570,"TCUs given P&D service","L203*L250",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(Line569,URCSTOFCPlans,MATCH(SG,URCSTOFCPlansHeaders,0),FALSE)*Line203*Line250))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(Line569,URCSTOFCPlans,MATCH(SG,URCSTOFCPlansHeaders,0),FALSE)*Line203*Line250))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(Line569,URCSTOFCPlans,MATCH(SG,URCSTOFCPlansHeaders,0),FALSE)*Line203*Line250))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(Line569,URCSTOFCPlans,MATCH(SG,URCSTOFCPlansHeaders,0),FALSE)*Line203*Line250))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(Line569,URCSTOFCPlans,MATCH(SG,URCSTOFCPlansHeaders,0),FALSE)*Line203*Line250))","v":""}]
[571,"UC TCU given P&D-OPR","E1L122C1",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C350,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C350,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C350,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C350,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Intermodal\",0,VLOOKUP(RR&\"-\"&$C350,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C350&\"=\"&VLOOKUP($C350,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E1L122C1=TCUs Picked Up and Delivered (PU&D), OPR Expense"}]
[572,"VC-TCU P&D-OPR","L570*L571",{"$f":"IF(ISBLANK(RR),\"\",Line570*Line571)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line570*Line571)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line570*Line571)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line570*Line571)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line570*Line571)","v":""}]
["HDR","Jurisdictional Add-On's: Single Car Movements","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[573,"Industry switch events","L305",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line305))))","v":4},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line305))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line305))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line305))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line305))))","v":""}]
[574,"Indus switch residual",{"$f":"IF(OWN=\"Railroad\",\"E2L301C1\",\"E2L301C2\")","v":"E2L301C1"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L301C2\",$C354),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":63.484170813081398},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L301C2\",$C354),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L301C2\",$C354),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L301C2\",$C354),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L301C2\",$C354),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C354&\"=\"&VLOOKUP($C354,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L301C1=Residual Factor, Industry Switching, Operating and Equipment"}]
[575,"Indus Switch add-on","L573*L574",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line573*Line574))","v":253.93668325232559},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line573*Line574))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line573*Line574))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line573*Line574))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line573*Line574))","v":""},{"$f":"SUM(D355:H355)","v":253.93668325232559}]
[576,"Carloads originated & terminated","L252",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line252))","v":2},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line252))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line252))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line252))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line252))","v":""}]
[577,"Station clerical resid",{"$f":"IF(OWN=\"Railroad\",\"E2L302C1\",\"E2L302C2\")","v":"E2L302C1"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L302C2\",$C357),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":36.997398464518703},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L302C2\",$C357),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L302C2\",$C357),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L302C2\",$C357),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L302C2\",$C357),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C357&\"=\"&VLOOKUP($C357,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L302C1=Residual Factor, Station Clerical, Operating and Equipment"}]
[578,"CLOT add-on","L576*L577",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line576*Line577))","v":73.994796929037406},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line576*Line577))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line576*Line577))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line576*Line577))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Multi\",SZ=\"Unit\",SZ=\"Intermodal\"),0,Line576*Line577))","v":""},{"$f":"SUM(D358:H358)","v":73.994796929037406}]
["HDR","Jurisdictional Add-On's: Single & Multiple Car Movements","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[579,"Carloads interchanged","L308",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line308))))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line308))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line308))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line308))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,IF(SG=\"IA\",Line323,IF(SG=\"IR\",Line324,Line308))))","v":""}]
[580,"Inter switch resid",{"$f":"IF(OWN=\"Railroad\",\"E2L303C1\",\"E2L303C2\")","v":"E2L303C1"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L303C2\",$C361),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":12.490785127130099},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L303C2\",$C361),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L303C2\",$C361),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L303C2\",$C361),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&IF(OR(SG=\"IA\",SG=\"IR\"),\"E2L303C2\",$C361),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C361&\"=\"&VLOOKUP($C361,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L303C1=Residual Factor, Interchange Switching, Operating and Equipment"}]
[581,"Inter Switch add-on","L579*L580",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line579*Line580))","v":0},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line579*Line580))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line579*Line580))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line579*Line580))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line579*Line580))","v":""},{"$f":"SUM(D362:H362)","v":0}]
[582,"Freight car miles","L205",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line205))","v":1976.92281083076},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line205))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line205))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line205))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,Line205))","v":""}]
[583,"I&I switching residual",{"$f":"IF(OWN=\"Railroad\",\"E2L304C1\",\"E2L304C2\")","v":"E2L304C1"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C364,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":69.741114160925804},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C364,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C364,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C364,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C364,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C364&\"=\"&VLOOKUP($C364,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L304C1=Residual Factor, I&I Switching, Operating and Equipment"}]
[584,"I&I Switching add-on","(L582/1000)*L583",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line583))","v":137.87279943748635},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line583))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line583))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line583))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line583))","v":""},{"$f":"SUM(D365:H365)","v":137.87279943748635}]
[585,"Mileage residual",{"$f":"IF(OWN=\"Railroad\",\"E2L305C1\",\"E2L305C2\")","v":"E2L305C1"},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C366,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":-1.48193672253884},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C366,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C366,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C366,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,VLOOKUP(RR&\"-\"&$C366,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},null,{"$f":"$C366&\"=\"&VLOOKUP($C366,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L305C1=Residual Factor, Mileage, Operating and Equipment"}]
[586,"Car-Mile add-on","(L582/1000)*L585",{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line585))","v":-2.9296745109948077},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line585))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line585))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line585))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(OR(SZ=\"Unit\",SZ=\"Intermodal\"),0,(Line582/1000)*Line585))","v":""},{"$f":"SUM(D367:H367)","v":-2.9296745109948077}]
[587,"Total jurisdictional add-on","L575+L578+L581+L584+L586",{"$f":"IF(ISBLANK(RR),\"\",IF(User_JurisdictionalAddOns=\"N\",0,Line575+Line578+Line581+Line584+Line586))","v":462.87460510785456},{"$f":"IF(ISBLANK(RR),\"\",IF(User_JurisdictionalAddOns=\"N\",0,Line575+Line578+Line581+Line584+Line586))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_JurisdictionalAddOns=\"N\",0,Line575+Line578+Line581+Line584+Line586))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_JurisdictionalAddOns=\"N\",0,Line575+Line578+Line581+Line584+Line586))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_JurisdictionalAddOns=\"N\",0,Line575+Line578+Line581+Line584+Line586))","v":""},462.87460510785456]
["HDR","Summary of Shipment Costs","Source",{"$f":"IF(ISBLANK(RR),\"\",RR)","v":"WEST"},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"IF(ISBLANK(RR),\"\",RR)","v":""},{"$f":"I$4","v":"Total"}]
[601,"Car mile-Other than clerical-OPR","L207",{"$f":"IF(ISBLANK(RR),\"\",Line207)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line207)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line207)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line207)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line207)","v":""},{"$f":"SUM(D370:H370)","v":0}]
[602,"Car mile-Other than clerical-DRL","L209",{"$f":"IF(ISBLANK(RR),\"\",Line209)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line209)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line209)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line209)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line209)","v":""},0]
[603,"Car mile-Other than clerical-ROI","L211",{"$f":"IF(ISBLANK(RR),\"\",Line211)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line211)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line211)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line211)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line211)","v":""},0]
[604,"Gross ton mile-OPR","L221",{"$f":"IF(ISBLANK(RR),\"\",Line221)","v":327.58079849965094},{"$f":"IF(ISBLANK(RR),\"\",Line221)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line221)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line221)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line221)","v":""},327.58079849965094]
[605,"Gross ton mile-DRL","L223",{"$f":"IF(ISBLANK(RR),\"\",Line223)","v":145.3898232913277},{"$f":"IF(ISBLANK(RR),\"\",Line223)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line223)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line223)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line223)","v":""},145.3898232913277]
[606,"Gross ton mile-ROI","L225",{"$f":"IF(ISBLANK(RR),\"\",Line225)","v":300.76294216706026},{"$f":"IF(ISBLANK(RR),\"\",Line225)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line225)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line225)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line225)","v":""},300.76294216706026]
[607,"Locomotive unit mile-OPR","L244",{"$f":"IF(ISBLANK(RR),\"\",Line244)","v":302.13888072546132},{"$f":"IF(ISBLANK(RR),\"\",Line244)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line244)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line244)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line244)","v":""},302.13888072546132]
[608,"Locomotive unit mile-DRL","L246",{"$f":"IF(ISBLANK(RR),\"\",Line246)","v":53.381176729159279},{"$f":"IF(ISBLANK(RR),\"\",Line246)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line246)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line246)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line246)","v":""},53.381176729159279]
[609,"Locomotive unit mile-ROI","L248",{"$f":"IF(ISBLANK(RR),\"\",Line248)","v":51.796452911686728},{"$f":"IF(ISBLANK(RR),\"\",Line248)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line248)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line248)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line248)","v":""},51.796452911686728]
[610,"Car mile-Clerical-OPR","L256",{"$f":"IF(ISBLANK(RR),\"\",Line256)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line256)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line256)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line256)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line256)","v":""},0]
[611,"CLOT-Clerical-OPR","L258",{"$f":"IF(ISBLANK(RR),\"\",Line258)","v":13.85667178274484},{"$f":"IF(ISBLANK(RR),\"\",Line258)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line258)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line258)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line258)","v":""},13.85667178274484]
[612,"CLOR-Clerical-OPR","L260",{"$f":"IF(ISBLANK(RR),\"\",Line260)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line260)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line260)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line260)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line260)","v":""},0]
[613,"CLOT-Other than clerical-OPR","L262",{"$f":"IF(ISBLANK(RR),\"\",Line262)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line262)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line262)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line262)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line262)","v":""},0]
[614,"CLOR-Other than clerical-OPR","L264",{"$f":"IF(ISBLANK(RR),\"\",Line264)","v":1.6930165994223101},{"$f":"IF(ISBLANK(RR),\"\",Line264)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line264)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line264)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line264)","v":""},1.6930165994223101]
[615,"CLOR-Other than clerical-DRL","L266",{"$f":"IF(ISBLANK(RR),\"\",Line266)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line266)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line266)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line266)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line266)","v":""},0]
[616,"CLOR-Other than clerical-ROI","L268",{"$f":"IF(ISBLANK(RR),\"\",Line268)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line268)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line268)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line268)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line268)","v":""},0]
[617,"Train miles-Crew-Unit train-OPR","L281",{"$f":"IF(ISBLANK(RR),\"\",Line281)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line281)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line281)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line281)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line281)","v":""},0]
[618,"Train miles-Crew-Way train-OPR","L282",{"$f":"IF(ISBLANK(RR),\"\",Line282)","v":9.6357247626964337},{"$f":"IF(ISBLANK(RR),\"\",Line282)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line282)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line282)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line282)","v":""},9.6357247626964337]
[619,"Train miles-Crew-Thru train-OPR","L283",{"$f":"IF(ISBLANK(RR),\"\",Line283)","v":211.5922202836467},{"$f":"IF(ISBLANK(RR),\"\",Line283)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line283)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line283)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line283)","v":""},211.5922202836467]
[620,"Train miles-Other than crew-OPR","L286",{"$f":"IF(ISBLANK(RR),\"\",Line286)","v":12.401633833704235},{"$f":"IF(ISBLANK(RR),\"\",Line286)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line286)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line286)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line286)","v":""},12.401633833704235]
[621,"Train miles-Other than crew-DRL","L288",{"$f":"IF(ISBLANK(RR),\"\",Line288)","v":-6.6765325131692759E-3},{"$f":"IF(ISBLANK(RR),\"\",Line288)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line288)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line288)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line288)","v":""},-6.6765325131692759E-3]
[622,"Train miles-Other than crew-ROI","L290",{"$f":"IF(ISBLANK(RR),\"\",Line290)","v":3.4532368562444252E-2},{"$f":"IF(ISBLANK(RR),\"\",Line290)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line290)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line290)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line290)","v":""},3.4532368562444252E-2]
[623,"SEM Industry, Interchange & I&I-OPR","L316",{"$f":"IF(ISBLANK(RR),\"\",Line316)","v":169.01403426292833},{"$f":"IF(ISBLANK(RR),\"\",Line316)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line316)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line316)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line316)","v":""},169.01403426292833]
[624,"SEM Industry, Interchange & I&I-DRL","L318",{"$f":"IF(ISBLANK(RR),\"\",Line318)","v":46.47499014095704},{"$f":"IF(ISBLANK(RR),\"\",Line318)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line318)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line318)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line318)","v":""},46.47499014095704]
[625,"SEM Industry, Interchange & I&I-ROI","L320",{"$f":"IF(ISBLANK(RR),\"\",Line320)","v":140.99407565269809},{"$f":"IF(ISBLANK(RR),\"\",Line320)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line320)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line320)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line320)","v":""},140.99407565269809]
[626,"SEM Intraterminal-OPR","L329",{"$f":"IF(ISBLANK(RR),\"\",Line329)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line329)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line329)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line329)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line329)","v":""},0]
[627,"SEM Intraterminal-DRL","L330",{"$f":"IF(ISBLANK(RR),\"\",Line330)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line330)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line330)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line330)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line330)","v":""},0]
[628,"SEM Intraterminal-ROI","L331",{"$f":"IF(ISBLANK(RR),\"\",Line331)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line331)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line331)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line331)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line331)","v":""},0]
[629,"SEM Interterminal-OPR","L332",{"$f":"IF(ISBLANK(RR),\"\",Line332)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line332)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line332)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line332)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line332)","v":""},0]
[630,"SEM Interterminal-DRL","L333",{"$f":"IF(ISBLANK(RR),\"\",Line333)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line333)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line333)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line333)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line333)","v":""},0]
[631,"SEM Interterminal-ROI","L334",{"$f":"IF(ISBLANK(RR),\"\",Line334)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line334)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line334)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line334)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line334)","v":""},0]
[632,"CM-Private car rental-DRL","L405",{"$f":"IF(ISBLANK(RR),\"\",Line405)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line405)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line405)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line405)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line405)","v":""},0]
[633,"CM-Railroad owned car [User]","L409",{"$f":"IF(ISBLANK(RR),\"\",Line409)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line409)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line409)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line409)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line409)","v":""},0]
[634,"CM(R)-Railroad owned (URCS)-OPR","L411",{"$f":"IF(ISBLANK(RR),\"\",Line411)","v":65.829766148781076},{"$f":"IF(ISBLANK(RR),\"\",Line411)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line411)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line411)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line411)","v":""},65.829766148781076]
[635,"CM(R)-Railroad owned (URCS)-DRL","L413",{"$f":"IF(ISBLANK(RR),\"\",Line413)","v":-1.8770724630503304},{"$f":"IF(ISBLANK(RR),\"\",Line413)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line413)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line413)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line413)","v":""},-1.8770724630503304]
[636,"CM(R)-Railroad owned (URCS)-ROI","L415",{"$f":"IF(ISBLANK(RR),\"\",Line415)","v":46.952164390333436},{"$f":"IF(ISBLANK(RR),\"\",Line415)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line415)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line415)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line415)","v":""},46.952164390333436]
[637,"CM(Y)-Railroad owned (URCS)-OPR","L427",{"$f":"IF(ISBLANK(RR),\"\",Line427)","v":2.2410298519611325},{"$f":"IF(ISBLANK(RR),\"\",Line427)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line427)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line427)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line427)","v":""},2.2410298519611325]
[638,"CM(Y)-Railroad owned (URCS)-DRL","L429",{"$f":"IF(ISBLANK(RR),\"\",Line429)","v":-6.3900810683159767E-2},{"$f":"IF(ISBLANK(RR),\"\",Line429)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line429)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line429)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line429)","v":""},-6.3900810683159767E-2]
[639,"CM(Y)-Railroad owned (URCS)-ROI","L431",{"$f":"IF(ISBLANK(RR),\"\",Line431)","v":1.5983833479692759},{"$f":"IF(ISBLANK(RR),\"\",Line431)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line431)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line431)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line431)","v":""},1.5983833479692759]
[640,"CD-Railroad owned [User]","L434",{"$f":"IF(ISBLANK(RR),\"\",Line434)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line434)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line434)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line434)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line434)","v":""},0]
[641,"CD(R)-Railroad owned (URCS)-OPR","L438",{"$f":"IF(ISBLANK(RR),\"\",Line438)","v":17.505178806547942},{"$f":"IF(ISBLANK(RR),\"\",Line438)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line438)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line438)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line438)","v":""},17.505178806547942]
[642,"CD(R)-Railroad owned (URCS)-DRL","L440",{"$f":"IF(ISBLANK(RR),\"\",Line440)","v":17.472556546360519},{"$f":"IF(ISBLANK(RR),\"\",Line440)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line440)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line440)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line440)","v":""},17.472556546360519]
[643,"CD(R)-Railroad owned (URCS)-ROI","L442",{"$f":"IF(ISBLANK(RR),\"\",Line442)","v":18.341834110233549},{"$f":"IF(ISBLANK(RR),\"\",Line442)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line442)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line442)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line442)","v":""},18.341834110233549]
[644,"CD(Y)-Railroad owned (URCS)-OPR","L453",{"$f":"IF(ISBLANK(RR),\"\",Line453)","v":54.262054495430249},{"$f":"IF(ISBLANK(RR),\"\",Line453)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line453)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line453)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line453)","v":""},54.262054495430249]
[645,"CD(Y)-Railroad owned (URCS)-DRL","L455",{"$f":"IF(ISBLANK(RR),\"\",Line455)","v":54.160932942796244},{"$f":"IF(ISBLANK(RR),\"\",Line455)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line455)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line455)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line455)","v":""},54.160932942796244]
[646,"CD(Y)-Railroad owned (URCS)-ROI","L457",{"$f":"IF(ISBLANK(RR),\"\",Line457)","v":56.855494767259842},{"$f":"IF(ISBLANK(RR),\"\",Line457)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line457)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line457)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line457)","v":""},56.855494767259842]
[647,"CM(R)-Accessorial-OPR","L459",{"$f":"IF(ISBLANK(RR),\"\",Line459)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line459)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line459)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line459)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line459)","v":""},0]
[648,"CM(R)-Accessorial-DRL","L461",{"$f":"IF(ISBLANK(RR),\"\",Line461)","v":1.6771691174974965},{"$f":"IF(ISBLANK(RR),\"\",Line461)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line461)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line461)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line461)","v":""},1.6771691174974965]
[649,"CM(R)-Accessorial-ROI","L463",{"$f":"IF(ISBLANK(RR),\"\",Line463)","v":1.816379812879253},{"$f":"IF(ISBLANK(RR),\"\",Line463)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line463)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line463)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line463)","v":""},1.816379812879253]
[650,"CM(Y)-Accessorial-OPR","L465",{"$f":"IF(ISBLANK(RR),\"\",Line465)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line465)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line465)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line465)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line465)","v":""},0]
[651,"CM(Y)-Accessorial-DRL","L467",{"$f":"IF(ISBLANK(RR),\"\",Line467)","v":5.7095540193845495E-2},{"$f":"IF(ISBLANK(RR),\"\",Line467)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line467)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line467)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line467)","v":""},5.7095540193845495E-2]
[652,"CM(Y)-Accessorial-ROI","L469",{"$f":"IF(ISBLANK(RR),\"\",Line469)","v":6.183466266555078E-2},{"$f":"IF(ISBLANK(RR),\"\",Line469)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line469)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line469)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line469)","v":""},6.183466266555078E-2]
[653,"CD(R)-Accessorial-OPR","L471",{"$f":"IF(ISBLANK(RR),\"\",Line471)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line471)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line471)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line471)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line471)","v":""},0]
[654,"CD(R)-Accessorial-DRL","L473",{"$f":"IF(ISBLANK(RR),\"\",Line473)","v":0.59078850553007922},{"$f":"IF(ISBLANK(RR),\"\",Line473)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line473)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line473)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line473)","v":""},0.59078850553007922]
[655,"CD(R)-Accessorial-ROI","L475",{"$f":"IF(ISBLANK(RR),\"\",Line475)","v":0.63414296405325665},{"$f":"IF(ISBLANK(RR),\"\",Line475)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line475)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line475)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line475)","v":""},0.63414296405325665]
[656,"CD(Y)-Accessorial-OPR","L477",{"$f":"IF(ISBLANK(RR),\"\",Line477)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line477)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line477)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line477)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line477)","v":""},0]
[657,"CD(Y)-Accessorial-DRL","L479",{"$f":"IF(ISBLANK(RR),\"\",Line479)","v":1.8313093763061508},{"$f":"IF(ISBLANK(RR),\"\",Line479)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line479)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line479)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line479)","v":""},1.8313093763061508]
[658,"CD(Y)-Accessorial-ROI","L481",{"$f":"IF(ISBLANK(RR),\"\",Line481)","v":1.9656982915524521},{"$f":"IF(ISBLANK(RR),\"\",Line481)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line481)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line481)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line481)","v":""},1.9656982915524521]
[659,"CM(Y)-Intraterminal-OPR","L486",{"$f":"IF(ISBLANK(RR),\"\",Line486)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line486)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line486)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line486)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line486)","v":""},0]
[660,"CM(Y)-Intraterminal-DRL","L487",{"$f":"IF(ISBLANK(RR),\"\",Line487)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line487)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line487)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line487)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line487)","v":""},0]
[661,"CM(Y)-Intraterminal-ROI","L488",{"$f":"IF(ISBLANK(RR),\"\",Line488)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line488)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line488)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line488)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line488)","v":""},0]
[662,"CM(Y)-Interterminal-OPR","L489",{"$f":"IF(ISBLANK(RR),\"\",Line489)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line489)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line489)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line489)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line489)","v":""},0]
[663,"CM(Y)-Interterminal-DRL","L490",{"$f":"IF(ISBLANK(RR),\"\",Line490)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line490)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line490)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line490)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line490)","v":""},0]
[664,"CM(Y)-Interterminal-ROI","L491",{"$f":"IF(ISBLANK(RR),\"\",Line491)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line491)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line491)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line491)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line491)","v":""},0]
[665,"CD(Y)-Intraterminal-OPR","L498",{"$f":"IF(ISBLANK(RR),\"\",Line498)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line498)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line498)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line498)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line498)","v":""},{"$f":"SUM(D434:H434)","v":0}]
[666,"CD(Y)-Intraterminal-DRL","L499",{"$f":"IF(ISBLANK(RR),\"\",Line499)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line499)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499)","v":""},0]
[667,"CD(Y)-Intraterminal-ROI","L499A",{"$f":"IF(ISBLANK(RR),\"\",Line499A)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line499A)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499A)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499A)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499A)","v":""},0]
[668,"CD(Y)-Interterminal-OPR","L499B",{"$f":"IF(ISBLANK(RR),\"\",Line499B)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line499B)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499B)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499B)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499B)","v":""},0]
[669,"CD(Y)-Interterminal-DRL","L499C",{"$f":"IF(ISBLANK(RR),\"\",Line499C)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line499C)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499C)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499C)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499C)","v":""},0]
[670,"CD(Y)-Interterminal-ROI","L499D",{"$f":"IF(ISBLANK(RR),\"\",Line499D)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line499D)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499D)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499D)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line499D)","v":""},0]
[671,"Ton miles-Lake transfer service-OPR","L503",{"$f":"IF(ISBLANK(RR),\"\",Line503)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line503)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line503)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line503)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line503)","v":""},0]
[672,"Ton miles-Lake transfer service-DRL","L505",{"$f":"IF(ISBLANK(RR),\"\",Line505)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line505)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line505)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line505)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line505)","v":""},0]
[673,"Ton miles-Lake transfer service-ROI","L507",{"$f":"IF(ISBLANK(RR),\"\",Line507)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line507)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line507)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line507)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line507)","v":""},0]
[674,"Tons at Coal terminals-OPR","L510",{"$f":"IF(ISBLANK(RR),\"\",Line510)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line510)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line510)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line510)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line510)","v":""},0]
[675,"Tons at Coal terminals-DRL","L512",{"$f":"IF(ISBLANK(RR),\"\",Line512)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line512)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line512)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line512)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line512)","v":""},0]
[676,"Tons at Coal terminals-ROI","L514",{"$f":"IF(ISBLANK(RR),\"\",Line514)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line514)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line514)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line514)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line514)","v":""},0]
[677,"Tons at Ore terminal-OPR","L517",{"$f":"IF(ISBLANK(RR),\"\",Line517)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line517)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line517)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line517)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line517)","v":""},0]
[678,"Tons at Ore terminal-DRL","L519",{"$f":"IF(ISBLANK(RR),\"\",Line519)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line519)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line519)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line519)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line519)","v":""},0]
[679,"Tons at Ore terminal-ROI","L521",{"$f":"IF(ISBLANK(RR),\"\",Line521)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line521)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line521)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line521)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line521)","v":""},0]
[680,"Tons at Other marine terminals-OPR","L524",{"$f":"IF(ISBLANK(RR),\"\",Line524)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line524)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line524)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line524)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line524)","v":""},0]
[681,"Tons at Other marine terminals-DRL","L526",{"$f":"IF(ISBLANK(RR),\"\",Line526)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line526)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line526)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line526)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line526)","v":""},0]
[682,"Tons at Other marine terminals-ROI","L528",{"$f":"IF(ISBLANK(RR),\"\",Line528)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line528)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line528)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line528)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line528)","v":""},0]
[683,"MVUs Loaded & Unloaded-OPR","L531",{"$f":"IF(ISBLANK(RR),\"\",Line531)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line531)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line531)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line531)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line531)","v":""},0]
[684,"Refrigerated car miles-OPR","L534",{"$f":"IF(ISBLANK(RR),\"\",Line534)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line534)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line534)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line534)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line534)","v":""},0]
[685,"TCUs Loaded & Unloaded-OPR","L543",{"$f":"IF(ISBLANK(RR),\"\",Line543)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line543)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line543)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line543)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line543)","v":""},0]
[686,"TCUs Loaded & Unloaded-DRL","L545",{"$f":"IF(ISBLANK(RR),\"\",Line545)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line545)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line545)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line545)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line545)","v":""},0]
[687,"TCUs Loaded & Unloaded-ROI","L547",{"$f":"IF(ISBLANK(RR),\"\",Line547)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line547)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line547)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line547)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line547)","v":""},0]
[688,"TCU Protective service-OPR","L560",{"$f":"IF(ISBLANK(RR),\"\",Line560)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line560)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line560)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line560)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line560)","v":""},0]
[689,"Refrigerated TCU days-OPR","L554",{"$f":"IF(ISBLANK(RR),\"\",Line554)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line554)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line554)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line554)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line554)","v":""},0]
[690,"Refrigerated TCU days-DRL","L556",{"$f":"IF(ISBLANK(RR),\"\",Line556)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line556)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line556)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line556)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line556)","v":""},0]
[691,"Refrigerated TCU days-ROI","L558",{"$f":"IF(ISBLANK(RR),\"\",Line558)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line558)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line558)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line558)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line558)","v":""},0]
[692,"Non-Ref TCU days-OPR","L562",{"$f":"IF(ISBLANK(RR),\"\",Line562)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line562)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line562)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line562)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line562)","v":""},0]
[693,"Non-Ref TCU days-DRL","L564",{"$f":"IF(ISBLANK(RR),\"\",Line564)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line564)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line564)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line564)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line564)","v":""},0]
[694,"Non-Ref TCU days-ROI","L566",{"$f":"IF(ISBLANK(RR),\"\",Line566)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line566)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line566)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line566)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line566)","v":""},0]
[695,"TCU-Pickup & Delivery-OPR","L572",{"$f":"IF(ISBLANK(RR),\"\",Line572)","v":0},{"$f":"IF(ISBLANK(RR),\"\",Line572)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line572)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line572)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line572)","v":""},0]
[696,"Total Variable Cost Less Loss & Damage","Sum of L601 to L695, plus L587",{"$f":"IF(ISBLANK(RR),\"\",SUM(D$370:D$464)+Line587)","v":2591.5277429916659},{"$f":"IF(ISBLANK(RR),\"\",SUM(E$370:E$464)+Line587)","v":""},{"$f":"IF(ISBLANK(RR),\"\",SUM(F$370:F$464)+Line587)","v":""},{"$f":"IF(ISBLANK(RR),\"\",SUM(G$370:G$464)+Line587)","v":""},{"$f":"IF(ISBLANK(RR),\"\",SUM(H$370:H$464)+Line587)","v":""},2591.5277429916659]
[697,"Constant Cost Markup Ratio","E2L220C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C466,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1.4522094029375101},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C466,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C466,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C466,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C466,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},null,{"$f":"$C466&\"=\"&VLOOKUP($C466,ECodeTable,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E2L220C1=Constant Cost Markup Ratio"}]
[698,"Fully Allocated Variable Cost Less Loss & Damage","L696*L697",{"$f":"IF(ISBLANK(RR),\"\",Line696*Line697)","v":3763.4409563459203},{"$f":"IF(ISBLANK(RR),\"\",Line696*Line697)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line696*Line697)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line696*Line697)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line696*Line697)","v":""},3763.4409563459203]
[699,"Loss & Damage Claims","L537",{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":1.3588848083408001},{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line537)","v":""},{"$f":"SUM(D468:H468)","v":1.3588848083408001}]
[700,"Total Variable Shipment Cost","L696+L699",{"$f":"IF(ISBLANK(RR),\"\",Line696+Line699)","v":2592.8866278000069},{"$f":"IF(ISBLANK(RR),\"\",Line696+Line699)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line696+Line699)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line696+Line699)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line696+Line699)","v":""},2592.8866278000069]
[701,"Total Fully Allocated Shipment Cost","L698+L699",{"$f":"IF(ISBLANK(RR),\"\",Line698+Line699)","v":3764.7998411542612},{"$f":"IF(ISBLANK(RR),\"\",Line698+Line699)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line698+Line699)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line698+Line699)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line698+Line699)","v":""},3764.7998411542612]
[702,"Total Variable Shipment Cost Per Hundredweight","L700/(20*NC*WT)",{"$f":"IF(ISBLANK(RR),\"\",Line700/(20*NC*WT))","v":1.6205541423750043},{"$f":"IF(ISBLANK(RR),\"\",Line700/(20*NC*WT))","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line700/(20*NC*WT))","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line700/(20*NC*WT))","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line700/(20*NC*WT))","v":""},1.6205541423750043]
[703,"Total Fully Allocated Shipment Cost Per Hundredweight","L701/(20*NC*WT)",{"$f":"IF(ISBLANK(RR),\"\",Line701/(20*NC*WT))","v":2.3529999007214131},{"$f":"IF(ISBLANK(RR),\"\",Line701/(20*NC*WT))","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line701/(20*NC*WT))","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line701/(20*NC*WT))","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line701/(20*NC*WT))","v":""},2.3529999007214131]
[]
[]
["Special Calculations Area"]
[]
["LINE","DESCRIPTION","SOURCE","ORR","JRR1","JRR2","JRR3","TRR"]
["L102","Circuity factor","Unit Train Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",1,1/VLOOKUP(RR&\"-\"&$C$25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",1,1/VLOOKUP(RR&\"-\"&$C$25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",1,1/VLOOKUP(RR&\"-\"&$C$25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",1,1/VLOOKUP(RR&\"-\"&$C$25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(SZ<>\"Unit\",1,1/VLOOKUP(RR&\"-\"&$C$25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
[]
["L106","Estimated way train miles including circuity",{"$f":"\"(E2L201C1/E2L118C4)*(\"&$C$25&\"/E2L118C7)*L250\"","v":"(E2L201C1/E2L118C4)*(E2L106C5/E2L118C7)*L250"},{"$f":"IF(ISBLANK(RR),\"\",MIN((D$482/D$485*D$484/D$483)*D$486,D$487))","v":15.902153970978807},{"$f":"IF(ISBLANK(RR),\"\",MIN((E$482/E$485*E$484/E$483)*E$486,E$487))","v":""},{"$f":"IF(ISBLANK(RR),\"\",MIN((F$482/F$485*F$484/F$483)*F$486,F$487))","v":""},{"$f":"IF(ISBLANK(RR),\"\",MIN((G$482/G$485*G$484/G$483)*G$486,G$487))","v":""},{"$f":"IF(ISBLANK(RR),\"\",MIN((H$482/H$485*H$484/H$483)*H$486,H$487))","v":""}]
[]
[null,{"$f":"VLOOKUP($C482,ECodeTable!$B$2:$C$975,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"Average Distance Per Car In Way Trains"},"E2L201C1",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C482,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":13.622462709699301},"","","",""]
[null,{"$f":"VLOOKUP($C483,ECodeTable!$B$2:$C$975,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"E/L Ratio, All Freight Cars, AVERAGE ALL FREIGHT CARS"},"E2L118C4",{"$f":"IF(ISBLANK(RR),\"\",VLOOKUP(RR&\"-\"&$C483,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1.69969970184774},"","","",""]
[null,{"$f":"VLOOKUP($C484,ECodeTable!$B$2:$C$975,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"Local circuity, HOPPER - COVERED"},{"$f":"$C$25","v":"E2L106C5"},1.1259999999999999,"","","",""]
[null,{"$f":"VLOOKUP($C485,ECodeTable!$B$2:$C$975,MATCH(\"eTitle_and_Desc\",ECodeHeaders,0),FALSE)","v":"Average circuity, AVERAGE ALL FREIGHT CARS"},"E2L118C7",1.135,"","","",""]
[null,"Shipment origination/termination","L250",{"$f":"IF(ISBLANK(RR),\"\",Line250)","v":2},{"$f":"IF(ISBLANK(RR),\"\",Line250)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line250)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line250)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line250)","v":""}]
[null,"Actual miles including circuity","L103",{"$f":"IF(ISBLANK(RR),\"\",Line103)","v":1000},{"$f":"IF(ISBLANK(RR),\"\",Line103)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103)","v":""},{"$f":"IF(ISBLANK(RR),\"\",Line103)","v":""}]
[]
["Make Whole Adjustment Factors"]
["LINE","DESCRIPTION","SOURCE","ORR","JRR1","JRR2","JRR3","TRR"]
["L105","E/L ratio, this car","Efficiency Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),1/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(User_EfficiencyAdjustments=\"N\",1,IF(OR(SZ=\"Single\",SZ=\"Multi\"),1,IF(SZ=\"Unit\",2/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(SZ=\"Intermodal\",1,1))))))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),1/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(User_EfficiencyAdjustments=\"N\",1,IF(OR(SZ=\"Single\",SZ=\"Multi\"),1,IF(SZ=\"Unit\",2/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(SZ=\"Intermodal\",1,1))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),1/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(User_EfficiencyAdjustments=\"N\",1,IF(OR(SZ=\"Single\",SZ=\"Multi\"),1,IF(SZ=\"Unit\",2/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(SZ=\"Intermodal\",1,1))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),1/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(User_EfficiencyAdjustments=\"N\",1,IF(OR(SZ=\"Single\",SZ=\"Multi\"),1,IF(SZ=\"Unit\",2/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(SZ=\"Intermodal\",1,1))))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),1/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(User_EfficiencyAdjustments=\"N\",1,IF(OR(SZ=\"Single\",SZ=\"Multi\"),1,IF(SZ=\"Unit\",2/VLOOKUP(RR&\"-\"&$C$28,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE),IF(SZ=\"Intermodal\",1,1))))))","v":""}]
["L257","UC per CLOT Cler-OPR","Make Whole Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(AND(SZ<>\"Single\",SZ<>\"Intermodal\"),0.75+(0.25/Line201),IF(AND(SZ=\"Intermodal\",ROUND(Line204,0)>=MultiCarDef),0.75+(0.25/Line204),1))))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(AND(SZ<>\"Single\",SZ<>\"Intermodal\"),0.75+(0.25/Line201),IF(AND(SZ=\"Intermodal\",ROUND(Line204,0)>=MultiCarDef),0.75+(0.25/Line204),1))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(AND(SZ<>\"Single\",SZ<>\"Intermodal\"),0.75+(0.25/Line201),IF(AND(SZ=\"Intermodal\",ROUND(Line204,0)>=MultiCarDef),0.75+(0.25/Line204),1))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(AND(SZ<>\"Single\",SZ<>\"Intermodal\"),0.75+(0.25/Line201),IF(AND(SZ=\"Intermodal\",ROUND(Line204,0)>=MultiCarDef),0.75+(0.25/Line204),1))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(AND(SZ<>\"Single\",SZ<>\"Intermodal\"),0.75+(0.25/Line201),IF(AND(SZ=\"Intermodal\",ROUND(Line204,0)>=MultiCarDef),0.75+(0.25/Line204),1))))","v":""}]
["L301","SEM per Industry switch event","Make Whole Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,1-VLOOKUP($A493,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE)))","v":1},"","","",""]
["L302","SEM per Interchange switch event","Make Whole Adjustment Factor",1,"","","",""]
["L303","SEM per I&I train switch event","Make Whole Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A495,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A495,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A495,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A495,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A495,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""}]
["L325","SEM per Intraterminal switch","Make Whole Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,1-VLOOKUP($A496,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE)))","v":1},"","","",""]
["L326","SEM per Interterminal switch","Make Whole Adjustment Factor",1,"","","",""]
["L419","CM(Y)/Industry switch (L-E)","Make Whole Adjustment Factor",1,"","","",""]
["L420","CM(Y)/Interchange switch (L-E)","Make Whole Adjustment Factor",1,"","","",""]
["L421","CM(Y)/I&I train switch (L-E)","Make Whole Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A500,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A500,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A500,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A500,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A500,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""}]
["L443","CD(Y)/Industry switch (L or E)","Make Whole Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,1-VLOOKUP($A501,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE)))","v":1},"","","",""]
["L444","CD(Y)/Interchange swt (L or E)","Make Whole Adjustment Factor",1,"","","",""]
["L445","CD(Y)/I&I train switch (L or E)","Make Whole Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A503,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A503,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A503,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A503,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,IF(SZ<>\"Intermodal\",1-VLOOKUP($A503,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE),IF(ROUND(Line204,0)<MultiCarDef,1,0))))","v":""}]
["L449","CD(Y)-per Loading & Unloading for Industry switch","Make Whole Adjustment Factor",{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,1-VLOOKUP($A504,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE)))","v":1},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,1-VLOOKUP($A504,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,1-VLOOKUP($A504,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,1-VLOOKUP($A504,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(RR),\"\",IF(User_EfficiencyAdjustments=\"N\",1,1-VLOOKUP($A504,MWAdjustmentFactors,MATCH(SZ,MWAdjustmentTitles,0),FALSE)))","v":""}]

{"sheet":"DetailedParameters","index":2,"n_rows":90,"n_cols":13,"rows_kept":90,"cut":false,"hidden":false,"merged":[]}
["Surface Transportation Board - Railroad Cost Program - Detailed Parameters"]
[]
[null,null,1,2,3,4,5,null,"Default Values of Detailed Parameters"]
["General","Source",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",INDEX(RR,C$3))","v":"WEST"},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",INDEX(RR,D$3))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",INDEX(RR,E$3))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",INDEX(RR,F$3))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",INDEX(RR,G$3))","v":""},"Line",{"$f":"IF(ISBLANK(C$4),\"\",C$4)","v":"WEST"},{"$f":"IF(ISBLANK(D$4),\"\",D$4)","v":""},"","",""]
["Circuity",{"$f":"RailroadCostProgram!C25","v":"E2L106C5"},1,null,null,null,null,"L102",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL102,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B5,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":1.1259999999999999},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL102,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B5,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL102,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B5,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL102,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B5,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL102,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B5,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
["Empty/Loaded Ratio",{"$f":"RailroadCostProgram!C28","v":"E2L106C2"},null,null,null,null,null,"L105",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",INDEX(AdjustL105,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B6,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1.9769228108307599},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",INDEX(AdjustL105,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B6,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",INDEX(AdjustL105,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B6,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",INDEX(AdjustL105,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B6,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",INDEX(AdjustL105,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B6,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""}]
["General Overhead Ratio",{"$f":"RailroadCostProgram!C169","v":"E2L219C1"},null,null,null,null,null,"L403/L408",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",VLOOKUP(INDEX(RR,C$3)&\"-\"&$B7,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":1.07001626723413},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",VLOOKUP(INDEX(RR,D$3)&\"-\"&$B7,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",VLOOKUP(INDEX(RR,E$3)&\"-\"&$B7,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",VLOOKUP(INDEX(RR,F$3)&\"-\"&$B7,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",VLOOKUP(INDEX(RR,G$3)&\"-\"&$B7,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""}]
["Tare Weight",{"$f":"RailroadCostProgram!C48","v":"E2L106C1"},null,null,null,null,null,"L212",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,VLOOKUP(INDEX(RR,C$3)&\"-\"&$B8,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":30.9}]
[]
[]
["Intermodal","Source",{"$f":"C$4","v":"WEST"},null,null,null,null,"Line","Intermodal\nORR"]
["Number of TCUs",{"$f":"RailroadCostProgram!C38","v":"[User]"},null,null,null,null,null,"L203",{"$f":"IF(SZ<>\"Intermodal\",\"n/a\",NC)","v":"n/a"}]
["Number of TCUs per Flat Car",{"$f":"RailroadCostProgram!C37","v":"E2L202C1"},null,null,null,null,null,"L202",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ<>\"Intermodal\",\"n/a\",IF(User_TOFCPlanCode=4,1,VLOOKUP(IF(ISTEXT(User_IntermodalORR),User_IntermodalORR,INDEX(RR,C$3))&\"-\"&$B13,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":"n/a"}]
["TOFC Plan Code",{"$f":"RailroadCostProgram!C348","v":"[User]"},null,null,null,null,null,"L569",{"$f":"IF(SZ<>\"Intermodal\",\"n/a\",1)","v":"n/a"}]
["Tare Weight of TCU",{"$f":"RailroadCostProgram!C50","v":"E2L204C1"},null,null,null,null,null,"L214",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ<>\"Intermodal\",\"n/a\",IF(User_TOFCPlanCode=4,13.9,VLOOKUP(IF(ISTEXT(User_IntermodalORR),User_IntermodalORR,INDEX(RR,C$3))&\"-\"&$B15,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":"n/a"}]
["E/L Ratio of TCU",{"$f":"RailroadCostProgram!C51","v":"E2L207C1"},null,null,null,null,null,"L215",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ<>\"Intermodal\",\"n/a\",VLOOKUP(INDEX(RR,C$3)&\"-\"&$B16,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":"n/a"}]
["Line Haul Miles per TCU Day","E2L205C1",null,null,null,null,null,"L549",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ<>\"Intermodal\",\"n/a\",VLOOKUP(INDEX(RR,C$3)&\"-\"&$B17,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":"n/a"}]
["TCU Days per O/T Event",{"$f":"RailroadCostProgram!C330","v":"E2L206C1"},null,null,null,null,null,"L550",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ<>\"Intermodal\",\"n/a\",VLOOKUP(INDEX(RR,C$3)&\"-\"&$B18,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":"n/a"}]
["Refrigerated TCU","[User]",null,null,null,null,null,"L214",{"$f":"IF(SZ<>\"Intermodal\",\"n/a\",\"N\")","v":"n/a"}]
["Number of MVUs",{"$f":"RailroadCostProgram!C307","v":"[User]"},null,null,null,null,null,"L529",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(CarIndex<>12,\"n/a\",(WT/2)*NC))","v":"n/a"}]
[]
[]
["Switching","Source",{"$f":"C$4","v":"WEST"},{"$f":"D$4","v":""},"","","","Line","WEST","","","",""]
["SEMs per Industry Switch",{"$f":"RailroadCostProgram!C131","v":"E2L106C25"},null,null,null,null,null,"L301",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL301,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B24,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":4.3365301515291002},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL301,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B24,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL301,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B24,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL301,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B24,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL301,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B24,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
["SEMs per Interchange Switch",{"$f":"RailroadCostProgram!C132","v":"E2L106C26"},null,null,null,null,null,"L302",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL302,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":2.3850915833410098},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL302,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL302,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL302,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL302,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B25,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
["SEMs per I&I Switch",{"$f":"RailroadCostProgram!C133","v":"E2L106C29"},null,null,null,null,null,"L303",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL303,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B26,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":1.0841325378822799},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL303,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B26,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL303,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B26,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL303,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B26,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL303,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B26,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
["Spotted-to-Pulled Ratio",{"$f":"RailroadCostProgram!C134","v":"E2L106C8"},null,null,null,null,null,"L304",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",VLOOKUP(INDEX(RR,C$3)&\"-\"&$B27,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":2},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",VLOOKUP(INDEX(RR,D$3)&\"-\"&$B27,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",VLOOKUP(INDEX(RR,E$3)&\"-\"&$B27,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",VLOOKUP(INDEX(RR,F$3)&\"-\"&$B27,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",VLOOKUP(INDEX(RR,G$3)&\"-\"&$B27,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""}]
["Cars Given Industry Switch",{"$f":"RailroadCostProgram!C135","v":"L252*L304; TOFC:L251*L304"},null,null,null,null,null,"L305",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line252,C$3)*INDEX(Line304,C$3),INDEX(Line251,C$3)*INDEX(Line304,C$3)))","v":4},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line252,D$3)*INDEX(Line304,D$3),INDEX(Line251,D$3)*INDEX(Line304,D$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line252,E$3)*INDEX(Line304,E$3),INDEX(Line251,E$3)*INDEX(Line304,E$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line252,F$3)*INDEX(Line304,F$3),INDEX(Line251,F$3)*INDEX(Line304,F$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line252,G$3)*INDEX(Line304,G$3),INDEX(Line251,G$3)*INDEX(Line304,G$3)))","v":""}]
["Cars Given Interchange Switch",{"$f":"RailroadCostProgram!C138","v":"L105*L201*L307; TOFC:L105*L204*L307"},null,null,null,null,null,"L308",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line105,C$3)*INDEX(Line201,C$3)*INDEX(Line307,C$3),INDEX(Line105,C$3)*INDEX(Line204,C$3)*INDEX(Line307,C$3)))","v":0},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line105,D$3)*INDEX(Line201,D$3)*INDEX(Line307,D$3),INDEX(Line105,D$3)*INDEX(Line204,D$3)*INDEX(Line307,D$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line105,E$3)*INDEX(Line201,E$3)*INDEX(Line307,E$3),INDEX(Line105,E$3)*INDEX(Line204,E$3)*INDEX(Line307,E$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line105,F$3)*INDEX(Line201,F$3)*INDEX(Line307,F$3),INDEX(Line105,F$3)*INDEX(Line204,F$3)*INDEX(Line307,F$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(SZ<>\"Intermodal\",INDEX(Line105,G$3)*INDEX(Line201,G$3)*INDEX(Line307,G$3),INDEX(Line105,G$3)*INDEX(Line204,G$3)*INDEX(Line307,G$3)))","v":""}]
["Miles Between I&I Switches",{"$f":"RailroadCostProgram!C139","v":"E2L106C23"},null,null,null,null,null,"L309",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",VLOOKUP(INDEX(RR,C$3)&\"-\"&$B30,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":200},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",VLOOKUP(INDEX(RR,D$3)&\"-\"&$B30,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",VLOOKUP(INDEX(RR,E$3)&\"-\"&$B30,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",VLOOKUP(INDEX(RR,F$3)&\"-\"&$B30,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",VLOOKUP(INDEX(RR,G$3)&\"-\"&$B30,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""}]
["Cars Given I&I Switch",{"$f":"RailroadCostProgram!C140","v":"L205/L309"},null,null,null,null,null,"L310",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",INDEX(Line205,C$3)/INDEX(Line309,C$3))","v":9.8846140541538006},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",INDEX(Line205,D$3)/INDEX(Line309,D$3))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",INDEX(Line205,E$3)/INDEX(Line309,E$3))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",INDEX(Line205,F$3)/INDEX(Line309,F$3))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",INDEX(Line205,G$3)/INDEX(Line309,G$3))","v":""}]
["Cars Given Intraterminal Switch",{"$f":"RailroadCostProgram!C152","v":"[User]"},null,null,null,null,null,"L321",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(INDEX(SG,C$3)<>\"IA\",0,NC))","v":0},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(INDEX(SG,D$3)<>\"IA\",0,NC))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(INDEX(SG,E$3)<>\"IA\",0,NC))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(INDEX(SG,F$3)<>\"IA\",0,NC))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(INDEX(SG,G$3)<>\"IA\",0,NC))","v":""}]
["Cars Given Interterminal Switch",{"$f":"RailroadCostProgram!C153","v":"[User]"},null,null,null,null,null,"L322",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(INDEX(SG,C$3)<>\"IR\",0,NC))","v":0},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(INDEX(SG,D$3)<>\"IR\",0,NC))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(INDEX(SG,E$3)<>\"IR\",0,NC))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(INDEX(SG,F$3)<>\"IR\",0,NC))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(INDEX(SG,G$3)<>\"IR\",0,NC))","v":""}]
["SEMs per Intraterminal Switch",{"$f":"RailroadCostProgram!C156","v":"E2L106C27"},null,null,null,null,null,"L325",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(INDEX(SG,C$3)<>\"IA\",0,INDEX(AdjustL325,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B34,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(INDEX(SG,D$3)<>\"IA\",0,INDEX(AdjustL325,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B34,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(INDEX(SG,E$3)<>\"IA\",0,INDEX(AdjustL325,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B34,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(INDEX(SG,F$3)<>\"IA\",0,INDEX(AdjustL325,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B34,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(INDEX(SG,G$3)<>\"IA\",0,INDEX(AdjustL325,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B34,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
["SEMs per Interterminal Switch",{"$f":"RailroadCostProgram!C157","v":"E2L106C28"},null,null,null,null,null,"L326",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(INDEX(SG,C$3)<>\"IR\",0,INDEX(AdjustL326,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B35,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(INDEX(SG,D$3)<>\"IR\",0,INDEX(AdjustL326,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B35,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(INDEX(SG,E$3)<>\"IR\",0,INDEX(AdjustL326,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B35,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(INDEX(SG,F$3)<>\"IR\",0,INDEX(AdjustL326,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B35,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(INDEX(SG,G$3)<>\"IR\",0,INDEX(AdjustL326,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B35,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
[]
[]
["Train Statistics","Source",{"$f":"C$4","v":"WEST"},{"$f":"D$4","v":""},"","","","Line","WEST","","","",""]
["Average Locomotives - Unit",{"$f":"RailroadCostProgram!C63","v":"E2L208C1"},null,null,null,null,null,"L226",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",VLOOKUP(INDEX(RR,C$3)&\"-\"&$B39,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":3.3800302893865402},"","","",""]
["Average Locomotives - Way",{"$f":"RailroadCostProgram!C64","v":"E2L209C1"},null,null,null,null,null,"L227",2.0571275181762698,"","","",""]
["Average Locomotives - Thru",{"$f":"RailroadCostProgram!C65","v":"E2L210C1"},null,null,null,null,null,"L228",3.31597647188162,"","","",""]
["Unit Train Weight",{"$f":"RailroadCostProgram!C69","v":"E2L211C1*L105"},null,null,null,null,null,"L232",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",INDEX(Line105,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&LEFT($B42,8),UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":20109.14742859266},"","","",""]
["Way Train Weight",{"$f":"RailroadCostProgram!C70","v":"E2L212C1*L105"},null,null,null,null,null,"L233",5229.6360278061547,"","","",""]
["Thru Train Weight",{"$f":"RailroadCostProgram!C71","v":"E2L213C1*L105"},null,null,null,null,null,"L234",14737.997599254424,"","","",""]
["Shipment Share - Unit Train Miles",{"$f":"RailroadCostProgram!C107","v":"L108"},null,null,null,null,null,"L269",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ<>\"Unit\",0,INDEX(Line108,C$3)))","v":0},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(SZ<>\"Unit\",0,INDEX(Line108,D$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(SZ<>\"Unit\",0,INDEX(Line108,E$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(SZ<>\"Unit\",0,INDEX(Line108,F$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(SZ<>\"Unit\",0,INDEX(Line108,G$3)))","v":""}]
["Shipment Share - Way Train Miles",{"$f":"RailroadCostProgram!C108","v":"L109*L237"},null,null,null,null,null,"L270",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line109,C$3)*INDEX(Line237,C$3)))","v":0.84812709873346093},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line109,D$3)*INDEX(Line237,D$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line109,E$3)*INDEX(Line237,E$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line109,F$3)*INDEX(Line237,F$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line109,G$3)*INDEX(Line237,G$3)))","v":""}]
["Shipment Share - Thru Train Miles",{"$f":"RailroadCostProgram!C109","v":"L110*L238"},null,null,null,null,null,"L271",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line110,C$3)*INDEX(Line238,C$3)))","v":18.624140925910162},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line110,D$3)*INDEX(Line238,D$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line110,E$3)*INDEX(Line238,E$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line110,F$3)*INDEX(Line238,F$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(SZ=\"Unit\",0,INDEX(Line110,G$3)*INDEX(Line238,G$3)))","v":""}]
["Crew Wages - Unit",{"$f":"RailroadCostProgram!C111","v":"[User]"},null,null,null,null,null,"L273"]
["Crew Wages - Way",{"$f":"RailroadCostProgram!C112","v":"[User]"},null,null,null,null,null,"L274"]
["Crew Wages - Thru",{"$f":"RailroadCostProgram!C113","v":"[User]"},null,null,null,null,null,"L275"]
[]
[]
["Freight Car Miles","Source",{"$f":"C$4","v":"WEST"},{"$f":"D$4","v":""},"","","","Line","WEST","","","",""]
["Car-Miles per Industry Switch",{"$f":"RailroadCostProgram!C186","v":"E2L106C17"},null,null,null,null,null,"L419",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL419,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B54,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":4},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL419,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B54,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL419,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B54,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL419,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B54,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL419,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B54,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
["Car-Miles per Interchange Switch",{"$f":"RailroadCostProgram!C187","v":"E2L106C18"},null,null,null,null,null,"L420",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL420,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B55,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":2.75},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL420,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B55,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL420,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B55,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL420,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B55,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL420,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B55,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
["Car-Miles per I&I Switch",{"$f":"RailroadCostProgram!C188","v":"E2L106C21"},null,null,null,null,null,"L421",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL421,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":1},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL421,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL421,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL421,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL421,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B56,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
["Actual Miles per Car Day",{"$f":"RailroadCostProgram!C203","v":"E2L106C22"},null,null,null,null,null,"L435",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",VLOOKUP(INDEX(RR,C$3)&\"-\"&$B57,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":473.48660392642898},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",VLOOKUP(INDEX(RR,D$3)&\"-\"&$B57,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",VLOOKUP(INDEX(RR,E$3)&\"-\"&$B57,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",VLOOKUP(INDEX(RR,F$3)&\"-\"&$B57,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",VLOOKUP(INDEX(RR,G$3)&\"-\"&$B57,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))","v":""}]
["Car-Miles per Intraterminal Switch",{"$f":"RailroadCostProgram!C252","v":"E2L106C19"},null,null,null,null,null,"L482",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(INDEX(SG,C$3)<>\"IA\",0,VLOOKUP(INDEX(RR,C$3)&\"-\"&$B58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(INDEX(SG,D$3)<>\"IA\",0,VLOOKUP(INDEX(RR,D$3)&\"-\"&$B58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(INDEX(SG,E$3)<>\"IA\",0,VLOOKUP(INDEX(RR,E$3)&\"-\"&$B58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(INDEX(SG,F$3)<>\"IA\",0,VLOOKUP(INDEX(RR,F$3)&\"-\"&$B58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(INDEX(SG,G$3)<>\"IA\",0,VLOOKUP(INDEX(RR,G$3)&\"-\"&$B58,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
["Car-Miles per Interterminal Switch",{"$f":"RailroadCostProgram!C253","v":"E2L106C20"},null,null,null,null,null,"L483",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(INDEX(SG,C$3)<>\"IR\",0,VLOOKUP(INDEX(RR,C$3)&\"-\"&$B59,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":0},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(INDEX(SG,D$3)<>\"IR\",0,VLOOKUP(INDEX(RR,D$3)&\"-\"&$B59,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(INDEX(SG,E$3)<>\"IR\",0,VLOOKUP(INDEX(RR,E$3)&\"-\"&$B59,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(INDEX(SG,F$3)<>\"IR\",0,VLOOKUP(INDEX(RR,F$3)&\"-\"&$B59,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(INDEX(SG,G$3)<>\"IR\",0,VLOOKUP(INDEX(RR,G$3)&\"-\"&$B59,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE)))","v":""}]
[]
[]
["Freight Car Days","Source",{"$f":"C$4","v":"WEST"},{"$f":"D$4","v":""},"","","","Line","WEST","","","",""]
["Car-Days Running",{"$f":"RailroadCostProgram!C204","v":"L406/L435"},null,null,null,null,null,"L436",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OWN<>\"Railroad\",0,INDEX(Line406,C$3)/INDEX(Line435,C$3)))","v":4.1752454967827077},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OWN<>\"Railroad\",0,INDEX(Line406,D$3)/INDEX(Line435,D$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OWN<>\"Railroad\",0,INDEX(Line406,E$3)/INDEX(Line435,E$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OWN<>\"Railroad\",0,INDEX(Line406,F$3)/INDEX(Line435,F$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OWN<>\"Railroad\",0,INDEX(Line406,G$3)/INDEX(Line435,G$3)))","v":""}]
["Car-Days per Industry Switch",{"$f":"RailroadCostProgram!C211","v":"E2L106C9"},null,null,null,null,null,"L443",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL443,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":1},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL443,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL443,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL443,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL443,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B64,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""}]
["Car-Days per Interchange Switch",{"$f":"RailroadCostProgram!C212","v":"E2L106C10"},null,null,null,null,null,"L444",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL444,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0.5},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL444,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL444,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL444,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL444,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B65,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""}]
["Car-Days per I&I Switch",{"$f":"RailroadCostProgram!C213","v":"E2L106C13"},null,null,null,null,null,"L445",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL445,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B66,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0.5},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL445,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B66,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL445,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B66,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL445,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B66,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL445,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B66,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""}]
["Car-Days per Load & Unload (L&UL)",{"$f":"RailroadCostProgram!C217","v":"E2L106C14"},null,null,null,null,null,"L449",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,C$3)=\"IA\",INDEX(SG,C$3)=\"IR\"),0,INDEX(AdjustL449,C$3)*VLOOKUP(INDEX(RR,C$3)&\"-\"&$B67,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":2},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,D$3)=\"IA\",INDEX(SG,D$3)=\"IR\"),0,INDEX(AdjustL449,D$3)*VLOOKUP(INDEX(RR,D$3)&\"-\"&$B67,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,E$3)=\"IA\",INDEX(SG,E$3)=\"IR\"),0,INDEX(AdjustL449,E$3)*VLOOKUP(INDEX(RR,E$3)&\"-\"&$B67,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,F$3)=\"IA\",INDEX(SG,F$3)=\"IR\"),0,INDEX(AdjustL449,F$3)*VLOOKUP(INDEX(RR,F$3)&\"-\"&$B67,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(OWN<>\"Railroad\",0,IF(OR(INDEX(SG,G$3)=\"IA\",INDEX(SG,G$3)=\"IR\"),0,INDEX(AdjustL449,G$3)*VLOOKUP(INDEX(RR,G$3)&\"-\"&$B67,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":""}]
["Car-Days in Yard",{"$f":"RailroadCostProgram!C219","v":"L446+L447+L448+L450"},null,null,null,null,null,"L451",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,INDEX(Line446,C$3)+INDEX(Line447,C$3)+INDEX(Line448,C$3)+INDEX(Line450,C$3)))","v":12.9423070270769},{"$f":"IF(ISBLANK(INDEX(RR,D$3)),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,INDEX(Line446,D$3)+INDEX(Line447,D$3)+INDEX(Line448,D$3)+INDEX(Line450,D$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,E$3)),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,INDEX(Line446,E$3)+INDEX(Line447,E$3)+INDEX(Line448,E$3)+INDEX(Line450,E$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,F$3)),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,INDEX(Line446,F$3)+INDEX(Line447,F$3)+INDEX(Line448,F$3)+INDEX(Line450,F$3)))","v":""},{"$f":"IF(ISBLANK(INDEX(RR,G$3)),\"\",IF(AND(SZ=\"Intermodal\",User_TOFCPlanCode=4),0,INDEX(Line446,G$3)+INDEX(Line447,G$3)+INDEX(Line448,G$3)+INDEX(Line450,G$3)))","v":""}]
["Car-Days per Intraterminal Switch",{"$f":"RailroadCostProgram!C262","v":"E2L106C11"},null,null,null,null,null,"L492",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OWN<>\"Railroad\",0,IF(INDEX(SG,C$3)<>\"IA\",0,VLOOKUP(INDEX(RR,C$3)&\"-\"&$B69,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0},"","","",""]
["Car-Days per L&UL - Intraterminal",{"$f":"RailroadCostProgram!C263","v":"E2L106C15"},null,null,null,null,null,"L493",0,"","","",""]
["Car-Days per Interterminal Switch",{"$f":"RailroadCostProgram!C264","v":"E2L106C12"},null,null,null,null,null,"L494",{"$f":"IF(ISBLANK(INDEX(RR,C$3)),\"\",IF(OWN<>\"Railroad\",0,IF(INDEX(SG,C$3)<>\"IR\",0,VLOOKUP(INDEX(RR,C$3)&\"-\"&$B71,UnitCostXML,MATCH(CostYear,UnitCostXMLHeaders,0),FALSE))))","v":0},"","","",""]
["Car-Days per L&UL - Interterminal",{"$f":"RailroadCostProgram!C265","v":"E2L106C16"},null,null,null,null,null,"L495",0,"","","",""]
[]
[]
["Freight Car Rental","Source",{"$f":"C$4","v":"WEST"},{"$f":"D$4","v":""},"","","","Line"]
["Car Mile Rental - Private",{"$f":"RailroadCostProgram!$C$168","v":"[User]"},null,null,null,null,null,"L402"]
["Charge per Car Mile",{"$f":"RailroadCostProgram!$C$174","v":"[User]"},null,null,null,null,null,"L407"]
["Charge per Car Day",{"$f":"RailroadCostProgram!$C$200","v":"[User]"},null,null,null,null,null,"L432"]
[]
[]
["Accessorial Services","Source",{"$f":"C$4","v":"WEST"},{"$f":"D$4","v":""},"","","","Line"]
["Lake Transfer Ton Miles",{"$f":"RailroadCostProgram!$C$275","v":"[User]"},null,null,null,null,null,"L501"]
["Coal Terminal Tons",{"$f":"RailroadCostProgram!$C$283","v":"[User]"},null,null,null,null,null,"L508"]
["Ore Terminal Tons",{"$f":"RailroadCostProgram!$C$291","v":"[User]"},null,null,null,null,null,"L515"]
["Marine Terminal Tons",{"$f":"RailroadCostProgram!$C$299","v":"[User]"},null,null,null,null,null,"L522"]
["Railroad Provides Accessorial Services","[User]",null,null,null,null,null,"L458+"]
[]
["Include Jurisdictional Add-On Charges?","[User]","Y"]
[]
["Include Efficiency Adjustments?","[User]","Y"]

{"sheet":"BatchCostProgram","index":3,"n_rows":10,"n_cols":29,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["Surface Transportation Board - Batch Cost Program - Input (Control Parameters File)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISBLANK($B1),\"\",$A1)","v":""},{"$f":"IF(ISBLANK($B1),\"\",IF(ISTEXT($B1),VLOOKUP($B1,RRAlphas,5,FALSE),VLOOKUP($B1,RRNumerics,8,FALSE)))","v":""},{"$f":"IF(ISBLANK($B1),\"\",$C1)","v":""},{"$f":"IF(ISBLANK($B1),\"\",VLOOKUP($D1,URCSSegments,1,FALSE))","v":""},{"$f":"IF(ISBLANK($B1),\"\",IF($E1<=17,VLOOKUP($E1,URCSCarTypes,3,FALSE),VLOOKUP($E1,STBCarTypes,2,FALSE)))","v":""},{"$f":"IF(ISBLANK($B1),\"\",$F1)","v":""},{"$f":"IF(ISBLANK($B1),\"\",VLOOKUP($G1,URCSOwnerships,2,FALSE))","v":""},{"$f":"IF(ISBLANK($B1),\"\",$H1)","v":""},{"$f":"IF(ISBLANK($B1),\"\",VLOOKUP(LEFT($I1&\"00000\",5),STCCCodes,3,FALSE))","v":""},{"$f":"IF(ISBLANK($B1),\"\",IF(ISNUMBER($J1),VLOOKUP($J1,URCSShipmentSizeCodes,2,FALSE),VLOOKUP($J1,URCSShipmentSizes,1,FALSE)))","v":""},{"$f":"IF(ISBLANK($B1),\"\",MAX(0,$M1-$C1))","v":""},{"$f":"IF(ISBLANK($B1),\"\",IF(ISBLANK($K1),\"\",IF(ISNUMBER($K1),$K1,NA())))","v":""},{"$f":"IF(ISBLANK($B1),\"\",IF(ISBLANK($L1),\"\",IF(ISNUMBER($L1),VLOOKUP($L1,URCSTOFCPlans,1,FALSE),VLOOKUP($L1,URCSTOFCServiceCodes,3,FALSE))))","v":""},{"$f":"IF(ISBLANK($B1),\"\",IF(OR(ISBLANK($N1),$Y1<>\"Intermodal\"),\"\",IF(ISTEXT($N1),VLOOKUP($N1,RRAlphas,5,FALSE),VLOOKUP($N1,RRNumerics,8,FALSE))))","v":""}]
[]
[{"$f":"\"Using \"&TEXT(CostYear,\"0000\")&\" Unit Costs\"","v":"Using 2021 Unit Costs"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"These columns convert the user entered codes in columns B thru N into the format needed by the RailroadCostProgram sheet.  These formulas are stored in Row 1.  Use AutoFilter to check for #N/A, which indicates an invalid value was entered."]
["ID","RR","DIS","SG","FC","NC","OWN","WT","COM","SZ","L102","L569","TDIS","ORR",null,{"$f":"A4","v":"ID"},"RR","DIS","SG","FC","NC","OWN","WT","COM","SZ","OtherRRDist","L102","L569","ORR"]
["Sample 1-Coal-OT","WEST",1000,"OT",42,1,"R",100,"11000",{"$f":"IF(OR($E5=11,$E5=46),\"Intermodal\",IF($F5<MultiCarDef,\"Single\",IF($F5<UnitTrainDef,\"Multi\",\"Unit\")))","v":"Single"},1]
["Sample 2-Grain-OD","WEST",800,"OD",41,25,"R",80,"01130","Multi",1,null,1200]
["Sample 2-Grain-RT","WEST",400,"RT",41,25,"R",80,"01130","Multi",1,null,1200]
["Sample 3-Intermodal-OT","WEST",1000,"OT",11,1,"P",15,"46100",4,1,null,1000,"WEST"]
["Sample 4-Intermodal-OD","WEST",1000,"OD",46,1,"P",15,"46100","Intermodal",1,3,1800,"WEST"]
["Sample 4-Intermodal-RT","EAST",800,"RT",46,1,"P",15,"46100","Intermodal",1,3,1800,"WEST"]

{"sheet":"BatchOutput","index":4,"n_rows":4,"n_cols":433,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["Surface Transportation Board - Batch Cost Program - Output",null,null,null,null,null,null,null,null,null,{"$f":"INDEX(Line101,1)","v":1000},{"$f":"INDEX(Line102,1)","v":1},{"$f":"INDEX(Line103,1)","v":1000},{"$f":"INDEX(Line104,1)","v":0},{"$f":"INDEX(Line105,1)","v":1.9769228108307599},{"$f":"INDEX(Line106,1)","v":15.902153970978807},{"$f":"INDEX(Line107,1)","v":984.09784602902118},{"$f":"INDEX(Line108,1)","v":0},{"$f":"INDEX(Line109,1)","v":31.437330926570954},{"$f":"INDEX(Line110,1)","v":1945.4854799041889},{"$f":"INDEX(Line111,1)","v":1976.92281083076},{"$f":"INDEX(Line201,1)","v":1},{"$f":"INDEX(Line202,1)","v":0},{"$f":"INDEX(Line203,1)","v":0},{"$f":"INDEX(Line204,1)","v":0},{"$f":"INDEX(Line205,1)","v":1976.92281083076},{"$f":"INDEX(Line206,1)","v":0},{"$f":"INDEX(Line207,1)","v":0},{"$f":"INDEX(Line208,1)","v":0},{"$f":"INDEX(Line209,1)","v":0},{"$f":"INDEX(Line210,1)","v":0},{"$f":"INDEX(Line211,1)","v":0},{"$f":"INDEX(Line212,1)","v":30.9},{"$f":"INDEX(Line213,1)","v":61086.914854670482},{"$f":"INDEX(Line214,1)","v":0},{"$f":"INDEX(Line215,1)","v":0},{"$f":"INDEX(Line216,1)","v":0},{"$f":"INDEX(Line217,1)","v":80},{"$f":"INDEX(Line218,1)","v":80000},{"$f":"INDEX(Line219,1)","v":141086.91485467047},{"$f":"INDEX(Line220,1)","v":2.3218368538080402E-3},{"$f":"INDEX(Line221,1)","v":327.58079849965094},{"$f":"INDEX(Line222,1)","v":1.0304982814394201E-3},{"$f":"INDEX(Line223,1)","v":145.3898232913277},{"$f":"INDEX(Line224,1)","v":2.1317564600293899E-3},{"$f":"INDEX(Line225,1)","v":300.76294216706026},{"$f":"INDEX(Line226,1)","v":3.3800302893865402},{"$f":"INDEX(Line227,1)","v":2.0571275181762698},{"$f":"INDEX(Line228,1)","v":3.31597647188162},{"$f":"INDEX(Line229,1)","v":0},{"$f":"INDEX(Line230,1)","v":64.670598547062994},{"$f":"INDEX(Line231,1)","v":6451.1840777496127},{"$f":"INDEX(Line232,1)","v":20109.14742859266},{"$f":"INDEX(Line233,1)","v":5229.6360278061547},{"$f":"INDEX(Line234,1)","v":14737.997599254424},{"$f":"INDEX(Line235,1)","v":141.08691485467048},{"$f":"INDEX(Line236,1)","v":0},{"$f":"INDEX(Line237,1)","v":2.6978343063361675E-2},{"$f":"INDEX(Line238,1)","v":9.5730043314573403E-3},{"$f":"INDEX(Line239,1)","v":0},{"$f":"INDEX(Line240,1)","v":1.7447055937156046},{"$f":"INDEX(Line241,1)","v":61.757213119325669},{"$f":"INDEX(Line242,1)","v":63.501918713041277},{"$f":"INDEX(Line243,1)","v":4.7579488438892099},{"$f":"INDEX(Line244,1)","v":302.13888072546132},{"$f":"INDEX(Line245,1)","v":0.84062305220072797},{"$f":"INDEX(Line246,1)","v":53.381176729159279},{"$f":"INDEX(Line247,1)","v":0.81566752566563605},{"$f":"INDEX(Line248,1)","v":51.796452911686728},{"$f":"INDEX(Line250,1)","v":2},{"$f":"INDEX(Line251,1)","v":0},{"$f":"INDEX(Line252,1)","v":2},{"$f":"INDEX(Line253,1)","v":0},{"$f":"INDEX(Line254,1)","v":1},{"$f":"INDEX(Line255,1)","v":0},{"$f":"INDEX(Line256,1)","v":0},{"$f":"INDEX(Line257,1)","v":6.92833589137242},{"$f":"INDEX(Line258,1)","v":13.85667178274484},{"$f":"INDEX(Line259,1)","v":0},{"$f":"INDEX(Line260,1)","v":0},{"$f":"INDEX(Line261,1)","v":0},{"$f":"INDEX(Line262,1)","v":0},{"$f":"INDEX(Line263,1)","v":1.6930165994223101},{"$f":"INDEX(Line264,1)","v":1.6930165994223101},{"$f":"INDEX(Line265,1)","v":0},{"$f":"INDEX(Line266,1)","v":0},{"$f":"INDEX(Line267,1)","v":0},{"$f":"INDEX(Line268,1)","v":0},{"$f":"INDEX(Line269,1)","v":0},{"$f":"INDEX(Line270,1)","v":0.84812709873346093},{"$f":"INDEX(Line271,1)","v":18.624140925910162},{"$f":"INDEX(Line272,1)","v":19.472268024643622},{"$f":"INDEX(Line273,1)","v":0},{"$f":"INDEX(Line274,1)","v":0},{"$f":"INDEX(Line275,1)","v":0},{"$f":"INDEX(Line276,1)","v":8.8760010513333292},{"$f":"INDEX(Line277,1)","v":1},{"$f":"INDEX(Line278,1)","v":1},{"$f":"INDEX(Line279,1)","v":1},{"$f":"INDEX(Line280,1)","v":11.361180154585099},{"$f":"INDEX(Line281,1)","v":0},{"$f":"INDEX(Line282,1)","v":9.6357247626964337},{"$f":"INDEX(Line283,1)","v":211.5922202836467},{"$f":"INDEX(Line284,1)","v":221.22794504634314},{"$f":"INDEX(Line285,1)","v":0.63688697269414296},{"$f":"INDEX(Line286,1)","v":12.401633833704235},{"$f":"INDEX(Line287,1)","v":-3.4287390173140699E-4},{"$f":"INDEX(Line288,1)","v":-6.6765325131692759E-3},{"$f":"INDEX(Line289,1)","v":1.77341275904486E-3},{"$f":"INDEX(Line290,1)","v":3.4532368562444252E-2},{"$f":"INDEX(Line301,1)","v":4.3365301515291002},{"$f":"INDEX(Line302,1)","v":2.3850915833410098},{"$f":"INDEX(Line303,1)","v":1.0841325378822799},{"$f":"INDEX(Line304,1)","v":2},{"$f":"INDEX(Line305,1)","v":4},{"$f":"INDEX(Line306,1)","v":1900.4198779763999},{"$f":"INDEX(Line307,1)","v":0},{"$f":"INDEX(Line308,1)","v":0},{"$f":"INDEX(Line309,1)","v":200},{"$f":"INDEX(Line310,1)","v":9.8846140541538006},{"$f":"INDEX(Line311,1)","v":17.346120606116401},{"$f":"INDEX(Line312,1)","v":0},{"$f":"INDEX(Line313,1)","v":10.716231720516612},{"$f":"INDEX(Line314,1)","v":28.062352326633011},{"$f":"INDEX(Line315,1)","v":6.0228035161016402},{"$f":"INDEX(Line316,1)","v":169.01403426292833},{"$f":"INDEX(Line317,1)","v":1.65613308535255},{"$f":"INDEX(Line318,1)","v":46.47499014095704},{"$f":"INDEX(Line319,1)","v":5.0243142132773198},{"$f":"INDEX(Line320,1)","v":140.99407565269809},{"$f":"INDEX(Line321,1)","v":0},{"$f":"INDEX(Line322,1)","v":0},{"$f":"INDEX(Line323,1)","v":0},{"$f":"INDEX(Line324,1)","v":0},{"$f":"INDEX(Line325,1)","v":0},{"$f":"INDEX(Line326,1)","v":0},{"$f":"INDEX(Line327,1)","v":0},{"$f":"INDEX(Line328,1)","v":0},{"$f":"INDEX(Line329,1)","v":0},{"$f":"INDEX(Line330,1)","v":0},{"$f":"INDEX(Line331,1)","v":0},{"$f":"INDEX(Line332,1)","v":0},{"$f":"INDEX(Line333,1)","v":0},{"$f":"INDEX(Line334,1)","v":0},{"$f":"INDEX(Line401,1)","v":0},{"$f":"INDEX(Line402,1)","v":0},{"$f":"INDEX(Line403,1)","v":1.07001626723413},{"$f":"INDEX(Line404,1)","v":0},{"$f":"INDEX(Line405,1)","v":0},{"$f":"INDEX(Line406,1)","v":1976.92281083076},{"$f":"INDEX(Line407,1)","v":0},{"$f":"INDEX(Line408,1)","v":1.07001626723413},{"$f":"INDEX(Line409,1)","v":0},{"$f":"INDEX(Line410,1)","v":3.3299107981417601E-2},{"$f":"INDEX(Line411,1)","v":65.829766148781076},{"$f":"INDEX(Line412,1)","v":-9.4949203518043801E-4},{"$f":"INDEX(Line413,1)","v":-1.8770724630503304},{"$f":"INDEX(Line414,1)","v":2.3750125261897698E-2},{"$f":"INDEX(Line415,1)","v":46.952164390333436},{"$f":"INDEX(Line416,1)","v":4},{"$f":"INDEX(Line417,1)","v":0},{"$f":"INDEX(Line418,1)","v":9.8846140541538006},{"$f":"INDEX(Line419,1)","v":4},{"$f":"INDEX(Line420,1)","v":2.75},{"$f":"INDEX(Line421,1)","v":1},{"$f":"INDEX(Line422,1)","v":16},{"$f":"INDEX(Line423,1)","v":0},{"$f":"INDEX(Line424,1)","v":9.8846140541538006},{"$f":"INDEX(Line425,1)","v":25.884614054153801},{"$f":"INDEX(Line426,1)","v":8.6577680751685995E-2},{"$f":"INDEX(Line427,1)","v":2.2410298519611325},{"$f":"INDEX(Line428,1)","v":-2.4686792914691098E-3},{"$f":"INDEX(Line429,1)","v":-6.3900810683159767E-2},{"$f":"INDEX(Line430,1)","v":6.1750325680933901E-2},{"$f":"INDEX(Line431,1)","v":1.5983833479692759},{"$f":"INDEX(Line432,1)","v":0},{"$f":"INDEX(Line433,1)","v":0},{"$f":"INDEX(Line434,1)","v":0},{"$f":"INDEX(Line435,1)","v":473.48660392642898},{"$f":"INDEX(Line436,1)","v":4.1752454967827077},{"$f":"INDEX(Line437,1)","v":4.1926106668546304},{"$f":"INDEX(Line438,1)","v":17.505178806547942},{"$f":"INDEX(Line439,1)","v":4.1847974112718003},{"$f":"INDEX(Line440,1)","v":17.472556546360519},{"$f":"INDEX(Line441,1)","v":4.3929953638335997},{"$f":"INDEX(Line442,1)","v":18.341834110233549},{"$f":"INDEX(Line443,1)","v":1},{"$f":"INDEX(Line444,1)","v":0.5},{"$f":"INDEX(Line445,1)","v":0.5},{"$f":"INDEX(Line446,1)","v":4},{"$f":"INDEX(Line447,1)","v":0},{"$f":"INDEX(Line448,1)","v":4.9423070270769003},{"$f":"INDEX(Line449,1)","v":2},{"$f":"INDEX(Line450,1)","v":4},{"$f":"INDEX(Line451,1)","v":12.9423070270769},{"$f":"INDEX(Line452,1)","v":4.1926106668546304},{"$f":"INDEX(Line453,1)","v":54.262054495430249},{"$f":"INDEX(Line454,1)","v":4.1847974112718003},{"$f":"INDEX(Line455,1)","v":54.160932942796244},{"$f":"INDEX(Line456,1)","v":4.3929953638335997},{"$f":"INDEX(Line457,1)","v":56.855494767259842},{"$f":"INDEX(Line458,1)","v":0},{"$f":"INDEX(Line459,1)","v":0},{"$f":"INDEX(Line460,1)","v":8.4837359774947495E-4},{"$f":"INDEX(Line461,1)","v":1.6771691174974965},{"$f":"INDEX(Line462,1)","v":9.1879146870481895E-4},{"$f":"INDEX(Line463,1)","v":1.816379812879253},{"$f":"INDEX(Line464,1)","v":0},{"$f":"INDEX(Line465,1)","v":0},{"$f":"INDEX(Line466,1)","v":2.2057713541486302E-3},{"$f":"INDEX(Line467,1)","v":5.7095540193845495E-2},{"$f":"INDEX(Line468,1)","v":2.3888578186325301E-3},{"$f":"INDEX(Line469,1)","v":6.183466266555078E-2},{"$f":"INDEX(Line470,1)","v":0},{"$f":"INDEX(Line471,1)","v":0},{"$f":"INDEX(Line472,1)","v":0.14149790856257899},{"$f":"INDEX(Line473,1)","v":0.59078850553007922},{"$f":"INDEX(Line474,1)","v":0.15188159942736401},{"$f":"INDEX(Line475,1)","v":0.63414296405325665},{"$f":"INDEX(Line476,1)","v":0},{"$f":"INDEX(Line477,1)","v":0},{"$f":"INDEX(Line478,1)","v":0.14149790856257899},{"$f":"INDEX(Line479,1)","v":1.8313093763061508},{"$f":"INDEX(Line480,1)","v":0.15188159942736401},{"$f":"INDEX(Line481,1)","v":1.9656982915524521},{"$f":"INDEX(Line482,1)","v":0},{"$f":"INDEX(Line483,1)","v":0},{"$f":"INDEX(Line484,1)","v":0},{"$f":"INDEX(Line485,1)","v":0},{"$f":"INDEX(Line486,1)","v":0},{"$f":"INDEX(Line487,1)","v":0},{"$f":"INDEX(Line488,1)","v":0},{"$f":"INDEX(Line489,1)","v":0},{"$f":"INDEX(Line490,1)","v":0},{"$f":"INDEX(Line491,1)","v":0},{"$f":"INDEX(Line492,1)","v":0},{"$f":"INDEX(Line493,1)","v":0},{"$f":"INDEX(Line494,1)","v":0},{"$f":"INDEX(Line495,1)","v":0},{"$f":"INDEX(Line496,1)","v":0},{"$f":"INDEX(Line497,1)","v":0},{"$f":"INDEX(Line498,1)","v":0},{"$f":"INDEX(Line499,1)","v":0},{"$f":"INDEX(Line499A,1)","v":0},{"$f":"INDEX(Line499B,1)","v":0},{"$f":"INDEX(Line499C,1)","v":0},{"$f":"INDEX(Line499D,1)","v":0},{"$f":"INDEX(Line501,1)","v":0},{"$f":"INDEX(Line502,1)","v":0},{"$f":"INDEX(Line503,1)","v":0},{"$f":"INDEX(Line504,1)","v":0},{"$f":"INDEX(Line505,1)","v":0},{"$f":"INDEX(Line506,1)","v":0},{"$f":"INDEX(Line507,1)","v":0},{"$f":"INDEX(Line508,1)","v":0},{"$f":"INDEX(Line509,1)","v":0},{"$f":"INDEX(Line510,1)","v":0},{"$f":"INDEX(Line511,1)","v":0},{"$f":"INDEX(Line512,1)","v":0},{"$f":"INDEX(Line513,1)","v":0},{"$f":"INDEX(Line514,1)","v":0},{"$f":"INDEX(Line515,1)","v":0},{"$f":"INDEX(Line516,1)","v":0},{"$f":"INDEX(Line517,1)","v":0},{"$f":"INDEX(Line518,1)","v":0},{"$f":"INDEX(Line519,1)","v":0},{"$f":"INDEX(Line520,1)","v":0},{"$f":"INDEX(Line521,1)","v":0},{"$f":"INDEX(Line522,1)","v":0},{"$f":"INDEX(Line523,1)","v":0},{"$f":"INDEX(Line524,1)","v":0},{"$f":"INDEX(Line525,1)","v":0},{"$f":"INDEX(Line526,1)","v":0},{"$f":"INDEX(Line527,1)","v":0},{"$f":"INDEX(Line528,1)","v":0},{"$f":"INDEX(Line529,1)","v":0},{"$f":"INDEX(Line530,1)","v":0},{"$f":"INDEX(Line531,1)","v":0},{"$f":"INDEX(Line532,1)","v":0},{"$f":"INDEX(Line533,1)","v":0},{"$f":"INDEX(Line534,1)","v":0},{"$f":"INDEX(Line535,1)","v":80},{"$f":"INDEX(Line536,1)","v":1.6986060104260001E-2},{"$f":"INDEX(Line537,1)","v":1.3588848083408001},{"$f":"INDEX(Line540,1)","v":0},{"$f":"INDEX(Line541,1)","v":0},{"$f":"INDEX(Line542,1)","v":0},{"$f":"INDEX(Line543,1)","v":0},{"$f":"INDEX(Line544,1)","v":0},{"$f":"INDEX(Line545,1)","v":0},{"$f":"INDEX(Line546,1)","v":0},{"$f":"INDEX(Line547,1)","v":0},{"$f":"INDEX(Line548,1)","v":0},{"$f":"INDEX(Line549,1)","v":0},{"$f":"INDEX(Line550,1)","v":0},{"$f":"INDEX(Line551,1)","v":0},{"$f":"INDEX(Line552,1)","v":0},{"$f":"INDEX(Line553,1)","v":0},{"$f":"INDEX(Line554,1)","v":0},{"$f":"INDEX(Line555,1)","v":0},{"$f":"INDEX(Line556,1)","v":0},{"$f":"INDEX(Line557,1)","v":0},{"$f":"INDEX(Line558,1)","v":0},{"$f":"INDEX(Line559,1)","v":0},{"$f":"INDEX(Line560,1)","v":0},{"$f":"INDEX(Line561,1)","v":0},{"$f":"INDEX(Line562,1)","v":0},{"$f":"INDEX(Line563,1)","v":0},{"$f":"INDEX(Line564,1)","v":0},{"$f":"INDEX(Line565,1)","v":0},{"$f":"INDEX(Line566,1)","v":0},{"$f":"INDEX(Line569,1)","v":0},{"$f":"INDEX(Line570,1)","v":0},{"$f":"INDEX(Line571,1)","v":0},{"$f":"INDEX(Line572,1)","v":0},{"$f":"INDEX(Line573,1)","v":4},{"$f":"INDEX(Line574,1)","v":63.484170813081398},{"$f":"INDEX(Line575,1)","v":253.93668325232559},{"$f":"INDEX(Line576,1)","v":2},{"$f":"INDEX(Line577,1)","v":36.997398464518703},{"$f":"INDEX(Line578,1)","v":73.994796929037406},{"$f":"INDEX(Line579,1)","v":0},{"$f":"INDEX(Line580,1)","v":12.490785127130099},{"$f":"INDEX(Line581,1)","v":0},{"$f":"INDEX(Line582,1)","v":1976.92281083076},{"$f":"INDEX(Line583,1)","v":69.741114160925804},{"$f":"INDEX(Line584,1)","v":137.87279943748635},{"$f":"INDEX(Line585,1)","v":-1.48193672253884},{"$f":"INDEX(Line586,1)","v":-2.9296745109948077},{"$f":"INDEX(Line587,1)","v":462.87460510785456},{"$f":"INDEX(Line601,1)","v":0},{"$f":"INDEX(Line602,1)","v":0},{"$f":"INDEX(Line603,1)","v":0},{"$f":"INDEX(Line604,1)","v":327.58079849965094},{"$f":"INDEX(Line605,1)","v":145.3898232913277},{"$f":"INDEX(Line606,1)","v":300.76294216706026},{"$f":"INDEX(Line607,1)","v":302.13888072546132},{"$f":"INDEX(Line608,1)","v":53.381176729159279},{"$f":"INDEX(Line609,1)","v":51.796452911686728},{"$f":"INDEX(Line610,1)","v":0},{"$f":"INDEX(Line611,1)","v":13.85667178274484},{"$f":"INDEX(Line612,1)","v":0},{"$f":"INDEX(Line613,1)","v":0},{"$f":"INDEX(Line614,1)","v":1.6930165994223101},{"$f":"INDEX(Line615,1)","v":0},{"$f":"INDEX(Line616,1)","v":0},{"$f":"INDEX(Line617,1)","v":0},{"$f":"INDEX(Line618,1)","v":9.6357247626964337},{"$f":"INDEX(Line619,1)","v":211.5922202836467},{"$f":"INDEX(Line620,1)","v":12.401633833704235},{"$f":"INDEX(Line621,1)","v":-6.6765325131692759E-3},{"$f":"INDEX(Line622,1)","v":3.4532368562444252E-2},{"$f":"INDEX(Line623,1)","v":169.01403426292833},{"$f":"INDEX(Line624,1)","v":46.47499014095704},{"$f":"INDEX(Line625,1)","v":140.99407565269809},{"$f":"INDEX(Line626,1)","v":0},{"$f":"INDEX(Line627,1)","v":0},{"$f":"INDEX(Line628,1)","v":0},{"$f":"INDEX(Line629,1)","v":0},{"$f":"INDEX(Line630,1)","v":0},{"$f":"INDEX(Line631,1)","v":0},{"$f":"INDEX(Line632,1)","v":0},{"$f":"INDEX(Line633,1)","v":0},{"$f":"INDEX(Line634,1)","v":65.829766148781076},{"$f":"INDEX(Line635,1)","v":-1.8770724630503304},{"$f":"INDEX(Line636,1)","v":46.952164390333436},{"$f":"INDEX(Line637,1)","v":2.2410298519611325},{"$f":"INDEX(Line638,1)","v":-6.3900810683159767E-2},{"$f":"INDEX(Line639,1)","v":1.5983833479692759},{"$f":"INDEX(Line640,1)","v":0},{"$f":"INDEX(Line641,1)","v":17.505178806547942},{"$f":"INDEX(Line642,1)","v":17.472556546360519},{"$f":"INDEX(Line643,1)","v":18.341834110233549},{"$f":"INDEX(Line644,1)","v":54.262054495430249},{"$f":"INDEX(Line645,1)","v":54.160932942796244},{"$f":"INDEX(Line646,1)","v":56.855494767259842},{"$f":"INDEX(Line647,1)","v":0},{"$f":"INDEX(Line648,1)","v":1.6771691174974965},{"$f":"INDEX(Line649,1)","v":1.816379812879253},{"$f":"INDEX(Line650,1)","v":0},{"$f":"INDEX(Line651,1)","v":5.7095540193845495E-2},{"$f":"INDEX(Line652,1)","v":6.183466266555078E-2},{"$f":"INDEX(Line653,1)","v":0},{"$f":"INDEX(Line654,1)","v":0.59078850553007922},{"$f":"INDEX(Line655,1)","v":0.63414296405325665},{"$f":"INDEX(Line656,1)","v":0},{"$f":"INDEX(Line657,1)","v":1.8313093763061508},{"$f":"INDEX(Line658,1)","v":1.9656982915524521},{"$f":"INDEX(Line659,1)","v":0},{"$f":"INDEX(Line660,1)","v":0},{"$f":"INDEX(Line661,1)","v":0},{"$f":"INDEX(Line662,1)","v":0},{"$f":"INDEX(Line663,1)","v":0},{"$f":"INDEX(Line664,1)","v":0},{"$f":"INDEX(Line665,1)","v":0},{"$f":"INDEX(Line666,1)","v":0},{"$f":"INDEX(Line667,1)","v":0},{"$f":"INDEX(Line668,1)","v":0},{"$f":"INDEX(Line669,1)","v":0},{"$f":"INDEX(Line670,1)","v":0},{"$f":"INDEX(Line671,1)","v":0},{"$f":"INDEX(Line672,1)","v":0},{"$f":"INDEX(Line673,1)","v":0},{"$f":"INDEX(Line674,1)","v":0},{"$f":"INDEX(Line675,1)","v":0},{"$f":"INDEX(Line676,1)","v":0},{"$f":"INDEX(Line677,1)","v":0},{"$f":"INDEX(Line678,1)","v":0},{"$f":"INDEX(Line679,1)","v":0},{"$f":"INDEX(Line680,1)","v":0},{"$f":"INDEX(Line681,1)","v":0},{"$f":"INDEX(Line682,1)","v":0},{"$f":"INDEX(Line683,1)","v":0},{"$f":"INDEX(Line684,1)","v":0},{"$f":"INDEX(Line685,1)","v":0},{"$f":"INDEX(Line686,1)","v":0},{"$f":"INDEX(Line687,1)","v":0},{"$f":"INDEX(Line688,1)","v":0},{"$f":"INDEX(Line689,1)","v":0},{"$f":"INDEX(Line690,1)","v":0},{"$f":"INDEX(Line691,1)","v":0},{"$f":"INDEX(Line692,1)","v":0},{"$f":"INDEX(Line693,1)","v":0},{"$f":"INDEX(Line694,1)","v":0},{"$f":"INDEX(Line695,1)","v":0},{"$f":"INDEX(Line696,1)","v":2591.5277429916659},{"$f":"INDEX(Line697,1)","v":1.4522094029375101},{"$f":"INDEX(Line698,1)","v":3763.4409563459203},{"$f":"INDEX(Line699,1)","v":1.3588848083408001},{"$f":"INDEX(Line700,1)","v":2592.8866278000069},{"$f":"INDEX(Line701,1)","v":3764.7998411542612},{"$f":"INDEX(Line702,1)","v":1.6205541423750043},{"$f":"INDEX(Line703,1)","v":2.3529999007214131}]
[]
[{"$f":"\"Using \"&TEXT(CostYear,\"0000\")&\" Unit Costs\"","v":"Using 2021 Unit Costs"}]
["ID","RR","DIS","SG","FC","NC","OWN","WT","COM","SZ","L101","L102","L103","L104","L105","L106","L107","L108","L109","L110","L111","L201","L202","L203","L204","L205","L206","L207","L208","L209","L210","L211","L212","L213","L214","L215","L216","L217","L218","L219","L220","L221","L222","L223","L224","L225","L226","L227","L228","L229","L230","L231","L232","L233","L234","L235","L236","L237","L238","L239","L240","L241","L242","L243","L244","L245","L246","L247","L248","L250","L251","L252","L253","L254","L255","L256","L257","L258","L259","L260","L261","L262","L263","L264","L265","L266","L267","L268","L269","L270","L271","L272","L273","L274","L275","L276","L277","L278","L279","L280","L281","L282","L283","L284","L285","L286","L287","L288","L289","L290","L301","L302","L303","L304","L305","L306","L307","L308","L309","L310","L311","L312","L313","L314","L315","L316","L317","L318","L319","L320","L321","L322","L323","L324","L325","L326","L327","L328","L329","L330","L331","L332","L333","L334","L401","L402","L403","L404","L405","L406","L407","L408","L409","L410","L411","L412","L413","L414","L415","L416","L417","L418","L419","L420","L421","L422","L423","L424","L425","L426","L427","L428","L429","L430","L431","L432","L433","L434","L435","L436","L437","L438","L439","L440","L441","L442","L443","L444","L445","L446","L447","L448","L449","L450","L451","L452","L453","L454","L455","L456","L457","L458","L459","L460","L461","L462","L463","L464","L465","L466","L467","L468","L469","L470","L471","L472","L473","L474","L475","L476","L477","L478","L479","L480","L481","L482","L483","L484","L485","L486","L487","L488","L489","L490","L491","L492","L493","L494","L495","L496","L497","L498","L499","L499A","L499B","L499C","L499D","L501","L502","L503","L504","L505","L506","L507","L508","L509","L510","L511","L512","L513","L514","L515","L516","L517","L518","L519","L520","L521","L522","L523","L524","L525","L526","L527","L528","L529","L530","L531","L532","L533","L534","L535","L536","L537","L540","L541","L542","L543","L544","L545","L546","L547","L548","L549","L550","L551","L552","L553","L554","L555","L556","L557","L558","L559","L560","L561","L562","L563","L564","L565","L566","L569","L570","L571","L572","L573","L574","L575","L576","L577","L578","L579","L580","L581","L582","L583","L584","L585","L586","L587","L601","L602","L603","L604","L605","L606","L607","L608","L609","L610","L611","L612","L613","L614","L615","L616","L617","L618","L619","L620","L621","L622","L623","L624","L625","L626","L627","L628","L629","L630","L631","L632","L633","L634","L635","L636","L637","L638","L639","L640","L641","L642","L643","L644","L645","L646","L647","L648","L649","L650","L651","L652","L653","L654","L655","L656","L657","L658","L659","L660","L661","L662","L663","L664","L665","L666","L667","L668","L669","L670","L671","L672","L673","L674","L675","L676","L677","L678","L679","L680","L681","L682","L683","L684","L685","L686","L687","L688","L689","L690","L691","L692","L693","L694","L695","L696","L697","L698","L699","L700","L701","L702","L703"]

{"sheet":"URCSInputs","index":5,"n_rows":84,"n_cols":52,"rows_kept":84,"cut":false,"hidden":false,"merged":[]}
["URCS Railroads",null,null,null,"URCS Segment Types",null,null,null,null,"URCS Car Types",null,null,null,null,"URCS STCC Types",null,null,null,null,"URCS Ownership Types",null,null,null,"URCS Shipment Sizes",null,null,null,null,"Refrigerated Trailer",null,null,"URCS TOFC Plans/Ownership & Protective Service Factors/Pickup & Delivery Factors (by Seg Type)",null,null,null,null,null,null,null,null,null,null,"URCS TOFC Service Codes",null,null,null,"Make Whole Adjustment Factors (Reductions)"]
["Railroad\nNumber","Railroad","Description",null,"Segment\nType","Description","L250","L307",null,"Car\nIndex","Sch 710\nLine\nNumber","Description","Car\nIndex",null,"STCC","Description","STCC-Description","STCC\nIndex",null,"Owner\nCode","Description","Owner\nIndex",null,"Size\nCode","Shipment Size","Description","Starts At",null,"Option","Description",null,"Plan\nCode","Title","Description","O&PS","OT","OD","RT","RD","IA","IR",null,"Service\nCode","Description","Plan\nCode",null,"LINE","DESCRIPTION","Single","Multi","Unit","Intermodal"]
[777,"BNSF","BNSF",null,"OT","Originate and Terminate",2,0,null,1,36,"Plain Box Cars 40'",1,null,"01000","Farm Products","01 All Farm Products",1,null,"P","Private",1,null,1,"Single","Single Car",1,null,"N","No",null,0,"Plan 0","Not Intermodal",0,0,0,0,0,0,0,null,"A",{"$f":"\"Plan \"&AS3","v":"Plan 1"},1,null,"L257","UC per CLOT Cler-OPR",0,"75%/25%","75%/25%","75%/25%"]
[103,"CN","CN",null,"OD","Originate and Deliver",1,1,null,2,37,"Plain Box Cars 50' and Longer",2,null,"0113","Grains","0113 Grains",2,null,"R","Railroad",2,null,2,"Multi","Multi-Car",6,null,"Y","Yes",null,1,"Plan 1","Shipper Trailers/No P or D",0,0,0,0,0,0,0,null,"B",{"$f":"\"Plan \"&AS4","v":"Plan 2"},2,null,"L301","SEM per Industry switch event",0,0.5,0.75,0.75]
[105,"CP","CP",null,"RT","Receive and Terminate",1,1,null,3,38,"Equipped Box Cars",3,null,"01195","Potatoes; Other than Sweet","01195 Potatoes; Other than Sweet",3,null,"T","TrailerTrain",3,null,3,"Unit","Unit Train",50,null,null,null,null,2,"Plan 2","Railroad trailers/P & D",1,1,1,1,0,0,0,null,"C","Plan 2.25",2.25,null,"L302","SEM per Interchange switch event",0,0,0.5,0.5]
[712,"CSXT","CSXT",null,"RD","Receivd and Deliver",0,2,null,4,39,"Plain Gondola Cars",4,null,"012","Fresh Fruits/Tree Nuts","012 Fresh Fruits/Tree Nuts",4,null,null,null,null,null,4,"Intermodal","Intermodal",1,null,null,null,null,2.25,"Plan 2.25","Railroad trailers/P or D",1,0.5,1,0,0,0,0,null,"D","Plan 5.1",5.0999999999999996,null,"L303","SEM per I&I train switch event",0,0,1,1]
[400,"KCS","KCS",null,"IA","Intra-Terminal",2,1,null,5,40,"Equipped Gondola Cars",5,null,"013","Fresh Vegetables","013 Fresh Vegetables",5,null,null,null,null,null,null,null,null,null,null,null,null,null,2.5,"Plan 2.5","Railroad trailers/No P or D",1,0,0,0,0,0,0,null,"E","Plan 5.2",5.2,null,"L325","SEM per Intraterminal switch",0,0.5,0.875,0.875]
[555,"NS","NS",null,"IR","Inter-Terminal",1,1,null,6,41,"Covered Hopper Cars",6,null,"01","Other Farm Products","01 Other Farm Products",6,null,null,null,null,null,null,"Unit","New Unit Train",75,null,null,null,null,3,"Plan 3","Shipper trailers/No P or D",0,0,0,0,0,0,0,null,"F","Plan 5.3",5.3,null,"L326","SEM per Interterminal switch",0,0.5,0.875,0.875]
[802,"UP","UP",null,null,null,null,null,null,7,42,"Open Top Hopper Cars-General Service",7,null,"10","Metallic Ores","10 Metallic Ores",7,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"Plan 4-RoadRailer","RoadRailer/No P or D",0,0,0,0,0,0,0,null,"G","Plan 5.4",5.4,null,"L419","CM(Y)/Industry switch (L-E)",0,0.5,0.5,0.5]
[900004,"EAST","EAST",null,"RT","Receive and Terminate",null,null,null,8,43,"Open Top Hopper Cars-Special Service",8,null,"11","Coal","11 Coal",8,null,null,null,null,null,null,null,null,null,null,null,null,null,5.0999999999999996,"Plan 5.1","Railroad Trailers/No P or D",1,0,0,0,0,0,0,null,"H","Plan 1",1,null,"L420","CM(Y)/Interchange switch (L-E)",0,0,0.5,0.5]
[900007,"WEST","WEST",null,"IR","Inter-Terminal",null,null,null,9,44,"Refrigerator Cars-Mechanical",9,null,"14","Non-Metallic Minerals","14 Non-Metallic Minerals",9,null,null,null,null,null,null,null,null,null,null,null,null,null,5.2,"Plan 5.2","Railroad Trailers/D but not P",1,0.5,0,1,0,0,0,null,"I","Plan 5.5",5.5,null,"L421","CM(Y)/I&I train switch (L-E)",0,0,1,1]
[null,null,null,null,null,null,null,null,null,10,45,"Refrigerator Cars-Non-Mechanical",10,null,"20000","Food & Kindred Products","20 All Food & Kindred Products",10,null,null,null,null,null,null,null,null,null,null,null,null,null,5.3,"Plan 5.3","Shipper Trailers/P & D",0,1,1,1,0,0,0,null,"K","Plan 5.3",5.3,null,"L443","CD(Y)/Industry switch (L or E)",0,0.5,0.5,0.5]
[null,null,null,null,null,null,null,null,null,11,46,"Flat Cars TOFC/COFC",11,null,"2011","Fresh Meats","2011 Fresh Meats",11,null,null,null,null,null,null,null,null,null,null,null,null,null,5.4,"Plan 5.4","Shipper Trailers/P but not D",0,0.5,1,0,0,0,0,null,"L","Plan 5.4",5.4,null,"L444","CD(Y)/Interchange swt (L or E)",0,0,0.5,0.5]
[null,null,null,null,null,null,null,null,null,12,47,"Flat Cars-Multi-Level",12,null,"202","Dairy Products","202 Dairy Products",12,null,null,null,null,null,null,null,null,null,null,null,null,null,5.5,"Plan 5.5","Shipper Trailers/D but not P",0,0.5,0,1,0,0,0,null,"M","Plan 1",1,null,"L445","CD(Y)/I&I train switch (L or E)",0,0,1,1]
[null,null,null,null,null,null,null,null,null,13,48,"Flat Cars-General Service",13,null,"203","Canned Fruits/Vegetables","203 Canned Fruits/Vegetables",13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N","Plan 5.5",5.5,null,"L449","CD(Y)-per Loading & Unloading for Industry switch",0,0.5,0.5,0.5]
[null,null,null,null,null,null,null,null,null,14,49,"Flat Cars-Other",14,null,"204","Grain Mill Products","204 Grain Mill Products",14,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O","Plan 5.3",5.3]
[null,null,null,null,null,null,null,null,null,15,50,"Tank Cars-Under 22000 Gallons",15,null,"2041","Flour","2041 Flour",15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P","Plan 5.4",5.4]
[null,null,null,null,null,null,null,null,null,16,51,"Tank Cars-22000 Gallons and Over",16,null,"2042","Prepared Feeds","2042 Prepared Feeds",16,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Q","Plan 1",1]
[null,null,null,null,null,null,null,null,null,17,52,"All Other Freight Cars",17,null,"2043","Cereal Preparations","2043 Cereal Preparations",17,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R","Plan 5.5",5.5]
[null,null,null,null,null,null,null,null,null,null,54,"All Other Freight Cars",17,null,"2044","Milled Rice/Flour/Meal","2044 Milled Rice/Flour/Meal",18,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TCS","RoadRailer",4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2045","Prepared Flour","2045 Prepared Flour",19,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X","Plan 1",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2046","Corn Milling Products","2046 Corn Milling Products",20]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2062","Refined Sugar","2062 Refined Sugar",21]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20821","Beer/Ale","20821 Beer/Ale",22]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2084","Wines/Brandy Spirits","2084 Wines/Brandy Spirits",23]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20851","Whiskey/Blended Liquors","20851 Whiskey/Blended Liquors",24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"209","Misc. Food Preparations","209 Misc. Food Preparations",25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"20","Other Food & Kindred Products","20 Other Food & Kindred Products",26]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"21","Tobacco Products","21 Tobacco Products",27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24000","Lumber & Wood Products","24 All Lumber & Wood Products",28]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2421","Lumber/Dimension Stock","2421 Lumber/Dimension Stock",29]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2432","Plywood or Veneer","2432 Plywood or Veneer",30]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"24","Other Lumber & Wood Products","24 Other Lumber & Wood Products",31]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"25","Furniture & Fixtures","25 Furniture & Fixtures",32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26000","Pulp & Paper Products","26 All Pulp & Paper Products",33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26211","Newsprint","26211 Newsprint",34]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26213","Printing Paper","26213 Printing Paper",35]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"263","Paperboard/Fibreboard","263 Paperboard/Fibreboard",36]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"264","Conv Paper/Paperboard","264 Conv Paper/Paperboard",37]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26471","Sanitary Tissues","26471 Sanitary Tissues",38]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"26","Other Paper Products","26 Other Paper Products",39]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"28000","Chemicals","28 All Chemicals",40]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"281","Industrial Chemicals","281 Industrial Chemicals",41]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2812","Potassium or Sodium","2812 Potassium or Sodium",42]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"282","Syn Fibers/Resins/Rubber","282 Syn Fibers/Resins/Rubber",43]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"289","Misc Chemical Products","289 Misc Chemical Products",44]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"28","Other Chemicals","28 Other Chemicals",45]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"29","Petroleum or Coal Products","29 Petroleum or Coal Products",46]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30000","Rubber & Misc. Plastics","30 All Rubber & Misc. Plastics",47]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"301","Rubber Tires/Innertubes","301 Rubber Tires/Innertubes",48]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"30","Other Rubber Products","30 Other Rubber Products",49]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32000","Stone; Clay; Glass","32 All Stone; Clay; Glass",50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"321","Flat Glass","321 Flat Glass",51]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3295","Non-Metallic Minerals/Earth","3295 Non-Metallic Minerals/Earth",52]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"32","Other Stone Products","32 Other Stone Products",53]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"33000","Primary Metal Products","33 All Primary Metal Products",54]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3312","Iron/Steel Products","3312 Iron/Steel Products",55]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3352","Aluminum Shapes","3352 Aluminum Shapes",56]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"33","Other Primary Metal Products","33 Other Primary Metal Products",57]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34000","Fabricated Metal Products","34 All Fabricated Metal Products",58]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"344","Fabric. Structural Metal","344 Fabric. Structural Metal",59]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"34","Other Fab. Metal Products","34 Other Fab. Metal Products",60]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"35000","Non-Electrical Machinery","35 All Non-Electrical Machinery",61]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"351","Engines/Turbines","351 Engines/Turbines",62]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"352","Farm Machinery","352 Farm Machinery",63]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"353","Constr./Mining/Hand Machinery","353 Constr./Mining/Hand Machinery",64]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"35","Other Non-Elec. Machinery","35 Other Non-Elec. Machinery",65]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36000","Electrical Machinery","36 All Electrical Machinery",66]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"361","Electrical Trans Equipment","361 Electrical Trans Equipment",67]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"363","Household Appliances","363 Household Appliances",68]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"365","Radio or TV Sets","365 Radio or TV Sets",69]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"36","Other Electrical Machinery","36 Other Electrical Machinery",70]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"37000","Transportation Equipment","37 All Transportation Equipment",71]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"37111","Automobiles","37111 Automobiles",72]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"37112","Trucks","37112 Trucks",73]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3714","Motor Vehicle Parts","3714 Motor Vehicle Parts",74]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"37","Other Trans. Equipment","37 Other Trans. Equipment",75]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"44","Freight Forwarder Traffic","44 Freight Forwarder Traffic",76]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"45","Shipper Assocation Traffic","45 Shipper Assocation Traffic",77]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"46000","Misc. Mixed Shipments","46 All Misc. Mixed Shipments",78]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"461","Misc. Mixed Shipments not TOFC","461 Misc. Mixed Shipments not TOFC",79]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"46","Other Misc. Mixed Shipments","46 Other Misc. Mixed Shipments",80]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"48","Hazardous Materials","48 Hazardous Materials",81]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Other","Other Commodities","Other Commodities",82]

{"sheet":"RailroadUnitCostXML","index":6,"n_rows":8759,"n_cols":22,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["VLOOKUP","Railroad","RR_Id","eCode","eCode_id","eTitle_and_Desc",2006,2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021]
[{"$f":"B2&\"-\"&D2","v":"BNSF-E1L101C1"},"BNSF",4,"E1L101C1",1,"Gross Ton Mile (GTM), OPR Expense",2.0089314784854698E-3,2.3040438536554601E-3,2.9324109200388202E-3,2.1163716446608301E-3,2.39365547895432E-3,2.9804133810102901E-3,3.0158874578774001E-3,2.9608923941850701E-3,2.8802831657230902E-3,2.1938748409669698E-3,2.0619653776254299E-3,2.2875185660923502E-3,2.61824008411728E-3,2.5035350773788198E-3,2.0697448295868498E-3,2.3882066605848801E-3]
["BNSF-E1L101C2","BNSF",4,"E1L101C2",2,"Gross Ton Mile (GTM), DRL Expense",5.3720513824373505E-4,5.9063924709335002E-4,6.1291037127375603E-4,7.2778953472152396E-4,6.9272494874894597E-4,6.9156155223026904E-4,6.9802848156541597E-4,6.9240597076713995E-4,7.1664166171103705E-4,7.1203336167843204E-4,8.2524604248590398E-4,8.7307903842902897E-4,7.8821022222056304E-4,8.5009386346942704E-4,9.5409189184198298E-4,8.9948718216224896E-4]
["BNSF-E1L101C3","BNSF",4,"E1L101C3",3,"Gross Ton Mile (GTM), ROI Expense",9.5000385772436901E-4,1.1606037151068399E-3,1.24599656555802E-3,1.2536674039438399E-3,1.2975656427442999E-3,1.38929369859397E-3,1.39219441916794E-3,1.52681884355843E-3,1.55592430382967E-3,1.6048617323604201E-3,1.72626436570203E-3,1.8649967130101399E-3,2.16171862521105E-3,1.71253827493554E-3,1.60782258878217E-3,2.0079636625825498E-3]
["BNSF-E1L102C1","BNSF",4,"E1L102C1",4,"Car Mile (CM) - Other Than Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L102C2","BNSF",4,"E1L102C2",5,"Car Mile (CM) - Other Than Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L102C3","BNSF",4,"E1L102C3",6,"Car Mile (CM) - Other Than Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L103C1","BNSF",4,"E1L103C1",7,"Train Mile (TM) - Other Than Crew, OPR Expense",0.25418618321418801,0.27546173334121699,0.27363562583923301,0.30975601077079801,0.307114958763123,0.325593322515488,0.30279088020324701,0.283287763595581,0.35175490379333502,0.83862446317728701,0.70256708704005699,0.62696955769911,0.76820804863247605,0.78072203185618605,0.785545665158766,0.61492320619726504]
["BNSF-E1L103C2","BNSF",4,"E1L103C2",8,"Train Mile (TM) - Other Than Crew, DRL Expense",8.1887468695640596E-4,7.1629218291491303E-4,1.67868903372437E-3,3.64962848834693E-3,3.7771016359329202E-3,4.1677993722259998E-3,3.7185337860137198E-3,2.11753253825009E-3,1.21776565720211E-5,-1.8820604865578199E-3,-1.6774035456219201E-3,-1.2868115100934201E-3,-1.31468927665879E-3,-1.2940539619659E-3,-7.64028899771709E-4,-9.1689935624480903E-4]
["BNSF-E1L103C3","BNSF",4,"E1L103C3",9,"Train Mile (TM) - Other Than Crew, ROI Expense",6.69637636747211E-4,1.2896708212792899E-2,7.9512344673275896E-3,5.81257371231914E-3,3.1385833863168998E-3,2.2723088040947901E-3,1.13878841511905E-3,1.79311924148351E-3,2.0813113078474998E-3,2.43011282609877E-3,2.86778995208625E-3,2.93916302719586E-3,3.3621633266563799E-3,2.7303525874667902E-3,2.6167309049405498E-3,3.1631866242454302E-3]
["BNSF-E1L104C1","BNSF",4,"E1L104C1",10,"Train Mile (TM) - Crew, OPR Expense",8.3105716705322301,8.6205883026122994,8.7481784820556605,8.7459325790405291,9.2477655410766602,9.4585065841674805,9.9785795211791992,10.8892154693604,12.069828033447299,12.7928007412941,12.4790105727851,12.1421115173306,12.499661926206601,12.9507069561566,12.3234507490479,11.1211751898225]
["BNSF-E1L104C2","BNSF",4,"E1L104C2",11,"Train Mile (TM) - Crew, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L104C3","BNSF",4,"E1L104C3",12,"Train Mile (TM) - Crew, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L105C1","BNSF",4,"E1L105C1",13,"Locomotive Unit Mile (LUM), OPR Expense",3.93920826911926,4.8817410469055202,6.4505090713501003,4.2912654876709002,5.1080245971679696,6.5487413406372097,6.5461859703064,6.3942117691040004,6.4031667709350604,4.2173262175974804,3.6111300301262301,4.1608983191367299,5.0024004488266298,4.7735038786358697,3.7084214589642399,4.7437888942013497]
["BNSF-E1L105C2","BNSF",4,"E1L105C2",14,"Locomotive Unit Mile (LUM), DRL Expense",0.43842065334320102,0.57568812370300304,0.61755269765853904,0.74752461910247803,0.72361963987350497,0.76605671644210804,0.77337259054184004,0.79367935657501198,0.88875722885131803,0.82482991025660402,0.89898351171151003,0.87906566095275296,0.69983311212007904,0.76141733721286997,0.80706906951548496,0.75468673365679795]
["BNSF-E1L105C3","BNSF",4,"E1L105C3",15,"Locomotive Unit Mile (LUM), ROI Expense",0.246301040053368,0.34296154975891102,0.38371667265892001,0.42450755834579501,0.50859355926513705,0.57347887754440297,0.60040807723999001,0.61288446187973,0.65904039144516002,0.62321077261412805,0.58836537081868201,0.63528707690697905,0.74355477474155396,0.58145874177579004,0.53539992116474999,0.67198965900097796]
["BNSF-E1L106C1","BNSF",4,"E1L106C1",16,"CLOR (Carloads Handled) - Other, OPR Expense",1.15001821517944,1.1403715610504199,1.2115781307220499,1.5778839588165301,1.9771927595138501,0.94258588552474998,1.1185601949691799,1.06150686740875,1.2976329326629601,1.0861363012707099,1.0006193787720099,0.94381559454884301,1.0046017776184699,1.1769049556305,1.2815281587569201,1.0744077722101399]
["BNSF-E1L106C2","BNSF",4,"E1L106C2",17,"CLOR (Carloads Handled) - Other, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L106C3","BNSF",4,"E1L106C3",18,"CLOR (Carloads Handled) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L107C1","BNSF",4,"E1L107C1",19,"CLOR (Carloads Handled) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L107C2","BNSF",4,"E1L107C2",20,"CLOR (Carloads Handled) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L107C3","BNSF",4,"E1L107C3",21,"CLOR (Carloads Handled) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L108C1","BNSF",4,"E1L108C1",22,"CLOT (Carloads Orig Or Term) - Other, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L108C2","BNSF",4,"E1L108C2",23,"CLOT (Carloads Orig Or Term) - Other, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L108C3","BNSF",4,"E1L108C3",24,"CLOT (Carloads Orig Or Term) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L109C1","BNSF",4,"E1L109C1",25,"CLOT (Carloads Orig Or Term) - Clerical, OPR Expense",7.4903440475463903,7.3709878921508798,8.2239398956298793,8.0509519577026403,8.4442567825317401,7.2944040298461896,6.6167464256286603,5.9643759727478001,6.8612837791442898,6.5117306180843304,6.4062629635156902,5.6134594827256103,4.5392726444615299,5.0891858712551903,4.91559088034988,3.7761907297556601]
["BNSF-E1L109C2","BNSF",4,"E1L109C2",26,"CLOT (Carloads Orig Or Term) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L109C3","BNSF",4,"E1L109C3",27,"CLOT (Carloads Orig Or Term) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L110C1","BNSF",4,"E1L110C1",28,"Car Mile (CM) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L110C2","BNSF",4,"E1L110C2",29,"Car Mile (CM) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L110C3","BNSF",4,"E1L110C3",30,"Car Mile (CM) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L111C1","BNSF",4,"E1L111C1",31,"Switch Engine Minutes (SEM), OPR Expense",4.7231860160827601,4.6325778961181596,5.4745249748229998,5.2134628295898402,5.5093078613281303,5.7684822082519496,6.2547802925109899,6.1597466468811,6.3290491104126003,5.96245816862361,6.0704254869485901,5.9583728976275703,6.3140462901884398,6.3380346049388097,6.1008788808867198,6.1894618192582103]
["BNSF-E1L111C2","BNSF",4,"E1L111C2",32,"Switch Engine Minutes (SEM), DRL Expense",0.493460923433304,0.58894044160842896,0.74603158235549905,1.0690611600875899,1.12371242046356,0.77158719301223799,0.79409247636795,0.77324205636978105,0.79969143867492698,0.82226425247591595,0.94524714631726403,1.13239433665358,1.1385226032098099,1.2289398035271499,1.5259200236725201,1.5815611560454901]
["BNSF-E1L111C3","BNSF",4,"E1L111C3",33,"Switch Engine Minutes (SEM), ROI Expense",1.5864446163177499,1.94580018520355,2.24503469467163,2.62610530853271,2.84949851036072,2.7268972396850599,2.7681002616882302,3.2804288864135698,3.5537765026092498,3.9531062916369,4.4065256126857699,5.0026008660476,5.6188216619442901,4.3958322904592899,4.4410196793770398,5.9857135095793401]
["BNSF-E1L112C1","BNSF",4,"E1L112C1",34,"Ton Miles In Lake Transfer Service, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L112C2","BNSF",4,"E1L112C2",35,"Ton Miles In Lake Transfer Service, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L112C3","BNSF",4,"E1L112C3",36,"Ton Miles In Lake Transfer Service, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L113C1","BNSF",4,"E1L113C1",37,"Tons Handled at Coal Terminals, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L113C2","BNSF",4,"E1L113C2",38,"Tons Handled at Coal Terminals, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L113C3","BNSF",4,"E1L113C3",39,"Tons Handled at Coal Terminals, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L114C1","BNSF",4,"E1L114C1",40,"Tons Handled at Ore Terminals, OPR Expense",0.70958721637725797,0.78982639312744096,0.87036168575286899,1.60781121253967,0.490983545780182,0.58150631189346302,0.46581920981407199,0.54515963792800903,0.35017040371894798,0.32622483607473901,0.32558361439962002,0.214726207943891,0.32020629803918599,0.32788997585231999,0.39664285523704101,0.24659538482673601]
["BNSF-E1L114C2","BNSF",4,"E1L114C2",41,"Tons Handled at Ore Terminals, DRL Expense",8.4470231086015701E-3,8.8303089141845703E-3,1.01442262530327E-2,6.3879653811454801E-2,1.7069080844521502E-2,1.40826236456633E-2,2.2141432389617001E-2,3.8088072091340998E-2,6.0593601316213601E-2,7.2918940799596002E-2,9.7594806843488299E-2,7.0152169493040595E-2,8.4327907786118303E-2,9.9854366374076006E-2,0.16354522912411701,9.24881129558323E-2]
["BNSF-E1L114C3","BNSF",4,"E1L114C3",42,"Tons Handled at Ore Terminals, ROI Expense",6.3781961798667894E-2,7.3119163513183594E-2,4.2722243815660498E-2,0.18948982656002,5.2864301949739498E-2,4.3120030313730198E-2,9.9125050008296994E-2,0.175754249095917,0.291424840688705,0.26064075427100902,0.319868737656059,0.24373943850082999,0.37797578473749299,0.32623657302574,0.453038510910176,0.33526974142518801]
["BNSF-E1L115C1","BNSF",4,"E1L115C1",43,"Tons Handled at Other Marine Terminals, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L115C2","BNSF",4,"E1L115C2",44,"Tons Handled at Other Marine Terminals, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L115C3","BNSF",4,"E1L115C3",45,"Tons Handled at Other Marine Terminals, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L116C1","BNSF",4,"E1L116C1",46,"Refrigerated Car Miles, OPR Expense",0.27648472785949701,0.27088436484336897,0.37807792425155601,0.18407942354679099,0.226117223501205,0.30826291441917397,0.30472132563590998,0.26998123526573198,0.348512202501297,0.240645151401957,0.189559110962157,0.22233919295747301,0.26018388627523298,0.248981223329413,0.208344028512227,0.23017327781484501]
["BNSF-E1L116C2","BNSF",4,"E1L116C2",47,"Refrigerated Car Miles, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L116C3","BNSF",4,"E1L116C3",48,"Refrigerated Car Miles, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L117C1","BNSF",4,"E1L117C1",49,"Protective Service Reefer TCU Days, OPR Expense",6.94605708122253E-2,0,0.149278938770294,0.14386451244354201,8.4869399666786194E-2,5.16879488714039E-4,4.5138774439692497E-3,1.6021349001675801E-3,1.84295643121004E-2,1.6264702772292802E-2,9.5092503573923001E-3,1.2469360813020899E-2,1.41356141961016E-2,1.09881611955713E-2,1.43779338039694E-2,6.2275647674312297E-2]
["BNSF-E1L117C2","BNSF",4,"E1L117C2",50,"Protective Service Reefer TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L117C3","BNSF",4,"E1L117C3",51,"Protective Service Reefer TCU Days, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L118C1","BNSF",4,"E1L118C1",52,"Refrigerated TCU Days, OPR Expense",4.2830519676208496,4.2289948463439897,3.6201353073120099,2.6797022819518999,2.1087722778320299,0.99081373214721702,0.484929829835892,4.53827194869518E-2,1.3888046145439099E-2,0,0,0,0,0,0,0]
["BNSF-E1L118C2","BNSF",4,"E1L118C2",53,"Refrigerated TCU Days, DRL Expense",2.1185894012451199,1.77333760261536,1.46590876579285,1.30994129180908,0.822340548038483,0.26109907031059298,0.164287835359573,6.9255502894520803E-3,2.2424198687076599E-3,0,0,0,0,0,0,0]
["BNSF-E1L118C3","BNSF",4,"E1L118C3",54,"Refrigerated TCU Days, ROI Expense",7.6807864010334001E-2,0.103843607008457,9.5884159207344097E-2,5.7209864258766202E-2,4.2221162468195003E-2,1.8210859969258301E-2,8.8190790265798603E-3,8.2011986523866697E-4,0.243569001555443,0.20073104775507999,0.16756315914372599,0.161925542904754,0.17196610398943099,0.122904460196988,8.4762799749217299E-2,8.7004556464387803E-2]
["BNSF-E1L119C1","BNSF",4,"E1L119C1",55,"Other (Non-Refrigerated) TCU Days, OPR Expense",1.59096562862396,1.65999460220337,1.4944880008697501,1.25887882709503,1.34877705574036,1.71878254413605,1.22420942783356,0.85226374864578203,0.83263444900512695,0.73430934161585604,0.70649662398805102,0.61643658740456897,0.67535965352912297,0.64925628068618202,0.59788461229538603,0.68425595768384595]
["BNSF-E1L119C2","BNSF",4,"E1L119C2",56,"Other (Non-Refrigerated) TCU Days, DRL Expense",0.48510709404945401,1.44212734699249,0.97311735153198198,0.81361931562423695,0.58430540561676003,0.46120405197143599,0.43421074748039201,0.14545731246471399,0.138653084635735,0.11923792295461499,9.7184154963033606E-2,0.146822427869339,0.126467384932168,0.16777527419036001,0.14492840424164199,0.13221993679603]
["BNSF-E1L119C3","BNSF",4,"E1L119C3",57,"Other (Non-Refrigerated) TCU Days, ROI Expense",4.4161163270473501E-2,5.0274748355150202E-2,6.0378450900316197E-2,5.6596677750349003E-2,6.4583048224449199E-2,7.0352151989936801E-2,6.15606531500816E-2,5.3918119519949001E-2,1.3499283231794799E-2,1.07136995679336E-2,9.1455275709980202E-3,9.5463314279139594E-3,1.21719569148583E-2,8.8151258582399496E-3,7.1757559755743997E-3,9.7113495566490803E-3]
["BNSF-E1L120C1","BNSF",4,"E1L120C1",58,"TCUs Loaded And Unloaded (L&UL), OPR Expense",46.688125610351598,51.163604736328097,52.699996948242202,46.863800048828097,48.046916961669901,44.695877075195298,42.801162719726598,41.7947807312012,43.499607086181598,42.140627491935099,42.489446881047897,48.124585032165399,50.565811752191699,52.806861595067602,51.504783708127,57.005005307787599]
["BNSF-E1L120C2","BNSF",4,"E1L120C2",59,"TCUs Loaded And Unloaded (L&UL), DRL Expense",1.21742975711823,1.6337205171585101,1.88110339641571,2.81920266151428,3.1951918601989702,3.12893867492676,3.2386023998260498,3.2793567180633501,3.3692531585693399,3.2652405913415699,3.5110957862174699,3.5856876137839002,3.6114825312354899,4.0444138929835898,4.0163649224733504,4.1773977143836696]
["BNSF-E1L120C3","BNSF",4,"E1L120C3",60,"TCUs Loaded And Unloaded (L&UL), ROI Expense",3.1484355926513699,5.2830214500427202,6.4845247268676802,8.8560342788696307,8.6742820739746094,9.0365924835205096,8.0589504241943395,8.6380872726440394,8.1470317840576207,7.6285920495105799,7.1752217985406999,8.0840322712075494,10.071355296120601,8.4543717077186198,7.1310392361461901,9.9724464113890701]
["BNSF-E1L121C1","BNSF",4,"E1L121C1",61,"MVUs Loaded And Unloaded (L&UL), OPR Expense",7.8900442123413104,9.9354877471923793,16.219396591186499,25.351926803588899,22.114704132080099,19.313922882080099,17.05837059021,17.312868118286101,15.0091390609741,16.793727459612001,16.2010019196412,15.9967386674448,18.306414575495101,20.1957063896037,19.9123015426199,20.464365047078299]
["BNSF-E1L121C2","BNSF",4,"E1L121C2",62,"MVUs Loaded And Unloaded (L&UL), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L121C3","BNSF",4,"E1L121C3",63,"MVUs Loaded And Unloaded (L&UL), ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L122C1","BNSF",4,"E1L122C1",64,"TCUs Picked Up and Delivered (PU&D), OPR Expense",169.71723937988301,266.7109375,208.66297912597699,125.599411010742,119.166702270508,187.59291076660199,142.81593322753901,225.74824523925801,285.31384277343801,272.56433716503801,271.90895769496399,353.741372309714,362.77217574894001,274.34565717017801,279.64204564986699,366.39306323879799]
[{"$f":"B66&\"-\"&D66","v":"BNSF-E1L122C2"},"BNSF",4,"E1L122C2",65,"TCUs Picked Up and Delivered (PU&D), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L122C3","BNSF",4,"E1L122C3",66,"TCUs Picked Up and Delivered (PU&D), ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L201C1","BNSF",4,"E1L201C1",67,"CM(R), OPR Expense, Railroad-Owned, BOX - 40 FT",0.104918107390404,9.6362285315990406E-2,4.5397792011499398E-2,4.5191854238510097E-2,4.2305193841457402E-2,4.6553149819374098E-2,5.0679888576269198E-2,5.4562639445066501E-2,5.88250197470188E-2,6.5597652344403304E-2,4.4763356593085703E-2,4.0582031445942801E-2,4.3268156317810301E-2,5.7697065097608399E-2,6.2124162905748501E-2,5.2087661138881899E-2]
["BNSF-E1L201C2","BNSF",4,"E1L201C2",68,"CM(R), DRL Expense, Railroad-Owned, BOX - 40 FT",6.2776915729045896E-2,6.3799053430557306E-2,6.7715801298618303E-2,5.89359998703003E-2,5.0515949726104702E-2,4.1969150304794298E-2,3.8883421570062603E-2,6.2181185930967303E-2,4.4067665934562697E-2,5.4943280345509701E-2,3.5868224964049199E-2,1.9652390260874199E-2,3.0752206324677098E-2,3.6078214874626098E-2,4.2049773188892803E-2,2.9546910634952999E-2]
["BNSF-E1L201C3","BNSF",4,"E1L201C3",69,"CM(R), ROI Expense, Railroad-Owned, BOX - 40 FT",1.29188010469079E-2,1.8455408513546E-2,1.9433075562119501E-2,1.48332142271101E-3,1.3214916689321401E-3,1.21498294174671E-3,1.3231815537437801E-3,1.8560908501967801E-3,1.4540656702592999E-3,1.6876993718448099E-3,9.9855843994216503E-4,1.2670096476274901E-4,1.0966838619923399E-3,9.5432908546670703E-4,1.0688753850684599E-3,1.1469334900699501E-3]
["BNSF-E1L201C4","BNSF",4,"E1L201C4",70,"CM(Y), OPR Expense, Railroad-Owned, BOX - 40 FT",0.27278730273246798,0.25054204463958701,0.118034332990646,0.11749872565269499,0.10999348014593099,0.121038287878036,0.13176761567592599,0.141862973570824,0.15294525027275099,0.17055389609544799,0.116384727142023,0.105513281759451,0.11249720642630701,0.150012369253782,0.16152282355494599,0.13542791896109299]
["BNSF-E1L201C5","BNSF",4,"E1L201C5",71,"CM(Y), DRL Expense, Railroad-Owned, BOX - 40 FT",0.16322024166584001,0.16587737202644301,0.17606118321418801,0.15323376655578599,0.131341353058815,0.10911958664655701,0.101096875965595,0.16167120635509499,0.114575766026974,0.142852528898325,9.3257384906528198E-2,5.1096214678273001E-2,7.99557364441605E-2,9.3803358674028101E-2,0.109329410291122,7.6821967650877801E-2]
["BNSF-E1L201C6","BNSF",4,"E1L201C6",72,"CM(Y), ROI Expense, Railroad-Owned, BOX - 40 FT",3.3588919788599E-2,4.7983981668949099E-2,5.0526060163974797E-2,3.85664193890989E-3,3.4358762204647099E-3,3.1589476857334401E-3,3.4402725286781801E-3,4.8258434981107703E-3,3.7805703468620799E-3,4.3880183667964999E-3,2.5962519438496399E-3,3.29422508383147E-4,2.8513780411800901E-3,2.48125562221344E-3,2.7790760011780001E-3,2.9820270741818598E-3]
["BNSF-E1L201C7","BNSF",4,"E1L201C7",73,"CD(R), OPR Expense, Railroad-Owned, BOX - 40 FT",13.784688949585,12.453692436218301,5.8115987777709996,5.8680887222290004,5.5190763473510698,6.0355668067932102,6.4638857841491699,6.8817863464355504,7.3430500030517596,8.2802579873445605,5.8547582467686601,5.4417342034161296,5.7326588152406996,7.4423487465895102,7.8117467020424503,6.4055880845309101]
["BNSF-E1L201C8","BNSF",4,"E1L201C8",74,"CD(R), DRL Expense, Railroad-Owned, BOX - 40 FT",17.6719646453857,18.274755477905298,18.340091705322301,9.9014434814453107,15.2776498794556,13.2780714035034,13.5395107269287,16.842536926269499,19.654598236083999,20.742561558968401,17.6124371946289,10.163256463067199,11.7730679117323,11.2628140866957,8.2927890997184406,11.280689138395299]
["BNSF-E1L201C9","BNSF",4,"E1L201C9",75,"CD(R), ROI Expense, Railroad-Owned, BOX - 40 FT",2.3450553417205802,3.3599615097045898,3.5866248607635498,0.19736027717590299,0.173742234706879,0.151662066578865,0.17081081867218001,0.236092284321785,0.17725422978401201,0.22614460272523301,0.14020278794357299,1.64795199621466E-2,0.14059717861286899,0.122301643451334,0.129627297538745,0.13771461603427901]
["BNSF-E1L201C10","BNSF",4,"E1L201C10",76,"CD(Y), OPR Expense, Railroad-Owned, BOX - 40 FT",13.784688949585,12.453693389892599,5.8115987777709996,5.8680887222290004,5.5190758705139196,6.0355672836303702,6.4638857841491699,6.8817863464355504,7.3430504798889196,8.2802579873445605,5.8547582467686601,5.4417342034161402,5.7326588152406996,7.4423487465895102,7.8117467020424396,6.4055880845309101]
["BNSF-E1L201C11","BNSF",4,"E1L201C11",77,"CD(Y), DRL Expense, Railroad-Owned, BOX - 40 FT",17.6719646453857,18.274753570556602,18.340089797973601,9.9014434814453107,15.2776498794556,13.2780714035034,13.5395107269287,16.842535018920898,19.654600143432599,20.742561558968401,17.6124371946289,10.163256463067199,11.7730679117323,11.2628140866957,8.2927890997184406,11.280689138395299]
["BNSF-E1L201C12","BNSF",4,"E1L201C12",78,"CD(Y), ROI Expense, Railroad-Owned, BOX - 40 FT",2.3450553417205802,3.3599612712860099,3.5866250991821298,0.19736026227474199,0.17374224960803999,0.151662066578865,0.17081081867218001,0.236092239618301,0.17725421488285101,0.22614460272523301,0.14020278794357299,1.64795199621466E-2,0.14059717861286899,0.122301643451334,0.129627297538745,0.13771461603427901]
["BNSF-E1L201C13","BNSF",4,"E1L201C13",79,"CM(R), DRL Expense, Privately-Owned, BOX - 40 FT",0.32035112380981401,0.34493309259414701,0.31178316473960899,0.343060493469238,0.208725661039352,0.24970203638076799,0.24144791066646601,0.21366363763809201,0.25171357393264798,0.2350677778002,0.256173048754605,0.25306929113516702,0.28376863591067197,0.26528635387191501,0.24633008763211101,0.23677002450732901]
["BNSF-E1L202C1","BNSF",4,"E1L202C1",80,"CM(R), OPR Expense, Railroad-Owned, BOX - 50 FT",0.104918107390404,9.6362285315990406E-2,4.5397792011499398E-2,4.5191854238510097E-2,4.2305193841457402E-2,4.6553149819374098E-2,5.0679888576269198E-2,5.4562639445066501E-2,5.88250197470188E-2,6.5597652344403304E-2,4.4763356593085703E-2,4.0582031445942801E-2,4.3268156317810301E-2,5.7697065097608399E-2,6.2124162905748501E-2,5.2087661138881899E-2]
["BNSF-E1L202C2","BNSF",4,"E1L202C2",81,"CM(R), DRL Expense, Railroad-Owned, BOX - 50 FT",6.2776915729045896E-2,6.3799053430557306E-2,6.7715801298618303E-2,5.89359998703003E-2,5.0515949726104702E-2,4.1969150304794298E-2,3.8883421570062603E-2,6.2181185930967303E-2,4.4067665934562697E-2,5.4943280345509701E-2,3.5868224964049199E-2,1.9652390260874199E-2,3.0752206324677098E-2,3.6078214874626098E-2,4.2049773188892803E-2,2.9546910634952999E-2]
["BNSF-E1L202C3","BNSF",4,"E1L202C3",82,"CM(R), ROI Expense, Railroad-Owned, BOX - 50 FT",1.29188010469079E-2,1.8455408513546E-2,1.9433075562119501E-2,1.48332142271101E-3,1.3214916689321401E-3,1.21498294174671E-3,1.3231815537437801E-3,1.8560908501967801E-3,1.4540656702592999E-3,1.6876993718448099E-3,9.9855843994216503E-4,1.2670096476274901E-4,1.0966838619923399E-3,9.5432908546670703E-4,1.0688753850684599E-3,1.1469334900699501E-3]
["BNSF-E1L202C4","BNSF",4,"E1L202C4",83,"CM(Y), OPR Expense, Railroad-Owned, BOX - 50 FT",0.27278730273246798,0.25054204463958701,0.118034332990646,0.11749872565269499,0.10999348014593099,0.121038287878036,0.13176761567592599,0.141862973570824,0.15294525027275099,0.17055389609544799,0.116384727142023,0.105513281759451,0.11249720642630701,0.150012369253782,0.16152282355494599,0.13542791896109299]
["BNSF-E1L202C5","BNSF",4,"E1L202C5",84,"CM(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",0.16322024166584001,0.16587737202644301,0.17606118321418801,0.15323376655578599,0.131341353058815,0.10911958664655701,0.101096875965595,0.16167120635509499,0.114575766026974,0.142852528898325,9.3257384906528198E-2,5.1096214678273001E-2,7.99557364441605E-2,9.3803358674028101E-2,0.109329410291122,7.6821967650877801E-2]
["BNSF-E1L202C6","BNSF",4,"E1L202C6",85,"CM(Y), ROI Expense, Railroad-Owned, BOX - 50 FT",3.3588919788599E-2,4.7983981668949099E-2,5.0526060163974797E-2,3.85664193890989E-3,3.4358762204647099E-3,3.1589476857334401E-3,3.4402725286781801E-3,4.8258434981107703E-3,3.7805703468620799E-3,4.3880183667964999E-3,2.5962519438496399E-3,3.29422508383147E-4,2.8513780411800901E-3,2.48125562221344E-3,2.7790760011780001E-3,2.9820270741818598E-3]
["BNSF-E1L202C7","BNSF",4,"E1L202C7",86,"CD(R), OPR Expense, Railroad-Owned, BOX - 50 FT",13.784688949585,12.453692436218301,5.8115987777709996,5.8680887222290004,5.5190763473510698,6.0355668067932102,6.4638857841491699,6.8817863464355504,7.3430500030517596,8.2802579873445605,5.8547582467686601,5.4417342034161296,5.7326588152406996,7.4423487465895102,7.8117467020424503,6.4055880845309101]
["BNSF-E1L202C8","BNSF",4,"E1L202C8",87,"CD(R), DRL Expense, Railroad-Owned, BOX - 50 FT",17.6719646453857,18.274755477905298,18.340091705322301,9.9014434814453107,15.2776498794556,13.2780714035034,13.5395107269287,16.842536926269499,19.654598236083999,20.742561558968401,17.6124371946289,10.163256463067199,11.7730679117323,11.2628140866957,8.2927890997184406,11.280689138395299]
["BNSF-E1L202C9","BNSF",4,"E1L202C9",88,"CD(R), ROI Expense, Railroad-Owned, BOX - 50 FT",2.3450553417205802,3.3599615097045898,3.5866248607635498,0.19736027717590299,0.173742234706879,0.151662066578865,0.17081081867218001,0.236092284321785,0.17725422978401201,0.22614460272523301,0.14020278794357299,1.64795199621466E-2,0.14059717861286899,0.122301643451334,0.129627297538745,0.13771461603427901]
["BNSF-E1L202C10","BNSF",4,"E1L202C10",89,"CD(Y), OPR Expense, Railroad-Owned, BOX - 50 FT",13.784688949585,12.453693389892599,5.8115987777709996,5.8680887222290004,5.5190758705139196,6.0355672836303702,6.4638857841491699,6.8817863464355504,7.3430504798889196,8.2802579873445605,5.8547582467686601,5.4417342034161402,5.7326588152406996,7.4423487465895102,7.8117467020424396,6.4055880845309101]
["BNSF-E1L202C11","BNSF",4,"E1L202C11",90,"CD(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",17.6719646453857,18.274753570556602,18.340089797973601,9.9014434814453107,15.2776498794556,13.2780714035034,13.5395107269287,16.842535018920898,19.654600143432599,20.742561558968401,17.6124371946289,10.163256463067199,11.7730679117323,11.2628140866957,8.2927890997184406,11.280689138395299]
["BNSF-E1L202C12","BNSF",4,"E1L202C12",91,"CD(Y), ROI Expense, Railroad-Owned, BOX - 50 FT",2.3450553417205802,3.3599612712860099,3.5866250991821298,0.19736026227474199,0.17374224960803999,0.151662066578865,0.17081081867218001,0.236092239618301,0.17725421488285101,0.22614460272523301,0.14020278794357299,1.64795199621466E-2,0.14059717861286899,0.122301643451334,0.129627297538745,0.13771461603427901]
["BNSF-E1L202C13","BNSF",4,"E1L202C13",92,"CM(R), DRL Expense, Privately-Owned, BOX - 50 FT",0.32035112380981401,0.34493309259414701,0.31178316473960899,0.343060493469238,0.208725661039352,0.24970203638076799,0.24144791066646601,0.21366363763809201,0.25171357393264798,0.2350677778002,0.256173048754605,0.25306929113516702,0.28376863591067197,0.26528635387191501,0.24633008763211101,0.23677002450732901]
["BNSF-E1L203C1","BNSF",4,"E1L203C1",93,"CM(R), OPR Expense, Railroad-Owned, BOX - EQUIPPED",3.2057676464319201E-2,3.3720046281814603E-2,3.8018878549337401E-2,4.13240008056164E-2,4.1243188083171803E-2,4.1219595819711699E-2,4.3523866683244698E-2,4.4614877551794101E-2,4.8612557351589203E-2,4.8821235193336199E-2,4.9834763370340103E-2,4.7869724229173502E-2,5.6600227760130399E-2,6.2296514643376703E-2,6.8827212977026597E-2,6.8975825877731295E-2]
["BNSF-E1L203C2","BNSF",4,"E1L203C2",94,"CM(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED",3.1859412789344801E-2,2.86431014537811E-2,3.4598976373672499E-2,3.4602567553520203E-2,3.34906205534935E-2,3.3878847956657403E-2,3.04339081048965E-2,3.9388440549373599E-2,3.4814603626728099E-2,3.9579618919060998E-2,3.0650859690194598E-2,3.1897446612481603E-2,2.6546340123694601E-2,2.8609275700972801E-2,3.11182206545642E-2,2.3801552898595198E-2]
["BNSF-E1L203C3","BNSF",4,"E1L203C3",95,"CM(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED",1.18681220337749E-2,9.2509547248482704E-3,1.0159533470869101E-2,1.2035274878144301E-2,1.87231115996838E-2,1.6105532646179199E-2,2.5118917226791399E-2,2.1988045424222901E-2,1.9864965230226499E-2,1.62720615952269E-2,1.4084729342750801E-2,1.7144022355828601E-2,2.10163295751267E-2,2.00397274258408E-2,1.9625146294304702E-2,2.4996307388570199E-2]
["BNSF-E1L203C4","BNSF",4,"E1L203C4",96,"CM(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED",8.3350010216236101E-2,8.7672151625156403E-2,9.8849028348922702E-2,0.107442393898964,0.10723233222961399,0.107170723378658,0.113162063062191,0.115998677909374,0.12639246881008101,0.12693521150267401,0.12957038476288399,0.12446128299585101,0.14716059217633901,0.16197093807278001,0.178950753740269,0.17933714728210101]
["BNSF-E1L203C5","BNSF",4,"E1L203C5",97,"CM(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED",8.2834489643573803E-2,7.4472062289714799E-2,8.9957192540168804E-2,8.9966535568237305E-2,8.7075740098953205E-2,8.8084809482097598E-2,7.9128324985504206E-2,0.102409951388836,9.05178338289261E-2,0.102907009189559,7.9692235194505898E-2,8.2933361192451996E-2,6.9020484321605693E-2,7.4384116822529406E-2,8.0907373701867E-2,6.1884037536347601E-2]
["BNSF-E1L203C6","BNSF",4,"E1L203C6",98,"CM(Y), ROI Expense, Railroad-Owned, BOX - EQUIPPED",3.0857101082801802E-2,2.4052444845438E-2,2.6414792984724E-2,3.1291633844375603E-2,4.8680130392312997E-2,4.1874293237924597E-2,6.53093457221985E-2,5.7168964296579403E-2,5.1648803055286401E-2,4.2307360147589998E-2,3.6620296291152099E-2,4.4574458125154197E-2,5.4642456895329497E-2,5.2103291307186099E-2,5.1025380365192302E-2,6.4990399210282407E-2]
["BNSF-E1L203C7","BNSF",4,"E1L203C7",99,"CD(R), OPR Expense, Railroad-Owned, BOX - EQUIPPED",3.8215303421020499,4.02994680404663,4.5951800346374503,5.1881189346313503,5.2756752967834499,5.1474332809448198,5.2089114189147896,5.0396747589111301,5.24961185455322,5.1831420496195699,5.3430024152247197,5.1879478569456801,6.1235163620530901,7.40285864769392,9.3891721563054702,10.8494690743006]
["BNSF-E1L203C8","BNSF",4,"E1L203C8",100,"CD(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED",12.8889760971069,12.882072448730501,12.9588060379028,10.8604326248169,11.9945573806763,10.849268913269,11.384449005126999,11.783424377441399,13.920641899108899,11.9635207977867,11.404715579276999,10.601428511718201,10.815395761085799,15.431118974260301,14.4539094762575,17.075157634896801]
["BNSF-E1L203C9","BNSF",4,"E1L203C9",101,"CD(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED",2.0272123813629199,1.62113285064697,1.7857708930969201,2.2814645767211901,3.5406081676483199,2.7070059776306201,4.2682981491088903,3.4946186542511,2.9224681854247998,2.5788094866061999,2.2883692624387302,2.5803659967832302,3.3133206189080702,4.4854303755202301,4.7028091729154502,5.5778813760156698]
["BNSF-E1L203C10","BNSF",4,"E1L203C10",102,"CD(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED",3.8215308189392099,4.02994680404663,4.5951800346374503,5.1881194114685103,5.2756752967834499,5.1474332809448198,5.2089114189147896,5.0396747589111301,5.24961185455322,5.1831420496195699,5.3430024152247197,5.1879478569456801,6.1235163620530901,7.40285864769392,9.3891721563054702,10.8494690743006]
["BNSF-E1L203C11","BNSF",4,"E1L203C11",103,"CD(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED",12.8889770507813,12.882072448730501,12.9588060379028,10.860431671142599,11.9945573806763,10.849267005920399,11.384449005126999,11.783424377441399,13.920641899108899,11.9635207977867,11.404715579276999,10.601428511718201,10.815395761085799,15.431118974260301,14.4539094762575,17.075157634896801]
["BNSF-E1L203C12","BNSF",4,"E1L203C12",104,"CD(Y), ROI Expense, Railroad-Owned, BOX - EQUIPPED",2.0272123813629199,1.62113296985626,1.7857707738876301,2.2814643383026101,3.5406081676483199,2.7070059776306201,4.2682981491088903,3.49461841583252,2.9224684238433798,2.5788094866061999,2.2883692624387302,2.5803659967832302,3.3133206189080702,4.4854303755202301,4.7028091729154502,5.5778813760156698]
["BNSF-E1L203C13","BNSF",4,"E1L203C13",105,"CM(R), DRL Expense, Privately-Owned, BOX - EQUIPPED",0.308298259973526,0.31248530745506298,0.30857902765273998,0.29820731282234197,0.309219390153885,0.314113259315491,0.30086895823478699,0.32273149490356401,0.36703586578369102,0.28755285945307102,0.287479427673416,0.32048959429207002,0.28370973582930997,0.28762361371829298,0.27966674786717199,0.291061144287449]
["BNSF-E1L204C1","BNSF",4,"E1L204C1",106,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",4.0793687105178798E-2,4.1025649756193203E-2,4.8256039619445801E-2,4.8152543604373897E-2,4.6956669539213201E-2,4.9578186124563203E-2,5.55925443768501E-2,5.6899007409810999E-2,5.5704202502965899E-2,5.7663374157114901E-2,5.5358707817167403E-2,4.6420778557917201E-2,4.0660678706728702E-2,4.5588298756379299E-2,5.2335201496716499E-2,5.1644798094750803E-2]
["BNSF-E1L204C2","BNSF",4,"E1L204C2",107,"CM(R), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",1.5484553296119001E-3,4.0353289805352697E-3,3.32804280333221E-3,2.36728903837502E-3,2.63333786278963E-3,1.91408023238182E-3,-9.3482359079644095E-4,2.2635790810454599E-4,2.8056525625288499E-3,3.5533423219473999E-3,4.3866697127177799E-3,1.47841687855644E-3,-6.1781084470348899E-3,1.58399495143349E-3,-4.0181762766815796E-3,-5.8436507508619201E-3]
["BNSF-E1L204C3","BNSF",4,"E1L204C3",108,"CM(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",5.6419330649077901E-3,5.6279175914824E-3,5.9064202941954101E-3,4.2978348210453996E-3,4.0130238048732298E-3,4.4233910739421801E-3,5.04428474232554E-3,7.2213453240692598E-3,8.8478680700063705E-3,7.1690959975242597E-3,7.4297259866644497E-3,7.7050352273972901E-3,8.3848349291944201E-3,7.3829000867211003E-3,7.1086362173877898E-3,8.9653974522238503E-3]
["BNSF-E1L204C4","BNSF",4,"E1L204C4",109,"CM(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",0.106063455343246,0.10666669905185699,0.12546561658382399,0.125196352601051,0.122087210416794,0.12890310585498799,0.14454063773155201,0.147937327623367,0.144830763339996,0.149924772808499,0.14393264032463499,0.12069402425058499,0.10571776463749499,0.118529576766587,0.13607152389146299,0.13427647504635201]
["BNSF-E1L204C5","BNSF",4,"E1L204C5",110,"CM(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",4.0259864181280101E-3,1.04918424040079E-2,8.6529124528169597E-3,6.1549567617476004E-3,6.8466830998659099E-3,4.9766129814088301E-3,-2.43053771555424E-3,5.8853271184489098E-4,7.2946939617395401E-3,9.2386900370632092E-3,1.1405341253066199E-2,3.8438838842467398E-3,-1.6063081962290698E-2,4.1183868737270698E-3,-1.0447258319372099E-2,-1.5193491952241E-2]
["BNSF-E1L204C6","BNSF",4,"E1L204C6",111,"CM(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",1.4669054187834299E-2,1.4632578939199401E-2,1.53566868975759E-2,1.1174377053976101E-2,1.0433868505060701E-2,1.1500840075314E-2,1.31151210516691E-2,1.8775537610053999E-2,2.30044517666101E-2,1.8639649593562999E-2,1.93172875653276E-2,2.0033091591232899E-2,2.1800570815905501E-2,1.91955402254749E-2,1.8482454165208301E-2,2.3310033375782E-2]
["BNSF-E1L204C7","BNSF",4,"E1L204C7",112,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",4.3272247314453098,4.2883815765380904,5.0696544647216797,5.2156796455383301,5.3090147972106898,5.6798801422119096,6.3365402221679696,6.2816858291626003,5.98960208892822,6.2643497796716998,6.1360622079920502,5.2611757769186296,4.6261159498460396,5.12888065899309,6.0086465368858804,5.8841599061436396]
["BNSF-E1L204C8","BNSF",4,"E1L204C8",113,"CD(R), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",0.33044078946113598,0.76876914501190197,0.70083439350128196,0.433044344186783,0.464343011379242,0.44350951910018899,0.48794251680374101,0.69961255788803101,0.92502284049987804,0.67599447179762895,0.54994968743528205,0.21989381427315699,-0.415354086447981,0.22941956120714199,5.5631114014863398E-2,3.8634070098156302E-2]
["BNSF-E1L204C9","BNSF",4,"E1L204C9",114,"CD(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",0.82604551315307595,0.81241375207901001,0.87305939197540305,0.65879607200622603,0.63457322120666504,0.660927534103394,0.74731582403182995,1.0773092508316,1.2995964288711499,1.1527000496779001,1.2108647461992199,1.2216882771144699,1.3830719324888801,1.17573552137111,1.1957151342079499,1.43257809484915]
["BNSF-E1L204C10","BNSF",4,"E1L204C10",115,"CD(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",4.3272247314453098,4.2883820533752397,5.0696539878845197,5.2156796455383301,5.3090152740478498,5.6798796653747603,6.3365402221679696,6.2816858291626003,5.98960256576538,6.2643497796716998,6.1360622079920502,5.2611757769186296,4.6261159498460396,5.12888065899309,6.0086465368858804,5.8841599061436396]
["BNSF-E1L204C11","BNSF",4,"E1L204C11",116,"CD(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",0.33044075965881298,0.76876914501190197,0.70083439350128196,0.433044373989105,0.464343041181564,0.44350951910018899,0.48794251680374101,0.699612617492676,0.92502278089523304,0.67599447179762895,0.54994968743528205,0.21989381427315699,-0.415354086447981,0.22941956120714199,5.5631114014863398E-2,3.8634070098156302E-2]
["BNSF-E1L204C12","BNSF",4,"E1L204C12",117,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",0.82604545354843095,0.81241375207901001,0.87305939197540305,0.65879607200622603,0.63457322120666504,0.660927534103394,0.74731588363647505,1.0773092508316,1.2995963096618699,1.1527000496779001,1.2108647461992199,1.2216882771144699,1.3830719324888801,1.17573552137111,1.1957151342079499,1.43257809484915]
["BNSF-E1L204C13","BNSF",4,"E1L204C13",118,"CM(R), DRL Expense, Privately-Owned, GONDOLA - PLAIN",7.7351467916742E-4,7.94146442785859E-4,7.1615463821217396E-4,1.11124909017235E-3,2.1618294995278098E-3,3.9131529629230499E-3,2.1956828422844401E-3,3.6552557721733999E-3,4.41434513777494E-3,3.9876247270560798E-3,8.72686122343009E-4,1.3998599794658899E-3,1.41238846587935E-3,1.7240138599998701E-3,1.34996388626182E-3,2.05380323731998E-3]
["BNSF-E1L205C1","BNSF",4,"E1L205C1",119,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",4.6084862202405902E-2,5.0917223095893901E-2,5.2130229771137203E-2,5.87817505002022E-2,5.84458485245705E-2,5.5123399943113299E-2,5.8184854686260203E-2,5.8191664516925798E-2,6.5043769776821095E-2,7.73460553169599E-2,8.7420507991371396E-2,7.9978729768642995E-2,6.8149250150376997E-2,6.02095893215902E-2,6.1750325770348301E-2,5.8706985418694499E-2]
["BNSF-E1L205C2","BNSF",4,"E1L205C2",120,"CM(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.3464960977435102E-2,2.8029719367623301E-2,3.3587612211704303E-2,3.31650488078594E-2,2.2051574662327801E-2,3.0475996434688599E-2,3.2505352050066001E-2,3.8965102285146699E-2,3.8210876286029802E-2,3.6998533482439602E-2,2.61253694418704E-2,2.5722167727196901E-2,2.1760349218661101E-2,2.6228029069279901E-2,2.1861874894922102E-2,1.5797375911073601E-2]
["BNSF-E1L205C3","BNSF",4,"E1L205C3",121,"CM(R), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",1.5057632699608799E-2,2.0448097959160801E-2,2.2054273635148999E-2,3.4476380795240402E-2,2.3821322247386E-2,1.90575681626797E-2,1.9071346148848499E-2,1.97226665914059E-2,2.1094219759106601E-2,3.1585709667577198E-2,2.7031106430735499E-2,2.3650902945017201E-2,2.90394200469784E-2,2.47492001654772E-2,2.1698572465760301E-2,2.48903496266904E-2]
["BNSF-E1L205C4","BNSF",4,"E1L205C4",122,"CM(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",0.119820617139339,0.13238483667373699,0.13553845882415799,0.152832746505737,0.15195930004119901,0.143320992588997,0.15128062665462499,0.151298433542252,0.169113755226135,0.20109974382409601,0.227293320777566,0.20794469739847199,0.17718805039098101,0.156544932236134,0.16055084700290501,0.15263816208860601]
["BNSF-E1L205C5","BNSF",4,"E1L205C5",123,"CM(Y), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",6.1008833348751103E-2,7.2877340018749195E-2,8.7327718734741197E-2,8.6228974163532299E-2,5.7334110140800497E-2,7.9237632453441606E-2,8.4514014422893496E-2,0.101309411227703,9.9348329007625594E-2,9.6196187054342894E-2,6.7925960548863198E-2,6.6877636090711998E-2,5.6576907968519101E-2,6.8192875580127696E-2,5.6840874726797497E-2,4.1073177368791403E-2]
["BNSF-E1L205C6","BNSF",4,"E1L205C6",124,"CM(Y), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",3.9149783551692997E-2,5.3165078163147E-2,5.7341098785400398E-2,8.9638426899910001E-2,6.1935417354106903E-2,4.9549717456102399E-2,4.9585517495870597E-2,5.1279015839099898E-2,5.4844994097948102E-2,8.2122845135700701E-2,7.0280876719912302E-2,6.1492347657044699E-2,7.5502492122143897E-2,6.4347920430240693E-2,5.6416288410976803E-2,6.4714909029395196E-2]
["BNSF-E1L205C7","BNSF",4,"E1L205C7",125,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",4.4808874130248997,5.0633177757263201,5.34395503997803,6.3391251564025897,6.2628550529479998,5.9207038879394496,6.2038278579711896,6.1208815574645996,6.6190218925476101,7.7632144980727098,8.9514016994400496,8.6234004832973401,7.6591804843576199,6.9508117738854303,7.4168114018820397,7.0075518593558499]
["BNSF-E1L205C8","BNSF",4,"E1L205C8",126,"CD(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",24.338758468627901,29.674228668212901,28.438371658325199,37.250621795654297,26.256160736083999,24.894578933715799,30.411373138427699,34.213909149169901,39.634750366210902,52.715205898245699,43.185654902504297,30.0574713891526,31.305815797788899,35.375840747116897,30.087000942347601,27.2495840625771]
["BNSF-E1L205C9","BNSF",4,"E1L205C9",127,"CD(R), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.0673661231994598,3.2049686908721902,3.3934907913207999,5.5620570182800302,3.6876077651977499,2.94025731086731,2.9734010696411102,2.9045362472534202,2.9191839694976802,4.7628345812507504,4.30486877386355,3.8071519739258899,4.9529698545915002,4.3387261395086902,3.9654046871215498,4.1876499753650203]
["BNSF-E1L205C10","BNSF",4,"E1L205C10",128,"CD(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",4.4808874130248997,5.0633177757263201,5.34395503997803,6.3391251564025897,6.2628550529479998,5.9207038879394496,6.2038278579711896,6.1208806037902797,6.6190218925476101,7.7632144980727098,8.9514016994400496,8.6234004832973401,7.6591804843576199,6.95081177388544,7.4168114018820397,7.0075518593558499]
[{"$f":"B130&\"-\"&D130","v":"BNSF-E1L205C11"},"BNSF",4,"E1L205C11",129,"CD(Y), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",24.338758468627901,29.674228668212901,28.438369750976602,37.250617980957003,26.256158828735401,24.894578933715799,30.411373138427699,34.213905334472699,39.634750366210902,52.715205898245699,43.185654902504297,30.0574713891526,31.305815797788899,35.375840747116897,30.087000942347601,27.2495840625771]
["BNSF-E1L205C12","BNSF",4,"E1L205C12",130,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.0673661231994598,3.2049689292907702,3.3934910297393799,5.5620560646057102,3.6876075267791699,2.94025731086731,2.9734008312225302,2.9045360088348402,2.9191842079162602,4.7628345812507504,4.30486877386355,3.8071519739258899,4.9529698545915002,4.3387261395086902,3.9654046871215498,4.1876499753650203]
["BNSF-E1L205C13","BNSF",4,"E1L205C13",131,"CM(R), DRL Expense, Privately-Owned, GONDOLA - EQUIPPED",2.4928665879997401E-5,2.3257440261659199E-5,1.8548086518421799E-4,9.3866714450996396E-5,3.5610661143437001E-5,2.6671747036743899E-5,2.22133294300875E-5,2.63157926383428E-5,3.3611195249250199E-5,3.0376113618873601E-2,2.01543513424523E-2,1.23657013363603E-2,3.7489955819157098E-3,4.4740396217598502E-4,1.3307655451925699E-3,1.367481611516E-4]
["BNSF-E1L206C1","BNSF",4,"E1L206C1",132,"CM(R), OPR Expense, Railroad-Owned, HOPPER - COVERED",2.5433888658881201E-2,2.8033385053276998E-2,3.23507115244865E-2,3.5169459879398297E-2,3.1771875917911502E-2,3.06032598018646E-2,3.0104272067546799E-2,3.1701683998107903E-2,3.27881313860416E-2,3.5911319081559402E-2,3.37798767107245E-2,3.0616853269100901E-2,2.8549644971416401E-2,2.99760070796142E-2,3.1080369595335701E-2,2.9705141093640398E-2]
["BNSF-E1L206C2","BNSF",4,"E1L206C2",133,"CM(R), DRL Expense, Railroad-Owned, HOPPER - COVERED",-1.2165922671556501E-3,-2.1173525601625399E-3,-1.1941689299419501E-3,-1.58906716387719E-3,-4.3897652067244096E-3,2.6574777439236598E-4,8.1616810348350595E-5,3.5128213930875102E-3,6.61851558834314E-3,4.5491677693511997E-3,5.9985541641174502E-3,5.9635122516578896E-3,2.0861575580879699E-3,6.0594866415379005E-4,-1.90131242859109E-4,1.93324626679489E-3]
["BNSF-E1L206C3","BNSF",4,"E1L206C3",134,"CM(R), ROI Expense, Railroad-Owned, HOPPER - COVERED",9.3352152034640295E-3,1.52859501540661E-2,1.5733679756522199E-2,1.6236400231719E-2,1.49068115279078E-2,1.72538850456476E-2,1.9269481301307699E-2,2.0788285881280899E-2,1.8302848562598201E-2,1.58409922473879E-2,1.29346351217165E-2,1.5206209139611101E-2,1.8451854292883801E-2,1.8122482781997601E-2,1.4501419021651999E-2,1.8452215696408699E-2]
["BNSF-E1L206C4","BNSF",4,"E1L206C4",135,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",6.6128216683864594E-2,7.2886772453784901E-2,8.4111817181110396E-2,9.1440595686435699E-2,8.2606799900531797E-2,7.9568497836589799E-2,7.8271254897117601E-2,8.2424275577068301E-2,8.5249148309230804E-2,9.3369429612054605E-2,8.78276794478835E-2,7.9603818499662499E-2,7.4229076925682397E-2,7.7937618406997297E-2,8.0808960947872793E-2,7.7233366843465004E-2]
["BNSF-E1L206C5","BNSF",4,"E1L206C5",136,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",-3.1631479505449499E-3,-5.5051245726645002E-3,-3.1048541422933301E-3,-4.1315793059766301E-3,-1.1413336731493501E-2,6.9092510966584097E-4,2.1218412439338901E-4,9.1333370655775105E-3,1.7208125442266499E-2,1.1827836200313101E-2,1.5596240826705399E-2,1.5505131854310499E-2,5.4240096510287201E-3,1.5754665267998401E-3,-4.9434123143371304E-4,5.0264402936667299E-3]
["BNSF-E1L206C6","BNSF",4,"E1L206C6",137,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED",2.42715552449226E-2,3.9743527770042399E-2,4.0907580405473702E-2,4.2214568704366698E-2,3.8757681846618701E-2,4.4860050082206698E-2,5.0100669264793403E-2,5.4049462080001803E-2,4.7587379813194303E-2,4.1186579843208601E-2,3.3630051316462899E-2,3.9536143762988897E-2,4.7974821161498003E-2,4.7118455233193697E-2,3.7703689456295202E-2,4.7975760810662703E-2]
["BNSF-E1L206C7","BNSF",4,"E1L206C7",138,"CD(R), OPR Expense, Railroad-Owned, HOPPER - COVERED",2.7931261062622101,3.07833647727966,3.5614647865295401,3.9743337631225599,3.6182625293731698,3.4969730377197301,3.4172096252441402,3.5437500476837198,3.6385695934295699,4.0418578960253999,3.8993189731801401,3.62545342360281,3.4812120518727601,3.6897760828220099,3.9586990548588599,3.7832720893457501]
["BNSF-E1L206C8","BNSF",4,"E1L206C8",139,"CD(R), DRL Expense, Railroad-Owned, HOPPER - COVERED",7.0871648788452104,8.1742725372314506,7.3523645401001003,8.5047445297241193,5.8631677627563503,6.5383744239807102,8.5506734848022496,8.2989473342895508,7.5877571105956996,6.1186775226596204,4.2541614252366902,3.9966525840337299,4.1186701026762096,3.76751553272338,3.8845589286325999,4.6929766098658403]
["BNSF-E1L206C9","BNSF",4,"E1L206C9",140,"CD(R), ROI Expense, Railroad-Owned, HOPPER - COVERED",1.45270276069641,2.5145339965820299,2.5631294250488299,2.7606945037841801,2.50106620788574,2.8506560325622599,3.21953153610229,3.3504805564880402,2.9609417915344198,2.7384186141174198,2.2654923667513698,2.6497356407585699,3.4628213150582301,3.2949230555273998,2.8096577427184699,3.4625836579693798]
["BNSF-E1L206C10","BNSF",4,"E1L206C10",141,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",2.7931265830993701,3.07833671569824,3.5614650249481201,3.9743335247039799,3.6182620525360099,3.4969725608825701,3.4172096252441402,3.5437500476837198,3.6385695934295699,4.0418578960253999,3.8993189731801401,3.62545342360281,3.4812120518727601,3.6897760828220099,3.9586990548588599,3.7832720893457501]
["BNSF-E1L206C11","BNSF",4,"E1L206C11",142,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",7.0871653556823704,8.1742725372314506,7.3523650169372603,8.5047445297241193,5.8631687164306596,6.5383744239807102,8.5506715774536097,8.2989473342895508,7.5877571105956996,6.1186775226596204,4.2541614252366902,3.9966525840337299,4.1186701026762096,3.76751553272338,3.8845589286325999,4.6929766098658403]
["BNSF-E1L206C12","BNSF",4,"E1L206C12",143,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED",1.4527028799057,2.5145339965820299,2.5631294250488299,2.7606940269470202,2.50106620788574,2.8506557941436799,3.21953153610229,3.3504803180694598,2.9609422683715798,2.7384186141174198,2.2654923667513698,2.6497356407585699,3.4628213150582301,3.2949230555273998,2.8096577427184699,3.4625836579693798]
["BNSF-E1L206C13","BNSF",4,"E1L206C13",144,"CM(R), DRL Expense, Privately-Owned, HOPPER - COVERED",1.5991024672985101E-2,1.5936158597469299E-2,1.3894944451749301E-2,1.82291958481073E-2,5.9681623242795502E-3,2.7156833093613399E-3,3.41975688934326E-3,3.5576026421040301E-3,4.3468880467116798E-3,3.9575556191767001E-3,2.6999837507642999E-2,2.2584208775490201E-2,2.1880977336752899E-2,2.4540876056971899E-2,2.3065124688367501E-2,2.33260527862378E-2]
["BNSF-E1L207C1","BNSF",4,"E1L207C1",145,"CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",3.9249509572982802E-2,4.3566223233938203E-2,5.0262853503227199E-2,4.8262916505336803E-2,4.1762735694646801E-2,3.5309638828039197E-2,3.4196555614471401E-2,3.18937934935093E-2,3.2893609255552299E-2,3.8745816713311898E-2,4.3504979627564298E-2,4.0940534683300098E-2,3.8590999873984899E-2,4.8127846653101103E-2,6.9552349027400096E-2,8.1541286183833203E-2]
["BNSF-E1L207C2","BNSF",4,"E1L207C2",146,"CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.0792522691190199E-2,1.12273776903749E-2,9.7235199064016307E-3,1.14042097702622E-2,1.01898750290275E-2,1.2382035143673399E-2,1.08271082863212E-2,1.02103389799595E-2,1.2341546826064601E-2,1.53341022827605E-2,1.71627722222427E-2,7.0923673780165604E-3,3.3088102815182598E-3,2.99594704350059E-3,1.1040468951689799E-2,3.96567975496481E-3]
["BNSF-E1L207C3","BNSF",4,"E1L207C3",147,"CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.5185305625200299E-2,3.15555594861507E-2,3.0554348602891E-2,3.3042114228010198E-2,3.0457340180873899E-2,2.65440922230482E-2,2.3279793560504899E-2,2.3108217865228702E-2,2.3552440106868699E-2,4.3658749062846398E-2,4.4188906288847002E-2,4.8513305137746099E-2,4.7141358907216199E-2,5.5958864887536999E-2,6.1971831447151397E-2,5.2909807711383101E-2]
["BNSF-E1L207C4","BNSF",4,"E1L207C4",148,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",0.102048613131046,0.11327207833528501,0.13068334758281699,0.125483527779579,0.10858310014009501,9.1805122792720795E-2,8.8911049067974104E-2,8.2923889160156306E-2,8.5523374378681197E-2,0.100739123454611,0.11311294703166699,0.10644539017658,0.100336599672361,0.125132401298063,0.18083610747124099,0.21200734407796701]
["BNSF-E1L207C5","BNSF",4,"E1L207C5",149,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.8060553595423698E-2,2.9191141948103901E-2,2.5281168520450599E-2,2.9650909826159502E-2,2.6493633165955498E-2,3.2193284481763798E-2,2.8150510042905801E-2,2.6546895503997799E-2,3.2087992876768098E-2,3.9868665935177197E-2,4.4623207777830999E-2,1.8440155182843102E-2,8.60290673194751E-3,7.7894623131015799E-3,2.8705219274393599E-2,1.03107673629085E-2]
["BNSF-E1L207C6","BNSF",4,"E1L207C6",150,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",6.5481804311275496E-2,8.2044340670108795E-2,7.9441301524639102E-2,8.5909456014633206E-2,7.9189047217369093E-2,6.9014631211757702E-2,6.0527428984642001E-2,6.0081437230110203E-2,6.1236266046762501E-2,0.113512747563401,0.114891156351002,0.12613459335814001,0.122567533158762,0.145493048707596,0.161126761762594,0.137565500049596]
["BNSF-E1L207C7","BNSF",4,"E1L207C7",151,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",3.4641952514648402,3.73549127578735,4.3604207038879403,4.2468066215515101,3.8975753784179701,3.4002490043640101,3.4202067852020299,3.1777319908142099,3.2254981994628902,3.58692299078586,3.7006191423605701,3.0971769080022402,3.20061588546077,4.1936306273645698,6.2213761312427396,6.8028925126648803]
["BNSF-E1L207C8","BNSF",4,"E1L207C8",152,"CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",0.44400981068611101,1.04161429405212,0.31612840294838002,0.99631708860397294,0.52144575119018599,0.54839122295379605,1.12277948856354,0.93477910757064797,0.97688043117523204,0.78906669432450405,-0.85694192629838595,-2.2771034341521199,-3.4786718058349901,-1.58164610446479,0.12141870380273199,-0.74275014111955595]
["BNSF-E1L207C9","BNSF",4,"E1L207C9",153,"CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",3.1757619380950901,3.88984942436218,4.0145468711853001,4.3679938316345197,4.4745812416076696,3.8335716724395801,3.4971339702606201,3.34908127784729,3.2418882846832302,5.1920565510355896,4.7394575875231801,5.2580025460809399,7.3181867980331097,7.1845405905340902,6.5843918823455896,7.0198760201947898]
["BNSF-E1L207C10","BNSF",4,"E1L207C10",154,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",3.4641952514648402,3.73549151420593,4.3604211807251003,4.2468061447143599,3.8975751399993901,3.4002490043640101,3.4202070236206099,3.1777319908142099,3.2254981994628902,3.58692299078586,3.7006191423605701,3.0971769080022402,3.20061588546077,4.1936306273645698,6.2213761312427396,6.8028925126648803]
["BNSF-E1L207C11","BNSF",4,"E1L207C11",155,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",0.44400975108146701,1.04161441326141,0.31612852215766901,0.99631720781326305,0.52144587039947499,0.54839134216308605,1.12277948856354,0.93477916717529297,0.97688055038452104,0.78906669432450405,-0.85694192629838595,-2.2771034341521199,-3.4786718058349901,-1.58164610446479,0.12141870380273199,-0.74275014111955595]
["BNSF-E1L207C12","BNSF",4,"E1L207C12",156,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",3.1757619380950901,3.8898499011993399,4.0145468711853001,4.3679938316345197,4.4745812416076696,3.8335716724395801,3.4971339702606201,3.34908127784729,3.2418882846832302,5.1920565510355896,4.7394575875231801,5.2580025460809399,7.3181867980331097,7.1845405905340902,6.5843918823455896,7.0198760201947898]
["BNSF-E1L207C13","BNSF",4,"E1L207C13",157,"CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - GENERAL",7.3341056122444597E-5,2.00427457457408E-5,2.9689277653233101E-5,6.9038446781632998E-6,9.4672426348552097E-4,3.4785602474585203E-4,1.2363485293462901E-3,1.5842547873035099E-3,1.41869962681085E-3,1.2496791421533599E-3,4.31395714574894E-3,1.64065537815164E-3,9.3327893101443E-4,1.38157796186714E-4,1.4640909045006899E-5,6.1360996982716104E-6]
["BNSF-E1L208C1","BNSF",4,"E1L208C1",158,"CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",3.52040641009808E-2,3.5990245640277897E-2,3.4884139895439099E-2,4.2961269617080702E-2,4.1257373988628401E-2,4.2800974100828199E-2,3.9816793054342298E-2,4.3657008558511699E-2,4.7838144004344899E-2,5.1285486079113402E-2,4.74172865760637E-2,4.0398933968978999E-2,3.4514197231487499E-2,3.4848009969765802E-2,3.6809760264751898E-2,4.01902117670404E-2]
["BNSF-E1L208C2","BNSF",4,"E1L208C2",159,"CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",-8.4925690316595096E-5,2.0052681211382198E-3,-2.91546224616468E-3,-1.46085824817419E-2,-1.3261348940432099E-2,-8.6999125778675097E-3,7.4335606768727303E-5,3.7941038608550999E-3,3.5535406786948399E-3,3.5210335559511001E-3,5.7757756934681296E-3,2.70824066113715E-3,-1.15935913759887E-3,-1.8091822020799501E-3,-7.9006252408815903E-5,1.7182262229446801E-3]
["BNSF-E1L208C3","BNSF",4,"E1L208C3",160,"CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",6.5896790474653201E-3,9.2859501019120199E-3,9.1397613286971994E-3,9.5679331570863706E-3,9.6933692693710292E-3,1.08736855909228E-2,1.6987729817628899E-2,1.61872543394566E-2,1.44373700022697E-2,1.5531358591509999E-2,1.6762109971586801E-2,1.5047158650651499E-2,1.4420316621059101E-2,1.19502043584537E-2,1.5574886966237199E-2,1.72292166439043E-2]
["BNSF-E1L208C4","BNSF",4,"E1L208C4",161,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",9.1530598700046498E-2,9.3574590981006595E-2,9.0698815882206005E-2,0.11169935017824199,0.107269331812859,0.111282706260681,0.103523731231689,0.11350819468498199,0.124379135668278,0.133342263805695,0.123284945097766,0.10503722831934501,8.9736912801867505E-2,9.06048259213907E-2,9.5705376688355007E-2,0.104494550594305]
["BNSF-E1L208C5","BNSF",4,"E1L208C5",162,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",-2.2080724011175299E-4,5.2136923186480999E-3,-7.5801885686814802E-3,-3.79823260009289E-2,-3.4479513764381402E-2,-2.2619770839810399E-2,1.9326103210914899E-4,9.8646543920040096E-3,9.2392191290855408E-3,9.1546872454728503E-3,1.50170168030171E-2,7.04142571895659E-3,-3.01433375775704E-3,-4.70387372540785E-3,-2.05416256262904E-4,4.4673881796561503E-3]
["BNSF-E1L208C6","BNSF",4,"E1L208C6",163,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.7133181914687198E-2,2.41434592753649E-2,2.3763343691825901E-2,2.4876616895198801E-2,2.5202766060829201E-2,2.8271583840251E-2,4.4168036431074101E-2,4.2086761444807101E-2,3.7537213414907497E-2,4.0381532337926102E-2,4.3581485926125499E-2,3.9122612491693999E-2,3.7492823214753598E-2,3.1070531331979699E-2,4.0494706112216797E-2,4.47959632741513E-2]
["BNSF-E1L208C7","BNSF",4,"E1L208C7",164,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.2532539367675799,2.4519588947296098,2.5053505897521999,3.3416073322296098,3.6396906375885001,4.2620782852172896,4.2035102844238299,4.6075258255004901,5.0880279541015598,5.4916170911718201,5.1063611976406502,4.3577255544979803,3.8045746111796501,3.4145523622930698,3.38791224815294,3.2085235898188298]
["BNSF-E1L208C8","BNSF",4,"E1L208C8",165,"CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",5.6389894485473597,7.8201580047607404,7.9562249183654803,8.1094274520874006,8.1711473464965803,10.498775482177701,13.6944742202759,12.6380310058594,10.277400970459,11.9506599652108,11.493378563097499,7.8635777917095204,5.7072850902171597,3.6036056121639901,5.3608606681750102,4.12246132520354]
["BNSF-E1L208C9","BNSF",4,"E1L208C9",166,"CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.65362721681594804,0.96671760082244895,0.98129302263259899,1.22657358646393,1.465780377388,1.62284600734711,2.6938164234161399,2.4812178611755402,2.2173917293548602,2.4979817981295001,2.6126409001986799,2.3384524338121899,2.43684325022691,1.41680051679777,1.8752518350434999,1.9129475954838]
["BNSF-E1L208C10","BNSF",4,"E1L208C10",167,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.2532539367675799,2.4519588947296098,2.5053505897521999,3.3416075706481898,3.6396906375885001,4.2620782852172896,4.2035107612609899,4.6075258255004901,5.0880279541015598,5.4916170911718201,5.1063611976406502,4.3577255544979803,3.8045746111796501,3.4145523622930698,3.38791224815294,3.2085235898188298]
["BNSF-E1L208C11","BNSF",4,"E1L208C11",168,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",5.6389894485473597,7.8201584815979004,7.9562239646911603,8.1094274520874006,8.1711492538452095,10.498775482177701,13.6944742202759,12.638030052185099,10.2774000167847,11.9506599652108,11.493378563097499,7.8635777917095204,5.7072850902171597,3.6036056121639901,5.3608606681750102,4.12246132520354]
["BNSF-E1L208C12","BNSF",4,"E1L208C12",169,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.65362721681594804,0.96671760082244895,0.98129284381866499,1.22657370567322,1.465780377388,1.62284600734711,2.6938166618347199,2.4812180995941202,2.2173914909362802,2.4979817981295001,2.6126409001986799,2.3384524338121899,2.43684325022691,1.41680051679777,1.8752518350434999,1.9129475954838]
["BNSF-E1L208C13","BNSF",4,"E1L208C13",170,"CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - SPECIAL",6.3735642470419398E-6,9.5366749519598704E-6,8.0185500337393006E-6,1.21021157610812E-5,4.1941611561924197E-4,1.3154466869309499E-3,3.58787045115605E-4,9.9998296718695201E-6,1.2289909645915001E-3,7.9075786530599396E-4,3.9152668947337397E-6,1.8120022004226901E-6,1.9008679556000599E-6,6.1782877190938502E-6,9.9605842709842395E-6,5.3202893594181596E-6]
["BNSF-E1L209C1","BNSF",4,"E1L209C1",171,"CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",3.5659156739711803E-2,3.92468497157097E-2,5.1496773958206198E-2,5.4212041199207299E-2,6.24595358967781E-2,6.2401115894317599E-2,6.2983170151710496E-2,5.7675328105688102E-2,5.3925499320030199E-2,5.7717853589431503E-2,5.8705852327687297E-2,5.6244708061766902E-2,5.9046454696955797E-2,6.0668848584387203E-2,6.3002411693195495E-2,5.8245919331929498E-2]
["BNSF-E1L209C2","BNSF",4,"E1L209C2",172,"CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",-2.3308854550123201E-2,-2.86177266389132E-2,-2.28562876582146E-2,-2.5155656039714799E-2,-2.8634011745452902E-2,-1.7771348357200598E-2,-2.5640921667218201E-2,-3.2916482537984799E-2,-1.5934880822896999E-2,-2.6040194689696299E-2,-9.1397030542599601E-3,-1.7783587559676E-2,-4.1386627337100898E-2,-3.7552142317429101E-2,-2.1875748912679498E-2,-1.80435359771502E-2]
["BNSF-E1L209C3","BNSF",4,"E1L209C3",173,"CM(R), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",1.9057586789131199E-2,9.2152208089828509E-3,9.4810584560036694E-3,8.4409955888986605E-3,2.8744044248014702E-3,2.41268612444401E-3,2.5320595595985699E-3,2.5157795753330001E-3,1.33387208916247E-3,1.2784159063811201E-3,1.4398064192819499E-3,1.4694639592326901E-3,1.3561921290348501E-3,9.8701492861390109E-4,3.7209053026648398E-2,4.30920165401249E-2]
["BNSF-E1L209C4","BNSF",4,"E1L209C4",174,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",9.2713788151741E-2,0.10204193741083099,0.13389131426811199,0.14095121622085599,0.16239483654499101,0.16224294900894201,0.16375647485256201,0.14995594322681399,0.14020641148090399,0.15006641933252199,0.15263521605198699,0.14623624096059401,0.15352078221208501,0.15773900631940699,0.163806270402307,0.151439390263017]
["BNSF-E1L209C5","BNSF",4,"E1L209C5",175,"CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",-6.0603003948926898E-2,-7.4406258761882796E-2,-5.94263933598995E-2,-6.5404869616031605E-2,-7.4448354542255402E-2,-4.6205468475818599E-2,-6.6666625440120697E-2,-8.5582919418811798E-2,-4.1430633515119601E-2,-6.7704506193210195E-2,-2.3763227941076E-2,-4.6237327655157499E-2,-0.107605231076462,-9.7635570025315796E-2,-5.6876947172966798E-2,-4.6913193540590703E-2]
["BNSF-E1L209C6","BNSF",4,"E1L209C6",176,"CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",4.9549717456102399E-2,2.3959616199135801E-2,2.4650728330016101E-2,2.1946627646684602E-2,7.4734459631145E-3,6.2729921191930797E-3,6.5833753906190404E-3,6.5410267561674101E-3,3.46806272864342E-3,3.3238813565909099E-3,3.7434966901330499E-3,3.8206062940049999E-3,3.5260995354906102E-3,2.5662388143961401E-3,9.6743537869285703E-2,0.112039243004325]
["BNSF-E1L209C7","BNSF",4,"E1L209C7",177,"CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",4.6071610450744602,5.0216856002807599,6.5722675323486301,7.0548882484436,8.1213350296020508,7.9825277328491202,7.9623274803161603,7.1516628265380904,6.58927345275879,7.0453445759267304,7.2729837024664601,7.0738574900859703,7.7458620296484204,8.2824101185788397,9.1396985706404905,8.5709574014177399]
["BNSF-E1L209C8","BNSF",4,"E1L209C8",178,"CD(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",-10.179205894470201,-11.3839921951294,-10.752718925476101,-5.8017311096191397,-9.9237575531005895,-7.2003440856933603,-6.15761041641235,-7.2869672775268599,-5.9690680503845197,-13.9264874701163,-23.8816792881384,-23.025119116419202,-35.980461048933201,-31.1999358216957,-22.748681274241001,-29.515202032896699]
["BNSF-E1L209C9","BNSF",4,"E1L209C9",179,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",3.5061242580413801,1.7006407976150499,1.71389019489288,1.54880034923553,0.429005116224289,0.34632942080497697,0.38301190733909601,0.35570353269576999,0.15702433884143799,0.161394414720643,0.184229123128303,0.18025374940614999,0.192259107896284,0.140208265228002,8.3297295052593494,9.4160802396621204]
["BNSF-E1L209C10","BNSF",4,"E1L209C10",180,"CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",4.6071610450744602,5.0216860771179199,6.5722675323486301,7.0548887252807599,8.1213350296020508,7.9825286865234402,7.9623274803161603,7.1516633033752397,6.5892744064331099,7.0453445759267401,7.2729837024664601,7.0738574900859703,7.7458620296484204,8.2824101185788397,9.1396985706404905,8.5709574014177399]
["BNSF-E1L209C11","BNSF",4,"E1L209C11",181,"CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",-10.179205894470201,-11.3839921951294,-10.752718925476101,-5.8017311096191397,-9.9237594604492205,-7.2003445625305202,-6.15761041641235,-7.2869672775268599,-5.9690685272216797,-13.9264874701163,-23.8816792881384,-23.025119116419202,-35.980461048933201,-31.199935821695799,-22.748681274241001,-29.515202032896699]
["BNSF-E1L209C12","BNSF",4,"E1L209C12",182,"CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",3.5061240196228001,1.7006407976150499,1.71389019489288,1.54880034923553,0.42900517582893399,0.34632942080497697,0.38301190733909601,0.35570353269576999,0.15702435374259899,0.161394414720643,0.184229123128303,0.18025374940614999,0.192259107896284,0.140208265228002,8.3297295052593494,9.4160802396621204]
["BNSF-E1L209C13","BNSF",4,"E1L209C13",183,"CM(R), DRL Expense, Privately-Owned, REFRIGERATED - MECH",3.9244486833922598E-4,1.8723508401308201E-4,1.6190003952942799E-4,2.15365987969562E-4,1.65827252203599E-4,7.1189895970746896E-4,8.8639213936403405E-4,1.0763371392386E-4,1.04480968730059E-4,3.9134411713082301E-4,4.6815473544930403E-4,6.5648843278026095E-4,7.02276994498786E-4,6.7938145774834298E-4,7.6907352627534199E-4,6.0245595957216197E-4]
["BNSF-E1L210C1","BNSF",4,"E1L210C1",184,"CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",1.3974029570817901E-2,1.4293372631073E-2,1.52764590457082E-2,1.51959946379066E-2,1.4057919383049001E-2,1.34918969124556E-2,1.41925401985645E-2,1.5485020354390099E-2,1.7254965379834199E-2,1.8786073132178501E-2,1.9537643912162599E-2,1.90063876374581E-2,2.2101973566009101E-2,2.65463908869467E-2,3.0985625615321599E-2,3.0012924878140099E-2]
["BNSF-E1L210C2","BNSF",4,"E1L210C2",185,"CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",3.8847720716148602E-3,-1.8323651747778099E-3,2.0398737397044901E-3,8.1472229212522507E-3,1.0624812915921201E-2,9.9973054602742195E-3,6.21127942577004E-3,6.1725927516818003E-3,1.3925075531005899E-2,2.5189956090843998E-2,2.7129250751545E-2,2.65116806761828E-2,3.07527201837451E-2,3.3020743792929498E-2,2.7835293693158101E-2,2.24046075527615E-2]
["BNSF-E1L210C3","BNSF",4,"E1L210C3",186,"CM(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",3.6824397742748302E-2,3.7612080574035603E-2,4.5524545013904599E-2,4.1444398462772397E-2,6.6189281642436995E-2,5.8171320706605897E-2,5.2536062896251699E-2,4.6267423778772403E-2,4.0631145238876301E-2,3.2197355343311501E-2,3.2092022413579002E-2,3.7838267585285398E-2,5.1993098358243901E-2,4.2131330036267602E-2,3.3240884836277303E-2,3.3143719978649899E-2]
["BNSF-E1L210C4","BNSF",4,"E1L210C4",187,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",3.6332476884126698E-2,3.7162795662879902E-2,3.9718724787235302E-2,3.95096391439438E-2,3.6550644785165801E-2,3.5078916698694201E-2,3.6900632083415999E-2,4.0261019021272701E-2,4.4862851500511197E-2,4.8843790143664002E-2,5.0797874171622501E-2,4.9416607857391E-2,5.74651312716239E-2,6.9020616306061294E-2,8.0562626599836304E-2,7.8033604683163907E-2]
["BNSF-E1L210C5","BNSF",4,"E1L210C5",188,"CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",1.0100412182509899E-2,-4.7641457058489297E-3,5.3036529570817904E-3,2.1182734519243199E-2,2.76244524866343E-2,2.59930472820997E-2,1.6149369999766398E-2,1.6048859804868702E-2,3.6205269396305098E-2,6.5493885836194296E-2,7.0536051954016701E-2,6.8930369758075094E-2,7.9957072477737201E-2,8.5853933861616299E-2,7.2371763602211397E-2,5.8251979637179901E-2]
["BNSF-E1L210C6","BNSF",4,"E1L210C6",189,"CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",9.5743358135223403E-2,9.77913662791252E-2,0.11836402118206001,0.107755221426487,0.172092169523239,0.15124548971653001,0.13659407198429099,0.120295114815235,0.105641111731529,8.3713123892609806E-2,8.3439258275305295E-2,9.8379495721742094E-2,0.13518205573143399,0.109541458094295,8.6426300574321699E-2,8.6173671944489702E-2]
["BNSF-E1L210C7","BNSF",4,"E1L210C7",190,"CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",1.57357597351074,1.62102091312408,1.7592705488205,1.80527448654175,1.7098853588104199,1.69196212291718,1.84119164943695,2.0192062854766801,2.20344209671021,2.3930332919508701,2.52411202648269,2.5369516803710801,3.02077600790963,3.6975423612671601,4.5488631501461896,4.4664746767756496]
["BNSF-E1L210C8","BNSF",4,"E1L210C8",191,"CD(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",11.728666305541999,12.231201171875,15.2017574310303,21.414257049560501,24.1042671203613,22.941389083862301,25.437938690185501,25.360582351684599,21.263475418090799,21.616398326079,29.719964582721399,29.3720528479775,45.560967103852597,50.168287774666297,26.300488056498899,22.391890849674098]
["BNSF-E1L210C9","BNSF",4,"E1L210C9",192,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",6.10559129714966,6.54428958892822,7.9034829139709499,7.5395474433898899,12.4548072814941,11.034618377685501,10.5419006347656,8.85443210601807,7.2414183616638201,6.3102553868804598,6.3859952961573301,7.3914307510672197,11.0458408790044,8.8759798345652303,7.5077757356918902,7.3026859049881399]
[{"$f":"B194&\"-\"&D194","v":"BNSF-E1L210C10"},"BNSF",4,"E1L210C10",193,"CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",1.57357585430145,1.62102127075195,1.75927066802979,1.80527460575104,1.7098855972289999,1.69196212291718,1.84119164943695,2.0192062854766801,2.20344209671021,2.3930332919508701,2.52411202648269,2.5369516803710801,3.02077600790963,3.6975423612671601,4.5488631501461896,4.4664746767756496]
["BNSF-E1L210C11","BNSF",4,"E1L210C11",194,"CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",11.728666305541999,12.231201171875,15.2017574310303,21.4142551422119,24.104270935058601,22.941389083862301,25.437940597534201,25.360582351684599,21.263473510742202,21.616398326079,29.719964582721399,29.3720528479775,45.560967103852597,50.168287774666297,26.300488056498899,22.391890849674098]
["BNSF-E1L210C12","BNSF",4,"E1L210C12",195,"CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",6.10559129714966,6.54428958892822,7.9034833908081099,7.5395464897155797,12.4548072814941,11.034618377685501,10.5418996810913,8.8544330596923793,7.2414183616638201,6.3102553868804598,6.3859952961573301,7.3914307510672197,11.0458408790044,8.8759798345652303,7.5077757356918902,7.3026859049881399]
["BNSF-E1L210C13","BNSF",4,"E1L210C13",196,"CM(R), DRL Expense, Privately-Owned, REFRIGERATED - NON-MECH",2.9705124907195598E-3,2.3101202677935401E-3,2.8603810351342002E-3,1.36569712776691E-3,6.1658658087253597E-3,4.1344626806676396E-3,4.6904264017939602E-3,5.3988406434655198E-3,2.3505091667175302E-3,2.7752482378409701E-3,4.5024843412803202E-4,2.8814301511837799E-4,4.2206856909553301E-4,2.7405929836366998E-4,2.6121506914516998E-4,1.4992614048417601E-4]
["BNSF-E1L211C1","BNSF",4,"E1L211C1",197,"CM(R), OPR Expense, Railroad-Owned, FLAT - TOFC",2.8554255142807999E-2,2.2796861827373501E-2,2.1079631522297901E-2,2.1318575367331501E-2,2.0472420379519501E-2,1.9028397276997601E-2,1.73049326986074E-2,1.44395558163524E-2,1.4202757738530599E-2,1.5814507972041002E-2,1.7708436135597701E-2,1.94756231765464E-2,2.42381187717352E-2,2.85944466648522E-2,3.2166713018459803E-2,3.4318876344616903E-2]
["BNSF-E1L211C2","BNSF",4,"E1L211C2",198,"CM(R), DRL Expense, Railroad-Owned, FLAT - TOFC",2.94925761409104E-3,9.9404260981827996E-4,4.4458417687565099E-4,3.3251519780606001E-3,1.06276688165963E-3,-1.90035242121667E-3,-3.3370656892657302E-3,-2.4455925449729E-3,-2.6778716128319502E-3,3.6248650059462302E-3,5.9872571994490304E-3,2.0570092035009399E-3,-1.6994046971159599E-2,-7.7640567763040602E-3,-9.0988319515049598E-3,-1.3354455600375501E-2]
["BNSF-E1L211C3","BNSF",4,"E1L211C3",199,"CM(R), ROI Expense, Railroad-Owned, FLAT - TOFC",1.09466910362244E-3,1.348837162368E-3,3.7831724621355499E-3,8.94734635949135E-3,9.5150535926222801E-3,1.7245169728994401E-2,1.8937176093459102E-2,1.7125288024544699E-2,1.7157537862658501E-2,1.3888011887444599E-2,1.12637630969648E-2,1.6012402638554302E-2,2.3582618501614999E-2,1.8227241864323299E-2,1.5455787741817301E-2,2.3896083576407601E-2]
["BNSF-E1L211C4","BNSF",4,"E1L211C4",200,"CM(Y), OPR Expense, Railroad-Owned, FLAT - TOFC",7.4241161346435505E-2,5.9271845966577502E-2,5.4806988686323201E-2,5.5428054183721501E-2,5.3228270262479803E-2,4.94738556444645E-2,4.49928566813469E-2,3.7542808800935697E-2,3.6927074193954502E-2,4.1117720727306302E-2,4.6041933952554001E-2,5.0636620259020299E-2,6.3019108806511806E-2,7.4345561328616E-2,8.3633453847995906E-2,8.9229078496004005E-2]
["BNSF-E1L211C5","BNSF",4,"E1L211C5",201,"CM(Y), DRL Expense, Railroad-Owned, FLAT - TOFC",7.6680909842252697E-3,2.5845123454928398E-3,1.15591322537512E-3,8.6453976109623892E-3,2.76320870034397E-3,-4.9409633502364202E-3,-8.6764059960842098E-3,-6.3586598262190801E-3,-6.9625149480998499E-3,9.4246490154601906E-3,1.5566868718567399E-2,5.3482239291023697E-3,-4.4184522125014801E-2,-2.0186547618390598E-2,-2.3656963073912698E-2,-3.4721584560976501E-2]
["BNSF-E1L211C6","BNSF",4,"E1L211C6",202,"CM(Y), ROI Expense, Railroad-Owned, FLAT - TOFC",2.8461385518312502E-3,3.5069726873189198E-3,9.8362257704138808E-3,2.3263080045580899E-2,2.4739060550928098E-2,4.48375716805458E-2,4.9236509948968901E-2,4.45258729159832E-2,4.4609718024730703E-2,3.6108830907356101E-2,2.92857840521085E-2,4.1632246860241098E-2,6.1314808104198697E-2,4.7390828847240399E-2,4.0185048128724699E-2,6.2129817298659698E-2]
["BNSF-E1L211C7","BNSF",4,"E1L211C7",203,"CD(R), OPR Expense, Railroad-Owned, FLAT - TOFC",4.0574388504028303,3.42051124572754,3.3171246051788299,3.4573502540588401,3.3698818683624299,3.16709184646606,2.9672515392303498,2.5329213142395002,2.48276567459106,2.7535216898304702,3.13544275455294,3.5611008265036799,4.4157224911864903,4.6459197409499202,4.9276504970842003,4.9569870216760696]
["BNSF-E1L211C8","BNSF",4,"E1L211C8",204,"CD(R), DRL Expense, Railroad-Owned, FLAT - TOFC",20.522506713867202,20.767625808715799,20.273485183715799,22.4758701324463,20.904708862304702,18.0469570159912,19.227058410644499,18.2117729187012,10.2882070541382,4.6810920423731304,2.2792936057863802,-3.41427283392707,6.0228739530756297,6.9373090070357497,7.3595329872580901,4.1771074812417002]
["BNSF-E1L211C9","BNSF",4,"E1L211C9",205,"CD(R), ROI Expense, Railroad-Owned, FLAT - TOFC",0.21333196759223899,0.27688515186309798,0.86279261112213101,2.21971535682678,2.2920379638671902,4.2207732200622603,5.1346449851989702,4.5041933059692401,4.2033019065856898,3.6795437139101699,3.1171302643860499,4.3048702825467098,6.1984415341452497,3.7312008529577101,3.4236250714477401,5.0846303726551501]
["BNSF-E1L211C10","BNSF",4,"E1L211C10",206,"CD(Y), OPR Expense, Railroad-Owned, FLAT - TOFC",4.0574388504028303,3.4205114841461199,3.3171253204345699,3.4573500156402601,3.3698818683624299,3.16709208488464,2.9672520160675,2.5329210758209202,2.48276567459106,2.7535216898304702,3.1354427545529302,3.5611008265036799,4.4157224911864903,4.6459197409499202,4.9276504970842003,4.9569870216760696]
["BNSF-E1L211C11","BNSF",4,"E1L211C11",207,"CD(Y), DRL Expense, Railroad-Owned, FLAT - TOFC",20.522506713867202,20.767625808715799,20.273485183715799,22.4758701324463,20.904708862304702,18.0469570159912,19.2270622253418,18.2117710113525,10.2882070541382,4.6810920423731304,2.2792936057863802,-3.41427283392707,6.0228739530756297,6.9373090070357497,7.3595329872580901,4.1771074812417002]
["BNSF-E1L211C12","BNSF",4,"E1L211C12",208,"CD(Y), ROI Expense, Railroad-Owned, FLAT - TOFC",0.21333195269107799,0.27688515186309798,0.86279261112213101,2.2197151184082,2.2920379638671902,4.2207732200622603,5.1346459388732901,4.5041928291320801,4.2033019065856898,3.6795437139101801,3.1171302643860499,4.3048702825467,6.1984415341452497,3.7312008529577101,3.4236250714477401,5.0846303726551501]
["BNSF-E1L211C13","BNSF",4,"E1L211C13",209,"CM(R), DRL Expense, Privately-Owned, FLAT - TOFC",0.148702457547188,0.14668799936771401,0.160789415240288,0.15391641855239899,0.13719196617603299,0.145672917366028,0.14707782864570601,0.145824119448662,0.154008999466896,0.14878933402245201,0.14336145401959599,0.14864210661878999,0.149849538836478,0.149313278779967,0.14326130230183601,0.14981519772195301]
["BNSF-E1L212C1","BNSF",4,"E1L212C1",210,"CM(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",1.91910949070007E-3,1.36183737777174E-3,1.8507897621020701E-3,2.0183806773275098E-3,2.2516520693898201E-3,1.81110436096787E-3,1.4806780964136099E-2,3.6272585391998298E-2,5.45368157327175E-2,6.5802366133758103E-2,7.2275165306339803E-2,7.0858312942475493E-2,6.7549924309164996E-2,6.9655954279201002E-2,6.76674002642393E-2,7.4366783080218907E-2]
["BNSF-E1L212C2","BNSF",4,"E1L212C2",211,"CM(R), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",6.9152586162090302E-2,7.8213572502136203E-2,5.3672328591346699E-2,6.0376852750778198E-2,5.5525694042444201E-2,5.7703748345375103E-2,4.0415231138467803E-2,5.96809163689613E-2,8.6155891418457003E-2,9.2762482247786299E-2,7.1244632003919603E-2,8.97640776848911E-2,6.6321506508993794E-2,6.7875551576624907E-2,5.5291094597586098E-2,5.3642351614849502E-2]
["BNSF-E1L212C3","BNSF",4,"E1L212C3",212,"CM(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",3.4819804131984697E-2,1.5944670885801301E-2,4.7150421887636199E-2,8.0527275800704998E-2,0.142104312777519,0.12790283560752899,8.7864898145198794E-2,0.112703740596771,0.134015753865242,0.13193574077405401,0.11832159055130501,0.12190708161033501,0.14869189406045299,0.102636238431922,9.3756771254565704E-2,0.12779720841025899]
["BNSF-E1L212C4","BNSF",4,"E1L212C4",213,"CM(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",4.9896892160177196E-3,3.5407806281000402E-3,4.8120515421032897E-3,5.2477917633950702E-3,5.8542839251458601E-3,4.7088731080293699E-3,3.8497604429721798E-2,9.4308711588382693E-2,0.14179557561874401,0.17108615194777099,0.18791542979648401,0.184231613650437,0.17562980320382801,0.18110548112592201,0.17593524068702199,0.193353636008569]
["BNSF-E1L212C5","BNSF",4,"E1L212C5",214,"CM(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",0.17979708313942,0.20335511863231701,0.13954804837703699,0.15697968006134,0.14436666667461401,0.15002959966659499,0.10507981479167899,0.15517032146453899,0.22400538623332999,0.241182453844245,0.18523604321018999,0.23338660198071601,0.172435916923384,0.176476434099225,0.14375684595372401,0.139470114198609]
["BNSF-E1L212C6","BNSF",4,"E1L212C6",215,"CM(Y), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",9.0531691908836406E-2,4.1456103324890102E-2,0.12259098887443499,0.20937101542949699,0.36947146058082603,0.33254685997963002,0.22844870388507801,0.29302942752838101,0.34844121336937001,0.34303292601254098,0.30763613543339102,0.31695841218687099,0.38659892455717698,0.26685421992299801,0.243767605261871,0.33227274186667499]
["BNSF-E1L212C7","BNSF",4,"E1L212C7",216,"CD(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",0.25056502223014798,0.17736507952213301,0.24634847044944799,0.27601596713066101,0.31342044472694403,0.24890644848346699,1.98297679424286,4.85670709609985,7.2675256729126003,8.9369149180683305,10.026370492029599,10.2101127357412,9.8517205315971008,9.3132706303376196,8.8073074540280594,9.2071032023041894]
["BNSF-E1L212C8","BNSF",4,"E1L212C8",217,"CD(R), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",55.646213531494098,60.002605438232401,63.970546722412102,70.055000305175795,59.430004119872997,48.5746040344238,41.141685485839801,40.680160522460902,51.686843872070298,13.411490685991099,61.775503641777,65.141520491075198,8.6037857903175894,-9.43230746681391,-7.37786041976908,-2.0149988944689401]
["BNSF-E1L212C9","BNSF",4,"E1L212C9",218,"CD(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",6.7384114265441903,2.8876490592956499,9.5082912445068395,17.2709350585938,29.176601409912099,25.1209926605225,17.4699897766113,22.732841491699201,25.9866752624512,27.740151113590599,25.380759013587902,26.229104625112701,32.135622773047999,17.794935656966398,18.139267393697601,23.476581062786501]
["BNSF-E1L212C10","BNSF",4,"E1L212C10",219,"CD(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",0.25056502223014798,0.17736507952213301,0.24634848535060899,0.27601599693298301,0.31342041492462203,0.24890643358230599,1.98297691345215,4.8567066192626998,7.2675256729126003,8.9369149180683305,10.026370492029599,10.2101127357412,9.8517205315971008,9.3132706303376196,8.8073074540280594,9.2071032023041894]
["BNSF-E1L212C11","BNSF",4,"E1L212C11",220,"CD(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",55.646217346191399,60.002605438232401,63.970558166503899,70.055000305175795,59.430007934570298,48.5746040344238,41.141685485839801,40.680160522460902,51.686847686767599,13.411490685991099,61.775503641777,65.141520491075198,8.6037857903175894,-9.4323074668138993,-7.37786041976908,-2.0149988944689401]
["BNSF-E1L212C12","BNSF",4,"E1L212C12",221,"CD(Y), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",6.7384114265441903,2.8876488208770801,9.5082912445068395,17.2709350585938,29.176601409912099,25.1209926605225,17.46999168396,22.732841491699201,25.9866752624512,27.740151113590599,25.380759013587799,26.229104625112701,32.135622773047999,17.794935656966398,18.139267393697601,23.476581062786501]
["BNSF-E1L212C13","BNSF",4,"E1L212C13",222,"CM(R), DRL Expense, Privately-Owned, FLAT - MULTILEVEL",0.16249170899391199,0.16849344968795801,0.20164796710014299,0.21305528283119199,0.21952658891677901,0.18548059463500999,0.15666911005973799,0.17894980311393699,0.20443540811538699,0.196957267428749,0.23067776109580199,0.24743418857452601,0.23843070637206801,0.255928551028683,0.30438877375944601,0.27401690461818301]
["BNSF-E1L213C1","BNSF",4,"E1L213C1",223,"CM(R), OPR Expense, Railroad-Owned, FLAT - GENERAL",2.0648159980773899,2.4697606563568102,2.4764659404754599,2.8126666545867902,2.7423782348632799,3.1237442493438698,2.9965975284576398,1.8450914621353101,0.89706289768219005,5.5832669171296201E-2,6.5735963567344693E-2,7.9432393514618893E-2,0.10371582985759099,0.10349905985707999,0.12376913372239901,8.2957644767535796E-2]
["BNSF-E1L213C2","BNSF",4,"E1L213C2",224,"CM(R), DRL Expense, Railroad-Owned, FLAT - GENERAL",8.8698089122772203E-2,7.61541277170181E-2,8.0664910376071902E-2,8.5147693753242507E-2,8.8367864489555401E-2,7.2201386094093295E-2,6.52926340699196E-2,5.8445181697606999E-2,5.74810691177845E-2,6.7359226948744202E-3,-1.79732801458393E-2,-4.6616024196595301E-3,2.37623357403275E-2,8.3441094236099606E-2,2.5002929025798201E-2,2.0529721436057399E-2]
["BNSF-E1L213C3","BNSF",4,"E1L213C3",225,"CM(R), ROI Expense, Railroad-Owned, FLAT - GENERAL",0.1111870855093,0.11487906426191299,0.10872669517993901,0.14360098540782901,0.13748414814472201,0.129710808396339,0.11555356532335299,9.5914267003536197E-2,7.3084905743598896E-2,5.4138906677857299E-2,3.4067734520693699E-2,6.0252651114641398E-2,6.1358863330485798E-2,2.5499440486423,4.1416988872669598E-2,4.18564475853535E-2]
["BNSF-E1L213C4","BNSF",4,"E1L213C4",226,"CM(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL",5.3685226440429696,6.4213833808898899,6.43882083892822,7.3129229545593297,7.1301736831665004,8.1217374801635707,7.7911562919616699,4.7972388267517099,2.33236479759216,0.14516493984536999,0.17091350527509599,0.20652422313801,0.26966115762973603,0.26909755562840798,0.32179974767823899,0.215689876395594]
["BNSF-E1L213C5","BNSF",4,"E1L213C5",227,"CM(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",0.230615109205246,0.19800059497356401,0.209728583693504,0.221384271979332,0.22975672781467399,0.18772362172603599,0.16976079344749501,0.151957392692566,0.14945076406002,1.7513399006673602E-2,-4.67305283791822E-2,-1.21201662911147E-2,6.17820729248513E-2,0.21694684501386,6.5007615467075494E-2,5.3377275733749299E-2]
["BNSF-E1L213C6","BNSF",4,"E1L213C6",228,"CM(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL",0.28908658027648898,0.29868543148040799,0.28268885612487799,0.37336286902427701,0.357459217309952,0.33724811673164401,0.30043905973434398,0.24937689304351801,0.19002085924148601,0.14076115736243,8.8576109753803395E-2,0.156656892898067,0.15953304465926299,6.6298545264699804,0.107684171068941,0.108826763721919]
["BNSF-E1L213C7","BNSF",4,"E1L213C7",229,"CD(R), OPR Expense, Railroad-Owned, FLAT - GENERAL",232.37170410156301,286.26467895507801,311.27264404296898,356.29302978515602,312.94461059570301,290.11462402343801,259.36221313476602,161.06710815429699,79.575515747070298,5.6883647102716903,7.6210912320249999,10.0569289861899,13.6125655687293,14.206005597636601,17.915887254544,11.791865555925201]
["BNSF-E1L213C8","BNSF",4,"E1L213C8",230,"CD(R), DRL Expense, Railroad-Owned, FLAT - GENERAL",12.329003334045399,14.149960517883301,15.683134078979499,7.9323587417602504,7.0884780883789098,6.8267316818237296,6.4912543296814,7.1894688606262198,13.1020975112915,3.0349265728829899,-5.7892954715687397,-2.7326585911391401,9.74954572333424,21.560636252554598,6.03721099971533,10.116703843231599]
["BNSF-E1L213C9","BNSF",4,"E1L213C9",231,"CD(R), ROI Expense, Railroad-Owned, FLAT - GENERAL",15.7082109451294,17.5532417297363,18.361660003662099,17.603569030761701,14.0928592681885,14.1499366760254,11.2472991943359,10.261945724487299,9.3312854766845703,10.576617162498501,6.5006195188593203,10.935124432569101,13.189250928862601,538.92354378958998,8.9327880824808297,8.5249331286963805]
["BNSF-E1L213C10","BNSF",4,"E1L213C10",232,"CD(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL",232.37171936035199,286.26467895507801,311.27261352539102,356.29302978515602,312.944580078125,290.11462402343801,259.36221313476602,161.06710815429699,79.575515747070298,5.6883647102716903,7.6210912320249902,10.0569289861899,13.6125655687293,14.206005597636601,17.915887254544,11.791865555925201]
["BNSF-E1L213C11","BNSF",4,"E1L213C11",233,"CD(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",12.329002380371101,14.149960517883301,15.6831350326538,7.9323582649231001,7.0884771347045898,6.8267307281494096,6.4912543296814,7.1894688606262198,13.1020965576172,3.0349265728829899,-5.7892954715687397,-2.7326585911391401,9.74954572333424,21.560636252554598,6.03721099971533,10.116703843231599]
["BNSF-E1L213C12","BNSF",4,"E1L213C12",234,"CD(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL",15.7082109451294,17.5532417297363,18.361660003662099,17.6035671234131,14.092858314514199,14.1499366760254,11.2472991943359,10.261945724487299,9.3312864303588903,10.576617162498501,6.5006195188593203,10.935124432569101,13.189250928862601,538.92354378958998,8.9327880824808297,8.5249331286963805]
["BNSF-E1L213C13","BNSF",4,"E1L213C13",235,"CM(R), DRL Expense, Privately-Owned, FLAT - GENERAL",0.20353817939758301,0.18649034202098799,0.125092163681984,0.21637488901615101,1.33765304088593,0.38920992612838701,0.25932714343071001,0.19751507043838501,0.181483224034309,0.21711600568241499,6.8035128019982097E-4,0.15220748938395701,0.17475414104526099,0.169112151105106,0.182042336300304,0.20683789889653101]
["BNSF-E1L214C1","BNSF",4,"E1L214C1",236,"CM(R), OPR Expense, Railroad-Owned, FLAT - OTHER",4.10186164081097E-2,4.4868499040603603E-2,5.29365800321102E-2,5.6651424616575199E-2,5.18784634768963E-2,4.9599599093198797E-2,5.2544526755809798E-2,5.5993121117353398E-2,6.0240879654884297E-2,6.2147673463376199E-2,5.7008792753933002E-2,5.1935854632750501E-2,5.5730695240617301E-2,6.1620246464599397E-2,6.5929756258339398E-2,6.0333432662109103E-2]
["BNSF-E1L214C2","BNSF",4,"E1L214C2",237,"CM(R), DRL Expense, Railroad-Owned, FLAT - OTHER",2.9946893453598002E-2,2.3993866518139801E-2,2.2881764918565799E-2,2.3969251662492801E-2,2.26982794702053E-2,2.9615962877869599E-2,2.4837272241711599E-2,2.4878943338990201E-2,2.5626229122281099E-2,3.6195814793229503E-2,3.4649010694629799E-2,3.40397092110283E-2,3.5944597042773301E-2,3.6860273336855001E-2,3.7436887382889E-2,3.4474880262323503E-2]
["BNSF-E1L214C3","BNSF",4,"E1L214C3",238,"CM(R), ROI Expense, Railroad-Owned, FLAT - OTHER",1.00791295990348E-2,2.6816992089152301E-2,3.1344320625066799E-2,1.6038859263062501E-2,8.7399724870920199E-3,1.94001216441393E-2,7.7671138569712604E-3,7.6545677147805699E-3,6.2251184135675404E-3,5.6550230657033103E-3,4.4249224449770096E-3,4.7843438428231497E-3,6.7111106648387996E-3,8.8546774647916392E-3,8.1766429746172493E-3,9.4317535083103705E-3]
["BNSF-E1L214C4","BNSF",4,"E1L214C4",239,"CM(Y), OPR Expense, Railroad-Owned, FLAT - OTHER",0.106648527085781,0.116658180952072,0.137635037302971,0.147293850779533,0.134884268045425,0.128958866000175,0.136615514755249,0.145581930875778,0.15662635862827301,0.16158395100477799,0.14822286116022601,0.135033222045151,0.144899807625605,0.160212640807958,0.171417366271682,0.15686692492148299]
["BNSF-E1L214C5","BNSF",4,"E1L214C5",240,"CM(Y), DRL Expense, Railroad-Owned, FLAT - OTHER",7.7861942350864397E-2,6.2384087592363399E-2,5.9492561966180801E-2,6.23199753463268E-2,5.90155422687531E-2,7.7001504600048107E-2,6.4576916396617903E-2,6.4685203135013594E-2,6.6628277301788302E-2,9.4109118462396599E-2,9.0087427806037498E-2,8.8503243948673802E-2,9.3455952311210802E-2,9.5836710675822806E-2,9.7335907195511301E-2,8.9634688682040997E-2]
["BNSF-E1L214C6","BNSF",4,"E1L214C6",241,"CM(Y), ROI Expense, Railroad-Owned, FLAT - OTHER",2.6205752044916202E-2,6.9724246859550504E-2,8.1495158374309498E-2,4.1700948029756497E-2,2.2723926231265099E-2,5.0440326333046001E-2,2.0194476470351198E-2,1.9901864230632799E-2,1.61853451281786E-2,1.4703059970828601E-2,1.15047983569403E-2,1.24392939913402E-2,1.74488877285809E-2,2.3022161408458201E-2,2.1259271734004801E-2,2.4522559121607002E-2]
["BNSF-E1L214C7","BNSF",4,"E1L214C7",242,"CD(R), OPR Expense, Railroad-Owned, FLAT - OTHER",4.9095320701599103,5.3281383514404297,6.1835951805114702,6.7494926452636701,6.2130208015441903,5.8746519088745099,6.1067957878112802,6.3927917480468803,6.7521028518676802,6.9963183797465502,6.6277560385815404,6.2546768906988301,6.8002445428627203,7.5164598744956601,8.3781443395289692,7.7578627257783603]
["BNSF-E1L214C8","BNSF",4,"E1L214C8",243,"CD(R), DRL Expense, Railroad-Owned, FLAT - OTHER",15.0074272155762,14.420524597168001,15.0146188735962,16.1834506988525,13.8693542480469,11.884396553039601,10.7136993408203,10.9035654067993,13.3208465576172,16.994850310123201,17.298075005760602,17.1438881530161,20.241465678271702,20.3860508636606,18.535354692203601,16.991517849424898]
["BNSF-E1L214C9","BNSF",4,"E1L214C9",244,"CD(R), ROI Expense, Railroad-Owned, FLAT - OTHER",1.6800897121429399,4.6232132911682102,5.3737144470214799,2.8255379199981698,1.4581493139267001,3.2056138515472399,1.26669120788574,1.20961689949036,0.92015004158019997,0.90099496467734197,0.74884666026919899,0.78800988213234002,1.13618863548886,1.56763619189515,1.58395840389067,1.6921900011220301]
["BNSF-E1L214C10","BNSF",4,"E1L214C10",245,"CD(Y), OPR Expense, Railroad-Owned, FLAT - OTHER",4.9095320701599103,5.3281378746032697,6.1835956573486301,6.7494921684265101,6.2130208015441903,5.8746519088745099,6.1067957878112802,6.3927917480468803,6.7521033287048304,6.9963183797465502,6.6277560385815404,6.2546768906988301,6.8002445428627203,7.5164598744956601,8.3781443395289692,7.7578627257783603]
["BNSF-E1L214C11","BNSF",4,"E1L214C11",246,"CD(Y), DRL Expense, Railroad-Owned, FLAT - OTHER",15.0074272155762,14.420524597168001,15.0146179199219,16.1834506988525,13.8693542480469,11.884396553039601,10.7136993408203,10.903567314147899,13.3208456039429,16.994850310123201,17.298075005760602,17.1438881530161,20.241465678271702,20.3860508636606,18.535354692203601,16.991517849424898]
["BNSF-E1L214C12","BNSF",4,"E1L214C12",247,"CD(Y), ROI Expense, Railroad-Owned, FLAT - OTHER",1.6800898313522299,4.6232137680053702,5.3737144470214799,2.8255379199981698,1.4581493139267001,3.2056138515472399,1.26669120788574,1.20961701869965,0.92015010118484497,0.90099496467734197,0.74884666026919899,0.78800988213234002,1.13618863548886,1.56763619189515,1.58395840389067,1.6921900011220301]
["BNSF-E1L214C13","BNSF",4,"E1L214C13",248,"CM(R), DRL Expense, Privately-Owned, FLAT - OTHER",0.19210174679756201,0.20361904799938199,0.23239223659038499,0.30522000789642301,0.28790941834449801,0.25590619444847101,0.25920963287353499,0.28555953502655002,0.28196761012077298,0.25709146151545098,0.25202453320677798,0.27247148420669898,0.31249739396094001,0.375302114748437,0.33013526591571102,0.299135686526045]
["BNSF-E1L215C1","BNSF",4,"E1L215C1",249,"CM(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C2","BNSF",4,"E1L215C2",250,"CM(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,6.6357799805700796E-3,0,5.9061041101813299E-3,7.7132411563786696E-3,2.0364370713935802E-3,1.25145679412598E-3,6.3202660684147903E-4,8.2523039278062902E-4,7.31689171218432E-4,8.0704928668343904E-4]
["BNSF-E1L215C3","BNSF",4,"E1L215C3",251,"CM(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C4","BNSF",4,"E1L215C4",252,"CM(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C5","BNSF",4,"E1L215C5",253,"CM(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C6","BNSF",4,"E1L215C6",254,"CM(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C7","BNSF",4,"E1L215C7",255,"CD(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C8","BNSF",4,"E1L215C8",256,"CD(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B258&\"-\"&D258","v":"BNSF-E1L215C9"},"BNSF",4,"E1L215C9",257,"CD(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C10","BNSF",4,"E1L215C10",258,"CD(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C11","BNSF",4,"E1L215C11",259,"CD(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C12","BNSF",4,"E1L215C12",260,"CD(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L215C13","BNSF",4,"E1L215C13",261,"CM(R), DRL Expense, Privately-Owned, TANK <22,000 GAL",2.06507965922356E-2,1.3534381985664401E-2,1.1674942448735201E-2,8.5571240633726103E-3,9.7629809752106701E-3,8.2201315090060199E-3,6.6357799805700796E-3,5.3326943889260301E-3,5.9061041101813299E-3,7.7132411563786696E-3,2.0364370713935802E-3,1.25145679412598E-3,6.3202660684147903E-4,8.2523039278062902E-4,7.31689171218432E-4,8.0704928668343904E-4]
["BNSF-E1L216C1","BNSF",4,"E1L216C1",262,"CM(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C2","BNSF",4,"E1L216C2",263,"CM(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,8.5003961203255998E-7,0,7.4272528290748596E-3,4.9093572760489298E-5,9.2121051893055697E-5,7.2573270256587804E-5,3.7014535344951E-7,4.8286719475096399E-3,1.6203420081015699E-6,1.19082687881707E-6]
["BNSF-E1L216C3","BNSF",4,"E1L216C3",264,"CM(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C4","BNSF",4,"E1L216C4",265,"CM(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C5","BNSF",4,"E1L216C5",266,"CM(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C6","BNSF",4,"E1L216C6",267,"CM(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C7","BNSF",4,"E1L216C7",268,"CD(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C8","BNSF",4,"E1L216C8",269,"CD(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C9","BNSF",4,"E1L216C9",270,"CD(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C10","BNSF",4,"E1L216C10",271,"CD(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C11","BNSF",4,"E1L216C11",272,"CD(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C12","BNSF",4,"E1L216C12",273,"CD(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L216C13","BNSF",4,"E1L216C13",274,"CM(R), DRL Expense, Privately-Owned, TANK >=22,000 GAL",4.7623519785702203E-3,1.49050098843873E-3,2.18772776424885E-2,5.5199541384354201E-4,1.73372458666563E-2,4.9496487918077003E-5,8.5003961203255998E-7,5.3975663831806699E-6,7.4272528290748596E-3,4.9093572760489298E-5,9.2121051893055697E-5,7.2573270256587804E-5,3.7014535344951E-7,4.8286719475096399E-3,1.6203420081015699E-6,1.19082687881707E-6]
["BNSF-E1L217C1","BNSF",4,"E1L217C1",275,"CM(R), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",9.1594964265823406E-2,0.16740678250789601,0.52023530006408703,0.56847518682479903,0.43212509155273399,0.34970894455909701,0.32657089829444902,0.33068767189979598,0.36015149950981101,0.55439615918152096,0.807310531016736,1.2829769345264801,1.1320107605721901,1.5938938072789499,2.3815473750459502,4.23847494965087]
["BNSF-E1L217C2","BNSF",4,"E1L217C2",276,"CM(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",3.82105843164027E-3,2.6214940007776E-3,5.8030872605740998E-3,6.2890653498470801E-3,5.1658470183610899E-3,5.1178960129618601E-3,4.75279800593853E-3,5.1969676278531603E-3,5.0937179476022703E-3,3.7662805681328002E-2,8.7468628392494599E-2,8.3801688284309603E-2,5.4759688246525801E-2,0.13667832063811999,0.246280232959916,0.16452453252583399]
["BNSF-E1L217C3","BNSF",4,"E1L217C3",277,"CM(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",1.72751266509295E-2,3.1546600162982899E-2,3.32684367895126E-2,2.1766267716884599E-2,1.8223065882921202E-2,1.53849488124251E-2,1.3444609940052E-2,1.3723692856728999E-2,1.4177659526467301E-2,5.2277133270573498E-2,4.2766186592910697E-2,4.4958331380282199E-2,3.5690852802174801E-2,7.6963075778839193E-2,8.3208999002013104E-2,0.11546029343179399]
["BNSF-E1L217C4","BNSF",4,"E1L217C4",278,"CM(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.238146811723709,0.43525785207748402,1.35261189937592,1.4780356884002701,1.12352502346039,0.909243404865265,0.84908419847488403,0.85978794097900402,0.93639421463012695,1.44143001387195,2.0990073806435099,3.33574002976885,2.9432279774876999,4.1441238989252804,6.1920231751194699,11.020034869092299]
["BNSF-E1L217C5","BNSF",4,"E1L217C5",279,"CM(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",9.9347522482275998E-3,6.8158847279846703E-3,1.5088029205799099E-2,1.6351575031876599E-2,1.3431203551590399E-2,1.3306526467204099E-2,1.23572750017047E-2,1.3512113131582701E-2,1.32436640560627E-2,9.7923294771452701E-2,0.22741843382048599,0.217884389539205,0.142375189440967,0.355363633659111,0.64032860569578198,0.42776378456716802]
["BNSF-E1L217C6","BNSF",4,"E1L217C6",280,"CM(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",4.4915329664945602E-2,8.2021154463291196E-2,8.6497940123081193E-2,5.6592296808958102E-2,4.7379974275827401E-2,4.0000859647989301E-2,3.4955985844135298E-2,3.5681601613760001E-2,3.6861907690763501E-2,0.135920546503491,0.111192085141568,0.116891661588734,9.2796217285654403E-2,0.20010399702498199,0.21634339740523401,0.30019676292266301]
["BNSF-E1L217C7","BNSF",4,"E1L217C7",281,"CD(R), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",6.2711563110351598,8.2835216522216797,9.5908346176147496,12.465729713439901,9.4988708496093803,7.6185402870178196,6.5462808609008798,6.7868480682373002,7.5360198020935103,8.8645369062423605,9.3471245751667595,8.2242325015926099,7.4119643359827503,10.3623282362088,15.8336833223015,31.527147630590399]
["BNSF-E1L217C8","BNSF",4,"E1L217C8",282,"CD(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.985712230205536,0.56342422962188698,0.60453003644943204,1.68500196933746,1.3390653133392301,1.32786321640015,1.3062219619751001,1.3723291158676101,1.02557444572449,2.5225202378407801,1.1628640786376301,0.391002982229742,1.1023815340182599,5.5801774101872104,0.33624483573907998,0.65779621125121701]
["BNSF-E1L217C9","BNSF",4,"E1L217C9",283,"CD(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.440375685691834,0.71805691719055198,0.74462765455246005,0.78650969266891502,0.44574621319770802,0.369485914707184,0.33455964922905002,0.34932291507720897,0.35109072923660301,0.388606400790732,0.35303859152335598,0.34229805335803398,0.25629033891617498,0.57208314828356599,0.63428076824945701,0.90741428764106402]
["BNSF-E1L217C10","BNSF",4,"E1L217C10",284,"CD(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",6.2711563110351598,8.2835216522216797,9.5908346176147496,12.4657278060913,9.4988727569580096,7.6185398101806596,6.5462808609008798,6.7868480682373002,7.5360198020935103,8.8645369062423605,9.3471245751667595,8.2242325015926099,7.4119643359827503,10.3623282362088,15.8336833223015,31.527147630590399]
["BNSF-E1L217C11","BNSF",4,"E1L217C11",285,"CD(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.985712230205536,0.56342422962188698,0.60452991724014304,1.68500208854675,1.3390654325485201,1.32786321640015,1.3062219619751001,1.3723291158676101,1.02557444572449,2.5225202378407801,1.1628640786376301,0.391002982229742,1.1023815340182599,5.5801774101872104,0.33624483573907998,0.65779621125121701]
["BNSF-E1L217C12","BNSF",4,"E1L217C12",286,"CD(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.44037574529647799,0.71805691719055198,0.74462759494781505,0.78650975227356001,0.44574624300003102,0.369485914707184,0.33455964922905002,0.34932291507720897,0.35109072923660301,0.388606400790732,0.35303859152335598,0.34229805335803398,0.25629033891617498,0.57208314828356599,0.63428076824945701,0.90741428764106402]
["BNSF-E1L217C13","BNSF",4,"E1L217C13",287,"CM(R), DRL Expense, Privately-Owned, ALL OTHER FREIGHT CARS",6.1039678985252998E-4,4.2006146395579002E-4,2.0851322915405E-4,1.08938293124083E-4,2.0253703405614899E-4,7.7554745075758506E-5,1.86140276491642E-2,4.3045300990343101E-2,2.6380794122815101E-2,0,2.7272776629487598E-4,0,0,0,3.6406961096743698E-5,0]
["BNSF-E1L218C1","BNSF",4,"E1L218C1",288,"CM(R), OPR Expense, Railroad-Owned, AUTO RACKS",0,0,0,0,0,0,0,0,0,0,0,0,1.13619870194933E-3,3.1731590977869999E-3,3.8419893999470699E-3,3.3812778078270399E-3]
["BNSF-E1L218C2","BNSF",4,"E1L218C2",289,"CM(R), DRL Expense, Railroad-Owned, AUTO RACKS",3.4632839262485497E-2,5.3744971752166699E-2,3.1186986714601499E-2,3.5504344850778601E-2,1.22404871508479E-2,1.4076454564929E-2,1.0043220594525301E-2,1.3442339375615101E-2,4.50247265398502E-2,4.9586861571426097E-2,5.0617946640025599E-2,5.1818316707156101E-2,5.0594845782367497E-2,5.4707619781824299E-2,3.9150612018365297E-2,4.1978649413980398E-2]
["BNSF-E1L218C3","BNSF",4,"E1L218C3",290,"CM(R), ROI Expense, Railroad-Owned, AUTO RACKS",2.9090907424688301E-2,1.0309578850865401E-2,1.55636817216873E-2,8.5742603987455403E-3,2.1765358746051799E-2,1.7965946346521398E-2,1.15866828709841E-2,5.3813759237527799E-2,7.9487770795822102E-2,7.8210414081677004E-2,7.0351844197132293E-2,7.3584778417130695E-2,9.9831453782191507E-2,6.9246984217240501E-2,6.2749118501194606E-2,8.6304795314469399E-2]
["BNSF-E1L218C4","BNSF",4,"E1L218C4",291,"CM(Y), OPR Expense, Railroad-Owned, AUTO RACKS",0,0,0,0,0,0,0,0,0,0,0,0,2.9541166250682499E-3,8.2502136542461808E-3,9.9891724398623906E-3,8.7913223003502992E-3]
["BNSF-E1L218C5","BNSF",4,"E1L218C5",292,"CM(Y), DRL Expense, Railroad-Owned, AUTO RACKS",9.0045548975467696E-2,0.13973684608936299,8.1086233258247403E-2,9.2311188578605693E-2,3.1825270503759398E-2,3.6598753184080103E-2,2.6112370193004601E-2,3.4950088709592798E-2,0.11706425249576601,0.12892584008570801,0.131606661264066,0.134727623438606,0.131546599034156,0.142239811432743,0.10179159124775,0.10914448847635]
["BNSF-E1L218C6","BNSF",4,"E1L218C6",293,"CM(Y), ROI Expense, Railroad-Owned, AUTO RACKS",7.5636513531207997E-2,2.6804896071553199E-2,4.0465522557496997E-2,2.2293034940957999E-2,5.6589934974908801E-2,4.6711437404155703E-2,3.0125405639410002E-2,0.13991579413413999,0.20666825771331801,0.20334707661236101,0.18291479491254301,0.19132042388453899,0.25956177983369799,0.180042158964826,0.163147708103106,0.22439246781762101]
["BNSF-E1L218C7","BNSF",4,"E1L218C7",294,"CD(R), OPR Expense, Railroad-Owned, AUTO RACKS",0,0,0,0,0,0,0,0,0,0,0,0,0.16570724829738301,0.424263650345719,0.50005736511696597,0.41862471983953897]
["BNSF-E1L218C8","BNSF",4,"E1L218C8",295,"CD(R), DRL Expense, Railroad-Owned, AUTO RACKS",47.757545471191399,47.564601898193402,45.597644805908203,58.4919242858887,42.330810546875,31.733339309692401,27.880186080932599,26.7308673858643,33.552089691162102,37.978121904832598,62.600173949001899,60.023019404209002,21.448139917415698,5.8016687794441699,8.7016045439821106,11.8006334305786]
["BNSF-E1L218C9","BNSF",4,"E1L218C9",296,"CD(R), ROI Expense, Railroad-Owned, AUTO RACKS",5.6220650672912598,1.7926931381225599,3.0566654205322301,1.7059962749481199,4.4346947669982901,3.4999077320098899,2.2873275279998802,10.883994102478001,15.438290596008301,16.468037468585798,15.1182083012379,15.853531136939599,21.610169719610901,12.019211703623601,12.1793412118175,15.9211235214336]
["BNSF-E1L218C10","BNSF",4,"E1L218C10",297,"CD(Y), OPR Expense, Railroad-Owned, AUTO RACKS",0,0,0,0,0,0,0,0,0,0,0,0,0.16570724829738301,0.424263650345719,0.50005736511696597,0.41862471983953897]
["BNSF-E1L218C11","BNSF",4,"E1L218C11",298,"CD(Y), DRL Expense, Railroad-Owned, AUTO RACKS",47.7575492858887,47.564601898193402,45.597652435302699,58.4919242858887,42.330814361572301,31.733339309692401,27.8801879882813,26.7308673858643,33.552089691162102,37.978121904832598,62.600173949001899,60.023019404209002,21.448139917415698,5.8016687794441699,8.7016045439821106,11.8006334305786]
["BNSF-E1L218C12","BNSF",4,"E1L218C12",299,"CD(Y), ROI Expense, Railroad-Owned, AUTO RACKS",5.6220650672912598,1.7926931381225599,3.0566654205322301,1.7059961557388299,4.4346952438354501,3.4999077320098899,2.2873275279998802,10.883994102478001,15.438291549682599,16.468037468585798,15.1182083012379,15.853531136939599,21.610169719610901,12.019211703623601,12.1793412118175,15.9211235214336]
["BNSF-E1L218C13","BNSF",4,"E1L218C13",300,"CM(R), DRL Expense, Privately-Owned, AUTO RACKS",6.3535362482070895E-2,6.4931511878967299E-2,8.0567963421344799E-2,8.5829347372055095E-2,8.5196934640407604E-2,6.7277163267135606E-2,5.2122741937637301E-2,6.4062394201755496E-2,8.2053788006305695E-2,8.6290493400995205E-2,0.230212775202464,0.11249021477389599,0.10752042290984801,0.114053724229432,0.13596620550796601,0.121893351622805]
["BNSF-E1L219C1","BNSF",4,"E1L219C1",301,"CM(R), OPR Expense, Railroad-Owned, ACCESSORIAL",3.0973867978900698E-5,6.3817227783147205E-5,7.9233344877138707E-5,9.5541290647815899E-5,4.4122887629782801E-5,8.6602885858155801E-5,1.61424977704883E-4,2.1383850253187101E-4,2.1531255333684401E-4,2.0352582269146999E-4,1.8525678406739301E-4,1.20917779979517E-4,4.6411328851024902E-5,5.748652979675E-6,0,0]
["BNSF-E1L219C2","BNSF",4,"E1L219C2",302,"CM(R), DRL Expense, Railroad-Owned, ACCESSORIAL",5.9797894209623303E-5,2.2911188716534501E-4,7.2140002157539097E-4,9.1207859804853797E-4,1.1200972367078101E-3,1.40493840444833E-3,1.4650896191597E-3,1.7909843008965299E-3,2.16605165041983E-3,1.73681493487184E-3,1.89543007812388E-3,1.46146436617536E-3,1.18048122319412E-3,9.68221595983423E-4,1.4226742910302E-3,1.45641715035104E-3]
["BNSF-E1L219C3","BNSF",4,"E1L219C3",303,"CM(R), ROI Expense, Railroad-Owned, ACCESSORIAL",1.2898066779598599E-4,2.9666780028492201E-4,5.6779483566060695E-4,3.6003897548653202E-4,1.5258394414559E-3,1.54085096437484E-3,1.50800938718021E-3,1.67654606048018E-3,1.6867693047970501E-3,1.6275827844261001E-3,1.57537722097578E-3,1.8725211697814899E-3,1.6644216526108999E-3,1.38834612255393E-3,1.1624238167371999E-3,1.61902997967683E-3]
["BNSF-E1L219C4","BNSF",4,"E1L219C4",304,"CM(Y), OPR Expense, Railroad-Owned, ACCESSORIAL",8.0532059655524804E-5,1.6592498286627201E-4,2.06006603548303E-4,2.4840759579092302E-4,1.14719594421331E-4,2.25167445023544E-4,4.1970511665567799E-4,5.5597972823306896E-4,5.5981246987357703E-4,5.2916713899782398E-4,4.8166763857522099E-4,3.1438622794674302E-4,1.20669455012665E-4,1.4946497747155E-5,0,0]
["BNSF-E1L219C5","BNSF",4,"E1L219C5",305,"CM(Y), DRL Expense, Railroad-Owned, ACCESSORIAL",1.5547449584119E-4,5.9569097356870803E-4,1.8756416393443901E-3,2.3714071139693299E-3,2.9122540727257698E-3,3.6528401542455001E-3,3.8092369213700299E-3,4.65655233711004E-3,5.6317267008125799E-3,4.5157188306667899E-3,4.9281182031220899E-3,3.7998073520559301E-3,3.0692511803047098E-3,2.5173761495568998E-3,3.6989531566785101E-3,3.7866845909126901E-3]
["BNSF-E1L219C6","BNSF",4,"E1L219C6",306,"CM(Y), ROI Expense, Railroad-Owned, ACCESSORIAL",3.3534938120283203E-4,7.7133573358878504E-4,1.47626793477684E-3,9.3610212206840504E-4,3.96718829870224E-3,4.0062218904495196E-3,3.9208298549056097E-3,4.3590115383267403E-3,4.3855966068804299E-3,4.2317152395078697E-3,4.0959807745370299E-3,4.8685550414318797E-3,4.3274962967883501E-3,3.60969991864021E-3,3.0223019235167E-3,4.20947794715976E-3]
["BNSF-E1L219C7","BNSF",4,"E1L219C7",307,"CD(R), OPR Expense, Railroad-Owned, ACCESSORIAL",3.3291331492364398E-3,6.8978127092122997E-3,8.6280666291713697E-3,1.07525074854493E-2,5.0503923557698701E-3,9.9478280171751993E-3,1.8469640985131298E-2,2.4232521653175399E-2,2.4142593145370501E-2,2.2907203320208899E-2,2.1293357474440801E-2,1.42127345623052E-2,5.5399482451247203E-3,6.8173073896258998E-4,0,0]
["BNSF-E1L219C8","BNSF",4,"E1L219C8",308,"CD(R), DRL Expense, Railroad-Owned, ACCESSORIAL",9.31187812238932E-3,3.7148423492908499E-2,0.11830872297287,0.159576416015625,0.19164751470089,0.23378595709800701,0.25200128555297902,0.29878839850425698,0.350334912538528,0.30024346674680802,0.33734565496296798,0.25182204027546101,0.21251920182831099,0.16921358356511901,0.26936321345903402,0.26354366989129602]
["BNSF-E1L219C9","BNSF",4,"E1L219C9",309,"CD(R), ROI Expense, Railroad-Owned, ACCESSORIAL",2.0155692473053901E-2,4.7846313565969502E-2,9.1702602803707095E-2,6.0307998210191699E-2,0.25968772172927901,0.25439018011093101,0.25753182172775302,0.27734813094139099,0.26958554983138999,0.278757485400975,0.27795763966696702,0.32154860911080002,0.298027176795232,0.24189529097617901,0.21746046745056399,0.28913191175278402]
["BNSF-E1L219C10","BNSF",4,"E1L219C10",310,"CD(Y), OPR Expense, Railroad-Owned, ACCESSORIAL",3.3291331492364398E-3,6.8978127092122997E-3,8.6280656978488003E-3,1.07525074854493E-2,5.0503923557698701E-3,9.9478270858526195E-3,1.8469639122486101E-2,2.4232521653175399E-2,2.4142591282725299E-2,2.2907203320208899E-2,2.1293357474440801E-2,1.42127345623052E-2,5.5399482451247203E-3,6.8173073896258998E-4,0,0]
["BNSF-E1L219C11","BNSF",4,"E1L219C11",311,"CD(Y), DRL Expense, Railroad-Owned, ACCESSORIAL",9.3118790537118894E-3,3.71484197676182E-2,0.11830872297287,0.159576416015625,0.191647499799728,0.23378595709800701,0.25200128555297902,0.29878836870193498,0.350334912538528,0.30024346674680802,0.33734565496296798,0.25182204027546101,0.21251920182831099,0.16921358356511901,0.26936321345903402,0.26354366989129602]
["BNSF-E1L219C12","BNSF",4,"E1L219C12",312,"CD(Y), ROI Expense, Railroad-Owned, ACCESSORIAL",2.0155692473053901E-2,4.7846313565969502E-2,9.1702610254287706E-2,6.0307998210191699E-2,0.25968772172927901,0.25439015030860901,0.25753179192543002,0.27734810113906899,0.26958554983138999,0.278757485400975,0.27795763966696702,0.32154860911080002,0.298027176795232,0.24189529097617901,0.21746046745056399,0.28913191175278402]
["BNSF-E1L219C13","BNSF",4,"E1L219C13",313,"CM(R), DRL Expense, Privately-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L220C1","BNSF",4,"E1L220C1",314,"CM(R), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.3335600048303597E-2,3.5596821457147598E-2,3.9067205041646999E-2,4.6173192560672802E-2,3.9200901985168499E-2,3.8740511983633E-2,4.0918108075857197E-2,4.2530562728643397E-2,4.30967584252357E-2,4.4198557777954797E-2,4.2503437525440502E-2,3.5791049341210503E-2,3.3689975091502997E-2,3.9197157702339502E-2,4.3451501879348597E-2,4.2272724168337099E-2]
["BNSF-E1L220C2","BNSF",4,"E1L220C2",315,"CM(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",7.9722609370946902E-3,6.9002695381641397E-3,6.5493634901940797E-3,5.45968115329742E-3,3.09164798818529E-3,5.5203363299369803E-3,4.9367416650056804E-3,8.2489969208836608E-3,9.9752377718687092E-3,1.07037260733726E-2,1.07293152796784E-2,9.4709892954843895E-3,2.4044390033914802E-3,4.7974861176816796E-3,3.0716991226472199E-3,2.7461961945447399E-3]
["BNSF-E1L220C3","BNSF",4,"E1L220C3",316,"CM(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.0009760968387099E-2,1.2712143361568499E-2,1.4050327241420701E-2,1.43910488113761E-2,1.47733353078365E-2,1.6995564103126502E-2,1.84906609356403E-2,1.9556740298867201E-2,1.8986539915204E-2,1.6725467432904199E-2,1.4521109154986901E-2,1.68098922115517E-2,2.0792248689124399E-2,1.8947758034075401E-2,1.64582662968988E-2,2.1061601555793501E-2]
["BNSF-E1L220C4","BNSF",4,"E1L220C4",317,"CM(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",9.7350455820560497E-2,0.117237731814384,0.22170658409595501,0.231429934501648,0.18290586769580799,0.178484752774239,0.20026452839374501,0.21864996850490601,0.23285585641861001,0.28477051879860399,0.34915696589337603,0.46904628917720897,0.44862283628872301,0.46972524182554298,0.51624378159529105,0.43761775204440301]
["BNSF-E1L220C5","BNSF",4,"E1L220C5",318,"CM(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",2.0340589806437499E-2,1.85546409338713E-2,1.7829822376370399E-2,1.3094335794448899E-2,8.3520710468292202E-3,1.67431551963091E-2,1.64993442595005E-2,2.5833144783973701E-2,3.0056275427341499E-2,3.8144408075071502E-2,5.5155838571154699E-2,4.96616091875344E-2,2.74044193833551E-2,2.3423579536443698E-2,2.6958949037615702E-2,1.9690595725138999E-2]
["BNSF-E1L220C6","BNSF",4,"E1L220C6",319,"CM(Y), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.1507682055234902E-2,4.3251022696495098E-2,4.6146783977746998E-2,4.1525878012180301E-2,4.1827104985714E-2,4.5478567481041003E-2,4.9449898302555098E-2,5.2282720804214498E-2,5.0348311662673999E-2,5.73934366348074E-2,5.0979984217952398E-2,5.4751934930374502E-2,5.9821687094504299E-2,5.3583721501343697E-2,4.8542848320660997E-2,6.0936345984065797E-2]
["BNSF-E1L220C7","BNSF",4,"E1L220C7",320,"CD(R), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.47469854354858,3.9275176525115998,4.2106728553771999,5.29372215270996,4.2038540840148899,3.90646600723267,4.6233973503112802,4.3261256217956499,3.9112110137939502,5.0289775920419997,5.3871886987737403,4.2330125796860401,3.9362141519248701,4.5252194441217704,5.9031545988778298,5.0698341620739296]
[{"$f":"B322&\"-\"&D322","v":"BNSF-E1L220C8"},"BNSF",4,"E1L220C8",321,"CD(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",10.074266433715801,11.0511837005615,10.4903354644775,11.255977630615201,9.2477703094482404,9.3844985961914098,11.299243927001999,11.331934928894,9.8962955474853498,7.5877009574447598,6.9729975148424499,5.4453245850331502,5.8730664211574002,6.0567821305009799,5.8381768258632603,5.6615780170701697]
["BNSF-E1L220C9","BNSF",4,"E1L220C9",322,"CD(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.53285872936249,2.0013737678527801,2.2705736160278298,2.5183911323547399,2.6092953681945801,3.0266890525817902,3.4594464302063002,3.5448951721191402,3.3107430934906001,3.11777933379823,2.7683011141334499,3.19889882300266,4.1575294106905503,3.4430589460413601,3.1962985221884601,3.93158307198533]
["BNSF-E1L220C10","BNSF",4,"E1L220C10",323,"CD(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.5498731136321999,3.9413118362426798,4.5981922149658203,5.71911668777466,4.7862300872802699,4.6364097595214799,4.9602460861206099,5.1494169235229501,5.2417259216308603,5.5294191196827498,5.4977245753558996,4.9030522592432604,4.8840235761276496,5.3958117838220501,6.2167884502310802,5.8170006215072902]
["BNSF-E1L220C11","BNSF",4,"E1L220C11",324,"CD(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",8.8564548492431605,9.7759628295898402,9.3044719696044904,9.8659467697143608,8.0083589553833008,8.1953773498535192,9.8294620513915998,9.81549072265625,9.2090473175048793,7.6912442126735501,6.8553020068038499,5.54292232046559,5.52727487188612,5.6128039323369903,5.43225238218547,5.4050132082223401]
["BNSF-E1L220C12","BNSF",4,"E1L220C12",325,"CD(Y), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.54051518440247,2.0553419589996298,2.2823290824890101,2.4501330852508501,2.4487760066986102,2.7070839405059801,3.0389492511749299,3.1082198619842498,2.9110064506530802,2.7959497379602598,2.5159343032999701,2.78482581030794,3.5530229637969701,3.2228752242641598,3.0406035627838399,3.6847717256250099]
["BNSF-E1L220C13","BNSF",4,"E1L220C13",326,"CM(R), DRL Expense, Privately-Owned, AVERAGE ALL FREIGHT CARS",4.0693987160921097E-2,3.4990482032299E-2,3.4544520080089597E-2,2.933962456882E-2,3.0113572254777E-2,3.2281018793582902E-2,3.2328255474567399E-2,3.43059599399567E-2,3.7933550775051103E-2,3.6855700051521903E-2,4.1283812703343803E-2,4.4492341766052199E-2,4.6046964453301302E-2,4.6205949387734799E-2,5.2616607504064897E-2,5.24383879359792E-2]
["BNSF-E1L221C1","BNSF",4,"E1L221C1",327,"CM(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",1.91910949070007E-3,1.36183737777174E-3,1.8507897621020701E-3,2.0183806773275098E-3,2.2516520693898201E-3,1.81110436096787E-3,1.4806780964136099E-2,3.6272585391998298E-2,5.45368157327175E-2,6.5802366133758103E-2,7.2275165306339803E-2,7.0858312942475493E-2,6.7549924309164996E-2,6.9655954279201002E-2,6.76674002642393E-2,7.4366783080218907E-2]
["BNSF-E1L221C2","BNSF",4,"E1L221C2",328,"CM(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",6.9152586162090302E-2,7.8213572502136203E-2,5.3672328591346699E-2,6.0376852750778198E-2,5.5525694042444201E-2,5.7703748345375103E-2,4.0415231138467803E-2,5.96809163689613E-2,8.6155891418457003E-2,9.2762482247786299E-2,7.1244632003919603E-2,8.97640776848911E-2,6.6321506508993794E-2,6.7875551576624907E-2,5.5291094597586098E-2,5.3642351614849502E-2]
["BNSF-E1L221C3","BNSF",4,"E1L221C3",329,"CM(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",3.4819804131984697E-2,1.5944670885801301E-2,4.7150421887636199E-2,8.0527275800704998E-2,0.142104312777519,0.12790283560752899,8.7864898145198794E-2,0.112703740596771,0.134015753865242,0.13193574077405401,0.11832159055130501,0.12190708161033501,0.14869189406045299,0.102636238431922,9.3756771254565704E-2,0.12779720841025899]
["BNSF-E1L221C4","BNSF",4,"E1L221C4",330,"CM(Y), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",4.9896892160177196E-3,3.5407806281000402E-3,4.8120515421032897E-3,5.2477917633950702E-3,5.8542839251458601E-3,4.7088731080293699E-3,3.8497604429721798E-2,9.4308711588382693E-2,0.14179557561874401,0.17108615194777099,0.18791542979648401,0.184231613650437,0.17562980320382801,0.18110548112592201,0.17593524068702199,0.193353636008569]
["BNSF-E1L221C5","BNSF",4,"E1L221C5",331,"CM(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.17979708313942,0.20335511863231701,0.13954804837703699,0.15697968006134,0.14436666667461401,0.15002959966659499,0.10507981479167899,0.15517032146453899,0.22400538623332999,0.241182453844245,0.18523604321018999,0.23338660198071601,0.172435916923384,0.176476434099225,0.14375684595372401,0.139470114198609]
["BNSF-E1L221C6","BNSF",4,"E1L221C6",332,"CM(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",9.0531691908836406E-2,4.1456103324890102E-2,0.12259098887443499,0.20937101542949699,0.36947146058082603,0.33254685997963002,0.22844870388507801,0.29302942752838101,0.34844121336937001,0.34303292601254098,0.30763613543339102,0.31695841218687099,0.38659892455717698,0.26685421992299801,0.243767605261871,0.33227274186667499]
["BNSF-E1L221C7","BNSF",4,"E1L221C7",333,"CD(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.25056502223014798,0.17736507952213301,0.24634847044944799,0.27601596713066101,0.31342044472694403,0.24890644848346699,1.98297679424286,4.85670709609985,7.2675256729126003,8.9369149180683305,10.026370492029599,10.2101127357412,9.8517205315971008,9.3132706303376196,8.8073074540280594,9.2071032023041894]
["BNSF-E1L221C8","BNSF",4,"E1L221C8",334,"CD(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",55.646213531494098,60.002605438232401,63.970546722412102,70.055000305175795,59.430004119872997,48.5746040344238,41.141685485839801,40.680160522460902,51.686843872070298,13.411490685991099,61.775503641777,65.141520491075198,8.6037857903175894,-9.43230746681391,-7.37786041976908,-2.0149988944689401]
["BNSF-E1L221C9","BNSF",4,"E1L221C9",335,"CD(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",6.7384114265441903,2.8876490592956499,9.5082912445068395,17.2709350585938,29.176601409912099,25.1209926605225,17.4699897766113,22.732841491699201,25.9866752624512,27.740151113590599,25.380759013587902,26.229104625112701,32.135622773047999,17.794935656966398,18.139267393697601,23.476581062786501]
["BNSF-E1L221C10","BNSF",4,"E1L221C10",336,"CD(Y), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.25056502223014798,0.17736507952213301,0.24634848535060899,0.27601599693298301,0.31342041492462203,0.24890643358230599,1.98297691345215,4.8567066192626998,7.2675256729126003,8.9369149180683305,10.026370492029599,10.2101127357412,9.8517205315971008,9.3132706303376196,8.8073074540280594,9.2071032023041894]
["BNSF-E1L221C11","BNSF",4,"E1L221C11",337,"CD(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",55.646217346191399,60.002605438232401,63.970558166503899,70.055000305175795,59.430007934570298,48.5746040344238,41.141685485839801,40.680160522460902,51.686847686767599,13.411490685991099,61.775503641777,65.141520491075198,8.6037857903175894,-9.4323074668138993,-7.37786041976908,-2.0149988944689401]
["BNSF-E1L221C12","BNSF",4,"E1L221C12",338,"CD(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",6.7384114265441903,2.8876488208770801,9.5082912445068395,17.2709350585938,29.176601409912099,25.1209926605225,17.46999168396,22.732841491699201,25.9866752624512,27.740151113590599,25.380759013587799,26.229104625112701,32.135622773047999,17.794935656966398,18.139267393697601,23.476581062786501]
["BNSF-E1L221C13","BNSF",4,"E1L221C13",339,"CM(R), DRL Expense, Privately-Owned, TOTAL FLAT, MULTILEVEL",0.16249170899391199,0.16849344968795801,0.20164796710014299,0.21305528283119199,0.21952658891677901,0.18548059463500999,0.15666911005973799,0.17894980311393699,0.20443540811538699,0.196957267428749,0.23067776109580199,0.24743418857452601,0.23843070637206801,0.255928551028683,0.30438877375944601,0.27401690461818301]
["BNSF-E1L301C1","BNSF",4,"E1L301C1",340,"L&D Expense, FARM PRODUCTS",6.0479726642370203E-2,4.3492771685123402E-2,5.2238646894693402E-2,5.0968628376722301E-2,3.09725925326347E-2,5.8702994138002403E-2,3.9931595325469998E-2,4.0919195860624299E-2,5.5300697684287997E-2,4.0740445742439298E-2,3.0235172829172E-2,4.2640386857255498E-2,3.0764167073179E-2,3.9305223656339899E-2,2.3084220232348799E-2,3.2991514790269003E-2]
["BNSF-E1L302C1","BNSF",4,"E1L302C1",341,"L&D Expense, GRAIN",2.6387264952063599E-2,2.4945870041847201E-2,3.6727432161569602E-2,3.52221131324768E-2,2.7508964762091598E-2,4.8060111701488502E-2,2.2179268300533302E-2,3.1123021617531801E-2,3.6137115210294703E-2,3.1673053208722303E-2,2.06520373319149E-2,3.17940606104282E-2,2.12862621972436E-2,1.6299519112691799E-2,1.6646101782829398E-2,1.6986060104260001E-2]
["BNSF-E1L303C1","BNSF",4,"E1L303C1",342,"L&D Expense, POTATOES OTHER THAN SWEET",3.6799578666686998,3.1860339641571001,1.57116758823395,2.0286219120025599,0.46845808625221302,0.59124863147735596,0.76070266962051403,0.51356053352356001,1.9531569480896001,2.51130048867766,2.4820239734348402,1.5628554724856101,1.5738487949622999,4.7855950282905102,2.6763798404894299,1.6733272275745501]
["BNSF-E1L304C1","BNSF",4,"E1L304C1",343,"L&D Expense, FRESH FRUITS",0.302319556474686,8.5989952087402302E-2,0.58841019868850697,8.6072228848934201E-2,1.4460543170571299E-2,0.126831129193306,0.49312025308608998,0.52817994356155396,0.16668255627155301,8.2599028253724796E-2,9.9674777409128404E-2,0.43295957620681202,8.8434329739041695E-2,0.85901773298737005,1.1195029946875601,0.48971047651869798]
["BNSF-E1L305C1","BNSF",4,"E1L305C1",344,"L&D Expense, FRESH VEGETABLES",0.60301697254180897,0.243790358304977,0.41229620575904802,0.19410522282123599,7.3158152401447296E-2,0.65559387207031306,0.35545039176940901,0.20792415738105799,0.48678919672965998,0.41470897303029602,0.34160943933107601,0.389577076844837,0.26595492810377602,0.63672310190342996,0.200726594272612,0.51497044391303703]
["BNSF-E1L306C1","BNSF",4,"E1L306C1",345,"L&D Expense, ALL OTHER FARM PRODUCTS",8.7879635393619496E-2,4.6295948326587698E-2,4.7562893480062499E-2,5.8936458081006997E-2,3.3297318965196603E-2,3.8297187536954901E-2,5.1949910819530501E-2,3.9584696292877197E-2,5.1575444638729102E-2,9.5663520052149797E-3,1.65227324418049E-2,3.6049529086921397E-2,3.7162508897451797E-2,4.2500157114610498E-2,5.3477487289282401E-3,4.7120247326328697E-2]
["BNSF-E1L307C1","BNSF",4,"E1L307C1",346,"L&D Expense, METALLIC ORES",1.6947247087955499E-2,7.1331090293824699E-3,3.3462069928646102E-2,7.0100501179695102E-2,4.2934261262416798E-2,3.86384478770196E-3,4.2152050882577896E-3,8.2664601504802704E-3,2.1994682028889699E-3,1.2440038637219399E-2,8.2511941540468301E-4,0,0,5.0977125450342798E-3,1.33905395969415E-4,0]
["BNSF-E1L308C1","BNSF",4,"E1L308C1",347,"L&D Expense, COAL",3.01631726324558E-3,3.2460147049277999E-3,3.05656832642853E-3,4.3408023193478602E-3,3.2279870938509698E-3,3.3305299002677198E-3,4.0287571027874903E-3,3.9105019532144096E-3,2.7237308677285901E-3,2.14346200941452E-3,2.0286106009389702E-3,4.8588212337537899E-3,4.4838032093151596E-3,3.9408800824081098E-3,1.5177075802263499E-3,2.1313169653889401E-3]
["BNSF-E1L309C1","BNSF",4,"E1L309C1",348,"L&D Expense, NONMETALLIC MINERALS",6.1751324683427802E-3,6.0367635451257203E-3,6.24764291569591E-3,1.1238164268434001E-2,1.2882996350526799E-2,1.0773151181638199E-2,1.14579824730754E-2,5.6324019096791701E-3,5.2316985093057199E-3,7.1841635102270198E-3,1.9460853891206499E-3,2.9566385317463602E-3,2.6945083219701502E-3,3.9923515321203399E-3,1.2879584932098101E-3,2.5697714472261999E-3]
["BNSF-E1L310C1","BNSF",4,"E1L310C1",349,"L&D Expense, FOOD AND KINDRED PRODUCTS",0.112814217805862,0.10337255895137799,0.15115562081337,0.103318996727467,7.9335421323776203E-2,8.1889294087886796E-2,0.113200463354588,0.10237280279398001,0.105734661221504,0.155869352854069,0.14200791172845001,0.110538880168726,0.16084816368765401,0.19031238664048999,0.105766987771637,0.100991336079819]
["BNSF-E1L311C1","BNSF",4,"E1L311C1",350,"L&D Expense, FRESH MEATS",0,0,0,0,6.0307089239358902E-2,0.14437814056873299,0.18296842277049999,0,0,0,0,0,0,0,0,0]
["BNSF-E1L312C1","BNSF",4,"E1L312C1",351,"L&D Expense, DAIRY PRODUCTS",0.26197466254234297,1.34666740894318,1.7574552297592201,0.46422058343887301,0.35715392231941201,0.464790970087051,0.49275985360145602,0.75572431087493896,1.05871522426605,2.0809273501940702,0.96986246387669905,0.98166953399452095,2.6580326093429498,4.3113833540049997,3.8502678120262801,1.82206074815941]
["BNSF-E1L313C1","BNSF",4,"E1L313C1",352,"L&D Expense, CANNED FRUITS/VEG",0.61201786994934104,0.45836937427520802,0.54955309629440297,0.46772405505180398,0.268973708152771,0.44812881946563698,0.364413142204285,0.32465270161628701,0.30047565698623702,0.54309701066336802,0.60036280662191399,0.59926710243978698,0.57379621654754098,0.79501823483980005,0.40052818960853498,0.33041247966923698]
["BNSF-E1L314C1","BNSF",4,"E1L314C1",353,"L&D Expense, GRAIN MILL PRODUCTS",3.1477384269237497E-2,6.5411634743213695E-2,8.0874219536781297E-2,6.5766513347625705E-2,5.2350562065839802E-2,5.79447709023952E-2,4.7625388950109503E-2,4.8314291983842898E-2,3.0080657452344901E-2,3.5506442073018903E-2,4.5023558881849897E-2,2.2275958202964401E-2,3.7569787654383499E-2,3.02891444533398E-2,2.6234808790303401E-2,6.1752196822825997E-2]
["BNSF-E1L315C1","BNSF",4,"E1L315C1",354,"L&D Expense, FLOUR",3.2923668622970602E-2,7.6696105301380199E-2,8.2328729331493405E-2,4.6068139374256099E-2,6.2322694808244698E-2,7.4686713516712203E-2,7.1782425045967102E-2,5.7252213358879103E-2,2.7048252522945401E-2,5.3978262161745102E-2,8.1389778583540101E-2,2.0658939350466098E-2,5.6218799270150201E-2,4.7762989723968197E-2,5.6966833978788899E-2,5.6377434374590599E-2]
["BNSF-E1L316C1","BNSF",4,"E1L316C1",355,"L&D Expense, PREPARED FEEDS",3.4461708273738601E-3,5.2915900945663501E-2,8.3416014909744304E-2,6.4005493186414198E-3,6.4121750183403501E-3,1.0765590704977499E-3,1.48906651884317E-2,1.21511137112975E-2,5.0596832297742401E-3,3.2849257204589803E-2,1.38959473594921E-2,6.32190753961661E-3,2.7778759021351199E-2,1.08453877778599E-3,2.5196986440421701E-5,1.02066313274846E-3]
["BNSF-E1L317C1","BNSF",4,"E1L317C1",356,"L&D Expense, CEREALS",0.13801950216293299,0.150457173585892,0.113301411271095,0.12655127048492401,0.114000834524632,5.6761432439088801E-2,2.6986366137862199E-2,9.9266923964023604E-2,4.1428942233324099E-2,2.69035785859623E-2,7.1618623461894307E-2,1.92697768762677E-2,5.9594076037541001E-2,1.39432972578182E-3,9.1593963957775203E-4,6.4883822884699701E-3]
["BNSF-E1L318C1","BNSF",4,"E1L318C1",357,"L&D Expense, RICE",0.18275606632232699,0.20021592080593101,0.26043739914894098,0.49083593487739602,0.26900073885917702,0.26474368572235102,0.105855084955692,0.30795875191688499,0.195555880665779,0.171957354616004,0.217271284411443,0.20353585332434401,0.10460667322949101,0.201985129218855,0.18705377019309699,0.27474099401881502]
["BNSF-E1L319C1","BNSF",4,"E1L319C1",358,"L&D Expense, PREPARED FLOUR",0.37972217798232999,0.44714790582656899,0.31831541657447798,0.25416249036788902,0.14075364172458599,4.0416184812784202E-2,0.17804516851902,0,0,0,0,0,0,0,0,0]
["BNSF-E1L320C1","BNSF",4,"E1L320C1",359,"L&D Expense, CORN PRODUCTS",1.34091908112168E-2,3.9376903325319297E-2,4.7181513160467099E-2,2.6431472972035401E-2,2.73294728249311E-2,3.8074269890785203E-2,3.7078451365232502E-2,1.75428669899702E-2,2.01527439057827E-2,4.1817161674595404E-3,1.34790764147741E-2,4.3508653131181197E-3,9.0233417435583996E-3,3.9086462228574504E-3,3.02978423330987E-5,2.0180023840311999E-2]
["BNSF-E1L321C1","BNSF",4,"E1L321C1",360,"L&D Expense, REFINED SUGAR",2.7943493798375098E-2,0.16404953598976099,3.96022871136665E-2,0.10142989456653601,3.3815246075391797E-2,7.3806062340736403E-2,0.14849175512790699,8.2387849688529996E-2,0.25767901539802601,0.19669764508510401,3.2387171869427901E-3,4.3898923629163901E-2,7.3782916037265098E-2,3.3899308291411599E-2,1.4090874839876401E-2,0.11818608416618399]
["BNSF-E1L322C1","BNSF",4,"E1L322C1",361,"L&D Expense, BEER",0.21311140060424799,0.13795143365859999,0.11230556666851001,0.209407404065132,0.334010690450668,0.38553339242935197,0.90072369575500499,0.90642565488815297,0.56750947237014804,1.0174552404741599,1.7311441019848299,1.9743613882701201,3.1530590569508399,8.7245439934215394,2.5082539988572998,1.4391021304396601]
["BNSF-E1L323C1","BNSF",4,"E1L323C1",362,"L&D Expense, WINES",0.84492164850234996,8.3208911120891599E-2,1.34687983989716,0.44220030307769798,0.205625951290131,6.3485205173492404E-2,0.24367405474185899,0.51581692695617698,0.34035617113113398,1.35427260144433,0.24422654004494099,0.105158524452878,0.36028833717952002,0.267506679227699,0.16329456182654101,0.12703334188972801]
["BNSF-E1L324C1","BNSF",4,"E1L324C1",363,"L&D Expense, WHISKEY",0.15329632163047799,4.5956458896398503E-2,1.3157946057617701E-2,0.17441810667514801,0.113551504909992,6.6947758197784396E-2,9.6811883151531206E-2,5.2685525268316297E-2,0.73190534114837602,0.41291941120203002,0.301251651267823,2.16556871024641E-2,2.35566983096023E-2,8.2224230857488294E-3,0.14673836468771501,6.9431467804815294E-2]
["BNSF-E1L325C1","BNSF",4,"E1L325C1",364,"L&D Expense, MISC FOOD PREPARATIONS",4.9347322434186901E-2,3.9073646068572998E-2,6.88051283359528E-2,4.7288753092288999E-2,7.3226988315582303E-2,4.44420874118805E-2,5.8179348707199097E-2,6.4795158803462996E-2,6.5988443791866302E-2,4.7256400580346102E-2,0.10027194560448401,5.8322594141169803E-2,4.7792372956870097E-2,4.0860279141872603E-2,3.6097560727487002E-2,5.5607518381965003E-2]
["BNSF-E1L326C1","BNSF",4,"E1L326C1",365,"L&D Expense, ALL OTHER FOOD PRODUCTS",9.1888576745986897E-2,7.9573296010494204E-2,0.12117470800876599,6.5014228224754306E-2,3.6592349410057103E-2,4.3420534580946003E-2,0.141043856739998,5.3964279592037201E-2,5.3006786853075E-2,7.9923448269122996E-2,9.9097557048061696E-2,8.1842532444312499E-2,0.19285248625642101,0.17873068167745801,0.111427994915152,8.3245180810300995E-2]
["BNSF-E1L327C1","BNSF",4,"E1L327C1",366,"L&D Expense, TOBACCO PRODUCTS",0,0,0,0,3.18567967414856,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E1L328C1","BNSF",4,"E1L328C1",367,"L&D Expense, LUMBER AND WOOD EX FURNITURE",6.4082108438014998E-2,6.3597209751606001E-2,4.2465981096029302E-2,5.5317327380180401E-2,2.6106728240847601E-2,4.5685745775699602E-2,2.36855149269104E-2,3.1761787831783302E-2,2.2764811292290701E-2,5.5634208764431099E-2,6.8785233747138505E-2,4.2106313382289699E-2,5.85751816640947E-2,5.6718723912763502E-2,5.8628574900259398E-2,0.141446267912923]
["BNSF-E1L329C1","BNSF",4,"E1L329C1",368,"L&D Expense, LUMBER/DIMENSION STOCK",6.9662675261497498E-2,6.6921301186084706E-2,5.0744507461786298E-2,4.2644336819648701E-2,2.0643839612603201E-2,7.3353521525859805E-2,1.56366545706987E-2,3.8499526679515797E-2,2.4210380390286401E-2,6.5480499825039798E-2,6.5441979456708904E-2,6.6382032559786502E-2,9.6643513669763995E-2,3.5730563075364201E-2,7.45180514067776E-2,0.18957337341988301]
["BNSF-E1L330C1","BNSF",4,"E1L330C1",369,"L&D Expense, PLYWOOD OR VENEER",7.4905700981617002E-2,4.27759401500225E-2,8.9939765632152599E-2,0.12727469205856301,8.0512069165706607E-2,9.6415840089321095E-2,4.3528910726308802E-2,3.7447415292263003E-2,2.03599594533443E-2,0.12145549472462901,0.216664798239351,2.9783990826895802E-2,7.0972097170494602E-2,6.9536828674594306E-2,6.8338321410531103E-2,0.117691760964366]
["BNSF-E1L331C1","BNSF",4,"E1L331C1",370,"L&D Expense, ALL OTHER LUMBER AND WOOD PRODUCTS",5.6283235549926799E-2,6.4753077924251598E-2,2.6934949681162799E-2,5.1356635987758602E-2,1.97196342051029E-2,1.67441107332706E-2,2.6319015771150599E-2,2.49072927981615E-2,2.19722930341959E-2,3.42567023876479E-2,4.1458401381328898E-2,2.14436371930571E-2,1.7770680455502699E-2,7.2241755483112693E-2,4.1882590552649701E-2,9.6173132143614795E-2]
["BNSF-E1L332C1","BNSF",4,"E1L332C1",371,"L&D Expense, FURNITURE AND FIXTURES",1.01506423950195,4.2289190292358398,3.8702409267425502,1.72642862796783,1.0335067510604901,0.56756269931793202,1.8485848903655999,0.51095122098922696,0.77477347850799605,0.87920951704397499,0.29486340670581901,0.40993634402058698,0.171194339057925,0.29584487614604099,0.37153646834541698,2.0288792699200302]
["BNSF-E1L333C1","BNSF",4,"E1L333C1",372,"L&D Expense, PULP, PAPER AND ALLIED PRODUCTS",0.26838248968124401,0.28085958957672102,0.29805308580398598,0.29972025752067599,0.20974843204021501,0.18133181333541901,0.162495583295822,0.17467743158340501,0.16834378242492701,0.12844722302166001,0.153450512751615,0.17213338337717099,0.106044886035222,0.12062119539989299,8.5510400889075799E-2,0.144576608542514]
["BNSF-E1L334C1","BNSF",4,"E1L334C1",373,"L&D Expense, NEWSPRINT",0.386345565319061,0.26457613706588701,0.24139791727066001,0.40231353044509899,0.33147549629211398,0.257203638553619,0.141914248466492,8.8899778202176094E-3,0.17850668728351601,0.192825144881663,9.4011005829416405E-2,0.20472030566705901,3.1076594371090002E-2,1.2324784383151699,2.51977665787704E-2,0.16148795459672499]
["BNSF-E1L335C1","BNSF",4,"E1L335C1",374,"L&D Expense, PRINTING PAPER",0.45069688558578502,0.77085703611373901,0.80805128812789895,0.78840303421020497,0.60578840970992998,0.33505225181579601,0.42516347765922502,0.31435161828994801,0.37708187103271501,0.39925658646490703,0.66945896095312996,1.11723782584026,0.58951542221150599,0.19435054877364999,0.121608076937136,0.190232288385774]
["BNSF-E1L336C1","BNSF",4,"E1L336C1",375,"L&D Expense, FIBREBD/PAPERDB/PULPDB",0.247822120785713,0.201040908694267,0.26354819536209101,0.315349161624908,0.22802263498306299,0.206928014755249,0.15028686821460699,0.219723805785179,0.196718350052834,0.13845131328341401,0.14237568256028199,0.14370424430854201,9.1790883821594699E-2,8.6933569886294401E-2,7.6629285275818401E-2,0.17068400098040601]
["BNSF-E1L337C1","BNSF",4,"E1L337C1",376,"L&D Expense, COV PAPER/PAPERBOARD",0.14351396262645699,2.3441700264811498E-2,5.0217267125844997E-2,4.3607987463474301E-2,3.0316181480884601E-2,3.9156388491392101E-2,6.6796630620956393E-2,3.8177575916051899E-2,0.123719930648804,8.9984059162479299E-2,4.7553798615383003E-2,9.2495401211793692E-3,6.3031332334864496E-3,3.4192846214227003E-2,6.3265511684125697E-2,8.0745058269087004E-3]
["BNSF-E1L338C1","BNSF",4,"E1L338C1",377,"L&D Expense, SANITARY TISSUES",0.122947245836258,3.0709726270288199E-3,6.65031932294369E-3,6.80103600025177E-2,1.2522803619503999E-2,0,0.10232835263013799,1.07538355514407E-2,9.4120344147086091E-3,2.9207028751322198E-2,1.1900797086969101E-3,1.39013832183855E-2,0,5.0166042535151603E-3,1.23663771402875E-3,4.3280785841464898E-3]
["BNSF-E1L339C1","BNSF",4,"E1L339C1",378,"L&D Expense, ALL OTHER PULP, PAPER & ALLIED PRODUCTS",0.17567807435989399,0.195987403392792,0.152946561574936,0.107534527778625,7.8239731490612002E-2,8.5699714720249204E-2,0.122758314013481,8.2997627556324005E-2,7.0808172225952107E-2,5.6488843821234702E-2,7.3495363821740795E-2,3.9105518177458103E-2,5.0811760324324599E-2,0.14501322871120401,0.100518870925555,0.10260932363021701]
["BNSF-E1L340C1","BNSF",4,"E1L340C1",379,"L&D Expense, CHEMICALS",5.11742942035198E-2,4.20025512576103E-2,3.6974240094423301E-2,4.2966037988662699E-2,3.3213671296834897E-2,4.8909343779087101E-2,5.0282698124647099E-2,3.2089069485664402E-2,3.1751915812492398E-2,3.2152053773539503E-2,4.5385256484858798E-2,3.7555629213460701E-2,3.01283549154009E-2,4.3525262911993302E-2,4.1050292308664603E-2,4.8456104800754497E-2]
["BNSF-E1L341C1","BNSF",4,"E1L341C1",380,"L&D Expense, INDUSTRIAL CHEMICALS",8.7614255025982891E-3,1.6192162409424799E-2,8.6116092279553396E-3,8.3545334637165104E-3,7.8697837889194506E-3,2.1585958078503598E-2,2.21712626516819E-2,1.10827656462789E-2,7.03930715098977E-3,7.1057580517135304E-3,1.15099133183999E-2,1.2581535809645E-2,1.27504083238833E-2,8.6896402574811304E-3,1.4742717925468E-2,1.0810643549472299E-2]
["BNSF-E1L342C1","BNSF",4,"E1L342C1",381,"L&D Expense, POTASSIUM OR SODIUM",2.7809889987111099E-2,1.60602275282145E-2,1.1788333766162401E-2,1.4397126622498001E-2,2.13480275124311E-2,1.2410043738782401E-2,9.0565774589776993E-3,7.6568066142499404E-3,1.3412986882031E-2,8.5684775629813106E-3,2.6314574467900101E-2,1.10570170436835E-2,1.12225187459802E-2,1.60371523159329E-2,1.1939958424653599E-2,5.9931752529763698E-3]
["BNSF-E1L343C1","BNSF",4,"E1L343C1",382,"L&D Expense, SYN FIBRES/RESINS/RUBBER",0.14274440705776201,6.1173558235168499E-2,8.7265506386756897E-2,0.10607888549566299,8.5183314979076399E-2,0.12817049026489299,0.132741883397102,9.0175598859787001E-2,0.100434817373753,8.3801154952120302E-2,0.11696684497985201,0.106955975079934,5.2621767832795201E-2,0.10260436617034099,6.5752737420087498E-2,0.139082763813134]
["BNSF-E1L344C1","BNSF",4,"E1L344C1",383,"L&D Expense, MISC CHEMICALS PRODUCTS",4.3860375881195103E-2,5.9413857758045197E-2,5.3479108959436403E-2,6.6045254468917805E-2,5.3832165896892499E-2,6.0841087251901599E-2,1.3048115186393301E-2,3.7528481334447902E-2,7.7735278755426398E-3,5.2866308194148698E-2,6.3770333647115898E-3,9.4641084932867905E-3,5.7108239653403999E-3,4.0468951069907904E-3,3.7185460949404302E-2,2.3238877916688001E-2]
["BNSF-E1L345C1","BNSF",4,"E1L345C1",384,"L&D Expense, ALL OTHER CHEMICALS",2.6043361052870799E-2,0.102892324328423,5.1314171403646497E-2,5.8835830539464999E-2,4.2031995952129399E-2,1.8057033419609101E-2,2.5860302150249499E-2,7.7346088364720301E-3,2.08973791450262E-2,2.2599386791942899E-2,5.1338501809845997E-2,4.6916238257755201E-4,7.0031947197344305E-2,9.0754973556344501E-2,0.11058293551930599,1.91782433824856E-2]
[{"$f":"B386&\"-\"&D386","v":"BNSF-E1L346C1"},"BNSF",4,"E1L346C1",385,"L&D Expense, PETROLEUM OR COAL PRODUCTS",5.6120855733752303E-3,2.0458623766899098E-2,1.4187679626047601E-2,1.6730939969420398E-2,9.0988166630268097E-3,2.5490145199000801E-3,7.7201277017593401E-3,7.4020400643348703E-3,7.5389896519482101E-3,2.8806192440008001E-3,3.97382980853935E-3,1.3481022730943801E-2,7.8551231896560793E-3,6.7912819925897497E-3,5.4264531937212798E-3,1.17302843534858E-2]
["BNSF-E1L347C1","BNSF",4,"E1L347C1",386,"L&D Expense, RUBBER AND MISC PLASTICS",0.121731825172901,8.4463320672512096E-2,5.7188738137483597E-2,2.3528395220637301E-2,1.31647260859609E-2,7.10021182894707E-2,0.156284719705582,9.4427227973938002E-2,0.101616881787777,2.8642241838434401E-2,2.2199691128442101E-2,1.54454766150119E-2,6.0183038438072003E-3,9.8465346002906795E-2,4.7641514960962097E-2,3.8674507534544302E-2]
["BNSF-E1L348C1","BNSF",4,"E1L348C1",387,"L&D Expense, RUBBER TIRES/INNER TUBES",0.134509116411209,8.9131239801645296E-3,1.7789637669920901E-2,4.3709573219530301E-4,6.3215277623385202E-4,0.12824502587318401,0.20823356509208699,0.172246068716049,0.101569473743439,5.1709465437767201E-2,4.1918087269156301E-3,3.8097494457809397E-2,6.2541206245703999E-3,5.4441562535281901E-2,7.61084379992156E-2,9.8839377049493804E-2]
["BNSF-E1L349C1","BNSF",4,"E1L349C1",388,"L&D Expense, ALL OTHER RUBBER PRODUCTS",0.11405962705612201,0.128890320658684,8.23671519756317E-2,3.9198044687509502E-2,2.3228943347930901E-2,2.2845545783638999E-2,0.11083518713712701,3.211560100317E-2,0.101654149591923,1.32252519852178E-2,3.40125415840088E-2,1.0177256724421E-3,5.8682357893787302E-3,0.123604358744922,3.6994674618663702E-2,1.0509528840878701E-2]
["BNSF-E1L350C1","BNSF",4,"E1L350C1",389,"L&D Expense, STONE, CLAY AND GLASS PRODUCTS",2.8050996363163001E-2,2.94760055840015E-2,2.3014681413769701E-2,2.2323321551084501E-2,1.25137800350785E-2,2.0365133881568898E-2,1.3885203748941401E-2,1.2379656545817901E-2,2.0123468711972198E-2,1.8672422852622099E-2,1.5618687233242201E-2,7.1743035945493697E-3,1.00761913642266E-2,1.1213559823315599E-2,1.4322538640667201E-2,1.0220925283838099E-2]
["BNSF-E1L351C1","BNSF",4,"E1L351C1",390,"L&D Expense, FLAT GLASS",7.9960972070693997E-2,0,0,4.9382718279957797E-3,0,0,0,0,0.24076983332634,7.4834149668299293E-2,0,0,0,2.46638667305578E-3,0,1.26070110068464E-2]
["BNSF-E1L352C1","BNSF",4,"E1L352C1",391,"L&D Expense, NONMETALLIC EARTH/MIN",3.5418793559074402E-2,2.9506977647542999E-2,3.24249938130379E-2,3.4120228141546201E-2,1.8458276987075799E-2,2.4468347430229201E-2,2.0480075851082798E-2,2.0243378356099101E-2,2.5672337040305099E-2,2.5089518608720399E-2,3.77997396445496E-2,7.6303684431867002E-3,1.4583935379803001E-2,1.4303699383296E-2,4.0311754906339203E-3,1.3603944578531899E-2]
["BNSF-E1L353C1","BNSF",4,"E1L353C1",392,"L&D Expense, ALL OTHER STONE & CLAY, GLASS PRODUCTS",2.3819899186492001E-2,2.95029655098915E-2,1.7426427453756301E-2,1.5901990234851799E-2,9.0113366022705997E-3,1.7641941085457798E-2,1.0626674629747901E-2,8.8174836710095406E-3,1.7466975376009899E-2,1.6213023466090899E-2,8.0123522222395605E-3,7.0282422645380101E-3,8.5392018813610897E-3,1.00639728338627E-2,1.8205648733177902E-2,8.8792988187615506E-3]
["BNSF-E1L354C1","BNSF",4,"E1L354C1",393,"L&D Expense, PRIMARY METAL PRODUCTS",3.4512434154748903E-2,5.7771623134613002E-2,4.6246688812971101E-2,0.105558961629868,4.7241918742656701E-2,4.59798015654087E-2,3.2263457775116001E-2,3.3330846577882801E-2,3.9058309048414203E-2,4.5040043560047503E-2,3.8303111795328998E-2,5.8488123741768101E-2,4.45886648461584E-2,8.2227833513675699E-2,4.9633379412000397E-2,6.0209103013003903E-2]
["BNSF-E1L355C1","BNSF",4,"E1L355C1",394,"L&D Expense, PRIMARY IRON/STEEL PRODUCTS",3.4884344786405598E-2,5.3362432867288603E-2,3.6286663264036199E-2,9.7192518413066906E-2,4.7952342778444297E-2,4.3800264596939101E-2,2.8834400698542598E-2,3.0930418521165799E-2,4.0773164480924599E-2,4.32040643335612E-2,3.8559282806765002E-2,6.04644823038471E-2,4.9514510216627401E-2,7.8182518416237898E-2,1.5334172940485001E-2,4.9781753141333498E-2]
["BNSF-E1L356C1","BNSF",4,"E1L356C1",395,"L&D Expense, ALUMINUM BASIC SHAPES",0.11286199837923,0.15163244307041199,0.19129206240177199,0.99977880716323897,9.2738665640354198E-2,0.365030497312546,0.13654950261116,0.40275806188583402,4.6725824475288398E-2,0.427446876899923,7.1842447765894907E-2,6.1801981514728398E-2,2.36256029762279E-4,0.97019829399741397,1.4380682533099101,1.67692641734201]
["BNSF-E1L357C1","BNSF",4,"E1L357C1",396,"L&D Expense, ALL OTHER PRIMARY METAL PRODUCTS",2.12727766484022E-2,9.5122657716274303E-2,0.135312050580978,4.1251994669437402E-2,3.5979904234409298E-2,3.8908191025257097E-2,5.8396480977535199E-2,1.43697401508689E-2,1.95995084941387E-2,2.3422915187733099E-2,3.1688528748677502E-2,3.7337457772167501E-2,8.8837298846552505E-4,7.0970671331329699E-2,0.279650607967111,9.53012962841015E-2]
["BNSF-E1L358C1","BNSF",4,"E1L358C1",397,"L&D Expense, FABRICATED METAL PRODUCTS",0.29441612958908098,8.34800750017166E-2,0.120782092213631,0.57032650709152199,0.127834737300873,0.121632412075996,0.10238241404295,0.34850579500198398,2.4500768631696701E-2,4.4205237424147302E-2,4.1813711219508103E-2,0.13085792181979899,5.4769202978317402E-2,0.17031496412081801,3.3467763128923302E-3,0.226221318634625]
["BNSF-E1L359C1","BNSF",4,"E1L359C1",398,"L&D Expense, FAB STRUC METAL PRODUCTS",1.3789104223251301,0.26735174655914301,0.109357416629791,0.55470359325408902,0.24174544215202301,0.26759335398674,8.8351674377918202E-2,2.4079890921711901E-2,1.6526019899174599E-3,0.13177579165119599,0.176593743188519,0.36042406768129098,0.20247041874306199,0.685889247456412,6.71721725659165E-3,0.61904499763286203]
["BNSF-E1L360C1","BNSF",4,"E1L360C1",399,"L&D Expense, ALL OTHER FAB METAL PRODUCTS",8.2236602902412401E-2,4.22826893627644E-2,0.12317106872797,0.57348483800888095,0.11085592955350899,0.104633316397667,0.104206696152687,0.41068261861801098,2.90865134447813E-2,2.6793860444710701E-2,1.17116840125649E-2,6.1026978151819303E-2,8.3779653724611707E-3,1.9695008077359299E-2,2.3129155730127701E-3,8.2394414457267903E-2]
["BNSF-E1L361C1","BNSF",4,"E1L361C1",400,"L&D Expense, MACHINERY EXCEPT ELECTRICAL",0.56518673896789595,0.32207629084587103,0.48734244704246499,0.78966307640075695,0.41966882348060602,0.16947755217552199,0.53890877962112405,0.47151488065719599,0.35861149430275002,0.237905620493821,0.107907509116882,0.111111250301434,0.57319507395133296,0.40923914491589602,4.4424753803321601E-2,0.24683393968713699]
["BNSF-E1L362C1","BNSF",4,"E1L362C1",401,"L&D Expense, ENGINES/TURBINES",0,0,0,0.65623474121093806,0.37552052736282299,3.18804383277893E-2,0.92005145549774203,0.18546940386295299,0.75826698541641202,0.10592373868414701,1.7432681007613301E-2,0.11374880081262601,0.19588503448769101,0.627909057749931,-6.83448356503671E-4,0.166006178271392]
["BNSF-E1L363C1","BNSF",4,"E1L363C1",402,"L&D Expense, FARM MACHINERY",2.4298570156097399,1.5298203229904199,1.5081578493118299,2.9845852851867698,1.5362756252288801,0.99220669269561801,0.70848298072814897,1.0776067972183201,0.70382529497146595,1.3448171672090701,0.559861487070207,0.61976011384427698,0.13272710665462301,0.15808913426766,0,0.16933120027486401]
["BNSF-E1L364C1","BNSF",4,"E1L364C1",403,"L&D Expense, CONST MIN/MAT HAND MACHINERY",5.3824152797460598E-2,0.14556503295898399,0.225022718310356,0.24387198686599701,0.111423380672932,1.9659049808979E-2,9.3566169962286897E-3,0.25835311412811302,9.0812714770436304E-3,2.4417359235743799E-2,0.226980429468987,0.123886814731048,5.6786413195415104,5.5626533761732502E-2,0.50608937133810405,2.0688925659798598]
["BNSF-E1L365C1","BNSF",4,"E1L365C1",404,"L&D Expense, ALL OTHER MACHINERY EXCEPT ELECTRICAL",0.51521039009094205,0.112866580486298,0.80271893739700295,0.47596234083175698,0.30874112248420699,4.8945009708404499E-2,0.31174495816230802,0.42183950543403598,4.2986869812011701E-3,0.15186131419488499,9.5799168819499E-2,2.66155263257274E-3,0.14928714522905701,0.14762019602208301,5.02985279069205E-2,3.62333789688866E-2]
["BNSF-E1L366C1","BNSF",4,"E1L366C1",405,"L&D Expense, ELECTRICAL MACHINERY",0.67479163408279397,0.47035461664199801,0.76611125469207797,0.65651184320449796,0.56727981567382801,0.21725417673587799,0.49147397279739402,0.91961038112640403,0.289804667234421,0.44987594767502198,0.21864727922893701,0.110947990600422,0.399700701714716,0.218458461333112,0.13409182722392801,1.67087861140951]
["BNSF-E1L367C1","BNSF",4,"E1L367C1",406,"L&D Expense, ELECTRICAL TRANS/DIST EQUIPMENT",4.9571437835693404,1.3843834400177,1.5912679433822601,0.52243554592132602,0.95162492990493797,1.35360562801361,0.46107843518257102,0.55019402503967296,0.73037481307983398,2.4718954756265998,0.72087862382857204,0.437231102871734,8.2663145076920408,0,1.4978214029207599,2.3871011726206701]
["BNSF-E1L368C1","BNSF",4,"E1L368C1",407,"L&D Expense, HOUSEHOLD APPLIANCES",0.205303609371185,0.23462562263011899,0.17131142318248699,0.277806997299194,0.25822886824607799,8.2644179463386494E-2,0.297059416770935,0.38408657908439597,0.13108573853969599,0.40999757319887098,0.15451085360087599,7.3435426620840294E-2,0.14930913105378599,0.247363305660388,7.2794077869062196E-2,8.71202277086814E-2]
["BNSF-E1L369C1","BNSF",4,"E1L369C1",408,"L&D Expense, RADIO OR TV SETS",6.56506299972534,7.9000549316406303,11.099229812622101,2.6888911724090598,3.2490937709808398,1.53677189350128,5.8817706108093297,24.248622894287099,3.8644213676452601,1.0204034771199,2.4656724349818999,0.16968987712112299,0.212309300578224,0.93635726795096297,0.93072368421052598,7.9683165020530504]
["BNSF-E1L370C1","BNSF",4,"E1L370C1",409,"L&D Expense, ALL OTHER ELECTRICAL MACHINERY",0.72443789243698098,0.124912194907665,1.22650158405304,2.0479607582092298,1.4720858335495,2.7940336614847201E-2,2.5568239390850098E-2,0.79280191659927401,0.32959437370300299,0.11638569092668601,0.15527288252874599,0.20274542735457399,3.8295146556108502E-2,0.100668737420884,0.10349523579893,6.5650136035665803]
["BNSF-E1L371C1","BNSF",4,"E1L371C1",410,"L&D Expense, TRANSPORTAION EQUIPMENT",1.3006241321563701,1.08988153934479,1.35968601703644,1.2409585714340201,0.75661820173263605,1.0195336341857899,1.6047393083572401,1.7275034189224201,2.29360747337341,1.4390260176603999,1.53309053496067,2.5685685982062201,2.42239663922193,2.64924837876096,2.5732802744444401,3.2399183966489802]
["BNSF-E1L372C1","BNSF",4,"E1L372C1",411,"L&D Expense, MOTOR PASSENGER CARS",1.6142339706420901,1.60462009906769,2.0916264057159402,1.80427742004395,1.1449105739593499,1.8661357164382899,2.4315426349639901,2.3879089355468799,2.9647860527038601,2.2775114836972699,2.3379065129382699,4.7704088395188302,3.82250992141388,3.6264625356952398,4.5673487040649103,7.7164689836323603]
["BNSF-E1L373C1","BNSF",4,"E1L373C1",412,"L&D Expense, MOTOR TRUCKS",2.1043250560760498,1.26811671257019,1.65900325775146,1.4032484292984,0.97844052314758301,0.82795894145965598,2.6402244567871098,2.5844602584838898,5.3508419990539604,2.3972440890440101,2.5053101151001802,3.01905989333518,4.5072670290018699,1.8358317475753301,1.9620481392513101,6.0876948799235704]
["BNSF-E1L374C1","BNSF",4,"E1L374C1",413,"L&D Expense, MOTOR VECHICLE PARTS",0.17642442882060999,0.27078187465667702,0.25748610496521002,0.82535320520401001,0.14550699293613401,0.17560070753097501,0.17617671191692399,0.84027493000030495,0.21214038133621199,8.8219921107315594E-2,0.393716560465393,0.212999234670077,0.10576437246174999,0.119489105755487,4.6983042073175697E-3,5.2852034619368202E-2]
["BNSF-E1L375C1","BNSF",4,"E1L375C1",414,"L&D Expense, ALL OTHER TRANSPORTATION EQUIPMENT",2.6227355003356899E-2,0.10049141198396699,3.2508585602045101E-2,6.5525375306606307E-2,0.26267328858375499,3.3132839947938898E-2,5.0899308174848598E-2,6.18039257824421E-2,9.2528991401195498E-2,3.1585700434175697E-2,7.6281476545512997E-2,0.119202553620429,7.6049686090451901E-2,4.0474509693458502,2.3140971066584299,1.6999942051205801E-2]
["BNSF-E1L376C1","BNSF",4,"E1L376C1",415,"L&D Expense, FREIGHT FORWARDER TRAFFIC",3.4748416393995299E-2,0.119148962199688,0.133060157299042,6.0009412467479699E-2,2.6239469647407501E-2,5.6703973561525303E-2,0.39763507246971103,0.102938175201416,0.42134848237037698,0.183535784884371,6.4649280290004899E-2,1.21218522459901E-2,9.2906133987932099E-3,3.4791419592622302E-2,1.53999961012668E-2,7.4345374257392599E-2]
["BNSF-E1L377C1","BNSF",4,"E1L377C1",416,"L&D Expense, SHIPPER ASSOCIATION TRAFFIC",6.9035097956657396E-2,4.24118414521217E-2,0,0,0,0,0.15256458520889299,0,0,0,0,3.9752304352468099E-2,0,1.2640222416189799E-2,0,0]
["BNSF-E1L378C1","BNSF",4,"E1L378C1",417,"L&D Expense, MISC MIXED SHIPMENTS",9.1315463185310405E-2,0.11395051330328,0.119482338428497,7.6815418899059296E-2,6.5753631293773707E-2,4.5803453773260103E-2,6.1025261878967299E-2,5.9127628803253202E-2,6.1889201402664198E-2,4.37200018110191E-2,7.5652365651906694E-2,3.3229987868641203E-2,3.2905317083349601E-2,3.0981519923329901E-2,4.4879455499843499E-2,4.5587054201045099E-2]
["BNSF-E1L379C1","BNSF",4,"E1L379C1",418,"L&D Expense, MISC MIXED SHIPMENTS NEC INC TOFC",9.1119572520256001E-2,0.112067364156246,0.119818732142448,7.3888465762138394E-2,6.1532124876975999E-2,4.5287456363439602E-2,6.1175230890512501E-2,5.8978945016860997E-2,5.8081496506929398E-2,4.2502426273880303E-2,7.4517811883176202E-2,3.2837985738498998E-2,3.2487919273463603E-2,1.9547644020149899E-2,3.9562979823806702E-2,4.5379167595824103E-2]
["BNSF-E1L380C1","BNSF",4,"E1L380C1",419,"L&D Expense, ALL OTHER MIXED SHIPMENTS",0.16601713001728099,0.88630723953247104,1.4442171668633799E-3,0.87179607152938798,0.75372087955474898,0.13352239131927501,3.1231531873345399E-2,9.3002393841743497E-2,1.03999447822571,0.416805851183083,0.345811739282818,0.14978310418351601,0.18150323928185,3.82302116571379,1.53221325354683,0.10334428935010299]
["BNSF-E1L381C1","BNSF",4,"E1L381C1",420,"L&D Expense, HAZARDOUS MATERIALS",3.3822157420218E-3,4.38846610486507E-2,6.9866083562374101E-2,4.1437070816755302E-2,3.1556442379951498E-2,2.9638551175594299E-2,1.43746230751276E-2,2.3880230262875599E-2,1.29652125760913E-2,2.8145488342284499E-2,1.9073883682287199E-2,6.4705703700832298E-3,1.8164087945304101E-2,3.0475595834185201E-2,1.6340194747313699E-2,2.5929638549913699E-2]
["BNSF-E1L382C1","BNSF",4,"E1L382C1",421,"L&D Expense, ALL OTHER COMMODITIES",3.7811581045389203E-2,0.571766257286072,0.50435817241668701,0.395120829343796,0.34854763746261602,0.28982281684875499,1.35337150096893,0.27479436993598899,2.1931312978267701E-2,0.35576115206112802,1.58875264111078,0.37422378104875798,0.25508157108880503,0.88390067928004001,0.16117152606319499,2.4966038048811998]
["BNSF-E2L101C1","BNSF",4,"E2L101C1",422,"Average Tare Weight, BOX - 40 FT",26.200000762939499,26.200000762939499,25.899999618530298,25.299999237060501,26,25.700000762939499,29,28.5,28.5,28.5,27.9,27.5,29,29,29.2,29.2]
["BNSF-E2L101C2","BNSF",4,"E2L101C2",423,"E/L Ratio, Railroad-Owned, BOX - 40 FT",1.7770195007324201,1.7633529901504501,1.74061119556427,1.8270651102066,1.6900835037231401,1.69674396514893,1.8321297168731701,1.75,1.7152529954910301,1.79339048328985,1.8373838055773299,1.8418424666084099,1.8023507931073799,1.8408314350797299,1.7892697466467999,1.7185573366214599]
["BNSF-E2L101C3","BNSF",4,"E2L101C3",424,"E/L Ratio, Privately-Owned, BOX - 40 FT",1.3200867176055899,1.3756275177002,1.4308068752288801,1.49343013763428,1.83215928077698,1.3949719667434699,1.5569306612014799,1.7514580488205,1.77383804321289,1.97731147540984,2.0123339658443999,1.53614718614719,1.57011457156689,1.6998857795545399,2.0009839291570999,1.81388577827548]
["BNSF-E2L101C4","BNSF",4,"E2L101C4",425,"E/L Ratio, All Freight Cars, BOX - 40 FT",1.49763643741608,1.5948581695556601,1.62956643104553,1.7435985803604099,1.7335562705993699,1.55438137054443,1.7011102437973,1.7507294416427599,1.74649298191071,1.8828633405639901,1.90231706458201,1.73002929300926,1.7061497326203201,1.8056703234078899,1.83849321335977,1.7429619861246499]
["BNSF-E2L101C5","BNSF",4,"E2L101C5",426,"Local circuity, BOX - 40 FT",1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999]
["BNSF-E2L101C6","BNSF",4,"E2L101C6",427,"Interline circuity, BOX - 40 FT",1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001]
["BNSF-E2L101C7","BNSF",4,"E2L101C7",428,"Average circuity, BOX - 40 FT",1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999]
["BNSF-E2L101C8","BNSF",4,"E2L101C8",429,"Spotted-to-Pulled Ratio, BOX - 40 FT",1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.8,1.8,1.8,1.8,1.8,1.8,1.8]
["BNSF-E2L101C9","BNSF",4,"E2L101C9",430,"CD per Industry Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L101C10","BNSF",4,"E2L101C10",431,"CD per Interchange Switch, BOX - 40 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L101C11","BNSF",4,"E2L101C11",432,"CD per Intraterminal Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L101C12","BNSF",4,"E2L101C12",433,"CD per Interterminal Switch, BOX - 40 FT",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L101C13","BNSF",4,"E2L101C13",434,"CD per I&I Switch, BOX - 40 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L101C14","BNSF",4,"E2L101C14",435,"CD per Load & Unload Industry Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L101C15","BNSF",4,"E2L101C15",436,"CD per Load & Unload Intraterminal Switch, BOX - 40 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L101C16","BNSF",4,"E2L101C16",437,"CD per Load & Unload Interterminal Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L101C17","BNSF",4,"E2L101C17",438,"CM per Industry Switch, BOX - 40 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L101C18","BNSF",4,"E2L101C18",439,"CM per Interchange Switch, BOX - 40 FT",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L101C19","BNSF",4,"E2L101C19",440,"CM per Intraterminal Switch, BOX - 40 FT",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L101C20","BNSF",4,"E2L101C20",441,"CM per Interterminal Switch, BOX - 40 FT",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L101C21","BNSF",4,"E2L101C21",442,"CM per I&I Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L101C22","BNSF",4,"E2L101C22",443,"Average CM per CD, Railroad-Owned, BOX - 40 FT",422.54244995117199,460.861083984375,462.57946777343801,518.47259521484398,480.34750366210898,441.79348754882801,0,0,370.20086669921898,0,0,0,0,0,0,0]
["BNSF-E2L101C23","BNSF",4,"E2L101C23",444,"Average Miles between I&I Switches, BOX - 40 FT",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L101C24","BNSF",4,"E2L101C24",445,"Average Miles between Interchange Switches, BOX - 40 FT",1820.61865234375,1641.09643554688,1575.5302734375,1476.10168457031,1459.7685546875,1558.6015625,1449.51342773438,1718.83557128906,1507.58996582031,1678.84261169615,1342.5263186915699,1553.22845359858,1597.0528714847001,1359.9146605942301,660.90104924362799,996.41550118520104]
["BNSF-E2L101C25","BNSF",4,"E2L101C25",446,"SEMs per Industry Switch, BOX - 40 FT",4.0653176307678196,4.4621381759643599,4.4837818145751998,4.1883964538574201,4.1100530624389604,0,0,4.3016629219055202,4.2219319343566903,0,0,4.0444730814308798,0,0,4.5028908500984999,0]
["BNSF-E2L101C26","BNSF",4,"E2L101C26",447,"SEMs per Interchange Switch, BOX - 40 FT",2.2359244823455802,2.4541757106781001,2.4660799503326398,2.3036184310913099,2.2605288028717001,0,0,0,0,0,0,0,0,0,0,0]
["BNSF-E2L101C27","BNSF",4,"E2L101C27",448,"SEMs per Intraterminal Switch, BOX - 40 FT",6.0979762077331499,6.6932077407836896,6.7256731986999503,6.2825951576232901,6.16507863998413,0,0,6.4524941444396999,6.3328976631164604,0,0,6.0667096221463197,0,0,6.7543362751477396,0]
[{"$f":"B450&\"-\"&D450","v":"BNSF-E2L101C28"},"BNSF",4,"E2L101C28",449,"SEMs per Interterminal Switch, BOX - 40 FT",4.8783807754516602,5.3545656204223597,5.3805384635925302,5.0260767936706499,4.9320626258850098,0,0,5.1619954109191903,5.0663189888000497,0,0,4.8533676977170499,0,0,5.4034690201181901,0]
["BNSF-E2L101C29","BNSF",4,"E2L101C29",450,"SEMs per I&I Switch, BOX - 40 FT",1.01632940769196,1.11553454399109,1.1209455728530899,1.0470992326736499,1.0275131464004501,1.0619697570800799,0,0,1.0554828643798799,0,0,0,0,0,0,0]
["BNSF-E2L102C1","BNSF",4,"E2L102C1",451,"Average Tare Weight, BOX - 50 FT",33.5,33.900001525878899,34.099998474121101,34.200000762939503,34.5,34.299999237060497,32.599998474121101,32.700000762939503,32.799999237060497,32.799999999999997,32.9,33,33.200000000000003,33.4,33.6,34]
["BNSF-E2L102C2","BNSF",4,"E2L102C2",452,"E/L Ratio, Railroad-Owned, BOX - 50 FT",1.7770195007324201,1.7633529901504501,1.74061119556427,1.8270651102066,1.6900835037231401,1.69674396514893,1.8321297168731701,1.75,1.7152529954910301,1.79339048328985,1.8373838055773299,1.8418424666084099,1.8023507931073799,1.8408314350797299,1.7892697466467999,1.7185573366214599]
["BNSF-E2L102C3","BNSF",4,"E2L102C3",453,"E/L Ratio, Privately-Owned, BOX - 50 FT",1.3200867176055899,1.3756275177002,1.4308068752288801,1.49343013763428,1.83215928077698,1.3949719667434699,1.5569306612014799,1.7514580488205,1.77383804321289,1.97731147540984,2.0123339658443999,1.53614718614719,1.57011457156689,1.6998857795545399,2.0009839291570999,1.81388577827548]
["BNSF-E2L102C4","BNSF",4,"E2L102C4",454,"E/L Ratio, All Freight Cars, BOX - 50 FT",1.49763643741608,1.5948581695556601,1.62956643104553,1.7435985803604099,1.7335562705993699,1.55438137054443,1.7011102437973,1.7507294416427599,1.74649298191071,1.8828633405639901,1.90231706458201,1.73002929300926,1.7061497326203201,1.8056703234078899,1.83849321335977,1.7429619861246499]
["BNSF-E2L102C5","BNSF",4,"E2L102C5",455,"Local circuity, BOX - 50 FT",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["BNSF-E2L102C6","BNSF",4,"E2L102C6",456,"Interline circuity, BOX - 50 FT",1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001]
["BNSF-E2L102C7","BNSF",4,"E2L102C7",457,"Average circuity, BOX - 50 FT",1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999]
["BNSF-E2L102C8","BNSF",4,"E2L102C8",458,"Spotted-to-Pulled Ratio, BOX - 50 FT",1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.8,1.8,1.8,1.8,1.8,1.8,1.8]
["BNSF-E2L102C9","BNSF",4,"E2L102C9",459,"CD per Industry Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L102C10","BNSF",4,"E2L102C10",460,"CD per Interchange Switch, BOX - 50 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L102C11","BNSF",4,"E2L102C11",461,"CD per Intraterminal Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L102C12","BNSF",4,"E2L102C12",462,"CD per Interterminal Switch, BOX - 50 FT",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L102C13","BNSF",4,"E2L102C13",463,"CD per I&I Switch, BOX - 50 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L102C14","BNSF",4,"E2L102C14",464,"CD per Load & Unload Industry Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L102C15","BNSF",4,"E2L102C15",465,"CD per Load & Unload Intraterminal Switch, BOX - 50 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L102C16","BNSF",4,"E2L102C16",466,"CD per Load & Unload Interterminal Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L102C17","BNSF",4,"E2L102C17",467,"CM per Industry Switch, BOX - 50 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L102C18","BNSF",4,"E2L102C18",468,"CM per Interchange Switch, BOX - 50 FT",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L102C19","BNSF",4,"E2L102C19",469,"CM per Intraterminal Switch, BOX - 50 FT",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L102C20","BNSF",4,"E2L102C20",470,"CM per Interterminal Switch, BOX - 50 FT",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L102C21","BNSF",4,"E2L102C21",471,"CM per I&I Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L102C22","BNSF",4,"E2L102C22",472,"Average CM per CD, Railroad-Owned, BOX - 50 FT",422.54251098632801,460.861083984375,462.57952880859398,518.47253417968795,480.34750366210898,441.79342651367199,489.76934814453102,435.22634887695301,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058699,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L102C23","BNSF",4,"E2L102C23",473,"Average Miles between I&I Switches, BOX - 50 FT",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L102C24","BNSF",4,"E2L102C24",474,"Average Miles between Interchange Switches, BOX - 50 FT",1820.61865234375,1641.09643554688,1575.5302734375,1476.10168457031,1459.7685546875,1558.6015625,1449.51342773438,1718.83557128906,1507.58996582031,1678.84261169615,1342.5263186915699,1553.22845359858,1597.0528714847001,1359.9146605942301,660.90104924362799,996.41550118520104]
["BNSF-E2L102C25","BNSF",4,"E2L102C25",475,"SEMs per Industry Switch, BOX - 50 FT",4.0653176307678196,4.4621386528015101,4.48378229141235,4.1883964538574201,4.1100525856018102,4.2478790283203098,4.2663950920104998,4.3016629219055202,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L102C26","BNSF",4,"E2L102C26",476,"SEMs per Interchange Switch, BOX - 50 FT",2.2359247207641602,2.4541759490966801,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363335132598899,2.34651756286621,2.3659148216247599,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L102C27","BNSF",4,"E2L102C27",477,"SEMs per Intraterminal Switch, BOX - 50 FT",6.0979762077331499,6.6932067871093803,6.7256727218627903,6.2825946807861301,6.16507911682129,6.3718180656433097,6.3995933532714799,6.4524946212768599,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L102C28","BNSF",4,"E2L102C28",478,"SEMs per Interterminal Switch, BOX - 50 FT",4.8783807754516602,5.3545660972595197,5.3805384635925302,5.0260758399963397,4.9320635795593297,5.0974555015564,5.1196742057800302,5.1619954109191903,5.0663189888000497,4.8917291675483998,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L102C29","BNSF",4,"E2L102C29",479,"SEMs per I&I Switch, BOX - 50 FT",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470991134643599,1.0275131464004501,1.0619698762893699,1.0665990114212001,1.0754158496856701,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L103C1","BNSF",4,"E2L103C1",480,"Average Tare Weight, BOX - EQUIPPED",36.099998474121101,36.099998474121101,36.200000762939503,36.099998474121101,36.200000762939503,36.200000762939503,36.400001525878899,36.5,36.5,36.5,36.6,36.700000000000003,36.799999999999997,37,37.1,37.299999999999997]
["BNSF-E2L103C2","BNSF",4,"E2L103C2",481,"E/L Ratio, Railroad-Owned, BOX - EQUIPPED",1.7681593894958501,1.7882493734359699,1.7763208150863601,1.8077707290649401,1.7327849864959699,1.7108185291290301,1.76632511615753,1.78800773620605,1.74324202537537,1.7758793671083599,1.8122837022940601,1.8174117856190599,1.7875356609756301,1.80574291771054,1.82297126855741,1.78214878318584]
["BNSF-E2L103C3","BNSF",4,"E2L103C3",482,"E/L Ratio, Privately-Owned, BOX - EQUIPPED",1.5019049644470199,1.4304791688919101,1.3944332599639899,1.4084784984588601,1.4066901206970199,1.3953210115432699,1.4117474555969201,1.4403547048568699,1.41904640197754,1.44599101988454,1.5174711567585399,1.48901201664563,1.4541362798016899,1.4906406021388601,1.47545303801966,1.42666005946482]
["BNSF-E2L103C4","BNSF",4,"E2L103C4",483,"E/L Ratio, All Freight Cars, BOX - EQUIPPED",1.7393386363983201,1.74484992027283,1.7247327566146899,1.7446541786193801,1.6830633878707899,1.67047739028931,1.71206951141357,1.7235753536224401,1.6836897134780899,1.7138176749911,1.7457228825782101,1.72695190747276,1.67319142515582,1.6829142094463101,1.6705160263696299,1.6251898375762599]
["BNSF-E2L103C5","BNSF",4,"E2L103C5",484,"Local circuity, BOX - EQUIPPED",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["BNSF-E2L103C6","BNSF",4,"E2L103C6",485,"Interline circuity, BOX - EQUIPPED",1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999]
["BNSF-E2L103C7","BNSF",4,"E2L103C7",486,"Average circuity, BOX - EQUIPPED",1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999]
["BNSF-E2L103C8","BNSF",4,"E2L103C8",487,"Spotted-to-Pulled Ratio, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L103C9","BNSF",4,"E2L103C9",488,"CD per Industry Switch, BOX - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L103C10","BNSF",4,"E2L103C10",489,"CD per Interchange Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L103C11","BNSF",4,"E2L103C11",490,"CD per Intraterminal Switch, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L103C12","BNSF",4,"E2L103C12",491,"CD per Interterminal Switch, BOX - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L103C13","BNSF",4,"E2L103C13",492,"CD per I&I Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L103C14","BNSF",4,"E2L103C14",493,"CD per Load & Unload Industry Switch, BOX - EQUIPP",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L103C15","BNSF",4,"E2L103C15",494,"CD per Load & Unload Intraterminal Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L103C16","BNSF",4,"E2L103C16",495,"CD per Load & Unload Interterminal Switch, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L103C17","BNSF",4,"E2L103C17",496,"CM per Industry Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L103C18","BNSF",4,"E2L103C18",497,"CM per Interchange Switch, BOX - EQUIPPED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L103C19","BNSF",4,"E2L103C19",498,"CM per Intraterminal Switch, BOX - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L103C20","BNSF",4,"E2L103C20",499,"CM per Interterminal Switch, BOX - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L103C21","BNSF",4,"E2L103C21",500,"CM per I&I Switch, BOX - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L103C22","BNSF",4,"E2L103C22",501,"Average CM per CD, Railroad-Owned, BOX - EQUIPPED",422.54244995117199,460.861083984375,462.57949829101602,518.47259521484398,480.34750366210898,441.79345703125,489.76934814453102,435.22640991210898,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L103C23","BNSF",4,"E2L103C23",502,"Average Miles between I&I Switches, BOX - EQUIPPED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L103C24","BNSF",4,"E2L103C24",503,"Average Miles between Interchange Switches, BOX - EQUIPPED",1337.46704101563,1390.27319335938,1441.04187011719,1706.44091796875,1515.40100097656,999.90710449218795,943.00030517578102,809.68011474609398,851.31604003906295,836.58335955770997,888.31423153950095,736.64022920878494,690.24500756374005,3681.45451230149,4518.6609495246903,4122.1757988478003]
["BNSF-E2L103C25","BNSF",4,"E2L103C25",504,"SEMs per Industry Switch, BOX - EQUIPPED",4.0653176307678196,4.4621381759643599,4.4837818145751998,4.1883969306945801,4.1100525856018102,4.2478790283203098,4.2663950920104998,4.3016633987426802,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L103C26","BNSF",4,"E2L103C26",505,"SEMs per Interchange Switch, BOX - EQUIPPED",2.2359247207641602,2.4541759490966801,2.4660801887512198,2.3036181926727299,2.2605288028717001,2.3363335132598899,2.34651756286621,2.3659145832061799,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L103C27","BNSF",4,"E2L103C27",506,"SEMs per Intraterminal Switch, BOX - EQUIPPED",6.0979757308959996,6.6932072639465297,6.7256731986999503,6.2825951576232901,6.16507863998413,6.3718175888061497,6.3995933532714799,6.4524946212768599,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L103C28","BNSF",4,"E2L103C28",507,"SEMs per Interterminal Switch, BOX - EQUIPPED",4.8783812522888201,5.3545660972595197,5.3805389404296902,5.0260767936706499,4.9320631027221697,5.0974550247192401,5.1196742057800302,5.1619954109191903,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L103C29","BNSF",4,"E2L103C29",508,"SEMs per I&I Switch, BOX - EQUIPPED",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619697570800799,1.0665988922119101,1.0754157304763801,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L104C1","BNSF",4,"E2L104C1",509,"Average Tare Weight, GONDOLA - PLAIN",26,25.899999618530298,25.799999237060501,25.600000381469702,25.5,25.600000381469702,25.299999237060501,25.700000762939499,25.700000762939499,25.6,25.6,25.6,25.7,25.9,26.1,26.3]
["BNSF-E2L104C2","BNSF",4,"E2L104C2",510,"E/L Ratio, Railroad-Owned, GONDOLA - PLAIN",2.0099616050720202,2.0304267406463601,2.0479295253753702,2.02835988998413,1.99021756649017,1.93743407726288,1.81718766689301,1.85487461090088,1.91633260250092,1.96311752539047,1.9724944761204599,1.9142136614635401,1.91910935359991,1.94335922239065,1.9352931089821099,1.8783899246398601]
["BNSF-E2L104C3","BNSF",4,"E2L104C3",511,"E/L Ratio, Privately-Owned, GONDOLA - PLAIN",2.0111155509948699,2.0223829746246298,2.0525860786438002,2.0330584049224898,2.0168092250824001,2.0168111324310298,2.0148065090179399,2.0115661621093799,2.0127766132354701,2.00620898763753,2.0239177595225102,2.0191568339966,2.0204335185726201,2.0158276832357398,2.02410216606975,2.0237784603827502]
["BNSF-E2L104C4","BNSF",4,"E2L104C4",512,"E/L Ratio, All Freight Cars, GONDOLA - PLAIN",2.0108556747436501,2.02430367469788,2.05148124694824,2.03193140029907,2.0101451873779301,1.9982550144195601,1.9706680774688701,1.9786362648010301,1.99484550952911,1.9972722785685499,2.0117359427088402,1.9936469937500401,1.99566582723866,1.99912665249503,2.0018811922578501,1.9874559603133199]
[{"$f":"B514&\"-\"&D514","v":"BNSF-E2L104C5"},"BNSF",4,"E2L104C5",513,"Local circuity, GONDOLA - PLAIN",1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.093,1.093,1.093,1.093,1.093,1.093,1.093]
["BNSF-E2L104C6","BNSF",4,"E2L104C6",514,"Interline circuity, GONDOLA - PLAIN",1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.151,1.151,1.151,1.151,1.151,1.151,1.151]
["BNSF-E2L104C7","BNSF",4,"E2L104C7",515,"Average circuity, GONDOLA - PLAIN",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["BNSF-E2L104C8","BNSF",4,"E2L104C8",516,"Spotted-to-Pulled Ratio, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L104C9","BNSF",4,"E2L104C9",517,"CD per Industry Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L104C10","BNSF",4,"E2L104C10",518,"CD per Interchange Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L104C11","BNSF",4,"E2L104C11",519,"CD per Intraterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L104C12","BNSF",4,"E2L104C12",520,"CD per Interterminal Switch, GONDOLA - PLAIN",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L104C13","BNSF",4,"E2L104C13",521,"CD per I&I Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L104C14","BNSF",4,"E2L104C14",522,"CD per Load & Unload Industry Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L104C15","BNSF",4,"E2L104C15",523,"CD per Load & Unload Intraterminal Switch, GONDOLA - PLAIN",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L104C16","BNSF",4,"E2L104C16",524,"CD per Load & Unload Interterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L104C17","BNSF",4,"E2L104C17",525,"CM per Industry Switch, GONDOLA - PLAIN",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L104C18","BNSF",4,"E2L104C18",526,"CM per Interchange Switch, GONDOLA - PLAIN",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L104C19","BNSF",4,"E2L104C19",527,"CM per Intraterminal Switch, GONDOLA - PLAIN",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L104C20","BNSF",4,"E2L104C20",528,"CM per Interterminal Switch, GONDOLA - PLAIN",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L104C21","BNSF",4,"E2L104C21",529,"CM per I&I Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L104C22","BNSF",4,"E2L104C22",530,"Average CM per CD, Railroad-Owned, GONDOLA - PLAIN",422.54244995117199,460.86105346679699,462.57952880859398,518.47253417968795,480.34753417968801,441.79345703125,489.76931762695301,435.22634887695301,370.20083618164102,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L104C23","BNSF",4,"E2L104C23",531,"Average Miles between I&I Switches, GONDOLA - PLAIN",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L104C24","BNSF",4,"E2L104C24",532,"Average Miles between Interchange Switches, GONDOLA - PLAIN",1723.33068847656,1958.47790527344,2049.78344726563,2338.42797851563,2825.38354492188,2487.1279296875,2482.17553710938,2751.71801757813,2880.85205078125,2318.8345061155901,2600.9430912933799,4083.7064502396902,3107.6849047021701,3336.5058900866402,3556.2727229808202,3545.4398019516698]
["BNSF-E2L104C25","BNSF",4,"E2L104C25",533,"SEMs per Industry Switch, GONDOLA - PLAIN",4.0653176307678196,4.4621386528015101,4.4837818145751998,4.1883964538574201,4.1100525856018102,4.2478785514831499,4.2663955688476598,4.3016633987426802,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L104C26","BNSF",4,"E2L104C26",534,"SEMs per Interchange Switch, GONDOLA - PLAIN",2.2359247207641602,2.4541757106781001,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363335132598899,2.34651780128479,2.3659148216247599,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L104C27","BNSF",4,"E2L104C27",535,"SEMs per Intraterminal Switch, GONDOLA - PLAIN",6.0979762077331499,6.6932072639465297,6.7256731986999503,6.2825951576232901,6.1650795936584499,6.3718185424804696,6.3995933532714799,6.4524946212768599,6.3328981399536097,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L104C28","BNSF",4,"E2L104C28",536,"SEMs per Interterminal Switch, GONDOLA - PLAIN",4.8783807754516602,5.3545660972595197,5.3805389404296902,5.0260767936706499,4.9320635795593297,5.0974550247192401,5.1196742057800302,5.1619954109191903,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L104C29","BNSF",4,"E2L104C29",537,"SEMs per I&I Switch, GONDOLA - PLAIN",1.01632940769196,1.11553454399109,1.1209455728530899,1.0470992326736499,1.0275131464004501,1.0619698762893699,1.0665988922119101,1.0754158496856701,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L105C1","BNSF",4,"E2L105C1",538,"Average Tare Weight, GONDOLA - EQUIPPED",33.099998474121101,33.200000762939503,33.400001525878899,33.299999237060497,33.299999237060497,33.299999237060497,33.299999237060497,33.099998474121101,33.099998474121101,33.200000000000003,33.200000000000003,33.1,33.1,33.1,33.1,33.1]
["BNSF-E2L105C2","BNSF",4,"E2L105C2",539,"E/L Ratio, Railroad-Owned, GONDOLA - EQUIPPED",1.87142133712769,1.9786674976348899,1.94682645797729,2.0709638595581099,1.9657680988311801,1.90189874172211,1.94499027729034,1.99526047706604,1.9332066774368299,2.0975424124131501,1.9928096308787699,1.96920138888889,1.88811872979023,1.9490785005439999,1.94286166230205,1.8634285274420801]
["BNSF-E2L105C3","BNSF",4,"E2L105C3",540,"E/L Ratio, Privately-Owned, GONDOLA - EQUIPPED",2.0592288970947301,2.10274457931519,2.1063144207000701,2.0495913028717001,2.0154328346252401,2.1018939018249498,2.01773953437805,2.0608935356140101,2.1164324283599898,2.0962396430847701,2.0554049474754299,2.0420131607491498,2.0612406610821798,2.05435660703982,2.0100792968376799,1.9965569408941499]
["BNSF-E2L105C4","BNSF",4,"E2L105C4",541,"E/L Ratio, All Freight Cars, GONDOLA - EQUIPPED",1.9537699222564699,2.0161478519439702,1.9709175825119001,2.0674247741699201,1.9738010168075599,1.9374738931655899,1.9610579013824501,2.0105116367340101,1.97121894359589,2.0972070298257099,2.0063669724770601,1.9832981002114001,1.92734664563375,1.9724715355421101,1.9609410132209499,1.89376396747658]
["BNSF-E2L105C5","BNSF",4,"E2L105C5",542,"Local circuity, GONDOLA - EQUIPPED",1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001]
["BNSF-E2L105C6","BNSF",4,"E2L105C6",543,"Interline circuity, GONDOLA - EQUIPPED",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["BNSF-E2L105C7","BNSF",4,"E2L105C7",544,"Average circuity, GONDOLA - EQUIPPED",1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.119,1.119,1.119,1.119,1.119,1.119,1.119]
["BNSF-E2L105C8","BNSF",4,"E2L105C8",545,"Spotted-to-Pulled Ratio, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L105C9","BNSF",4,"E2L105C9",546,"CD per Industry Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L105C10","BNSF",4,"E2L105C10",547,"CD per Interchange Switch, GONDOLA - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L105C11","BNSF",4,"E2L105C11",548,"CD per Intraterminal Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L105C12","BNSF",4,"E2L105C12",549,"CD per Interterminal Switch, GONDOLA - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L105C13","BNSF",4,"E2L105C13",550,"CD per I&I Switch, GONDOLA - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L105C14","BNSF",4,"E2L105C14",551,"CD per Load & Unload Industry Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L105C15","BNSF",4,"E2L105C15",552,"CD per Load & Unload Intraterminal Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L105C16","BNSF",4,"E2L105C16",553,"CD per Load & Unload Interterminal Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L105C17","BNSF",4,"E2L105C17",554,"CM per Industry Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L105C18","BNSF",4,"E2L105C18",555,"CM per Interchange Switch, GONDOLA - EQUIPPED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L105C19","BNSF",4,"E2L105C19",556,"CM per Intraterminal Switch, GONDOLA - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L105C20","BNSF",4,"E2L105C20",557,"CM per Interterminal Switch, GONDOLA - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L105C21","BNSF",4,"E2L105C21",558,"CM per I&I Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L105C22","BNSF",4,"E2L105C22",559,"Average CM per CD, Railroad-Owned, GONDOLA - EQUIPPED",422.54244995117199,460.86105346679699,462.57952880859398,518.47253417968795,480.34750366210898,441.79345703125,489.76931762695301,435.22637939453102,370.20089721679699,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L105C23","BNSF",4,"E2L105C23",560,"Average Miles between I&I Switches, GONDOLA - EQUIPPED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L105C24","BNSF",4,"E2L105C24",561,"Average Miles between Interchange Switches, GONDOLA - EQUIPPED",1782.30200195313,1182.69958496094,1112.12426757813,1321.07299804688,1408.08935546875,1132.27099609375,1037.96069335938,990.025634765625,848.43127441406295,945.84619996344702,999.84180129458105,1222.7331094040401,1408.6939690607001,1439.1741271062899,1692.47107768161,1364.30463081419]
["BNSF-E2L105C25","BNSF",4,"E2L105C25",562,"SEMs per Industry Switch, GONDOLA - EQUIPPED",4.0653181076049796,4.4621381759643599,4.4837818145751998,4.1883964538574201,4.1100525856018102,4.2478790283203098,4.2663950920104998,4.3016633987426802,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L105C26","BNSF",4,"E2L105C26",563,"SEMs per Interchange Switch, GONDOLA - EQUIPPED",2.2359244823455802,2.4541759490966801,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363335132598899,2.34651756286621,2.3659145832061799,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L105C27","BNSF",4,"E2L105C27",564,"SEMs per Intraterminal Switch, GONDOLA - EQUIPPED",6.0979757308959996,6.6932072639465297,6.7256731986999503,6.2825951576232901,6.16507816314697,6.3718185424804696,6.3995933532714799,6.4524941444396999,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L105C28","BNSF",4,"E2L105C28",565,"SEMs per Interterminal Switch, GONDOLA - EQUIPPED",4.8783812522888201,5.3545660972595197,5.3805389404296902,5.0260758399963397,4.9320631027221697,5.0974555015564,5.1196742057800302,5.1619954109191903,5.0663185119628897,4.8917291675483998,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L105C29","BNSF",4,"E2L105C29",566,"SEMs per I&I Switch, GONDOLA - EQUIPPED",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619698762893699,1.0665990114212001,1.0754157304763801,1.0554828643798799,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L106C1","BNSF",4,"E2L106C1",567,"Average Tare Weight, HOPPER - COVERED",31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.200000762939499,31.100000381469702,31,30.8,30.8,30.8,30.8,30.8,30.8,30.9]
["BNSF-E2L106C2","BNSF",4,"E2L106C2",568,"E/L Ratio, Railroad-Owned, HOPPER - COVERED",1.9814705848693801,1.9681659936904901,1.96775710582733,1.9690639972686801,1.97383189201355,1.9710119962692301,1.9980370998382599,2.0126354694366499,1.9676166772842401,2.0134177826431698,1.97740751560489,2.0166272299606698,2.0005220769807202,2.0072083686224902,1.94922876966772,1.9377398486897399]
["BNSF-E2L106C3","BNSF",4,"E2L106C3",569,"E/L Ratio, Privately-Owned, HOPPER - COVERED",1.98851311206818,2.0119080543518102,2.0223300457000701,2.0270829200744598,2.0084269046783398,2.0160112380981401,2.03424000740051,2.0226976871490501,2.02357006072998,2.07016812219933,2.06407110563091,2.0500381784255701,2.0541079871082601,2.0866313598454198,2.0658502100054101,2.0373271972243701]
["BNSF-E2L106C4","BNSF",4,"E2L106C4",570,"E/L Ratio, All Freight Cars, HOPPER - COVERED",1.9840738773345901,1.9841099977493299,1.9866813421249401,1.9905202388763401,1.98578941822052,1.9870418310165401,2.0119144916534402,2.0168917179107702,1.9916400909423799,2.03620725606382,2.01059985564613,2.0310240913538,2.0233717169137999,2.04136471954051,1.9925411053897999,1.9779674678672601]
["BNSF-E2L106C5","BNSF",4,"E2L106C5",571,"Local circuity, HOPPER - COVERED",1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999]
["BNSF-E2L106C6","BNSF",4,"E2L106C6",572,"Interline circuity, HOPPER - COVERED",1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999]
["BNSF-E2L106C7","BNSF",4,"E2L106C7",573,"Average circuity, HOPPER - COVERED",1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999]
["BNSF-E2L106C8","BNSF",4,"E2L106C8",574,"Spotted-to-Pulled Ratio, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L106C9","BNSF",4,"E2L106C9",575,"CD per Industry Switch, HOPPER - COVERED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L106C10","BNSF",4,"E2L106C10",576,"CD per Interchange Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[{"$f":"B578&\"-\"&D578","v":"BNSF-E2L106C11"},"BNSF",4,"E2L106C11",577,"CD per Intraterminal Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L106C12","BNSF",4,"E2L106C12",578,"CD per Interterminal Switch, HOPPER - COVERED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L106C13","BNSF",4,"E2L106C13",579,"CD per I&I Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L106C14","BNSF",4,"E2L106C14",580,"CD per Load & Unload Industry Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L106C15","BNSF",4,"E2L106C15",581,"CD per Load & Unload Intraterminal Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L106C16","BNSF",4,"E2L106C16",582,"CD per Load & Unload Interterminal Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L106C17","BNSF",4,"E2L106C17",583,"CM per Industry Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L106C18","BNSF",4,"E2L106C18",584,"CM per Interchange Switch, HOPPER - COVERED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L106C19","BNSF",4,"E2L106C19",585,"CM per Intraterminal Switch, HOPPER - COVERED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L106C20","BNSF",4,"E2L106C20",586,"CM per Interterminal Switch, HOPPER - COVERED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L106C21","BNSF",4,"E2L106C21",587,"CM per I&I Switch, HOPPER - COVERED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L106C22","BNSF",4,"E2L106C22",588,"Average CM per CD, Railroad-Owned, HOPPER - COVERED",422.54244995117199,460.86102294921898,462.57949829101602,518.47259521484398,480.34747314453102,441.79345703125,489.76937866210898,435.22637939453102,370.20083618164102,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058699,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L106C23","BNSF",4,"E2L106C23",589,"Average Miles between I&I Switches, HOPPER - COVERED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L106C24","BNSF",4,"E2L106C24",590,"Average Miles between Interchange Switches, HOPPER - COVERED",1821.92834472656,2364.462890625,2743.46655273438,3555.02368164063,3235.60375976563,3229.568359375,2693.39990234375,2766.91870117188,3023.23291015625,3127.40532365833,3594.30583338621,2899.4380634588301,3714.7046797623002,3837.3410283673102,4859.6554056372397,4642.89927242678]
["BNSF-E2L106C25","BNSF",4,"E2L106C25",591,"SEMs per Industry Switch, HOPPER - COVERED",4.0653176307678196,4.4621386528015101,4.4837818145751998,4.1883964538574201,4.1100525856018102,4.2478790283203098,4.2663955688476598,4.3016629219055202,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L106C26","BNSF",4,"E2L106C26",592,"SEMs per Interchange Switch, HOPPER - COVERED",2.2359247207641602,2.4541757106781001,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363335132598899,2.34651780128479,2.3659148216247599,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L106C27","BNSF",4,"E2L106C27",593,"SEMs per Intraterminal Switch, HOPPER - COVERED",6.0979762077331499,6.6932077407836896,6.7256731986999503,6.2825946807861301,6.16507863998413,6.3718185424804696,6.3995933532714799,6.4524946212768599,6.3328971862793004,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L106C28","BNSF",4,"E2L106C28",594,"SEMs per Interterminal Switch, HOPPER - COVERED",4.8783807754516602,5.3545660972595197,5.3805389404296902,5.0260763168334996,4.9320635795593297,5.0974550247192401,5.1196742057800302,5.1619954109191903,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L106C29","BNSF",4,"E2L106C29",595,"SEMs per I&I Switch, HOPPER - COVERED",1.01632928848267,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619697570800799,1.0665988922119101,1.0754157304763801,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L107C1","BNSF",4,"E2L107C1",596,"Average Tare Weight, HOPPER - OPEN TOP - GENERAL",29.799999237060501,29.700000762939499,29.600000381469702,29.600000381469702,29.5,29.600000381469702,29.399999618530298,29.200000762939499,29,28.9,28.8,28.8,28.7,28.5,28.4,28.3]
["BNSF-E2L107C2","BNSF",4,"E2L107C2",597,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.0714659690856898,2.18712377548218,2.0212545394897501,2.1689324378967298,2.0496950149536102,2.1988396644592298,2.3384380340576199,2.3389210700988801,2.2904250621795699,2.3846267118244699,2.37579063424824,2.2346614655893,2.2036083589322,2.5173896053145799,2.6716399805919502,2.37989904988124]
["BNSF-E2L107C3","BNSF",4,"E2L107C3",598,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - GENERAL",1.9856146574020399,2.0077121257782,2.0112378597259499,2.0360877513885498,1.9975789785385101,2.0218589305877699,2.0244765281677202,2.0046355724334699,1.9864016771316499,2.0053726899051698,2.0013681762211002,2.00228686911663,2.0015096968993098,2.02970782791115,2.01084674597621,2.0117632469396098]
["BNSF-E2L107C4","BNSF",4,"E2L107C4",599,"E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - GENERAL",2.0266997814178498,2.0872004032135001,2.0156619548797599,2.0891866683960001,2.0192120075225799,2.0916435718536399,2.1542108058929399,2.1441335678100599,2.1061818599700901,2.09940730463568,2.0865992999141398,2.05836942195443,2.0639751801976498,2.1164886515353798,2.1021143278380898,2.08269569072784]
["BNSF-E2L107C5","BNSF",4,"E2L107C5",600,"Local circuity, HOPPER - OPEN TOP - GENERAL",1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001]
["BNSF-E2L107C6","BNSF",4,"E2L107C6",601,"Interline circuity, HOPPER - OPEN TOP - GENERAL",1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.137,1.137,1.137,1.137,1.137,1.137,1.137]
["BNSF-E2L107C7","BNSF",4,"E2L107C7",602,"Average circuity, HOPPER - OPEN TOP - GENERAL",1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001]
["BNSF-E2L107C8","BNSF",4,"E2L107C8",603,"Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L107C9","BNSF",4,"E2L107C9",604,"CD per Industry Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L107C10","BNSF",4,"E2L107C10",605,"CD per Interchange Switch, HOPPER - OPEN TOP - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L107C11","BNSF",4,"E2L107C11",606,"CD per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L107C12","BNSF",4,"E2L107C12",607,"CD per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L107C13","BNSF",4,"E2L107C13",608,"CD per I&I Switch, HOPPER - OPEN TOP - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L107C14","BNSF",4,"E2L107C14",609,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L107C15","BNSF",4,"E2L107C15",610,"CD per Load & Unload Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L107C16","BNSF",4,"E2L107C16",611,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L107C17","BNSF",4,"E2L107C17",612,"CM per Industry Switch, HOPPER - OPEN TOP - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L107C18","BNSF",4,"E2L107C18",613,"CM per Interchange Switch, HOPPER - OPEN TOP - GENERAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L107C19","BNSF",4,"E2L107C19",614,"CM per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L107C20","BNSF",4,"E2L107C20",615,"CM per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L107C21","BNSF",4,"E2L107C21",616,"CM per I&I Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L107C22","BNSF",4,"E2L107C22",617,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",422.54244995117199,460.86105346679699,462.57952880859398,518.47259521484398,480.34747314453102,441.79345703125,489.76934814453102,435.22637939453102,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L107C23","BNSF",4,"E2L107C23",618,"Average Miles between I&I Switches, HOPPER - OPEN TOP - GENERAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L107C24","BNSF",4,"E2L107C24",619,"Average Miles between Interchange Switches, HOPPER - OPEN TOP - GENERAL",509.41418457031301,419.03842163085898,538.05218505859398,757.96466064453102,715.513427734375,1027.85363769531,1335.67724609375,1118.81848144531,1110.15576171875,631.44535960284895,2630.2275185719,2378.7271811659598,3083.4983138369398,2882.55164903676,3072.9295651535499,2237.7493173849198]
["BNSF-E2L107C25","BNSF",4,"E2L107C25",620,"SEMs per Industry Switch, HOPPER - OPEN TOP - GENERAL",4.0653176307678196,4.4621386528015101,4.4837818145751998,4.1883969306945801,4.1100525856018102,4.2478785514831499,4.2663950920104998,4.3016629219055202,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L107C26","BNSF",4,"E2L107C26",621,"SEMs per Interchange Switch, HOPPER - OPEN TOP - GENERAL",2.2359247207641602,2.4541759490966801,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363332748413099,2.34651756286621,2.3659145832061799,2.3220627307891801,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L107C27","BNSF",4,"E2L107C27",622,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",6.0979762077331499,6.6932072639465297,6.7256736755371103,6.2825951576232901,6.16507863998413,6.3718180656433097,6.3995938301086399,6.45249366760254,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L107C28","BNSF",4,"E2L107C28",623,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",4.8783807754516602,5.3545660972595197,5.3805389404296902,5.0260758399963397,4.9320635795593297,5.0974550247192401,5.1196742057800302,5.1619954109191903,5.0663189888000497,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L107C29","BNSF",4,"E2L107C29",624,"SEMs per I&I Switch, HOPPER - OPEN TOP - GENERAL",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470991134643599,1.0275131464004501,1.0619697570800799,1.0665990114212001,1.0754157304763801,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L108C1","BNSF",4,"E2L108C1",625,"Average Tare Weight, HOPPER - OPEN TOP - SPECIAL",27.299999237060501,27.399999618530298,26.899999618530298,26.799999237060501,26.700000762939499,26.799999237060501,26.5,26.5,26.399999618530298,26.4,26.4,26.2,26.1,26.1,26,26]
["BNSF-E2L108C2","BNSF",4,"E2L108C2",626,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.95420110225677,2.0021722316741899,2.00008296966553,2.0415613651275599,2.0155766010284402,2.0691711902618399,2.1781671047210698,2.12883424758911,2.0200672149658199,2.0162982956850102,2.0129656112968499,2.0046262405192299,2.0062094136607098,2.0105091914755202,2.0037300231483801,2.0117478284449701]
["BNSF-E2L108C3","BNSF",4,"E2L108C3",627,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - SPECIAL",2.02046465873718,2.0175929069518999,2.0243399143218999,2.0305912494659402,2.0346095561981201,2.0303037166595499,2.0162873268127401,2.0190665721893302,2.0164277553558398,2.0001997919896199,2.0112196978884498,2.00982554184302,2.0245043775787499,2.0574411308643801,2.02131929617549,2.0177119584783401]
["BNSF-E2L108C4","BNSF",4,"E2L108C4",628,"E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - SPECIAL",2.00988101959229,2.0151572227478001,2.0205285549163801,2.0320904254913299,2.0315647125244101,2.0360348224639901,2.0419037342071502,2.0355451107025102,2.0170657634735099,2.0027943817593798,2.0114833220120798,2.0089529970819502,2.0201269113973601,2.04725855752194,2.0179240423339899,2.0166591778342902]
["BNSF-E2L108C5","BNSF",4,"E2L108C5",629,"Local circuity, HOPPER - OPEN TOP - SPECIAL",1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.202,1.202,1.202,1.202,1.202,1.202,1.202]
["BNSF-E2L108C6","BNSF",4,"E2L108C6",630,"Interline circuity, HOPPER - OPEN TOP - SPECIAL",1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999]
["BNSF-E2L108C7","BNSF",4,"E2L108C7",631,"Average circuity, HOPPER - OPEN TOP - SPECIAL",1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001]
["BNSF-E2L108C8","BNSF",4,"E2L108C8",632,"Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L108C9","BNSF",4,"E2L108C9",633,"CD per Industry Switch, HOPPER - OPEN TOP - SPECIAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L108C10","BNSF",4,"E2L108C10",634,"CD per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L108C11","BNSF",4,"E2L108C11",635,"CD per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L108C12","BNSF",4,"E2L108C12",636,"CD per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L108C13","BNSF",4,"E2L108C13",637,"CD per I&I Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L108C14","BNSF",4,"E2L108C14",638,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L108C15","BNSF",4,"E2L108C15",639,"CD per Load & Unload Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L108C16","BNSF",4,"E2L108C16",640,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
[{"$f":"B642&\"-\"&D642","v":"BNSF-E2L108C17"},"BNSF",4,"E2L108C17",641,"CM per Industry Switch, HOPPER - OPEN TOP - SPECIAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L108C18","BNSF",4,"E2L108C18",642,"CM per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L108C19","BNSF",4,"E2L108C19",643,"CM per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L108C20","BNSF",4,"E2L108C20",644,"CM per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L108C21","BNSF",4,"E2L108C21",645,"CM per I&I Switch, HOPPER - OPEN TOP - SPECIAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L108C22","BNSF",4,"E2L108C22",646,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",422.54248046875,460.86105346679699,462.57949829101602,518.47259521484398,480.34753417968801,441.79345703125,489.76931762695301,435.22637939453102,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058699,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L108C23","BNSF",4,"E2L108C23",647,"Average Miles between I&I Switches, HOPPER - OPEN TOP - SPECIAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L108C24","BNSF",4,"E2L108C24",648,"Average Miles between Interchange Switches, HOPPER - OPEN TOP - SPECIAL",1985.42260742188,1809.76452636719,1646.25244140625,1762.01965332031,1788.31701660156,2011.74633789063,2364.822265625,2498.8154296875,2181.14404296875,2352.5426925591401,2133.2392484131801,1878.1919285624699,2278.3002327863601,1592.5317094576201,1373.60585714226,1429.0413811045801]
["BNSF-E2L108C25","BNSF",4,"E2L108C25",649,"SEMs per Industry Switch, HOPPER - OPEN TOP - SPECIAL",4.0653171539306596,4.4621381759643599,4.4837818145751998,4.1883964538574201,4.1100530624389604,4.2478790283203098,4.2663950920104998,4.3016629219055202,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L108C26","BNSF",4,"E2L108C26",650,"SEMs per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",2.2359247207641602,2.4541757106781001,2.4660804271697998,2.3036179542541499,2.2605290412902801,2.3363332748413099,2.34651780128479,2.3659145832061799,2.3220627307891801,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L108C27","BNSF",4,"E2L108C27",651,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",6.0979762077331499,6.6932072639465297,6.7256727218627903,6.2825946807861301,6.16507863998413,6.3718190193176296,6.3995933532714799,6.4524946212768599,6.3328971862793004,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L108C28","BNSF",4,"E2L108C28",652,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",4.8783807754516602,5.3545660972595197,5.3805389404296902,5.0260763168334996,4.9320631027221697,5.0974555015564,5.1196742057800302,5.1619954109191903,5.0663189888000497,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L108C29","BNSF",4,"E2L108C29",653,"SEMs per I&I Switch, HOPPER - OPEN TOP - SPECIAL",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470991134643599,1.0275131464004501,1.0619697570800799,1.0665990114212001,1.0754156112670901,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L109C1","BNSF",4,"E2L109C1",654,"Average Tare Weight, REFRIGERATED - MECH",46.099998474121101,46.099998474121101,46.400001525878899,46.599998474121101,46.599998474121101,46.5,46.599998474121101,47,47.200000762939503,47.5,48.2,48.3,48.4,48.6,48.9,49.2]
["BNSF-E2L109C2","BNSF",4,"E2L109C2",655,"E/L Ratio, Railroad-Owned, REFRIGERATED - MECH",1.7828347682952901,1.71640968322754,1.6582058668136599,1.56750583648682,1.56626188755035,1.48890864849091,1.59937024116516,1.6357409954071001,1.61179983615875,1.64271086650454,1.5767090289891199,1.54194991825144,1.6019713001884299,1.6605098361692701,1.6771435917213,1.7902559358618599]
["BNSF-E2L109C3","BNSF",4,"E2L109C3",656,"E/L Ratio, Privately-Owned, REFRIGERATED - MECH",2.0862562656402601,1.9416322708129901,1.9705212116241499,1.97628939151764,2.0044276714325,1.9983670711517301,1.9507856369018599,2.0337586402893102,2.0531132221221902,2.04095623132361,2.0776131045241799,2.1084661560753499,2.1741230299949201,2.17310572027553,2.2344312918167799,2.20893484198205]
["BNSF-E2L109C4","BNSF",4,"E2L109C4",657,"E/L Ratio, All Freight Cars, REFRIGERATED - MECH",1.8215149641037001,1.7559913396835301,1.7225300073623699,1.67633104324341,1.6745194196701001,1.5837640762329099,1.6618722677230799,1.72817671298981,1.7120521068573,1.7490030494956601,1.7263354109628899,1.7083029418915601,1.7289081885856099,1.74989555044913,1.7885208804772701,1.8908204863877001]
["BNSF-E2L109C5","BNSF",4,"E2L109C5",658,"Local circuity, REFRIGERATED - MECH",1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.079,1.079,1.079,1.079,1.079,1.079,1.079]
["BNSF-E2L109C6","BNSF",4,"E2L109C6",659,"Interline circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["BNSF-E2L109C7","BNSF",4,"E2L109C7",660,"Average circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["BNSF-E2L109C8","BNSF",4,"E2L109C8",661,"Spotted-to-Pulled Ratio, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L109C9","BNSF",4,"E2L109C9",662,"CD per Industry Switch, REFRIGERATED - MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L109C10","BNSF",4,"E2L109C10",663,"CD per Interchange Switch, REFRIGERATED - MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L109C11","BNSF",4,"E2L109C11",664,"CD per Intraterminal Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L109C12","BNSF",4,"E2L109C12",665,"CD per Interterminal Switch, REFRIGERATED - MECH",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L109C13","BNSF",4,"E2L109C13",666,"CD per I&I Switch, REFRIGERATED - MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L109C14","BNSF",4,"E2L109C14",667,"CD per Load & Unload Industry Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L109C15","BNSF",4,"E2L109C15",668,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L109C16","BNSF",4,"E2L109C16",669,"CD per Load & Unload Interterminal Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L109C17","BNSF",4,"E2L109C17",670,"CM per Industry Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L109C18","BNSF",4,"E2L109C18",671,"CM per Interchange Switch, REFRIGERATED - MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L109C19","BNSF",4,"E2L109C19",672,"CM per Intraterminal Switch, REFRIGERATED - MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L109C20","BNSF",4,"E2L109C20",673,"CM per Interterminal Switch, REFRIGERATED - MECH",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L109C21","BNSF",4,"E2L109C21",674,"CM per I&I Switch, REFRIGERATED - MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L109C22","BNSF",4,"E2L109C22",675,"Average CM per CD, Railroad-Owned, REFRIGERATED - MECH",422.54244995117199,460.86102294921898,462.57955932617199,518.47253417968795,480.34753417968801,441.79348754882801,489.76931762695301,435.22637939453102,370.20089721679699,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L109C23","BNSF",4,"E2L109C23",676,"Average Miles between I&I Switches, REFRIGERATED - MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L109C24","BNSF",4,"E2L109C24",677,"Average Miles between Interchange Switches, REFRIGERATED - MECH",1442.69396972656,1557.25646972656,1683.06530761719,2286.88647460938,2452.89916992188,2070.86376953125,1857.876953125,1885.7255859375,2307.62426757813,1596.0823189365201,1838.62198397509,1583.5270507642399,1921.74620582638,1969.04205541186,2210.0400813880701,2019.9803400154599]
["BNSF-E2L109C25","BNSF",4,"E2L109C25",678,"SEMs per Industry Switch, REFRIGERATED - MECH",4.0653176307678196,4.4621381759643599,4.48378229141235,4.1883964538574201,4.1100530624389604,4.2478790283203098,4.2663950920104998,4.3016629219055202,4.2219314575195304,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L109C26","BNSF",4,"E2L109C26",679,"SEMs per Interchange Switch, REFRIGERATED - MECH",2.2359247207641602,2.4541759490966801,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363332748413099,2.3465173244476301,2.3659148216247599,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L109C27","BNSF",4,"E2L109C27",680,"SEMs per Intraterminal Switch, REFRIGERATED - MECH",6.0979757308959996,6.6932072639465297,6.7256736755371103,6.2825946807861301,6.16507863998413,6.3718185424804696,6.3995938301086399,6.4524946212768599,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L109C28","BNSF",4,"E2L109C28",681,"SEMs per Interterminal Switch, REFRIGERATED - MECH",4.8783812522888201,5.3545660972595197,5.3805384635925302,5.0260763168334996,4.9320631027221697,5.0974550247192401,5.1196742057800302,5.1619958877563503,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L109C29","BNSF",4,"E2L109C29",682,"SEMs per I&I Switch, REFRIGERATED - MECH",1.01632940769196,1.11553454399109,1.1209455728530899,1.0470992326736499,1.0275131464004501,1.0619698762893699,1.0665988922119101,1.0754158496856701,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L110C1","BNSF",4,"E2L110C1",683,"Average Tare Weight, REFRIGERATED - NON-MECH",42.799999237060497,42.900001525878899,43.099998474121101,43.299999237060497,43.799999237060497,43.400001525878899,44,44.099998474121101,44.099998474121101,44.2,44.2,44.2,44.2,44.2,44.6,45.2]
["BNSF-E2L110C2","BNSF",4,"E2L110C2",684,"E/L Ratio, Railroad-Owned, REFRIGERATED - NON-MECH",1.6517231464386,1.69428098201752,1.6462640762329099,1.6685549020767201,1.76438772678375,1.7673796415328999,1.7749259471893299,1.74956631660461,1.74260401725769,1.76588298921516,1.74667153018421,1.76512088783195,1.67804378782485,1.7663614258368301,1.8717779971481801,1.8941894000283701]
["BNSF-E2L110C3","BNSF",4,"E2L110C3",685,"E/L Ratio, Privately-Owned, REFRIGERATED - NON-MECH",2.1410789489746098,1.9571734666824301,2.1091954708099401,2.04887723922729,1.97924292087555,1.9935233592987101,1.94254446029663,2.0307414531707799,2.0793268680572501,1.9762532981530301,2.0132743362831902,2.0045558086560402,2.07600950118765,2.1555555555555599,2.9591836734693899,2.07784431137725]
["BNSF-E2L110C4","BNSF",4,"E2L110C4",686,"E/L Ratio, All Freight Cars, REFRIGERATED - NON-MECH",1.65549075603485,1.6964651346206701,1.6511732339859,1.67573022842407,1.7696048021316499,1.7725626230239899,1.77878105640411,1.7544745206832899,1.7472223043441799,1.7683892870614899,1.7509958014856299,1.76921578557793,1.68536233783253,1.7681651990318801,1.8775910975343699,1.8970444496160099]
["BNSF-E2L110C5","BNSF",4,"E2L110C5",687,"Local circuity, REFRIGERATED - NON-MECH",1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001]
["BNSF-E2L110C6","BNSF",4,"E2L110C6",688,"Interline circuity, REFRIGERATED - NON-MECH",1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.159,1.159,1.159,1.159,1.159,1.159,1.159]
["BNSF-E2L110C7","BNSF",4,"E2L110C7",689,"Average circuity, REFRIGERATED - NON-MECH",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["BNSF-E2L110C8","BNSF",4,"E2L110C8",690,"Spotted-to-Pulled Ratio, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L110C9","BNSF",4,"E2L110C9",691,"CD per Industry Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L110C10","BNSF",4,"E2L110C10",692,"CD per Interchange Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L110C11","BNSF",4,"E2L110C11",693,"CD per Intraterminal Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L110C12","BNSF",4,"E2L110C12",694,"CD per Interterminal Switch, REFRIGERATED - NON-MECH",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L110C13","BNSF",4,"E2L110C13",695,"CD per I&I Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L110C14","BNSF",4,"E2L110C14",696,"CD per Load & Unload Industry Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L110C15","BNSF",4,"E2L110C15",697,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - NON-MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L110C16","BNSF",4,"E2L110C16",698,"CD per Load & Unload Interterminal Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L110C17","BNSF",4,"E2L110C17",699,"CM per Industry Switch, REFRIGERATED - NON-MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L110C18","BNSF",4,"E2L110C18",700,"CM per Interchange Switch, REFRIGERATED - NON-MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L110C19","BNSF",4,"E2L110C19",701,"CM per Intraterminal Switch, REFRIGERATED - NON-MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L110C20","BNSF",4,"E2L110C20",702,"CM per Interterminal Switch, REFRIGERATED - NON-MECH",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L110C21","BNSF",4,"E2L110C21",703,"CM per I&I Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L110C22","BNSF",4,"E2L110C22",704,"Average CM per CD, Railroad-Owned, REFRIGERATED - NON-MECH",422.54248046875,460.86102294921898,462.57949829101602,518.47259521484398,480.34747314453102,441.79348754882801,489.76934814453102,435.22637939453102,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
[{"$f":"B706&\"-\"&D706","v":"BNSF-E2L110C23"},"BNSF",4,"E2L110C23",705,"Average Miles between I&I Switches, REFRIGERATED - NON-MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L110C24","BNSF",4,"E2L110C24",706,"Average Miles between Interchange Switches, REFRIGERATED - NON-MECH",1345.96887207031,1481.07214355469,1701.6572265625,1886.69543457031,3320.2578125,6484.208984375,7477.35498046875,9101.9423828125,11108.994140625,19079.826605723199,12436.004271359299,8782.5810787847604,16318.0043105487,23449.252517218301,20045.8312787086,13021.627116341901]
["BNSF-E2L110C25","BNSF",4,"E2L110C25",707,"SEMs per Industry Switch, REFRIGERATED - NON-MECH",4.0653171539306596,4.4621381759643599,4.4837818145751998,4.1883964538574201,4.1100530624389604,4.2478790283203098,4.2663950920104998,4.3016629219055202,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L110C26","BNSF",4,"E2L110C26",708,"SEMs per Interchange Switch, REFRIGERATED - NON-MECH",2.2359247207641602,2.4541757106781001,2.4660801887512198,2.3036181926727299,2.2605292797088601,2.3363337516784699,2.34651756286621,2.3659148216247599,2.3220627307891801,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L110C27","BNSF",4,"E2L110C27",709,"SEMs per Intraterminal Switch, REFRIGERATED - NON-MECH",6.0979757308959996,6.6932072639465297,6.7256727218627903,6.2825946807861301,6.16507911682129,6.3718185424804696,6.3995933532714799,6.4524941444396999,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L110C28","BNSF",4,"E2L110C28",710,"SEMs per Interterminal Switch, REFRIGERATED - NON-MECH",4.8783807754516602,5.3545656204223597,5.3805384635925302,5.0260763168334996,4.9320631027221697,5.0974555015564,5.1196742057800302,5.1619958877563503,5.0663189888000497,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L110C29","BNSF",4,"E2L110C29",711,"SEMs per I&I Switch, REFRIGERATED - NON-MECH",1.01632952690125,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619697570800799,1.0665988922119101,1.0754157304763801,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L111C1","BNSF",4,"E2L111C1",712,"Average Tare Weight, FLAT - TOFC",58.299999237060497,59.700000762939503,59.400001525878899,59.5,59.099998474121101,59.299999237060497,58.200000762939503,57.799999237060497,57.799999237060497,58.3,58.6,58.6,58.5,58.9,58.7,58.6]
["BNSF-E2L111C2","BNSF",4,"E2L111C2",713,"E/L Ratio, Railroad-Owned, FLAT - TOFC",1.18312203884125,1.11481893062592,1.10697817802429,1.1028020381927499,1.11939001083374,1.10613548755646,1.10506808757782,1.10299921035767,1.0967432260513299,1.1455837768028101,1.12787152122794,1.1355997936164599,1.1334516901990499,1.14161324688664,1.1371226159496399,1.1878105015523801]
["BNSF-E2L111C3","BNSF",4,"E2L111C3",714,"E/L Ratio, Privately-Owned, FLAT - TOFC",1.1663357019424401,1.1271157264709499,1.11635994911194,1.11025249958038,1.1094839572906501,1.1030508279800399,1.1070755720138501,1.09890401363373,1.0951341390609699,1.11347425800542,1.09090683871698,1.1019553550063199,1.10851388186691,1.11266718641719,1.10908083465475,1.1520468739382601]
["BNSF-E2L111C4","BNSF",4,"E2L111C4",715,"E/L Ratio, All Freight Cars, FLAT - TOFC",1.1712874174118,1.12243711948395,1.1125471591949501,1.1069089174270601,1.11327052116394,1.1042238473892201,1.10624504089355,1.1004725694656401,1.0956552028655999,1.1238129560902901,1.10399017718115,1.1128116413737099,1.11585456660024,1.1225848921547501,1.11889847598035,1.1618718795240801]
["BNSF-E2L111C5","BNSF",4,"E2L111C5",716,"Local circuity, FLAT - TOFC",1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.069,1.069,1.069,1.069,1.069,1.069,1.069]
["BNSF-E2L111C6","BNSF",4,"E2L111C6",717,"Interline circuity, FLAT - TOFC",1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.107,1.107,1.107,1.107,1.107,1.107,1.107]
["BNSF-E2L111C7","BNSF",4,"E2L111C7",718,"Average circuity, FLAT - TOFC",1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.085,1.085,1.085,1.085,1.085,1.085,1.085]
["BNSF-E2L111C8","BNSF",4,"E2L111C8",719,"Spotted-to-Pulled Ratio, FLAT - TOFC",1.1712874174118,1.12243711948395,1.1125471591949501,1.1069089174270601,1.11327052116394,1.1042238473892201,1.10624504089355,1.1004725694656401,1.0956552028655999,1.1238129560902901,1.10399017718115,1.1128116413737099,1.11585456660024,1.1225848921547501,1.11889847598035,1.1618718795240801]
["BNSF-E2L111C9","BNSF",4,"E2L111C9",720,"CD per Industry Switch, FLAT - TOFC",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L111C10","BNSF",4,"E2L111C10",721,"CD per Interchange Switch, FLAT - TOFC",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L111C11","BNSF",4,"E2L111C11",722,"CD per Intraterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L111C12","BNSF",4,"E2L111C12",723,"CD per Interterminal Switch, FLAT - TOFC",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L111C13","BNSF",4,"E2L111C13",724,"CD per I&I Switch, FLAT - TOFC",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L111C14","BNSF",4,"E2L111C14",725,"CD per Load & Unload Industry Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L111C15","BNSF",4,"E2L111C15",726,"CD per Load & Unload Intraterminal Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L111C16","BNSF",4,"E2L111C16",727,"CD per Load & Unload Interterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L111C17","BNSF",4,"E2L111C17",728,"CM per Industry Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L111C18","BNSF",4,"E2L111C18",729,"CM per Interchange Switch, FLAT - TOFC",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L111C19","BNSF",4,"E2L111C19",730,"CM per Intraterminal Switch, FLAT - TOFC",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L111C20","BNSF",4,"E2L111C20",731,"CM per Interterminal Switch, FLAT - TOFC",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L111C21","BNSF",4,"E2L111C21",732,"CM per I&I Switch, FLAT - TOFC",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L111C22","BNSF",4,"E2L111C22",733,"Average CM per CD, Railroad-Owned, FLAT - TOFC",422.54244995117199,460.861083984375,462.57949829101602,518.47253417968795,480.34753417968801,441.79345703125,489.76934814453102,435.22637939453102,370.20083618164102,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L111C23","BNSF",4,"E2L111C23",734,"Average Miles between I&I Switches, FLAT - TOFC",4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162]
["BNSF-E2L111C24","BNSF",4,"E2L111C24",735,"Average Miles between Interchange Switches, FLAT - TOFC",20022.115234375,41690.66796875,68356.609375,87842.8125,91060.2578125,111060.5859375,159710.546875,179351.21875,215933.46875,186099.02224162599,210219.69398129699,145797.862959672,121613.63246918299,25607.7681503694,26144.307998177701,23111.423754818301]
["BNSF-E2L111C25","BNSF",4,"E2L111C25",736,"SEMs per Industry Switch, FLAT - TOFC",4.0653171539306596,4.4621381759643599,4.4837818145751998,4.1883964538574201,4.1100530624389604,4.2478790283203098,4.2663950920104998,4.3016629219055202,4.2219314575195304,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L111C26","BNSF",4,"E2L111C26",737,"SEMs per Interchange Switch, FLAT - TOFC",2.2359247207641602,2.4541757106781001,2.4660799503326398,2.3036181926727299,2.2605290412902801,2.3363335132598899,2.34651780128479,2.3659145832061799,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L111C27","BNSF",4,"E2L111C27",738,"SEMs per Intraterminal Switch, FLAT - TOFC",6.0979757308959996,6.6932072639465297,6.7256731986999503,6.2825946807861301,6.16507863998413,6.3718185424804696,6.3995933532714799,6.4524941444396999,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L111C28","BNSF",4,"E2L111C28",739,"SEMs per Interterminal Switch, FLAT - TOFC",4.8783807754516602,5.3545660972595197,5.3805389404296902,5.0260763168334996,4.9320631027221697,5.0974555015564,5.1196742057800302,5.1619949340820304,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L111C29","BNSF",4,"E2L111C29",740,"SEMs per I&I Switch, FLAT - TOFC",1.01632940769196,1.11553466320038,1.1209454536437999,1.0470991134643599,1.0275131464004501,1.0619697570800799,1.0665988922119101,1.0754158496856701,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L112C1","BNSF",4,"E2L112C1",741,"Average Tare Weight, FLAT - MULTILEVEL",54.299999237060497,54.299999237060497,54.200000762939503,54.400001525878899,54.900001525878899,54.5,54,54,53.799999237060497,53.6,53.6,53.4,53.3,53.1,53.1,53.1]
["BNSF-E2L112C2","BNSF",4,"E2L112C2",742,"E/L Ratio, Railroad-Owned, FLAT - MULTILEVEL",1.26762163639069,1.2180769443512001,1.26669013500214,1.3024667501449601,1.24350142478943,1.2401249408721899,1.32628273963928,1.35322642326355,1.36216652393341,1.3491645530407199,1.3255249914101499,1.3356548013855101,1.26346264346647,1.29200195927507,1.3691720730108601,1.2896480108855199]
["BNSF-E2L112C3","BNSF",4,"E2L112C3",743,"E/L Ratio, Privately-Owned, FLAT - MULTILEVEL",1.24361371994019,1.22113120555878,1.21377825737,1.23304450511932,1.1832172870636,1.1943453550338701,1.2910956144332899,1.32672703266144,1.3365225791931199,1.3085451146042499,1.2974776850698999,1.2975621293777799,1.23733860256494,1.2458807852482501,1.2954232758734701,1.2453691318431599]
["BNSF-E2L112C4","BNSF",4,"E2L112C4",744,"E/L Ratio, All Freight Cars, FLAT - MULTILEVEL",1.24766385555267,1.22058618068695,1.2240080833435101,1.2476561069488501,1.1943205595016499,1.2028605937957799,1.2976312637329099,1.3321400880813601,1.3411329984664899,1.3147070658415301,1.30120449570974,1.3026119749305101,1.24141202741167,1.2537478038347001,1.30754945364705,1.2521243673332301]
["BNSF-E2L112C5","BNSF",4,"E2L112C5",745,"Local circuity, FLAT - MULTILEVEL",1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999]
["BNSF-E2L112C6","BNSF",4,"E2L112C6",746,"Interline circuity, FLAT - MULTILEVEL",1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999]
["BNSF-E2L112C7","BNSF",4,"E2L112C7",747,"Average circuity, FLAT - MULTILEVEL",1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999]
["BNSF-E2L112C8","BNSF",4,"E2L112C8",748,"Spotted-to-Pulled Ratio, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L112C9","BNSF",4,"E2L112C9",749,"CD per Industry Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L112C10","BNSF",4,"E2L112C10",750,"CD per Interchange Switch, FLAT - MULTILEVEL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L112C11","BNSF",4,"E2L112C11",751,"CD per Intraterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L112C12","BNSF",4,"E2L112C12",752,"CD per Interterminal Switch, FLAT - MULTILEVEL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L112C13","BNSF",4,"E2L112C13",753,"CD per I&I Switch, FLAT - MULTILEVEL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L112C14","BNSF",4,"E2L112C14",754,"CD per Load & Unload Industry Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L112C15","BNSF",4,"E2L112C15",755,"CD per Load & Unload Intraterminal Switch, FLAT - MULTILEVEL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L112C16","BNSF",4,"E2L112C16",756,"CD per Load & Unload Interterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L112C17","BNSF",4,"E2L112C17",757,"CM per Industry Switch, FLAT - MULTILEVEL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L112C18","BNSF",4,"E2L112C18",758,"CM per Interchange Switch, FLAT - MULTILEVEL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L112C19","BNSF",4,"E2L112C19",759,"CM per Intraterminal Switch, FLAT - MULTILEVEL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L112C20","BNSF",4,"E2L112C20",760,"CM per Interterminal Switch, FLAT - MULTILEVEL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L112C21","BNSF",4,"E2L112C21",761,"CM per I&I Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L112C22","BNSF",4,"E2L112C22",762,"Average CM per CD, Railroad-Owned, FLAT - MULTILEVEL",422.54244995117199,460.861083984375,462.57952880859398,518.47253417968795,480.34750366210898,441.79345703125,489.76934814453102,435.22640991210898,370.20083618164102,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L112C23","BNSF",4,"E2L112C23",763,"Average Miles between I&I Switches, FLAT - MULTILEVEL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L112C24","BNSF",4,"E2L112C24",764,"Average Miles between Interchange Switches, FLAT - MULTILEVEL",3280.2880859375,3129.47802734375,3754.31030273438,4049.24389648438,3989.58642578125,6361.35400390625,12468.224609375,13651.2685546875,14205.36328125,10469.9768549297,5169.5991777221498,6180.6690210609204,9472.9097241947802,4673.6021007842301,6695.7833064817096,7778.3734102013595]
["BNSF-E2L112C25","BNSF",4,"E2L112C25",765,"SEMs per Industry Switch, FLAT - MULTILEVEL",4.0653176307678196,4.4621386528015101,4.48378229141235,4.1883969306945801,4.1100530624389604,4.2478790283203098,4.2663950920104998,4.3016624450683603,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L112C26","BNSF",4,"E2L112C26",766,"SEMs per Interchange Switch, FLAT - MULTILEVEL",2.2359247207641602,2.4541757106781001,2.4660799503326398,2.3036181926727299,2.2605288028717001,2.3363332748413099,2.34651780128479,2.3659145832061799,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L112C27","BNSF",4,"E2L112C27",767,"SEMs per Intraterminal Switch, FLAT - MULTILEVEL",6.0979762077331499,6.6932063102722203,6.7256731986999503,6.2825942039489702,6.16507863998413,6.3718180656433097,6.3995933532714799,6.4524946212768599,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L112C28","BNSF",4,"E2L112C28",768,"SEMs per Interterminal Switch, FLAT - MULTILEVEL",4.8783802986145002,5.3545665740966797,5.3805384635925302,5.0260763168334996,4.9320631027221697,5.0974555015564,5.1196746826171902,5.1619954109191903,5.0663194656372097,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
[{"$f":"B770&\"-\"&D770","v":"BNSF-E2L112C29"},"BNSF",4,"E2L112C29",769,"SEMs per I&I Switch, FLAT - MULTILEVEL",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619697570800799,1.0665988922119101,1.0754157304763801,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L113C1","BNSF",4,"E2L113C1",770,"Average Tare Weight, FLAT - GENERAL",33.599998474121101,34.099998474121101,34,32.900001525878899,32.200000762939503,33,32.200000762939503,32.799999237060497,32.799999237060497,32.5,32.4,32.200000000000003,32.1,32.200000000000003,32.299999999999997,32.299999999999997]
["BNSF-E2L113C2","BNSF",4,"E2L113C2",771,"E/L Ratio, Railroad-Owned, FLAT - GENERAL",3.13636374473572,2.9423077106475799,2.6688001155853298,4.9466667175293004,3.3165266513824498,4.4370369911193803,3.9258065223693799,3.2611277103424099,3.44274806976318,3.6287128712871302,3.4530612244898,3.5704697986577201,2.78974358974359,2.9682539682539701,2.9457831325301198,2.99470899470899]
["BNSF-E2L113C3","BNSF",4,"E2L113C3",772,"E/L Ratio, Privately-Owned, FLAT - GENERAL",2.8062500953674299,2.3194444179534899,2.7117903232574498,2.8984017372131299,1.9634146690368699,2.1126761436462398,2.8217821121215798,2.49259257316589,2.2511012554168701,2.7896551724137901,2.0754716981132102,2.6449438202247202,2.4189189189189202,2.7925925925925901,2.1614035087719299,1.9418604651162801]
["BNSF-E2L113C4","BNSF",4,"E2L113C4",773,"E/L Ratio, All Freight Cars, FLAT - GENERAL",3.0483334064483598,2.80722880363464,2.6803278923034699,4.9204545021057102,3.3314917087554901,4.4714283943176296,3.65450119972229,2.9192750453949001,2.6871509552002002,3.1341463414634099,3.4015503875969002,2.8771043771043798,2.5320813771517998,2.86492374727669,2.4501108647450098,2.66545454545455]
["BNSF-E2L113C5","BNSF",4,"E2L113C5",774,"Local circuity, FLAT - GENERAL",1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001]
["BNSF-E2L113C6","BNSF",4,"E2L113C6",775,"Interline circuity, FLAT - GENERAL",1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.177,1.177,1.177,1.177,1.177,1.177,1.177]
["BNSF-E2L113C7","BNSF",4,"E2L113C7",776,"Average circuity, FLAT - GENERAL",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["BNSF-E2L113C8","BNSF",4,"E2L113C8",777,"Spotted-to-Pulled Ratio, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L113C9","BNSF",4,"E2L113C9",778,"CD per Industry Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L113C10","BNSF",4,"E2L113C10",779,"CD per Interchange Switch, FLAT - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L113C11","BNSF",4,"E2L113C11",780,"CD per Intraterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L113C12","BNSF",4,"E2L113C12",781,"CD per Interterminal Switch, FLAT - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L113C13","BNSF",4,"E2L113C13",782,"CD per I&I Switch, FLAT - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L113C14","BNSF",4,"E2L113C14",783,"CD per Load & Unload Industry Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L113C15","BNSF",4,"E2L113C15",784,"CD per Load & Unload Intraterminal Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L113C16","BNSF",4,"E2L113C16",785,"CD per Load & Unload Interterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L113C17","BNSF",4,"E2L113C17",786,"CM per Industry Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L113C18","BNSF",4,"E2L113C18",787,"CM per Interchange Switch, FLAT - GENERAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L113C19","BNSF",4,"E2L113C19",788,"CM per Intraterminal Switch, FLAT - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L113C20","BNSF",4,"E2L113C20",789,"CM per Interterminal Switch, FLAT - GENERAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L113C21","BNSF",4,"E2L113C21",790,"CM per I&I Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L113C22","BNSF",4,"E2L113C22",791,"Average CM per CD, Railroad-Owned, FLAT - GENERAL",422.54248046875,460.86105346679699,462.57952880859398,518.47259521484398,480.34750366210898,441.79345703125,489.76937866210898,435.22634887695301,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L113C23","BNSF",4,"E2L113C23",792,"Average Miles between I&I Switches, FLAT - GENERAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L113C24","BNSF",4,"E2L113C24",793,"Average Miles between Interchange Switches, FLAT - GENERAL",705.72644042968795,1081.91174316406,1945.65173339844,273.57513427734398,238.31468200683599,226.17127990722699,223.61262512207,363.46697998046898,768.11639404296898,1973.1593038822,816.13067491872005,517.96302755493502,1118.9161881761499,497.04553136619103,1980.0615212528,639.11579139870196]
["BNSF-E2L113C25","BNSF",4,"E2L113C25",794,"SEMs per Industry Switch, FLAT - GENERAL",4.0653176307678196,4.4621386528015101,4.4837818145751998,4.1883964538574201,4.1100530624389604,4.2478790283203098,4.2663955688476598,4.3016629219055202,4.2219314575195304,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L113C26","BNSF",4,"E2L113C26",795,"SEMs per Interchange Switch, FLAT - GENERAL",2.2359247207641602,2.4541757106781001,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363332748413099,2.34651756286621,2.3659148216247599,2.3220627307891801,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L113C27","BNSF",4,"E2L113C27",796,"SEMs per Intraterminal Switch, FLAT - GENERAL",6.0979762077331499,6.6932072639465297,6.7256731986999503,6.2825951576232901,6.16507863998413,6.3718180656433097,6.3995943069457999,6.45249366760254,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L113C28","BNSF",4,"E2L113C28",797,"SEMs per Interterminal Switch, FLAT - GENERAL",4.8783807754516602,5.3545660972595197,5.3805384635925302,5.0260763168334996,4.9320631027221697,5.0974550247192401,5.1196742057800302,5.1619949340820304,5.0663189888000497,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L113C29","BNSF",4,"E2L113C29",798,"SEMs per I&I Switch, FLAT - GENERAL",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619697570800799,1.0665990114212001,1.0754158496856701,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L114C1","BNSF",4,"E2L114C1",799,"Average Tare Weight, FLAT - OTHER",34.599998474121101,34.599998474121101,34.700000762939503,34.700000762939503,34.700000762939503,34.700000762939503,35.099998474121101,35.200000762939503,35.200000762939503,35.299999999999997,35.299999999999997,35.299999999999997,35.4,35.299999999999997,35.4,35.4]
["BNSF-E2L114C2","BNSF",4,"E2L114C2",800,"E/L Ratio, Railroad-Owned, FLAT - OTHER",1.97129142284393,1.99087357521057,2.03214406967163,2.0166673660278298,1.9875115156173699,1.9518115520477299,1.96585953235626,1.93677818775177,1.97621369361877,1.9418576154883,1.91956616255978,1.93057625434675,1.9088932086016299,1.9338442044288899,1.97667089537291,1.9675501580113599]
["BNSF-E2L114C3","BNSF",4,"E2L114C3",801,"E/L Ratio, Privately-Owned, FLAT - OTHER",1.87571454048157,1.93245565891266,2.04100561141968,1.92019271850586,1.98608994483948,1.95481264591217,2.01166963577271,1.9773687124252299,1.9047662019729601,2.0015318535427902,1.9741281193198199,1.87706427845528,1.8768275687317899,1.93338018644,1.99972734956512,1.93840801594851]
["BNSF-E2L114C4","BNSF",4,"E2L114C4",802,"E/L Ratio, All Freight Cars, FLAT - OTHER",1.9304225444793699,1.9661103487014799,2.03593969345093,1.9855430126190201,1.98697149753571,1.9531881809234599,1.9878133535385101,1.95549309253693,1.94059693813324,1.9686698696321101,1.9418759724383201,1.9070914868707101,1.89319647730092,1.93362311881626,1.98808005990326,1.9535133303208301]
["BNSF-E2L114C5","BNSF",4,"E2L114C5",803,"Local circuity, FLAT - OTHER",1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001]
["BNSF-E2L114C6","BNSF",4,"E2L114C6",804,"Interline circuity, FLAT - OTHER",1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.17,1.17,1.17,1.17,1.17,1.17,1.17]
["BNSF-E2L114C7","BNSF",4,"E2L114C7",805,"Average circuity, FLAT - OTHER",1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.155,1.155,1.155,1.155,1.155,1.155,1.155]
["BNSF-E2L114C8","BNSF",4,"E2L114C8",806,"Spotted-to-Pulled Ratio, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L114C9","BNSF",4,"E2L114C9",807,"CD per Industry Switch, FLAT - OTHER",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L114C10","BNSF",4,"E2L114C10",808,"CD per Interchange Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L114C11","BNSF",4,"E2L114C11",809,"CD per Intraterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L114C12","BNSF",4,"E2L114C12",810,"CD per Interterminal Switch, FLAT - OTHER",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L114C13","BNSF",4,"E2L114C13",811,"CD per I&I Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L114C14","BNSF",4,"E2L114C14",812,"CD per Load & Unload Industry Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L114C15","BNSF",4,"E2L114C15",813,"CD per Load & Unload Intraterminal Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L114C16","BNSF",4,"E2L114C16",814,"CD per Load & Unload Interterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L114C17","BNSF",4,"E2L114C17",815,"CM per Industry Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L114C18","BNSF",4,"E2L114C18",816,"CM per Interchange Switch, FLAT - OTHER",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L114C19","BNSF",4,"E2L114C19",817,"CM per Intraterminal Switch, FLAT - OTHER",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L114C20","BNSF",4,"E2L114C20",818,"CM per Interterminal Switch, FLAT - OTHER",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L114C21","BNSF",4,"E2L114C21",819,"CM per I&I Switch, FLAT - OTHER",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L114C22","BNSF",4,"E2L114C22",820,"Average CM per CD, Railroad-Owned, FLAT - OTHER",422.54248046875,460.86105346679699,462.57955932617199,518.47259521484398,480.34753417968801,441.79345703125,489.76931762695301,435.22637939453102,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058699,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L114C23","BNSF",4,"E2L114C23",821,"Average Miles between I&I Switches, FLAT - OTHER",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L114C24","BNSF",4,"E2L114C24",822,"Average Miles between Interchange Switches, FLAT - OTHER",2101.880859375,1773.47497558594,1710.66772460938,1757.17565917969,1881.48889160156,1612.64880371094,1585.11999511719,1735.84411621094,1590.88208007813,1601.46075196577,2229.7306207500301,1958.02878710645,1846.78117436602,2136.7424390656602,2460.04281827674,2612.9776355354702]
["BNSF-E2L114C25","BNSF",4,"E2L114C25",823,"SEMs per Industry Switch, FLAT - OTHER",4.0653176307678196,4.4621381759643599,4.4837818145751998,4.1883964538574201,4.1100525856018102,4.2478790283203098,4.2663955688476598,4.3016624450683603,4.2219314575195304,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L114C26","BNSF",4,"E2L114C26",824,"SEMs per Interchange Switch, FLAT - OTHER",2.2359247207641602,2.4541759490966801,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363332748413099,2.34651780128479,2.3659148216247599,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L114C27","BNSF",4,"E2L114C27",825,"SEMs per Intraterminal Switch, FLAT - OTHER",6.0979757308959996,6.6932072639465297,6.7256727218627903,6.2825946807861301,6.16507816314697,6.3718185424804696,6.3995933532714799,6.4524941444396999,6.3328971862793004,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611296,6.7543362751477396,6.3097340048834498]
["BNSF-E2L114C28","BNSF",4,"E2L114C28",826,"SEMs per Interterminal Switch, FLAT - OTHER",4.8783802986145002,5.3545656204223597,5.3805389404296902,5.0260763168334996,4.9320631027221697,5.0974550247192401,5.1196746826171902,5.1619954109191903,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L114C29","BNSF",4,"E2L114C29",827,"SEMs per I&I Switch, FLAT - OTHER",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275132656097401,1.0619698762893699,1.0665990114212001,1.0754158496856701,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L115C1","BNSF",4,"E2L115C1",828,"Average Tare Weight, TANK <22,000 GAL",32.700000000000003,32.700000000000003,32.6,32.6,32.6,32.6,32.6,32.6,32.6,32.700000000000003,32.700000000000003,32.799999999999997,32.799999999999997,32.9,32.9,32.9]
["BNSF-E2L115C2","BNSF",4,"E2L115C2",829,"E/L Ratio, Railroad-Owned, TANK <22,000 GAL",7.6677145957946804,8.5768146514892596,12.0664205551147,2.05408883094788,1.94023633003235,2.20015597343445,2.2964425086975102,2.40827536582947,2.4854698181152299,3.9055374592833898,4.3346153846153799,2.3689655172413802,2.6660617059891099,1.8991304347826099,1.88264462809917,2.2513761467889899]
["BNSF-E2L115C3","BNSF",4,"E2L115C3",830,"E/L Ratio, Privately-Owned, TANK <22,000 GAL",2.0103130340576199,2.0219135284423801,2.06432104110718,2.0590574741363499,2.0390863418579102,2.0359861850738499,2.0335431098938002,2.05839991569519,2.0376422405242902,2.05323225361819,2.0587400099534499,2.0521307643216198,2.0455244774629899,2.0413558852072602,2.0563657407407399,2.0279305036287698]
["BNSF-E2L115C4","BNSF",4,"E2L115C4",831,"E/L Ratio, All Freight Cars, TANK <22,000 GAL",2.0103130340576199,2.0219135284423801,2.06432104110718,2.0590574741363499,2.0390863418579102,2.0359861850738499,2.0335431098938002,2.05839991569519,2.0376422405242902,2.05323225361819,2.0587400099534499,2.0521307643216198,2.0455244774629899,2.0413558852072602,2.0563657407407399,2.0279305036287698]
["BNSF-E2L115C5","BNSF",4,"E2L115C5",832,"Local circuity, TANK <22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
[{"$f":"B834&\"-\"&D834","v":"BNSF-E2L115C6"},"BNSF",4,"E2L115C6",833,"Interline circuity, TANK <22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["BNSF-E2L115C7","BNSF",4,"E2L115C7",834,"Average circuity, TANK <22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["BNSF-E2L115C8","BNSF",4,"E2L115C8",835,"Spotted-to-Pulled Ratio, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L115C9","BNSF",4,"E2L115C9",836,"CD per Industry Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L115C10","BNSF",4,"E2L115C10",837,"CD per Interchange Switch, TANK <22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L115C11","BNSF",4,"E2L115C11",838,"CD per Intraterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L115C12","BNSF",4,"E2L115C12",839,"CD per Interterminal Switch, TANK <22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L115C13","BNSF",4,"E2L115C13",840,"CD per I&I Switch, TANK <22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L115C14","BNSF",4,"E2L115C14",841,"CD per Load & Unload Industry Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L115C15","BNSF",4,"E2L115C15",842,"CD per Load & Unload Intraterminal Switch, TANK <22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L115C16","BNSF",4,"E2L115C16",843,"CD per Load & Unload Interterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L115C17","BNSF",4,"E2L115C17",844,"CM per Industry Switch, TANK <22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L115C18","BNSF",4,"E2L115C18",845,"CM per Interchange Switch, TANK <22,000 GAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L115C19","BNSF",4,"E2L115C19",846,"CM per Intraterminal Switch, TANK <22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L115C20","BNSF",4,"E2L115C20",847,"CM per Interterminal Switch, TANK <22,000 GAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L115C21","BNSF",4,"E2L115C21",848,"CM per I&I Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L115C22","BNSF",4,"E2L115C22",849,"Average CM per CD, Railroad-Owned, TANK <22,000 GAL",422.54244995117199,460.86105346679699,462.57952880859398,518.47253417968795,480.34747314453102,441.79342651367199,489.76937866210898,435.22634887695301,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L115C23","BNSF",4,"E2L115C23",850,"Average Miles between I&I Switches, TANK <22,000 GAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L115C24","BNSF",4,"E2L115C24",851,"Average Miles between Interchange Switches, TANK <22,000 GAL",836.135498046875,995.706787109375,1314.88891601563,1623.20654296875,1451.93188476563,1301.28186035156,1072.986328125,983.08929443359398,947.80401611328102,1936.0784581789001,891.956248970621,934.15006146661199,1161.8770463159599,2338.0157970699402,2758.8550923177299,3677.2490209429502]
["BNSF-E2L115C25","BNSF",4,"E2L115C25",852,"SEMs per Industry Switch, TANK <22,000 GAL",4.0653176307678196,4.4621386528015101,4.48378229141235,4.1883969306945801,4.1100525856018102,4.2478790283203098,4.2663950920104998,4.3016629219055202,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L115C26","BNSF",4,"E2L115C26",853,"SEMs per Interchange Switch, TANK <22,000 GAL",2.2359244823455802,2.4541759490966801,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363335132598899,2.34651756286621,2.3659148216247599,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L115C27","BNSF",4,"E2L115C27",854,"SEMs per Intraterminal Switch, TANK <22,000 GAL",6.0979762077331499,6.6932072639465297,6.7256731986999503,6.2825946807861301,6.16507816314697,6.3718190193176296,6.3995928764343297,6.4524946212768599,6.3328971862793004,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L115C28","BNSF",4,"E2L115C28",855,"SEMs per Interterminal Switch, TANK <22,000 GAL",4.8783812522888201,5.3545660972595197,5.3805389404296902,5.0260763168334996,4.9320635795593297,5.0974550247192401,5.1196742057800302,5.1619954109191903,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L115C29","BNSF",4,"E2L115C29",856,"SEMs per I&I Switch, TANK <22,000 GAL",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619697570800799,1.0665988922119101,1.0754157304763801,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L116C1","BNSF",4,"E2L116C1",857,"Average Tare Weight, TANK >=22,000 GAL",39.799999999999997,39.200000000000003,38.9,38.9,39,38.9,38.9,39.1,39.5,40.1,40.4,40.700000000000003,41,41.4,41.7,41.9]
["BNSF-E2L116C2","BNSF",4,"E2L116C2",858,"E/L Ratio, Railroad-Owned, TANK >=22,000 GAL",7.6677145957946804,8.5768146514892596,12.0664205551147,2.05408883094788,1.94023633003235,2.20015597343445,2.2964425086975102,2.40827536582947,2.4854698181152299,3.9055374592833898,4.3346153846153799,2.3689655172413802,2.6660617059891099,1.8991304347826099,1.88264462809917,2.2513761467889899]
["BNSF-E2L116C3","BNSF",4,"E2L116C3",859,"E/L Ratio, Privately-Owned, TANK >=22,000 GAL",2.0493810176849401,2.0886530876159699,2.11864185333252,2.1199545860290501,2.07545018196106,2.0724074840545699,2.0626525878906299,2.0723288059234601,2.0567653179168701,2.0726609174707402,2.0584698620258002,2.0674275196865501,2.0478700368481202,2.0601389212004402,2.0717056311031299,2.0400692657417401]
["BNSF-E2L116C4","BNSF",4,"E2L116C4",860,"E/L Ratio, All Freight Cars, TANK >=22,000 GAL",2.0493810176849401,2.0886530876159699,2.11864185333252,2.1199545860290501,2.07545018196106,2.0724074840545699,2.0626525878906299,2.0723288059234601,2.0567653179168701,2.0726609174707402,2.0584698620258002,2.0674275196865501,2.0478700368481202,2.0601389212004402,2.0717056311031299,2.0400692657417401]
["BNSF-E2L116C5","BNSF",4,"E2L116C5",861,"Local circuity, TANK >=22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["BNSF-E2L116C6","BNSF",4,"E2L116C6",862,"Interline circuity, TANK >=22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["BNSF-E2L116C7","BNSF",4,"E2L116C7",863,"Average circuity, TANK >=22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["BNSF-E2L116C8","BNSF",4,"E2L116C8",864,"Spotted-to-Pulled Ratio, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L116C9","BNSF",4,"E2L116C9",865,"CD per Industry Switch, TANK >=22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L116C10","BNSF",4,"E2L116C10",866,"CD per Interchange Switch, TANK >=22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L116C11","BNSF",4,"E2L116C11",867,"CD per Intraterminal Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L116C12","BNSF",4,"E2L116C12",868,"CD per Interterminal Switch, TANK >=22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L116C13","BNSF",4,"E2L116C13",869,"CD per I&I Switch, TANK >=22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L116C14","BNSF",4,"E2L116C14",870,"CD per Load & Unload Industry Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L116C15","BNSF",4,"E2L116C15",871,"CD per Load & Unload Intraterminal Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L116C16","BNSF",4,"E2L116C16",872,"CD per Load & Unload Interterminal Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L116C17","BNSF",4,"E2L116C17",873,"CM per Industry Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L116C18","BNSF",4,"E2L116C18",874,"CM per Interchange Switch, TANK >=22,000 GAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L116C19","BNSF",4,"E2L116C19",875,"CM per Intraterminal Switch, TANK >=22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L116C20","BNSF",4,"E2L116C20",876,"CM per Interterminal Switch, TANK >=22,000 GAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L116C21","BNSF",4,"E2L116C21",877,"CM per I&I Switch, TANK >=22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L116C22","BNSF",4,"E2L116C22",878,"Average CM per CD, Railroad-Owned, TANK >=22,000 GAL",422.54244995117199,460.86105346679699,462.57952880859398,518.47253417968795,480.34747314453102,441.79342651367199,489.76937866210898,435.22634887695301,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L116C23","BNSF",4,"E2L116C23",879,"Average Miles between I&I Switches, TANK >=22,000 GAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L116C24","BNSF",4,"E2L116C24",880,"Average Miles between Interchange Switches, TANK >=22,000 GAL",836.135498046875,995.706787109375,1314.88891601563,1623.20654296875,1451.93188476563,1301.28186035156,1072.986328125,983.08929443359398,947.80401611328102,1936.0784581789001,891.956248970621,934.15006146661199,1161.8770463159599,2338.0157970699402,2758.8550923177299,3677.2490209429502]
["BNSF-E2L116C25","BNSF",4,"E2L116C25",881,"SEMs per Industry Switch, TANK >=22,000 GAL",4.0653176307678196,4.4621386528015101,4.48378229141235,4.1883969306945801,4.1100525856018102,4.2478790283203098,4.2663950920104998,4.3016629219055202,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L116C26","BNSF",4,"E2L116C26",882,"SEMs per Interchange Switch, TANK >=22,000 GAL",2.2359244823455802,2.4541759490966801,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363335132598899,2.34651756286621,2.3659148216247599,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L116C27","BNSF",4,"E2L116C27",883,"SEMs per Intraterminal Switch, TANK >=22,000 GAL",6.0979762077331499,6.6932072639465297,6.7256731986999503,6.2825946807861301,6.16507816314697,6.3718190193176296,6.3995928764343297,6.4524946212768599,6.3328971862793004,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L116C28","BNSF",4,"E2L116C28",884,"SEMs per Interterminal Switch, TANK >=22,000 GAL",4.8783812522888201,5.3545660972595197,5.3805389404296902,5.0260763168334996,4.9320635795593297,5.0974550247192401,5.1196742057800302,5.1619954109191903,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L116C29","BNSF",4,"E2L116C29",885,"SEMs per I&I Switch, TANK >=22,000 GAL",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619697570800799,1.0665988922119101,1.0754157304763801,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L117C1","BNSF",4,"E2L117C1",886,"Average Tare Weight, ALL OTHER FREIGHT CARS",36.799999237060497,39.200000762939503,36.5,36.599998474121101,36.700000762939503,36.599998474121101,36.799999237060497,37.099998474121101,37.5,38.1,38.4,38.6,38.9,39.299999999999997,39.6,39.799999999999997]
["BNSF-E2L117C2","BNSF",4,"E2L117C2",887,"E/L Ratio, Railroad-Owned, ALL OTHER FREIGHT CARS",7.6677145957946804,8.5768146514892596,12.0664205551147,2.05408883094788,1.94023633003235,2.20015597343445,2.2964425086975102,2.40827536582947,2.4854698181152299,3.9055374592833898,4.3346153846153799,2.3689655172413802,2.6660617059891099,1.8991304347826099,1.88264462809917,2.2513761467889899]
["BNSF-E2L117C3","BNSF",4,"E2L117C3",888,"E/L Ratio, Privately-Owned, ALL OTHER FREIGHT CARS",1.4850879907607999,1.5072757005691499,1.44416391849518,1.7160508632659901,1.80008220672607,2.8486747741699201,1.24125993251801,1.4703516960144001,1.5498248338699301,1.2962017482788,2.1969273743016799,1.8595166163142001,2.15465729349736,2.06859756097561,2.18877551020408,2.2648401826483999]
["BNSF-E2L117C4","BNSF",4,"E2L117C4",889,"E/L Ratio, All Freight Cars, ALL OTHER FREIGHT CAR",2.0401148796081499,2.0631287097930899,2.0887937545776398,2.0874872207641602,2.0547397136688201,2.0754990577697798,2.0702602863311799,2.08208203315735,2.06812596321106,2.0592873336147202,2.05941862738708,2.0644937790524298,2.0479465970458999,2.0570236021191599,2.0688764771429802,2.03812292848303]
["BNSF-E2L117C5","BNSF",4,"E2L117C5",890,"Local circuity, ALL OTHER FREIGHT CARS",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["BNSF-E2L117C6","BNSF",4,"E2L117C6",891,"Interline circuity, ALL OTHER FREIGHT CARS",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["BNSF-E2L117C7","BNSF",4,"E2L117C7",892,"Average circuity, ALL OTHER FREIGHT CARS",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["BNSF-E2L117C8","BNSF",4,"E2L117C8",893,"Spotted-to-Pulled Ratio, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L117C9","BNSF",4,"E2L117C9",894,"CD per Industry Switch, ALL OTHER FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L117C10","BNSF",4,"E2L117C10",895,"CD per Interchange Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L117C11","BNSF",4,"E2L117C11",896,"CD per Intraterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
[{"$f":"B898&\"-\"&D898","v":"BNSF-E2L117C12"},"BNSF",4,"E2L117C12",897,"CD per Interterminal Switch, ALL OTHER FREIGHT CARS",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L117C13","BNSF",4,"E2L117C13",898,"CD per I&I Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L117C14","BNSF",4,"E2L117C14",899,"CD per Load & Unload Industry Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L117C15","BNSF",4,"E2L117C15",900,"CD per Load & Unload Intraterminal Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L117C16","BNSF",4,"E2L117C16",901,"CD per Load & Unload Interterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L117C17","BNSF",4,"E2L117C17",902,"CM per Industry Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L117C18","BNSF",4,"E2L117C18",903,"CM per Interchange Switch, ALL OTHER FREIGHT CARS",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L117C19","BNSF",4,"E2L117C19",904,"CM per Intraterminal Switch, ALL OTHER FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L117C20","BNSF",4,"E2L117C20",905,"CM per Interterminal Switch, ALL OTHER FREIGHT CARS",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L117C21","BNSF",4,"E2L117C21",906,"CM per I&I Switch, ALL OTHER FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L117C22","BNSF",4,"E2L117C22",907,"Average CM per CD, Railroad-Owned, ALL OTHER FREIGHT CARS",422.54244995117199,460.86105346679699,462.57952880859398,518.47253417968795,480.34747314453102,441.79342651367199,489.76937866210898,435.22634887695301,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058602,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L117C23","BNSF",4,"E2L117C23",908,"Average Miles between I&I Switches, ALL OTHER FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L117C24","BNSF",4,"E2L117C24",909,"Average Miles between Interchange Switches, ALL OTHER FREIGHT CARS",836.135498046875,995.706787109375,1314.88891601563,1623.20654296875,1451.93188476563,1301.28186035156,1072.986328125,983.08929443359398,947.80401611328102,1936.0784581789001,891.956248970621,934.15006146661199,1161.8770463159599,2338.0157970699402,2758.8550923177299,3677.2490209429502]
["BNSF-E2L117C25","BNSF",4,"E2L117C25",910,"SEMs per Industry Switch, ALL OTHER FREIGHT CARS",4.0653176307678196,4.4621386528015101,4.48378229141235,4.1883969306945801,4.1100525856018102,4.2478790283203098,4.2663950920104998,4.3016629219055202,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L117C26","BNSF",4,"E2L117C26",911,"SEMs per Interchange Switch, ALL OTHER FREIGHT CARS",2.2359244823455802,2.4541759490966801,2.4660801887512198,2.3036181926727299,2.2605290412902801,2.3363335132598899,2.34651756286621,2.3659148216247599,2.3220624923706099,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L117C27","BNSF",4,"E2L117C27",912,"SEMs per Intraterminal Switch, ALL OTHER FREIGHT CARS",6.0979762077331499,6.6932072639465297,6.7256731986999503,6.2825946807861301,6.16507816314697,6.3718190193176296,6.3995928764343297,6.4524946212768599,6.3328971862793004,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611403,6.7543362751477396,6.3097340048834498]
["BNSF-E2L117C28","BNSF",4,"E2L117C28",913,"SEMs per Interterminal Switch, ALL OTHER FREIGHT CARS",4.8783812522888201,5.3545660972595197,5.3805389404296902,5.0260763168334996,4.9320635795593297,5.0974550247192401,5.1196742057800302,5.1619954109191903,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L117C29","BNSF",4,"E2L117C29",914,"SEMs per I&I Switch, ALL OTHER FREIGHT CARS",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619697570800799,1.0665988922119101,1.0754157304763801,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L118C1","BNSF",4,"E2L118C1",915,"Average Tare Weight, AVERAGE ALL FREIGHT CARS",34.400001525878899,34.400001525878899,34.299999237060497,34.299999237060497,34.299999237060497,34.299999237060497,34.200000762939503,34.299999237060497,34.400001525878899,34.6,34.799999999999997,34.799999999999997,34.9,35.200000000000003,35.299999999999997,35.4]
["BNSF-E2L118C2","BNSF",4,"E2L118C2",916,"E/L Ratio, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.77822053432465,1.7516466379165601,1.74870049953461,1.73591673374176,1.75037825107574,1.7234539985656701,1.70011651515961,1.6918530464172401,1.7079203128814699,1.74438071890359,1.7022913002246001,1.7260650754245399,1.73959866069589,1.71523944161897,1.69389099602349,1.7266715380354001]
["BNSF-E2L118C3","BNSF",4,"E2L118C3",917,"E/L Ratio, Privately-Owned, AVERAGE ALL FREIGHT CARS",1.7419365644455,1.77307713031769,1.8056169748306301,1.83560347557068,1.7956610918045,1.78504598140717,1.7901353836059599,1.78259205818176,1.76978087425232,1.7673269512185199,1.72695735126946,1.720358423969,1.71425369406156,1.7438863698314699,1.71324322957603,1.7001680093051299]
["BNSF-E2L118C4","BNSF",4,"E2L118C4",918,"E/L Ratio, All Freight Cars, AVERAGE ALL FREIGHT CARS",1.7545484304428101,1.7652384042739899,1.7843940258026101,1.7993096113205,1.7793266773223899,1.7632521390914899,1.75896108150482,1.7539165019989,1.75146043300629,1.7604436937951999,1.7187731179222701,1.72217537536058,1.7223641226252,1.7347993276560001,1.7065748655344,1.70856902159025]
["BNSF-E2L118C5","BNSF",4,"E2L118C5",919,"Local circuity, AVERAGE ALL FREIGHT CARS",1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.097,1.097,1.097,1.097,1.097,1.097,1.097]
["BNSF-E2L118C6","BNSF",4,"E2L118C6",920,"Interline circuity, AVERAGE ALL FREIGHT CARS",1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.157,1.157,1.157,1.157,1.157,1.157,1.157]
["BNSF-E2L118C7","BNSF",4,"E2L118C7",921,"Average circuity, AVERAGE ALL FREIGHT CARS",1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.135,1.135,1.135,1.135,1.135,1.135,1.135]
["BNSF-E2L118C8","BNSF",4,"E2L118C8",922,"Spotted-to-Pulled Ratio, AVERAGE ALL FREIGHT CARS",1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.9,1.9,1.9,1.9,1.9,1.9,1.9]
["BNSF-E2L118C9","BNSF",4,"E2L118C9",923,"CD per Industry Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L118C10","BNSF",4,"E2L118C10",924,"CD per Interchange Switch, AVERAGE ALL FREIGHT CAR",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L118C11","BNSF",4,"E2L118C11",925,"CD per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L118C12","BNSF",4,"E2L118C12",926,"CD per Interterminal Switch, AVERAGE ALL FREIGHT CARS",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["BNSF-E2L118C13","BNSF",4,"E2L118C13",927,"CD per I&I Switch, AVERAGE ALL FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["BNSF-E2L118C14","BNSF",4,"E2L118C14",928,"CD per Load & Unload Industry Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L118C15","BNSF",4,"E2L118C15",929,"CD per Load & Unload Intraterminal Switch, AVERAGE ALL FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L118C16","BNSF",4,"E2L118C16",930,"CD per Load & Unload Interterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["BNSF-E2L118C17","BNSF",4,"E2L118C17",931,"CM per Industry Switch, AVERAGE ALL FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["BNSF-E2L118C18","BNSF",4,"E2L118C18",932,"CM per Interchange Switch, AVERAGE ALL FREIGHT CAR",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["BNSF-E2L118C19","BNSF",4,"E2L118C19",933,"CM per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["BNSF-E2L118C20","BNSF",4,"E2L118C20",934,"CM per Interterminal Switch, AVERAGE ALL FREIGHT CARS",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["BNSF-E2L118C21","BNSF",4,"E2L118C21",935,"CM per I&I Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["BNSF-E2L118C22","BNSF",4,"E2L118C22",936,"Average CM per CD, Railroad-Owned, AVERAGE ALL FREIGHT CARS",422.54248046875,460.86105346679699,462.57952880859398,518.47253417968795,480.34750366210898,441.79345703125,489.76931762695301,435.22640991210898,370.20086669921898,449.47042203949798,500.42965310944902,456.98231543909401,429.76247396058699,404.75335749881901,474.111459846287,422.945976663289]
["BNSF-E2L118C23","BNSF",4,"E2L118C23",937,"Average Miles between I&I Switches, AVERAGE ALL FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["BNSF-E2L118C24","BNSF",4,"E2L118C24",938,"Average Miles between Interchange Switches, AVERAGE ALL FREIGHT CARS",1771.19921875,1849.68823242188,2001.76147460938,2374.90625,2425.3134765625,2371.55078125,2238.38452148438,2172.59838867188,2152.44018554688,2588.1371334432702,2336.60528423712,2434.9630271122101,2686.9424431349198,3180.4725544344701,3599.5314455971902,3635.8603507018202]
["BNSF-E2L118C25","BNSF",4,"E2L118C25",939,"SEMs per Industry Switch, AVERAGE ALL FREIGHT CARS",4.0653176307678196,4.4621381759643599,4.4837818145751998,4.1883964538574201,4.1100525856018102,4.2478790283203098,4.2663950920104998,4.3016629219055202,4.2219319343566903,4.0764409729570001,4.1165431191688304,4.0444730814308798,4.2218032054037797,4.4436614147740903,4.5028908500984999,4.2064893365889704]
["BNSF-E2L118C26","BNSF",4,"E2L118C26",940,"SEMs per Interchange Switch, AVERAGE ALL FREIGHT CARS",2.2359247207641602,2.4541754722595202,2.4660804271697998,2.3036181926727299,2.2605290412902801,2.3363335132598899,2.34651756286621,2.3659145832061799,2.3220627307891801,2.24204253512635,2.2640987155428598,2.22446019478698,2.3219917629720799,2.44401377812575,2.4765899675541698,2.31356913512393]
["BNSF-E2L118C27","BNSF",4,"E2L118C27",941,"SEMs per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",6.0979762077331499,6.6932082176208496,6.7256731986999503,6.2825951576232901,6.1650805473327601,6.3718190193176296,6.3995928764343297,6.4524946212768599,6.3328976631164604,6.11466145943551,6.1748146787532496,6.0667096221463197,6.33270480810567,6.6654921221611296,6.7543362751477396,6.3097340048834498]
["BNSF-E2L118C28","BNSF",4,"E2L118C28",942,"SEMs per Interterminal Switch, AVERAGE ALL FREIGHT CARS",4.8783812522888201,5.3545665740966797,5.3805389404296902,5.0260767936706499,4.9320631027221697,5.0974550247192401,5.1196737289428702,5.1619949340820304,5.0663185119628897,4.8917291675484096,4.9398517430025999,4.8533676977170499,5.0661638464845398,5.3323936977289099,5.4034690201181901,5.0477872039067604]
["BNSF-E2L118C29","BNSF",4,"E2L118C29",943,"SEMs per I&I Switch, AVERAGE ALL FREIGHT CARS",1.01632940769196,1.11553454399109,1.1209454536437999,1.0470992326736499,1.0275131464004501,1.0619697570800799,1.0665988922119101,1.0754157304763801,1.0554829835891699,1.01911024323925,1.02913577979221,1.01111827035772,1.05545080135095,1.1109153536935199,1.1257227125246201,1.0516223341472399]
["BNSF-E2L201C1","BNSF",4,"E2L201C1",944,"Average Distance Per Car In Way Trains",11.5939531326294,11.247911453247101,12.8964853286743,11.6529035568237,10.8891925811768,10.7967977523804,10.5477914810181,9.7689609527587908,10.0364170074463,9.4384301708575506,9.3272894397501602,8.6188005045620493,8.3268747991586096,8.3550894168567602,9.1845515011982997,8.1263775661624607]
["BNSF-E2L202C1","BNSF",4,"E2L202C1",945,"Average TCUs Per Flat Car",7,6.59,6.48,6.14,5.9,5.76,5.29,5.4,5.23,5.24,5.2,5.19,5.14,5.46,5.1100000000000003,5.04]
["BNSF-E2L203C1","BNSF",4,"E2L203C1",946,"Average Tare Weight - Refrigerated TCU",7.3000001907348597,7.3000001907348597,7.1999998092651403,7.0999999046325701,7,7.0999999046325701,6.9000000953674299,6.9000000953674299,6.9000000953674299,6.9,6.9,6.8,6.9,6.9,7.1,7.1]
["BNSF-E2L204C1","BNSF",4,"E2L204C1",947,"Average Tare Weight - Non-Refrigerated TCU",5,5,5,4.9000000953674299,4.9000000953674299,4.9000000953674299,4.9000000953674299,5,5,5,4.9000000000000004,4.7,4.9000000000000004,4.9000000000000004,4.8,4.8]
["BNSF-E2L205C1","BNSF",4,"E2L205C1",948,"Linehaul Miles Per TCU Day",478,478,478,478,478,478,478,478,478,478,478,478,478,478,478,478]
["BNSF-E2L206C1","BNSF",4,"E2L206C1",949,"TCU Days Per Orig Or Term Event",3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.645,3.645,3.645,3.645,3.645,3.645,3.645]
["BNSF-E2L207C1","BNSF",4,"E2L207C1",950,"L/E Ratio - Refrigerated/Non-Refrigerated - TCU",1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.48,1.48,1.48,1.48,1.48,1.48,1.48]
["BNSF-E2L208C1","BNSF",4,"E2L208C1",951,"Average Locomotive Units - Unit Train",2.9182717800140399,3.1163296699523899,3.1666939258575399,3.2731573581695601,3.2497074604034402,3.2535066604614298,3.2315762042999299,3.19236159324646,3.1759829521179199,3.40630912955478,3.4029263319953,3.42271604031537,3.38630368739154,3.4076175686634498,3.4006220357886301,3.43405359007919]
["BNSF-E2L209C1","BNSF",4,"E2L209C1",952,"Average Locomotive Units - Way Train",2.0461404323577899,2.2639610767364502,2.2635848522186302,2.2036592960357702,2.1845781803131099,2.1568307876586901,2.17223119735718,2.1753799915313698,2.1456394195556601,2.2034187910463401,2.2336093539641899,2.23318704231975,2.22603589084911,2.27550721016084,2.21482502026321,2.1290889718864299]
["BNSF-E2L210C1","BNSF",4,"E2L210C1",953,"Average Locomotive Units - Through Train",3.40043377876282,3.1125907897949201,3.1772015094757098,3.3489561080932599,3.2009370326995898,3.12625956535339,3.1368746757507302,3.1394929885864298,3.0181930065154998,3.2930233275752498,3.4783520538516099,3.33504784846318,3.2621870267789901,3.29950440616647,3.4094403909855302,3.4316907022457501]
["BNSF-E2L211C1","BNSF",4,"E2L211C1",954,"Average Gross Tons - Unit Train",9103.470703125,9441.05859375,9431.2607421875,9675.9248046875,9639.728515625,9440.3623046875,9597.525390625,9577.7333984375,9548.5478515625,9745.0119063368093,9613.8461789840003,9629.1657345328604,9656.6338820999608,9711.8554395512492,9888.5903374349291,10083.4896544978]
["BNSF-E2L212C1","BNSF",4,"E2L212C1",955,"Average Gross Tons - Way Train",1960.3642578125,2145.64428710938,2235.25659179688,1965.38500976563,2038.900390625,2044.7939453125,2011.54455566406,2042.38256835938,2103.5400390625,1983.6471341308199,2026.0358348197001,2076.7436845050802,2157.8329885972998,2207.4021112177102,2320.0316073527001,2607.86710969152]
["BNSF-E2L213C1","BNSF",4,"E2L213C1",956,"Average Gross Tons - Through Train",5327.1201171875,5321.45556640625,5407.05517578125,5677.0927734375,5672.30419921875,5616.9130859375,5558.736328125,5566.49462890625,5665.55029296875,5747.2263022674597,5746.0727082486801,5697.3321307853003,5717.2690748336599,5948.0098050168199,6207.2836862539198,6537.3407274988504]
["BNSF-E2L214C1","BNSF",4,"E2L214C1",957,"Engine Crews (Excl Train Switching)",600801.875,559087.4375,582520.4375,439073.84375,543894.375,613201.25,669298.25,755835.875,877897.8125,808006.18774026004,660234.34763149102,732866.115342948,849113.74520670995,796370.52654882905,612543.12454636104,637342.99423887895]
["BNSF-E2L215C1","BNSF",4,"E2L215C1",958,"Train Crews (Excl Train Switching)",534348.1875,547870.625,550512,432496,469141.84375,516961.84375,551034.5625,633833.875,697943.75,677132.07816989801,587797.598534983,635967.37566156802,708749.449759771,696876.21256854699,552741.94576088502,557130.58126565302]
["BNSF-E2L216C1","BNSF",4,"E2L216C1",959,"Total Crew Wages (Excl Train Switching)",1135150,1106958,1133032.5,871569.875,1013036.25,1130163.125,1220332.75,1389669.75,1575841.5,1485138.26591016,1248031.9461664699,1368833.4910045201,1557863.1949664799,1493246.73911738,1165285.0703072499,1194473.57550453]
["BNSF-E2L217C1","BNSF",4,"E2L217C1",960,"Train Miles - Running",174802.71875,170896.734375,166926.53125,139637.578125,152439.421875,158025.453125,162711.84375,167265.59375,171525.796875,166443.804,155849.34899999999,164426.845,172194.93599999999,161392.821,142743.00899999999,143163.10699999999]
[{"$f":"B962&\"-\"&D962","v":"BNSF-E2L218C1"},"BNSF",4,"E2L218C1",961,"Average Crew Wages (Assigned To TM-Crew)",6.4938921928405797,6.4773502349853498,6.7876119613647496,6.2416572570800799,6.6455006599426296,7.1517791748046902,7.4999628067016602,8.3081626892089808,9.1871986389160192,8.9227608971864001,8.0079381413808406,8.3248784041591009,9.0470906471168302,9.2522500682813895,8.1635176284342403,8.3434454625557404]
["BNSF-E2L219C1","BNSF",4,"E2L219C1",962,"General Overhead Ratio",1.0778490304946899,1.0795303583145099,1.08192670345306,1.0876226425170901,1.09486556053162,1.0781713724136399,1.0792661905288701,1.0740994215011599,1.0761349201202399,1.07045701023158,1.09190706419191,1.07468931474788,1.06866927521521,1.0667481989588501,1.0711381521522001,1.06302791199326]
["BNSF-E2L220C1","BNSF",4,"E2L220C1",963,"Constant Cost Markup Ratio",1.2898648977279701,1.29185962677002,1.27911365032196,1.3389712572097801,1.3194119930267301,1.30023765563965,1.2986861467361499,1.3094699382782,1.3074597120285001,1.34435863180554,1.3722635254326101,1.3720617448604799,1.37557590483425,1.36733385158861,1.40448123963547,1.4105194935258401]
["BNSF-E2L301C1","BNSF",4,"E2L301C1",964,"Residual Factor, Industry Switching, Railroad-Owned",68.650069332913006,80.301427763391104,97.308020638565097,113.30856056944999,116.500761623275,113.12717373816,120.78764819305,129.12676633185467,135.32227165100099,142.98808956540799,134.87218056665199,138.11083968026401,153.410906514793,144.255767274524,138.43225051087387,152.74503061111099]
["BNSF-E2L301C2","BNSF",4,"E2L301C2",965,"Residual Factor, Industry Switching, Privately-Owned",54.863995516430698,63.568560914363502,78.454831527878596,90.215431279961606,94.247411896422193,89.909556639960897,93.622606864122204,101.93747236704849,108.412462638883,113.399577118702,107.634386104086,113.03477574404,127.506196311304,120.094768250656,111.60757739114582,125.589313514788]
["BNSF-E2L302C1","BNSF",4,"E2L302C1",966,"Residual Factor, Station Clerical, Railroad-Owned",33.101997186486599,39.538796163999798,44.621472063031597,54.837295934087599,52.769711911020302,54.448901788988401,62.829555763008997,62.786175960826696,60.217738918733197,64.299588152762496,58.664538747084698,52.6217133562483,56.846708409618799,55.118374469848,60.409937296251918,58.465014092784401]
["BNSF-E2L302C2","BNSF",4,"E2L302C2",967,"Residual Factor, Station Clerical, Privately-Owned",4.4678704079737797,4.40464395196478,5.1176314510729002,5.93482270963829,6.1373002487220498,4.9021843172493202,4.2710303869370403,4.0045174593162018,4.7754211913526001,4.8896125828691996,4.1782942530972296,3.6939630793282801,2.9833360300641898,3.29607819437441,2.7728548487879481,2.2358964509666901]
["BNSF-E2L303C1","BNSF",4,"E2L303C1",968,"Residual Factor, Interchange Switching, Railroad-Owned",11.405683740943401,13.160941525472699,15.4301059972201,19.774800248954399,21.390234227225601,20.0159388246948,20.223277824884601,21.06303222579859,28.696572981873899,23.466883696758298,20.184025114837102,17.4731335902297,19.204105545001401,17.338768463897701,15.397576224628505,16.655768566010298]
["BNSF-E2L303C2","BNSF",4,"E2L303C2",969,"Residual Factor, Interchange Switching, Privately-Owned",9.8388786154501702,11.22822642148,13.292484132143899,16.908032212357799,18.560452014119601,16.850774521553902,16.079217790844499,17.883557858262037,24.060135595759899,19.6524152518137,17.287642550253501,15.512534846978999,16.814050252767501,15.2743314486953,13.16527611889722,14.318857567746701]
["BNSF-E2L304C1","BNSF",4,"E2L304C1",970,"Residual Factor, I&I Switching, Railroad-Owned",83.682030415883105,100.01751874123001,118.866273295326,142.88594715586501,153.90007732859499,142.72168674080001,149.48974666848599,156.44789863608261,190.03464841205499,174.981956736532,166.28227102261499,162.805651796658,188.41217179537401,166.618524330025,161.16195264273756,173.020867265101]
["BNSF-E2L304C2","BNSF",4,"E2L304C2",971,"Residual Factor, I&I Switching, Privately-Owned",55.719488228837101,64.712150836900705,78.711560393291293,94.059475214274201,102.62399258498,93.361819479191198,93.313312610389502,104.79012412654549,125.553584822216,114.404494915283,105.713110456143,107.59874586868899,126.193611675498,117.67866396059701,104.380732873632,112.270702115085]
["BNSF-E2L305C1","BNSF",4,"E2L305C1",972,"Residual Factor, Mileage, Railroad-Owned",0.13230835427743701,1.95352279657439,5.4441601190265203,4.4168951489989698,1.10479604141859,1.4357566300756699,0.20775488797149,2.9914560537140549,0.112062594800001,4.4614837876009998,1.98426780284501,1.88872179030475,1.47027728615575,4.9655950885963902,-2.5900320972199218,-8.1424671375698807]
["BNSF-E2L305C2","BNSF",4,"E2L305C2",973,"Residual Factor, Mileage, Privately-Owned",0.48336283220432202,1.7763901960776201,3.94625122111337,3.8534609034526999,1.8572968691881,2.2503270728048999,1.43465566719772,3.6132643013776411,2.6760977830654902,3.7099855229161198,2.51148005097608,2.64691356696212,2.8265904768453201,5.36412156722995,1.1155060016353127,-2.4356542648980599]
["CN-E1L101C1","CN",1,"E1L101C1",1,"Gross Ton Mile (GTM), OPR Expense",1.8575512804091001E-3,1.9204950658604501E-3,2.4033321533352102E-3,1.95178296416998E-3,2.0685270428657501E-3,2.8866559732705398E-3,2.5090491399168999E-3,2.7003674767911399E-3,2.7921702712774298E-3,2.3435959605790299E-3,2.2210347049364801E-3,2.5321370517948998E-3,2.6878596375007101E-3,2.68024174784132E-3,2.3028881898264101E-3,2.3617264129235501E-3]
["CN-E1L101C2","CN",1,"E1L101C2",2,"Gross Ton Mile (GTM), DRL Expense",8.2539295544847803E-4,8.4689538925886198E-4,8.94131429959089E-4,1.1382562806829799E-3,5.8711424935609102E-4,1.54226180166006E-3,1.42293167300522E-3,9.4008666928857597E-4,1.09591137152165E-3,1.10524616089443E-3,1.42446695473875E-3,1.4581804690940699E-3,1.54351092938562E-3,1.54738053289447E-3,1.77966025315473E-3,1.6718236231197E-3]
["CN-E1L101C3","CN",1,"E1L101C3",3,"Gross Ton Mile (GTM), ROI Expense",2.83871009014547E-3,3.2283128239214399E-3,3.7522090133279601E-3,4.2436062358319803E-3,2.5774822570383501E-3,6.0987276956439001E-3,4.2870375327765898E-3,3.5473632160574202E-3,3.2393813598900999E-3,3.26161479613906E-3,3.39966365393523E-3,3.7842466249651801E-3,4.48851718687271E-3,3.7728949917259602E-3,3.6263362998818498E-3,4.5759431384198501E-3]
["CN-E1L102C1","CN",1,"E1L102C1",4,"Car Mile (CM) - Other Than Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L102C2","CN",1,"E1L102C2",5,"Car Mile (CM) - Other Than Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L102C3","CN",1,"E1L102C3",6,"Car Mile (CM) - Other Than Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L103C1","CN",1,"E1L103C1",7,"Train Mile (TM) - Other Than Crew, OPR Expense",0.80618542432785001,0.76995664834976196,0.79841321706771895,0.96293330192565896,0.86702585220336903,1.15756952762604,1.24767029285431,0.78289872407913197,0.53926372528076205,1.0221751399696599,0.74081685436259403,1.33107062357225,1.0559964086292799,0.89372972896440706,0.83795162679787705,0.66348537322314305]
["CN-E1L103C2","CN",1,"E1L103C2",8,"Train Mile (TM) - Other Than Crew, DRL Expense",-4.2794953333213898E-4,1.93407048936933E-3,2.6684260228648798E-4,5.5724679259583397E-4,4.4763286132365498E-4,2.3678627330809801E-3,2.1664206869900201E-3,2.0228563807904699E-3,2.3568547330796701E-3,4.2047758154764399E-3,4.5600948771232297E-3,4.2840578368342E-3,4.1968013498785497E-3,3.7247675460949001E-3,3.8222888023557201E-3,3.0401304987760901E-3]
["CN-E1L103C3","CN",1,"E1L103C3",9,"Train Mile (TM) - Other Than Crew, ROI Expense",-1.0612044716253901E-3,2.1501742303371399E-3,2.43846629746258E-3,2.8083403594791898E-3,-1.1259664315730301E-3,2.46882648207247E-3,2.0368006080389001E-3,1.7701348988339301E-3,1.3874446740373999E-3,9.3407747618722502E-4,5.7947848019966597E-4,4.1327612755508099E-4,6.8148131670595798E-6,-3.8893194750105902E-4,-7.0856445706092704E-4,-1.2583437517450101E-3]
["CN-E1L104C1","CN",1,"E1L104C1",10,"Train Mile (TM) - Crew, OPR Expense",5.27822065353394,5.7154693603515598,6.6658415794372603,8.0402021408081108,8.1793479919433594,7.9740180969238299,9.1604890823364293,9.3670568466186506,10.9297494888306,10.639978095829299,11.456353517694501,12.868544515562901,12.817077181351699,12.671518757809,12.1344345328225,10.417480352818901]
["CN-E1L104C2","CN",1,"E1L104C2",11,"Train Mile (TM) - Crew, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L104C3","CN",1,"E1L104C3",12,"Train Mile (TM) - Crew, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L105C1","CN",1,"E1L105C1",13,"Locomotive Unit Mile (LUM), OPR Expense",3.3701007366180402,3.9789688587188698,5.3844695091247603,3.6695747375488299,4.4814591407775897,7.5816564559936497,6.1564593315124503,6.7580847740173304,6.73781061172485,4.6532416851860399,4.1373164022878104,5.01830818614562,5.7228742075305696,5.2774010050848599,3.8559936514293298,4.7439905452140803]
["CN-E1L105C2","CN",1,"E1L105C2",14,"Locomotive Unit Mile (LUM), DRL Expense",0.25062194466590898,0.25271654129028298,0.28275951743125899,0.336517244577408,0.209038510918617,0.34643524885177601,1.7328413724899301,0.56782144308090199,1.23195016384125,0.57344669741738696,1.1638647509687901,1.3338993215192401,1.6575065863823999,1.0925459684902199,1.1009609447653701,0.97516621165869199]
["CN-E1L105C3","CN",1,"E1L105C3",15,"Locomotive Unit Mile (LUM), ROI Expense",0.34186652302741999,0.49845308065414401,0.50602847337722801,0.57710903882980302,0.51531654596328702,0.57787060737609897,0.52272593975067105,0.54548394680023204,0.67359894514083896,0.89290372152981001,1.21228507804838,1.3560041286544999,1.74764935970729,1.81330164917922,1.8425290633506799,2.51720947949027]
["CN-E1L106C1","CN",1,"E1L106C1",16,"CLOR (Carloads Handled) - Other, OPR Expense",2.4279756546020499,2.5229418277740501,2.7528920173645002,2.4129223823547399,2.8580398559570299,2.9572298526763898,8.6013431549072301,11.3943729400635,11.3382968902588,10.284252039482899,0.758738288635463,3.1650372855575002,3.6687025050375901,3.2238572746631098,2.3111144244000998,2.6648292151094202]
["CN-E1L106C2","CN",1,"E1L106C2",17,"CLOR (Carloads Handled) - Other, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L106C3","CN",1,"E1L106C3",18,"CLOR (Carloads Handled) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L107C1","CN",1,"E1L107C1",19,"CLOR (Carloads Handled) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L107C2","CN",1,"E1L107C2",20,"CLOR (Carloads Handled) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L107C3","CN",1,"E1L107C3",21,"CLOR (Carloads Handled) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L108C1","CN",1,"E1L108C1",22,"CLOT (Carloads Orig Or Term) - Other, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L108C2","CN",1,"E1L108C2",23,"CLOT (Carloads Orig Or Term) - Other, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L108C3","CN",1,"E1L108C3",24,"CLOT (Carloads Orig Or Term) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L109C1","CN",1,"E1L109C1",25,"CLOT (Carloads Orig Or Term) - Clerical, OPR Expense",10.5983009338379,13.026421546936,19.280757904052699,19.837730407714801,18.995822906494102,17.491998672485401,24.4986877441406,24.549476623535199,20.4632968902588,25.403232584862401,24.773782552210101,25.301400727524499,24.3594123026133,21.301836514764101,18.579875974909399,18.887133623624699]
["CN-E1L109C2","CN",1,"E1L109C2",26,"CLOT (Carloads Orig Or Term) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L109C3","CN",1,"E1L109C3",27,"CLOT (Carloads Orig Or Term) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L110C1","CN",1,"E1L110C1",28,"Car Mile (CM) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L110C2","CN",1,"E1L110C2",29,"Car Mile (CM) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L110C3","CN",1,"E1L110C3",30,"Car Mile (CM) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L111C1","CN",1,"E1L111C1",31,"Switch Engine Minutes (SEM), OPR Expense",3.33935642242432,3.4382185935974099,4.01548051834106,3.98137235641479,4.3757352828979501,4.57458591461182,4.4267902374267596,4.8098340034484899,5.2163648605346697,4.8586806101414197,4.6858893037352196,4.8973735981744397,5.7767157772247302,5.8963939183214302,5.4722543594727204,5.2157476622897496]
["CN-E1L111C2","CN",1,"E1L111C2",32,"Switch Engine Minutes (SEM), DRL Expense",0.106353677809238,0.166318014264107,8.5286892950534807E-2,8.6529478430748E-2,1.0104620456695601,-0.93862485885620095,8.5763238370418493E-2,0.55008029937744096,0.660020291805267,0.741876592204051,0.94115548969113605,0.94948793192779601,0.92513304270553398,0.93145444031706803,1.16934634832635,1.0537246808879199]
["CN-E1L111C3","CN",1,"E1L111C3",33,"Switch Engine Minutes (SEM), ROI Expense",1.3135353326797501,1.7393773794174201,1.7288278341293299,1.9643195867538501,5.2444615364074698,-1.8386814594268801,1.3397296667098999,3.4136667251586901,3.2947962284088099,3.5203551051671602,3.7552718966461098,4.0752624326104003,4.3528804632782201,3.5415895681002398,3.5436408915455799,4.6801208556857397]
["CN-E1L112C1","CN",1,"E1L112C1",34,"Ton Miles In Lake Transfer Service, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L112C2","CN",1,"E1L112C2",35,"Ton Miles In Lake Transfer Service, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L112C3","CN",1,"E1L112C3",36,"Ton Miles In Lake Transfer Service, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L113C1","CN",1,"E1L113C1",37,"Tons Handled at Coal Terminals, OPR Expense",1.5945284366607699,1.6153678894043,7.2490253448486301,1.4397553205490099,1.0101910829544101,0.78281891345977805,1.0329946279525799,0.43563318252563499,0.63039964437484697,0.72805859013834795,1.5688142179276201,0.88668643424147697,0.46711316320347002,0.67308146714442196,0.35366210183979702,0.37447031819964699]
["CN-E1L113C2","CN",1,"E1L113C2",38,"Tons Handled at Coal Terminals, DRL Expense",0.12097813189029701,0.112806528806686,0.41638582944870001,0,6.5030567348003401E-2,5.7181995362043402E-2,1.3415892124176001,0.112246103584766,3.6368875298649099E-3,1.1798256135052801E-2,0.93123471777098699,1.78231139003895,0,0,0,0]
["CN-E1L113C3","CN",1,"E1L113C3",39,"Tons Handled at Coal Terminals, ROI Expense",0.232727020978928,0.40079495310783397,1.6256061792373699,0,0.219241142272949,0.24294033646583599,5.7407746315002397,0.49884405732154802,2.4863678961992298E-2,4.0994761964646902E-2,2.7068680289527398,6.1307145124774403,0,0,0,0]
["CN-E1L114C1","CN",1,"E1L114C1",40,"Tons Handled at Ore Terminals, OPR Expense",0.80884534120559703,0.72069013118743896,0.78045612573623702,1.1739729642868,4.9218916893005398,5.53902387619019,0.92208689451217696,1.2596747875213601,1.2740997076034499,1.2050610471952099,1.3949288718972099,0.78074749434115798,0.652182303040856,0.58411038141611504,0.48023672834950198,0.370811712961155]
["CN-E1L114C2","CN",1,"E1L114C2",41,"Tons Handled at Ore Terminals, DRL Expense",7.1378566324710804E-2,4.19277101755142E-2,4.1056819260120399E-2,6.8113796412944794E-2,4.9162451177835499E-2,4.8142772167921101E-2,5.2162177860736798E-2,5.52648454904556E-2,3.8949877023696899E-2,8.2862467812519894E-2,8.6459168456100896E-2,8.9518785610987001E-2,9.6355384699157803E-2,0.10970349647506999,0.128099230157913,0.12476397976787]
["CN-E1L114C3","CN",1,"E1L114C3",42,"Tons Handled at Ore Terminals, ROI Expense",0.137311771512032,0.148966684937477,0.160289391875267,0.244083106517792,0.16574409604072601,0.20453676581382799,0.223206371068954,0.24560798704624201,0.26628187298774703,0.28791773164553802,0.251315328388791,0.30792269025035002,0.40558546859736599,0.30831476453361301,0.29380240861047502,0.38718889821668201]
["CN-E1L115C1","CN",1,"E1L115C1",43,"Tons Handled at Other Marine Terminals, OPR Expense",7.6534070968627903,8.3686332702636701,8.9106769561767596,2.07472825050354,0.816034495830536,0.72023224830627397,0.70061749219894398,0.98489195108413696,1.08628726005554,2.9168613327431299,5.4700962831337003,6.6309954580811201,8.0361043297679693,11.437185351012101,8.6856865349827999,6.85045988991937]
["CN-E1L115C2","CN",1,"E1L115C2",44,"Tons Handled at Other Marine Terminals, DRL Expense",0.97848808765411399,2.6609671767800999E-3,1.9397237338125699E-3,3.8949593435972899E-3,5.8412912767380498E-4,0,0,0,0,0,-3.3751558105508297E-2,3.4838173427371499E-2,-5.5588987606818097E-3,2.9705911026185201E-2,-1.5381575847325699E-3,-1.42100017537579E-3]
["CN-E1L115C3","CN",1,"E1L115C3",45,"Tons Handled at Other Marine Terminals, ROI Expense",-4.1021451354026801E-2,0,0,0,0,0,0,0,0,0,2.6856430206540498E-3,9.0222533751654604E-3,-7.5972631677192898E-2,0,1.04508040774286E-4,2.57249123993682E-4]
["CN-E1L116C1","CN",1,"E1L116C1",46,"Refrigerated Car Miles, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L116C2","CN",1,"E1L116C2",47,"Refrigerated Car Miles, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L116C3","CN",1,"E1L116C3",48,"Refrigerated Car Miles, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L117C1","CN",1,"E1L117C1",49,"Protective Service Reefer TCU Days, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L117C2","CN",1,"E1L117C2",50,"Protective Service Reefer TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L117C3","CN",1,"E1L117C3",51,"Protective Service Reefer TCU Days, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B1026&\"-\"&D1026","v":"CN-E1L118C1"},"CN",1,"E1L118C1",52,"Refrigerated TCU Days, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L118C2","CN",1,"E1L118C2",53,"Refrigerated TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L118C3","CN",1,"E1L118C3",54,"Refrigerated TCU Days, ROI Expense",1.8221466541290301,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L119C1","CN",1,"E1L119C1",55,"Other (Non-Refrigerated) TCU Days, OPR Expense",7.4991393089294398,8.2208003997802699,8.0811910629272496,6.1792922019958496,4.0179157257080096,2.7137684822082502,3.0856580734252899,3.4371554851532,2.9966225624084499,2.6289915078007602,2.5115217636081799,3.12805920761559,2.6468570495496899,2.9074087898879402,2.3312973049599899,2.5751508424679699]
["CN-E1L119C2","CN",1,"E1L119C2",56,"Other (Non-Refrigerated) TCU Days, DRL Expense",4.7361559867858896,2.14719939231873,1.3551653623580899,1.0045907497405999,1.6531459093093901,1.3231297731399501,6.7762292921543094E-2,6.7118823528289795E-2,9.2062443494796795E-2,2.6483643260067601E-2,-7.01877597920354E-3,0.117626514807521,0.14890328290847599,0.44159813204293602,1.03744072985295,0.91767782454214397]
["CN-E1L119C3","CN",1,"E1L119C3",57,"Other (Non-Refrigerated) TCU Days, ROI Expense",0.35720852017402599,1.01979315280914,0.51058423519134499,0.46842798590660101,0.37806263566017201,0.40606257319450401,0.42418935894966098,0.46849668025970498,0.48528021574020402,0.34233096092098197,0.46062516377360202,1.00068963994948,1.6097821055488,2.2407094758792598,0.80089078133121905,1.1707419419779801]
["CN-E1L120C1","CN",1,"E1L120C1",58,"TCUs Loaded And Unloaded (L&UL), OPR Expense",16.4449863433838,18.0909118652344,17.6102104187012,23.831829071044901,18.5386142730713,15.467669486999499,1.976078748703,0.87977695465087902,0.60014677047729503,13.004317073716599,41.157436161577699,53.003314849511497,54.197176488981,51.480574589545498,45.191198152279199,47.587189740073597]
["CN-E1L120C2","CN",1,"E1L120C2",59,"TCUs Loaded And Unloaded (L&UL), DRL Expense",2.0886766910553001,1.85466873645782,1.7807699441909799,2.0211327075958301,1.82267713546753,1.6629539728164699,1.3233786821365401,1.09196329116821,0.85547381639480602,0.34338037965837298,0.16566953236618701,0.205716262039077,0.35892670879830901,0.85498782346771096,1.95283084423826,1.3505365559951801]
["CN-E1L120C3","CN",1,"E1L120C3",60,"TCUs Loaded And Unloaded (L&UL), ROI Expense",3.8098709583282502,5.2988348007202104,5.3841223716735804,5.3629727363586399,4.9313502311706499,4.8426432609558097,3.7293388843536399,2.42415571212769,2.0592970848083501,2.1317603225111399,2.4426535338179001,3.0388807570202001,3.7709584112989099,3.1664455255244301,3.00397766225753,4.5371641941708498]
["CN-E1L121C1","CN",1,"E1L121C1",61,"MVUs Loaded And Unloaded (L&UL), OPR Expense",1.5157231092453001,1.4611786603927599,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L121C2","CN",1,"E1L121C2",62,"MVUs Loaded And Unloaded (L&UL), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L121C3","CN",1,"E1L121C3",63,"MVUs Loaded And Unloaded (L&UL), ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L122C1","CN",1,"E1L122C1",64,"TCUs Picked Up and Delivered (PU&D), OPR Expense",325.34844970703102,174.40516662597699,436.801025390625,369.26281738281301,318.12371826171898,84.328269958496094,583.60626220703102,164.38839721679699,354.14932250976602,241.17712185853199,83.031754731495099,16.329036398127698,7.0495603124579702,93.937955229209095,127.268758258964,253.12785567099499]
["CN-E1L122C2","CN",1,"E1L122C2",65,"TCUs Picked Up and Delivered (PU&D), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L122C3","CN",1,"E1L122C3",66,"TCUs Picked Up and Delivered (PU&D), ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L201C1","CN",1,"E1L201C1",67,"CM(R), OPR Expense, Railroad-Owned, BOX - 40 FT",6.7061558365821797E-2,2.1243495866656299E-3,1.34288985282183E-3,1.0611352045089E-3,7.2970153996720899E-4,3.4752377541735801E-4,3.6962606827728499E-4,1.029601553455E-4,0,0,0,9.2686525920288401E-4,2.86983057773872E-3,8.7650115780430297E-3,1.2287527345179799E-2,1.3137423750651E-2]
["CN-E1L201C2","CN",1,"E1L201C2",68,"CM(R), DRL Expense, Railroad-Owned, BOX - 40 FT",4.5290686190128299E-2,4.66260984539986E-2,0.146831184625626,5.60570396482944E-2,5.1841221749782597E-2,5.1457300782203702E-2,5.6717082858085598E-2,5.0548586994409603E-2,5.1774788647890098E-2,6.5733579700533507E-2,6.0835004225564301E-2,3.5006102340330997E-2,2.6734203085149202E-2,3.11879485055311E-2,2.7921703424016599E-2,1.7161142368643301E-2]
["CN-E1L201C3","CN",1,"E1L201C3",69,"CM(R), ROI Expense, Railroad-Owned, BOX - 40 FT",8.8601903989911097E-3,1.10988216474652E-2,0.24370352923870101,1.81724112480879E-2,1.57079380005598E-2,1.75473988056183E-2,1.9707165658474E-2,1.7269900068640699E-2,1.76690388470888E-2,1.65326010666813E-2,1.46206724069834E-2,1.20723588303456E-2,9.6016606735596297E-3,5.6919345002197702E-3,4.0808718666540001E-3,5.0447693757863302E-3]
["CN-E1L201C4","CN",1,"E1L201C4",70,"CM(Y), OPR Expense, Railroad-Owned, BOX - 40 FT",0.17435991764068601,5.5233137682080304E-3,3.49150900729001E-3,2.75895395316184E-3,1.8972230609506399E-3,9.0356252621859301E-4,9.6102774841710903E-4,2.6769636315293599E-4,0,0,0,2.4098496739275001E-3,7.4615595021206797E-3,2.27890301029119E-2,3.19475710974675E-2,3.4157301751692501E-2]
["CN-E1L201C5","CN",1,"E1L201C5",71,"CM(Y), DRL Expense, Railroad-Owned, BOX - 40 FT",0.11775575578212701,0.121227890253067,0.38176071643829301,0.145748481154442,0.13478694856166801,0.13378882408142101,0.147464454174042,0.131426155567169,0.13461466133594499,0.170907307221387,0.15817101098646699,9.1015866084860703E-2,6.9508928021388097E-2,8.1088666114381105E-2,7.2596428902442695E-2,4.4618970158472597E-2]
["CN-E1L201C6","CN",1,"E1L201C6",72,"CM(Y), ROI Expense, Railroad-Owned, BOX - 40 FT",2.3036506026983299E-2,2.88569107651711E-2,0.633628249168396,4.7248296439647702E-2,4.0840554982423803E-2,4.56231944262981E-2,5.1238652318716001E-2,4.4901713728904703E-2,4.5939534902572597E-2,4.2984762773371397E-2,3.8013748258156899E-2,3.1388132958898703E-2,2.49643177512551E-2,1.47990297005714E-2,1.06102668533003E-2,1.31164003770445E-2]
["CN-E1L201C7","CN",1,"E1L201C7",73,"CD(R), OPR Expense, Railroad-Owned, BOX - 40 FT",8.5551099777221697,0.276733428239822,0.179143637418747,0.145340740680695,0.10442405194044101,4.7428127378225299E-2,4.6402696520090103E-2,1.22421495616436E-2,0,0,0,0.117067405547248,0.42199540587634599,1.46153537293832,2.21331936586239,2.47464708774603]
["CN-E1L201C8","CN",1,"E1L201C8",74,"CD(R), DRL Expense, Railroad-Owned, BOX - 40 FT",91.756393432617202,142.74302673339801,215.17181396484401,202.88853454589801,95.851600646972699,73.152656555175795,65.938308715820298,59.205703735351598,60.204307556152301,56.697086694192699,55.140561119847497,47.269349575900101,20.188631558900799,195.30998186717599,184.85573985368799,157.508452983756]
["CN-E1L201C9","CN",1,"E1L201C9",75,"CD(R), ROI Expense, Railroad-Owned, BOX - 40 FT",1.7347373962402299,2.1842882633209202,49.351749420166001,4.0987319946289098,3.4525909423828098,3.1001071929931601,3.3590064048767099,3.2371015548706099,3.5778889656066899,2.7556030591485601,2.71264091486076,2.5788863394794301,2.37490592480524,1.55492863674576,1.13621572615567,1.4131727356068899]
["CN-E1L201C10","CN",1,"E1L201C10",76,"CD(Y), OPR Expense, Railroad-Owned, BOX - 40 FT",8.5551109313964808,0.276733458042145,0.179143637418747,0.145340740680695,0.10442405194044101,4.7428123652935E-2,4.6402692794799798E-2,1.22421495616436E-2,0,0,0,0.117067405547248,0.42199540587634599,1.46153537293832,2.21331936586239,2.47464708774603]
["CN-E1L201C11","CN",1,"E1L201C11",77,"CD(Y), DRL Expense, Railroad-Owned, BOX - 40 FT",91.756393432617202,142.74302673339801,215.17181396484401,202.88851928710901,95.851600646972699,73.152664184570298,65.938308715820298,59.205703735351598,60.204299926757798,56.697086694192699,55.140561119847497,47.269349575900101,20.188631558900799,195.30998186717599,184.85573985368799,157.508452983756]
["CN-E1L201C12","CN",1,"E1L201C12",78,"CD(Y), ROI Expense, Railroad-Owned, BOX - 40 FT",1.7347373962402299,2.1842882633209202,49.3517456054688,4.0987319946289098,3.4525907039642298,3.10010766983032,3.3590064048767099,3.2371015548706099,3.5778889656066899,2.7556030591485601,2.71264091486076,2.5788863394794301,2.37490592480524,1.55492863674576,1.13621572615567,1.4131727356068899]
["CN-E1L201C13","CN",1,"E1L201C13",79,"CM(R), DRL Expense, Privately-Owned, BOX - 40 FT",0.36192020773887601,0.45378997921943698,0.46559363603591902,0.81836670637130704,0.59161847829818703,0.2439915984869,0.34094971418380698,0.245825424790382,0.29127544164657598,0.26727229224085702,0.29877328257941899,0.269697293505753,0.26379971454066597,0.25584899360581598,0.21277144042535301,0.26235446919710198]
["CN-E1L202C1","CN",1,"E1L202C1",80,"CM(R), OPR Expense, Railroad-Owned, BOX - 50 FT",6.7061558365821797E-2,2.1243495866656299E-3,1.34288985282183E-3,1.0611352045089E-3,7.2970153996720899E-4,3.4752377541735801E-4,3.6962606827728499E-4,1.029601553455E-4,0,0,0,9.2686525920288401E-4,2.86983057773872E-3,8.7650115780430297E-3,1.2287527345179799E-2,1.3137423750651E-2]
["CN-E1L202C2","CN",1,"E1L202C2",81,"CM(R), DRL Expense, Railroad-Owned, BOX - 50 FT",4.5290686190128299E-2,4.66260984539986E-2,0.146831184625626,5.60570396482944E-2,5.1841221749782597E-2,5.1457300782203702E-2,5.6717082858085598E-2,5.0548586994409603E-2,5.1774788647890098E-2,6.5733579700533507E-2,6.0835004225564301E-2,3.5006102340330997E-2,2.6734203085149202E-2,3.11879485055311E-2,2.7921703424016599E-2,1.7161142368643301E-2]
["CN-E1L202C3","CN",1,"E1L202C3",82,"CM(R), ROI Expense, Railroad-Owned, BOX - 50 FT",8.8601903989911097E-3,1.10988216474652E-2,0.24370352923870101,1.81724112480879E-2,1.57079380005598E-2,1.75473988056183E-2,1.9707165658474E-2,1.7269900068640699E-2,1.76690388470888E-2,1.65326010666813E-2,1.46206724069834E-2,1.20723588303456E-2,9.6016606735596297E-3,5.6919345002197702E-3,4.0808718666540001E-3,5.0447693757863302E-3]
["CN-E1L202C4","CN",1,"E1L202C4",83,"CM(Y), OPR Expense, Railroad-Owned, BOX - 50 FT",0.17435991764068601,5.5233137682080304E-3,3.49150900729001E-3,2.75895395316184E-3,1.8972230609506399E-3,9.0356252621859301E-4,9.6102774841710903E-4,2.6769636315293599E-4,0,0,0,2.4098496739275001E-3,7.4615595021206797E-3,2.27890301029119E-2,3.19475710974675E-2,3.4157301751692501E-2]
["CN-E1L202C5","CN",1,"E1L202C5",84,"CM(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",0.11775575578212701,0.121227890253067,0.38176071643829301,0.145748481154442,0.13478694856166801,0.13378882408142101,0.147464454174042,0.131426155567169,0.13461466133594499,0.170907307221387,0.15817101098646699,9.1015866084860703E-2,6.9508928021388097E-2,8.1088666114381105E-2,7.2596428902442695E-2,4.4618970158472597E-2]
["CN-E1L202C6","CN",1,"E1L202C6",85,"CM(Y), ROI Expense, Railroad-Owned, BOX - 50 FT",2.3036506026983299E-2,2.88569107651711E-2,0.633628249168396,4.7248296439647702E-2,4.0840554982423803E-2,4.56231944262981E-2,5.1238652318716001E-2,4.4901713728904703E-2,4.5939534902572597E-2,4.2984762773371397E-2,3.8013748258156899E-2,3.1388132958898703E-2,2.49643177512551E-2,1.47990297005714E-2,1.06102668533003E-2,1.31164003770445E-2]
["CN-E1L202C7","CN",1,"E1L202C7",86,"CD(R), OPR Expense, Railroad-Owned, BOX - 50 FT",8.5551099777221697,0.276733428239822,0.179143637418747,0.145340740680695,0.10442405194044101,4.7428127378225299E-2,4.6402696520090103E-2,1.22421495616436E-2,0,0,0,0.117067405547248,0.42199540587634599,1.46153537293832,2.21331936586239,2.47464708774603]
["CN-E1L202C8","CN",1,"E1L202C8",87,"CD(R), DRL Expense, Railroad-Owned, BOX - 50 FT",91.756393432617202,142.74302673339801,215.17181396484401,202.88853454589801,95.851600646972699,73.152656555175795,65.938308715820298,59.205703735351598,60.204307556152301,56.697086694192699,55.140561119847497,47.269349575900101,20.188631558900799,195.30998186717599,184.85573985368799,157.508452983756]
["CN-E1L202C9","CN",1,"E1L202C9",88,"CD(R), ROI Expense, Railroad-Owned, BOX - 50 FT",1.7347373962402299,2.1842882633209202,49.351749420166001,4.0987319946289098,3.4525909423828098,3.1001071929931601,3.3590064048767099,3.2371015548706099,3.5778889656066899,2.7556030591485601,2.71264091486076,2.5788863394794301,2.37490592480524,1.55492863674576,1.13621572615567,1.4131727356068899]
["CN-E1L202C10","CN",1,"E1L202C10",89,"CD(Y), OPR Expense, Railroad-Owned, BOX - 50 FT",8.5551109313964808,0.276733458042145,0.179143637418747,0.145340740680695,0.10442405194044101,4.7428123652935E-2,4.6402692794799798E-2,1.22421495616436E-2,0,0,0,0.117067405547248,0.42199540587634599,1.46153537293832,2.21331936586239,2.47464708774603]
["CN-E1L202C11","CN",1,"E1L202C11",90,"CD(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",91.756393432617202,142.74302673339801,215.17181396484401,202.88851928710901,95.851600646972699,73.152664184570298,65.938308715820298,59.205703735351598,60.204299926757798,56.697086694192699,55.140561119847497,47.269349575900101,20.188631558900799,195.30998186717599,184.85573985368799,157.508452983756]
["CN-E1L202C12","CN",1,"E1L202C12",91,"CD(Y), ROI Expense, Railroad-Owned, BOX - 50 FT",1.7347373962402299,2.1842882633209202,49.3517456054688,4.0987319946289098,3.4525907039642298,3.10010766983032,3.3590064048767099,3.2371015548706099,3.5778889656066899,2.7556030591485601,2.71264091486076,2.5788863394794301,2.37490592480524,1.55492863674576,1.13621572615567,1.4131727356068899]
["CN-E1L202C13","CN",1,"E1L202C13",92,"CM(R), DRL Expense, Privately-Owned, BOX - 50 FT",0.36192020773887601,0.45378997921943698,0.46559363603591902,0.81836670637130704,0.59161847829818703,0.2439915984869,0.34094971418380698,0.245825424790382,0.29127544164657598,0.26727229224085702,0.29877328257941899,0.269697293505753,0.26379971454066597,0.25584899360581598,0.21277144042535301,0.26235446919710198]
["CN-E1L203C1","CN",1,"E1L203C1",93,"CM(R), OPR Expense, Railroad-Owned, BOX - EQUIPPED",3.5907283425331102E-2,3.4749630838632597E-2,3.7249714136123699E-2,3.9939668029546703E-2,3.98533940315247E-2,3.70602570474148E-2,3.7079188972711598E-2,3.4017566591501201E-2,3.7053171545267098E-2,4.7465575517510801E-2,5.77543777626272E-2,6.8733324490264897E-2,6.7381617108799405E-2,7.7538935257401603E-2,7.6799113622456297E-2,7.0195488719353397E-2]
["CN-E1L203C2","CN",1,"E1L203C2",94,"CM(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED",-6.2180506065487896E-3,1.1757244355976601E-2,1.9172795116901401E-2,3.4928943961858701E-2,2.5650983676314399E-2,3.6502145230770097E-2,4.3940648436546298E-2,3.3518780022859601E-2,4.7366786748170901E-2,8.2919942114252299E-2,8.5581649697426099E-2,9.0316558179866099E-2,7.7444844633326099E-2,9.7792538883234706E-2,9.69324355715145E-2,0.104913185311515]
["CN-E1L203C3","CN",1,"E1L203C3",95,"CM(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED",2.9874335974454901E-2,4.8412073403596899E-2,5.4896079003810903E-2,7.22965598106384E-2,6.2863409519195598E-2,7.7208936214446994E-2,9.12144109606743E-2,8.8390313088893904E-2,8.8324032723903698E-2,7.7907523837387402E-2,7.9987366100152002E-2,9.3688491304997498E-2,0.10833947113883501,9.6134439477601794E-2,8.0827302727961903E-2,0.10707317891889]
["CN-E1L203C4","CN",1,"E1L203C4",96,"CM(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED",9.3358911573886899E-2,9.0349078178405803E-2,9.6849165856838199E-2,0.10384318977594401,0.10361885279417,9.6356615424156203E-2,9.6405819058418302E-2,8.8445633649826105E-2,9.6338227391242995E-2,0.123410496345528,0.15016138218283101,0.178706643674689,0.17519220448287801,0.20160123166924401,0.19967769541838601,0.18250827067031899]
["CN-E1L203C5","CN",1,"E1L203C5",97,"CM(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED",-1.61669254302979E-2,3.0568839982151999E-2,4.9849323928356198E-2,9.0815216302871704E-2,6.66925683617592E-2,9.4905503094196306E-2,0.114245608448982,8.7148785591125502E-2,0.123153701424599,0.21559184949705601,0.22251228921330801,0.23482305126765199,0.20135659604664799,0.25426060109641002,0.25202433248593697,0.27277428180994001]
["CN-E1L203C6","CN",1,"E1L203C6",98,"CM(Y), ROI Expense, Railroad-Owned, BOX - EQUIPPED",7.7673308551311507E-2,0.125871255993843,0.14272980391979201,0.187970817089081,0.16344486176967599,0.20074312388896901,0.23715750873088801,0.229814648628235,0.229642748832703,0.20255956197720701,0.20796715186039599,0.24359007739299399,0.28168262496097202,0.249949542641764,0.210150987092701,0.27839026518911397]
["CN-E1L203C7","CN",1,"E1L203C7",99,"CD(R), OPR Expense, Railroad-Owned, BOX - EQUIPPED",3.5790069103240998,3.5310616493225102,3.8423171043396001,4.1799364089965803,4.2093653678893999,3.8904051780700701,3.65719795227051,3.22260594367981,3.3686037063598602,4.2904473794760598,4.9475959466191002,5.6316299282447604,5.4279099462916403,6.3364941162214201,6.4971900702392098,6.1264256843238201]
["CN-E1L203C8","CN",1,"E1L203C8",100,"CD(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED",4.0353832244873002,7.2481360435485804,13.361676216125501,18.209356307983398,15.3288764953613,16.390663146972699,20.011772155761701,18.723556518554702,25.861381530761701,31.334425663294699,26.0682614560281,24.4595595441352,23.6796936416699,23.533472050482501,26.448846683939401,21.380371103346199]
["CN-E1L203C9","CN",1,"E1L203C9",101,"CD(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED",4.5846939086914098,7.4027056694030797,8.5276384353637695,11.6698713302612,9.8085136413574201,11.7631568908691,12.0339136123657,12.3133955001831,11.9952182769775,10.0261829800163,9.4797245881660306,11.196874255988501,13.260291942100199,11.8799767153953,10.758468338532399,14.4121063482315]
["CN-E1L203C10","CN",1,"E1L203C10",102,"CD(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED",3.5790069103240998,3.5310616493225102,3.8423171043396001,4.1799359321594203,4.2093653678893999,3.8904051780700701,3.65719795227051,3.22260594367981,3.3686039447784402,4.2904473794760598,4.9475959466191002,5.6316299282447604,5.4279099462916403,6.3364941162214299,6.4971900702392098,6.1264256843238201]
["CN-E1L203C11","CN",1,"E1L203C11",103,"CD(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED",4.0353832244873002,7.2481355667114302,13.361676216125501,18.209356307983398,15.328874588012701,16.390663146972699,20.011772155761701,18.723558425903299,25.861383438110401,31.334425663294699,26.0682614560281,24.4595595441352,23.6796936416699,23.533472050482501,26.448846683939401,21.380371103346199]
["CN-E1L203C12","CN",1,"E1L203C12",104,"CD(Y), ROI Expense, Railroad-Owned, BOX - EQUIPPED",4.58469438552856,7.4027047157287598,8.5276384353637695,11.6698703765869,9.8085136413574201,11.7631568908691,12.03391456604,12.313396453857401,11.9952192306519,10.0261829800163,9.4797245881660306,11.196874255988501,13.260291942100199,11.8799767153953,10.758468338532399,14.4121063482315]
["CN-E1L203C13","CN",1,"E1L203C13",105,"CM(R), DRL Expense, Privately-Owned, BOX - EQUIPPED",0.26090341806411699,0.26738736033439597,0.28307324647903398,0.55660361051559404,0.391777724027634,0.42243444919586198,0.42096155881881703,0.376184612512589,0.37624353170394897,0.36082353430541397,0.33078934880102701,0.38777803958642998,0.39112115842661699,0.399339806540631,0.31623765760267403,0.40811645889841602]
["CN-E1L204C1","CN",1,"E1L204C1",106,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",3.1555671244859702E-2,4.7058993950486201E-3,7.6534799300134199E-3,8.01829993724823E-3,6.6333217546343803E-3,5.3864191286265902E-3,5.3146639838814701E-3,5.8774179778993104E-3,8.5590789094567299E-3,1.10576947673481E-2,1.2734659750969201E-2,1.424107572523E-2,1.1860792482238799E-2,1.4134862829935899E-2,1.1485601177082401E-2,1.0380349047659301E-2]
["CN-E1L204C2","CN",1,"E1L204C2",107,"CM(R), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",1.2475459836423401E-2,-1.47519577294588E-2,7.5672711245715601E-3,1.9125858321785899E-2,1.8282119184732399E-2,2.48017925769091E-2,2.88469865918159E-2,2.1971188485622399E-2,2.0220270380377801E-2,4.3239858246807199E-2,3.1777325362661202E-2,1.5525707786634001E-2,1.42470745663621E-2,2.80118498353636E-2,4.1639777239979602E-2,3.5924043520599101E-2]
["CN-E1L204C3","CN",1,"E1L204C3",108,"CM(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",3.5903286188840901E-2,4.0961675345897702E-2,1.3689617626368999E-3,2.2996660321950899E-2,2.46822647750378E-2,2.1142881363630298E-2,2.6452349498867999E-2,2.0001418888568899E-2,1.68673023581505E-2,1.31673134528816E-2,1.31279788410609E-2,1.7078547833828301E-2,1.09469351198549E-2,2.6161026337109199E-2,2.34591827923099E-2,2.5749510904295302E-2]
["CN-E1L204C4","CN",1,"E1L204C4",109,"CM(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",8.2044735550880404E-2,1.2235330417752301E-2,1.9899025559425399E-2,2.0847586914897E-2,1.7246630042791401E-2,1.40046821907163E-2,1.3818135485053101E-2,1.5281268395483501E-2,2.22536083310843E-2,2.87500063951051E-2,3.3110115352520002E-2,3.7026796885597901E-2,3.0838060453820901E-2,3.6750643357833297E-2,2.98625630604142E-2,2.6988907523914099E-2]
["CN-E1L204C5","CN",1,"E1L204C5",110,"CM(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",3.2436180859804202E-2,-3.8355156779289197E-2,1.9674902781844101E-2,4.9727205187082298E-2,4.7533519566059099E-2,6.4484663307666806E-2,7.5002089142799405E-2,5.71250654757023E-2,5.2572682499885601E-2,0.11242363144169901,8.2621045942919094E-2,4.0366840245248399E-2,3.7042393872541497E-2,7.2830809571945307E-2,0.10826342082394699,9.3402513153557506E-2]
["CN-E1L204C6","CN",1,"E1L204C6",111,"CM(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",9.3348503112792997E-2,0.10650067031383501,3.5592962522059701E-3,5.9791274368762998E-2,6.4173944294452695E-2,5.49715869128704E-2,6.8775966763496399E-2,5.2003622055053697E-2,4.3854977935552597E-2,3.4235014977492199E-2,3.41327449867583E-2,4.44042243679535E-2,2.84620313116229E-2,6.8018668476483801E-2,6.0993875260005603E-2,6.6948728351167802E-2]
["CN-E1L204C7","CN",1,"E1L204C7",112,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",1.82581186294556,0.68442249298095703,0.874717116355896,0.77571302652358998,0.60023725032806396,0.55927485227584794,0.68910485506057695,0.72825580835342396,0.59054422378539995,0.51118548073173098,0.44893705370176101,0.48958224565854003,0.40990930445477802,0.52294114900578204,0.39321287575681901,0.35642101796914799]
["CN-E1L204C8","CN",1,"E1L204C8",113,"CD(R), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",3.3540775775909402,-3.6623234748840301,1.1222463846206701,4.3334307670593297,9.3430061340331996,10.633074760436999,21.594667434692401,11.489382743835399,1.82263267040253,2.5560799923447601,2.2385933296685798,3.19791719979635,0.995428357897998,5.7778078742678698,5.26879944317536,4.6312981098049502]
["CN-E1L204C9","CN",1,"E1L204C9",114,"CD(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",7.5152449607849103,10.0548753738403,0.175754204392433,2.7622141838073699,3.9091210365295401,4.3048133850097701,6.4502911567687997,2.9314305782318102,1.04914963245392,0.65996770147226003,0.60713339676941203,1.06112344356646,0.55257964592728903,1.47651531261323,1.0888299800543599,1.31861058415556]
["CN-E1L204C10","CN",1,"E1L204C10",115,"CD(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",1.82581162452698,0.68442243337631203,0.87471717596054099,0.77571302652358998,0.60023725032806396,0.55927479267120395,0.68910491466522195,0.72825580835342396,0.59054422378539995,0.51118548073173098,0.44893705370176101,0.48958224565854003,0.40990930445477802,0.52294114900578204,0.39321287575681801,0.35642101796914799]
[{"$f":"B1090&\"-\"&D1090","v":"CN-E1L204C11"},"CN",1,"E1L204C11",116,"CD(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",3.3540785312652601,-3.6623234748840301,1.1222465038299601,4.3334307670593297,9.3430061340331996,10.633074760436999,21.594669342041001,11.489382743835399,1.82263267040253,2.5560799923447601,2.2385933296685798,3.19791719979635,0.995428357897998,5.7778078742678698,5.26879944317536,4.6312981098049502]
["CN-E1L204C12","CN",1,"E1L204C12",117,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",7.5152459144592303,10.0548763275146,0.175754219293594,2.7622144222259499,3.9091212749481201,4.3048138618469203,6.4502906799316397,2.9314305782318102,1.04914963245392,0.65996770147226003,0.60713339676941203,1.06112344356646,0.55257964592728903,1.47651531261323,1.0888299800543599,1.31861058415556]
["CN-E1L204C13","CN",1,"E1L204C13",118,"CM(R), DRL Expense, Privately-Owned, GONDOLA - PLAIN",7.3050484061241202E-3,1.0580310598015801E-2,5.5069490335881701E-3,4.89917350932956E-3,7.3880883865058396E-3,1.1993658728897599E-2,1.8720937892794599E-2,1.6588695347309099E-2,1.26703837886453E-2,9.4889635688472605E-3,1.1233679496449499E-2,2.1578816897233101E-2,3.4732193852660201E-2,1.9384797689181599E-2,1.2236948144360899E-2,1.62739587228855E-2]
["CN-E1L205C1","CN",1,"E1L205C1",119,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",3.2223474234342603E-2,3.7258822470903397E-2,4.0058746933937101E-2,4.5676842331886298E-2,4.3399766087532002E-2,3.7453163415193599E-2,3.2542709261178998E-2,3.0515020713210099E-2,3.8066897541284603E-2,5.28716925181359E-2,6.6907513473381294E-2,7.5761855958489194E-2,6.9886417941279505E-2,8.0393941231365201E-2,7.3849953624047199E-2,5.8219297730652798E-2]
["CN-E1L205C2","CN",1,"E1L205C2",120,"CM(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",-1.8951855599880201E-2,1.27828621771187E-3,-8.61333217471838E-3,1.5498853288590899E-2,-7.5524696148931997E-3,-3.96774522960186E-3,9.4634275883436203E-3,1.6113480553030999E-2,3.8287895731627902E-3,1.94155072510637E-2,4.6223118941277799E-2,1.9116667723722499E-2,8.6564595679434701E-3,2.1900779449050601E-2,4.53707597216104E-2,7.8057317507545604E-2]
["CN-E1L205C3","CN",1,"E1L205C3",121,"CM(R), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",7.5534626841545105E-2,9.6602857112884494E-2,9.2111088335514096E-2,0.13903144001960799,7.9658947885036496E-2,7.0590928196907002E-2,7.0331692695617704E-2,7.5893759727478E-2,7.1871355175971999E-2,7.5368378437095498E-2,9.4872088544030606E-2,9.8392005144906994E-2,0.107339808009943,8.4347119511669497E-2,8.0765014090158002E-2,7.8764510549626104E-2]
["CN-E1L205C4","CN",1,"E1L205C4",122,"CM(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",8.3781152963638306E-2,9.6872843801975306E-2,0.104152634739876,0.118759781122208,0.112839438021183,9.7378142178058597E-2,8.4611080586910206E-2,7.9338975250721006E-2,9.8973952233791407E-2,0.13746640054715401,0.17395953503079101,0.19698082549207199,0.181704686647327,0.209024247201549,0.19200987942252301,0.151370174099697]
["CN-E1L205C5","CN",1,"E1L205C5",123,"CM(Y), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",-4.9274839460849797E-2,3.3235726878046998E-3,-2.2394640371203402E-2,4.0296982973813997E-2,-1.9636465236544599E-2,-1.03160953149199E-2,2.4604897946119302E-2,4.1894983500242199E-2,9.9548632279038395E-3,5.0480318852765299E-2,0.120180109247322,4.9703336081678401E-2,2.25067948766529E-2,5.6942026567531702E-2,0.117963975276187,0.20294902551961899]
["CN-E1L205C6","CN",1,"E1L205C6",124,"CM(Y), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",0.19638997316360499,0.25116732716560403,0.23948901891708399,0.36148157715797402,0.207113221287727,0.18353660404682201,0.18286235630512199,0.197323799133301,0.18686558306217199,0.195957783936449,0.24666743021447901,0.255819213376759,0.27908350082585098,0.21930251073034099,0.20998903663441101,0.20478772742902801]
["CN-E1L205C7","CN",1,"E1L205C7",125,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",3.1912994384765598,3.9437527656555198,4.3872437477111799,5.0508384704589799,4.8780441284179696,3.64366555213928,2.9310605525970499,2.7186307907104501,3.4539833068847701,5.1153079986750303,6.1521391345803398,6.8537146865901502,5.74791857970206,6.4530247117466999,5.7609361011281104,4.6625528083824497]
["CN-E1L205C8","CN",1,"E1L205C8",126,"CD(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",-2.8107590675353999,0.291748136281967,1.1345747709274301,1.3455284833908101,5.7166695594787598,6.3106460571289098,8.4212141036987305,17.329605102539102,5.8807916641235396,15.183789029022501,22.170386365094,14.1676385325587,15.353111590434199,5.1902356286689102,9.2654807595191002,18.001969193387701]
["CN-E1L205C9","CN",1,"E1L205C9",127,"CD(R), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",12.223059654235801,15.494524955749499,15.5853614807129,23.027439117431602,13.0693063735962,8.8224029541015607,8.7562522888183594,11.6806488037109,9.4286117553710902,11.1490587003453,12.4508772432981,12.133251948080799,12.351660456676999,10.1934728079087,9.0603166179725694,9.7668143980337607]
["CN-E1L205C10","CN",1,"E1L205C10",128,"CD(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",3.1912994384765598,3.9437527656555198,4.3872432708740199,5.0508384704589799,4.8780436515808097,3.64366507530212,2.9310605525970499,2.7186307907104501,3.4539828300476101,5.1153079986750303,6.1521391345803398,6.8537146865901502,5.7479185797020502,6.4530247117466999,5.7609361011281104,4.6625528083824497]
["CN-E1L205C11","CN",1,"E1L205C11",129,"CD(Y), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",-2.8107595443725599,0.291748136281967,1.1345742940902701,1.3455284833908101,5.7166700363159197,6.3106460571289098,8.4212150573730504,17.329605102539102,5.8807907104492196,15.183789029022501,22.170386365094,14.1676385325587,15.353111590434199,5.1902356286689102,9.2654807595191002,18.001969193387701]
["CN-E1L205C12","CN",1,"E1L205C12",130,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",12.2230577468872,15.494524955749499,15.5853633880615,23.027439117431602,13.069307327270501,8.8224039077758807,8.7562522888183594,11.6806478500366,9.4286108016967791,11.1490587003453,12.4508772432981,12.133251948080799,12.351660456676999,10.1934728079087,9.0603166179725694,9.7668143980337607]
["CN-E1L205C13","CN",1,"E1L205C13",131,"CM(R), DRL Expense, Privately-Owned, GONDOLA - EQUIPPED",2.7681680876412398E-5,1.2088873190805301E-3,4.8591810627840497E-4,6.5039440989494296E-2,4.0155090391635902E-2,1.9341140985488899E-2,1.9931390881538402E-2,1.9820811226964E-2,2.3809771984815601E-2,3.0376113618873601E-2,2.01543513424523E-2,1.23657013363603E-2,3.7489955819157098E-3,4.4740396217598502E-4,1.3307655451925699E-3,1.32370543706512E-4]
["CN-E1L206C1","CN",1,"E1L206C1",132,"CM(R), OPR Expense, Railroad-Owned, HOPPER - COVERED",2.68092956393957E-2,2.7023397386074101E-2,2.8333751484751701E-2,3.4886792302131701E-2,3.7628218531608602E-2,4.0071085095405599E-2,3.9007551968097701E-2,3.9854642003774601E-2,4.96001839637756E-2,6.6193266390617705E-2,7.8376393622037993E-2,8.6183900906708799E-2,7.4275365559485301E-2,8.0034629605131996E-2,7.0686194560006896E-2,5.45424145343371E-2]
["CN-E1L206C2","CN",1,"E1L206C2",133,"CM(R), DRL Expense, Railroad-Owned, HOPPER - COVERED",-6.8165436387062099E-3,-4.6684481203556104E-3,-3.9030851330608099E-3,-1.0611210949719001E-2,-7.1778935380280001E-3,8.0192759633064305E-3,-9.3267345800995792E-3,3.8807024247944398E-3,9.7582284361124004E-3,3.8220392377562501E-2,3.6257332994088502E-2,4.1426403741800302E-2,3.3831676466112903E-2,3.2631081323318302E-2,3.2632427513858801E-2,3.1895116906702298E-2]
["CN-E1L206C3","CN",1,"E1L206C3",134,"CM(R), ROI Expense, Railroad-Owned, HOPPER - COVERED",1.0416442528366999E-2,1.8041420727968199E-2,1.51688866317272E-2,6.4251609146595001E-2,5.5510003119707101E-2,6.7066036164760603E-2,7.2663299739360795E-2,6.6065587103366893E-2,5.9338465332984897E-2,5.8742893832074802E-2,5.9230038528924098E-2,6.6883858328149498E-2,9.2572372892428104E-2,5.37937969813558E-2,3.9532095325365203E-2,4.51830155794853E-2]
["CN-E1L206C4","CN",1,"E1L206C4",135,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",6.9704070687294006E-2,7.0260807871818501E-2,7.3667667806148501E-2,9.0705566108226804E-2,9.7833283245563493E-2,0.10418489575386,0.101419515907764,0.103622145950794,0.128960475325584,0.17210249261560601,0.20377862341729899,0.224078142357443,0.19311595045466201,0.208090036973343,0.18378410585601801,0.14181027778927599]
["CN-E1L206C5","CN",1,"E1L206C5",136,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",-1.7723057419061699E-2,-1.2137951329350499E-2,-1.0148014873266199E-2,-2.7589112520217899E-2,-1.8662564456462898E-2,2.0850202068686499E-2,-2.4249386042356501E-2,1.00897792726755E-2,2.5371354073286102E-2,9.9373020181662497E-2,9.4269065784629999E-2,0.10770864972868099,8.7962358811893904E-2,8.4840811440627995E-2,8.4844311536033307E-2,8.2927303957426299E-2]
["CN-E1L206C6","CN",1,"E1L206C6",137,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED",2.7082785964012101E-2,4.6907700598239899E-2,3.9439097046852098E-2,0.16705411672592199,0.144326061010361,0.17437176406383501,0.18892429769039201,0.17177067697048201,0.15427987277507799,0.15273152396339401,0.15399810017520299,0.17389803165318801,0.24068816952031399,0.13986387215152499,0.10278344784595,0.117475840506662]
["CN-E1L206C7","CN",1,"E1L206C7",138,"CD(R), OPR Expense, Railroad-Owned, HOPPER - COVERED",2.6973421573638898,2.90674924850464,3.1843521595001198,3.99644899368286,4.3290448188781703,4.5238008499145499,4.1114058494567898,4.0290026664733896,4.91867876052856,6.6236140928059504,7.8785436682360297,8.7194088699035905,7.8376916648142201,8.5134124189535196,7.4882101310611704,5.7064953718181002]
["CN-E1L206C8","CN",1,"E1L206C8",139,"CD(R), DRL Expense, Railroad-Owned, HOPPER - COVERED",5.9409642219543501,6.76635646820068,10.4346723556519,18.4113063812256,13.6351871490479,11.010827064514199,7.1509070396423304,5.6971931457519496,2.38539814949036,8.52683352700158,8.9517868592884593,7.6946168856878199,6.7217445149667698,8.3522045276598504,5.1616180139201502,7.9929101345361904]
["CN-E1L206C9","CN",1,"E1L206C9",140,"CD(R), ROI Expense, Railroad-Owned, HOPPER - COVERED",1.7256770133972199,2.9926183223724401,2.5493946075439502,11.436302185058601,9.2832489013671893,10.7860622406006,10.3094320297241,9.8272542953491193,9.0631656646728498,8.4597466678696591,8.9194279785595096,10.536164758185601,15.0561209872783,8.3191070349884892,6.1248877632115102,7.0124324172544998]
["CN-E1L206C10","CN",1,"E1L206C10",141,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",2.6973416805267298,2.90674924850464,3.1843523979186998,3.99644923210144,4.3290457725524902,4.5238013267517099,4.1114058494567898,4.0290031433105504,4.91867876052856,6.6236140928059504,7.8785436682360297,8.7194088699035905,7.8376916648142201,8.5134124189535196,7.4882101310611704,5.7064953718181002]
["CN-E1L206C11","CN",1,"E1L206C11",142,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",5.9409651756286603,6.76635694503784,10.4346723556519,18.4113063812256,13.6351871490479,11.010827064514199,7.1509060859680202,5.6971936225891104,2.3854000568389901,8.52683352700158,8.9517868592884593,7.6946168856878296,6.7217445149667698,8.3522045276598504,5.1616180139201502,7.9929101345361904]
["CN-E1L206C12","CN",1,"E1L206C12",143,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED",1.7256770133972199,2.9926183223724401,2.5493946075439502,11.436302185058601,9.2832489013671893,10.7860612869263,10.309431076049799,9.8272542953491193,9.0631656646728498,8.4597466678696591,8.9194279785595096,10.536164758185601,15.0561209872783,8.3191070349884892,6.1248877632115102,7.0124324172544998]
["CN-E1L206C13","CN",1,"E1L206C13",144,"CM(R), DRL Expense, Privately-Owned, HOPPER - COVERED",1.0340888053178799E-2,2.4269528221339E-3,1.1334272101521501E-2,9.4122616574168205E-3,8.8882641866803204E-3,8.5460711270570807E-3,7.2155962698161602E-3,6.9728265516459898E-3,8.0031184479594196E-3,7.8057148078771402E-3,9.3297662181765894E-3,6.4846065687761802E-3,6.1323004028371103E-3,5.7767179958993203E-3,3.7107158862655001E-6,5.8599081772374902E-5]
["CN-E1L207C1","CN",1,"E1L207C1",145,"CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.71593986451626E-2,1.8918264657259001E-2,3.1705420464277302E-2,4.2887959629297298E-2,4.3298739939928103E-2,3.3869761973619503E-2,3.1564265489578198E-2,2.6683161035180099E-2,3.9537589997053098E-2,5.4453738507568503E-2,6.9506245961142299E-2,8.9234972053826106E-2,9.9582904669238401E-2,0.106075912755749,7.5439546668737506E-2,3.1278033450843297E-2]
["CN-E1L207C2","CN",1,"E1L207C2",146,"CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",-1.94702688604593E-2,3.3412586897611597E-2,2.8896925970912E-2,5.4621681571006803E-2,6.9267489016056102E-2,0.14050488173961601,0.161858409643173,0.14917224645614599,0.164068788290024,0.253089303612615,0.283278688961971,0.27290567951502198,0.24569763233604999,0.37431853675378302,0.40599371708881299,0.18469888367033699]
["CN-E1L207C3","CN",1,"E1L207C3",147,"CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",7.3338657617568997E-2,0.15672138333320601,0.164950892329216,0.19831348955631301,0.25692981481552102,0.36160379648208602,0.36809009313583402,0.31607779860496499,0.27870780229568498,0.29516842150334599,0.31466765751517201,0.33197744781713701,0.38108694627485601,0.37159501473141299,0.29347162085724099,0.19045964239945001]
["CN-E1L207C4","CN",1,"E1L207C4",148,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",4.46144342422485E-2,4.9187488853931399E-2,8.2434058189392104E-2,0.11150867491960501,0.112576693296432,8.8061414659023299E-2,8.2067072391509996E-2,6.9376192986965193E-2,0.102797776460648,0.14157972011967801,0.18071623949897,0.23201092733994799,0.25891555214001999,0.27579737316494601,0.19614282133871799,8.1322886972192601E-2]
["CN-E1L207C5","CN",1,"E1L207C5",149,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",-5.0622686743736302E-2,8.6872734129428905E-2,7.5131990015506703E-2,0.142016306519508,0.18009553849697099,0.36531269550323497,0.42083168029785201,0.38784766197204601,0.42657881975174,0.65803218939279895,0.73652459130112502,0.70955476673905804,0.63881384407372999,0.97322819555983697,1.05558366443091,0.480217097542877]
["CN-E1L207C6","CN",1,"E1L207C6",150,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",0.19068051874637601,0.40747556090354897,0.42887225747108498,0.51561486721038796,0.66801786422729503,0.94016975164413497,0.95703381299972501,0.821802258491516,0.72464013099670399,0.76743789590869904,0.81813590953944704,0.86314136432455801,0.99082606031462594,0.96614703830167503,0.76302621422882799,0.49519507023857101]
["CN-E1L207C7","CN",1,"E1L207C7",151,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",0.74377697706222501,0.71110743284225497,1.1704194545745801,1.4973344802856401,1.5188738107681301,1.1235615015029901,1.0344929695129399,0.89189922809600797,1.3710128068923999,1.9330589781678,2.4286159123274,3.0048618505925,3.36415275145476,3.6008123354900801,2.5764295178917198,1.3191418577888301]
["CN-E1L207C8","CN",1,"E1L207C8",152,"CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.6743465662002599,3.7753057479858398,2.7725980281829798,4.4975962638854998,7.4332566261291504,11.014362335205099,12.8359575271606,12.971737861633301,12.114702224731399,17.1651194631777,19.675466456843701,18.178285542459701,19.837199808024799,25.223979030828801,29.066597111811099,21.846697875927099]
["CN-E1L207C9","CN",1,"E1L207C9",153,"CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",4.2243852615356401,7.9773483276367196,9.3050298690795898,9.7253437042236293,13.1022901535034,17.711277008056602,17.333971023559599,17.142438888549801,15.2011833190918,14.833444579815,16.249155486239101,16.414199723616299,19.3087252351316,19.588992679135501,14.6736841977397,16.080803155197]
["CN-E1L207C10","CN",1,"E1L207C10",154,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",0.74377691745758101,0.71110755205154397,1.1704193353653001,1.4973344802856401,1.5188738107681301,1.1235613822937001,1.0344928503036499,0.89189922809600797,1.3710125684738199,1.9330589781678,2.4286159123274,3.0048618505925,3.36415275145476,3.6008123354900801,2.5764295178917198,1.3191418577888301]
["CN-E1L207C11","CN",1,"E1L207C11",155,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.6743465662002599,3.7753057479858398,2.7725977897643999,4.4975962638854998,7.4332566261291504,11.014362335205099,12.8359575271606,12.971738815307599,12.114703178405801,17.1651194631777,19.675466456843701,18.178285542459701,19.837199808024799,25.223979030828801,29.066597111811099,21.846697875927099]
["CN-E1L207C12","CN",1,"E1L207C12",156,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",4.2243852615356401,7.9773488044738796,9.3050298690795898,9.7253437042236293,13.1022891998291,17.711277008056602,17.333969116210898,17.142440795898398,15.201185226440399,14.833444579815,16.249155486239101,16.414199723616299,19.3087252351316,19.588992679135501,14.6736841977397,16.080803155197]
["CN-E1L207C13","CN",1,"E1L207C13",157,"CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - GENERAL",2.1721285520470701E-5,3.9766197005519603E-5,2.9689277653233101E-5,4.5204865746200102E-3,1.31279621273279E-2,3.69827798567712E-3,4.7192615456879104E-3,7.0771803148090796E-3,4.8595215193927297E-3,4.7397135280318999E-3,4.31395714574894E-3,1.64065537815164E-3,9.3327893101443E-4,1.38157796186714E-4,1.4640909045006899E-5,6.1360996982716104E-6]
["CN-E1L208C1","CN",1,"E1L208C1",158,"CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.97162572294474E-2,1.6947301104664799E-2,2.2519320249557499E-2,2.8741832822561299E-2,2.4880360811948801E-2,2.15558614581823E-2,1.4585107564926101E-2,1.23328668996692E-2,1.2314778752625001E-2,1.9263527710230901E-2,2.8574073438845399E-2,3.9305786424742098E-2,3.5925998655338798E-2,3.82889450116497E-2,3.6505544844238999E-2,3.6959992271891902E-2]
["CN-E1L208C2","CN",1,"E1L208C2",159,"CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",3.2221430446952599E-3,5.1244110800325897E-3,5.7901823893189404E-3,4.3431059457361698E-3,2.5268159806728402E-3,1.6103028319776099E-3,2.5669324677437501E-3,2.0978625398129199E-3,2.0300133619457501E-3,4.0132686662587898E-3,3.34414319092162E-3,2.92649117723394E-3,2.9854075237222598E-3,2.6920730743257401E-3,3.1659826027143202E-3,6.1487842959094601E-3]
["CN-E1L208C3","CN",1,"E1L208C3",160,"CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",6.7161391489207701E-3,9.0602822601795197E-3,9.8089855164289492E-3,5.0108660943806197E-3,2.3166611790657E-3,3.1919768080115301E-3,3.4648401197045998E-3,2.90437135845423E-3,2.6275499258190402E-3,2.9353807864017198E-3,2.60308816945052E-3,2.5903565606676701E-3,2.9025453919051601E-3,2.01380508237708E-3,1.6900647307968701E-3,1.6794808599557699E-3]
["CN-E1L208C4","CN",1,"E1L208C4",161,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",5.1262278109788902E-2,4.4062975794076899E-2,5.85502199828625E-2,7.4728779494762407E-2,6.4688928425312001E-2,5.6045241653919199E-2,3.7921275943517699E-2,3.2065443694591501E-2,3.2018430531024898E-2,5.0085172046600498E-2,7.4292590940998104E-2,0.102195044704329,9.3407596503880794E-2,9.9551257030289206E-2,9.4914416595021395E-2,9.6095979906918996E-2]
["CN-E1L208C5","CN",1,"E1L208C5",162,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",8.3775697275996208E-3,1.33234681561589E-2,1.50544662028551E-2,1.1292074806988199E-2,6.5697198733687401E-3,4.1867867112159703E-3,6.6740233451127997E-3,5.4544429294765004E-3,5.2780346013605603E-3,1.0434498532272799E-2,8.6947722963961905E-3,7.6088770608082404E-3,7.76205956167787E-3,6.99938999324693E-3,8.2315547670572392E-3,1.5986839169364601E-2]
["CN-E1L208C6","CN",1,"E1L208C6",163,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.74619592726231E-2,2.35567316412926E-2,2.55033541470766E-2,1.30282528698444E-2,6.0233175754547102E-3,8.2991402596235293E-3,9.0085836127400398E-3,7.5513673946261397E-3,6.8316296674311196E-3,7.6319900446444799E-3,6.7680292405713398E-3,6.7349270577359496E-3,7.5466180189534297E-3,5.2358932141804001E-3,4.3941683000718601E-3,4.36665023588501E-3]
["CN-E1L208C7","CN",1,"E1L208C7",164,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.54301524162292503,0.43812796473503102,0.540813207626343,0.61137580871581998,0.46691635251045199,0.37336677312851002,0.24576824903488201,0.20998091995716101,0.212221398949623,0.34833543968630598,0.52925128146133005,0.69999720612572003,0.62510622149778095,0.63063735739168902,0.586994594634202,0.607549475442551]
["CN-E1L208C8","CN",1,"E1L208C8",165,"CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.83975744247436501,0.52253115177154497,0.43875488638877902,0.33197647333145103,0.400358617305756,0.28532388806343101,0.36270821094512901,0.47105249762535101,0.39009025692939803,0.633869803472078,0.52828947564851103,0.404874299306832,0.69106002565029501,0.491353602833769,0.62075323525472603,0.57082486794876597]
["CN-E1L208C9","CN",1,"E1L208C9",166,"CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.244927793741226,0.32201558351516701,0.33702313899993902,0.11511249095201501,5.42553924024105E-2,8.0152474343776703E-2,7.5713872909545898E-2,7.43216201663017E-2,7.0371478796005194E-2,7.4182033884101203E-2,6.8943413562114794E-2,5.8057959007558099E-2,6.2734846759102098E-2,4.10128307960623E-2,3.1975017170781501E-2,3.5207551965792498E-2]
["CN-E1L208C10","CN",1,"E1L208C10",167,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.54301524162292503,0.43812790513038602,0.540813207626343,0.61137580871581998,0.46691635251045199,0.37336680293083202,0.24576824903488201,0.20998091995716101,0.212221398949623,0.34833543968630598,0.52925128146133005,0.69999720612572003,0.62510622149777995,0.63063735739168902,0.586994594634202,0.607549475442551]
["CN-E1L208C11","CN",1,"E1L208C11",168,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.83975744247436501,0.52253115177154497,0.43875485658645602,0.33197647333145103,0.400358617305756,0.28532388806343101,0.36270821094512901,0.47105249762535101,0.39009025692939803,0.633869803472078,0.52828947564851103,0.404874299306832,0.69106002565029501,0.491353602833769,0.62075323525472603,0.57082486794876597]
["CN-E1L208C12","CN",1,"E1L208C12",169,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.244927793741226,0.32201558351516701,0.33702313899993902,0.11511249095201501,5.42553924024105E-2,8.0152474343776703E-2,7.5713865458965302E-2,7.4321612715721103E-2,7.0371471345424694E-2,7.4182033884101203E-2,6.8943413562114794E-2,5.8057959007558099E-2,6.2734846759102195E-2,4.10128307960623E-2,3.1975017170781501E-2,3.5207551965792498E-2]
["CN-E1L208C13","CN",1,"E1L208C13",170,"CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - SPECIAL",4.7244720917660701E-6,9.9036760730086792E-6,7.2794355219230098E-6,8.2155445124953996E-4,5.1881329454772598E-6,1.3324297469807799E-6,4.9811533244792399E-5,3.08459675579797E-5,5.2639719797298301E-4,6.5708676698200698E-6,3.9152668947337397E-6,1.8120022004226901E-6,1.9008679556000599E-6,6.1782877190938502E-6,9.9605842709842395E-6,5.3202893594181596E-6]
["CN-E1L209C1","CN",1,"E1L209C1",171,"CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",2.5552952662110301E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L209C2","CN",1,"E1L209C2",172,"CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",1.2967680231668101E-4,0,0.122301578521729,0.119849376380444,0.12322008609771699,0.117113657295704,0.14109423756599401,0.121675968170166,0.12330192327499399,0.119061254809878,0.122734506603182,0.119160204695554,0.111940862886571,0.11937149936314,0.13053015129989301,0.117383635369468]
["CN-E1L209C3","CN",1,"E1L209C3",173,"CM(R), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",3.08651942759752E-4,0,0,-8.8177919678855701E-5,6.3574709929525896E-4,-1.07936844869982E-4,-1.5951710520312201E-4,-1.63863733178005E-4,-1.6412441618740599E-4,-1.93730203276652E-4,-2.3384950086121299E-4,-3.7874839593153798E-4,-4.2145424363865502E-4,-3.38020518415039E-4,-4.5754873247693301E-4,-4.2015379438076401E-4]
["CN-E1L209C4","CN",1,"E1L209C4",174,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",6.6437676548957797E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L209C5","CN",1,"E1L209C5",175,"CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",3.3715966856107099E-4,0,0.31798410415649397,0.31160831451415999,0.32037189602851901,0.30449545383453402,0.36684504151344299,0.31635734438896201,0.32058522105217002,0.309559262505684,0.31910971716827202,0.30981653220844002,0.29104624350508601,0.310365898344165,0.33937839337972098,0.30519745196061698]
["CN-E1L209C6","CN",1,"E1L209C6",176,"CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",8.0249522579833898E-4,0,0,-2.2926254314370499E-4,1.6529408749193001E-3,-2.80635751551017E-4,-4.1474465979263197E-4,-4.2604576447047299E-4,-4.2672341805882801E-4,-5.0369852851929605E-4,-6.0800870223915295E-4,-9.8474582942199699E-4,-1.0957810334605001E-3,-8.7885334787910104E-4,-1.18962670444003E-3,-1.0923998653899899E-3]
["CN-E1L209C7","CN",1,"E1L209C7",177,"CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",1.94050776958466,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L209C8","CN",1,"E1L209C8",178,"CD(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",9.1132018715143204E-3,0,43.314327239990199,37.090885162353501,37.999324798583999,41.5166015625,37.817668914794901,32.334136962890597,36.381877899169901,38.003983783089602,37.208844671971001,35.638833928117798,43.142013579354703,35.197436525200303,100.208397756672,120.420189041543]
["CN-E1L209C9","CN",1,"E1L209C9",179,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",2.1690905094146701E-2,0,0,-7.9676583409309405E-3,5.8252882212400402E-2,-1.1019869707524801E-2,-1.52828451246023E-2,-1.8058408051729199E-2,-1.7574349418282498E-2,-1.92514780072305E-2,-2.4909073831063E-2,-4.8547432008980498E-2,-5.8010173003322903E-2,-5.0966321640570501E-2,-5.72709075265957E-2,-4.9440827286919301E-2]
[{"$f":"B1154&\"-\"&D1154","v":"CN-E1L209C10"},"CN",1,"E1L209C10",180,"CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",1.94050753116608,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L209C11","CN",1,"E1L209C11",181,"CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",9.1132018715143204E-3,0,43.314327239990199,37.090885162353501,37.999324798583999,41.5166015625,37.817672729492202,32.334136962890597,36.381881713867202,38.003983783089701,37.208844671971001,35.638833928117798,43.142013579354703,35.197436525200303,100.208397756672,120.420189041543]
["CN-E1L209C12","CN",1,"E1L209C12",182,"CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",2.1690905094146701E-2,0,0,-7.9676583409309405E-3,5.8252874761819798E-2,-1.10198687762022E-2,-1.5282846055924899E-2,-1.80584099143744E-2,-1.75743531435728E-2,-1.92514780072305E-2,-2.4909073831063E-2,-4.8547432008980401E-2,-5.8010173003322903E-2,-5.0966321640570501E-2,-5.72709075265957E-2,-4.9440827286919301E-2]
["CN-E1L209C13","CN",1,"E1L209C13",183,"CM(R), DRL Expense, Privately-Owned, REFRIGERATED - MECH",3.92394373193383E-4,1.9144187681376899E-3,3.21391550824046E-3,2.9502232791855899E-4,1.0566678829491099E-3,6.8260938860475995E-4,9.5976237207651095E-4,3.7110046832822301E-4,9.7113649826496796E-4,7.4394550194554598E-4,6.9312261815133102E-4,5.9341738169993604E-4,1.1951431420817399E-3,5.7960871542505797E-4,5.6582100242543799E-4,7.0977038093725004E-4]
["CN-E1L210C1","CN",1,"E1L210C1",184,"CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",1.86767242848873E-2,3.0000962316989899E-2,1.19914710521698E-2,3.86828696355224E-3,2.7874612715095299E-3,9.2744285939261296E-4,0,0,0,0,0,0,0,0,0,0]
["CN-E1L210C2","CN",1,"E1L210C2",185,"CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",0.14847947657108301,0.39059561491012601,0.171666979789734,9.5127455890178694E-2,8.4450721740722698E-2,0.10105846822261801,0.116871178150177,0.116613134741783,0.14056019484996801,0.82716476881693202,1.4276203897616699,1.93019537866764,0.75627464645450804,2.04491827470902,3.3504339075518801,1.41399738679278]
["CN-E1L210C3","CN",1,"E1L210C3",186,"CM(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",5.5007673799991601E-2,0.243972212076187,0.23848955333232899,0.22082705795764901,3.0881265178322799E-2,0.309002965688705,0.43739441037178001,0.40679907798767101,0.50400465726852395,0.50266343561528104,0.72652203906572299,1.0300611979110601,0.43490445896373098,0.75574193746827301,0.80451655188966198,0.42501550176620501]
["CN-E1L210C4","CN",1,"E1L210C4",187,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",4.8559390008449603E-2,7.8002467751503005E-2,3.1177796423435201E-2,1.0057554580271201E-2,7.2474069893360103E-3,2.4113499093800801E-3,0,0,0,0,0,0,0,0,0,0]
["CN-E1L210C5","CN",1,"E1L210C5",188,"CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",0.38604611158370999,1.01554787158966,0.44633418321609503,0.24733145534992201,0.219571813941002,0.26275190711021401,0.30386507511138899,0.30319404602050798,0.36545655131339999,2.1506283989240198,3.71181301338035,5.0185079845358702,1.9663140807817201,5.31678751424346,8.7111281596348995,3.6763932056612201]
["CN-E1L210C6","CN",1,"E1L210C6",189,"CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",0.14301979541778601,0.63432675600051902,0.62007266283035301,0.57415056228637695,8.0291241407394395E-2,0.80340737104415905,1.1372258663177499,1.0576757192611701,1.3104113340377801,1.3069249325997301,1.88895730157089,2.6781591145687602,1.1307515933057,1.9649290374175099,2.0917430349131299,1.10504030459213]
["CN-E1L210C7","CN",1,"E1L210C7",190,"CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",2.11828708648682,3.6296830177307098,1.5025056600570701,0.50294446945190396,0.35775679349899298,0.13580358028411901,0,0,0,0,0,0,0,0,0,0]
["CN-E1L210C8","CN",1,"E1L210C8",191,"CD(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",73.150459289550795,170.71624755859401,38.910068511962898,35.658607482910199,22.918998718261701,27.134191513061499,34.446277618408203,36.034374237060497,33.687980651855497,160.4172709961,279.09357597369802,319.796020603523,50.378590282871897,239.75672071113601,606.97848272516501,251.08374925444599]
["CN-E1L210C9","CN",1,"E1L210C9",192,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",10.4422750473022,52.024646759033203,35.730438232421903,52.714389801025398,6.4629936218261701,56.654338836669901,83.290855407714801,77.551322937011705,80.087890625,89.798044315842205,138.764293207218,165.95861812736501,25.016443190601802,100.417500730059,145.32536670557201,73.910773743663896]
["CN-E1L210C10","CN",1,"E1L210C10",193,"CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",2.11828708648682,3.6296830177307098,1.5025056600570701,0.50294446945190396,0.35775673389434798,0.13580358028411901,0,0,0,0,0,0,0,0,0,0]
["CN-E1L210C11","CN",1,"E1L210C11",194,"CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",73.150466918945298,170.71624755859401,38.910068511962898,35.658611297607401,22.9189968109131,27.134189605712901,34.446277618408203,36.034378051757798,33.687980651855497,160.4172709961,279.09357597369802,319.796020603523,50.378590282871897,239.75672071113601,606.97848272516501,251.08374925444599]
["CN-E1L210C12","CN",1,"E1L210C12",195,"CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",10.4422760009766,52.024650573730497,35.730442047119098,52.714389801025398,6.4629931449890101,56.654331207275398,83.290847778320298,77.551322937011705,80.087890625,89.798044315842205,138.764293207218,165.95861812736501,25.016443190601802,100.417500730059,145.32536670557201,73.910773743663896]
["CN-E1L210C13","CN",1,"E1L210C13",196,"CM(R), DRL Expense, Privately-Owned, REFRIGERATED - NON-MECH",2.9705124907195598E-3,4.2559057474136396E-3,2.4513114476576399E-4,3.54655412957072E-3,3.8688094355166002E-3,6.6280523315072103E-3,1.28866825252771E-2,1.28209334798157E-3,4.5684641227126104E-3,1.0189270516069401E-3,4.5024843412803202E-4,2.8814301511837799E-4,4.2206856909553301E-4,2.7405929836366998E-4,2.6121506914516998E-4,1.4992614048417601E-4]
["CN-E1L211C1","CN",1,"E1L211C1",197,"CM(R), OPR Expense, Railroad-Owned, FLAT - TOFC",1.41393896192312E-2,1.1354803107678901E-2,1.23582743108273E-2,1.0623312555253501E-2,5.3337025456130496E-3,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L211C2","CN",1,"E1L211C2",198,"CM(R), DRL Expense, Railroad-Owned, FLAT - TOFC",2.24884282797575E-2,1.9197326153516801E-2,2.1826487034559298E-2,1.5284903347492201E-2,1.53523692861199E-2,-4.9863655120134402E-2,-0.17427109181881001,-0.18165971338748901,-0.14175225794315299,-0.139948040055247,-0.13028817925231101,-9.8008728275310403E-2,-8.0696740946139198E-2,-7.1245457953930794E-2,-5.7222131707661099E-2,-6.8067228489118906E-2]
["CN-E1L211C3","CN",1,"E1L211C3",199,"CM(R), ROI Expense, Railroad-Owned, FLAT - TOFC",4.3129525147378401E-4,6.9635035470128103E-4,3.8592974306084199E-4,-3.7654556217603402E-4,-4.6608436969108901E-4,-5.0420762272551699E-4,-4.0789102786220599E-4,-3.5270929220132503E-4,-2.4421152193099298E-4,-1.7781533422416801E-4,-1.61165258112663E-4,-1.36764368340736E-4,-1.2499677548096701E-4,-9.5210590440766298E-5,-6.0583754390822799E-5,-8.0931076411483099E-5]
["CN-E1L211C4","CN",1,"E1L211C4",200,"CM(Y), OPR Expense, Railroad-Owned, FLAT - TOFC",3.6762408912181903E-2,2.9522486031055499E-2,3.2131507992744397E-2,2.76206079870462E-2,1.3867625966668099E-2,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L211C5","CN",1,"E1L211C5",201,"CM(Y), DRL Expense, Railroad-Owned, FLAT - TOFC",5.8469906449317897E-2,4.9913041293621098E-2,5.6748867034912102E-2,3.9740744978189503E-2,3.9916161447763401E-2,-0.129645481705666,-0.45310488343238797,-0.47231525182723999,-0.36855593323707603,-0.36386490414364098,-0.33874926605601002,-0.254822693515807,-0.20981152645996201,-0.18523819068021999,-0.148777542439919,-0.17697479407170899]
["CN-E1L211C6","CN",1,"E1L211C6",202,"CM(Y), ROI Expense, Railroad-Owned, FLAT - TOFC",1.1213675606995799E-3,1.8105105264112401E-3,1.00341730285436E-3,-9.7901839762926102E-4,-1.2118192389607399E-3,-1.31093978416175E-3,-1.0605168063193601E-3,-9.1704417718574405E-4,-6.3494994537904902E-4,-4.6231986898283598E-4,-4.1902967109292398E-4,-3.5558735768591201E-4,-3.24991616250514E-4,-2.4754753514599201E-4,-1.5751776141613899E-4,-2.1042079866985601E-4]
["CN-E1L211C7","CN",1,"E1L211C7",203,"CD(R), OPR Expense, Railroad-Owned, FLAT - TOFC",0.22823841869831099,0.15934947133064301,0.14549626410007499,0.10020601004362099,4.2395703494548798E-2,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L211C8","CN",1,"E1L211C8",204,"CD(R), DRL Expense, Railroad-Owned, FLAT - TOFC",1.29311788082123,0.80825883150100697,0.75677472352981601,0.304014712572098,0.54724985361099199,-0.274810880422592,-1.18632435798645,-1.4941276311874401,-1.0012347698211701,-0.78952317258327798,-1.1323642742553399,-0.69682457475903203,-0.35499128357560999,-0.28928136176161701,-0.74442680293745001,0.379055305917048]
["CN-E1L211C9","CN",1,"E1L211C9",205,"CD(R), ROI Expense, Railroad-Owned, FLAT - TOFC",8.1729898229241406E-3,1.06329182162881E-2,3.4092946443706799E-3,-5.6921201758086699E-3,-5.8479080908000504E-3,-6.3429418951272999E-3,-4.5860046520829201E-3,-3.9786887355148801E-3,-3.0731989536434399E-3,-2.0834720692877802E-3,-1.9332749837303899E-3,-1.7616469200973999E-3,-1.6782249914756701E-3,-1.2466937540956901E-3,-1.0198895814772799E-3,-1.50369121175439E-3]
["CN-E1L211C10","CN",1,"E1L211C10",206,"CD(Y), OPR Expense, Railroad-Owned, FLAT - TOFC",0.22823841869831099,0.15934947133064301,0.14549626410007499,0.10020601004362099,4.2395710945129401E-2,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L211C11","CN",1,"E1L211C11",207,"CD(Y), DRL Expense, Railroad-Owned, FLAT - TOFC",1.29311776161194,0.80825889110565197,0.75677466392517101,0.304014712572098,0.54724985361099199,-0.274810880422592,-1.18632435798645,-1.4941276311874401,-1.0012347698211701,-0.78952317258327798,-1.1323642742553399,-0.69682457475903203,-0.35499128357560999,-0.28928136176161701,-0.74442680293745001,0.379055305917048]
["CN-E1L211C12","CN",1,"E1L211C12",208,"CD(Y), ROI Expense, Railroad-Owned, FLAT - TOFC",8.1729888916015608E-3,1.06329182162881E-2,3.4092946443706799E-3,-5.6921192444860901E-3,-5.8479080908000504E-3,-6.34294142946601E-3,-4.5860046520829201E-3,-3.9786887355148801E-3,-3.0731987208128001E-3,-2.0834720692877802E-3,-1.9332749837303899E-3,-1.7616469200973999E-3,-1.6782249914756701E-3,-1.2466937540956901E-3,-1.0198895814772799E-3,-1.50369121175439E-3]
["CN-E1L211C13","CN",1,"E1L211C13",209,"CM(R), DRL Expense, Privately-Owned, FLAT - TOFC",0.18554650247096999,0.24734105169773099,0.24596591293811801,0.24491830170154599,0.28212684392929099,0.27449846267700201,0.32787555456161499,0.29121184349060097,0.32130599021911599,0.30966338865250698,0.300270679367802,0.44571578305595799,0.487313109644128,0.49287119373845301,0.208453802660337,0.173200549983516]
["CN-E1L212C1","CN",1,"E1L212C1",210,"CM(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",6.0187961906194701E-2,3.7410635501146303E-2,5.7645291090011597E-2,7.6689623296260806E-2,8.1523634493350997E-2,6.0861498117446899E-2,5.59648461639881E-2,5.03341108560562E-2,7.4491463601589203E-2,0.10296208964065599,0.105120687087356,8.1169459245025402E-2,4.2756652580585697E-2,3.9891362432777397E-2,3.4671700113056599E-2,2.7459567716841798E-2]
["CN-E1L212C2","CN",1,"E1L212C2",211,"CM(R), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",9.0082257986068698E-2,5.2308320999145501E-2,7.8433439135551494E-2,5.4246455430984497E-2,2.91040446609259E-2,6.3939034938812297E-2,6.6615946590900393E-2,5.18450066447258E-2,8.5496872663497897E-2,6.7846074017322303E-2,6.3443047588414805E-2,7.2654101187810197E-2,8.0795982229538404E-2,0.10358645260691,0.111408117096351,0.120539908863352]
["CN-E1L212C3","CN",1,"E1L212C3",212,"CM(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",0.2215506285429,0.25129991769790599,0.384703099727631,0.15960599482059501,0.11244599521160099,0.105255804955959,0.110402882099152,9.1020412743091597E-2,8.0382838845253005E-2,6.3361617227570596E-2,4.9536273909268499E-2,5.5949081831193202E-2,6.5164459299132102E-2,0.13810563218573799,9.4705031843033999E-2,0.120389772462257]
["CN-E1L212C4","CN",1,"E1L212C4",213,"CM(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",0.15648873150348699,9.7267597913742093E-2,0.14987775683403001,0.199392884969711,0.21196138858795199,0.158239930868149,0.14550855755806,0.130868479609489,0.193677693605423,0.26770143306570499,0.27331378642712401,0.21104059403706599,0.11116729670952299,0.103717542325221,9.0146420293947205E-2,7.1394876063788498E-2]
["CN-E1L212C5","CN",1,"E1L212C5",214,"CM(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",0.234213978052139,0.136001616716385,0.203926712274551,0.14104096591472601,7.5670592486858396E-2,0.166241645812988,0.17320150136947601,0.13479699194431299,0.22229193150997201,0.17639979244503801,0.16495192372987899,0.188900663088306,0.21006955379680001,0.26932477677796501,0.28966110445051402,0.31340376304471601]
["CN-E1L212C6","CN",1,"E1L212C6",215,"CM(Y), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",0.57603168487548795,0.65337949991226196,1.00022768974304,0.41497540473937999,0.29235941171646102,0.27366513013839699,0.28704741597175598,0.23665311932563801,0.208995521068573,0.164740204791684,0.12879431216409801,0.14546761276110201,0.169427594177744,0.35907464368291903,0.24623308279188799,0.31301340840186698]
["CN-E1L212C7","CN",1,"E1L212C7",216,"CD(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",3.7022340297699001,2.2715969085693399,3.4434289932250999,4.58862257003784,4.9639749526977504,3.82381319999695,3.40494632720947,3.0964014530181898,4.7348566055297896,6.86250480015336,7.1533015190480702,5.5876947113978401,2.8528836906811299,2.4567613440584402,2.1978427351661498,1.87715441317308]
["CN-E1L212C8","CN",1,"E1L212C8",217,"CD(R), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",-65.865333557128906,-73.551864624023395,-125.493156433105,-142.73333740234401,-89.2647705078125,-73.696853637695298,-71.473937988281307,-53.288063049316399,-68.722557067871094,-66.660748520929502,-108.98336624922,-101.45620725380201,-88.955128030839504,-94.038962410127098,-158.12251793287001,2.10614413527149]
["CN-E1L212C9","CN",1,"E1L212C9",218,"CD(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",20.203851699829102,22.676841735839801,33.046585083007798,14.8061866760254,10.593142509460399,9.8553037643432599,9.3617687225341797,8.7717514038085902,8.2357845306396502,6.1965220358778703,5.0497259511191199,5.9431639156302696,5.92163603015016,11.2694135255598,10.8840987266322,13.8415509949832]
["CN-E1L212C10","CN",1,"E1L212C10",219,"CD(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",3.7022342681884801,2.2715969085693399,3.4434289932250999,4.58862209320068,4.9639749526977504,3.82381319999695,3.40494608879089,3.0964014530181898,4.7348566055297896,6.86250480015336,7.1533015190480702,5.5876947113978401,2.8528836906811299,2.4567613440584402,2.1978427351661498,1.87715441317308]
["CN-E1L212C11","CN",1,"E1L212C11",220,"CD(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",-65.865341186523395,-73.551856994628906,-125.49314880371099,-142.73333740234401,-89.264762878417997,-73.696853637695298,-71.473937988281307,-53.288063049316399,-68.722549438476605,-66.660748520929502,-108.98336624922,-101.45620725380201,-88.955128030839504,-94.038962410127098,-158.12251793287001,2.1061441352714998]
["CN-E1L212C12","CN",1,"E1L212C12",221,"CD(Y), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",20.203853607177699,22.676841735839801,33.046585083007798,14.806185722351101,10.593141555786101,9.8553028106689506,9.3617687225341797,8.7717523574829102,8.2357845306396502,6.1965220358778703,5.0497259511191199,5.9431639156302696,5.92163603015016,11.2694135255598,10.8840987266322,13.8415509949832]
["CN-E1L212C13","CN",1,"E1L212C13",222,"CM(R), DRL Expense, Privately-Owned, FLAT - MULTILEVEL",0.24380102753639199,0.27643129229545599,0.484655231237412,0.44659811258316001,0.31857234239578203,0.28852164745330799,0.28590971231460599,0.25427457690239003,0.26718491315841703,0.28384758792981901,0.33181675827430201,0.29512441416823798,0.26446548264564201,0.30702232638319099,0.41104151009523898,0.295243289748501]
["CN-E1L213C1","CN",1,"E1L213C1",223,"CM(R), OPR Expense, Railroad-Owned, FLAT - GENERAL",1.37400782108307,0.37962272763252303,4.3157745152711903E-2,4.0644120424985899E-2,3.9434093981981298E-2,9.2638716101646396E-2,8.5385106503963498E-2,8.5254415869712802E-2,9.1275654733181E-2,0.110066912080238,9.6491990271148603E-2,8.0285772545710996E-2,5.5659999310172299E-2,4.0418690300912899E-2,1.43651855634914E-2,0]
["CN-E1L213C2","CN",1,"E1L213C2",224,"CM(R), DRL Expense, Railroad-Owned, FLAT - GENERAL",0.114419519901276,-3.4590702503919601E-2,2.64109596610069E-2,4.6000294685363796,3.77670550346375,4.3020381927490199,3.8061509132385298,4.9661512374877903,5.7511515617370597,6.9298418338632599,5.2282323295482902,-1.67186122220109,19.644641819032699,44.983782427310501,18.748066034475301,48.048325102393697]
["CN-E1L213C3","CN",1,"E1L213C3",225,"CM(R), ROI Expense, Railroad-Owned, FLAT - GENERAL",0.22355411946773501,8.1062637269496904E-2,8.4946339484304201E-4,12.476416587829601,11.8745527267456,8.4421148300170898,7.3834118843078604,9.4347267150878906,8.3849191665649396,16.586131417608598,10.166460255078499,20.5643298320166,25.425364607971101,46.619047116175899,9.1359860325128093,21.541171821667799]
["CN-E1L213C4","CN",1,"E1L213C4",226,"CM(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL",3.5724124908447301,0.98701959848403897,0.11221017688512799,0.105674780905247,0.10252851247787501,0.240860670804977,0.222001522779465,0.221661552786827,0.23731669783592199,0.286173971408618,0.250879174704987,0.20874300861884801,0.14471599820644801,0.10508859478237401,3.7349482465077598E-2,0]
["CN-E1L213C5","CN",1,"E1L213C5",227,"CM(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",0.29749053716659501,-8.9935809373855605E-2,6.8668514490127605E-2,11.9600639343262,9.8194112777709996,11.1853036880493,9.8959798812866193,12.911991119384799,14.952977180481,18.017588768044501,13.5934040568255,-4.3468391777228303,51.076068729484902,116.95783431100701,48.744971689635904,124.925645266223]
["CN-E1L213C6","CN",1,"E1L213C6",228,"CM(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL",0.58124107122421298,0.21076312661171001,2.2086014505475799E-3,32.438667297363303,30.8738117218018,21.949485778808601,19.196773529052699,24.5303134918213,21.800758361816399,43.123941685782498,26.432796663204101,53.467257563243002,66.105947980725205,121.20952250205799,23.7535636845335,56.007046736336299]
["CN-E1L213C7","CN",1,"E1L213C7",229,"CD(R), OPR Expense, Railroad-Owned, FLAT - GENERAL",278.84146118164102,67.974540710449205,7.9665975570678702,6.6251263618469203,6.0140109062194798,11.527987480163601,13.723956108093301,15.2586421966553,16.579473495483398,9.1980013259555999,13.514579409828,13.616607086793399,10.11304345982,6.98965460008099,2.4302067275571901,0]
["CN-E1L213C8","CN",1,"E1L213C8",230,"CD(R), DRL Expense, Railroad-Owned, FLAT - GENERAL",35.8042182922363,-4.7329950332641602,9.3927974700927699,703.61279296875,818.69927978515602,897.04315185546898,1342.41430664063,1580.26184082031,1143.06616210938,739.28425469583101,1433.76868105376,-522.81551895385905,4647.3643191065403,9286.5771133926191,5427.7418457198601,13030.094721416899]
["CN-E1L213C9","CN",1,"E1L213C9",231,"CD(R), ROI Expense, Railroad-Owned, FLAT - GENERAL",67.215965270996094,19.167812347412099,0.17324593663215601,2046.25891113281,2574.119140625,1731.10949707031,2555.4130859375,2961.52026367188,1658.03686523438,1757.34633176126,2772.4210187774902,6547.9387743857196,5981.7262828252997,9609.7843134430095,2639.1795348595701,5838.4148627684099]
["CN-E1L213C10","CN",1,"E1L213C10",232,"CD(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL",278.84146118164102,67.974533081054702,7.9665975570678702,6.6251268386840803,6.0140113830566397,11.527991294860801,13.723956108093301,15.2586421966553,16.579473495483398,9.1980013259555999,13.514579409828,13.616607086793399,10.11304345982,6.98965460008099,2.4302067275571901,0]
["CN-E1L213C11","CN",1,"E1L213C11",233,"CD(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",35.8042182922363,-4.7329950332641602,9.3927984237670898,703.61279296875,818.69921875,897.04315185546898,1342.41442871094,1580.26171875,1143.06604003906,739.28425469583101,1433.76868105376,-522.81551895385905,4647.3643191065403,9286.5771133926191,5427.7418457198601,13030.094721416899]
["CN-E1L213C12","CN",1,"E1L213C12",234,"CD(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL",67.215965270996094,19.167812347412099,0.17324595153331801,2046.2587890625,2574.119140625,1731.10949707031,2555.41333007813,2961.52026367188,1658.03686523438,1757.34633176126,2772.4210187774902,6547.9387743857196,5981.7262828252997,9609.7843134430095,2639.1795348595701,5838.4148627684099]
["CN-E1L213C13","CN",1,"E1L213C13",235,"CM(R), DRL Expense, Privately-Owned, FLAT - GENERAL",9.9709004163742093E-2,8.7084971368312794E-2,6.7252412438392598E-2,0.91095608472824097,1.0914763212203999,0.112252548336983,9.0064153075218201E-2,0.11092077940702399,0.27194368839263899,0.190360801265991,0.19016678489984401,2.2688592825901001E-2,2.47564312118125E-2,3.3140902426552099E-2,3.1835549412605198E-2,0.133626659520208]
["CN-E1L214C1","CN",1,"E1L214C1",236,"CM(R), OPR Expense, Railroad-Owned, FLAT - OTHER",2.0956216380000101E-2,2.7616843581199601E-2,3.3015787601470899E-2,3.79286222159863E-2,3.6918412894010502E-2,3.8644082844257403E-2,3.9668027311563499E-2,4.1333295404911E-2,4.7320555895566899E-2,5.5189330467187499E-2,5.5063108000267702E-2,5.3869737385949801E-2,4.5422424421310198E-2,5.3494458607233501E-2,4.9112433061794802E-2,4.2602507620665697E-2]
["CN-E1L214C2","CN",1,"E1L214C2",237,"CM(R), DRL Expense, Railroad-Owned, FLAT - OTHER",-1.8131971359252898E-2,-1.5015407465398299E-2,-1.6347827389836301E-2,-2.00855769217014E-2,-2.0838117226958299E-2,-2.48789601027966E-2,-2.3106418550014499E-2,-3.5760883241891903E-2,-1.3740720227360699E-2,-9.6824824460526593E-3,-1.0423889157752501E-2,-8.9868855579552792E-3,-7.3395208282825202E-3,-4.7894811372638704E-3,-6.1449974818147202E-3,6.4930297239246103E-3]
["CN-E1L214C3","CN",1,"E1L214C3",238,"CM(R), ROI Expense, Railroad-Owned, FLAT - OTHER",1.2215852737426799E-2,1.6754120588302598E-2,1.9196152687072799E-2,3.3087069168686901E-3,2.2761344444006699E-3,3.5902971867471899E-3,3.6544129252433799E-3,3.2176661770790798E-3,2.8989173006266399E-3,2.2735163845407501E-3,1.8829281622163201E-3,2.4253791609735701E-3,2.85855153477152E-3,2.1076118991440701E-3,1.7773223544273601E-3,1.7642688973011501E-3]
["CN-E1L214C4","CN",1,"E1L214C4",239,"CM(Y), OPR Expense, Railroad-Owned, FLAT - OTHER",5.4486140608787502E-2,7.1803756058216095E-2,8.5840955376625103E-2,9.8614364862442003E-2,9.5987834036350306E-2,0.100474499166012,0.103137023746967,0.10746647417545301,0.12303350120782899,0.143492259214687,0.14316408080069601,0.14006131720347001,0.118098303495406,0.13908559237880699,0.12769232596066599,0.11076651981373099]
["CN-E1L214C5","CN",1,"E1L214C5",240,"CM(Y), DRL Expense, Railroad-Owned, FLAT - OTHER",-4.7143116593360901E-2,-3.9040096104145099E-2,-4.2504303157329601E-2,-5.2222494035959202E-2,-5.4179102182388299E-2,-6.46852552890778E-2,-6.00767582654953E-2,-9.2978455126285595E-2,-3.5725861787796E-2,-2.5174454359736899E-2,-2.7102111810156499E-2,-2.33659024506838E-2,-1.9082754153534599E-2,-1.2452650956886101E-2,-1.5976993452718299E-2,1.6881877282204E-2]
["CN-E1L214C6","CN",1,"E1L214C6",241,"CM(Y), ROI Expense, Railroad-Owned, FLAT - OTHER",3.17612402141094E-2,4.3560735881328597E-2,4.9909956753253902E-2,8.6026312783360499E-3,5.9179426170885598E-3,9.3347709625959396E-3,9.5014804974198307E-3,8.3659384399652498E-3,7.5371852144599004E-3,5.9111425998059396E-3,4.8956132217624296E-3,6.3059858185312801E-3,7.4322339904059499E-3,5.4797909377745802E-3,4.6210381215111502E-3,4.5870991329829899E-3]
["CN-E1L214C7","CN",1,"E1L214C7",242,"CD(R), OPR Expense, Railroad-Owned, FLAT - OTHER",2.5844349861145002,3.5336151123046902,4.1811480522155797,4.7951364517211896,4.5410099029540998,4.7216167449951199,4.5597209930419904,4.6959586143493697,5.4034304618835396,6.3941835910711804,6.3933076714341697,6.23024272036412,5.4139272280380801,6.3319738096258096,5.9575683561564903,5.3293641983234297]
["CN-E1L214C8","CN",1,"E1L214C8",243,"CD(R), DRL Expense, Railroad-Owned, FLAT - OTHER",6.1260080337524396,5.1377639770507804,7.2308716773986799,17.015186309814499,8.6918573379516602,6.2748236656189,8.7073106765747106,6.4327363967895499,17.361778259277301,17.6735042029248,14.0554712020799,16.482626081124099,30.490911883888401,36.036748991131702,32.627255996085701,33.175266892072798]
[{"$f":"B1218&\"-\"&D1218","v":"CN-E1L214C9"},"CN",1,"E1L214C9",244,"CD(R), ROI Expense, Railroad-Owned, FLAT - OTHER",2.3334867954254199,3.2855174541473402,3.3858156204223602,0.55444234609603904,0.34236654639244102,0.54959726333618197,0.51045870780944802,0.49995964765548701,0.44520592689514199,0.319189954401637,0.280754486328683,0.35672883572614,0.41642829949009802,0.29451962929421499,0.25889773199619398,0.26178331952976902]
["CN-E1L214C10","CN",1,"E1L214C10",245,"CD(Y), OPR Expense, Railroad-Owned, FLAT - OTHER",2.5844352245330802,3.5336151123046902,4.1811480522155797,4.7951369285583496,4.5410103797912598,4.7216172218322798,4.5597209930419904,4.6959586143493697,5.4034304618835396,6.3941835910711804,6.3933076714341697,6.23024272036412,5.4139272280380801,6.3319738096258096,5.9575683561564903,5.3293641983234403]
["CN-E1L214C11","CN",1,"E1L214C11",246,"CD(Y), DRL Expense, Railroad-Owned, FLAT - OTHER",6.1260080337524396,5.1377639770507804,7.2308726310729998,17.015184402465799,8.6918563842773402,6.2748227119445801,8.7073106765747106,6.4327359199523899,17.3617763519287,17.6735042029248,14.0554712020799,16.482626081124099,30.490911883888401,36.036748991131702,32.627255996085701,33.175266892072798]
["CN-E1L214C12","CN",1,"E1L214C12",247,"CD(Y), ROI Expense, Railroad-Owned, FLAT - OTHER",2.3334867954254199,3.2855176925659202,3.3858156204223602,0.55444240570068404,0.34236651659011802,0.54959720373153698,0.51045870780944802,0.499959707260132,0.44520595669746399,0.319189954401637,0.280754486328683,0.35672883572614,0.41642829949009802,0.29451962929421399,0.25889773199619398,0.26178331952976902]
["CN-E1L214C13","CN",1,"E1L214C13",248,"CM(R), DRL Expense, Privately-Owned, FLAT - OTHER",0.214919924736023,0.23854425549507099,0.26286056637763999,0.55145639181137096,0.67334944009780895,0.52990531921386697,0.50321793556213401,0.36110731959343001,0.34434568881988498,0.39836189737607702,0.351369183443554,0.249283945689075,0.326357296384019,0.52279273582020402,0.372743337593543,0.41218994387003]
["CN-E1L215C1","CN",1,"E1L215C1",249,"CM(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C2","CN",1,"E1L215C2",250,"CM(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,8.2250004634261097E-3,0,5.8049084618687604E-3,5.3032404581388297E-3,6.1380793535374201E-3,5.8958440628251599E-3,5.7981106790344098E-3,1.25599006308922E-2,9.22010805574211E-3,7.3819895560674302E-3]
["CN-E1L215C3","CN",1,"E1L215C3",251,"CM(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C4","CN",1,"E1L215C4",252,"CM(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C5","CN",1,"E1L215C5",253,"CM(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C6","CN",1,"E1L215C6",254,"CM(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C7","CN",1,"E1L215C7",255,"CD(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C8","CN",1,"E1L215C8",256,"CD(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C9","CN",1,"E1L215C9",257,"CD(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C10","CN",1,"E1L215C10",258,"CD(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C11","CN",1,"E1L215C11",259,"CD(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C12","CN",1,"E1L215C12",260,"CD(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L215C13","CN",1,"E1L215C13",261,"CM(R), DRL Expense, Privately-Owned, TANK <22,000 GAL",3.74680273234844E-2,3.0870974063873301E-2,2.6349049061536799E-2,2.8822652995586399E-2,2.6203209534287501E-2,1.4506957493722401E-2,8.2250004634261097E-3,6.68131932616234E-3,5.8049084618687604E-3,5.3032404581388297E-3,6.1380793535374201E-3,5.8958440628251599E-3,5.7981106790344098E-3,1.25599006308922E-2,9.22010805574211E-3,7.3819895560674302E-3]
["CN-E1L216C1","CN",1,"E1L216C1",262,"CM(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C2","CN",1,"E1L216C2",263,"CM(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,1.0543582029640701E-2,0,7.4272528290748596E-3,6.4300410176499102E-3,6.6299190049544801E-3,6.3173500711627998E-3,6.1162004258980499E-3,3.34654422941735E-5,1.60776496523786E-5,3.7101758080977602E-3]
["CN-E1L216C3","CN",1,"E1L216C3",264,"CM(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C4","CN",1,"E1L216C4",265,"CM(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C5","CN",1,"E1L216C5",266,"CM(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C6","CN",1,"E1L216C6",267,"CM(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C7","CN",1,"E1L216C7",268,"CD(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C8","CN",1,"E1L216C8",269,"CD(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C9","CN",1,"E1L216C9",270,"CD(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C10","CN",1,"E1L216C10",271,"CD(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C11","CN",1,"E1L216C11",272,"CD(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C12","CN",1,"E1L216C12",273,"CD(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L216C13","CN",1,"E1L216C13",274,"CM(R), DRL Expense, Privately-Owned, TANK >=22,000 GAL",5.8673989027738599E-2,2.6461226865649199E-2,3.1784209568286301E-5,6.6777879510482299E-6,1.0555216431384899E-4,1.5107460319995899E-2,1.0543582029640701E-2,8.5642607882618904E-3,7.4272528290748596E-3,6.4300410176499102E-3,6.6299190049544801E-3,6.3173500711627998E-3,6.1162004258980499E-3,3.34654422941735E-5,1.60776496523786E-5,3.7101758080977602E-3]
["CN-E1L217C1","CN",1,"E1L217C1",275,"CM(R), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",4.6541713178157799E-2,5.2033457905054099E-2,6.1087369918823201E-2,7.6195135712623596E-2,7.2932571172714206E-2,8.4063656628131894E-2,7.4575923383235904E-2,6.1372734606266001E-2,3.8031503558158902E-2,5.2936669000712699E-2,5.8372863410096502E-2,5.0895471358807301E-2,2.5748700598206699E-2,2.3053114535719E-2,3.6385046024727599E-2,5.0622634835862997E-2]
["CN-E1L217C2","CN",1,"E1L217C2",276,"CM(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",6.8544601090252399E-3,5.5987574160099004E-3,4.5525007881224199E-3,3.9943470619618901E-3,4.7141145914792997E-3,5.2747642621397998E-3,5.5474899709224701E-3,5.3632659837603604E-3,3.7819819990545498E-3,1.6217712111912499E-2,1.8694668433107901E-2,1.15730260863819E-2,5.5826160443944997E-3,6.2059739237599202E-3,9.5048983656623801E-2,9.6548500804562995E-2]
["CN-E1L217C3","CN",1,"E1L217C3",277,"CM(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-4.2738555930554901E-3,-4.9420781433582297E-3,-5.5943718180060404E-3,1.46560659632087E-2,1.2176085263490699E-2,1.4770369976759E-2,1.3062298297882099E-2,1.0033374652266501E-2,7.3815723881125502E-3,6.1797695354238796E-3,5.4821998314938296E-3,3.9047580754058399E-3,-8.7239634131220406E-2,-2.7727920034620102E-2,7.6975151754106897E-3,1.28260499719571E-3]
["CN-E1L217C4","CN",1,"E1L217C4",278,"CM(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.121008448302746,0.13528698682785001,0.15882714092731501,0.19810739159584001,0.18962465226650199,0.218565449118614,0.19389736652374301,0.15956902503967299,9.8881870508193997E-2,0.13763533940185299,0.15176944486625099,0.132328225532898,6.6946621555337399E-2,5.9938097792869502E-2,9.4601119664291605E-2,0.13161885057324399]
["CN-E1L217C5","CN",1,"E1L217C5",279,"CM(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",1.7821596935391398E-2,1.45567674189806E-2,1.18365008383989E-2,1.03852981701493E-2,1.22566949576139E-2,1.37143703177571E-2,1.44234756007791E-2,1.3944487087428599E-2,9.8331561312079395E-3,4.2166051490972502E-2,4.8606137926080803E-2,3.0089867824592699E-2,1.45148017154257E-2,1.6135532201775798E-2,0.24712735750722201,0.25102610209186399]
["CN-E1L217C6","CN",1,"E1L217C6",280,"CM(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-1.1112027801573301E-2,-1.2849404476583001E-2,-1.4545367099344699E-2,3.8105756044387797E-2,3.1657814979553202E-2,3.8402911275625201E-2,3.3961985260248198E-2,2.60867867618799E-2,1.9192103296518302E-2,1.6067400792102102E-2,1.4253719561883999E-2,1.0152370996055199E-2,-0.22682304874117401,-7.2092592090012106E-2,2.0013539456067798E-2,3.3347729927088502E-3]
["CN-E1L217C7","CN",1,"E1L217C7",281,"CD(R), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",2.4997930526733398,2.1472108364105198,2.0885112285614,2.5452423095703098,2.5540580749511701,3.95495510101318,4.7336955070495597,7.0231032371520996,4.2795534133911097,6.4486599059635497,7.1628883953654503,7.2808909137553499,3.6052050479948901,3.02981352055532,3.5530502358463698,3.1232469704905599]
["CN-E1L217C8","CN",1,"E1L217C8",282,"CD(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-0.65247750282287598,-0.554423809051514,0.343310356140137,1.1867032051086399,0.50327479839324996,2.85449171066284,3.1846354007720898,4.2022786140441903,1.30868256092072,4.2209915886710103,4.4425091364791101,3.2831716849465802,1.90223948934097,1.6987196841467,2.9518657299830302,3.2896832879894]
["CN-E1L217C9","CN",1,"E1L217C9",283,"CD(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-0.262448459863663,-0.25830554962158198,-0.29160118103027299,0.76169192790985096,0.639337599277496,2.19429659843445,2.0054614543914799,1.8041802644729601,1.11502313613892,1.2371529887830199,0.98642027251921505,0.82711871844208795,-17.850212056255302,-4.7497047472092904,0.139139201961965,-3.1519470639124303E-2]
["CN-E1L217C10","CN",1,"E1L217C10",284,"CD(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",2.4997930526733398,2.1472108364105198,2.08851146697998,2.5452423095703098,2.5540583133697501,3.95495510101318,4.7336945533752397,7.0231027603149396,4.2795534133911097,6.4486599059635497,7.1628883953654503,7.2808909137553499,3.6052050479948901,3.02981352055532,3.5530502358463698,3.1232469704905599]
["CN-E1L217C11","CN",1,"E1L217C11",285,"CD(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-0.65247744321823098,-0.554423809051514,0.343310356140137,1.1867032051086399,0.50327479839324996,2.85449147224426,3.1846356391906698,4.2022786140441903,1.30868244171143,4.2209915886710103,4.4425091364791101,3.2831716849465802,1.90223948934097,1.6987196841467,2.9518657299830302,3.2896832879894]
["CN-E1L217C12","CN",1,"E1L217C12",286,"CD(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-0.262448400259018,-0.25830554962158198,-0.29160118103027299,0.76169180870056197,0.639337599277496,2.19429659843445,2.0054614543914799,1.8041802644729601,1.11502313613892,1.2371529887830199,0.98642027251921505,0.82711871844208795,-17.850212056255302,-4.7497047472092904,0.139139201961965,-3.1519470639124303E-2]
["CN-E1L217C13","CN",1,"E1L217C13",287,"CM(R), DRL Expense, Privately-Owned, ALL OTHER FREIGHT CARS",0.105315759778023,2.9617365449667001E-2,2.4998129811137902E-3,8.3498518506530699E-5,2.0253703405614899E-4,3.60885006375611E-3,1.0242064017802501E-3,1.31523665913846E-5,9.07796493265778E-6,0,2.7272776629487598E-4,0,0,0,3.6406961096743698E-5,0]
["CN-E1L218C1","CN",1,"E1L218C1",288,"CM(R), OPR Expense, Railroad-Owned, AUTO RACKS",2.3919898085296202E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L218C2","CN",1,"E1L218C2",289,"CM(R), DRL Expense, Railroad-Owned, AUTO RACKS",5.75377456843853E-2,4.5073583722114598E-2,6.7062564194202395E-2,7.6323188841342898E-2,5.3417712450027501E-2,7.6713621616363498E-2,7.9200632870197296E-2,6.5721601247787503E-2,8.0323435366153703E-2,5.8273356889015998E-2,5.3726389233357999E-2,5.1760240916136499E-2,5.8075349325062101E-2,8.2033264976264897E-2,9.2190164760499294E-2,8.83724429693723E-2]
["CN-E1L218C3","CN",1,"E1L218C3",290,"CM(R), ROI Expense, Railroad-Owned, AUTO RACKS",5.9087131172418601E-2,8.9087255299091297E-2,0.135418295860291,0.13752661645412401,9.7366489470004994E-2,8.8311173021793393E-2,8.8233955204486805E-2,7.1512162685394301E-2,6.01436570286751E-2,4.5218933528138799E-2,3.4283752376434599E-2,4.0900112883419298E-2,5.1641936143875099E-2,0.130103984661192,9.0788986812390907E-2,0.117391580397224]
["CN-E1L218C4","CN",1,"E1L218C4",291,"CM(Y), OPR Expense, Railroad-Owned, AUTO RACKS",6.2191719189286197E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L218C5","CN",1,"E1L218C5",292,"CM(Y), DRL Expense, Railroad-Owned, AUTO RACKS",0.14959812164306599,0.11719124019146,0.17436261475086201,0.19844026863575001,0.13888604938983901,0.19945551455020899,0.205921590328217,0.170876160264015,0.20884099602699299,0.15151072791144199,0.13968861200673099,0.134576626381955,0.15099590824516099,0.213286488938288,0.23969442837729901,0.229768351720368]
["CN-E1L218C6","CN",1,"E1L218C6",293,"CM(Y), ROI Expense, Railroad-Owned, AUTO RACKS",0.15362644195556599,0.23162662982940699,0.35208746790885898,0.35756906867027299,0.25315269827842701,0.22960907220840501,0.229408174753189,0.18593163788318601,0.15637363493442499,0.117569227173161,8.9137756178729904E-2,0.10634029349689,0.134269033974075,0.338270360119099,0.23605136571221599,0.30521810903278401]
["CN-E1L218C7","CN",1,"E1L218C7",294,"CD(R), OPR Expense, Railroad-Owned, AUTO RACKS",0.10575807094574,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L218C8","CN",1,"E1L218C8",295,"CD(R), DRL Expense, Railroad-Owned, AUTO RACKS",8.5294675827026403,-21.0666904449463,-30.5458679199219,-33.475803375244098,-24.655351638793899,-31.294944763183601,-30.539493560791001,-20.527000427246101,-40.266887664794901,-46.393217817981501,-81.026138312164804,-79.307608826112101,-71.725548306271193,-74.068729429505794,-113.996698622081,-25.340435791037699]
["CN-E1L218C9","CN",1,"E1L218C9",296,"CD(R), ROI Expense, Railroad-Owned, AUTO RACKS",3.7783050537109402,8.04852199554443,11.6522073745728,12.8341388702393,9.2330751419067401,8.3159313201904297,7.5227198600768999,6.9266490936279297,6.2091493606567401,4.4687220883262002,3.53962280633458,4.3886357843997699,4.7282050673712002,10.6408540383412,10.4625432789879,13.5281724358217]
["CN-E1L218C10","CN",1,"E1L218C10",297,"CD(Y), OPR Expense, Railroad-Owned, AUTO RACKS",0.10575807839632,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L218C11","CN",1,"E1L218C11",298,"CD(Y), DRL Expense, Railroad-Owned, AUTO RACKS",8.5294666290283203,-21.0666904449463,-30.5458660125732,-33.475803375244098,-24.655351638793899,-31.294944763183601,-30.539497375488299,-20.527002334594702,-40.266883850097699,-46.393217817981501,-81.026138312164804,-79.307608826112101,-71.725548306271193,-74.068729429505794,-113.996698622081,-25.340435791037699]
["CN-E1L218C12","CN",1,"E1L218C12",299,"CD(Y), ROI Expense, Railroad-Owned, AUTO RACKS",3.7783045768737802,8.04852199554443,11.6522064208984,12.834137916564901,9.2330741882324201,8.3159303665161097,7.5227198600768999,6.9266495704650897,6.2091498374939,4.4687220883262002,3.53962280633458,4.3886357843997699,4.7282050673712002,10.6408540383412,10.4625432789879,13.5281724358217]
["CN-E1L218C13","CN",1,"E1L218C13",300,"CM(R), DRL Expense, Privately-Owned, AUTO RACKS",1.6569355500000001E-2,1.7995601519942301E-2,2.4581553414464E-2,9.921002201735969E-4,2.5866871699690801E-2,0.12996378540992701,0.124186493456364,0.112969420850277,0.13395518064498901,0.15270659064324199,0.185611674067369,0.16679301665287899,0.15039538516385401,0.15708022323600301,0.22856112531755601,0.13047371533784299]
["CN-E1L219C1","CN",1,"E1L219C1",301,"CM(R), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L219C2","CN",1,"E1L219C2",302,"CM(R), DRL Expense, Railroad-Owned, ACCESSORIAL",-1.2194319424452301E-5,-5.8742516557685997E-6,-6.4381201809737797E-6,-1.8706403352553001E-5,-1.6346091797458899E-5,-1.6257661627605601E-5,-1.9070053895120499E-5,-1.7169752027257302E-5,-2.0690176825155501E-5,-1.8690179392784901E-5,-1.9948165459628999E-5,-1.9658796376883201E-5,0,0,0,0]
["CN-E1L219C3","CN",1,"E1L219C3",303,"CM(R), ROI Expense, Railroad-Owned, ACCESSORIAL",-1.59240553330164E-5,-1.9251387129770599E-5,-2.0284194761188701E-5,-3.9116007428674501E-6,-9.4676431672269203E-7,1.0546027624514001E-6,3.0893927487341001E-6,4.6133282012306196E-6,6.3911438701325096E-6,7.5321442615263401E-6,9.1060560163731693E-6,1.24057778235604E-5,1.421460434628E-5,1.12505266279245E-5,1.01420212561362E-5,1.23167066955732E-5]
["CN-E1L219C4","CN",1,"E1L219C4",304,"CM(Y), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L219C5","CN",1,"E1L219C5",305,"CM(Y), DRL Expense, Railroad-Owned, ACCESSORIAL",-3.1705225410405499E-5,-1.5273040844476799E-5,-1.67391244758619E-5,-4.8636658902978497E-5,-4.2499836126808097E-5,-4.2269915866199901E-5,-4.9582096835365499E-5,-4.4641346903517802E-5,-5.3794472478330101E-5,-4.85944664212409E-5,-5.1865230195035301E-5,-5.1112870579896301E-5,0,0,0,0]
["CN-E1L219C6","CN",1,"E1L219C6",306,"CM(Y), ROI Expense, Railroad-Owned, ACCESSORIAL",-4.1402530769118999E-5,-5.0053582526743398E-5,-5.2738971135113402E-5,-1.01701598396176E-5,-2.4615872007416299E-6,2.7419682737672701E-6,8.0324134614784304E-6,1.19946544145932E-5,1.6616973880445602E-5,1.9583575079968501E-5,2.3675745642570301E-5,3.2255022341257E-5,3.6957971300328001E-5,2.92513692326038E-5,2.6369255265954199E-5,3.2023437408490397E-5]
["CN-E1L219C7","CN",1,"E1L219C7",307,"CD(R), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B1282&\"-\"&D1282","v":"CN-E1L219C8"},"CN",1,"E1L219C8",308,"CD(R), DRL Expense, Railroad-Owned, ACCESSORIAL",-1.1437659850344101E-3,-5.3755409317091097E-4,-5.6869949912652395E-4,-1.4112159842625299E-3,-1.1206455528736099E-3,-1.08938536141068E-3,-1.1028655571863101E-3,-1.0858570458367499E-3,-1.27257499843836E-3,-1.1093600260019001E-3,-1.2037504229518701E-3,-1.0842216247501E-3,0,0,0,0]
["CN-E1L219C9","CN",1,"E1L219C9",309,"CD(R), ROI Expense, Railroad-Owned, ACCESSORIAL",-1.4935964718461E-3,-1.76169897895306E-3,-1.79176696110517E-3,-2.9509220621548598E-4,-6.49077046546154E-5,7.0666304964106503E-5,1.7866678535938301E-4,2.91758129606023E-4,3.9309522253461198E-4,4.4707220718505201E-4,5.4949508030281203E-4,6.8420326098732895E-4,7.7681822445314105E-4,5.9987331564876701E-4,5.2289882646571503E-4,6.9376114801883004E-4]
["CN-E1L219C10","CN",1,"E1L219C10",310,"CD(Y), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L219C11","CN",1,"E1L219C11",311,"CD(Y), DRL Expense, Railroad-Owned, ACCESSORIAL",-1.14376586861908E-3,-5.3755409317091097E-4,-5.6869944091886304E-4,-1.4112159842625299E-3,-1.1206455528736099E-3,-1.0893854778259999E-3,-1.10286579001695E-3,-1.0858569294214201E-3,-1.27257499843836E-3,-1.1093600260019001E-3,-1.2037504229518701E-3,-1.0842216247501E-3,0,0,0,0]
["CN-E1L219C12","CN",1,"E1L219C12",312,"CD(Y), ROI Expense, Railroad-Owned, ACCESSORIAL",-1.4935963554307801E-3,-1.76169897895306E-3,-1.79176696110517E-3,-2.9509220621548598E-4,-6.49077046546154E-5,7.0666304964106503E-5,1.7866678535938301E-4,2.91758129606023E-4,3.9309519343078098E-4,4.4707220718505201E-4,5.4949508030281203E-4,6.8420326098732895E-4,7.7681822445314105E-4,5.9987331564876798E-4,5.2289882646571503E-4,6.9376114801883004E-4]
["CN-E1L219C13","CN",1,"E1L219C13",313,"CM(R), DRL Expense, Privately-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L220C1","CN",1,"E1L220C1",314,"CM(R), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",2.8887953609228099E-2,3.02953273057938E-2,3.4882802516222E-2,4.8729326575994499E-2,3.7964474409818601E-2,3.3317618072032901E-2,3.69318574666977E-2,3.02143525332212E-2,3.4721598029136699E-2,5.0924222321503697E-2,5.9812310493196998E-2,6.2568156616949394E-2,5.1383107007933103E-2,5.8998300708539703E-2,5.7963239257240097E-2,4.3867025595890001E-2]
["CN-E1L220C2","CN",1,"E1L220C2",315,"CM(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",-5.8356476947665197E-3,4.0872842073440604E-3,6.7995269782841197E-3,1.29219926893711E-2,7.5180432759225403E-3,1.5977697446942302E-2,1.5813091769814502E-2,1.29484217613935E-2,2.0171914249658598E-2,3.9916280495119499E-2,4.1297554015478903E-2,3.6260092499717803E-2,3.7589454089079398E-2,4.7078798418368303E-2,5.505991905872E-2,5.4558210710879497E-2]
["CN-E1L220C3","CN",1,"E1L220C3",316,"CM(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",2.7532896026969001E-2,4.16886396706104E-2,4.6698831021785701E-2,6.2139343470335E-2,5.2299469709396397E-2,6.0827285051345797E-2,6.6909112036228194E-2,6.1012830585241297E-2,5.5305421352386502E-2,5.3206942227529398E-2,5.3984934498145599E-2,6.0806559194201998E-2,6.4796101924741195E-2,5.6506472313406803E-2,4.7825714736100901E-2,5.1994254230141403E-2]
["CN-E1L220C4","CN",1,"E1L220C4",317,"CM(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",6.0259152203798301E-2,6.2889106571674305E-2,7.5052417814731598E-2,9.4704568386077895E-2,6.9193229079246493E-2,6.00966699421406E-2,5.2953556180000298E-2,4.6026725322008098E-2,5.0279758870601703E-2,6.5639743688575003E-2,8.6533864255895196E-2,9.2991093774576497E-2,8.0236625766993405E-2,8.96550480706194E-2,8.4352221434195004E-2,7.4498089637194606E-2]
["CN-E1L220C5","CN",1,"E1L220C5",318,"CM(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",-5.6653185747563804E-3,2.0197460427880301E-2,2.4041190743446399E-2,3.3451762050390202E-2,3.97568792104721E-2,3.3088423311710399E-2,-5.9731779620051401E-3,-1.42522733658552E-2,1.7967127496376599E-3,2.1364084610207099E-2,2.7735805280782899E-2,2.92500096256973E-2,2.7920774438463299E-2,3.8857114883696198E-2,4.8263701722104098E-2,4.1791053246375803E-2]
["CN-E1L220C6","CN",1,"E1L220C6",319,"CM(Y), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",6.22579380869865E-2,9.6514850854873699E-2,0.100973591208458,9.6310243010520893E-2,0.32754468917846702,9.4576291739940602E-2,9.3904584646225003E-2,8.1283144652843503E-2,7.3539331555366502E-2,7.5622484521438396E-2,6.9802478618771993E-2,7.2439947166576799E-2,7.8088753933835797E-2,6.4707507650967097E-2,4.9945944099583903E-2,4.9378429998499E-2]
["CN-E1L220C7","CN",1,"E1L220C7",320,"CD(R), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.09001612663269,3.0653560161590598,3.2763803005218501,5.3418283462524396,3.65612745285034,2.9280965328216602,3.2468953132629399,2.69065189361572,3.11841988563538,4.6238934756405401,5.1937218953087703,5.3264859252998598,4.2137658960682298,4.96353664569373,5.2294645480011503,3.9398859276233602]
["CN-E1L220C8","CN",1,"E1L220C8",321,"CD(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.72985816001892,5.2854504585266104,8.4167776107788104,13.425383567810099,9.32190036773682,8.6446151733398402,9.8168087005615199,9.4884157180786097,10.214056968689,14.310623617536001,11.679694155509701,9.6962806609510093,14.4505353746958,18.780368416461499,18.077501642696198,22.301803719741201]
["CN-E1L220C9","CN",1,"E1L220C9",322,"CD(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.68265652656555,5.5980811119079599,6.2930779457092303,8.9070568084716797,7.1627345085143999,7.7239651679992702,8.0245790481567401,7.81310939788818,6.6548428535461399,6.0650642470441403,6.9020511191052902,8.3751388436365293,7.9542326512237098,6.6471178447590704,6.2995998696416002,6.9315782588302302]
["CN-E1L220C10","CN",1,"E1L220C10",323,"CD(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.6783295869827299,1.72618448734283,1.93188488483429,2.2420210838317902,1.5781046152114899,1.3571975231170701,1.2489807605743399,1.12932813167572,1.2516115903854399,1.73168749677828,2.1041016540295598,2.0029809349687002,1.64022046885305,1.8216893987157901,1.70954400879086,1.4563199860612801]
["CN-E1L220C11","CN",1,"E1L220C11",324,"CD(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.7493475675582899,2.38930439949036,3.5397381782531698,4.7417459487915004,3.41470146179199,3.3574867248535201,3.4338860511779798,3.5449562072753902,3.7627577781677202,5.4543560653343901,4.2641901698358398,3.40270160226699,4.2393538825391897,4.4564900359108099,3.7648202254549799,6.1291292411141098]
["CN-E1L220C12","CN",1,"E1L220C12",325,"CD(Y), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",2.45807957649231,3.6261188983917201,3.8749029636383101,4.2353978157043501,4.0141639709472701,3.6559536457061799,3.4009273052215598,3.37962818145752,2.98914575576782,2.77465520424298,2.8019436357849199,2.8045287655708302,2.9885249379719401,2.5378076860651801,2.0292485957219402,2.4283774394261899]
["CN-E1L220C13","CN",1,"E1L220C13",326,"CM(R), DRL Expense, Privately-Owned, AVERAGE ALL FREIGHT CARS",4.5610427856445299E-2,4.4645633548498202E-2,4.7807537019252798E-2,4.54373322427273E-2,4.6865783631801598E-2,4.2668826878070797E-2,3.8754064589738797E-2,4.05618958175182E-2,4.0155410766601597E-2,4.65044134439788E-2,5.2433157714337299E-2,5.0132353669983899E-2,4.6454051868337003E-2,5.4368163990414102E-2,6.1208159394916098E-2,4.7210909662245497E-2]
["CN-E1L221C1","CN",1,"E1L221C1",327,"CM(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",6.0187961906194701E-2,3.7410635501146303E-2,5.7645291090011597E-2,7.6689623296260806E-2,8.1523634493350997E-2,6.0861498117446899E-2,5.59648461639881E-2,5.03341108560562E-2,7.4491463601589203E-2,0.10296208964065599,0.105120687087356,8.1169459245025402E-2,4.2756652580585697E-2,3.9891362432777397E-2,3.4671700113056599E-2,2.7459567716841798E-2]
["CN-E1L221C2","CN",1,"E1L221C2",328,"CM(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",9.0082257986068698E-2,5.2308320999145501E-2,7.8433439135551494E-2,5.4246455430984497E-2,2.91040446609259E-2,6.3939034938812297E-2,6.6615946590900393E-2,5.18450066447258E-2,8.5496872663497897E-2,6.7846074017322303E-2,6.3443047588414805E-2,7.2654101187810197E-2,8.0795982229538404E-2,0.10358645260691,0.111408117096351,0.120539908863352]
["CN-E1L221C3","CN",1,"E1L221C3",329,"CM(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.2215506285429,0.25129991769790599,0.384703099727631,0.15960599482059501,0.11244599521160099,0.105255804955959,0.110402882099152,9.1020412743091597E-2,8.0382838845253005E-2,6.3361617227570596E-2,4.9536273909268499E-2,5.5949081831193202E-2,6.5164459299132102E-2,0.13810563218573799,9.4705031843033999E-2,0.120389772462257]
["CN-E1L221C4","CN",1,"E1L221C4",330,"CM(Y), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.15648873150348699,9.7267597913742093E-2,0.14987775683403001,0.199392884969711,0.21196138858795199,0.158239930868149,0.14550855755806,0.130868479609489,0.193677693605423,0.26770143306570499,0.27331378642712401,0.21104059403706599,0.11116729670952299,0.103717542325221,9.0146420293947205E-2,7.1394876063788498E-2]
["CN-E1L221C5","CN",1,"E1L221C5",331,"CM(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.234213978052139,0.136001616716385,0.203926712274551,0.14104096591472601,7.5670592486858396E-2,0.166241645812988,0.17320150136947601,0.13479699194431299,0.22229193150997201,0.17639979244503801,0.16495192372987899,0.188900663088306,0.21006955379680001,0.26932477677796501,0.28966110445051402,0.31340376304471601]
["CN-E1L221C6","CN",1,"E1L221C6",332,"CM(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.57603168487548795,0.65337949991226196,1.00022768974304,0.41497540473937999,0.29235941171646102,0.27366513013839699,0.28704741597175598,0.23665311932563801,0.208995521068573,0.164740204791684,0.12879431216409801,0.14546761276110201,0.169427594177744,0.35907464368291903,0.24623308279188799,0.31301340840186698]
["CN-E1L221C7","CN",1,"E1L221C7",333,"CD(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",3.7022340297699001,2.2715969085693399,3.4434289932250999,4.58862257003784,4.9639749526977504,3.82381319999695,3.40494632720947,3.0964014530181898,4.7348566055297896,6.86250480015336,7.1533015190480702,5.5876947113978401,2.8528836906811299,2.4567613440584402,2.1978427351661498,1.87715441317308]
["CN-E1L221C8","CN",1,"E1L221C8",334,"CD(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",-65.865333557128906,-73.551864624023395,-125.493156433105,-142.73333740234401,-89.2647705078125,-73.696853637695298,-71.473937988281307,-53.288063049316399,-68.722557067871094,-66.660748520929502,-108.98336624922,-101.45620725380201,-88.955128030839504,-94.038962410127098,-158.12251793287001,2.10614413527149]
["CN-E1L221C9","CN",1,"E1L221C9",335,"CD(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",20.203851699829102,22.676841735839801,33.046585083007798,14.8061866760254,10.593142509460399,9.8553037643432599,9.3617687225341797,8.7717514038085902,8.2357845306396502,6.1965220358778703,5.0497259511191199,5.9431639156302696,5.92163603015016,11.2694135255598,10.8840987266322,13.8415509949832]
["CN-E1L221C10","CN",1,"E1L221C10",336,"CD(Y), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",3.7022342681884801,2.2715969085693399,3.4434289932250999,4.58862209320068,4.9639749526977504,3.82381319999695,3.40494608879089,3.0964014530181898,4.7348566055297896,6.86250480015336,7.1533015190480702,5.5876947113978401,2.8528836906811299,2.4567613440584402,2.1978427351661498,1.87715441317308]
["CN-E1L221C11","CN",1,"E1L221C11",337,"CD(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",-65.865341186523395,-73.551856994628906,-125.49314880371099,-142.73333740234401,-89.264762878417997,-73.696853637695298,-71.473937988281307,-53.288063049316399,-68.722549438476605,-66.660748520929502,-108.98336624922,-101.45620725380201,-88.955128030839504,-94.038962410127098,-158.12251793287001,2.1061441352714998]
["CN-E1L221C12","CN",1,"E1L221C12",338,"CD(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",20.203853607177699,22.676841735839801,33.046585083007798,14.806185722351101,10.593141555786101,9.8553028106689506,9.3617687225341797,8.7717523574829102,8.2357845306396502,6.1965220358778703,5.0497259511191199,5.9431639156302696,5.92163603015016,11.2694135255598,10.8840987266322,13.8415509949832]
["CN-E1L221C13","CN",1,"E1L221C13",339,"CM(R), DRL Expense, Privately-Owned, TOTAL FLAT, MULTILEVEL",0.24380102753639199,0.27643129229545599,0.484655231237412,0.44659811258316001,0.31857234239578203,0.28852164745330799,0.28590971231460599,0.25427457690239003,0.26718491315841703,0.28384758792981901,0.33181675827430201,0.29512441416823798,0.26446548264564201,0.30702232638319099,0.41104151009523898,0.295243289748501]
["CN-E1L301C1","CN",1,"E1L301C1",340,"L&D Expense, FARM PRODUCTS",6.0479726642370203E-2,4.3492771685123402E-2,5.2238646894693402E-2,5.0968628376722301E-2,3.09725925326347E-2,5.8702994138002403E-2,3.9931595325469998E-2,4.0919195860624299E-2,5.5300697684287997E-2,4.0740445742439298E-2,3.0235172829172E-2,4.2640386857255498E-2,3.0764167073179E-2,3.9305223656339899E-2,2.3084220232348799E-2,3.2991514790269003E-2]
["CN-E1L302C1","CN",1,"E1L302C1",341,"L&D Expense, GRAIN",2.6387264952063599E-2,2.4945870041847201E-2,3.6727432161569602E-2,3.52221131324768E-2,2.7508964762091598E-2,4.8060111701488502E-2,2.2179268300533302E-2,3.1123021617531801E-2,3.6137115210294703E-2,3.1673053208722303E-2,2.06520373319149E-2,3.17940606104282E-2,2.12862621972436E-2,1.6299519112691799E-2,1.6646101782829398E-2,1.6986060104260001E-2]
["CN-E1L303C1","CN",1,"E1L303C1",342,"L&D Expense, POTATOES OTHER THAN SWEET",3.6799578666686998,3.1860339641571001,1.57116758823395,2.0286219120025599,0.46845808625221302,0.59124863147735596,0.76070266962051403,0.51356053352356001,1.9531569480896001,2.51130048867766,2.4820239734348402,1.5628554724856101,1.5738487949622999,4.7855950282905102,2.6763798404894299,1.6733272275745501]
["CN-E1L304C1","CN",1,"E1L304C1",343,"L&D Expense, FRESH FRUITS",0.302319556474686,8.5989952087402302E-2,0.58841019868850697,8.6072228848934201E-2,1.4460543170571299E-2,0.126831129193306,0.49312025308608998,0.52817994356155396,0.16668255627155301,8.2599028253724796E-2,9.9674777409128404E-2,0.43295957620681202,8.8434329739041695E-2,0.85901773298737005,1.1195029946875601,0.48971047651869798]
["CN-E1L305C1","CN",1,"E1L305C1",344,"L&D Expense, FRESH VEGETABLES",0.60301697254180897,0.243790358304977,0.41229620575904802,0.19410522282123599,7.3158152401447296E-2,0.65559387207031306,0.35545039176940901,0.20792415738105799,0.48678919672965998,0.41470897303029602,0.34160943933107601,0.389577076844837,0.26595492810377602,0.63672310190342996,0.200726594272612,0.51497044391303703]
["CN-E1L306C1","CN",1,"E1L306C1",345,"L&D Expense, ALL OTHER FARM PRODUCTS",8.7879635393619496E-2,4.6295948326587698E-2,4.7562893480062499E-2,5.8936458081006997E-2,3.3297318965196603E-2,3.8297187536954901E-2,5.1949910819530501E-2,3.9584696292877197E-2,5.1575444638729102E-2,9.5663520052149797E-3,1.65227324418049E-2,3.6049529086921397E-2,3.7162508897451797E-2,4.2500157114610498E-2,5.3477487289282401E-3,4.7120247326328697E-2]
["CN-E1L307C1","CN",1,"E1L307C1",346,"L&D Expense, METALLIC ORES",1.6947247087955499E-2,7.1331090293824699E-3,3.3462069928646102E-2,7.0100501179695102E-2,4.2934261262416798E-2,3.86384478770196E-3,4.2152050882577896E-3,8.2664601504802704E-3,2.1994682028889699E-3,1.2440038637219399E-2,8.2511941540468301E-4,0,0,5.0977125450342798E-3,1.33905395969415E-4,0]
["CN-E1L308C1","CN",1,"E1L308C1",347,"L&D Expense, COAL",3.01631726324558E-3,3.2460147049277999E-3,3.05656832642853E-3,4.3408023193478602E-3,3.2279870938509698E-3,3.3305299002677198E-3,4.0287571027874903E-3,3.9105019532144096E-3,2.7237308677285901E-3,2.14346200941452E-3,2.0286106009389702E-3,4.8588212337537899E-3,4.4838032093151596E-3,3.9408800824081098E-3,1.5177075802263499E-3,2.1313169653889401E-3]
["CN-E1L309C1","CN",1,"E1L309C1",348,"L&D Expense, NONMETALLIC MINERALS",6.1751324683427802E-3,6.0367635451257203E-3,6.24764291569591E-3,1.1238164268434001E-2,1.2882996350526799E-2,1.0773151181638199E-2,1.14579824730754E-2,5.6324019096791701E-3,5.2316985093057199E-3,7.1841635102270198E-3,1.9460853891206499E-3,2.9566385317463602E-3,2.6945083219701502E-3,3.9923515321203399E-3,1.2879584932098101E-3,2.5697714472261999E-3]
["CN-E1L310C1","CN",1,"E1L310C1",349,"L&D Expense, FOOD AND KINDRED PRODUCTS",0.112814217805862,0.10337255895137799,0.15115562081337,0.103318996727467,7.9335421323776203E-2,8.1889294087886796E-2,0.113200463354588,0.10237280279398001,0.105734661221504,0.155869352854069,0.14200791172845001,0.110538880168726,0.16084816368765401,0.19031238664048999,0.105766987771637,0.100991336079819]
["CN-E1L311C1","CN",1,"E1L311C1",350,"L&D Expense, FRESH MEATS",0,0,0,0,6.0307089239358902E-2,0.14437814056873299,0.18296842277049999,0,0,0,0,0,0,0,0,0]
["CN-E1L312C1","CN",1,"E1L312C1",351,"L&D Expense, DAIRY PRODUCTS",0.26197466254234297,1.34666740894318,1.7574552297592201,0.46422058343887301,0.35715392231941201,0.464790970087051,0.49275985360145602,0.75572431087493896,1.05871522426605,2.0809273501940702,0.96986246387669905,0.98166953399452095,2.6580326093429498,4.3113833540049997,3.8502678120262801,1.82206074815941]
["CN-E1L313C1","CN",1,"E1L313C1",352,"L&D Expense, CANNED FRUITS/VEG",0.61201786994934104,0.45836937427520802,0.54955309629440297,0.46772405505180398,0.268973708152771,0.44812881946563698,0.364413142204285,0.32465270161628701,0.30047565698623702,0.54309701066336802,0.60036280662191399,0.59926710243978698,0.57379621654754098,0.79501823483980005,0.40052818960853498,0.33041247966923698]
["CN-E1L314C1","CN",1,"E1L314C1",353,"L&D Expense, GRAIN MILL PRODUCTS",3.1477384269237497E-2,6.5411634743213695E-2,8.0874219536781297E-2,6.5766513347625705E-2,5.2350562065839802E-2,5.79447709023952E-2,4.7625388950109503E-2,4.8314291983842898E-2,3.0080657452344901E-2,3.5506442073018903E-2,4.5023558881849897E-2,2.2275958202964401E-2,3.7569787654383499E-2,3.02891444533398E-2,2.6234808790303401E-2,6.1752196822825997E-2]
["CN-E1L315C1","CN",1,"E1L315C1",354,"L&D Expense, FLOUR",3.2923668622970602E-2,7.6696105301380199E-2,8.2328729331493405E-2,4.6068139374256099E-2,6.2322694808244698E-2,7.4686713516712203E-2,7.1782425045967102E-2,5.7252213358879103E-2,2.7048252522945401E-2,5.3978262161745102E-2,8.1389778583540101E-2,2.0658939350466098E-2,5.6218799270150201E-2,4.7762989723968197E-2,5.6966833978788899E-2,5.6377434374590599E-2]
["CN-E1L316C1","CN",1,"E1L316C1",355,"L&D Expense, PREPARED FEEDS",3.4461708273738601E-3,5.2915900945663501E-2,8.3416014909744304E-2,6.4005493186414198E-3,6.4121750183403501E-3,1.0765590704977499E-3,1.48906651884317E-2,1.21511137112975E-2,5.0596832297742401E-3,3.2849257204589803E-2,1.38959473594921E-2,6.32190753961661E-3,2.7778759021351199E-2,1.08453877778599E-3,2.5196986440421701E-5,1.02066313274846E-3]
["CN-E1L317C1","CN",1,"E1L317C1",356,"L&D Expense, CEREALS",0.13801950216293299,0.150457173585892,0.113301411271095,0.12655127048492401,0.114000834524632,5.6761432439088801E-2,2.6986366137862199E-2,9.9266923964023604E-2,4.1428942233324099E-2,2.69035785859623E-2,7.1618623461894307E-2,1.92697768762677E-2,5.9594076037541001E-2,1.39432972578182E-3,9.1593963957775203E-4,6.4883822884699701E-3]
["CN-E1L318C1","CN",1,"E1L318C1",357,"L&D Expense, RICE",0.18275606632232699,0.20021592080593101,0.26043739914894098,0.49083593487739602,0.26900073885917702,0.26474368572235102,0.105855084955692,0.30795875191688499,0.195555880665779,0.171957354616004,0.217271284411443,0.20353585332434401,0.10460667322949101,0.201985129218855,0.18705377019309699,0.27474099401881502]
["CN-E1L319C1","CN",1,"E1L319C1",358,"L&D Expense, PREPARED FLOUR",0.37972217798232999,0.44714790582656899,0.31831541657447798,0.25416249036788902,0.14075364172458599,4.0416184812784202E-2,0.17804516851902,0,0,0,0,0,0,0,0,0]
["CN-E1L320C1","CN",1,"E1L320C1",359,"L&D Expense, CORN PRODUCTS",1.34091908112168E-2,3.9376903325319297E-2,4.7181513160467099E-2,2.6431472972035401E-2,2.73294728249311E-2,3.8074269890785203E-2,3.7078451365232502E-2,1.75428669899702E-2,2.01527439057827E-2,4.1817161674595404E-3,1.34790764147741E-2,4.3508653131181197E-3,9.0233417435583996E-3,3.9086462228574504E-3,3.02978423330987E-5,2.0180023840311999E-2]
["CN-E1L321C1","CN",1,"E1L321C1",360,"L&D Expense, REFINED SUGAR",2.7943493798375098E-2,0.16404953598976099,3.96022871136665E-2,0.10142989456653601,3.3815246075391797E-2,7.3806062340736403E-2,0.14849175512790699,8.2387849688529996E-2,0.25767901539802601,0.19669764508510401,3.2387171869427901E-3,4.3898923629163901E-2,7.3782916037265098E-2,3.3899308291411599E-2,1.4090874839876401E-2,0.11818608416618399]
["CN-E1L322C1","CN",1,"E1L322C1",361,"L&D Expense, BEER",0.21311140060424799,0.13795143365859999,0.11230556666851001,0.209407404065132,0.334010690450668,0.38553339242935197,0.90072369575500499,0.90642565488815297,0.56750947237014804,1.0174552404741599,1.7311441019848299,1.9743613882701201,3.1530590569508399,8.7245439934215394,2.5082539988572998,1.4391021304396601]
["CN-E1L323C1","CN",1,"E1L323C1",362,"L&D Expense, WINES",0.84492164850234996,8.3208911120891599E-2,1.34687983989716,0.44220030307769798,0.205625951290131,6.3485205173492404E-2,0.24367405474185899,0.51581692695617698,0.34035617113113398,1.35427260144433,0.24422654004494099,0.105158524452878,0.36028833717952002,0.267506679227699,0.16329456182654101,0.12703334188972801]
["CN-E1L324C1","CN",1,"E1L324C1",363,"L&D Expense, WHISKEY",0.15329632163047799,4.5956458896398503E-2,1.3157946057617701E-2,0.17441810667514801,0.113551504909992,6.6947758197784396E-2,9.6811883151531206E-2,5.2685525268316297E-2,0.73190534114837602,0.41291941120203002,0.301251651267823,2.16556871024641E-2,2.35566983096023E-2,8.2224230857488294E-3,0.14673836468771501,6.9431467804815294E-2]
["CN-E1L325C1","CN",1,"E1L325C1",364,"L&D Expense, MISC FOOD PREPARATIONS",4.9347322434186901E-2,3.9073646068572998E-2,6.88051283359528E-2,4.7288753092288999E-2,7.3226988315582303E-2,4.44420874118805E-2,5.8179348707199097E-2,6.4795158803462996E-2,6.5988443791866302E-2,4.7256400580346102E-2,0.10027194560448401,5.8322594141169803E-2,4.7792372956870097E-2,4.0860279141872603E-2,3.6097560727487002E-2,5.5607518381965003E-2]
["CN-E1L326C1","CN",1,"E1L326C1",365,"L&D Expense, ALL OTHER FOOD PRODUCTS",9.1888576745986897E-2,7.9573296010494204E-2,0.12117470800876599,6.5014228224754306E-2,3.6592349410057103E-2,4.3420534580946003E-2,0.141043856739998,5.3964279592037201E-2,5.3006786853075E-2,7.9923448269122996E-2,9.9097557048061696E-2,8.1842532444312499E-2,0.19285248625642101,0.17873068167745801,0.111427994915152,8.3245180810300995E-2]
["CN-E1L327C1","CN",1,"E1L327C1",366,"L&D Expense, TOBACCO PRODUCTS",0,0,0,0,3.18567967414856,0,0,0,0,0,0,0,0,0,0,0]
["CN-E1L328C1","CN",1,"E1L328C1",367,"L&D Expense, LUMBER AND WOOD EX FURNITURE",6.4082108438014998E-2,6.3597209751606001E-2,4.2465981096029302E-2,5.5317327380180401E-2,2.6106728240847601E-2,4.5685745775699602E-2,2.36855149269104E-2,3.1761787831783302E-2,2.2764811292290701E-2,5.5634208764431099E-2,6.8785233747138505E-2,4.2106313382289699E-2,5.85751816640947E-2,5.6718723912763502E-2,5.8628574900259398E-2,0.141446267912923]
["CN-E1L329C1","CN",1,"E1L329C1",368,"L&D Expense, LUMBER/DIMENSION STOCK",6.9662675261497498E-2,6.6921301186084706E-2,5.0744507461786298E-2,4.2644336819648701E-2,2.0643839612603201E-2,7.3353521525859805E-2,1.56366545706987E-2,3.8499526679515797E-2,2.4210380390286401E-2,6.5480499825039798E-2,6.5441979456708904E-2,6.6382032559786502E-2,9.6643513669763995E-2,3.5730563075364201E-2,7.45180514067776E-2,0.18957337341988301]
["CN-E1L330C1","CN",1,"E1L330C1",369,"L&D Expense, PLYWOOD OR VENEER",7.4905700981617002E-2,4.27759401500225E-2,8.9939765632152599E-2,0.12727469205856301,8.0512069165706607E-2,9.6415840089321095E-2,4.3528910726308802E-2,3.7447415292263003E-2,2.03599594533443E-2,0.12145549472462901,0.216664798239351,2.9783990826895802E-2,7.0972097170494602E-2,6.9536828674594306E-2,6.8338321410531103E-2,0.117691760964366]
["CN-E1L331C1","CN",1,"E1L331C1",370,"L&D Expense, ALL OTHER LUMBER AND WOOD PRODUCTS",5.6283235549926799E-2,6.4753077924251598E-2,2.6934949681162799E-2,5.1356635987758602E-2,1.97196342051029E-2,1.67441107332706E-2,2.6319015771150599E-2,2.49072927981615E-2,2.19722930341959E-2,3.42567023876479E-2,4.1458401381328898E-2,2.14436371930571E-2,1.7770680455502699E-2,7.2241755483112693E-2,4.1882590552649701E-2,9.6173132143614795E-2]
["CN-E1L332C1","CN",1,"E1L332C1",371,"L&D Expense, FURNITURE AND FIXTURES",1.01506423950195,4.2289190292358398,3.8702409267425502,1.72642862796783,1.0335067510604901,0.56756269931793202,1.8485848903655999,0.51095122098922696,0.77477347850799605,0.87920951704397499,0.29486340670581901,0.40993634402058698,0.171194339057925,0.29584487614604099,0.37153646834541698,2.0288792699200302]
[{"$f":"B1346&\"-\"&D1346","v":"CN-E1L333C1"},"CN",1,"E1L333C1",372,"L&D Expense, PULP, PAPER AND ALLIED PRODUCTS",0.26838248968124401,0.28085958957672102,0.29805308580398598,0.29972025752067599,0.20974843204021501,0.18133181333541901,0.162495583295822,0.17467743158340501,0.16834378242492701,0.12844722302166001,0.153450512751615,0.17213338337717099,0.106044886035222,0.12062119539989299,8.5510400889075799E-2,0.144576608542514]
["CN-E1L334C1","CN",1,"E1L334C1",373,"L&D Expense, NEWSPRINT",0.386345565319061,0.26457613706588701,0.24139791727066001,0.40231353044509899,0.33147549629211398,0.257203638553619,0.141914248466492,8.8899778202176094E-3,0.17850668728351601,0.192825144881663,9.4011005829416405E-2,0.20472030566705901,3.1076594371090002E-2,1.2324784383151699,2.51977665787704E-2,0.16148795459672499]
["CN-E1L335C1","CN",1,"E1L335C1",374,"L&D Expense, PRINTING PAPER",0.45069688558578502,0.77085703611373901,0.80805128812789895,0.78840303421020497,0.60578840970992998,0.33505225181579601,0.42516347765922502,0.31435161828994801,0.37708187103271501,0.39925658646490703,0.66945896095312996,1.11723782584026,0.58951542221150599,0.19435054877364999,0.121608076937136,0.190232288385774]
["CN-E1L336C1","CN",1,"E1L336C1",375,"L&D Expense, FIBREBD/PAPERDB/PULPDB",0.247822120785713,0.201040908694267,0.26354819536209101,0.315349161624908,0.22802263498306299,0.206928014755249,0.15028686821460699,0.219723805785179,0.196718350052834,0.13845131328341401,0.14237568256028199,0.14370424430854201,9.1790883821594699E-2,8.6933569886294401E-2,7.6629285275818401E-2,0.17068400098040601]
["CN-E1L337C1","CN",1,"E1L337C1",376,"L&D Expense, COV PAPER/PAPERBOARD",0.14351396262645699,2.3441700264811498E-2,5.0217267125844997E-2,4.3607987463474301E-2,3.0316181480884601E-2,3.9156388491392101E-2,6.6796630620956393E-2,3.8177575916051899E-2,0.123719930648804,8.9984059162479299E-2,4.7553798615383003E-2,9.2495401211793692E-3,6.3031332334864496E-3,3.4192846214227003E-2,6.3265511684125697E-2,8.0745058269087004E-3]
["CN-E1L338C1","CN",1,"E1L338C1",377,"L&D Expense, SANITARY TISSUES",0.122947245836258,3.0709726270288199E-3,6.65031932294369E-3,6.80103600025177E-2,1.2522803619503999E-2,0,0.10232835263013799,1.07538355514407E-2,9.4120344147086091E-3,2.9207028751322198E-2,1.1900797086969101E-3,1.39013832183855E-2,0,5.0166042535151603E-3,1.23663771402875E-3,4.3280785841464898E-3]
["CN-E1L339C1","CN",1,"E1L339C1",378,"L&D Expense, ALL OTHER PULP, PAPER & ALLIED PRODUCTS",0.17567807435989399,0.195987403392792,0.152946561574936,0.107534527778625,7.8239731490612002E-2,8.5699714720249204E-2,0.122758314013481,8.2997627556324005E-2,7.0808172225952107E-2,5.6488843821234702E-2,7.3495363821740795E-2,3.9105518177458103E-2,5.0811760324324599E-2,0.14501322871120401,0.100518870925555,0.10260932363021701]
["CN-E1L340C1","CN",1,"E1L340C1",379,"L&D Expense, CHEMICALS",5.11742942035198E-2,4.20025512576103E-2,3.6974240094423301E-2,4.2966037988662699E-2,3.3213671296834897E-2,4.8909343779087101E-2,5.0282698124647099E-2,3.2089069485664402E-2,3.1751915812492398E-2,3.2152053773539503E-2,4.5385256484858798E-2,3.7555629213460701E-2,3.01283549154009E-2,4.3525262911993302E-2,4.1050292308664603E-2,4.8456104800754497E-2]
["CN-E1L341C1","CN",1,"E1L341C1",380,"L&D Expense, INDUSTRIAL CHEMICALS",8.7614255025982891E-3,1.6192162409424799E-2,8.6116092279553396E-3,8.3545334637165104E-3,7.8697837889194506E-3,2.1585958078503598E-2,2.21712626516819E-2,1.10827656462789E-2,7.03930715098977E-3,7.1057580517135304E-3,1.15099133183999E-2,1.2581535809645E-2,1.27504083238833E-2,8.6896402574811304E-3,1.4742717925468E-2,1.0810643549472299E-2]
["CN-E1L342C1","CN",1,"E1L342C1",381,"L&D Expense, POTASSIUM OR SODIUM",2.7809889987111099E-2,1.60602275282145E-2,1.1788333766162401E-2,1.4397126622498001E-2,2.13480275124311E-2,1.2410043738782401E-2,9.0565774589776993E-3,7.6568066142499404E-3,1.3412986882031E-2,8.5684775629813106E-3,2.6314574467900101E-2,1.10570170436835E-2,1.12225187459802E-2,1.60371523159329E-2,1.1939958424653599E-2,5.9931752529763698E-3]
["CN-E1L343C1","CN",1,"E1L343C1",382,"L&D Expense, SYN FIBRES/RESINS/RUBBER",0.14274440705776201,6.1173558235168499E-2,8.7265506386756897E-2,0.10607888549566299,8.5183314979076399E-2,0.12817049026489299,0.132741883397102,9.0175598859787001E-2,0.100434817373753,8.3801154952120302E-2,0.11696684497985201,0.106955975079934,5.2621767832795201E-2,0.10260436617034099,6.5752737420087498E-2,0.139082763813134]
["CN-E1L344C1","CN",1,"E1L344C1",383,"L&D Expense, MISC CHEMICALS PRODUCTS",4.3860375881195103E-2,5.9413857758045197E-2,5.3479108959436403E-2,6.6045254468917805E-2,5.3832165896892499E-2,6.0841087251901599E-2,1.3048115186393301E-2,3.7528481334447902E-2,7.7735278755426398E-3,5.2866308194148698E-2,6.3770333647115898E-3,9.4641084932867905E-3,5.7108239653403999E-3,4.0468951069907904E-3,3.7185460949404302E-2,2.3238877916688001E-2]
["CN-E1L345C1","CN",1,"E1L345C1",384,"L&D Expense, ALL OTHER CHEMICALS",2.6043361052870799E-2,0.102892324328423,5.1314171403646497E-2,5.8835830539464999E-2,4.2031995952129399E-2,1.8057033419609101E-2,2.5860302150249499E-2,7.7346088364720301E-3,2.08973791450262E-2,2.2599386791942899E-2,5.1338501809845997E-2,4.6916238257755201E-4,7.0031947197344305E-2,9.0754973556344501E-2,0.11058293551930599,1.91782433824856E-2]
["CN-E1L346C1","CN",1,"E1L346C1",385,"L&D Expense, PETROLEUM OR COAL PRODUCTS",5.6120855733752303E-3,2.0458623766899098E-2,1.4187679626047601E-2,1.6730939969420398E-2,9.0988166630268097E-3,2.5490145199000801E-3,7.7201277017593401E-3,7.4020400643348703E-3,7.5389896519482101E-3,2.8806192440008001E-3,3.97382980853935E-3,1.3481022730943801E-2,7.8551231896560793E-3,6.7912819925897497E-3,5.4264531937212798E-3,1.17302843534858E-2]
["CN-E1L347C1","CN",1,"E1L347C1",386,"L&D Expense, RUBBER AND MISC PLASTICS",0.121731825172901,8.4463320672512096E-2,5.7188738137483597E-2,2.3528395220637301E-2,1.31647260859609E-2,7.10021182894707E-2,0.156284719705582,9.4427227973938002E-2,0.101616881787777,2.8642241838434401E-2,2.2199691128442101E-2,1.54454766150119E-2,6.0183038438072003E-3,9.8465346002906795E-2,4.7641514960962097E-2,3.8674507534544302E-2]
["CN-E1L348C1","CN",1,"E1L348C1",387,"L&D Expense, RUBBER TIRES/INNER TUBES",0.134509116411209,8.9131239801645296E-3,1.7789637669920901E-2,4.3709573219530301E-4,6.3215277623385202E-4,0.12824502587318401,0.20823356509208699,0.172246068716049,0.101569473743439,5.1709465437767201E-2,4.1918087269156301E-3,3.8097494457809397E-2,6.2541206245703999E-3,5.4441562535281901E-2,7.61084379992156E-2,9.8839377049493804E-2]
["CN-E1L349C1","CN",1,"E1L349C1",388,"L&D Expense, ALL OTHER RUBBER PRODUCTS",0.11405962705612201,0.128890320658684,8.23671519756317E-2,3.9198044687509502E-2,2.3228943347930901E-2,2.2845545783638999E-2,0.11083518713712701,3.211560100317E-2,0.101654149591923,1.32252519852178E-2,3.40125415840088E-2,1.0177256724421E-3,5.8682357893787302E-3,0.123604358744922,3.6994674618663702E-2,1.0509528840878701E-2]
["CN-E1L350C1","CN",1,"E1L350C1",389,"L&D Expense, STONE, CLAY AND GLASS PRODUCTS",2.8050996363163001E-2,2.94760055840015E-2,2.3014681413769701E-2,2.2323321551084501E-2,1.25137800350785E-2,2.0365133881568898E-2,1.3885203748941401E-2,1.2379656545817901E-2,2.0123468711972198E-2,1.8672422852622099E-2,1.5618687233242201E-2,7.1743035945493697E-3,1.00761913642266E-2,1.1213559823315599E-2,1.4322538640667201E-2,1.0220925283838099E-2]
["CN-E1L351C1","CN",1,"E1L351C1",390,"L&D Expense, FLAT GLASS",7.9960972070693997E-2,0,0,4.9382718279957797E-3,0,0,0,0,0.24076983332634,7.4834149668299293E-2,0,0,0,2.46638667305578E-3,0,1.26070110068464E-2]
["CN-E1L352C1","CN",1,"E1L352C1",391,"L&D Expense, NONMETALLIC EARTH/MIN",3.5418793559074402E-2,2.9506977647542999E-2,3.24249938130379E-2,3.4120228141546201E-2,1.8458276987075799E-2,2.4468347430229201E-2,2.0480075851082798E-2,2.0243378356099101E-2,2.5672337040305099E-2,2.5089518608720399E-2,3.77997396445496E-2,7.6303684431867002E-3,1.4583935379803001E-2,1.4303699383296E-2,4.0311754906339203E-3,1.3603944578531899E-2]
["CN-E1L353C1","CN",1,"E1L353C1",392,"L&D Expense, ALL OTHER STONE & CLAY, GLASS PRODUCTS",2.3819899186492001E-2,2.95029655098915E-2,1.7426427453756301E-2,1.5901990234851799E-2,9.0113366022705997E-3,1.7641941085457798E-2,1.0626674629747901E-2,8.8174836710095406E-3,1.7466975376009899E-2,1.6213023466090899E-2,8.0123522222395605E-3,7.0282422645380101E-3,8.5392018813610897E-3,1.00639728338627E-2,1.8205648733177902E-2,8.8792988187615506E-3]
["CN-E1L354C1","CN",1,"E1L354C1",393,"L&D Expense, PRIMARY METAL PRODUCTS",3.4512434154748903E-2,5.7771623134613002E-2,4.6246688812971101E-2,0.105558961629868,4.7241918742656701E-2,4.59798015654087E-2,3.2263457775116001E-2,3.3330846577882801E-2,3.9058309048414203E-2,4.5040043560047503E-2,3.8303111795328998E-2,5.8488123741768101E-2,4.45886648461584E-2,8.2227833513675699E-2,4.9633379412000397E-2,6.0209103013003903E-2]
["CN-E1L355C1","CN",1,"E1L355C1",394,"L&D Expense, PRIMARY IRON/STEEL PRODUCTS",3.4884344786405598E-2,5.3362432867288603E-2,3.6286663264036199E-2,9.7192518413066906E-2,4.7952342778444297E-2,4.3800264596939101E-2,2.8834400698542598E-2,3.0930418521165799E-2,4.0773164480924599E-2,4.32040643335612E-2,3.8559282806765002E-2,6.04644823038471E-2,4.9514510216627401E-2,7.8182518416237898E-2,1.5334172940485001E-2,4.9781753141333498E-2]
["CN-E1L356C1","CN",1,"E1L356C1",395,"L&D Expense, ALUMINUM BASIC SHAPES",0.11286199837923,0.15163244307041199,0.19129206240177199,0.99977880716323897,9.2738665640354198E-2,0.365030497312546,0.13654950261116,0.40275806188583402,4.6725824475288398E-2,0.427446876899923,7.1842447765894907E-2,6.1801981514728398E-2,2.36256029762279E-4,0.97019829399741397,1.4380682533099101,1.67692641734201]
["CN-E1L357C1","CN",1,"E1L357C1",396,"L&D Expense, ALL OTHER PRIMARY METAL PRODUCTS",2.12727766484022E-2,9.5122657716274303E-2,0.135312050580978,4.1251994669437402E-2,3.5979904234409298E-2,3.8908191025257097E-2,5.8396480977535199E-2,1.43697401508689E-2,1.95995084941387E-2,2.3422915187733099E-2,3.1688528748677502E-2,3.7337457772167501E-2,8.8837298846552505E-4,7.0970671331329699E-2,0.279650607967111,9.53012962841015E-2]
["CN-E1L358C1","CN",1,"E1L358C1",397,"L&D Expense, FABRICATED METAL PRODUCTS",0.29441612958908098,8.34800750017166E-2,0.120782092213631,0.57032650709152199,0.127834737300873,0.121632412075996,0.10238241404295,0.34850579500198398,2.4500768631696701E-2,4.4205237424147302E-2,4.1813711219508103E-2,0.13085792181979899,5.4769202978317402E-2,0.17031496412081801,3.3467763128923302E-3,0.226221318634625]
["CN-E1L359C1","CN",1,"E1L359C1",398,"L&D Expense, FAB STRUC METAL PRODUCTS",1.3789104223251301,0.26735174655914301,0.109357416629791,0.55470359325408902,0.24174544215202301,0.26759335398674,8.8351674377918202E-2,2.4079890921711901E-2,1.6526019899174599E-3,0.13177579165119599,0.176593743188519,0.36042406768129098,0.20247041874306199,0.685889247456412,6.71721725659165E-3,0.61904499763286203]
["CN-E1L360C1","CN",1,"E1L360C1",399,"L&D Expense, ALL OTHER FAB METAL PRODUCTS",8.2236602902412401E-2,4.22826893627644E-2,0.12317106872797,0.57348483800888095,0.11085592955350899,0.104633316397667,0.104206696152687,0.41068261861801098,2.90865134447813E-2,2.6793860444710701E-2,1.17116840125649E-2,6.1026978151819303E-2,8.3779653724611707E-3,1.9695008077359299E-2,2.3129155730127701E-3,8.2394414457267903E-2]
["CN-E1L361C1","CN",1,"E1L361C1",400,"L&D Expense, MACHINERY EXCEPT ELECTRICAL",0.56518673896789595,0.32207629084587103,0.48734244704246499,0.78966307640075695,0.41966882348060602,0.16947755217552199,0.53890877962112405,0.47151488065719599,0.35861149430275002,0.237905620493821,0.107907509116882,0.111111250301434,0.57319507395133296,0.40923914491589602,4.4424753803321601E-2,0.24683393968713699]
["CN-E1L362C1","CN",1,"E1L362C1",401,"L&D Expense, ENGINES/TURBINES",0,0,0,0.65623474121093806,0.37552052736282299,3.18804383277893E-2,0.92005145549774203,0.18546940386295299,0.75826698541641202,0.10592373868414701,1.7432681007613301E-2,0.11374880081262601,0.19588503448769101,0.627909057749931,-6.83448356503671E-4,0.166006178271392]
["CN-E1L363C1","CN",1,"E1L363C1",402,"L&D Expense, FARM MACHINERY",2.4298570156097399,1.5298203229904199,1.5081578493118299,2.9845852851867698,1.5362756252288801,0.99220669269561801,0.70848298072814897,1.0776067972183201,0.70382529497146595,1.3448171672090701,0.559861487070207,0.61976011384427698,0.13272710665462301,0.15808913426766,0,0.16933120027486401]
["CN-E1L364C1","CN",1,"E1L364C1",403,"L&D Expense, CONST MIN/MAT HAND MACHINERY",5.3824152797460598E-2,0.14556503295898399,0.225022718310356,0.24387198686599701,0.111423380672932,1.9659049808979E-2,9.3566169962286897E-3,0.25835311412811302,9.0812714770436304E-3,2.4417359235743799E-2,0.226980429468987,0.123886814731048,5.6786413195415104,5.5626533761732502E-2,0.50608937133810405,2.0688925659798598]
["CN-E1L365C1","CN",1,"E1L365C1",404,"L&D Expense, ALL OTHER MACHINERY EXCEPT ELECTRICAL",0.51521039009094205,0.112866580486298,0.80271893739700295,0.47596234083175698,0.30874112248420699,4.8945009708404499E-2,0.31174495816230802,0.42183950543403598,4.2986869812011701E-3,0.15186131419488499,9.5799168819499E-2,2.66155263257274E-3,0.14928714522905701,0.14762019602208301,5.02985279069205E-2,3.62333789688866E-2]
["CN-E1L366C1","CN",1,"E1L366C1",405,"L&D Expense, ELECTRICAL MACHINERY",0.67479163408279397,0.47035461664199801,0.76611125469207797,0.65651184320449796,0.56727981567382801,0.21725417673587799,0.49147397279739402,0.91961038112640403,0.289804667234421,0.44987594767502198,0.21864727922893701,0.110947990600422,0.399700701714716,0.218458461333112,0.13409182722392801,1.67087861140951]
["CN-E1L367C1","CN",1,"E1L367C1",406,"L&D Expense, ELECTRICAL TRANS/DIST EQUIPMENT",4.9571437835693404,1.3843834400177,1.5912679433822601,0.52243554592132602,0.95162492990493797,1.35360562801361,0.46107843518257102,0.55019402503967296,0.73037481307983398,2.4718954756265998,0.72087862382857204,0.437231102871734,8.2663145076920408,0,1.4978214029207599,2.3871011726206701]
["CN-E1L368C1","CN",1,"E1L368C1",407,"L&D Expense, HOUSEHOLD APPLIANCES",0.205303609371185,0.23462562263011899,0.17131142318248699,0.277806997299194,0.25822886824607799,8.2644179463386494E-2,0.297059416770935,0.38408657908439597,0.13108573853969599,0.40999757319887098,0.15451085360087599,7.3435426620840294E-2,0.14930913105378599,0.247363305660388,7.2794077869062196E-2,8.71202277086814E-2]
["CN-E1L369C1","CN",1,"E1L369C1",408,"L&D Expense, RADIO OR TV SETS",6.56506299972534,7.9000549316406303,11.099229812622101,2.6888911724090598,3.2490937709808398,1.53677189350128,5.8817706108093297,24.248622894287099,3.8644213676452601,1.0204034771199,2.4656724349818999,0.16968987712112299,0.212309300578224,0.93635726795096297,0.93072368421052598,7.9683165020530504]
["CN-E1L370C1","CN",1,"E1L370C1",409,"L&D Expense, ALL OTHER ELECTRICAL MACHINERY",0.72443789243698098,0.124912194907665,1.22650158405304,2.0479607582092298,1.4720858335495,2.7940336614847201E-2,2.5568239390850098E-2,0.79280191659927401,0.32959437370300299,0.11638569092668601,0.15527288252874599,0.20274542735457399,3.8295146556108502E-2,0.100668737420884,0.10349523579893,6.5650136035665803]
["CN-E1L371C1","CN",1,"E1L371C1",410,"L&D Expense, TRANSPORTAION EQUIPMENT",1.3006241321563701,1.08988153934479,1.35968601703644,1.2409585714340201,0.75661820173263605,1.0195336341857899,1.6047393083572401,1.7275034189224201,2.29360747337341,1.4390260176603999,1.53309053496067,2.5685685982062201,2.42239663922193,2.64924837876096,2.5732802744444401,3.2399183966489802]
["CN-E1L372C1","CN",1,"E1L372C1",411,"L&D Expense, MOTOR PASSENGER CARS",1.6142339706420901,1.60462009906769,2.0916264057159402,1.80427742004395,1.1449105739593499,1.8661357164382899,2.4315426349639901,2.3879089355468799,2.9647860527038601,2.2775114836972699,2.3379065129382699,4.7704088395188302,3.82250992141388,3.6264625356952398,4.5673487040649103,7.7164689836323603]
["CN-E1L373C1","CN",1,"E1L373C1",412,"L&D Expense, MOTOR TRUCKS",2.1043250560760498,1.26811671257019,1.65900325775146,1.4032484292984,0.97844052314758301,0.82795894145965598,2.6402244567871098,2.5844602584838898,5.3508419990539604,2.3972440890440101,2.5053101151001802,3.01905989333518,4.5072670290018699,1.8358317475753301,1.9620481392513101,6.0876948799235704]
["CN-E1L374C1","CN",1,"E1L374C1",413,"L&D Expense, MOTOR VECHICLE PARTS",0.17642442882060999,0.27078187465667702,0.25748610496521002,0.82535320520401001,0.14550699293613401,0.17560070753097501,0.17617671191692399,0.84027493000030495,0.21214038133621199,8.8219921107315594E-2,0.393716560465393,0.212999234670077,0.10576437246174999,0.119489105755487,4.6983042073175697E-3,5.2852034619368202E-2]
["CN-E1L375C1","CN",1,"E1L375C1",414,"L&D Expense, ALL OTHER TRANSPORTATION EQUIPMENT",2.6227355003356899E-2,0.10049141198396699,3.2508585602045101E-2,6.5525375306606307E-2,0.26267328858375499,3.3132839947938898E-2,5.0899308174848598E-2,6.18039257824421E-2,9.2528991401195498E-2,3.1585700434175697E-2,7.6281476545512997E-2,0.119202553620429,7.6049686090451901E-2,4.0474509693458502,2.3140971066584299,1.6999942051205801E-2]
["CN-E1L376C1","CN",1,"E1L376C1",415,"L&D Expense, FREIGHT FORWARDER TRAFFIC",3.4748416393995299E-2,0.119148962199688,0.133060157299042,6.0009412467479699E-2,2.6239469647407501E-2,5.6703973561525303E-2,0.39763507246971103,0.102938175201416,0.42134848237037698,0.183535784884371,6.4649280290004899E-2,1.21218522459901E-2,9.2906133987932099E-3,3.4791419592622302E-2,1.53999961012668E-2,7.4345374257392599E-2]
["CN-E1L377C1","CN",1,"E1L377C1",416,"L&D Expense, SHIPPER ASSOCIATION TRAFFIC",6.9035097956657396E-2,4.24118414521217E-2,0,0,0,0,0.15256458520889299,0,0,0,0,3.9752304352468099E-2,0,1.2640222416189799E-2,0,0]
["CN-E1L378C1","CN",1,"E1L378C1",417,"L&D Expense, MISC MIXED SHIPMENTS",9.1315463185310405E-2,0.11395051330328,0.119482338428497,7.6815418899059296E-2,6.5753631293773707E-2,4.5803453773260103E-2,6.1025261878967299E-2,5.9127628803253202E-2,6.1889201402664198E-2,4.37200018110191E-2,7.5652365651906694E-2,3.3229987868641203E-2,3.2905317083349601E-2,3.0981519923329901E-2,4.4879455499843499E-2,4.5587054201045099E-2]
["CN-E1L379C1","CN",1,"E1L379C1",418,"L&D Expense, MISC MIXED SHIPMENTS NEC INC TOFC",9.1119572520256001E-2,0.112067364156246,0.119818732142448,7.3888465762138394E-2,6.1532124876975999E-2,4.5287456363439602E-2,6.1175230890512501E-2,5.8978945016860997E-2,5.8081496506929398E-2,4.2502426273880303E-2,7.4517811883176202E-2,3.2837985738498998E-2,3.2487919273463603E-2,1.9547644020149899E-2,3.9562979823806702E-2,4.5379167595824103E-2]
["CN-E1L380C1","CN",1,"E1L380C1",419,"L&D Expense, ALL OTHER MIXED SHIPMENTS",0.16601713001728099,0.88630723953247104,1.4442171668633799E-3,0.87179607152938798,0.75372087955474898,0.13352239131927501,3.1231531873345399E-2,9.3002393841743497E-2,1.03999447822571,0.416805851183083,0.345811739282818,0.14978310418351601,0.18150323928185,3.82302116571379,1.53221325354683,0.10334428935010299]
["CN-E1L381C1","CN",1,"E1L381C1",420,"L&D Expense, HAZARDOUS MATERIALS",3.3822157420218E-3,4.38846610486507E-2,6.9866083562374101E-2,4.1437070816755302E-2,3.1556442379951498E-2,2.9638551175594299E-2,1.43746230751276E-2,2.3880230262875599E-2,1.29652125760913E-2,2.8145488342284499E-2,1.9073883682287199E-2,6.4705703700832298E-3,1.8164087945304101E-2,3.0475595834185201E-2,1.6340194747313699E-2,2.5929638549913699E-2]
["CN-E1L382C1","CN",1,"E1L382C1",421,"L&D Expense, ALL OTHER COMMODITIES",3.7811581045389203E-2,0.571766257286072,0.50435817241668701,0.395120829343796,0.34854763746261602,0.28982281684875499,1.35337150096893,0.27479436993598899,2.1931312978267701E-2,0.35576115206112802,1.58875264111078,0.37422378104875798,0.25508157108880503,0.88390067928004001,0.16117152606319499,2.4966038048811998]
["CN-E2L101C1","CN",1,"E2L101C1",422,"Average Tare Weight, BOX - 40 FT",26.200000762939499,26.200000762939499,25.899999618530298,25.299999237060501,26,25.700000762939499,29,28.5,28.5,28.5,27.9,27.5,29,29,29.2,29.2]
["CN-E2L101C2","CN",1,"E2L101C2",423,"E/L Ratio, Railroad-Owned, BOX - 40 FT",1.9905751943588299,1.9910314083099401,1.98044109344482,2.0674772262573198,1.9863142967224099,2.01117610931396,2.0061690807342498,1.9499489068985001,1.97714602947235,1.9993702770780899,1.96461824953445,1.9943502824858801,1.94369721614013,1.8647030651340999,1.8796178343948999,1.88336755646817]
["CN-E2L101C3","CN",1,"E2L101C3",424,"E/L Ratio, Privately-Owned, BOX - 40 FT",1.5385514497757,1.4681880474090601,1.3517699241638199,1.79009902477264,1.90848588943481,1.57208693027496,1.9226932525634799,2.3177282810211199,2.1452682018279998,1.92463958060288,1.92242114236999,1.91553328561203,2.3668430335097002,2.2533889468195998,2.05023255813953,2.0472334682861]
["CN-E2L101C4","CN",1,"E2L101C4",425,"E/L Ratio, All Freight Cars, BOX - 40 FT",1.7849423885345499,1.8170310258865401,1.7536579370498699,2.0023255348205602,1.9691176414489699,1.81489109992981,1.97853899002075,2.09690284729004,2.0579206943511998,1.96274887604367,1.9468390804597699,1.9630786708321499,2.0544908797044599,1.9372930866601801,1.9113223854796899,1.92159949622166]
["CN-E2L101C5","CN",1,"E2L101C5",426,"Local circuity, BOX - 40 FT",1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999]
["CN-E2L101C6","CN",1,"E2L101C6",427,"Interline circuity, BOX - 40 FT",1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001]
["CN-E2L101C7","CN",1,"E2L101C7",428,"Average circuity, BOX - 40 FT",1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999]
["CN-E2L101C8","CN",1,"E2L101C8",429,"Spotted-to-Pulled Ratio, BOX - 40 FT",1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.8,1.8,1.8,1.8,1.8,1.8,1.8]
["CN-E2L101C9","CN",1,"E2L101C9",430,"CD per Industry Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L101C10","CN",1,"E2L101C10",431,"CD per Interchange Switch, BOX - 40 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L101C11","CN",1,"E2L101C11",432,"CD per Intraterminal Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L101C12","CN",1,"E2L101C12",433,"CD per Interterminal Switch, BOX - 40 FT",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L101C13","CN",1,"E2L101C13",434,"CD per I&I Switch, BOX - 40 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L101C14","CN",1,"E2L101C14",435,"CD per Load & Unload Industry Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
[{"$f":"B1410&\"-\"&D1410","v":"CN-E2L101C15"},"CN",1,"E2L101C15",436,"CD per Load & Unload Intraterminal Switch, BOX - 40 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L101C16","CN",1,"E2L101C16",437,"CD per Load & Unload Interterminal Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L101C17","CN",1,"E2L101C17",438,"CM per Industry Switch, BOX - 40 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L101C18","CN",1,"E2L101C18",439,"CM per Interchange Switch, BOX - 40 FT",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L101C19","CN",1,"E2L101C19",440,"CM per Intraterminal Switch, BOX - 40 FT",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L101C20","CN",1,"E2L101C20",441,"CM per Interterminal Switch, BOX - 40 FT",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L101C21","CN",1,"E2L101C21",442,"CM per I&I Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L101C22","CN",1,"E2L101C22",443,"Average CM per CD, Railroad-Owned, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E2L101C23","CN",1,"E2L101C23",444,"Average Miles between I&I Switches, BOX - 40 FT",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L101C24","CN",1,"E2L101C24",445,"Average Miles between Interchange Switches, BOX - 40 FT",495.435791015625,336.39437866210898,322.10842895507801,311.52020263671898,346.42794799804699,249.59208679199199,214.66181945800801,278.37808227539102,299.09994506835898,166.432739696982,198.03419904654999,242.25389408579699,476.03249970673897,619.30762456244099,623.37282104409701,592.43665710760604]
["CN-E2L101C25","CN",1,"E2L101C25",446,"SEMs per Industry Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E2L101C26","CN",1,"E2L101C26",447,"SEMs per Interchange Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E2L101C27","CN",1,"E2L101C27",448,"SEMs per Intraterminal Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E2L101C28","CN",1,"E2L101C28",449,"SEMs per Interterminal Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E2L101C29","CN",1,"E2L101C29",450,"SEMs per I&I Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CN-E2L102C1","CN",1,"E2L102C1",451,"Average Tare Weight, BOX - 50 FT",33.5,33.900001525878899,34.099998474121101,34.200000762939503,34.5,34.299999237060497,32.599998474121101,32.700000762939503,32.799999237060497,32.799999999999997,32.9,33,33.200000000000003,33.4,33.6,34]
["CN-E2L102C2","CN",1,"E2L102C2",452,"E/L Ratio, Railroad-Owned, BOX - 50 FT",1.9905751943588299,1.9910314083099401,1.98044109344482,2.0674772262573198,1.9863142967224099,2.01117610931396,2.0061690807342498,1.9499489068985001,1.97714602947235,1.9993702770780899,1.96461824953445,1.9943502824858801,1.94369721614013,1.8647030651340999,1.8796178343948999,1.88336755646817]
["CN-E2L102C3","CN",1,"E2L102C3",453,"E/L Ratio, Privately-Owned, BOX - 50 FT",1.5385514497757,1.4681880474090601,1.3517699241638199,1.79009902477264,1.90848588943481,1.57208693027496,1.9226932525634799,2.3177282810211199,2.1452682018279998,1.92463958060288,1.92242114236999,1.91553328561203,2.3668430335097002,2.2533889468195998,2.05023255813953,2.0472334682861]
["CN-E2L102C4","CN",1,"E2L102C4",454,"E/L Ratio, All Freight Cars, BOX - 50 FT",1.7849423885345499,1.8170310258865401,1.7536579370498699,2.0023255348205602,1.9691176414489699,1.81489109992981,1.97853899002075,2.09690284729004,2.0579206943511998,1.96274887604367,1.9468390804597699,1.9630786708321499,2.0544908797044599,1.9372930866601801,1.9113223854796899,1.92159949622166]
["CN-E2L102C5","CN",1,"E2L102C5",455,"Local circuity, BOX - 50 FT",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["CN-E2L102C6","CN",1,"E2L102C6",456,"Interline circuity, BOX - 50 FT",1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001]
["CN-E2L102C7","CN",1,"E2L102C7",457,"Average circuity, BOX - 50 FT",1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999]
["CN-E2L102C8","CN",1,"E2L102C8",458,"Spotted-to-Pulled Ratio, BOX - 50 FT",1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.8,1.8,1.8,1.8,1.8,1.8,1.8]
["CN-E2L102C9","CN",1,"E2L102C9",459,"CD per Industry Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L102C10","CN",1,"E2L102C10",460,"CD per Interchange Switch, BOX - 50 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L102C11","CN",1,"E2L102C11",461,"CD per Intraterminal Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L102C12","CN",1,"E2L102C12",462,"CD per Interterminal Switch, BOX - 50 FT",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L102C13","CN",1,"E2L102C13",463,"CD per I&I Switch, BOX - 50 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L102C14","CN",1,"E2L102C14",464,"CD per Load & Unload Industry Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L102C15","CN",1,"E2L102C15",465,"CD per Load & Unload Intraterminal Switch, BOX - 50 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L102C16","CN",1,"E2L102C16",466,"CD per Load & Unload Interterminal Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L102C17","CN",1,"E2L102C17",467,"CM per Industry Switch, BOX - 50 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L102C18","CN",1,"E2L102C18",468,"CM per Interchange Switch, BOX - 50 FT",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L102C19","CN",1,"E2L102C19",469,"CM per Intraterminal Switch, BOX - 50 FT",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L102C20","CN",1,"E2L102C20",470,"CM per Interterminal Switch, BOX - 50 FT",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L102C21","CN",1,"E2L102C21",471,"CM per I&I Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L102C22","CN",1,"E2L102C22",472,"Average CM per CD, Railroad-Owned, BOX - 50 FT",832.70574951171898,838.40826416015602,803.459228515625,985.422607421875,877.11328125,813.18524169921898,783.69476318359398,752.58532714843795,757.49157714843795,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L102C23","CN",1,"E2L102C23",473,"Average Miles between I&I Switches, BOX - 50 FT",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L102C24","CN",1,"E2L102C24",474,"Average Miles between Interchange Switches, BOX - 50 FT",495.435791015625,336.39437866210898,322.10842895507801,311.52020263671898,346.42794799804699,249.59208679199199,214.66181945800801,278.37808227539102,299.09994506835898,166.432739696982,198.03419904654999,242.25389408579699,476.03249970673897,619.30762456244099,623.37282104409701,592.43665710760604]
["CN-E2L102C25","CN",1,"E2L102C25",475,"SEMs per Industry Switch, BOX - 50 FT",6.5772333145141602,6.1651020050048801,5.9204263687133798,5.26851606369019,4.4945411682128897,4.5362834930419904,4.2201857566833496,3.8595821857452401,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L102C26","CN",1,"E2L102C26",476,"SEMs per Interchange Switch, BOX - 50 FT",3.6174778938293501,3.3908064365386998,3.2562344074249299,2.89768385887146,2.4719977378845202,2.49495601654053,2.3211021423339799,2.12277030944824,1.9858651161193801,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L102C27","CN",1,"E2L102C27",477,"SEMs per Intraterminal Switch, BOX - 50 FT",9.8658494949340803,9.2476539611816406,8.8806400299072301,7.9027738571167001,6.7418112754821804,6.8044242858886701,6.3302783966064498,5.7893738746643102,5.4159960746765101,4.7527343927396304,4.5217903658888003,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L102C28","CN",1,"E2L102C28",478,"SEMs per Interterminal Switch, BOX - 50 FT",7.89267921447754,7.3981237411498997,7.1045122146606401,6.3222193717956499,5.3934493064880398,5.4435405731201199,5.0642228126525897,4.6314992904663104,4.3327970504760698,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L102C29","CN",1,"E2L102C29",479,"SEMs per I&I Switch, BOX - 50 FT",1.64430820941925,1.54127550125122,1.4801067113876301,1.3171290159225499,1.12363541126251,1.1340708732605,1.0550464391708401,0.96489560604095503,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L103C1","CN",1,"E2L103C1",480,"Average Tare Weight, BOX - EQUIPPED",36.099998474121101,36.099998474121101,36.200000762939503,36.099998474121101,36.200000762939503,36.200000762939503,36.400001525878899,36.5,36.5,36.5,36.6,36.700000000000003,36.799999999999997,37,37.1,37.299999999999997]
["CN-E2L103C2","CN",1,"E2L103C2",481,"E/L Ratio, Railroad-Owned, BOX - EQUIPPED",1.8847314119339,1.86826980113983,1.8554439544677701,1.8319610357284499,1.8242172002792401,1.8287609815597501,1.8202990293502801,1.8019940853118901,1.8192487955093399,1.8529376474823001,1.8230933143922601,1.89879720003944,1.8961869023120701,1.86322841289729,1.9027743543395499,1.84234003864075]
["CN-E2L103C3","CN",1,"E2L103C3",482,"E/L Ratio, Privately-Owned, BOX - EQUIPPED",1.7342439889907799,1.789266705513,1.8450524806976301,1.7002096176147501,1.6715440750122099,1.63823413848877,1.78583252429962,1.7664203643798799,1.7568992376327499,1.7190830945558699,1.80439495467087,1.9419233078836799,1.90499351491569,1.87837606837607,1.7814580991092299,1.8058281077093301]
["CN-E2L103C4","CN",1,"E2L103C4",483,"E/L Ratio, All Freight Cars, BOX - EQUIPPED",1.8801136016845701,1.8653969764709499,1.85507524013519,1.8282955884933501,1.8184463977813701,1.8211814165115401,1.8183795213699301,1.79928803443909,1.81190598011017,1.8330523914116901,1.81965579710145,1.9084225238852,1.8982121884379499,1.86671652659962,1.8735959730426801,1.83218805768087]
["CN-E2L103C5","CN",1,"E2L103C5",484,"Local circuity, BOX - EQUIPPED",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["CN-E2L103C6","CN",1,"E2L103C6",485,"Interline circuity, BOX - EQUIPPED",1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999]
["CN-E2L103C7","CN",1,"E2L103C7",486,"Average circuity, BOX - EQUIPPED",1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999]
["CN-E2L103C8","CN",1,"E2L103C8",487,"Spotted-to-Pulled Ratio, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L103C9","CN",1,"E2L103C9",488,"CD per Industry Switch, BOX - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L103C10","CN",1,"E2L103C10",489,"CD per Interchange Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L103C11","CN",1,"E2L103C11",490,"CD per Intraterminal Switch, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L103C12","CN",1,"E2L103C12",491,"CD per Interterminal Switch, BOX - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L103C13","CN",1,"E2L103C13",492,"CD per I&I Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L103C14","CN",1,"E2L103C14",493,"CD per Load & Unload Industry Switch, BOX - EQUIPP",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L103C15","CN",1,"E2L103C15",494,"CD per Load & Unload Intraterminal Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L103C16","CN",1,"E2L103C16",495,"CD per Load & Unload Interterminal Switch, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L103C17","CN",1,"E2L103C17",496,"CM per Industry Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L103C18","CN",1,"E2L103C18",497,"CM per Interchange Switch, BOX - EQUIPPED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L103C19","CN",1,"E2L103C19",498,"CM per Intraterminal Switch, BOX - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L103C20","CN",1,"E2L103C20",499,"CM per Interterminal Switch, BOX - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
[{"$f":"B1474&\"-\"&D1474","v":"CN-E2L103C21"},"CN",1,"E2L103C21",500,"CM per I&I Switch, BOX - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L103C22","CN",1,"E2L103C22",501,"Average CM per CD, Railroad-Owned, BOX - EQUIPPED",832.70574951171898,838.408203125,803.459228515625,985.42266845703102,877.11334228515602,813.18518066406295,783.69476318359398,752.58532714843795,757.49157714843795,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L103C23","CN",1,"E2L103C23",502,"Average Miles between I&I Switches, BOX - EQUIPPED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L103C24","CN",1,"E2L103C24",503,"Average Miles between Interchange Switches, BOX - EQUIPPED",406.67715454101602,343.84353637695301,345.85070800781301,346.92929077148398,345.77014160156301,341.35900878906301,261.51373291015602,283.29653930664102,302.37109375,210.073957280126,175.49211049671399,179.369289495327,185.06010785429399,197.51779988727401,216.698303232022,207.75075023530599]
["CN-E2L103C25","CN",1,"E2L103C25",504,"SEMs per Industry Switch, BOX - EQUIPPED",6.5772333145141602,6.1651020050048801,5.9204268455505398,5.26851606369019,4.4945411682128897,4.5362834930419904,4.2201857566833496,3.8595821857452401,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L103C26","CN",1,"E2L103C26",505,"SEMs per Interchange Switch, BOX - EQUIPPED",3.6174778938293501,3.3908064365386998,3.2562344074249299,2.89768362045288,2.4719977378845202,2.49495577812195,2.3211021423339799,2.12277054786682,1.9858651161193801,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L103C27","CN",1,"E2L103C27",506,"SEMs per Intraterminal Switch, BOX - EQUIPPED",9.8658494949340803,9.2476539611816406,8.8806390762329102,7.9027743339538601,6.7418117523193404,6.8044252395629901,6.3302779197692898,5.7893743515014604,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L103C28","CN",1,"E2L103C28",507,"SEMs per Interterminal Switch, BOX - EQUIPPED",7.89267921447754,7.3981232643127397,7.1045126914978001,6.3222188949584996,5.3934493064880398,5.4435405731201199,5.0642228126525897,4.6314992904663104,4.3327965736389196,3.8021875141916999,3.6174322927110301,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L103C29","CN",1,"E2L103C29",508,"SEMs per I&I Switch, BOX - EQUIPPED",1.64430820941925,1.54127538204193,1.4801065921783401,1.3171290159225499,1.12363529205322,1.13407099246979,1.0550463199615501,0.96489566564559903,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L104C1","CN",1,"E2L104C1",509,"Average Tare Weight, GONDOLA - PLAIN",26,25.899999618530298,25.799999237060501,25.600000381469702,25.5,25.600000381469702,25.299999237060501,25.700000762939499,25.700000762939499,25.6,25.6,25.6,25.7,25.9,26.1,26.3]
["CN-E2L104C2","CN",1,"E2L104C2",510,"E/L Ratio, Railroad-Owned, GONDOLA - PLAIN",2.0175755023956299,2.0490517616271999,2.0765321254730198,2.0365936756134002,1.9925776720046999,1.99639785289764,1.99855148792267,2.0583658218383798,1.92853283882141,1.9975557153127199,1.96713615023474,1.94046121593291,1.99594972067039,2.0287631831256001,2.02173061863743,2.0054719562243499]
["CN-E2L104C3","CN",1,"E2L104C3",511,"E/L Ratio, Privately-Owned, GONDOLA - PLAIN",2.0212371349334699,2.0100352764129599,2.0240433216095002,2.03002905845642,2.0305550098419198,2.0432436466217001,2.10431003570557,2.0773437023162802,2.0312309265136701,2.4238546997877899,2.0648189539561899,2.0882547232131099,2.1172971686890301,2.0454545454545499,2.1097543859649099,2.0500494839530599]
["CN-E2L104C4","CN",1,"E2L104C4",512,"E/L Ratio, All Freight Cars, GONDOLA - PLAIN",2.0204670429229701,2.0176122188568102,2.0358948707580602,2.0314738750457799,2.0205838680267298,2.0277726650238002,2.07136011123657,2.0712907314300502,2.0012614727020299,2.2948165556861202,2.0266004490101399,2.0311208363724802,2.0614801490427901,2.0382873610539298,2.07299926428513,2.0298738487733199]
["CN-E2L104C5","CN",1,"E2L104C5",513,"Local circuity, GONDOLA - PLAIN",1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.093,1.093,1.093,1.093,1.093,1.093,1.093]
["CN-E2L104C6","CN",1,"E2L104C6",514,"Interline circuity, GONDOLA - PLAIN",1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.151,1.151,1.151,1.151,1.151,1.151,1.151]
["CN-E2L104C7","CN",1,"E2L104C7",515,"Average circuity, GONDOLA - PLAIN",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["CN-E2L104C8","CN",1,"E2L104C8",516,"Spotted-to-Pulled Ratio, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L104C9","CN",1,"E2L104C9",517,"CD per Industry Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L104C10","CN",1,"E2L104C10",518,"CD per Interchange Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L104C11","CN",1,"E2L104C11",519,"CD per Intraterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L104C12","CN",1,"E2L104C12",520,"CD per Interterminal Switch, GONDOLA - PLAIN",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L104C13","CN",1,"E2L104C13",521,"CD per I&I Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L104C14","CN",1,"E2L104C14",522,"CD per Load & Unload Industry Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L104C15","CN",1,"E2L104C15",523,"CD per Load & Unload Intraterminal Switch, GONDOLA - PLAIN",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L104C16","CN",1,"E2L104C16",524,"CD per Load & Unload Interterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L104C17","CN",1,"E2L104C17",525,"CM per Industry Switch, GONDOLA - PLAIN",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L104C18","CN",1,"E2L104C18",526,"CM per Interchange Switch, GONDOLA - PLAIN",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L104C19","CN",1,"E2L104C19",527,"CM per Intraterminal Switch, GONDOLA - PLAIN",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L104C20","CN",1,"E2L104C20",528,"CM per Interterminal Switch, GONDOLA - PLAIN",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L104C21","CN",1,"E2L104C21",529,"CM per I&I Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L104C22","CN",1,"E2L104C22",530,"Average CM per CD, Railroad-Owned, GONDOLA - PLAIN",832.70587158203102,838.408203125,803.459228515625,985.42272949218795,877.11328125,813.18524169921898,783.69476318359398,752.58532714843795,757.49157714843795,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L104C23","CN",1,"E2L104C23",531,"Average Miles between I&I Switches, GONDOLA - PLAIN",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L104C24","CN",1,"E2L104C24",532,"Average Miles between Interchange Switches, GONDOLA - PLAIN",215.96461486816401,317.44866943359398,302.76312255859398,184.98091125488301,147.56962585449199,132.62754821777301,151.43119812011699,183.97880554199199,113.963455200195,79.206491712696703,61.548609413685298,73.037055161446801,70.895792547235502,70.403726245195699,76.665561900818005,79.953119613814195]
["CN-E2L104C25","CN",1,"E2L104C25",533,"SEMs per Industry Switch, GONDOLA - PLAIN",6.5772333145141602,6.1651020050048801,5.9204268455505398,5.26851606369019,4.4945406913757298,4.5362834930419904,4.2201852798461896,3.8595821857452401,3.6106636524200399,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L104C26","CN",1,"E2L104C26",534,"SEMs per Interchange Switch, GONDOLA - PLAIN",3.6174778938293501,3.3908064365386998,3.2562341690063499,2.89768385887146,2.4719974994659402,2.49495577812195,2.3211021423339799,2.12277054786682,1.9858652353286701,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L104C27","CN",1,"E2L104C27",535,"SEMs per Intraterminal Switch, GONDOLA - PLAIN",9.8658494949340803,9.2476539611816406,8.8806400299072301,7.9027743339538601,6.7418117523193404,6.8044247627258301,6.3302788734436,5.7893743515014604,5.4159951210021999,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L104C28","CN",1,"E2L104C28",536,"SEMs per Interterminal Switch, GONDOLA - PLAIN",7.89267921447754,7.3981232643127397,7.10451316833496,6.3222188949584996,5.3934493064880398,5.4435410499572798,5.0642232894897496,4.6314997673034703,4.3327970504760698,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L104C29","CN",1,"E2L104C29",537,"SEMs per I&I Switch, GONDOLA - PLAIN",1.64430820941925,1.54127550125122,1.4801065921783401,1.3171291351318399,1.12363529205322,1.1340708732605,1.0550464391708401,0.96489566564559903,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L105C1","CN",1,"E2L105C1",538,"Average Tare Weight, GONDOLA - EQUIPPED",33.099998474121101,33.200000762939503,33.400001525878899,33.299999237060497,33.299999237060497,33.299999237060497,33.299999237060497,33.099998474121101,33.099998474121101,33.200000000000003,33.200000000000003,33.1,33.1,33.1,33.1,33.1]
["CN-E2L105C2","CN",1,"E2L105C2",539,"E/L Ratio, Railroad-Owned, GONDOLA - EQUIPPED",2.17748022079468,2.0679802894592298,2.0247993469238299,2.0784540176391602,2.01729083061218,2.07761549949646,2.1123628616332999,2.1410453319549601,1.9989960193634,2.01420202378839,2.0287788663401001,2.0034644889878699,1.9981795155928399,2.0923841059602601,2.0932211976897399,2.0800915331807799]
["CN-E2L105C3","CN",1,"E2L105C3",540,"E/L Ratio, Privately-Owned, GONDOLA - EQUIPPED",2.0086033344268799,2.0233628749847399,2.0089859962463401,2.0407509803771999,2.0318641662597701,2.0766479969024698,2.0151212215423602,2.04132032394409,2.0226995944976802,1.96011999294159,2.0304540420819501,2.05909771932745,2.0757450331125802,2.0763283666010701,2.0518226332970602,2.0652542372881402]
["CN-E2L105C4","CN",1,"E2L105C4",541,"E/L Ratio, All Freight Cars, GONDOLA - EQUIPPED",2.1516864299774201,2.0625538825988801,2.0228695869445801,2.0715692043304399,2.01946020126343,2.0774712562561,2.0949344635009801,2.1250252723693799,2.0028784275054901,2.0006204023752501,2.0293175074184,2.0218974076116898,2.0264560909365299,2.08643326039387,2.07554729690494,2.0742368509052702]
["CN-E2L105C5","CN",1,"E2L105C5",542,"Local circuity, GONDOLA - EQUIPPED",1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001]
["CN-E2L105C6","CN",1,"E2L105C6",543,"Interline circuity, GONDOLA - EQUIPPED",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["CN-E2L105C7","CN",1,"E2L105C7",544,"Average circuity, GONDOLA - EQUIPPED",1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.119,1.119,1.119,1.119,1.119,1.119,1.119]
["CN-E2L105C8","CN",1,"E2L105C8",545,"Spotted-to-Pulled Ratio, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L105C9","CN",1,"E2L105C9",546,"CD per Industry Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L105C10","CN",1,"E2L105C10",547,"CD per Interchange Switch, GONDOLA - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L105C11","CN",1,"E2L105C11",548,"CD per Intraterminal Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L105C12","CN",1,"E2L105C12",549,"CD per Interterminal Switch, GONDOLA - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L105C13","CN",1,"E2L105C13",550,"CD per I&I Switch, GONDOLA - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L105C14","CN",1,"E2L105C14",551,"CD per Load & Unload Industry Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L105C15","CN",1,"E2L105C15",552,"CD per Load & Unload Intraterminal Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L105C16","CN",1,"E2L105C16",553,"CD per Load & Unload Interterminal Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L105C17","CN",1,"E2L105C17",554,"CM per Industry Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L105C18","CN",1,"E2L105C18",555,"CM per Interchange Switch, GONDOLA - EQUIPPED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L105C19","CN",1,"E2L105C19",556,"CM per Intraterminal Switch, GONDOLA - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L105C20","CN",1,"E2L105C20",557,"CM per Interterminal Switch, GONDOLA - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L105C21","CN",1,"E2L105C21",558,"CM per I&I Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L105C22","CN",1,"E2L105C22",559,"Average CM per CD, Railroad-Owned, GONDOLA - EQUIPPED",832.70574951171898,838.40814208984398,803.459228515625,985.422607421875,877.11334228515602,813.18518066406295,783.69482421875,752.58532714843795,757.49157714843795,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L105C23","CN",1,"E2L105C23",560,"Average Miles between I&I Switches, GONDOLA - EQUIPPED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L105C24","CN",1,"E2L105C24",561,"Average Miles between Interchange Switches, GONDOLA - EQUIPPED",523.89239501953102,402.14291381835898,410.830810546875,502.12564086914102,843.927734375,534.23138427734398,555.218017578125,780.24658203125,542.62921142578102,284.58243401516597,278.319737841814,218.377784972174,237.40564689745801,206.60275112836501,273.32928503008202,242.87281617718099]
["CN-E2L105C25","CN",1,"E2L105C25",562,"SEMs per Industry Switch, GONDOLA - EQUIPPED",6.5772328376770002,6.1651020050048801,5.9204263687133798,5.2685165405273402,4.4945411682128897,4.5362834930419904,4.2201857566833496,3.8595821857452401,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L105C26","CN",1,"E2L105C26",563,"SEMs per Interchange Switch, GONDOLA - EQUIPPED",3.6174781322479199,3.3908061981201199,3.2562341690063499,2.89768385887146,2.4719977378845202,2.49495601654053,2.3211021423339799,2.12277054786682,1.9858652353286701,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
[{"$f":"B1538&\"-\"&D1538","v":"CN-E2L105C27"},"CN",1,"E2L105C27",564,"SEMs per Intraterminal Switch, GONDOLA - EQUIPPED",9.8658494949340803,9.2476520538330096,8.8806390762329102,7.9027743339538601,6.7418107986450204,6.8044242858886701,6.3302788734436,5.7893743515014604,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L105C28","CN",1,"E2L105C28",565,"SEMs per Interterminal Switch, GONDOLA - EQUIPPED",7.8926796913146999,7.3981232643127397,7.1045117378234899,6.3222193717956499,5.3934493064880398,5.4435400962829599,5.0642232894897496,4.6314992904663104,4.3327970504760698,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L105C29","CN",1,"E2L105C29",566,"SEMs per I&I Switch, GONDOLA - EQUIPPED",1.64430832862854,1.54127538204193,1.4801067113876301,1.3171290159225499,1.12363529205322,1.1340708732605,1.0550463199615501,0.96489560604095503,0.90266591310501099,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L106C1","CN",1,"E2L106C1",567,"Average Tare Weight, HOPPER - COVERED",31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.200000762939499,31.100000381469702,31,30.8,30.8,30.8,30.8,30.8,30.8,30.9]
["CN-E2L106C2","CN",1,"E2L106C2",568,"E/L Ratio, Railroad-Owned, HOPPER - COVERED",2.0491888523101802,2.0324745178222701,2.09728956222534,2.0617535114288299,2.0335450172424299,2.10721015930176,2.0861868858337398,2.1005299091339098,2.09647417068481,2.1410018552875698,2.0712143611404401,2.0262578121487298,2.0611135466900499,2.0524010448061101,2.0645261293179802,2.1739091439078]
["CN-E2L106C3","CN",1,"E2L106C3",569,"E/L Ratio, Privately-Owned, HOPPER - COVERED",2.0487573146820099,2.02796483039856,2.1014938354492201,2.06874799728394,2.0831549167633101,2.10292625427246,2.0518202781677202,2.05488133430481,2.0608077049255402,2.0893762332166301,2.0624040098962202,2.0567990205028499,2.0702955615219598,2.0751704460129101,2.0517158144587002,2.1236804075734201]
["CN-E2L106C4","CN",1,"E2L106C4",570,"E/L Ratio, All Freight Cars, HOPPER - COVERED",2.0489189624786399,2.0294649600982702,2.10016942024231,2.0668272972106898,2.0689830780029301,2.1040525436401398,2.0588943958282502,2.0644826889038099,2.0667750835418701,2.0970824949698201,2.06356740476323,2.0535405043677701,2.0692527533807299,2.0722094481605402,2.0534002632161301,2.12971493532033]
["CN-E2L106C5","CN",1,"E2L106C5",571,"Local circuity, HOPPER - COVERED",1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999]
["CN-E2L106C6","CN",1,"E2L106C6",572,"Interline circuity, HOPPER - COVERED",1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999]
["CN-E2L106C7","CN",1,"E2L106C7",573,"Average circuity, HOPPER - COVERED",1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999]
["CN-E2L106C8","CN",1,"E2L106C8",574,"Spotted-to-Pulled Ratio, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L106C9","CN",1,"E2L106C9",575,"CD per Industry Switch, HOPPER - COVERED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L106C10","CN",1,"E2L106C10",576,"CD per Interchange Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L106C11","CN",1,"E2L106C11",577,"CD per Intraterminal Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L106C12","CN",1,"E2L106C12",578,"CD per Interterminal Switch, HOPPER - COVERED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L106C13","CN",1,"E2L106C13",579,"CD per I&I Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L106C14","CN",1,"E2L106C14",580,"CD per Load & Unload Industry Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L106C15","CN",1,"E2L106C15",581,"CD per Load & Unload Intraterminal Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L106C16","CN",1,"E2L106C16",582,"CD per Load & Unload Interterminal Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L106C17","CN",1,"E2L106C17",583,"CM per Industry Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L106C18","CN",1,"E2L106C18",584,"CM per Interchange Switch, HOPPER - COVERED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L106C19","CN",1,"E2L106C19",585,"CM per Intraterminal Switch, HOPPER - COVERED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L106C20","CN",1,"E2L106C20",586,"CM per Interterminal Switch, HOPPER - COVERED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L106C21","CN",1,"E2L106C21",587,"CM per I&I Switch, HOPPER - COVERED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L106C22","CN",1,"E2L106C22",588,"Average CM per CD, Railroad-Owned, HOPPER - COVERED",832.705810546875,838.408203125,803.459228515625,985.42272949218795,877.11328125,813.18524169921898,783.69476318359398,752.58532714843795,757.49151611328102,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L106C23","CN",1,"E2L106C23",589,"Average Miles between I&I Switches, HOPPER - COVERED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L106C24","CN",1,"E2L106C24",590,"Average Miles between Interchange Switches, HOPPER - COVERED",631.62530517578102,757.58758544921898,675.37567138671898,639.92572021484398,690.77105712890602,647.768310546875,620.41632080078102,571.75451660156295,685.18914794921898,336.65950745894901,372.83921517216203,416.08422238373402,385.12129492753201,512.39115789114703,465.04034025978302,513.66059585713003]
["CN-E2L106C25","CN",1,"E2L106C25",591,"SEMs per Industry Switch, HOPPER - COVERED",6.5772328376770002,6.1651024818420401,5.9204263687133798,5.26851606369019,4.4945411682128897,4.5362830162048304,4.2201852798461896,3.8595824241638201,3.6106636524200399,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L106C26","CN",1,"E2L106C26",592,"SEMs per Interchange Switch, HOPPER - COVERED",3.6174776554107702,3.3908066749572798,3.2562341690063499,2.89768385887146,2.4719974994659402,2.49495577812195,2.3211019039154102,2.12277054786682,1.9858652353286701,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L106C27","CN",1,"E2L106C27",593,"SEMs per Intraterminal Switch, HOPPER - COVERED",9.8658485412597692,9.2476530075073207,8.8806390762329102,7.9027748107910201,6.7418107986450204,6.8044252395629901,6.3302774429321298,5.7893738746643102,5.4159960746765101,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L106C28","CN",1,"E2L106C28",594,"SEMs per Interterminal Switch, HOPPER - COVERED",7.89267921447754,7.3981227874755904,7.1045126914978001,6.3222188949584996,5.3934493064880398,5.4435400962829599,5.0642228126525897,4.6314992904663104,4.3327965736389196,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L106C29","CN",1,"E2L106C29",595,"SEMs per I&I Switch, HOPPER - COVERED",1.64430820941925,1.54127550125122,1.4801065921783401,1.3171290159225499,1.12363517284393,1.1340708732605,1.0550463199615501,0.96489560604095503,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L107C1","CN",1,"E2L107C1",596,"Average Tare Weight, HOPPER - OPEN TOP - GENERAL",29.799999237060501,29.700000762939499,29.600000381469702,29.600000381469702,29.5,29.600000381469702,29.399999618530298,29.200000762939499,29,28.9,28.8,28.8,28.7,28.5,28.4,28.3]
["CN-E2L107C2","CN",1,"E2L107C2",597,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.9281190633773799,2.02834177017212,2.02031373977661,2.01968622207642,2.0071318149566699,1.99061822891235,1.99708652496338,1.9964975118637101,2.01496529579163,2.0097295750464998,2.0415730337078699,2.0453172205438102,1.9859133126935,2.0160827110855801,1.94339996041955,1.9913611250627801]
["CN-E2L107C3","CN",1,"E2L107C3",598,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - GENERAL",2.0722839832305899,1.9245952367782599,2.0696554183960001,1.99266529083252,1.9868255853653001,1.97575128078461,2.01121950149536,2.0301253795623802,2.0155999660491899,1.9954502667084999,2.0023192887514498,1.9770533312232901,1.99797533591018,2.0106827682303798,1.9860181173690401,1.9984967622571701]
["CN-E2L107C4","CN",1,"E2L107C4",599,"E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - GENERAL",1.9794216156005899,1.9791452884674099,2.0402088165283199,2.00622653961182,1.9952894449234,1.9834443330764799,2.0066270828247101,2.0143847465515101,2.01530909538269,2.00291850632343,2.0237635917221999,2.0111040609137101,1.99142352644413,2.0136425648021801,1.9647616227420801,1.9946782776971499]
["CN-E2L107C5","CN",1,"E2L107C5",600,"Local circuity, HOPPER - OPEN TOP - GENERAL",1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001]
["CN-E2L107C6","CN",1,"E2L107C6",601,"Interline circuity, HOPPER - OPEN TOP - GENERAL",1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.137,1.137,1.137,1.137,1.137,1.137,1.137]
["CN-E2L107C7","CN",1,"E2L107C7",602,"Average circuity, HOPPER - OPEN TOP - GENERAL",1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001]
["CN-E2L107C8","CN",1,"E2L107C8",603,"Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L107C9","CN",1,"E2L107C9",604,"CD per Industry Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L107C10","CN",1,"E2L107C10",605,"CD per Interchange Switch, HOPPER - OPEN TOP - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L107C11","CN",1,"E2L107C11",606,"CD per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L107C12","CN",1,"E2L107C12",607,"CD per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L107C13","CN",1,"E2L107C13",608,"CD per I&I Switch, HOPPER - OPEN TOP - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L107C14","CN",1,"E2L107C14",609,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L107C15","CN",1,"E2L107C15",610,"CD per Load & Unload Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L107C16","CN",1,"E2L107C16",611,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L107C17","CN",1,"E2L107C17",612,"CM per Industry Switch, HOPPER - OPEN TOP - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L107C18","CN",1,"E2L107C18",613,"CM per Interchange Switch, HOPPER - OPEN TOP - GENERAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L107C19","CN",1,"E2L107C19",614,"CM per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L107C20","CN",1,"E2L107C20",615,"CM per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L107C21","CN",1,"E2L107C21",616,"CM per I&I Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L107C22","CN",1,"E2L107C22",617,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",832.70574951171898,838.408203125,803.45916748046898,985.422607421875,877.11328125,813.18518066406295,783.69476318359398,752.58538818359398,757.49157714843795,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L107C23","CN",1,"E2L107C23",618,"Average Miles between I&I Switches, HOPPER - OPEN TOP - GENERAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L107C24","CN",1,"E2L107C24",619,"Average Miles between Interchange Switches, HOPPER - OPEN TOP - GENERAL",240.185958862305,327.23941040039102,304.89334106445301,324.50640869140602,498.99984741210898,373.17153930664102,920.72863769531295,771.21435546875,615.73309326171898,260.095551728202,530.34837949068299,304.90387334041702,622.58600129330705,1776.8580654288301,1606.8806990099799,4835.72749678939]
["CN-E2L107C25","CN",1,"E2L107C25",620,"SEMs per Industry Switch, HOPPER - OPEN TOP - GENERAL",6.5772333145141602,6.1651024818420401,5.9204263687133798,5.26851606369019,4.4945411682128897,4.5362834930419904,4.2201857566833496,3.8595821857452401,3.6106636524200399,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L107C26","CN",1,"E2L107C26",621,"SEMs per Interchange Switch, HOPPER - OPEN TOP - GENERAL",3.6174776554107702,3.3908064365386998,3.2562346458435099,2.89768362045288,2.4719977378845202,2.49495577812195,2.3211021423339799,2.12277030944824,1.9858651161193801,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L107C27","CN",1,"E2L107C27",622,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",9.8658485412597692,9.2476530075073207,8.8806400299072301,7.9027748107910201,6.7418112754821804,6.8044252395629901,6.3302783966064498,5.7893743515014604,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L107C28","CN",1,"E2L107C28",623,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",7.89267921447754,7.3981232643127397,7.1045117378234899,6.3222184181213397,5.3934493064880398,5.4435405731201199,5.0642228126525897,4.6314992904663104,4.3327965736389196,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L107C29","CN",1,"E2L107C29",624,"SEMs per I&I Switch, HOPPER - OPEN TOP - GENERAL",1.64430820941925,1.54127538204193,1.4801067113876301,1.3171290159225499,1.12363529205322,1.1340708732605,1.0550463199615501,0.96489566564559903,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L108C1","CN",1,"E2L108C1",625,"Average Tare Weight, HOPPER - OPEN TOP - SPECIAL",27.299999237060501,27.399999618530298,26.899999618530298,26.799999237060501,26.700000762939499,26.799999237060501,26.5,26.5,26.399999618530298,26.4,26.4,26.2,26.1,26.1,26,26]
["CN-E2L108C2","CN",1,"E2L108C2",626,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.0410122871398899,2.0407009124755899,1.9908928871154801,1.9913022518157999,2.00058245658875,1.9857034683227499,2.0001459121704102,2.02291059494019,1.9855324029922501,1.9912667043101799,2.0145449092817498,2.0063434853126698,2.00953433743264,2.0124571554933102,2.0179994337256799,1.9984346628263701]
["CN-E2L108C3","CN",1,"E2L108C3",627,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - SPECIAL",2.0449383258819598,2.0591487884521502,2.0520906448364298,2.0147516727447501,2.01876592636108,2.0083525180816699,2.00785136222839,2.0328075885772701,2.0144712924957302,2.0267462621963301,2.0344703877544901,2.0001303384455,2.0098707688569699,2.0130576943360401,2.0121064665533201,2.0106830583130599]
[{"$f":"B1602&\"-\"&D1602","v":"CN-E2L108C4"},"CN",1,"E2L108C4",628,"E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - SPECIAL",2.0423221588134801,2.0459463596343999,2.0093746185302699,2.0036866664886501,2.0101113319396999,1.99806451797485,2.00557637214661,2.0287008285522501,2.0036458969116202,2.0152538652880101,2.0256299376299398,2.0024668266037802,2.0097680355278,2.0128390887869299,2.01458266057073,2.0064664927898601]
["CN-E2L108C5","CN",1,"E2L108C5",629,"Local circuity, HOPPER - OPEN TOP - SPECIAL",1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.202,1.202,1.202,1.202,1.202,1.202,1.202]
["CN-E2L108C6","CN",1,"E2L108C6",630,"Interline circuity, HOPPER - OPEN TOP - SPECIAL",1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999]
["CN-E2L108C7","CN",1,"E2L108C7",631,"Average circuity, HOPPER - OPEN TOP - SPECIAL",1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001]
["CN-E2L108C8","CN",1,"E2L108C8",632,"Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L108C9","CN",1,"E2L108C9",633,"CD per Industry Switch, HOPPER - OPEN TOP - SPECIAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L108C10","CN",1,"E2L108C10",634,"CD per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L108C11","CN",1,"E2L108C11",635,"CD per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L108C12","CN",1,"E2L108C12",636,"CD per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L108C13","CN",1,"E2L108C13",637,"CD per I&I Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L108C14","CN",1,"E2L108C14",638,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L108C15","CN",1,"E2L108C15",639,"CD per Load & Unload Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L108C16","CN",1,"E2L108C16",640,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L108C17","CN",1,"E2L108C17",641,"CM per Industry Switch, HOPPER - OPEN TOP - SPECIAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L108C18","CN",1,"E2L108C18",642,"CM per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L108C19","CN",1,"E2L108C19",643,"CM per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L108C20","CN",1,"E2L108C20",644,"CM per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L108C21","CN",1,"E2L108C21",645,"CM per I&I Switch, HOPPER - OPEN TOP - SPECIAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L108C22","CN",1,"E2L108C22",646,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",832.70574951171898,838.408203125,803.45916748046898,985.42266845703102,877.11340332031295,813.18524169921898,783.69476318359398,752.58532714843795,757.49151611328102,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L108C23","CN",1,"E2L108C23",647,"Average Miles between I&I Switches, HOPPER - OPEN TOP - SPECIAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L108C24","CN",1,"E2L108C24",648,"Average Miles between Interchange Switches, HOPPER - OPEN TOP - SPECIAL",642.41339111328102,610.88134765625,580.92205810546898,497.18185424804699,617.630859375,802.52166748046898,1352.99755859375,1724.21069335938,1628.40209960938,1316.13734493219,1260.42035652341,2367.7199765852902,2561.7210216909102,1948.42147290552,1919.4219997074099,2488.4982472955799]
["CN-E2L108C25","CN",1,"E2L108C25",649,"SEMs per Industry Switch, HOPPER - OPEN TOP - SPECIAL",6.5772328376770002,6.1651020050048801,5.9204268455505398,5.26851606369019,4.4945416450500497,4.5362834930419904,4.2201857566833496,3.8595821857452401,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L108C26","CN",1,"E2L108C26",650,"SEMs per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",3.6174776554107702,3.3908064365386998,3.2562344074249299,2.89768385887146,2.4719977378845202,2.49495601654053,2.3211021423339799,2.12277054786682,1.9858651161193801,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L108C27","CN",1,"E2L108C27",651,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",9.8658494949340803,9.2476539611816406,8.8806390762329102,7.9027743339538601,6.7418107986450204,6.8044247627258301,6.3302779197692898,5.7893743515014604,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L108C28","CN",1,"E2L108C28",652,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",7.89267921447754,7.3981227874755904,7.1045126914978001,6.3222193717956499,5.39345026016235,5.4435405731201199,5.0642232894897496,4.6314992904663104,4.3327965736389196,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L108C29","CN",1,"E2L108C29",653,"SEMs per I&I Switch, HOPPER - OPEN TOP - SPECIAL",1.64430832862854,1.54127550125122,1.4801065921783401,1.3171290159225499,1.12363529205322,1.1340708732605,1.0550463199615501,0.96489566564559903,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L109C1","CN",1,"E2L109C1",654,"Average Tare Weight, REFRIGERATED - MECH",46.099998474121101,46.099998474121101,46.400001525878899,46.599998474121101,46.599998474121101,46.5,46.599998474121101,47,47.200000762939503,47.5,48.2,48.3,48.4,48.6,48.9,49.2]
["CN-E2L109C2","CN",1,"E2L109C2",655,"E/L Ratio, Railroad-Owned, REFRIGERATED - MECH",1.6358268260955799,1.6340425014495801,1.56919646263123,1.5279805660247801,1.54487180709839,1.5466321706771899,1.9896372556686399,2.0972971916198699,1.9569892883300799,1.8767123287671199,1.9537037037036999,1.7976190476190499,1.7922077922077899,1.8857142857142899,1.8837209302325599,1.63380281690141]
["CN-E2L109C3","CN",1,"E2L109C3",656,"E/L Ratio, Privately-Owned, REFRIGERATED - MECH",2.1428570747375502,2.0595238208770801,1.94782602787018,1.86111116409302,1.98181819915771,1.83529412746429,1.5215311050414999,1.38571429252625,1.41269838809967,1.4739583333333299,1.7405857740585799,1.7686832740213501,1.8529411764705901,1.9514237855946399,1.89357798165138,1.9049429657794701]
["CN-E2L109C4","CN",1,"E2L109C4",657,"E/L Ratio, All Freight Cars, REFRIGERATED - MECH",1.64942526817322,1.6985559463501001,1.6465364694595299,1.5776396989822401,1.6103541851043699,1.59872615337372,1.7462686300277701,1.7907692193985001,1.7371795177459699,1.6479289940828401,1.80691642651297,1.77534246575342,1.8425720620842601,1.94452773613193,1.8928571428571399,1.8726968174204399]
["CN-E2L109C5","CN",1,"E2L109C5",658,"Local circuity, REFRIGERATED - MECH",1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.079,1.079,1.079,1.079,1.079,1.079,1.079]
["CN-E2L109C6","CN",1,"E2L109C6",659,"Interline circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["CN-E2L109C7","CN",1,"E2L109C7",660,"Average circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["CN-E2L109C8","CN",1,"E2L109C8",661,"Spotted-to-Pulled Ratio, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L109C9","CN",1,"E2L109C9",662,"CD per Industry Switch, REFRIGERATED - MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L109C10","CN",1,"E2L109C10",663,"CD per Interchange Switch, REFRIGERATED - MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L109C11","CN",1,"E2L109C11",664,"CD per Intraterminal Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L109C12","CN",1,"E2L109C12",665,"CD per Interterminal Switch, REFRIGERATED - MECH",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L109C13","CN",1,"E2L109C13",666,"CD per I&I Switch, REFRIGERATED - MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L109C14","CN",1,"E2L109C14",667,"CD per Load & Unload Industry Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L109C15","CN",1,"E2L109C15",668,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L109C16","CN",1,"E2L109C16",669,"CD per Load & Unload Interterminal Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L109C17","CN",1,"E2L109C17",670,"CM per Industry Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L109C18","CN",1,"E2L109C18",671,"CM per Interchange Switch, REFRIGERATED - MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L109C19","CN",1,"E2L109C19",672,"CM per Intraterminal Switch, REFRIGERATED - MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L109C20","CN",1,"E2L109C20",673,"CM per Interterminal Switch, REFRIGERATED - MECH",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L109C21","CN",1,"E2L109C21",674,"CM per I&I Switch, REFRIGERATED - MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L109C22","CN",1,"E2L109C22",675,"Average CM per CD, Railroad-Owned, REFRIGERATED - MECH",832.705810546875,838.40826416015602,803.45916748046898,985.42254638671898,877.11334228515602,813.18518066406295,783.69482421875,752.58532714843795,757.49157714843795,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L109C23","CN",1,"E2L109C23",676,"Average Miles between I&I Switches, REFRIGERATED - MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L109C24","CN",1,"E2L109C24",677,"Average Miles between Interchange Switches, REFRIGERATED - MECH",275.17132568359398,239.102294921875,252.240158081055,231.546142578125,240.65574645996099,277.87609863281301,236.93704223632801,246.77297973632801,239.81552124023401,196.61834815515999,260.31507876969198,337.67207488355399,354.55974842767301,465.15563182229897,426.08695652173901,450.82098765432102]
["CN-E2L109C25","CN",1,"E2L109C25",678,"SEMs per Industry Switch, REFRIGERATED - MECH",6.5772333145141602,6.1651020050048801,5.9204268455505398,5.2685165405273402,4.4945411682128897,4.5362834930419904,4.2201857566833496,3.8595824241638201,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L109C26","CN",1,"E2L109C26",679,"SEMs per Interchange Switch, REFRIGERATED - MECH",3.6174778938293501,3.3908064365386998,3.2562346458435099,2.89768385887146,2.4719974994659402,2.49495601654053,2.3211021423339799,2.12277054786682,1.9858651161193801,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L109C27","CN",1,"E2L109C27",680,"SEMs per Intraterminal Switch, REFRIGERATED - MECH",9.8658485412597692,9.2476539611816406,8.8806400299072301,7.9027743339538601,6.7418112754821804,6.8044247627258301,6.3302783966064498,5.7893743515014604,5.4159951210021999,4.7527343927396304,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L109C28","CN",1,"E2L109C28",681,"SEMs per Interterminal Switch, REFRIGERATED - MECH",7.89267921447754,7.3981232643127397,7.1045126914978001,6.3222193717956499,5.3934493064880398,5.4435405731201199,5.0642228126525897,4.6314992904663104,4.3327965736389196,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L109C29","CN",1,"E2L109C29",682,"SEMs per I&I Switch, REFRIGERATED - MECH",1.64430820941925,1.54127550125122,1.4801067113876301,1.3171290159225499,1.12363529205322,1.1340708732605,1.0550463199615501,0.96489560604095503,0.90266591310501099,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L110C1","CN",1,"E2L110C1",683,"Average Tare Weight, REFRIGERATED - NON-MECH",42.799999237060497,42.900001525878899,43.099998474121101,43.299999237060497,43.799999237060497,43.400001525878899,44,44.099998474121101,44.099998474121101,44.2,44.2,44.2,44.2,44.2,44.6,45.2]
["CN-E2L110C2","CN",1,"E2L110C2",684,"E/L Ratio, Railroad-Owned, REFRIGERATED - NON-MECH",2.1108870506286599,1.94259822368622,1.9429429769516,1.8560311794280999,1.86341464519501,1.9835164546966599,2.0241935253143302,2.1484375,1.9619047641754199,1.8444444444444399,2.06666666666667,2.125,2.1,2.1071428571428599,1.9473684210526301,2.05714285714286]
["CN-E2L110C3","CN",1,"E2L110C3",685,"E/L Ratio, Privately-Owned, REFRIGERATED - NON-MECH",1.90163934230804,2.0588235855102499,1.9069766998291,1.9056603908538801,2.07142853736877,2.0250000953674299,2,2.0526316165924099,2.0588235855102499,2.4444444444444402,2.0476190476190501,2.0526315789473699,2.0526315789473699,2.3125,1.9615384615384599,2.25]
["CN-E2L110C4","CN",1,"E2L110C4",686,"E/L Ratio, All Freight Cars, REFRIGERATED - NON-MECH",2.0879712104797399,1.9581152200698899,1.9388297796249401,1.8645161390304601,1.9080460071563701,1.9909909963607799,2.0215828418731698,2.1265060901641801,1.9754098653793299,1.94444444444444,2.0606060606060601,2.0980392156862702,2.0886075949367102,2.1818181818181799,1.9555555555555599,2.1176470588235299]
["CN-E2L110C5","CN",1,"E2L110C5",687,"Local circuity, REFRIGERATED - NON-MECH",1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001]
["CN-E2L110C6","CN",1,"E2L110C6",688,"Interline circuity, REFRIGERATED - NON-MECH",1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.159,1.159,1.159,1.159,1.159,1.159,1.159]
["CN-E2L110C7","CN",1,"E2L110C7",689,"Average circuity, REFRIGERATED - NON-MECH",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["CN-E2L110C8","CN",1,"E2L110C8",690,"Spotted-to-Pulled Ratio, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L110C9","CN",1,"E2L110C9",691,"CD per Industry Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
[{"$f":"B1666&\"-\"&D1666","v":"CN-E2L110C10"},"CN",1,"E2L110C10",692,"CD per Interchange Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L110C11","CN",1,"E2L110C11",693,"CD per Intraterminal Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L110C12","CN",1,"E2L110C12",694,"CD per Interterminal Switch, REFRIGERATED - NON-MECH",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L110C13","CN",1,"E2L110C13",695,"CD per I&I Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L110C14","CN",1,"E2L110C14",696,"CD per Load & Unload Industry Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L110C15","CN",1,"E2L110C15",697,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - NON-MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L110C16","CN",1,"E2L110C16",698,"CD per Load & Unload Interterminal Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L110C17","CN",1,"E2L110C17",699,"CM per Industry Switch, REFRIGERATED - NON-MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L110C18","CN",1,"E2L110C18",700,"CM per Interchange Switch, REFRIGERATED - NON-MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L110C19","CN",1,"E2L110C19",701,"CM per Intraterminal Switch, REFRIGERATED - NON-MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L110C20","CN",1,"E2L110C20",702,"CM per Interterminal Switch, REFRIGERATED - NON-MECH",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L110C21","CN",1,"E2L110C21",703,"CM per I&I Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L110C22","CN",1,"E2L110C22",704,"Average CM per CD, Railroad-Owned, REFRIGERATED - NON-MECH",832.70574951171898,838.40814208984398,803.45916748046898,985.42266845703102,877.11328125,813.18524169921898,783.69476318359398,752.58532714843795,757.49157714843795,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L110C23","CN",1,"E2L110C23",705,"Average Miles between I&I Switches, REFRIGERATED - NON-MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L110C24","CN",1,"E2L110C24",706,"Average Miles between Interchange Switches, REFRIGERATED - NON-MECH",700.50164794921898,296.44219970703102,139.012130737305,511.16131591796898,642.86071777343795,90.924842834472699,307.10070800781301,450.35787963867199,223.20611572265599,260.369003690037,532.25806451612902,560.43956043955995,27.521226262233501,392.857142857143,725.80645161290295,472.222222222222]
["CN-E2L110C25","CN",1,"E2L110C25",707,"SEMs per Industry Switch, REFRIGERATED - NON-MECH",6.5772328376770002,6.1651024818420401,5.9204268455505398,5.2685165405273402,4.4945406913757298,4.5362834930419904,4.2201857566833496,3.8595821857452401,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L110C26","CN",1,"E2L110C26",708,"SEMs per Interchange Switch, REFRIGERATED - NON-MECH",3.6174781322479199,3.3908064365386998,3.2562344074249299,2.89768362045288,2.4719974994659402,2.49495601654053,2.3211023807525599,2.12277054786682,1.9858653545379601,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L110C27","CN",1,"E2L110C27",709,"SEMs per Intraterminal Switch, REFRIGERATED - NON-MECH",9.8658494949340803,9.2476530075073207,8.8806400299072301,7.9027743339538601,6.7418107986450204,6.8044252395629901,6.3302779197692898,5.7893748283386204,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L110C28","CN",1,"E2L110C28",710,"SEMs per Interterminal Switch, REFRIGERATED - NON-MECH",7.8926796913146999,7.3981232643127397,7.1045122146606401,6.3222193717956499,5.3934497833251998,5.4435400962829599,5.0642228126525897,4.6314992904663104,4.3327965736389196,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L110C29","CN",1,"E2L110C29",711,"SEMs per I&I Switch, REFRIGERATED - NON-MECH",1.64430820941925,1.54127538204193,1.4801067113876301,1.3171290159225499,1.12363529205322,1.1340708732605,1.0550463199615501,0.96489566564559903,0.90266597270965598,0.79212239878993695,0.75363172764813202,0.75501600530493096,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L111C1","CN",1,"E2L111C1",712,"Average Tare Weight, FLAT - TOFC",58.299999237060497,59.700000762939503,59.400001525878899,59.5,59.099998474121101,59.299999237060497,58.200000762939503,57.799999237060497,57.799999237060497,58.3,58.6,58.6,58.5,58.9,58.7,58.6]
["CN-E2L111C2","CN",1,"E2L111C2",713,"E/L Ratio, Railroad-Owned, FLAT - TOFC",1.2066333293914799,1.2562015056610101,1.1946387290954601,1.1805555820465099,1.14861464500427,1.1925349235534699,1.13502109050751,1.07532227039337,1.1071972846984901,1.05281182408075,1.05837651122625,1.0521808937650501,1.0391511575124801,1.05968346019089,1.06739661167419,1.04517453798768]
["CN-E2L111C3","CN",1,"E2L111C3",714,"E/L Ratio, Privately-Owned, FLAT - TOFC",1.1489504575729399,1.21747994422913,1.1440911293029801,1.1320483684539799,1.1202027797698999,1.16655993461609,1.1228326559066799,1.0667859315872199,1.0934963226318399,1.04544890103067,1.05405451073824,1.0467309799540201,1.03389508362899,1.0349560368861199,1.0521436254673999,1.03828337040589]
["CN-E2L111C4","CN",1,"E2L111C4",715,"E/L Ratio, All Freight Cars, FLAT - TOFC",1.16653275489807,1.2266275882720901,1.1501663923263501,1.13591992855072,1.12251472473145,1.16910147666931,1.1239491701126101,1.0674974918365501,1.0948908329010001,1.0460326987938,1.0544396730849099,1.04748505100246,1.0347197493056099,1.03839180795703,1.0537216333091,1.0391773815443599]
["CN-E2L111C5","CN",1,"E2L111C5",716,"Local circuity, FLAT - TOFC",1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.069,1.069,1.069,1.069,1.069,1.069,1.069]
["CN-E2L111C6","CN",1,"E2L111C6",717,"Interline circuity, FLAT - TOFC",1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.107,1.107,1.107,1.107,1.107,1.107,1.107]
["CN-E2L111C7","CN",1,"E2L111C7",718,"Average circuity, FLAT - TOFC",1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.085,1.085,1.085,1.085,1.085,1.085,1.085]
["CN-E2L111C8","CN",1,"E2L111C8",719,"Spotted-to-Pulled Ratio, FLAT - TOFC",1.16653275489807,1.2266275882720901,1.1501663923263501,1.13591992855072,1.12251472473145,1.16910147666931,1.1239491701126101,1.0674974918365501,1.0948908329010001,1.0460326987938,1.0544396730849099,1.04748505100246,1.0347197493056099,1.03839180795703,1.0537216333091,1.0391773815443599]
["CN-E2L111C9","CN",1,"E2L111C9",720,"CD per Industry Switch, FLAT - TOFC",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L111C10","CN",1,"E2L111C10",721,"CD per Interchange Switch, FLAT - TOFC",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L111C11","CN",1,"E2L111C11",722,"CD per Intraterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L111C12","CN",1,"E2L111C12",723,"CD per Interterminal Switch, FLAT - TOFC",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L111C13","CN",1,"E2L111C13",724,"CD per I&I Switch, FLAT - TOFC",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L111C14","CN",1,"E2L111C14",725,"CD per Load & Unload Industry Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L111C15","CN",1,"E2L111C15",726,"CD per Load & Unload Intraterminal Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L111C16","CN",1,"E2L111C16",727,"CD per Load & Unload Interterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L111C17","CN",1,"E2L111C17",728,"CM per Industry Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L111C18","CN",1,"E2L111C18",729,"CM per Interchange Switch, FLAT - TOFC",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L111C19","CN",1,"E2L111C19",730,"CM per Intraterminal Switch, FLAT - TOFC",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L111C20","CN",1,"E2L111C20",731,"CM per Interterminal Switch, FLAT - TOFC",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L111C21","CN",1,"E2L111C21",732,"CM per I&I Switch, FLAT - TOFC",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L111C22","CN",1,"E2L111C22",733,"Average CM per CD, Railroad-Owned, FLAT - TOFC",832.705810546875,838.408203125,803.45910644531295,985.42266845703102,877.11328125,813.18524169921898,783.69482421875,752.58538818359398,757.49151611328102,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L111C23","CN",1,"E2L111C23",734,"Average Miles between I&I Switches, FLAT - TOFC",4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162]
["CN-E2L111C24","CN",1,"E2L111C24",735,"Average Miles between Interchange Switches, FLAT - TOFC",244.02890014648401,250.76393127441401,265.153564453125,289.46157836914102,288.80505371093801,295.65908813476602,233.03454589843801,280.09762573242199,260.85308837890602,151.53480344985499,199.45777228555301,149.63925706595501,148.605140964528,146.38640894806599,310.88064462199799,306.79263965157298]
["CN-E2L111C25","CN",1,"E2L111C25",736,"SEMs per Industry Switch, FLAT - TOFC",6.5772328376770002,6.1651020050048801,5.9204263687133798,5.26851606369019,4.4945406913757298,4.5362834930419904,4.2201857566833496,3.8595824241638201,3.6106636524200399,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L111C26","CN",1,"E2L111C26",737,"SEMs per Interchange Switch, FLAT - TOFC",3.6174776554107702,3.3908064365386998,3.2562344074249299,2.89768385887146,2.4719977378845202,2.49495625495911,2.3211019039154102,2.12277054786682,1.9858651161193801,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L111C27","CN",1,"E2L111C27",738,"SEMs per Intraterminal Switch, FLAT - TOFC",9.8658494949340803,9.2476520538330096,8.8806390762329102,7.9027743339538601,6.7418112754821804,6.8044242858886701,6.3302783966064498,5.7893748283386204,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L111C28","CN",1,"E2L111C28",739,"SEMs per Interterminal Switch, FLAT - TOFC",7.89267921447754,7.3981232643127397,7.1045126914978001,6.3222193717956499,5.3934493064880398,5.4435400962829599,5.0642223358154297,4.6314992904663104,4.3327970504760698,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L111C29","CN",1,"E2L111C29",740,"SEMs per I&I Switch, FLAT - TOFC",1.64430832862854,1.54127550125122,1.4801067113876301,1.3171291351318399,1.12363529205322,1.1340708732605,1.0550463199615501,0.96489566564559903,0.90266591310501099,0.79212239878993795,0.75363172764813202,0.75501600530493096,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L112C1","CN",1,"E2L112C1",741,"Average Tare Weight, FLAT - MULTILEVEL",54.299999237060497,54.299999237060497,54.200000762939503,54.400001525878899,54.900001525878899,54.5,54,54,53.799999237060497,53.6,53.6,53.4,53.3,53.1,53.1,53.1]
["CN-E2L112C2","CN",1,"E2L112C2",742,"E/L Ratio, Railroad-Owned, FLAT - MULTILEVEL",1.4589545726776101,1.4644113779068,1.4298734664917001,1.54168033599854,1.40757608413696,1.4598568677902199,1.42446041107178,1.4516453742980999,1.4331638813018801,1.4816262705238501,1.5400743494423801,1.6239127229839301,1.62116091109478,1.5900104058272599,1.4402130794514301,1.52615826649108]
["CN-E2L112C3","CN",1,"E2L112C3",743,"E/L Ratio, Privately-Owned, FLAT - MULTILEVEL",1.42665219306946,1.4121463298797601,1.3515388965606701,1.40109527111053,1.35803747177124,1.38527607917786,1.3558492660522501,1.4142967462539699,1.3694754838943499,1.4458626841514799,1.4899305373296201,1.55468911027138,1.5408208085862201,1.4864714397060499,1.3756692151168499,1.46450062598441]
["CN-E2L112C4","CN",1,"E2L112C4",744,"E/L Ratio, All Freight Cars, FLAT - MULTILEVEL",1.4301882982253999,1.4177426099777199,1.3596608638763401,1.4159196615219101,1.36340391635895,1.3928034305572501,1.3632960319519001,1.41861689090729,1.3763526678085301,1.44962643583583,1.4952096183349499,1.5619125271141301,1.5500608436993,1.49796248329566,1.38524948689479,1.47339956803456]
["CN-E2L112C5","CN",1,"E2L112C5",745,"Local circuity, FLAT - MULTILEVEL",1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999]
["CN-E2L112C6","CN",1,"E2L112C6",746,"Interline circuity, FLAT - MULTILEVEL",1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999]
["CN-E2L112C7","CN",1,"E2L112C7",747,"Average circuity, FLAT - MULTILEVEL",1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999]
["CN-E2L112C8","CN",1,"E2L112C8",748,"Spotted-to-Pulled Ratio, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L112C9","CN",1,"E2L112C9",749,"CD per Industry Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L112C10","CN",1,"E2L112C10",750,"CD per Interchange Switch, FLAT - MULTILEVEL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L112C11","CN",1,"E2L112C11",751,"CD per Intraterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L112C12","CN",1,"E2L112C12",752,"CD per Interterminal Switch, FLAT - MULTILEVEL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L112C13","CN",1,"E2L112C13",753,"CD per I&I Switch, FLAT - MULTILEVEL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L112C14","CN",1,"E2L112C14",754,"CD per Load & Unload Industry Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L112C15","CN",1,"E2L112C15",755,"CD per Load & Unload Intraterminal Switch, FLAT - MULTILEVEL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
[{"$f":"B1730&\"-\"&D1730","v":"CN-E2L112C16"},"CN",1,"E2L112C16",756,"CD per Load & Unload Interterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L112C17","CN",1,"E2L112C17",757,"CM per Industry Switch, FLAT - MULTILEVEL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L112C18","CN",1,"E2L112C18",758,"CM per Interchange Switch, FLAT - MULTILEVEL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L112C19","CN",1,"E2L112C19",759,"CM per Intraterminal Switch, FLAT - MULTILEVEL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L112C20","CN",1,"E2L112C20",760,"CM per Interterminal Switch, FLAT - MULTILEVEL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L112C21","CN",1,"E2L112C21",761,"CM per I&I Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L112C22","CN",1,"E2L112C22",762,"Average CM per CD, Railroad-Owned, FLAT - MULTILEVEL",832.705810546875,838.40814208984398,803.459228515625,985.42272949218795,877.11328125,813.18524169921898,783.69476318359398,752.58532714843795,757.49151611328102,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L112C23","CN",1,"E2L112C23",763,"Average Miles between I&I Switches, FLAT - MULTILEVEL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L112C24","CN",1,"E2L112C24",764,"Average Miles between Interchange Switches, FLAT - MULTILEVEL",891.68566894531295,684.95227050781295,780.28955078125,1049.37341308594,836.041015625,851.30310058593795,781.98675537109398,847.72863769531295,881.73748779296898,292.18788319480001,540.31894018379103,674.94220143232701,613.74241628455604,593.04124837876202,982.478861551568,1029.78012152974]
["CN-E2L112C25","CN",1,"E2L112C25",765,"SEMs per Industry Switch, FLAT - MULTILEVEL",6.5772328376770002,6.1651020050048801,5.9204268455505398,5.2685165405273402,4.4945411682128897,4.5362834930419904,4.2201857566833496,3.8595821857452401,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L112C26","CN",1,"E2L112C26",766,"SEMs per Interchange Switch, FLAT - MULTILEVEL",3.6174778938293501,3.3908061981201199,3.2562344074249299,2.89768385887146,2.4719974994659402,2.49495601654053,2.3211021423339799,2.12277054786682,1.9858652353286701,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L112C27","CN",1,"E2L112C27",767,"SEMs per Intraterminal Switch, FLAT - MULTILEVEL",9.8658494949340803,9.2476530075073207,8.8806390762329102,7.9027743339538601,6.7418112754821804,6.8044247627258301,6.3302779197692898,5.7893743515014604,5.4159955978393599,4.7527343927396304,4.5217903658888003,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L112C28","CN",1,"E2L112C28",768,"SEMs per Interterminal Switch, FLAT - MULTILEVEL",7.89267921447754,7.3981227874755904,7.1045126914978001,6.3222193717956499,5.3934493064880398,5.4435405731201199,5.0642228126525897,4.6314992904663104,4.3327965736389196,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L112C29","CN",1,"E2L112C29",769,"SEMs per I&I Switch, FLAT - MULTILEVEL",1.64430820941925,1.54127562046051,1.4801067113876301,1.3171290159225499,1.12363529205322,1.1340708732605,1.0550464391708401,0.96489566564559903,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L113C1","CN",1,"E2L113C1",770,"Average Tare Weight, FLAT - GENERAL",33.599998474121101,34.099998474121101,34,32.900001525878899,32.200000762939503,33,32.200000762939503,32.799999237060497,32.799999237060497,32.5,32.4,32.200000000000003,32.1,32.200000000000003,32.299999999999997,32.299999999999997]
["CN-E2L113C2","CN",1,"E2L113C2",771,"E/L Ratio, Railroad-Owned, FLAT - GENERAL",2.6111111640930198,2.7252748012542698,2.61666655540466,2.6956522464752202,3.4500000476837198,2.04347825050354,2.2666666507720898,3.0384614467620898,2.625,2.45714285714286,2.1067961165048499,2.1538461538461502,2.25454545454545,2,2.1294117647058801,2.19354838709677]
["CN-E2L113C3","CN",1,"E2L113C3",772,"E/L Ratio, Privately-Owned, FLAT - GENERAL",2.1919643878936799,2.1370370388031001,2.8199999332428001,13,1.86440682411194,2.1126761436462398,2.6749999523162802,3,2.24091768264771,2.1818181818181799,2.2222222222222201,2.0268817204301102,2.08119658119658,2.09375,2.2291666666666701,2.9471365638766498]
["CN-E2L113C4","CN",1,"E2L113C4",773,"E/L Ratio, All Freight Cars, FLAT - GENERAL",2.91463422775269,2.9553570747375502,2.67647051811218,3.88461542129517,3.8148148059845002,2.6756756305694598,2.45882344245911,3.14893627166748,3.5151515007018999,2.98,2.1239669421487601,2.0597609561753001,2.1141868512110702,2.0750000000000002,2.1654135338345899,2.8565891472868201]
["CN-E2L113C5","CN",1,"E2L113C5",774,"Local circuity, FLAT - GENERAL",1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001]
["CN-E2L113C6","CN",1,"E2L113C6",775,"Interline circuity, FLAT - GENERAL",1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.177,1.177,1.177,1.177,1.177,1.177,1.177]
["CN-E2L113C7","CN",1,"E2L113C7",776,"Average circuity, FLAT - GENERAL",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["CN-E2L113C8","CN",1,"E2L113C8",777,"Spotted-to-Pulled Ratio, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L113C9","CN",1,"E2L113C9",778,"CD per Industry Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L113C10","CN",1,"E2L113C10",779,"CD per Interchange Switch, FLAT - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L113C11","CN",1,"E2L113C11",780,"CD per Intraterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L113C12","CN",1,"E2L113C12",781,"CD per Interterminal Switch, FLAT - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L113C13","CN",1,"E2L113C13",782,"CD per I&I Switch, FLAT - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L113C14","CN",1,"E2L113C14",783,"CD per Load & Unload Industry Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L113C15","CN",1,"E2L113C15",784,"CD per Load & Unload Intraterminal Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L113C16","CN",1,"E2L113C16",785,"CD per Load & Unload Interterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L113C17","CN",1,"E2L113C17",786,"CM per Industry Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L113C18","CN",1,"E2L113C18",787,"CM per Interchange Switch, FLAT - GENERAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L113C19","CN",1,"E2L113C19",788,"CM per Intraterminal Switch, FLAT - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L113C20","CN",1,"E2L113C20",789,"CM per Interterminal Switch, FLAT - GENERAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L113C21","CN",1,"E2L113C21",790,"CM per I&I Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L113C22","CN",1,"E2L113C22",791,"Average CM per CD, Railroad-Owned, FLAT - GENERAL",832.705810546875,838.408203125,803.459228515625,985.42266845703102,877.11334228515602,813.18518066406295,783.69476318359398,752.58538818359398,757.49157714843795,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L113C23","CN",1,"E2L113C23",792,"Average Miles between I&I Switches, FLAT - GENERAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L113C24","CN",1,"E2L113C24",793,"Average Miles between Interchange Switches, FLAT - GENERAL",2813.05688476563,452.110107421875,525.64361572265602,751.81072998046898,1108.15368652344,1121.21215820313,4762.25830078125,3636.29907226563,1099.78125,43.411151842562198,310.25641025640999,220.17543859649101,194.08999328408299,102.739726027397,190,310.46931407942202]
["CN-E2L113C25","CN",1,"E2L113C25",794,"SEMs per Industry Switch, FLAT - GENERAL",6.5772328376770002,6.1651020050048801,5.9204268455505398,5.26851606369019,4.4945411682128897,4.5362834930419904,4.2201852798461896,3.8595824241638201,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L113C26","CN",1,"E2L113C26",795,"SEMs per Interchange Switch, FLAT - GENERAL",3.6174778938293501,3.3908064365386998,3.2562344074249299,2.89768362045288,2.4719974994659402,2.49495577812195,2.3211021423339799,2.12277054786682,1.9858653545379601,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L113C27","CN",1,"E2L113C27",796,"SEMs per Intraterminal Switch, FLAT - GENERAL",9.8658494949340803,9.2476530075073207,8.8806390762329102,7.9027743339538601,6.7418107986450204,6.8044252395629901,6.3302783966064498,5.7893743515014604,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L113C28","CN",1,"E2L113C28",797,"SEMs per Interterminal Switch, FLAT - GENERAL",7.89267921447754,7.3981232643127397,7.1045122146606401,6.3222188949584996,5.3934497833251998,5.4435405731201199,5.0642232894897496,4.6314997673034703,4.3327970504760698,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L113C29","CN",1,"E2L113C29",798,"SEMs per I&I Switch, FLAT - GENERAL",1.64430832862854,1.54127562046051,1.4801067113876301,1.3171290159225499,1.12363517284393,1.1340708732605,1.0550464391708401,0.96489566564559903,0.90266603231430098,0.79212239878993795,0.75363172764813202,0.75501600530493096,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L114C1","CN",1,"E2L114C1",799,"Average Tare Weight, FLAT - OTHER",34.599998474121101,34.599998474121101,34.700000762939503,34.700000762939503,34.700000762939503,34.700000762939503,35.099998474121101,35.200000762939503,35.200000762939503,35.299999999999997,35.299999999999997,35.299999999999997,35.4,35.299999999999997,35.4,35.4]
["CN-E2L114C2","CN",1,"E2L114C2",800,"E/L Ratio, Railroad-Owned, FLAT - OTHER",2.0994725227356001,2.08657002449036,2.0826787948608398,2.0801939964294398,2.1216607093811,2.0309131145477299,2.06700539588928,1.9802436828613299,2.02625679969788,2.0760257043994099,2.0877478577403998,2.0874828193195198,2.0565555134520701,2.0540452261306501,2.0860094498278201,2.1046799861186898]
["CN-E2L114C3","CN",1,"E2L114C3",801,"E/L Ratio, Privately-Owned, FLAT - OTHER",1.73315894603729,1.8126477003097501,1.8942338228225699,1.8984674215316799,1.89279508590698,1.9496879577636701,1.96587562561035,1.9829980134964,1.91870748996735,1.96331120943953,1.9191829484902301,1.96441434951736,1.95417226451709,2.00533902829685,2.0145365301113798,1.8831730769230799]
["CN-E2L114C4","CN",1,"E2L114C4",802,"E/L Ratio, All Freight Cars, FLAT - OTHER",2.0299375057220499,2.03312420845032,2.0559322834014901,2.0635852813720699,2.0926496982574498,2.01961374282837,2.0469176769256601,1.9808477163314799,2.0076992511749299,2.0627015953273502,2.0721687562842401,2.06983805668016,2.04253623040288,2.04801955128911,2.0771551522522098,2.07500751363188]
["CN-E2L114C5","CN",1,"E2L114C5",803,"Local circuity, FLAT - OTHER",1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001]
["CN-E2L114C6","CN",1,"E2L114C6",804,"Interline circuity, FLAT - OTHER",1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.17,1.17,1.17,1.17,1.17,1.17,1.17]
["CN-E2L114C7","CN",1,"E2L114C7",805,"Average circuity, FLAT - OTHER",1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.155,1.155,1.155,1.155,1.155,1.155,1.155]
["CN-E2L114C8","CN",1,"E2L114C8",806,"Spotted-to-Pulled Ratio, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L114C9","CN",1,"E2L114C9",807,"CD per Industry Switch, FLAT - OTHER",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L114C10","CN",1,"E2L114C10",808,"CD per Interchange Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L114C11","CN",1,"E2L114C11",809,"CD per Intraterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L114C12","CN",1,"E2L114C12",810,"CD per Interterminal Switch, FLAT - OTHER",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L114C13","CN",1,"E2L114C13",811,"CD per I&I Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L114C14","CN",1,"E2L114C14",812,"CD per Load & Unload Industry Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L114C15","CN",1,"E2L114C15",813,"CD per Load & Unload Intraterminal Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L114C16","CN",1,"E2L114C16",814,"CD per Load & Unload Interterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L114C17","CN",1,"E2L114C17",815,"CM per Industry Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L114C18","CN",1,"E2L114C18",816,"CM per Interchange Switch, FLAT - OTHER",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L114C19","CN",1,"E2L114C19",817,"CM per Intraterminal Switch, FLAT - OTHER",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L114C20","CN",1,"E2L114C20",818,"CM per Interterminal Switch, FLAT - OTHER",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L114C21","CN",1,"E2L114C21",819,"CM per I&I Switch, FLAT - OTHER",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
[{"$f":"B1794&\"-\"&D1794","v":"CN-E2L114C22"},"CN",1,"E2L114C22",820,"Average CM per CD, Railroad-Owned, FLAT - OTHER",832.70568847656295,838.40826416015602,803.45916748046898,985.42266845703102,877.11334228515602,813.18524169921898,783.69476318359398,752.58538818359398,757.49157714843795,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L114C23","CN",1,"E2L114C23",821,"Average Miles between I&I Switches, FLAT - OTHER",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L114C24","CN",1,"E2L114C24",822,"Average Miles between Interchange Switches, FLAT - OTHER",396.97619628906301,392.33016967773398,385.41973876953102,425.98013305664102,431.47299194335898,409.96249389648398,333.15377807617199,403.85729980468801,352.54275512695301,210.77940035672299,207.01682216925099,201.232954773285,204.64681452823999,199.26352195176599,240.12886356446401,234.426390237959]
["CN-E2L114C25","CN",1,"E2L114C25",823,"SEMs per Industry Switch, FLAT - OTHER",6.5772333145141602,6.1651024818420401,5.9204263687133798,5.26851606369019,4.4945411682128897,4.5362830162048304,4.2201857566833496,3.8595824241638201,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L114C26","CN",1,"E2L114C26",824,"SEMs per Interchange Switch, FLAT - OTHER",3.6174778938293501,3.3908064365386998,3.2562344074249299,2.89768409729004,2.4719974994659402,2.49495601654053,2.3211021423339799,2.12277054786682,1.9858651161193801,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L114C27","CN",1,"E2L114C27",825,"SEMs per Intraterminal Switch, FLAT - OTHER",9.8658494949340803,9.2476530075073207,8.8806390762329102,7.9027743339538601,6.7418112754821804,6.80442571640015,6.3302779197692898,5.7893743515014604,5.4159951210021999,4.7527343927396197,4.5217903658888003,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L114C28","CN",1,"E2L114C28",826,"SEMs per Interterminal Switch, FLAT - OTHER",7.89267921447754,7.3981232643127397,7.1045122146606401,6.3222193717956499,5.3934488296508798,5.4435405731201199,5.0642232894897496,4.6314997673034703,4.3327970504760698,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L114C29","CN",1,"E2L114C29",827,"SEMs per I&I Switch, FLAT - OTHER",1.64430832862854,1.54127550125122,1.4801067113876301,1.3171290159225499,1.12363529205322,1.1340708732605,1.0550463199615501,0.96489572525024403,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530493096,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L115C1","CN",1,"E2L115C1",828,"Average Tare Weight, TANK <22,000 GAL",32.700000000000003,32.700000000000003,32.6,32.6,32.6,32.6,32.6,32.6,32.6,32.700000000000003,32.700000000000003,32.799999999999997,32.799999999999997,32.9,32.9,32.9]
["CN-E2L115C2","CN",1,"E2L115C2",829,"E/L Ratio, Railroad-Owned, TANK <22,000 GAL",1.6895714998245199,1.5536141395568801,1.4515423774719201,1.22512030601501,1.3009463548660301,1.2404767274856601,1.24703228473663,1.1719552278518699,1.1494325399398799,1.1288779731127201,1.1515058859501599,1.11975116640747,1.1580328360446801,1.21547427992229,1.77754237288136,1.6875]
["CN-E2L115C3","CN",1,"E2L115C3",830,"E/L Ratio, Privately-Owned, TANK <22,000 GAL",2.03905153274536,2.0434539318084699,2.1019251346588099,2.0596368312835698,2.0696890354156499,2.0737707614898699,2.06474781036377,2.03631567955017,2.04345798492432,2.0497437443473001,2.0431333896555,2.0350146747662299,2.0437009139760298,2.0363086232980301,2.04855205833702,2.0478547478387799]
["CN-E2L115C4","CN",1,"E2L115C4",831,"E/L Ratio, All Freight Cars, TANK <22,000 GAL",2.03905153274536,2.0434539318084699,2.1019251346588099,2.0596368312835698,2.0696890354156499,2.0737707614898699,2.06474781036377,2.03631567955017,2.04345798492432,2.0497437443473001,2.0431333896555,2.0350146747662299,2.0437009139760298,2.0363086232980301,2.04855205833702,2.0478547478387799]
["CN-E2L115C5","CN",1,"E2L115C5",832,"Local circuity, TANK <22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["CN-E2L115C6","CN",1,"E2L115C6",833,"Interline circuity, TANK <22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["CN-E2L115C7","CN",1,"E2L115C7",834,"Average circuity, TANK <22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["CN-E2L115C8","CN",1,"E2L115C8",835,"Spotted-to-Pulled Ratio, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L115C9","CN",1,"E2L115C9",836,"CD per Industry Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L115C10","CN",1,"E2L115C10",837,"CD per Interchange Switch, TANK <22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L115C11","CN",1,"E2L115C11",838,"CD per Intraterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L115C12","CN",1,"E2L115C12",839,"CD per Interterminal Switch, TANK <22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L115C13","CN",1,"E2L115C13",840,"CD per I&I Switch, TANK <22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L115C14","CN",1,"E2L115C14",841,"CD per Load & Unload Industry Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L115C15","CN",1,"E2L115C15",842,"CD per Load & Unload Intraterminal Switch, TANK <22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L115C16","CN",1,"E2L115C16",843,"CD per Load & Unload Interterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L115C17","CN",1,"E2L115C17",844,"CM per Industry Switch, TANK <22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L115C18","CN",1,"E2L115C18",845,"CM per Interchange Switch, TANK <22,000 GAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L115C19","CN",1,"E2L115C19",846,"CM per Intraterminal Switch, TANK <22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L115C20","CN",1,"E2L115C20",847,"CM per Interterminal Switch, TANK <22,000 GAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L115C21","CN",1,"E2L115C21",848,"CM per I&I Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L115C22","CN",1,"E2L115C22",849,"Average CM per CD, Railroad-Owned, TANK <22,000 GAL",832.70574951171898,838.408203125,803.45916748046898,985.42266845703102,877.11328125,813.18524169921898,783.69482421875,752.58532714843795,757.49151611328102,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L115C23","CN",1,"E2L115C23",850,"Average Miles between I&I Switches, TANK <22,000 GAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L115C24","CN",1,"E2L115C24",851,"Average Miles between Interchange Switches, TANK <22,000 GAL",421.93167114257801,488.90451049804699,514.757568359375,547.32159423828102,567.44793701171898,562.88098144531295,687.20989990234398,618.49938964843795,582.97668457031295,500.37854751552902,335.79441363695997,392.12348096189299,384.27116387048801,321.74956246896602,234.888128329995,249.32602336077801]
["CN-E2L115C25","CN",1,"E2L115C25",852,"SEMs per Industry Switch, TANK <22,000 GAL",6.5772333145141602,6.1651024818420401,5.9204268455505398,5.26851606369019,4.4945411682128897,4.5362830162048304,4.2201857566833496,3.8595824241638201,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L115C26","CN",1,"E2L115C26",853,"SEMs per Interchange Switch, TANK <22,000 GAL",3.6174781322479199,3.3908061981201199,3.2562344074249299,2.89768385887146,2.4719977378845202,2.49495601654053,2.3211021423339799,2.12277030944824,1.9858653545379601,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L115C27","CN",1,"E2L115C27",854,"SEMs per Intraterminal Switch, TANK <22,000 GAL",9.8658494949340803,9.2476520538330096,8.8806390762329102,7.9027743339538601,6.7418107986450204,6.8044247627258301,6.3302779197692898,5.7893748283386204,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L115C28","CN",1,"E2L115C28",855,"SEMs per Interterminal Switch, TANK <22,000 GAL",7.89267873764038,7.3981227874755904,7.1045126914978001,6.3222188949584996,5.3934493064880398,5.4435405731201199,5.0642232894897496,4.6314992904663104,4.3327970504760698,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L115C29","CN",1,"E2L115C29",856,"SEMs per I&I Switch, TANK <22,000 GAL",1.64430832862854,1.54127550125122,1.4801067113876301,1.3171291351318399,1.12363529205322,1.1340708732605,1.0550464391708401,0.96489566564559903,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L116C1","CN",1,"E2L116C1",857,"Average Tare Weight, TANK >=22,000 GAL",39.799999999999997,39.200000000000003,38.9,38.9,39,38.9,38.9,39.1,39.5,40.1,40.4,40.700000000000003,41,41.4,41.7,41.9]
["CN-E2L116C2","CN",1,"E2L116C2",858,"E/L Ratio, Railroad-Owned, TANK >=22,000 GAL",1.6895714998245199,1.5536141395568801,1.4515423774719201,1.22512030601501,1.3009463548660301,1.2404767274856601,1.24703228473663,1.1719552278518699,1.1494325399398799,1.1288779731127201,1.1515058859501599,1.11975116640747,1.1580328360446801,1.21547427992229,1.77754237288136,1.6875]
["CN-E2L116C3","CN",1,"E2L116C3",859,"E/L Ratio, Privately-Owned, TANK >=22,000 GAL",2.0867471694946298,2.0555059909820601,2.0691351890564,2.0575811862945601,2.0408492088317902,2.0626566410064702,2.0292539596557599,2.0378572940826398,2.0645849704742401,2.0481797730256801,2.0775368878030802,2.0480950767294401,2.0649998556040101,2.0533132180573301,2.0810478316279499,2.0698671334949301]
["CN-E2L116C4","CN",1,"E2L116C4",860,"E/L Ratio, All Freight Cars, TANK >=22,000 GAL",2.0867471694946298,2.0555059909820601,2.0691351890564,2.0575811862945601,2.0408492088317902,2.0626566410064702,2.0292539596557599,2.0378572940826398,2.0645849704742401,2.0481797730256801,2.0775368878030802,2.0480950767294401,2.0649998556040101,2.0533132180573301,2.0810478316279499,2.0698671334949301]
["CN-E2L116C5","CN",1,"E2L116C5",861,"Local circuity, TANK >=22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["CN-E2L116C6","CN",1,"E2L116C6",862,"Interline circuity, TANK >=22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["CN-E2L116C7","CN",1,"E2L116C7",863,"Average circuity, TANK >=22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["CN-E2L116C8","CN",1,"E2L116C8",864,"Spotted-to-Pulled Ratio, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L116C9","CN",1,"E2L116C9",865,"CD per Industry Switch, TANK >=22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L116C10","CN",1,"E2L116C10",866,"CD per Interchange Switch, TANK >=22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L116C11","CN",1,"E2L116C11",867,"CD per Intraterminal Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L116C12","CN",1,"E2L116C12",868,"CD per Interterminal Switch, TANK >=22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L116C13","CN",1,"E2L116C13",869,"CD per I&I Switch, TANK >=22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L116C14","CN",1,"E2L116C14",870,"CD per Load & Unload Industry Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L116C15","CN",1,"E2L116C15",871,"CD per Load & Unload Intraterminal Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L116C16","CN",1,"E2L116C16",872,"CD per Load & Unload Interterminal Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L116C17","CN",1,"E2L116C17",873,"CM per Industry Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L116C18","CN",1,"E2L116C18",874,"CM per Interchange Switch, TANK >=22,000 GAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L116C19","CN",1,"E2L116C19",875,"CM per Intraterminal Switch, TANK >=22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L116C20","CN",1,"E2L116C20",876,"CM per Interterminal Switch, TANK >=22,000 GAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L116C21","CN",1,"E2L116C21",877,"CM per I&I Switch, TANK >=22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L116C22","CN",1,"E2L116C22",878,"Average CM per CD, Railroad-Owned, TANK >=22,000 GAL",832.70574951171898,838.408203125,803.45916748046898,985.42266845703102,877.11328125,813.18524169921898,783.69482421875,752.58532714843795,757.49151611328102,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L116C23","CN",1,"E2L116C23",879,"Average Miles between I&I Switches, TANK >=22,000 GAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L116C24","CN",1,"E2L116C24",880,"Average Miles between Interchange Switches, TANK >=22,000 GAL",421.93167114257801,488.90451049804699,514.757568359375,547.32159423828102,567.44793701171898,562.88098144531295,687.20989990234398,618.49938964843795,582.97668457031295,500.37854751552902,335.79441363695997,392.12348096189299,384.27116387048801,321.74956246896602,234.888128329995,249.32602336077801]
["CN-E2L116C25","CN",1,"E2L116C25",881,"SEMs per Industry Switch, TANK >=22,000 GAL",6.5772333145141602,6.1651024818420401,5.9204268455505398,5.26851606369019,4.4945411682128897,4.5362830162048304,4.2201857566833496,3.8595824241638201,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L116C26","CN",1,"E2L116C26",882,"SEMs per Interchange Switch, TANK >=22,000 GAL",3.6174781322479199,3.3908061981201199,3.2562344074249299,2.89768385887146,2.4719977378845202,2.49495601654053,2.3211021423339799,2.12277030944824,1.9858653545379601,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L116C27","CN",1,"E2L116C27",883,"SEMs per Intraterminal Switch, TANK >=22,000 GAL",9.8658494949340803,9.2476520538330096,8.8806390762329102,7.9027743339538601,6.7418107986450204,6.8044247627258301,6.3302779197692898,5.7893748283386204,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
[{"$f":"B1858&\"-\"&D1858","v":"CN-E2L116C28"},"CN",1,"E2L116C28",884,"SEMs per Interterminal Switch, TANK >=22,000 GAL",7.89267873764038,7.3981227874755904,7.1045126914978001,6.3222188949584996,5.3934493064880398,5.4435405731201199,5.0642232894897496,4.6314992904663104,4.3327970504760698,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L116C29","CN",1,"E2L116C29",885,"SEMs per I&I Switch, TANK >=22,000 GAL",1.64430832862854,1.54127550125122,1.4801067113876301,1.3171291351318399,1.12363529205322,1.1340708732605,1.0550464391708401,0.96489566564559903,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L117C1","CN",1,"E2L117C1",886,"Average Tare Weight, ALL OTHER FREIGHT CARS",36.799999237060497,36.700000762939503,36.5,36.599998474121101,36.700000762939503,36.599998474121101,36.799999237060497,37.099998474121101,37.5,38.1,38.4,38.6,38.9,39.299999999999997,39.6,39.799999999999997]
["CN-E2L117C2","CN",1,"E2L117C2",887,"E/L Ratio, Railroad-Owned, ALL OTHER FREIGHT CARS",1.6895714998245199,1.5536141395568801,1.4515423774719201,1.22512030601501,1.3009463548660301,1.2404767274856601,1.24703228473663,1.1719552278518699,1.1494325399398799,1.1288779731127201,1.1515058859501599,1.11975116640747,1.1580328360446801,1.21547427992229,1.77754237288136,1.6875]
["CN-E2L117C3","CN",1,"E2L117C3",888,"E/L Ratio, Privately-Owned, ALL OTHER FREIGHT CARS",1.20515143871307,1.1758214235305799,1.15120720863342,1.14410507678986,1.12294793128967,1.1681767702102701,1.1968628168106099,1.3117703199386599,1.4312435388565099,1.2703770842519599,1.21755492270138,1.21807828328238,1.3246135162635,1.4265313272117099,1.1572700296735901,2.1196094385679398]
["CN-E2L117C4","CN",1,"E2L117C4",889,"E/L Ratio, All Freight Cars, ALL OTHER FREIGHT CAR",1.9768818616867101,1.93826127052307,1.95299756526947,1.90906870365143,1.8970144987106301,1.93070900440216,1.91932725906372,1.8573626279830899,1.8535454273223899,1.81553749255256,1.81505028476678,1.74319042407556,1.7836216936198099,1.7850662373630599,2.0707436524607301,2.0643131558960701]
["CN-E2L117C5","CN",1,"E2L117C5",890,"Local circuity, ALL OTHER FREIGHT CARS",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["CN-E2L117C6","CN",1,"E2L117C6",891,"Interline circuity, ALL OTHER FREIGHT CARS",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["CN-E2L117C7","CN",1,"E2L117C7",892,"Average circuity, ALL OTHER FREIGHT CARS",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["CN-E2L117C8","CN",1,"E2L117C8",893,"Spotted-to-Pulled Ratio, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L117C9","CN",1,"E2L117C9",894,"CD per Industry Switch, ALL OTHER FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L117C10","CN",1,"E2L117C10",895,"CD per Interchange Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L117C11","CN",1,"E2L117C11",896,"CD per Intraterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L117C12","CN",1,"E2L117C12",897,"CD per Interterminal Switch, ALL OTHER FREIGHT CARS",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L117C13","CN",1,"E2L117C13",898,"CD per I&I Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L117C14","CN",1,"E2L117C14",899,"CD per Load & Unload Industry Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L117C15","CN",1,"E2L117C15",900,"CD per Load & Unload Intraterminal Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L117C16","CN",1,"E2L117C16",901,"CD per Load & Unload Interterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L117C17","CN",1,"E2L117C17",902,"CM per Industry Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L117C18","CN",1,"E2L117C18",903,"CM per Interchange Switch, ALL OTHER FREIGHT CARS",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L117C19","CN",1,"E2L117C19",904,"CM per Intraterminal Switch, ALL OTHER FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L117C20","CN",1,"E2L117C20",905,"CM per Interterminal Switch, ALL OTHER FREIGHT CARS",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L117C21","CN",1,"E2L117C21",906,"CM per I&I Switch, ALL OTHER FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L117C22","CN",1,"E2L117C22",907,"Average CM per CD, Railroad-Owned, ALL OTHER FREIGHT CARS",832.70574951171898,838.408203125,803.45916748046898,985.42266845703102,877.11328125,813.18524169921898,783.69482421875,752.58532714843795,757.49151611328102,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L117C23","CN",1,"E2L117C23",908,"Average Miles between I&I Switches, ALL OTHER FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L117C24","CN",1,"E2L117C24",909,"Average Miles between Interchange Switches, ALL OTHER FREIGHT CARS",421.93167114257801,488.90451049804699,514.757568359375,547.32159423828102,567.44793701171898,562.88098144531295,687.20989990234398,618.49938964843795,582.97668457031295,500.37854751552902,335.79441363695997,392.12348096189299,384.27116387048801,321.74956246896602,234.888128329995,249.32602336077801]
["CN-E2L117C25","CN",1,"E2L117C25",910,"SEMs per Industry Switch, ALL OTHER FREIGHT CARS",6.5772333145141602,6.1651024818420401,5.9204268455505398,5.26851606369019,4.4945411682128897,4.5362830162048304,4.2201857566833496,3.8595824241638201,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L117C26","CN",1,"E2L117C26",911,"SEMs per Interchange Switch, ALL OTHER FREIGHT CARS",3.6174781322479199,3.3908061981201199,3.2562344074249299,2.89768385887146,2.4719977378845202,2.49495601654053,2.3211021423339799,2.12277030944824,1.9858653545379601,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L117C27","CN",1,"E2L117C27",912,"SEMs per Intraterminal Switch, ALL OTHER FREIGHT CARS",9.8658494949340803,9.2476520538330096,8.8806390762329102,7.9027743339538601,6.7418107986450204,6.8044247627258301,6.3302779197692898,5.7893748283386204,5.4159955978393599,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L117C28","CN",1,"E2L117C28",913,"SEMs per Interterminal Switch, ALL OTHER FREIGHT CARS",7.89267873764038,7.3981227874755904,7.1045126914978001,6.3222188949584996,5.3934493064880398,5.4435405731201199,5.0642232894897496,4.6314992904663104,4.3327970504760698,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L117C29","CN",1,"E2L117C29",914,"SEMs per I&I Switch, ALL OTHER FREIGHT CARS",1.64430832862854,1.54127550125122,1.4801067113876301,1.3171291351318399,1.12363529205322,1.1340708732605,1.0550464391708401,0.96489566564559903,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530492996,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L118C1","CN",1,"E2L118C1",915,"Average Tare Weight, AVERAGE ALL FREIGHT CARS",34.400001525878899,34.400001525878899,34.299999237060497,34.299999237060497,34.299999237060497,34.299999237060497,34.200000762939503,34.299999237060497,34.400001525878899,34.6,34.799999999999997,34.799999999999997,34.9,35.200000000000003,35.299999999999997,35.4]
["CN-E2L118C2","CN",1,"E2L118C2",916,"E/L Ratio, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.96826159954071,1.95848500728607,1.9624103307723999,1.94033420085907,1.93484234809875,1.9369753599166899,1.9373687505721999,1.919304728508,1.9001719951629601,1.9192076518080099,1.9143383631936,1.8962967422716499,1.8822761829116099,1.88916063761589,1.90594522299025,1.9187691879061901]
["CN-E2L118C3","CN",1,"E2L118C3",917,"E/L Ratio, Privately-Owned, AVERAGE ALL FREIGHT CARS",1.89208960533142,1.8776546716690099,1.9093753099441499,1.8846141099929801,1.8616898059845,1.8753845691680899,1.8761620521545399,1.8339710235595701,1.8400619029998799,1.81612497273353,1.79960498601816,1.8128553954900699,1.83757955983719,1.8154290747906101,1.7833995448216899,1.8486867422708699]
["CN-E2L118C4","CN",1,"E2L118C4",918,"E/L Ratio, All Freight Cars, AVERAGE ALL FREIGHT CARS",1.9272443056106601,1.9118959903717001,1.93100190162659,1.90441334247589,1.8875058889389,1.89656293392181,1.8926800489425699,1.85849273204803,1.8559324741363501,1.8416189584904099,1.8281127600607201,1.8316438769788199,1.84774115174995,1.8320238614869799,1.81149225686978,1.86536404378343]
["CN-E2L118C5","CN",1,"E2L118C5",919,"Local circuity, AVERAGE ALL FREIGHT CARS",1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.097,1.097,1.097,1.097,1.097,1.097,1.097]
["CN-E2L118C6","CN",1,"E2L118C6",920,"Interline circuity, AVERAGE ALL FREIGHT CARS",1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.157,1.157,1.157,1.157,1.157,1.157,1.157]
["CN-E2L118C7","CN",1,"E2L118C7",921,"Average circuity, AVERAGE ALL FREIGHT CARS",1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.135,1.135,1.135,1.135,1.135,1.135,1.135]
["CN-E2L118C8","CN",1,"E2L118C8",922,"Spotted-to-Pulled Ratio, AVERAGE ALL FREIGHT CARS",1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.9,1.9,1.9,1.9,1.9,1.9,1.9]
["CN-E2L118C9","CN",1,"E2L118C9",923,"CD per Industry Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L118C10","CN",1,"E2L118C10",924,"CD per Interchange Switch, AVERAGE ALL FREIGHT CAR",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L118C11","CN",1,"E2L118C11",925,"CD per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L118C12","CN",1,"E2L118C12",926,"CD per Interterminal Switch, AVERAGE ALL FREIGHT CARS",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CN-E2L118C13","CN",1,"E2L118C13",927,"CD per I&I Switch, AVERAGE ALL FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CN-E2L118C14","CN",1,"E2L118C14",928,"CD per Load & Unload Industry Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L118C15","CN",1,"E2L118C15",929,"CD per Load & Unload Intraterminal Switch, AVERAGE ALL FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L118C16","CN",1,"E2L118C16",930,"CD per Load & Unload Interterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CN-E2L118C17","CN",1,"E2L118C17",931,"CM per Industry Switch, AVERAGE ALL FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CN-E2L118C18","CN",1,"E2L118C18",932,"CM per Interchange Switch, AVERAGE ALL FREIGHT CAR",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CN-E2L118C19","CN",1,"E2L118C19",933,"CM per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CN-E2L118C20","CN",1,"E2L118C20",934,"CM per Interterminal Switch, AVERAGE ALL FREIGHT CARS",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CN-E2L118C21","CN",1,"E2L118C21",935,"CM per I&I Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CN-E2L118C22","CN",1,"E2L118C22",936,"Average CM per CD, Railroad-Owned, AVERAGE ALL FREIGHT CARS",832.705810546875,838.408203125,803.45916748046898,985.42266845703102,877.11328125,813.18518066406295,783.69482421875,752.58532714843795,757.49151611328102,753.97203179109704,740.87119133657802,741.89313027901505,713.07433860176604,719.674767521018,764.06752470554295,776.63192705167205]
["CN-E2L118C23","CN",1,"E2L118C23",937,"Average Miles between I&I Switches, AVERAGE ALL FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CN-E2L118C24","CN",1,"E2L118C24",938,"Average Miles between Interchange Switches, AVERAGE ALL FREIGHT CARS",456.66467285156301,484.79064941406301,470.23077392578102,455.89779663085898,489.96112060546898,481.62704467773398,525.455322265625,525.82897949218795,502.923095703125,303.95791056994602,297.46877540205702,332.75420791653102,331.45174673738398,325.063318069383,317.13563968710201,349.62618363644799]
["CN-E2L118C25","CN",1,"E2L118C25",939,"SEMs per Industry Switch, AVERAGE ALL FREIGHT CARS",6.5772333145141602,6.1651024818420401,5.9204263687133798,5.26851606369019,4.4945411682128897,4.5362834930419904,4.2201857566833496,3.8595824241638201,3.61066341400146,3.16848959515975,3.0145269105925299,3.0200640212197198,2.9489833525992002,2.9522303405822301,2.76842753556239,2.7475694642338002]
["CN-E2L118C26","CN",1,"E2L118C26",940,"SEMs per Interchange Switch, AVERAGE ALL FREIGHT CARS",3.6174774169921902,3.3908059597015399,3.2562341690063499,2.89768362045288,2.4719979763031001,2.49495577812195,2.3211016654968302,2.12277054786682,1.9858654737472501,1.74266927733786,1.65798980082589,1.66103521167085,1.6219408439295599,1.6237266873202301,1.52263514455932,1.5111632053285899]
["CN-E2L118C27","CN",1,"E2L118C27",941,"SEMs per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",9.8658504486084002,9.2476530075073207,8.8806400299072301,7.9027752876281703,6.7418122291564897,6.8044247627258301,6.3302774429321298,5.7893743515014604,5.4159960746765101,4.7527343927396197,4.5217903658887897,4.5300960318295802,4.4234750288987996,4.42834551087335,4.1526413033435903,4.1213541963507003]
["CN-E2L118C28","CN",1,"E2L118C28",942,"SEMs per Interterminal Switch, AVERAGE ALL FREIGHT CARS",7.89267921447754,7.3981227874755904,7.10451316833496,6.3222188949584996,5.3934493064880398,5.4435405731201199,5.0642228126525897,4.6314988136291504,4.3327965736389196,3.8021875141916999,3.6174322927110398,3.6240768254636699,3.5387800231190401,3.5426764086986799,3.3221130426748702,3.29708335708056]
["CN-E2L118C29","CN",1,"E2L118C29",943,"SEMs per I&I Switch, AVERAGE ALL FREIGHT CARS",1.64430820941925,1.54127550125122,1.4801067113876301,1.3171290159225499,1.12363529205322,1.1340708732605,1.0550463199615501,0.96489560604095503,0.90266597270965598,0.79212239878993795,0.75363172764813202,0.75501600530493096,0.73724583814980005,0.73805758514555897,0.69210688389059805,0.68689236605845005]
["CN-E2L201C1","CN",1,"E2L201C1",944,"Average Distance Per Car In Way Trains",27.8728427886963,28.439661026001001,30.833131790161101,33.650413513183601,38.996040344238303,41.183010101318402,43.783523559570298,48.950469970703097,50.0124702453613,62.195835085226598,70.902070902070903,70.722642845049194,62.311569769202599,46.614017198294697,41.5339843849288,42.4450941804499]
["CN-E2L202C1","CN",1,"E2L202C1",945,"Average TCUs Per Flat Car",4.33,4.4400000000000004,4.22,4,4.4000000000000004,4.46,4.71,4.5199999999999996,4.6100000000000003,5.0599999999999996,5.05,5.12,5.28,5.59,5.47,5.43]
["CN-E2L203C1","CN",1,"E2L203C1",946,"Average Tare Weight - Refrigerated TCU",7.3000001907348597,7.3000001907348597,7.1999998092651403,7.0999999046325701,7,7.0999999046325701,6.9000000953674299,6.9000000953674299,6.9000000953674299,6.9,6.9,6.8,6.9,6.9,7.1,7.1]
["CN-E2L204C1","CN",1,"E2L204C1",947,"Average Tare Weight - Non-Refrigerated TCU",5,5,5,4.9000000953674299,4.9000000953674299,4.9000000953674299,4.9000000953674299,5,5,5,4.9000000000000004,4.7,4.9000000000000004,4.9000000000000004,4.8,4.8]
[{"$f":"B1922&\"-\"&D1922","v":"CN-E2L205C1"},"CN",1,"E2L205C1",948,"Linehaul Miles Per TCU Day",343,343,343,343,343,343,343,343,343,343,343,343,343,343,343,343]
["CN-E2L206C1","CN",1,"E2L206C1",949,"TCU Days Per Orig Or Term Event",3.6150000095367401,3.6150000095367401,3.6150000095367401,3.6150000095367401,3.6150000095367401,3.6150000095367401,3.6150000095367401,3.6150000095367401,3.6150000095367401,3.6150000000000002,3.6150000000000002,3.6150000000000002,3.6150000000000002,3.6150000000000002,3.6150000000000002,3.6150000000000002]
["CN-E2L207C1","CN",1,"E2L207C1",950,"L/E Ratio - Refrigerated/Non-Refrigerated - TCU",1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33,1.33,1.33,1.33,1.33,1.33,1.33]
["CN-E2L208C1","CN",1,"E2L208C1",951,"Average Locomotive Units - Unit Train",2.1591114997863801,2.2363252639770499,2.5220873355865501,2.4609022140502899,2.5051827430725102,2.4917755126953098,2.6221215724945099,2.6721835136413601,2.6039164066314702,2.4462825850378702,2.58210490632734,2.5474717695169602,2.5209987023002198,2.5303066563100902,2.5866327309281001,2.5698806594580001]
["CN-E2L209C1","CN",1,"E2L209C1",952,"Average Locomotive Units - Way Train",1.5975415706634499,1.5638905763626101,1.6462752819061299,1.61387610435486,1.67573642730713,1.62678158283234,1.6344534158706701,1.6696478128433201,1.7221325635910001,1.69999185864891,1.64076592056899,1.6881925809749501,1.6941139302525901,1.70477269675868,1.71114209615768,1.74058635817986]
["CN-E2L210C1","CN",1,"E2L210C1",953,"Average Locomotive Units - Through Train",2.3075544834136998,2.3276522159576398,2.3380279541015598,2.2948241233825701,2.3296458721160902,2.2588050365447998,2.2346849441528298,2.2504930496215798,2.2368800640106201,2.1475694095115698,2.14765665483533,2.1870395378978,2.2216133596264198,2.2073925591857102,2.20324792342528,2.20420536622371]
["CN-E2L211C1","CN",1,"E2L211C1",954,"Average Gross Tons - Unit Train",7839.779296875,7580.5791015625,7860.40966796875,7910.5283203125,8175.86669921875,8341.119140625,8920.919921875,8974.677734375,9187.2080078125,9431.3880631843895,9686.0941997605496,10030.1695951642,10028.8739096438,9666.3833236999508,9726.5722848053301,10107.358889408701]
["CN-E2L212C1","CN",1,"E2L212C1",955,"Average Gross Tons - Way Train",2107.10595703125,2371.357421875,2588.72509765625,2699.21118164063,3102.24169921875,3118.05053710938,3157.66479492188,3215.51538085938,3457.98046875,3061.3804026910402,3236.9008841321502,3613.5723462546598,3561.4375834310199,2851.83379034462,2849.7871352361399,2804.2743829732499]
["CN-E2L213C1","CN",1,"E2L213C1",956,"Average Gross Tons - Through Train",7071.03955078125,7479.70361328125,7319.23046875,7318.197265625,7989.05126953125,7809.2080078125,7805.912109375,7999.3935546875,8200.4609375,7911.4870990607897,8229.1802220551199,8365.0290582736507,8200.3044532275999,7984.2812503141604,8287.4549855245605,8542.2022197406404]
["CN-E2L214C1","CN",1,"E2L214C1",957,"Engine Crews (Excl Train Switching)",43728.24609375,48752.01953125,51291.84765625,44424.44921875,51810.17578125,61875.01953125,70544.0546875,76323.6328125,88205.5703125,78667.463797253105,74475.897648403901,85548.879780110103,95661.633828001402,93249.139276187998,74121.859312407105,77649.533475661796]
["CN-E2L215C1","CN",1,"E2L215C1",958,"Train Crews (Excl Train Switching)",45152.703125,46935.2734375,49997.25390625,43136.953125,50271.31640625,52104.11328125,65763.75,66645.5078125,86433.2890625,79396.688293102095,74640.0641908619,86092.274567542496,96431.321616975198,94304.948930044397,76588.894789272497,80541.623889712093]
["CN-E2L216C1","CN",1,"E2L216C1",959,"Total Crew Wages (Excl Train Switching)",88880.953125,95687.296875,101289.1015625,87561.40625,102081.4921875,113979.1328125,136307.8125,142969.140625,174638.859375,158064.152090355,149115.961839266,171641.15434765301,192092.95544497701,187554.088206232,150710.75410168001,158191.15736537401]
["CN-E2L217C1","CN",1,"E2L217C1",960,"Train Miles - Running",16635.658203125,16016.669921875,15793.8974609375,13126.0361328125,14211.9765625,14790.8896484375,15816.1357421875,16755.623046875,17538.390625,17372.300999999999,15966.052,16721.621999999999,17758.848999999998,17883.858,15447.376,15969.494000000001]
["CN-E2L218C1","CN",1,"E2L218C1",961,"Average Crew Wages (Assigned To TM-Crew)",5.3427972793579102,5.9742317199706996,6.4131793975830096,6.6708188056945801,7.18277931213379,7.7060360908508301,8.6182756423950195,8.5326070785522496,9.95751953125,9.0986307507770707,9.3395638345200105,10.264623512459099,10.8167458062725,10.487339376449601,9.7563983748229806,9.9058340461741601]
["CN-E2L219C1","CN",1,"E2L219C1",962,"General Overhead Ratio",1.0761872529983501,1.0488741397857699,1.10186696052551,1.1216766834259,1.11772525310516,1.1003994941711399,1.1020426750183101,1.0956671237945601,1.1044222116470299,1.0909972596234001,1.1065045061521901,1.1193261249725099,1.1022213734983499,1.11179302751452,1.11541783591972,1.0449111660909101]
["CN-E2L220C1","CN",1,"E2L220C1",963,"Constant Cost Markup Ratio",1.5771080255508401,1.5790984630584699,1.5519503355026201,1.63928151130676,1.5592564344406099,1.52821958065033,1.50557065010071,1.5112154483795199,1.4828453063964799,1.52229376285405,1.5228444127027601,1.5083669215861699,1.49397220392207,1.4780155680628499,1.5211310947087799,1.5246100773558999]
["CN-E2L301C1","CN",1,"E2L301C1",964,"Residual Factor, Industry Switching, Railroad-Owned",24.5422436583459,26.6695310608353,30.386633147273201,39.0096840774047,61.771965200589399,17.226045579904401,35.593847055745798,45.046923436921062,46.061078164322602,37.011851521998899,35.856734316226898,41.968139309839998,47.965411639500701,48.025028037875401,49.515911445835215,55.487186254366897]
["CN-E2L301C2","CN",1,"E2L301C2",965,"Residual Factor, Industry Switching, Privately-Owned",21.5931267479517,23.186972911478101,26.662530737091,32.887552366397699,53.876438620340799,9.1844829972080309,27.7288587539995,36.817110109548885,38.430116435205001,28.545332712454702,25.9779343985239,31.162892284239302,36.268802358249999,35.428808219469502,36.304658044093053,41.463458678642802]
["CN-E2L302C1","CN",1,"E2L302C1",966,"Residual Factor, Station Clerical, Railroad-Owned",7.79018446268672,9.1191087229797407,11.320735077692399,17.2169598701716,21.0183886472417,20.293783610255002,22.631402057045701,23.117338966455559,20.7989174995502,22.543691691550698,24.0961797732013,26.341429964993999,28.397053897829899,28.830225483757999,29.687834777682482,32.501720191051099]
["CN-E2L302C2","CN",1,"E2L302C2",967,"Residual Factor, Station Clerical, Privately-Owned",2.49852493827041,3.1041785535541502,4.9395553539100199,6.7464395306436398,7.1467222554102197,6.4039800952160704,8.9445561658725907,8.556570813620116,7.5753131668575397,8.0061806412911292,7.2468124770975004,8.3707140429297198,8.6528531245364295,7.7960167274975003,7.5774194471885057,8.3180839007981806]
["CN-E2L303C1","CN",1,"E2L303C1",968,"Residual Factor, Interchange Switching, Railroad-Owned",2.5379230808412099,2.1200080537194701,2.5690474563941499,3.07887393520758,4.7753420315731603,1.15720873497029,2.6939037651449,2.8870773368145497,3.5658648560071899,3.0640973042776301,2.73689891671938,2.7204012044296899,2.8790619029598798,3.5421093298698398,3.3485274096610791,3.1561825840001698]
["CN-E2L303C2","CN",1,"E2L303C2",969,"Residual Factor, Interchange Switching, Privately-Owned",2.1458747967101899,1.69288599446424,2.08777551896164,2.38380099535431,4.1003884441683303,0.67515130281703195,2.0302011248294498,2.3621760559238942,3.1454165854818599,2.4858777854874798,2.26135854060899,2.2230704090061999,2.6028469145808999,3.0754152623973599,2.7696545664642742,2.8799504132876099]
["CN-E2L304C1","CN",1,"E2L304C1",970,"Residual Factor, I&I Switching, Railroad-Owned",8.2024250574768391,8.2204016695487692,9.3128446914842904,10.8958875637726,16.9408707848118,7.2303222139079697,13.8718508409573,13.134100487360129,14.0741573259826,13.7994327894138,15.542351996047399,20.718228297261302,31.263841736616701,18.843300777302801,17.124094961031386,22.359011307178498]
["CN-E2L304C2","CN",1,"E2L304C2",971,"Residual Factor, I&I Switching, Privately-Owned",6.1823051377989504,6.2325695374408099,6.8740650862027399,6.8386615056125999,12.3501476331892,2.1760420776826002,7.2632346751385199,8.4458665353167195,10.6491409080915,8.1976615464058291,10.773324841819701,14.7947110959492,24.281371523504099,14.2022358682788,12.507244163553244,16.706307286702302]
["CN-E2L305C1","CN",1,"E2L305C1",972,"Residual Factor, Mileage, Railroad-Owned",0.38095559443376198,0.473554430047886,1.03814554223623,0.73436826075572703,0.71247874478559603,1.86642632412151,1.07295909248154,1.4725557428066323,1.2141155679326601,2.2386259501802299,1.9847869899105399,1.6701582801850401,2.9215208088945199,3.3309760374591799,4.0457604621437753,6.86123582383886]
["CN-E2L305C2","CN",1,"E2L305C2",973,"Residual Factor, Mileage, Privately-Owned",0.40858836414278599,0.37501799184940099,0.95728451434463102,0.62198976422448304,0.59855362788203004,1.5298442266029799,0.88441814753432002,1.1281974345630521,1.01107107893179,1.7283760739594101,1.5029372998973001,1.28885499301666,2.6733025199827898,3.0000822247797299,4.0985790134348559,6.3437375289533797]
["CP-E1L101C1","CP",6,"E1L101C1",1,"Gross Ton Mile (GTM), OPR Expense",1.8800311954692E-3,1.88463891390711E-3,2.4432505015283801E-3,1.8583445344120301E-3,2.2641625255346298E-3,2.8175332117825699E-3,4.0033324621617803E-3,2.9264132026583E-3,2.86888470873237E-3,2.1998590808814601E-3,2.0829669577020898E-3,2.4195621585572E-3,2.6034963986884302E-3,2.6503443920890902E-3,2.2862563084409802E-3,2.5443424076676E-3]
["CP-E1L101C2","CP",6,"E1L101C2",2,"Gross Ton Mile (GTM), DRL Expense",5.2551174303516702E-4,4.2978840065188701E-4,4.44429431809112E-4,5.4590520448982705E-4,7.1282463613897605E-4,6.6498701926320802E-4,6.5427942899987102E-4,6.2538357451558102E-4,6.0648983344435703E-4,5.7326084630182302E-4,7.2470410849732197E-4,7.1696427544132096E-4,6.9744831249622197E-4,7.9001214579413901E-4,9.6661010970487205E-4,8.9922621376512001E-4]
["CP-E1L101C3","CP",6,"E1L101C3",3,"Gross Ton Mile (GTM), ROI Expense",8.9071411639452002E-4,1.16679212078452E-3,1.33396429009736E-3,1.31601630710065E-3,2.12954357266426E-3,2.2883599158376499E-3,2.3383568041026601E-3,2.20007752068341E-3,1.8836235394701401E-3,1.8237439907020699E-3,2.0815842733092498E-3,2.1963412022073699E-3,2.4091654137181001E-3,1.9348982601664099E-3,1.9522201300284901E-3,2.4724392413642601E-3]
["CP-E1L102C1","CP",6,"E1L102C1",4,"Car Mile (CM) - Other Than Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L102C2","CP",6,"E1L102C2",5,"Car Mile (CM) - Other Than Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L102C3","CP",6,"E1L102C3",6,"Car Mile (CM) - Other Than Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L103C1","CP",6,"E1L103C1",7,"Train Mile (TM) - Other Than Crew, OPR Expense",0.44837316870689398,0.42839401960372903,0.776921927928925,0.64582473039627097,0.58156663179397605,0.76377832889556896,0.70635259151458696,0.40651872754097002,0.41292804479598999,0.54482914558707196,0.54364723794220804,0.36415151454021799,0.42855725665019401,0.48499515021841499,0.381005380510958,0.36470664685905602]
["CP-E1L103C2","CP",6,"E1L103C2",8,"Train Mile (TM) - Other Than Crew, DRL Expense",4.0220213122665899E-3,-2.36420296132565E-2,-2.4444483220577198E-2,-2.0903820171952199E-2,-9.7801107913255692E-3,-9.8356860689818902E-4,-3.1739971600472901E-3,3.58434370718896E-3,3.3459020778536801E-3,3.3557450965947498E-3,5.4148295648329403E-3,-2.6295595020192899E-3,-2.4436100000147999E-3,-4.0688370248217302E-2,-1.22566645538052E-2,-1.2275103439430101E-2]
["CP-E1L103C3","CP",6,"E1L103C3",9,"Train Mile (TM) - Other Than Crew, ROI Expense",-9.3434108421206492E-3,-7.6436083763837797E-3,-3.7640219088643798E-3,-7.29012652300298E-4,6.9153448566794395E-4,7.4157165363430999E-4,4.06292849220335E-4,-1.5513927792199E-5,1.2022986629745E-4,-4.5910682975850998E-4,-1.0557751744458799E-3,-1.07504632765431E-3,-7.1160375772948495E-4,-1.6419973888758201E-3,1.25024466354516E-3,-5.3149857580574796E-4]
["CP-E1L104C1","CP",6,"E1L104C1",10,"Train Mile (TM) - Crew, OPR Expense",5.3252873420715297,4.97043657302856,5.52799320220947,6.1603312492370597,6.6033067703247097,7.6208314895629901,8.1185712814331108,7.2541136741638201,8.9301662445068395,11.0249626531981,10.873447510919499,10.940013976761,11.3456900227277,11.6970281414648,11.031844780390101,11.1238523599575]
["CP-E1L104C2","CP",6,"E1L104C2",11,"Train Mile (TM) - Crew, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L104C3","CP",6,"E1L104C3",12,"Train Mile (TM) - Crew, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L105C1","CP",6,"E1L105C1",13,"Locomotive Unit Mile (LUM), OPR Expense",4.1714420318603498,4.2501664161682102,5.7245907783508301,4.0375900268554696,4.5962028503418004,5.8749256134033203,6.4466814994812003,6.63928127288818,7.22841453552246,4.5850840571539999,3.9118493879837901,5.0857277122435196,5.8083588923529001,5.39008086299705,4.4855707001123903,6.3054730183872101]
["CP-E1L105C2","CP",6,"E1L105C2",14,"Locomotive Unit Mile (LUM), DRL Expense",0.81619960069656405,0.58095848560333296,0.53902757167816195,0.68415522575378396,0.43730366230010997,0.35207089781761203,0.301463723182678,0.29267808794975297,0.125604763627052,3.9736242357267998E-4,-0.121783191080339,0.108253842756476,0.24510498965121999,0.28453556767240201,0.23530685797648199,0.166940026808227]
["CP-E1L105C3","CP",6,"E1L105C3",15,"Locomotive Unit Mile (LUM), ROI Expense",0.29901081323623702,0.83150368928909302,0.84027171134948697,0.60196691751480103,0.49881112575531,0.52544987201690696,0.51636475324630704,0.69539517164230302,0.64477711915969804,0.75811328036464698,0.96395338439644696,1.0375126294716499,1.37774520946141,1.0626604542443601,1.1580565549027599,1.54283324472577]
["CP-E1L106C1","CP",6,"E1L106C1",16,"CLOR (Carloads Handled) - Other, OPR Expense",0,0,0.25326359272003202,0.67434161901473999,0.57381749153137196,1.0648285150528001,1.19916439056396,1.17713582515717,0.74952626228332497,0.670179393682519,0.26048019658940602,0.20359232892447199,6.7080124576074499E-2,3.6527472375797503E-2,0.125941684037429,0.22841087273731001]
["CP-E1L106C2","CP",6,"E1L106C2",17,"CLOR (Carloads Handled) - Other, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L106C3","CP",6,"E1L106C3",18,"CLOR (Carloads Handled) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L107C1","CP",6,"E1L107C1",19,"CLOR (Carloads Handled) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L107C2","CP",6,"E1L107C2",20,"CLOR (Carloads Handled) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L107C3","CP",6,"E1L107C3",21,"CLOR (Carloads Handled) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L108C1","CP",6,"E1L108C1",22,"CLOT (Carloads Orig Or Term) - Other, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L108C2","CP",6,"E1L108C2",23,"CLOT (Carloads Orig Or Term) - Other, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L108C3","CP",6,"E1L108C3",24,"CLOT (Carloads Orig Or Term) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L109C1","CP",6,"E1L109C1",25,"CLOT (Carloads Orig Or Term) - Clerical, OPR Expense",15.1141977310181,13.140795707702599,15.289400100708001,19.458724975585898,11.684365272521999,12.7430019378662,12.653094291686999,13.6496429443359,16.6213073730469,13.397347094124401,12.120381193158099,9.2815224132670995,9.3429674439441204,9.7901535612415707,9.8538087174958395,7.9186360746555797]
["CP-E1L109C2","CP",6,"E1L109C2",26,"CLOT (Carloads Orig Or Term) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L109C3","CP",6,"E1L109C3",27,"CLOT (Carloads Orig Or Term) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L110C1","CP",6,"E1L110C1",28,"Car Mile (CM) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L110C2","CP",6,"E1L110C2",29,"Car Mile (CM) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L110C3","CP",6,"E1L110C3",30,"Car Mile (CM) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L111C1","CP",6,"E1L111C1",31,"Switch Engine Minutes (SEM), OPR Expense",3.7092123031616202,3.5826618671417201,4.1675167083740199,4.1187725067138699,3.94721460342407,4.5896167755126998,5.6940031051635698,4.7315707206726101,5.6135749816894496,5.3323109378451701,5.3889804209490499,6.2184395472401199,6.8935773494889796,7.0722734797448501,7.1217742957985504,7.4604167727036304]
["CP-E1L111C2","CP",6,"E1L111C2",32,"Switch Engine Minutes (SEM), DRL Expense",0.30173525214195301,0.29134657979011502,0.29541960358619701,0.33139339089393599,0.40704646706581099,0.38828226923942599,0.38128009438514698,0.40777879953384399,0.52059745788574197,0.59709919080940499,0.94549704198309503,1.12277383551979,1.2358063521476601,1.41216687376574,1.8957367267969101,1.72317525401896]
["CP-E1L111C3","CP",6,"E1L111C3",33,"Switch Engine Minutes (SEM), ROI Expense",0.50597542524337802,0.70781040191650402,0.75963896512985196,0.68696361780166604,1.90801334381104,2.0257725715637198,2.1737196445465101,2.2220001220703098,2.18321561813354,2.3191242757839801,2.9979015759415502,3.8730750251105301,4.5105848772570898,3.7462152083475502,4.1905598207920303,5.5275154831776003]
["CP-E1L112C1","CP",6,"E1L112C1",34,"Ton Miles In Lake Transfer Service, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L112C2","CP",6,"E1L112C2",35,"Ton Miles In Lake Transfer Service, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L112C3","CP",6,"E1L112C3",36,"Ton Miles In Lake Transfer Service, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L113C1","CP",6,"E1L113C1",37,"Tons Handled at Coal Terminals, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L113C2","CP",6,"E1L113C2",38,"Tons Handled at Coal Terminals, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B1986&\"-\"&D1986","v":"CP-E1L113C3"},"CP",6,"E1L113C3",39,"Tons Handled at Coal Terminals, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L114C1","CP",6,"E1L114C1",40,"Tons Handled at Ore Terminals, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L114C2","CP",6,"E1L114C2",41,"Tons Handled at Ore Terminals, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L114C3","CP",6,"E1L114C3",42,"Tons Handled at Ore Terminals, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L115C1","CP",6,"E1L115C1",43,"Tons Handled at Other Marine Terminals, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L115C2","CP",6,"E1L115C2",44,"Tons Handled at Other Marine Terminals, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L115C3","CP",6,"E1L115C3",45,"Tons Handled at Other Marine Terminals, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L116C1","CP",6,"E1L116C1",46,"Refrigerated Car Miles, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L116C2","CP",6,"E1L116C2",47,"Refrigerated Car Miles, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L116C3","CP",6,"E1L116C3",48,"Refrigerated Car Miles, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L117C1","CP",6,"E1L117C1",49,"Protective Service Reefer TCU Days, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L117C2","CP",6,"E1L117C2",50,"Protective Service Reefer TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L117C3","CP",6,"E1L117C3",51,"Protective Service Reefer TCU Days, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L118C1","CP",6,"E1L118C1",52,"Refrigerated TCU Days, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L118C2","CP",6,"E1L118C2",53,"Refrigerated TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L118C3","CP",6,"E1L118C3",54,"Refrigerated TCU Days, ROI Expense",0.97661149501800504,0.92459839582443204,0.75003629922866799,0.70307016372680697,0.42942896485328702,0.403649181127548,0.30046004056930498,7.9810738563537598E-2,0.76014775037765503,1.51372698644861,0,4.3364804895530096,4.3923890004624999,3.3970099127370301,2.8522602326434399,6.4730414097464601]
["CP-E1L120C1","CP",6,"E1L120C1",58,"TCUs Loaded And Unloaded (L&UL), OPR Expense",34.706352233886697,41.500446319580099,43.8747749328613,45.377418518066399,51.034267425537102,47.013011932372997,66.000267028808594,70.554656982421903,72.816703796386705,79.105762442828805,71.780810081512897,59.905894016962101,61.696104152309999,62.437868427679803,83.1361725485596,80.694317305502807]
["CP-E1L121C1","CP",6,"E1L121C1",61,"MVUs Loaded And Unloaded (L&UL), OPR Expense",2.03891229629517,1.81526362895966,3.2269425392150901,3.2125906944274898,5.1279993057251003,3.1819496154785201,3.52769899368286,2.0759596824646001,0.310688406229019,3.4727441099292801E-2,9.9605829895990894,10.9227006431907,9.8877230979679798,15.457289041143801,16.301442700509099,21.343354128373299]
["CP-E1L122C2","CP",6,"E1L122C2",65,"TCUs Picked Up and Delivered (PU&D), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L201C2","CP",6,"E1L201C2",68,"CM(R), DRL Expense, Railroad-Owned, BOX - 40 FT",-2.4538084398955098E-3,-9.5712229609489399E-2,-0.14838233590125999,-0.450222939252853,-5.88069558143616E-2,0.14019538462162001,0.101834282279015,0.140630438923836,0.113162606954575,0.14981023558760401,0.15061689294289099,8.6623196592746199E-2,4.7871207128131997E-2,7.84696693766887E-2,4.57887404531645E-2,4.4949382449287999E-2]
["CP-E1L201C5","CP",6,"E1L201C5",71,"CM(Y), DRL Expense, Railroad-Owned, BOX - 40 FT",-6.3799000345170498E-3,-0.24885191023349801,-0.38579434156417802,-1.17058110237122,-0.15289825201034499,0.364507555961609,0.264769017696381,0.365639448165894,0.29422220587730402,0.38950661252777002,0.39160392165151597,0.22522031114113999,0.124465138533143,0.20402114037939101,0.119050725178228,0.116868394368149]
["CP-E1L201C6","CP",6,"E1L201C6",72,"CM(Y), ROI Expense, Railroad-Owned, BOX - 40 FT",-0.11883531510829901,-0.16517198085784901,0.31668674945831299,0.57748806476592995,0.14601533114910101,4.9171246588230098E-2,3.2963626086711897E-2,4.1336536407470703E-2,7.02188014984131E-2,4.9067118254573702E-2,2.1406445241935902E-2,1.09408414683303E-2,-1.65426261822182E-6,-4.5620728537822597E-3,-4.9138457441282504E-3,-4.7344180531939698E-3]
["CP-E1L201C9","CP",6,"E1L201C9",75,"CD(R), ROI Expense, Railroad-Owned, BOX - 40 FT",-10.2671365737915,-11.8472280502319,25.031003952026399,46.574558258056598,15.274863243103001,3.5742094516754199,2.41949486732483,3.0825214385986301,5.0245265960693404,3.7330318355403702,1.36021431587139,0.65463551516131602,-7.0781774938238201E-2,-0.32629313393211101,-0.28445035356554899,-0.32519855148499599]
["CP-E1L202C1","CP",6,"E1L202C1",80,"CM(R), OPR Expense, Railroad-Owned, BOX - 50 FT",6.2058098614215899E-2,6.7253097891807598E-2,6.6179797053337097E-2,9.3401245772838606E-2,7.3442690074443803E-2,6.4327195286750793E-2,4.9754928797483403E-2,4.2093612253665903E-2,3.3422123640775701E-2,4.8835527054599301E-2,5.4105137593317101E-2,4.5841258981160198E-2,1.0856701505639801E-2,2.9437515109410997E-4,1.18930292588286E-4,2.3569573464134701E-4]
["CP-E1L202C4","CP",6,"E1L202C4",83,"CM(Y), OPR Expense, Railroad-Owned, BOX - 50 FT",0.16135106980800601,0.174858093261719,0.172067150473595,0.24284330010414101,0.19095107913017301,0.16725073754787401,0.129362717270851,0.109443306922913,8.6897641420364394E-2,0.12697237034195799,0.14067335774262399,0.119187273351017,2.8227423914663499E-2,7.6537539284468701E-4,3.0921876072954299E-4,6.1280891006750199E-4]
["CP-E1L202C7","CP",6,"E1L202C7",86,"CD(R), OPR Expense, Railroad-Owned, BOX - 50 FT",6.2642593383789098,7.8248825073242196,9.0698280334472692,12.231610298156699,11.574791908264199,9.5897045135497994,7.1086087226867702,5.6480951309204102,4.4967885017395002,6.84362537382383,7.4875591275746203,6.1706864668943204,1.58011018594771,3.88350264628557E-2,1.45833518434664E-2,2.56907050852389E-2]
["CP-E1L202C11","CP",6,"E1L202C11",90,"CD(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",-7.37734127044678,-23.032722473144499,-37.597312927246101,-93.495956420898395,62.906482696533203,85.656715393066406,48.825630187988303,43.335563659667997,37.1399116516113,49.388545047773697,44.918140069322398,26.322490799107399,22.476635890443699,20.416982381002601,49.197477962126598,44.467639171953003]
["CP-E1L203C1","CP",6,"E1L203C1",93,"CM(R), OPR Expense, Railroad-Owned, BOX - EQUIPPED",1.9782925024628601E-2,2.1795786917209601E-2,2.05575507134199E-2,1.27611989155412E-2,7.3575349524617204E-3,7.304472848773E-3,7.2292503900826003E-3,4.4295587576925798E-3,1.9583208486437802E-3,5.2896771538228995E-4,1.6966897153883001E-4,2.8585349655708601E-4,6.9738515127368305E-4,6.95544685878613E-4,7.2113788316444903E-3,1.38425472729608E-2]
["CP-E1L203C4","CP",6,"E1L203C4",96,"CM(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED",5.1435593515634502E-2,5.6669034063816098E-2,5.3449608385562897E-2,3.3179156482219703E-2,1.9129566848278001E-2,1.89916305243969E-2,1.8796062096953399E-2,1.15168550983071E-2,5.0916341133415699E-3,1.37531605999396E-3,4.4113932600095898E-4,7.4321909104842297E-4,1.8132013933115801E-3,1.80841618328439E-3,1.87495849622757E-2,3.5990622909698101E-2]
["CP-E1L203C5","CP",6,"E1L203C5",97,"CM(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED",0.15033344924449901,0.15538185834884599,0.17392283678054801,0.164615944027901,0.184110462665558,0.17036174237728099,0.16825556755065901,0.16820557415485399,0.180371403694153,0.19138776777140201,0.20276103622154601,0.19978751251143201,0.21751849332644799,0.221757968500189,0.17192491500371301,0.17859905870100901]
["CP-E1L203C8","CP",6,"E1L203C8",100,"CD(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED",22.715122222900401,21.5320930480957,23.439205169677699,31.964006423950199,30.909013748168899,21.636741638183601,16.826694488525401,21.366010665893601,26.223127365112301,22.239966830099402,20.611118468806499,18.569475794477899,17.9393515505067,15.938536889621901,15.060041361593999,13.2328229666624]
["CP-E1L203C13","CP",6,"E1L203C13",105,"CM(R), DRL Expense, Privately-Owned, BOX - EQUIPPED",0.127306252717972,0.15377813577652,0.178874626755714,0.26425057649612399,0.1180819272995,0.14273367822170299,0.13459315896034199,0.14714372158050501,0.27422979474067699,0.298259651795169,0.39615425857313502,0.464573777353184,0.48903194965388103,0.56060189263337101,0.45113713801468103,0.47147479919250501]
["CP-E1L204C3","CP",6,"E1L204C3",108,"CM(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",2.4868585751391898E-4,2.20066664041951E-4,3.9836819632910197E-4,6.7573419073596597E-4,4.66243247501552E-4,6.4746504904178403E-6,8.9232726168120297E-6,4.7709909267723603E-6,0,0,0,0,0,0,0,0]
["CP-E1L204C6","CP",6,"E1L204C6",111,"CM(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",6.4658257178962198E-4,5.7217269204556899E-4,1.03575643151999E-3,1.7569143092259799E-3,1.2122284388169601E-3,1.68340739037376E-5,2.3200489522423599E-5,1.2404585504555099E-5,0,0,0,0,0,0,0,0]
["CP-E1L204C10","CP",6,"E1L204C10",115,"CD(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",2.51669049263,2.4554877281189,6.8354926109314,7.0095911026001003,6.2633824348449698,0.11233749985694901,9.9366858601570102E-2,7.2982735931873294E-2,0,0,0,0,0,0,0,0]
["CP-E1L204C13","CP",6,"E1L204C13",118,"CM(R), DRL Expense, Privately-Owned, GONDOLA - PLAIN",4.8113116063177603E-3,7.6456572860479398E-3,6.8485499359667301E-3,6.2697320245206399E-3,1.9228808581829099E-2,2.2508567199110999E-2,2.1515019237995099E-2,2.38421838730574E-2,3.91642414033413E-2,2.5841204132211699E-2,1.80659423918842E-2,2.7772671895393401E-2,3.4078965873809597E-2,3.9971930150009001E-2,2.7937847237459401E-2,4.5013738020303999E-2]
["CP-E1L205C1","CP",6,"E1L205C1",119,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.9005037620663601E-2,3.6052379757165902E-2,3.59876081347466E-2,3.81115265190601E-2,2.7703650295734399E-2,2.5840710848569901E-2,2.97328308224678E-2,2.92926374822855E-2,3.0349796637892699E-2,3.75648467679187E-2,4.3133044097391701E-2,6.8551469451372804E-2,7.7320878331871803E-2,7.8607702372975499E-2,6.9652334427243195E-2,7.0989140288835004E-2]
["CP-E1L205C4","CP",6,"E1L205C4",122,"CM(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",7.5413063168525696E-2,9.3736357986927005E-2,9.3567818403244005E-2,9.90896746516228E-2,7.2029478847980499E-2,6.7185826599597903E-2,7.7305421233177199E-2,7.6160833239555401E-2,7.8909493982791901E-2,9.7668601596588703E-2,0.11214591465321901,0.17823382057356901,0.20103428366286699,0.204380026169736,0.18109606951083199,0.18457176475097101]
["CP-E1L205C7","CP",6,"E1L205C7",125,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",5.0107331275939897,6.7752308845520002,7.2360515594482404,7.3122982978820801,4.7625403404235804,3.2650132179260298,3.4464097023010298,3.2608349323272701,3.5249817371368399,4.6774583803784697,5.37381868142021,8.3709066763588105,8.8525192305312892,8.8260638181506703,7.8653343826307598,7.7063610555614002]
["CP-E1L205C12","CP",6,"E1L205C12",130,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",1.4962782859802199,1.6918009519577,2.0672469139099099,3.7539246082305899,2.9364676475524898,2.70284843444824,2.5770065784454301,3.83288478851318,1.61542284488678,2.18309671644935,2.1809210668066599,5.0283733257196603,6.3469631431068096,5.6945550483997396,5.4085879566175601,7.2463383016777003]
["CP-E1L206C2","CP",6,"E1L206C2",133,"CM(R), DRL Expense, Railroad-Owned, HOPPER - COVERED",-6.5395474433898898E-2,-6.22326917946339E-2,-5.5958837270736701E-2,-3.7494469434022903E-2,-2.80717797577381E-2,-3.62665578722954E-2,-3.6319438368081998E-2,-4.20933775603771E-2,-8.3288609981536907E-2,-8.3662384650897204E-2,-0.107854583035548,-0.100152478374694,-0.107311780324816,-0.11969168153344099,-0.163870285243716,-0.144450227528861]
["CP-E1L206C5","CP",6,"E1L206C5",136,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",-0.170028045773506,-0.16180510818958299,-0.14549301564693501,-9.7485683858394595E-2,-7.2986617684364305E-2,-9.4293057918548598E-2,-9.4430528581142398E-2,-0.109442859888077,-0.216550543904305,-0.217522200092333,-0.28042191589242599,-0.26039644377420301,-0.27901062884452199,-0.311198371986947,-0.42606274163366198,-0.37557059157503803]
["CP-E1L206C9","CP",6,"E1L206C9",140,"CD(R), ROI Expense, Railroad-Owned, HOPPER - COVERED",11.978472709655801,8.8187923431396502,8.3188562393188494,7.1775693893432599,4.6476998329162598,5.6143741607665998,6.2836418151855504,6.5206785202026403,5.9520020484924299,6.7495291423869199,6.0863038232056201,7.15953894372009,9.2888324465321297,7.6467557209650403,6.1611416536588903,7.1913291026945103]
["CP-E1L206C12","CP",6,"E1L206C12",143,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED",11.978472709655801,8.8187923431396502,8.3188562393188494,7.1775693893432599,4.6477003097534197,5.6143736839294398,6.2836413383483896,6.5206785202026403,5.9520015716552699,6.7495291423869199,6.0863038232056201,7.15953894372009,9.2888324465321297,7.6467557209650403,6.1611416536588903,7.1913291026944997]
["CP-E1L206C13","CP",6,"E1L206C13",144,"CM(R), DRL Expense, Privately-Owned, HOPPER - COVERED",2.4352202191948901E-2,2.2118460386991501E-2,9.5900027081370406E-3,5.4572224617004403E-3,9.3157999217510206E-3,4.9615311436355097E-3,3.6538299173116701E-3,6.24160224106163E-4,3.6744062526850003E-5,2.69815193495225E-2,2.6999837507642999E-2,2.2584208775490201E-2,2.1880977336752899E-2,2.4540876056971899E-2,6.0452184340604298E-6,2.33260527862378E-2]
["CP-E1L207C6","CP",6,"E1L207C6",150,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",3.3689253032207503E-2,-2.1340681239962599E-2,9.6642717719078106E-2,0.15673461556434601,0.113832384347916,0.11344648152589799,0.119867257773876,7.83524960279465E-2,0.13395084440708199,0.127547981125439,0.228583687501594,0.55007723874800696,0.46246207814594797,0.39074792580564299,0.51936368622437901,1.2625288301386599]
["CP-E1L207C7","CP",6,"E1L207C7",151,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.97123050689697,3.6722822189331099,5.3680324554443404,5.4236097335815403,5.0039086341857901,4.2986941337585396,5.7695784568786603,9.8579998016357404,11.944247245788601,13.5242506667505,13.201297818414099,11.186782859686,10.998181740269899,5.43522065722079,2.8053052710427702,1.2379923401227699]
["CP-E1L207C11","CP",6,"E1L207C11",155,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",3.5320007801055899,3.5191941261291499,11.624274253845201,24.093704223632798,14.288475036621101,0.40872937440872198,33.955249786377003,51.112247467041001,34.333431243896499,31.120167535692101,60.061665277394603,71.050139928517794,109.162541480643,-239.64552205644199,-129.424694172687,-400.06755099456302]
["CP-E1L208C1","CP",6,"E1L208C1",158,"CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.34405938535929E-2,2.2690379992127401E-2,1.5563142485916601E-2,1.0958407074213E-2,0,0,0,3.3588772639632199E-3,2.8939894400537001E-3,4.81312442916832E-3,4.5902598626356202E-3,5.3267637722536898E-3,2.96062294857065E-3,0,0,0]
["CP-E1L208C4","CP",6,"E1L208C4",161,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",6.0945518314838402E-2,5.8995310217142098E-2,4.0464200079441098E-2,2.8491828590631499E-2,0,0,0,8.7331049144268001E-3,7.5243804603815096E-3,1.25141235158376E-2,1.1934675642852499E-2,1.38495858078597E-2,7.6976196662836803E-3,0,0,0]
["CP-E1L208C8","CP",6,"E1L208C8",165,"CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",117.582572937012,79.929626464843807,4.3254876136779803,290.52862548828102,3253.56884765625,7789.58447265625,7120.791015625,11738.7080078125,3310.89526367188,151.963312544383,97.927434276260996,15.046793748069501,-134.90250116476901,13.781405590945001,7.7022328678094603,16.958035846112899]
["CP-E1L208C11","CP",6,"E1L208C11",168,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",117.58258056640599,79.929626464843807,4.3254876136779803,290.52862548828102,3253.56860351563,7789.58447265625,7120.791015625,11738.70703125,3310.89526367188,151.963312544383,97.927434276260996,15.046793748069501,-134.90250116476901,13.781405590945001,7.7022328678094603,16.958035846112899]
["CP-E1L208C12","CP",6,"E1L208C12",169,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",9.3571096658706707E-2,9.7265154123306302E-2,6.5882839262485504E-2,0.182754591107368,0,0,0,1.3749245554208801E-2,6.1438013799488501E-3,3.6339467906489902E-3,2.71181762179286E-2,0.113702514094165,1.37446207819527E-2,0,0,0]
["CP-E1L209C5","CP",6,"E1L209C5",175,"CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",0.36518698930740401,0.341594457626343,0.32517564296722401,0.35326075553893999,0.30425140261650102,0.26590880751609802,0.26186084747314498,0.21635663509368899,0.322823166847229,0.47010179917205602,0.88230840182013603,0.89209933639527095,0.39785176829698998,0.23581816073522499,0.23828275554435799,0.24763508266020601]
["CP-E1L209C6","CP",6,"E1L209C6",176,"CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",6.1911734519526395E-4,9.28834197111428E-4,4.9731123726814996E-4,1.6219685494434099E-4,3.5407934774411802E-5,5.6989636505022598E-5,4.61156996607315E-5,0,0,0,0,0,0,0,0,0]
["CP-E1L209C10","CP",6,"E1L209C10",180,"CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",2.7134034633636501,3.9969630241393999,3.1421587467193599,1.4539489746093801,0.28343236446380599,0.16008035838604001,0.120411708950996,0,0,0,0,0,0,0,0,0]
["CP-E1L209C13","CP",6,"E1L209C13",183,"CM(R), DRL Expense, Privately-Owned, REFRIGERATED - MECH",7.12515180930495E-3,1.1036193463951299E-3,3.21391550824046E-3,5.0343276234343605E-4,9.8361819982528708E-4,7.1189895970746896E-4,5.6088087148964405E-4,3.4781752037815798E-4,1.32896902505308E-3,3.9134411713082301E-4,4.6815473544930403E-4,6.5648843278026095E-4,7.02276994498786E-4,6.7938145774834298E-4,7.6907352627534199E-4,6.0245595957216197E-4]
["CP-E1L210C4","CP",6,"E1L210C4",187,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",5.9902831912040697E-2,5.8688461780548103E-2,4.5531980693340302E-2,2.7296964079141599E-2,2.1947098895907399E-2,2.59202979505062E-2,0.17185592651367201,0.21786345541477201,0.26855957508087203,6.8942062452884006E-2,5.3598770421663798E-2,6.1975853771806803E-2,0,0,0,0]
["CP-E1L210C7","CP",6,"E1L210C7",190,"CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",5.4073076248168901,5.3283209800720197,4.2388653755187997,2.4885990619659402,1.6489182710647601,1.4286459684371899,8.0648231506347692,9.3209180831909197,11.5458421707153,3.63986287280667,3.3090719386998102,4.6705152289876803,0,0,0,0]
["CP-E1L210C10","CP",6,"E1L210C10",193,"CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",5.4073071479797399,5.3283200263977104,4.2388658523559597,2.4885990619659402,1.6489182710647601,1.4286462068557699,8.0648231506347692,9.3209171295165998,11.5458421707153,3.6398628728066802,3.3090719386998102,4.6705152289876803,0,0,0,0]
["CP-E1L210C11","CP",6,"E1L210C11",194,"CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",26.331274032592798,-14.078834533691399,-13.1412801742554,-1.22814846038818,43.401889801025398,54.403770446777301,64.591400146484403,35.464561462402301,28.067512512206999,21.223857033803998,-17.196737341188499,0.81064233290015697,-26.273290751085099,-14.322488269703999,0,0]
["CP-E1L211C4","CP",6,"E1L211C4",200,"CM(Y), OPR Expense, Railroad-Owned, FLAT - TOFC",3.8185205310583101E-2,4.0139820426702499E-2,3.3290147781372098E-2,2.3514449596405002E-2,4.2433128692209703E-3,8.2680361811071602E-4,0,0,0,0,0,0,0,0,0,0]
["CP-E1L211C5","CP",6,"E1L211C5",201,"CM(Y), DRL Expense, Railroad-Owned, FLAT - TOFC",8.9144773781299605E-2,0.10019489377736999,8.5692234337329906E-2,8.6673185229301494E-2,7.2301082313060802E-2,8.4363557398319203E-2,7.9381436109542805E-2,7.1246899664401994E-2,8.5644587874412495E-2,5.8999890015995898E-2,0.101307231860675,0.13237787149231001,0.13499152282448701,0.14926983520700701,0.11179582240967199,0.110676670894322]
["CP-E1L211C9","CP",6,"E1L211C9",205,"CD(R), ROI Expense, Railroad-Owned, FLAT - TOFC",-4.8466797918081297E-2,-0.154585361480713,0.72762382030487105,0.74959564208984397,3.1376969069242498E-2,2.9308008030056999E-2,2.1331835538148901E-2,-0.101565204560757,5.5466961860656703,4.82250324058539,0,0,0,0,0,0]
["CP-E1L211C12","CP",6,"E1L211C12",208,"CD(Y), ROI Expense, Railroad-Owned, FLAT - TOFC",-4.8466805368661901E-2,-0.154585376381874,0.72762376070022605,0.74959570169448897,3.1376969069242498E-2,2.9308008030056999E-2,2.1331831812858599E-2,-0.101565212011337,5.5466961860656703,4.82250324058539,0,0,0,0,0,0]
["CP-E1L212C3","CP",6,"E1L212C3",212,"CM(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",0.123173408210278,0.14053121209144601,0.18728218972683,0.23385986685752899,0.15817497670650499,0.21928985416889199,0.268363237380981,0.425419121980667,0.41230803728103599,0.48083794656601703,0.59681120966387502,0.68424974803299199,0.63479787059608195,0.58093622654520805,0.55885855302614895,0.706950790851544]
["CP-E1L212C6","CP",6,"E1L212C6",215,"CM(Y), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",0.32025030255317699,0.36538103222847002,0.48693472146987898,0.60803550481796298,0.41125458478927601,0.57015317678451505,0.69774395227432295,1.1060889959335301,1.0720015764236499,1.2501786610716501,1.55170914512608,1.77904934488578,1.6504744635498101,1.5104341890175399,1.4530322378679901,1.83807205621402]
["CP-E1L212C9","CP",6,"E1L212C9",218,"CD(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",37.400569915771499,37.646240234375,46.9936332702637,61.663017272949197,39.157249450683601,35.958213806152301,46.699943542480497,80.913612365722699,72.466148376464801,86.575397243137601,97.835097067439605,106.500200282805,94.566418847861996,91.747290561533404,86.069314291764101,110.62286754620401]
["CP-E1L212C10","CP",6,"E1L212C10",219,"CD(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",24.287143707275401,28.1719856262207,39.917396545410199,56.491592407226598,53.2752494812012,35.724098205566399,22.441480636596701,27.481487274169901,24.2153720855713,34.645005186361097,29.600614954972801,32.736349067435903,19.280119392808999,11.627074324617199,7.87223245430524,8.5564872005704995]
["CP-E1L213C3","CP",6,"E1L213C3",225,"CM(R), ROI Expense, Railroad-Owned, FLAT - GENERAL",-4.1314181871712199E-3,-1.06141762807965E-2,4.8424981650896398E-4,-2.9718242585659001E-3,2.70294025540352E-3,6.5132803283631802E-3,4.8970915377140002E-3,5.9567685239017001E-3,9.5595733728259802E-4,7.0194158939677204E-4,0,0,0,0,0,0]
["CP-E1L213C5","CP",6,"E1L213C5",227,"CM(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",0.29774588346481301,0.33287855982780501,0.25925874710083002,0.33159455657005299,-0.16947618126869199,0.17820838093757599,0.20547673106193501,0.19877378642559099,0.221901655197144,0.29867537519300502,0.291367602500199,0.27953633952847101,0.26606055847447602,0.34199916214201398,0.25364996848590399,0.25606050791753199]
["CP-E1L213C8","CP",6,"E1L213C8",230,"CD(R), DRL Expense, Railroad-Owned, FLAT - GENERAL",15.497163772583001,21.8752841949463,15.071312904357899,27.961198806762699,-12.782590866088899,34.901493072509801,32.822574615478501,26.649995803833001,27.307624816894499,32.170193498031097,30.882242368693301,28.3069572731787,23.505576119517901,28.1364929217347,22.4837318836788,17.382946772787101]
["CP-E1L213C11","CP",6,"E1L213C11",233,"CD(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",15.4971628189087,21.8752841949463,15.071311950683601,27.961198806762699,-12.782588958740201,34.9014892578125,32.822578430175803,26.649997711181602,27.307622909545898,32.170193498031203,30.882242368693301,28.3069572731787,23.505576119517901,28.1364929217347,22.4837318836788,17.382946772787101]
["CP-E1L214C2","CP",6,"E1L214C2",237,"CM(R), DRL Expense, Railroad-Owned, FLAT - OTHER",-0.10290228575468099,-0.101562589406967,-0.10773724317550699,-6.8599820137023898E-2,-4.3156020343303701E-2,-7.6109975576400798E-2,-7.0707581937313094E-2,-5.56939207017422E-2,-8.1922248005867004E-2,-8.2147173136406307E-2,-7.3964322090955104E-2,-8.5140523783929306E-2,-8.0320449089927706E-2,-8.2858262283471595E-2,-0.107073855717548,-9.3118282233152105E-2]
["CP-E1L214C5","CP",6,"E1L214C5",240,"CM(Y), DRL Expense, Railroad-Owned, FLAT - OTHER",-0.26754561066627502,-0.264062941074371,-0.28011640906333901,-0.17835971713066101,-0.112205758690834,-0.19788585603237199,-0.183839872479439,-0.14480423927307101,-0.21299798786640201,-0.213582650154656,-0.19230723743648301,-0.22136536183821601,-0.20883316763381199,-0.21543148193702599,-0.27839202486562398,-0.24210753380619501]
["CP-E1L214C8","CP",6,"E1L214C8",243,"CD(R), DRL Expense, Railroad-Owned, FLAT - OTHER",16.8021564483643,9.8822050094604492,1.5822393894195601,9.9224729537963903,12.601489067077599,10.972484588623001,6.3230328559875497,3.2091717720031698,-3.149569272995,-1.56729902736559,-1.0590454202772901,-2.5926609528520101,0.68814523400536998,-6.09308127432055,-8.7565376302574407,-8.5091766448377903]
["CP-E1L214C11","CP",6,"E1L214C11",246,"CD(Y), DRL Expense, Railroad-Owned, FLAT - OTHER",16.802152633666999,9.8822088241577095,1.5822393894195601,9.9224777221679705,12.601487159729,10.972484588623001,6.3230352401733398,3.2091758251190199,-3.1495714187622101,-1.56729902736559,-1.0590454202772901,-2.5926609528520199,0.68814523400536998,-6.09308127432055,-8.7565376302574407,-8.5091766448377903]
["CP-E1L214C13","CP",6,"E1L214C13",248,"CM(R), DRL Expense, Privately-Owned, FLAT - OTHER",9.4108968973159804E-2,0.12164840847253799,0.163715749979019,0.26566228270530701,0.26030302047729498,0.25927656888961798,0.21890924870967901,0.17049923539161699,0.25761172175407399,0.26700892539889898,0.29998742675860202,0.30327670318262001,0.30426186990062198,0.38373980774472799,0.39140126784245799,0.36273890062394298]
["CP-E1L215C4","CP",6,"E1L215C4",252,"CM(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L215C7","CP",6,"E1L215C7",255,"CD(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L215C10","CP",6,"E1L215C10",258,"CD(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L216C1","CP",6,"E1L216C1",262,"CM(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L216C4","CP",6,"E1L216C4",265,"CM(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L216C7","CP",6,"E1L216C7",268,"CD(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L216C10","CP",6,"E1L216C10",271,"CD(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L216C12","CP",6,"E1L216C12",273,"CD(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E1L217C3","CP",6,"E1L217C3",277,"CM(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-2.11848150938749E-2,-4.88625839352608E-2,-2.0703591406345399E-2,2.58730258792639E-3,3.9631146937608702E-3,4.7675822861492599E-3,3.3857717644423199E-3,0,0,0,0,0,0,0,9.9805413209296495E-6,1.2027338162592201E-5]
["CP-E1L217C6","CP",6,"E1L217C6",280,"CM(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-5.5080585181713097E-2,-0.12704290449619299,-5.38293421268463E-2,6.7269932478666297E-3,1.0304116643965199E-2,1.2395683676004399E-2,8.8029969483614003E-3,0,0,0,0,0,0,0,2.5949407434417102E-5,3.1271079222739601E-5]
["CP-E1L217C9","CP",6,"E1L217C9",283,"CD(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-6.5421514511108398,-14.907193183898899,-7.4343223571777299,0.53985607624053999,0.93004006147384599,1.0790044069290201,0.78180718421936002,0,0,0,0,0,0,0,2.42603141061664E-3,2.8570346406515401E-3]
["CP-E1L217C13","CP",6,"E1L217C13",287,"CM(R), DRL Expense, Privately-Owned, ALL OTHER FREIGHT CARS",2.62569133192301E-2,1.05352401733398E-2,6.4964555203914599E-3,8.3498518506530699E-5,2.0253703405614899E-4,0.58393031358718905,9.5382994040846807E-3,1.12817017361522E-2,7.3358290828764404E-3,0,2.7272776629487598E-4,0,0,0,3.6406961096743698E-5,0]
["CP-E1L218C3","CP",6,"E1L218C3",290,"CM(R), ROI Expense, Railroad-Owned, AUTO RACKS",0.12162522971630101,0.13860365748405501,0.151786938309669,0.162470042705536,0.112955011427402,0.18046055734157601,0.23163615167141,0.37977480888366699,0.40928566455841098,0.47762496635420498,0.50033010933815103,0.57539924092390105,0.52191022377887497,0.49715855202488102,0.48386913559692901,0.61245758273438999]
["CP-E1L218C4","CP",6,"E1L218C4",291,"CM(Y), OPR Expense, Railroad-Owned, AUTO RACKS",9.74776446819305E-2,0.104971744120121,0.14389431476593001,0.31972599029540999,0.28713521361351002,0.18927510082721699,0,0,0,0,0,0,0,0,0,0]
["CP-E1L218C9","CP",6,"E1L218C9",296,"CD(R), ROI Expense, Railroad-Owned, AUTO RACKS",37.083961486816399,37.297714233398402,38.2317085266113,42.884799957275398,28.051948547363299,29.6408996582031,40.3844184875488,72.352859497070298,72.109039306640597,86.187036495557194,82.083066055594401,89.6722470579477,77.815065383691305,78.554888605526301,74.546917392830196,95.873616943197902]
["CP-E1L218C11","CP",6,"E1L218C11",298,"CD(Y), DRL Expense, Railroad-Owned, AUTO RACKS",177.86163330078099,170.07640075683599,149.24205017089801,191.90106201171901,123.86416625976599,68.261001586914105,59.755775451660199,53.512111663818402,42.880382537841797,39.401002465568098,-14.954285807358801,-32.581247499678803,-19.998008067639901,-21.5082311865159,-31.0695512201189,-27.7184030732707]
["CP-E1L219C2","CP",6,"E1L219C2",302,"CM(R), DRL Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,1.0421731921894699E-8,1.2257229009549101E-8,1.6014521794595299E-8,0,0,0,0,0,0]
["CP-E1L219C5","CP",6,"E1L219C5",305,"CM(Y), DRL Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,2.7096474397580999E-8,3.1868822247815803E-8,4.1637756665947799E-8,0,0,0,0,0,0]
["CP-E1L219C8","CP",6,"E1L219C8",308,"CD(R), DRL Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,1.2503332982305399E-6,1.37502445340942E-6,1.9705589502682801E-6,0,0,0,0,0,0]
["CP-E1L219C12","CP",6,"E1L219C12",312,"CD(Y), ROI Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,4.81559573017876E-6,4.5164974835643096E-6,5.6071130866731001E-6,0,0,0,0,0,0]
["CP-E1L220C2","CP",6,"E1L220C2",315,"CM(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",-3.9413563907146502E-2,-3.9451327174901997E-2,-3.3252477645874003E-2,-2.4331994354724901E-2,-1.16141103208065E-2,-1.93687360733747E-2,-2.0605882629752201E-2,-2.6941187679767602E-2,-5.6242663413286202E-2,-4.3786174820989801E-2,-5.3005671237185199E-2,-5.2282677454963802E-2,-5.02577614758139E-2,-5.5805246120168801E-2,-8.9473860627226995E-2,-8.0177090010088506E-2]
["CP-E1L220C4","CP",6,"E1L220C4",317,"CM(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",0.188205480575562,0.141216039657593,0.14335323870182001,0.186822488903999,0.13743069767951999,0.13617442548274999,0.158447876572609,0.15231429040432001,0.16234740614891099,0.226623087361006,0.26240122052086201,0.29660130610594299,0.31128738274227002,0.28779963240741102,0.27825173336638798,0.23196382017599201]
["CP-E1L220C7","CP",6,"E1L220C7",320,"CD(R), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",4.6669640541076696,5.0839948654174796,5.9457221031189,7.0704846382141104,4.2312111854553196,4.6869444847106898,6.4765548706054696,5.8989229202270499,4.8944602012634304,8.82670095622451,10.9420205964138,10.5423665539594,8.9618740515557693,9.8206627476178507,9.7116106019777693,7.2852914572562097]
["CP-E1L220C10","CP",6,"E1L220C10",323,"CD(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",6.30885982513428,5.3862113952636701,5.9041891098022496,6.9214558601379403,5.1118588447570801,5.1550130844116202,6.1292138099670401,6.0943961143493697,6.5704517364501998,9.1362633663117396,10.046659437468399,11.247989094629199,11.287267086878201,10.6788240228846,10.011062593977201,8.3927919858632904]
["CP-E1L221C1","CP",6,"E1L221C1",327,"CM(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.15104445815086401,0.16639611124992401,0.21667577326297799,0.32074153423309298,0.31324744224548301,0.25941914319992099,0.18082737922668499,0.23173953592777299,0.200886875391006,0.283724660139688,0.25564485972762402,0.29344054410561199,0.18477603945256799,0.112284875869927,7.62904830405947E-2,8.1622927493338895E-2]
["CP-E1L221C4","CP",6,"E1L221C4",330,"CM(Y), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.39271491765976002,0.43263018131256098,0.56335687637329102,0.83392858505249001,0.81444394588470503,0.67448931932449296,0.470150947570801,0.60252308845519997,0.52230626344680797,0.73768411636318698,0.66467663529182097,0.76294541467459098,0.48041770257667599,0.29194067726181,0.19835525590554601,0.21221961148268101]
["CP-E1L221C7","CP",6,"E1L221C7",333,"CD(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",24.287143707275401,28.1719856262207,39.917392730712898,56.491584777832003,53.275245666503899,35.724094390869098,22.441478729248001,27.4814853668213,24.215370178222699,34.645005186361097,29.600614954972801,32.736349067435903,19.280119392808999,11.627074324617199,7.87223245430524,8.5564872005704995]
["CP-E1L221C11","CP",6,"E1L221C11",337,"CD(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",87.654396057128906,96.463882446289105,138.22393798828099,201.31623840332,81.760948181152301,45.062576293945298,33.550205230712898,32.092979431152301,-17.841873168945298,75.892607562885999,48.206908043597601,29.430243780700401,41.070404110013897,27.6921430234311,12.918030185826799,19.807797558745701]
["CP-E1L301C1","CP",6,"E1L301C1",340,"L&D Expense, FARM PRODUCTS",6.0479726642370203E-2,4.3492771685123402E-2,5.2238646894693402E-2,5.0968628376722301E-2,3.09725925326347E-2,5.8702994138002403E-2,3.9931595325469998E-2,4.0919195860624299E-2,5.5300697684287997E-2,4.0740445742439298E-2,3.0235172829172E-2,4.2640386857255498E-2,3.0764167073179E-2,3.9305223656339899E-2,2.3084220232348799E-2,3.2991514790269003E-2]
["CP-E1L303C1","CP",6,"E1L303C1",342,"L&D Expense, POTATOES OTHER THAN SWEET",3.6799578666686998,3.1860339641571001,1.57116758823395,2.0286219120025599,0.46845808625221302,0.59124863147735596,0.76070266962051403,0.51356053352356001,1.9531569480896001,2.51130048867766,2.4820239734348402,1.5628554724856101,1.5738487949622999,4.7855950282905102,2.6763798404894299,1.6733272275745501]
["CP-E1L306C1","CP",6,"E1L306C1",345,"L&D Expense, ALL OTHER FARM PRODUCTS",8.7879635393619496E-2,4.6295948326587698E-2,4.7562893480062499E-2,5.8936458081006997E-2,3.3297318965196603E-2,3.8297187536954901E-2,5.1949910819530501E-2,3.9584696292877197E-2,5.1575444638729102E-2,9.5663520052149797E-3,1.65227324418049E-2,3.6049529086921397E-2,3.7162508897451797E-2,4.2500157114610498E-2,5.3477487289282401E-3,4.7120247326328697E-2]
["CP-E1L309C1","CP",6,"E1L309C1",348,"L&D Expense, NONMETALLIC MINERALS",6.1751324683427802E-3,6.0367635451257203E-3,6.24764291569591E-3,1.1238164268434001E-2,1.2882996350526799E-2,1.0773151181638199E-2,1.14579824730754E-2,5.6324019096791701E-3,5.2316985093057199E-3,7.1841635102270198E-3,1.9460853891206499E-3,2.9566385317463602E-3,2.6945083219701502E-3,3.9923515321203399E-3,1.2879584932098101E-3,2.5697714472261999E-3]
["CP-E1L313C1","CP",6,"E1L313C1",352,"L&D Expense, CANNED FRUITS/VEG",0.61201786994934104,0.45836937427520802,0.54955309629440297,0.46772405505180398,0.268973708152771,0.44812881946563698,0.364413142204285,0.32465270161628701,0.30047565698623702,0.54309701066336802,0.60036280662191399,0.59926710243978698,0.57379621654754098,0.79501823483980005,0.40052818960853498,0.33041247966923698]
["CP-E1L316C1","CP",6,"E1L316C1",355,"L&D Expense, PREPARED FEEDS",3.4461708273738601E-3,5.2915900945663501E-2,8.3416014909744304E-2,6.4005493186414198E-3,6.4121750183403501E-3,1.0765590704977499E-3,1.48906651884317E-2,1.21511137112975E-2,5.0596832297742401E-3,3.2849257204589803E-2,1.38959473594921E-2,6.32190753961661E-3,2.7778759021351199E-2,1.08453877778599E-3,2.5196986440421701E-5,1.02066313274846E-3]
[{"$f":"B2306&\"-\"&D2306","v":"CP-E1L320C1"},"CP",6,"E1L320C1",359,"L&D Expense, CORN PRODUCTS",1.34091908112168E-2,3.9376903325319297E-2,4.7181513160467099E-2,2.6431472972035401E-2,2.73294728249311E-2,3.8074269890785203E-2,3.7078451365232502E-2,1.75428669899702E-2,2.01527439057827E-2,4.1817161674595404E-3,1.34790764147741E-2,4.3508653131181197E-3,9.0233417435583996E-3,3.9086462228574504E-3,3.02978423330987E-5,2.0180023840311999E-2]
["CP-E1L323C1","CP",6,"E1L323C1",362,"L&D Expense, WINES",0.84492164850234996,8.3208911120891599E-2,1.34687983989716,0.44220030307769798,0.205625951290131,6.3485205173492404E-2,0.24367405474185899,0.51581692695617698,0.34035617113113398,1.35427260144433,0.24422654004494099,0.105158524452878,0.36028833717952002,0.267506679227699,0.16329456182654101,0.12703334188972801]
["CP-E1L326C1","CP",6,"E1L326C1",365,"L&D Expense, ALL OTHER FOOD PRODUCTS",9.1888576745986897E-2,7.9573296010494204E-2,0.12117470800876599,6.5014228224754306E-2,3.6592349410057103E-2,4.3420534580946003E-2,0.141043856739998,5.3964279592037201E-2,5.3006786853075E-2,7.9923448269122996E-2,9.9097557048061696E-2,8.1842532444312499E-2,0.19285248625642101,0.17873068167745801,0.111427994915152,8.3245180810300995E-2]
["CP-E1L328C1","CP",6,"E1L328C1",367,"L&D Expense, LUMBER AND WOOD EX FURNITURE",6.4082108438014998E-2,6.3597209751606001E-2,4.2465981096029302E-2,5.5317327380180401E-2,2.6106728240847601E-2,4.5685745775699602E-2,2.36855149269104E-2,3.1761787831783302E-2,2.2764811292290701E-2,5.5634208764431099E-2,6.8785233747138505E-2,4.2106313382289699E-2,5.85751816640947E-2,5.6718723912763502E-2,5.8628574900259398E-2,0.141446267912923]
["CP-E1L331C1","CP",6,"E1L331C1",370,"L&D Expense, ALL OTHER LUMBER AND WOOD PRODUCTS",5.6283235549926799E-2,6.4753077924251598E-2,2.6934949681162799E-2,5.1356635987758602E-2,1.97196342051029E-2,1.67441107332706E-2,2.6319015771150599E-2,2.49072927981615E-2,2.19722930341959E-2,3.42567023876479E-2,4.1458401381328898E-2,2.14436371930571E-2,1.7770680455502699E-2,7.2241755483112693E-2,4.1882590552649701E-2,9.6173132143614795E-2]
["CP-E1L334C1","CP",6,"E1L334C1",373,"L&D Expense, NEWSPRINT",0.386345565319061,0.26457613706588701,0.24139791727066001,0.40231353044509899,0.33147549629211398,0.257203638553619,0.141914248466492,8.8899778202176094E-3,0.17850668728351601,0.192825144881663,9.4011005829416405E-2,0.20472030566705901,3.1076594371090002E-2,1.2324784383151699,2.51977665787704E-2,0.16148795459672499]
["CP-E1L338C1","CP",6,"E1L338C1",377,"L&D Expense, SANITARY TISSUES",0.122947245836258,3.0709726270288199E-3,6.65031932294369E-3,6.80103600025177E-2,1.2522803619503999E-2,0,0.10232835263013799,1.07538355514407E-2,9.4120344147086091E-3,2.9207028751322198E-2,1.1900797086969101E-3,1.39013832183855E-2,0,5.0166042535151603E-3,1.23663771402875E-3,4.3280785841464898E-3]
["CP-E1L341C1","CP",6,"E1L341C1",380,"L&D Expense, INDUSTRIAL CHEMICALS",8.7614255025982891E-3,1.6192162409424799E-2,8.6116092279553396E-3,8.3545334637165104E-3,7.8697837889194506E-3,2.1585958078503598E-2,2.21712626516819E-2,1.10827656462789E-2,7.03930715098977E-3,7.1057580517135304E-3,1.15099133183999E-2,1.2581535809645E-2,1.27504083238833E-2,8.6896402574811304E-3,1.4742717925468E-2,1.0810643549472299E-2]
["CP-E1L345C1","CP",6,"E1L345C1",384,"L&D Expense, ALL OTHER CHEMICALS",2.6043361052870799E-2,0.102892324328423,5.1314171403646497E-2,5.8835830539464999E-2,4.2031995952129399E-2,1.8057033419609101E-2,2.5860302150249499E-2,7.7346088364720301E-3,2.08973791450262E-2,2.2599386791942899E-2,5.1338501809845997E-2,4.6916238257755201E-4,7.0031947197344305E-2,9.0754973556344501E-2,0.11058293551930599,1.91782433824856E-2]
["CP-E1L348C1","CP",6,"E1L348C1",387,"L&D Expense, RUBBER TIRES/INNER TUBES",0.134509116411209,8.9131239801645296E-3,1.7789637669920901E-2,4.3709573219530301E-4,6.3215277623385202E-4,0.12824502587318401,0.20823356509208699,0.172246068716049,0.101569473743439,5.1709465437767201E-2,4.1918087269156301E-3,3.8097494457809397E-2,6.2541206245703999E-3,5.4441562535281901E-2,7.61084379992156E-2,9.8839377049493804E-2]
["CP-E1L351C1","CP",6,"E1L351C1",390,"L&D Expense, FLAT GLASS",7.9960972070693997E-2,0,0,4.9382718279957797E-3,0,0,0,0,0.24076983332634,7.4834149668299293E-2,0,0,0,2.46638667305578E-3,0,1.26070110068464E-2]
["CP-E1L353C1","CP",6,"E1L353C1",392,"L&D Expense, ALL OTHER STONE & CLAY, GLASS PRODUCTS",2.3819899186492001E-2,2.95029655098915E-2,1.7426427453756301E-2,1.5901990234851799E-2,9.0113366022705997E-3,1.7641941085457798E-2,1.0626674629747901E-2,8.8174836710095406E-3,1.7466975376009899E-2,1.6213023466090899E-2,8.0123522222395605E-3,7.0282422645380101E-3,8.5392018813610897E-3,1.00639728338627E-2,1.8205648733177902E-2,8.8792988187615506E-3]
["CP-E1L356C1","CP",6,"E1L356C1",395,"L&D Expense, ALUMINUM BASIC SHAPES",0.11286199837923,0.15163244307041199,0.19129206240177199,0.99977880716323897,9.2738665640354198E-2,0.365030497312546,0.13654950261116,0.40275806188583402,4.6725824475288398E-2,0.427446876899923,7.1842447765894907E-2,6.1801981514728398E-2,2.36256029762279E-4,0.97019829399741397,1.4380682533099101,1.67692641734201]
["CP-E1L360C1","CP",6,"E1L360C1",399,"L&D Expense, ALL OTHER FAB METAL PRODUCTS",8.2236602902412401E-2,4.22826893627644E-2,0.12317106872797,0.57348483800888095,0.11085592955350899,0.104633316397667,0.104206696152687,0.41068261861801098,2.90865134447813E-2,2.6793860444710701E-2,1.17116840125649E-2,6.1026978151819303E-2,8.3779653724611707E-3,1.9695008077359299E-2,2.3129155730127701E-3,8.2394414457267903E-2]
["CP-E1L363C1","CP",6,"E1L363C1",402,"L&D Expense, FARM MACHINERY",2.4298570156097399,1.5298203229904199,1.5081578493118299,2.9845852851867698,1.5362756252288801,0.99220669269561801,0.70848298072814897,1.0776067972183201,0.70382529497146595,1.3448171672090701,0.559861487070207,0.61976011384427698,0.13272710665462301,0.15808913426766,0,0.16933120027486401]
["CP-E1L366C1","CP",6,"E1L366C1",405,"L&D Expense, ELECTRICAL MACHINERY",0.67479163408279397,0.47035461664199801,0.76611125469207797,0.65651184320449796,0.56727981567382801,0.21725417673587799,0.49147397279739402,0.91961038112640403,0.289804667234421,0.44987594767502198,0.21864727922893701,0.110947990600422,0.399700701714716,0.218458461333112,0.13409182722392801,1.67087861140951]
["CP-E1L370C1","CP",6,"E1L370C1",409,"L&D Expense, ALL OTHER ELECTRICAL MACHINERY",0.72443789243698098,0.124912194907665,1.22650158405304,2.0479607582092298,1.4720858335495,2.7940336614847201E-2,2.5568239390850098E-2,0.79280191659927401,0.32959437370300299,0.11638569092668601,0.15527288252874599,0.20274542735457399,3.8295146556108502E-2,0.100668737420884,0.10349523579893,6.5650136035665803]
["CP-E1L373C1","CP",6,"E1L373C1",412,"L&D Expense, MOTOR TRUCKS",2.1043250560760498,1.26811671257019,1.65900325775146,1.4032484292984,0.97844052314758301,0.82795894145965598,2.6402244567871098,2.5844602584838898,5.3508419990539604,2.3972440890440101,2.5053101151001802,3.01905989333518,4.5072670290018699,1.8358317475753301,1.9620481392513101,6.0876948799235704]
["CP-E1L374C1","CP",6,"E1L374C1",413,"L&D Expense, MOTOR VECHICLE PARTS",0.17642442882060999,0.27078187465667702,0.25748610496521002,0.82535320520401001,0.14550699293613401,0.17560070753097501,0.17617671191692399,0.84027493000030495,0.21214038133621199,8.8219921107315594E-2,0.393716560465393,0.212999234670077,0.10576437246174999,0.119489105755487,4.6983042073175697E-3,5.2852034619368202E-2]
["CP-E1L378C1","CP",6,"E1L378C1",417,"L&D Expense, MISC MIXED SHIPMENTS",9.1315463185310405E-2,0.11395051330328,0.119482338428497,7.6815418899059296E-2,6.5753631293773707E-2,4.5803453773260103E-2,6.1025261878967299E-2,5.9127628803253202E-2,6.1889201402664198E-2,4.37200018110191E-2,7.5652365651906694E-2,3.3229987868641203E-2,3.2905317083349601E-2,3.0981519923329901E-2,4.4879455499843499E-2,4.5587054201045099E-2]
["CP-E1L381C1","CP",6,"E1L381C1",420,"L&D Expense, HAZARDOUS MATERIALS",3.3822157420218E-3,4.38846610486507E-2,6.9866083562374101E-2,4.1437070816755302E-2,3.1556442379951498E-2,2.9638551175594299E-2,1.43746230751276E-2,2.3880230262875599E-2,1.29652125760913E-2,2.8145488342284499E-2,1.9073883682287199E-2,6.4705703700832298E-3,1.8164087945304101E-2,3.0475595834185201E-2,1.6340194747313699E-2,2.5929638549913699E-2]
["CP-E2L101C3","CP",6,"E2L101C3",424,"E/L Ratio, Privately-Owned, BOX - 40 FT",1.6759002208709699,1.95982146263123,2.1115384101867698,2.4152743816375701,1.91719079017639,1.7722960710525499,1.8104650974273699,1.8970588445663501,2.03125,1.9746543778801799,1.6541554959785501,1.5442176870748301,1.43170320404722,1.7974025974026,1.94907407407407,1.9153846153846199]
["CP-E2L101C6","CP",6,"E2L101C6",427,"Interline circuity, BOX - 40 FT",1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001]
["CP-E2L101C9","CP",6,"E2L101C9",430,"CD per Industry Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L101C13","CP",6,"E2L101C13",434,"CD per I&I Switch, BOX - 40 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L101C16","CP",6,"E2L101C16",437,"CD per Load & Unload Interterminal Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L101C17","CP",6,"E2L101C17",438,"CM per Industry Switch, BOX - 40 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L101C21","CP",6,"E2L101C21",442,"CM per I&I Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L101C24","CP",6,"E2L101C24",445,"Average Miles between Interchange Switches, BOX - 40 FT",594.31976318359398,534.13171386718795,603.97314453125,401.86297607421898,637.82598876953102,448.30361938476602,410.40206909179699,521.88690185546898,483.64074707031301,407.35321017011199,229.85216992832201,152.09950022070001,243.19644650367599,78.629526253676303,89.254953855280107,160.90359492484501]
["CP-E2L101C28","CP",6,"E2L101C28",449,"SEMs per Interterminal Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CP-E2L102C2","CP",6,"E2L102C2",452,"E/L Ratio, Railroad-Owned, BOX - 50 FT",2.1127517223358199,2.1869487762451199,2.1227622032165501,2.3567838668823198,2.02344822883606,2.0106222629547101,2.11349701881409,2.0907781124114999,2.0571429729461701,1.9648033126294,1.98863636363636,2.02877697841727,1.3682310469314101,2.0201465201465201,2.0147849462365599,1.98168103448276]
["CP-E2L102C5","CP",6,"E2L102C5",455,"Local circuity, BOX - 50 FT",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["CP-E2L102C9","CP",6,"E2L102C9",459,"CD per Industry Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L102C12","CP",6,"E2L102C12",462,"CD per Interterminal Switch, BOX - 50 FT",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CP-E2L102C13","CP",6,"E2L102C13",463,"CD per I&I Switch, BOX - 50 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L102C17","CP",6,"E2L102C17",467,"CM per Industry Switch, BOX - 50 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L102C20","CP",6,"E2L102C20",470,"CM per Interterminal Switch, BOX - 50 FT",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CP-E2L102C24","CP",6,"E2L102C24",474,"Average Miles between Interchange Switches, BOX - 50 FT",594.31976318359398,534.13171386718795,603.97314453125,401.86297607421898,637.82598876953102,448.30361938476602,410.40206909179699,521.88690185546898,483.64074707031301,407.35321017011199,229.85216992832201,152.09950022070001,243.19644650367599,78.629526253676303,89.254953855280107,160.90359492484501]
["CP-E2L102C27","CP",6,"E2L102C27",477,"SEMs per Intraterminal Switch, BOX - 50 FT",26.226448059081999,20.023302078247099,19.610774993896499,19.980493545532202,21.7528476715088,14.531662940979,13.5956773757935,11.731157302856399,9.9727468490600604,9.6316500136580601,8.2884512091815807,6.9020239983878504,6.4731011049627396,6.0054973395416296,5.4028905546403996,5.0176931416353003]
["CP-E2L103C1","CP",6,"E2L103C1",480,"Average Tare Weight, BOX - EQUIPPED",36.099998474121101,36.099998474121101,36.200000762939503,36.099998474121101,36.200000762939503,36.200000762939503,36.400001525878899,36.5,36.5,36.5,36.6,36.700000000000003,36.799999999999997,37,37.1,37.299999999999997]
["CP-E2L103C5","CP",6,"E2L103C5",484,"Local circuity, BOX - EQUIPPED",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["CP-E2L103C9","CP",6,"E2L103C9",488,"CD per Industry Switch, BOX - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L103C10","CP",6,"E2L103C10",489,"CD per Interchange Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L103C13","CP",6,"E2L103C13",492,"CD per I&I Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L103C16","CP",6,"E2L103C16",495,"CD per Load & Unload Interterminal Switch, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L103C20","CP",6,"E2L103C20",499,"CM per Interterminal Switch, BOX - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CP-E2L103C23","CP",6,"E2L103C23",502,"Average Miles between I&I Switches, BOX - EQUIPPED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CP-E2L103C27","CP",6,"E2L103C27",506,"SEMs per Intraterminal Switch, BOX - EQUIPPED",26.226448059081999,20.023302078247099,19.610776901245099,19.980491638183601,21.752849578857401,14.5316610336304,13.5956773757935,11.731158256530801,9.9727478027343803,9.6316500136580601,8.2884512091815807,6.9020239983878504,6.4731011049627396,6.0054973395416296,5.4028905546403996,5.0176931416353003]
["CP-E2L104C1","CP",6,"E2L104C1",509,"Average Tare Weight, GONDOLA - PLAIN",26,25.899999618530298,25.799999237060501,25.600000381469702,25.5,25.600000381469702,25.299999237060501,25.700000762939499,25.700000762939499,25.6,25.6,25.6,25.7,25.9,26.1,26.3]
["CP-E2L104C5","CP",6,"E2L104C5",513,"Local circuity, GONDOLA - PLAIN",1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.093,1.093,1.093,1.093,1.093,1.093,1.093]
["CP-E2L104C6","CP",6,"E2L104C6",514,"Interline circuity, GONDOLA - PLAIN",1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.151,1.151,1.151,1.151,1.151,1.151,1.151]
["CP-E2L104C9","CP",6,"E2L104C9",517,"CD per Industry Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L104C12","CP",6,"E2L104C12",520,"CD per Interterminal Switch, GONDOLA - PLAIN",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CP-E2L104C16","CP",6,"E2L104C16",524,"CD per Load & Unload Interterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L104C19","CP",6,"E2L104C19",527,"CM per Intraterminal Switch, GONDOLA - PLAIN",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CP-E2L104C23","CP",6,"E2L104C23",531,"Average Miles between I&I Switches, GONDOLA - PLAIN",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CP-E2L104C26","CP",6,"E2L104C26",534,"SEMs per Interchange Switch, GONDOLA - PLAIN",9.6163663864135707,7.3418779373168901,7.1906180381774902,7.3261818885803196,7.9760451316833496,5.3282766342163104,4.9850816726684597,4.3014249801635698,3.6566741466522199,3.5316050050079499,3.0390987766999098,2.5307421327422102,2.3734704051529998,2.20201569116526,1.9810598700348101,1.8398208185996101]
["CP-E2L105C1","CP",6,"E2L105C1",538,"Average Tare Weight, GONDOLA - EQUIPPED",33.099998474121101,33.200000762939503,33.400001525878899,33.299999237060497,33.299999237060497,33.299999237060497,33.299999237060497,33.099998474121101,33.099998474121101,33.200000000000003,33.200000000000003,33.1,33.1,33.1,33.1,33.1]
["CP-E2L105C2","CP",6,"E2L105C2",539,"E/L Ratio, Railroad-Owned, GONDOLA - EQUIPPED",1.9566074609756501,2.04234766960144,2.0773510932922399,2.24675321578979,2.0434732437133798,2.0268356800079301,2.1120688915252699,2.01145315170288,1.9841434955596899,2.19126147568854,2.1416978776529301,1.99652551574376,1.9632271005125901,2.0573111944295701,1.9908452853219401,1.91940201494963]
["CP-E2L105C5","CP",6,"E2L105C5",542,"Local circuity, GONDOLA - EQUIPPED",1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001]
["CP-E2L105C8","CP",6,"E2L105C8",545,"Spotted-to-Pulled Ratio, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L105C12","CP",6,"E2L105C12",549,"CD per Interterminal Switch, GONDOLA - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CP-E2L105C15","CP",6,"E2L105C15",552,"CD per Load & Unload Intraterminal Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L105C19","CP",6,"E2L105C19",556,"CM per Intraterminal Switch, GONDOLA - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CP-E2L105C22","CP",6,"E2L105C22",559,"Average CM per CD, Railroad-Owned, GONDOLA - EQUIPPED",794.16223144531295,704.79345703125,662.05419921875,708.21771240234398,572.548095703125,552.27032470703102,658.933349609375,697.05426025390602,501.30459594726602,679.54669551331597,701.72396178223403,716.35840094921502,607.54568750537396,736.13795584933098,763.82806884259105,713.16588025175702]
["CP-E2L105C26","CP",6,"E2L105C26",563,"SEMs per Interchange Switch, GONDOLA - EQUIPPED",9.6163663864135707,7.3418779373168901,7.1906175613403303,7.3261814117431596,7.9760446548461896,5.3282761573791504,4.9850811958312997,4.3014249801635698,3.6566741466522199,3.5316050050079499,3.0390987766999098,2.5307421327422102,2.3734704051529998,2.20201569116526,1.9810598700348101,1.8398208185996101]
["CP-E2L105C27","CP",6,"E2L105C27",564,"SEMs per Intraterminal Switch, GONDOLA - EQUIPPED",26.2264518737793,20.023302078247099,19.610774993896499,19.980493545532202,21.7528476715088,14.531662940979,13.5956764221191,11.731158256530801,9.9727468490600604,9.6316500136580601,8.2884512091815807,6.9020239983878504,6.4731011049627396,6.0054973395416296,5.4028905546403996,5.0176931416353003]
["CP-E2L106C1","CP",6,"E2L106C1",567,"Average Tare Weight, HOPPER - COVERED",31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.200000762939499,31.100000381469702,31,30.8,30.8,30.8,30.8,30.8,30.8,30.9]
["CP-E2L106C5","CP",6,"E2L106C5",571,"Local circuity, HOPPER - COVERED",1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999]
["CP-E2L106C8","CP",6,"E2L106C8",574,"Spotted-to-Pulled Ratio, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L106C11","CP",6,"E2L106C11",577,"CD per Intraterminal Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L106C15","CP",6,"E2L106C15",581,"CD per Load & Unload Intraterminal Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L106C18","CP",6,"E2L106C18",584,"CM per Interchange Switch, HOPPER - COVERED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CP-E2L106C22","CP",6,"E2L106C22",588,"Average CM per CD, Railroad-Owned, HOPPER - COVERED",794.16223144531295,704.79339599609398,662.05426025390602,708.21771240234398,572.548095703125,552.27032470703102,658.933349609375,697.05432128906295,501.30462646484398,679.54669551331597,701.72396178223403,716.35840094921502,607.54568750537396,736.13795584933098,763.82806884259105,713.16588025175702]
["CP-E2L106C23","CP",6,"E2L106C23",589,"Average Miles between I&I Switches, HOPPER - COVERED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CP-E2L106C26","CP",6,"E2L106C26",592,"SEMs per Interchange Switch, HOPPER - COVERED",9.6163654327392596,7.3418779373168901,7.1906185150146502,7.3261814117431596,7.9760451316833496,5.3282761573791504,4.9850816726684597,4.3014249801635698,3.6566741466522199,3.5316050050079499,3.0390987766999098,2.5307421327422102,2.3734704051529998,2.20201569116526,1.9810598700348101,1.8398208185996101]
["CP-E2L107C1","CP",6,"E2L107C1",596,"Average Tare Weight, HOPPER - OPEN TOP - GENERAL",29.799999237060501,29.700000762939499,29.600000381469702,29.600000381469702,29.5,29.600000381469702,29.399999618530298,29.200000762939499,29,28.9,28.8,28.8,28.7,28.5,28.4,28.3]
["CP-E2L107C4","CP",6,"E2L107C4",599,"E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - GENERAL",1.7360970973968499,1.4951541423797601,1.56308305263519,1.55395066738129,1.97724044322968,2.1020920276641801,2.1233141422271702,2.1058659553527801,2.08714079856873,2.0558631102164102,2.1244813278008299,2.0047125353440101,2.0706976744186001,2.0271186440678002,2.00648648648649,2.0209973753280801]
["CP-E2L107C7","CP",6,"E2L107C7",602,"Average circuity, HOPPER - OPEN TOP - GENERAL",1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001]
["CP-E2L107C11","CP",6,"E2L107C11",606,"CD per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L107C14","CP",6,"E2L107C14",609,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L107C18","CP",6,"E2L107C18",613,"CM per Interchange Switch, HOPPER - OPEN TOP - GENERAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CP-E2L107C19","CP",6,"E2L107C19",614,"CM per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CP-E2L107C22","CP",6,"E2L107C22",617,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",794.16217041015602,704.79339599609398,662.05426025390602,708.21771240234398,572.548095703125,552.27032470703102,658.933349609375,697.05426025390602,501.30465698242199,679.54669551331597,701.72396178223403,716.35840094921502,607.54568750537396,736.13795584933098,763.82806884259105,713.16588025175702]
["CP-E2L107C26","CP",6,"E2L107C26",621,"SEMs per Interchange Switch, HOPPER - OPEN TOP - GENERAL",9.6163663864135707,7.3418774604797399,7.1906180381774902,7.3261809349060103,7.9760460853576696,5.3282766342163104,4.9850821495056197,4.3014249801635698,3.6566739082336399,3.5316050050079499,3.0390987766999098,2.5307421327422102,2.3734704051529998,2.20201569116526,1.9810598700348101,1.8398208185996101]
["CP-E2L107C29","CP",6,"E2L107C29",624,"SEMs per I&I Switch, HOPPER - OPEN TOP - GENERAL",4.3710746765136701,3.3372170925140399,3.2684626579284699,3.3300821781158398,3.6254746913909899,2.4219439029693599,2.2659461498260498,1.9551931619644201,1.6621242761611901,1.60527500227634,1.3814085348636,1.15033733306464,1.0788501841604601,1.00091622325694,0.900481759106734,0.83628219027255102]
["CP-E2L108C3","CP",6,"E2L108C3",627,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - SPECIAL",2.2264151573181201,2.1666667461395299,2.0512821674346902,1.5505514144897501,1.54850745201111,1.99435245990753,2.02602982521057,2.0458571910858199,2.00971484184265,2.0202387130254298,2.0111524163568801,1.9552599758161999,2.00416666666667,1.90133037694013,1.91036088474971,1.92580101180438]
["CP-E2L108C7","CP",6,"E2L108C7",631,"Average circuity, HOPPER - OPEN TOP - SPECIAL",1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001]
["CP-E2L108C10","CP",6,"E2L108C10",634,"CD per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L108C12","CP",6,"E2L108C12",636,"CD per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CP-E2L108C15","CP",6,"E2L108C15",639,"CD per Load & Unload Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L108C18","CP",6,"E2L108C18",642,"CM per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CP-E2L108C22","CP",6,"E2L108C22",646,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",794.16217041015602,704.79339599609398,662.05419921875,708.21771240234398,572.548095703125,552.27032470703102,658.933349609375,697.05432128906295,501.30459594726602,679.54669551331597,701.72396178223403,716.35840094921502,607.54568750537396,736.13795584933098,763.82806884259105,713.16588025175702]
["CP-E2L108C25","CP",6,"E2L108C25",649,"SEMs per Industry Switch, HOPPER - OPEN TOP - SPECIAL",17.484300613403299,13.3488683700562,13.073850631713899,13.320329666137701,14.5019016265869,0,0,0,0,0,0,0,0,0,0,0]
["CP-E2L108C28","CP",6,"E2L108C28",652,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",20.981159210205099,16.018642425537099,15.6886205673218,15.9843969345093,17.402280807495099,0,0,0,0,0,0,0,0,0,0,0]
["CP-E2L109C3","CP",6,"E2L109C3",656,"E/L Ratio, Privately-Owned, REFRIGERATED - MECH",1.9805942773819001,1.95194387435913,1.97031545639038,1.98218262195587,1.9963190555572501,2.0748341083526598,2.07808136940002,2.2697074413299601,2.1645162105560298,1.98141637368157,1.97759376522163,1.98440792246102,1.96367346938776,1.9823321554770299,2.06570004531038,2.0249400479616302]
["CP-E2L109C6","CP",6,"E2L109C6",659,"Interline circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["CP-E2L109C8","CP",6,"E2L109C8",661,"Spotted-to-Pulled Ratio, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L109C11","CP",6,"E2L109C11",664,"CD per Intraterminal Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L109C14","CP",6,"E2L109C14",667,"CD per Load & Unload Industry Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L109C18","CP",6,"E2L109C18",671,"CM per Interchange Switch, REFRIGERATED - MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CP-E2L109C21","CP",6,"E2L109C21",674,"CM per I&I Switch, REFRIGERATED - MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L109C25","CP",6,"E2L109C25",678,"SEMs per Industry Switch, REFRIGERATED - MECH",17.484300613403299,13.3488674163818,13.073850631713899,13.320329666137701,14.501899719238301,9.6877746582031303,9.0637855529785192,7.8207716941833496,6.64849805831909,6.4211000091053698,5.5256341394543904,4.6013493322585699,4.3154007366418199,4.0036648930277501,3.6019270364269298,3.3451287610902001]
["CP-E2L109C27","CP",6,"E2L109C27",680,"SEMs per Intraterminal Switch, REFRIGERATED - MECH",26.2264499664307,20.0233039855957,19.610774993896499,19.980495452880898,21.7528476715088,14.531662940979,13.5956773757935,11.731158256530801,9.9727468490600604,9.6316500136580601,8.2884512091815807,6.9020239983878504,6.4731011049627396,6.0054973395416296,5.4028905546403996,5.0176931416353003]
["CP-E2L110C3","CP",6,"E2L110C3",685,"E/L Ratio, Privately-Owned, REFRIGERATED - NON-MECH",2.03345727920532,2.9700000286102299,2.20652174949646,2,1.9579287767410301,1.8351647853851301,2.4141790866851802,2.1428570747375502,2.2125000953674299,2.4,2.5,2.75,2,2,2.01223491027732,3]
["CP-E2L110C4","CP",6,"E2L110C4",686,"E/L Ratio, All Freight Cars, REFRIGERATED - NON-MECH",1.9620418548584,1.9754098653793299,1.9423729181289699,2.04065036773682,2.1836345195770299,2.1006224155425999,2.1223628520965598,1.98916971683502,1.9791122674942001,2.3454545454545501,2.0619469026548698,2.1298701298701301,2.12,2.75,0,3]
["CP-E2L110C7","CP",6,"E2L110C7",689,"Average circuity, REFRIGERATED - NON-MECH",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["CP-E2L110C10","CP",6,"E2L110C10",692,"CD per Interchange Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L110C14","CP",6,"E2L110C14",696,"CD per Load & Unload Industry Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L110C17","CP",6,"E2L110C17",699,"CM per Industry Switch, REFRIGERATED - NON-MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L110C21","CP",6,"E2L110C21",703,"CM per I&I Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L110C23","CP",6,"E2L110C23",705,"Average Miles between I&I Switches, REFRIGERATED - NON-MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CP-E2L110C28","CP",6,"E2L110C28",710,"SEMs per Interterminal Switch, REFRIGERATED - NON-MECH",20.9811611175537,16.0186443328857,15.688621520996101,15.984395980835,17.402280807495099,11.6253318786621,10.8765411376953,9.3849267959594709,7.9781985282897896,7.7053200109264504,6.6307609673452603,5.5216191987102796,5.1784808839701899,4.8043978716332996,0,0]
["CP-E2L110C29","CP",6,"E2L110C29",711,"SEMs per I&I Switch, REFRIGERATED - NON-MECH",4.3710746765136701,3.3372170925140399,3.2684626579284699,3.3300824165344198,3.6254744529724099,2.4219439029693599,2.2659463882446298,1.9551930427551301,1.6621243953704801,1.60527500227634,1.3814085348636,1.15033733306464,1.0788501841604601,1.00091622325694,0,0.83628219027255102]
["CP-E2L111C3","CP",6,"E2L111C3",714,"E/L Ratio, Privately-Owned, FLAT - TOFC",1.0601658821105999,1.06015729904175,1.06980800628662,1.0971833467483501,1.0754857063293499,1.0737544298171999,1.078373670578,1.05547058582306,1.0535135269164999,1.0716666666666701,1.0500285225328001,1.0293299131234399,1.0295638980206401,1.04110320284698,1.0607970027247999,1.05286198067234]
["CP-E2L111C6","CP",6,"E2L111C6",717,"Interline circuity, FLAT - TOFC",1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.107,1.107,1.107,1.107,1.107,1.107,1.107]
["CP-E2L111C10","CP",6,"E2L111C10",721,"CD per Interchange Switch, FLAT - TOFC",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L111C13","CP",6,"E2L111C13",724,"CD per I&I Switch, FLAT - TOFC",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L111C17","CP",6,"E2L111C17",728,"CM per Industry Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L111C19","CP",6,"E2L111C19",730,"CM per Intraterminal Switch, FLAT - TOFC",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CP-E2L111C24","CP",6,"E2L111C24",735,"Average Miles between Interchange Switches, FLAT - TOFC",1508645.5,1859082,351737.0625,1683159.875,8886982,4336879.5,11920114,0,3193478,10712802.8026626,37177574.920758203,41449866.779702097,7126925.9705609996,22821750.6039306,5959498.4641300198,7146461.3716684096]
["CP-E2L111C25","CP",6,"E2L111C25",736,"SEMs per Industry Switch, FLAT - TOFC",17.484300613403299,13.3488674163818,13.073850631713899,13.320329666137701,14.501899719238301,9.6877746582031303,9.0637845993041992,0,6.64849805831909,6.4211000091053698,5.5256341394543904,4.6013493322585699,4.3154007366418199,4.0036648930277501,3.6019270364269298,3.3451287610902001]
["CP-E2L111C28","CP",6,"E2L111C28",739,"SEMs per Interterminal Switch, FLAT - TOFC",20.981159210205099,16.018642425537099,15.6886205673218,15.9843969345093,17.402278900146499,11.625332832336399,10.8765420913696,0,7.9781980514526403,7.7053200109264504,6.6307609673452603,5.5216191987102796,5.1784808839701899,4.8043978716332996,4.3223124437123204,4.0141545133082399]
[{"$f":"B2690&\"-\"&D2690","v":"CP-E2L112C3"},"CP",6,"E2L112C3",743,"E/L Ratio, Privately-Owned, FLAT - MULTILEVEL",1.32952880859375,1.2699838876724201,1.3201117515564,1.3977843523025499,1.3699413537979099,1.40323209762573,1.5690602064132699,1.3916417360305799,1.45977234840393,1.63536886692552,1.58579291640077,1.7257800418448099,1.69622140427713,1.57089924469146,1.5552082282948501,1.3945501378281899]
["CP-E2L112C6","CP",6,"E2L112C6",746,"Interline circuity, FLAT - MULTILEVEL",1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999]
["CP-E2L112C9","CP",6,"E2L112C9",749,"CD per Industry Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L112C11","CP",6,"E2L112C11",751,"CD per Intraterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L112C17","CP",6,"E2L112C17",757,"CM per Industry Switch, FLAT - MULTILEVEL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L112C20","CP",6,"E2L112C20",760,"CM per Interterminal Switch, FLAT - MULTILEVEL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CP-E2L112C21","CP",6,"E2L112C21",761,"CM per I&I Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L112C24","CP",6,"E2L112C24",764,"Average Miles between Interchange Switches, FLAT - MULTILEVEL",5741.9033203125,4112.20654296875,3714.91650390625,4119.89599609375,4067.03955078125,776.22412109375,701.32781982421898,830.5673828125,818.19281005859398,722.14676253869902,540.63871594245404,396.273946274921,483.082550895618,657.39336455605803,582.93633998194298,627.88541821062802]
["CP-E2L112C28","CP",6,"E2L112C28",768,"SEMs per Interterminal Switch, FLAT - MULTILEVEL",20.9811611175537,16.018642425537099,15.6886205673218,15.984398841857899,17.402278900146499,11.6253309249878,10.8765420913696,9.3849277496337908,7.9781985282897896,7.7053200109264504,6.6307609673452603,5.5216191987102796,5.1784808839701899,4.8043978716332996,4.3223124437123204,4.0141545133082399]
["CP-E2L113C2","CP",6,"E2L113C2",771,"E/L Ratio, Railroad-Owned, FLAT - GENERAL",2.2631578445434601,2.1428570747375502,2.65957450866699,3,2.4166667461395299,2.4545454978942902,2.4333333969116202,2.6956522464752202,2.5803570747375502,2.4950495049504999,2.5520833333333299,3.1549295774647899,2.2325581395348801,2.7362637362637399,2.1967213114754101,2.1153846153846199]
["CP-E2L113C5","CP",6,"E2L113C5",774,"Local circuity, FLAT - GENERAL",1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001]
["CP-E2L113C7","CP",6,"E2L113C7",776,"Average circuity, FLAT - GENERAL",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["CP-E2L113C13","CP",6,"E2L113C13",782,"CD per I&I Switch, FLAT - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L113C16","CP",6,"E2L113C16",785,"CD per Load & Unload Interterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L113C17","CP",6,"E2L113C17",786,"CM per Industry Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L113C20","CP",6,"E2L113C20",789,"CM per Interterminal Switch, FLAT - GENERAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CP-E2L113C24","CP",6,"E2L113C24",793,"Average Miles between Interchange Switches, FLAT - GENERAL",453.44128417968801,346.23464965820301,84.542053222656307,437.88818359375,1375.28967285156,3681.3994140625,1135.13513183594,1416.66662597656,513.39288330078102,482.54259939859702,512.31673490952301,218.24104234527701,519.99466808851002,670.09425878320496,396.56533754441398,264.25243143509402]
["CP-E2L113C27","CP",6,"E2L113C27",796,"SEMs per Intraterminal Switch, FLAT - GENERAL",26.2264518737793,20.0233039855957,19.610773086547901,19.980493545532202,21.7528476715088,14.531663894653301,13.5956773757935,11.731159210205099,9.9727468490600604,9.6316500136580601,8.2884512091815807,6.9020239983878504,6.4731011049627396,6.0054973395416296,5.4028905546403996,5.0176931416353003]
["CP-E2L114C1","CP",6,"E2L114C1",799,"Average Tare Weight, FLAT - OTHER",34.599998474121101,34.599998474121101,34.700000762939503,34.700000762939503,34.700000762939503,34.700000762939503,35.099998474121101,35.200000762939503,35.200000762939503,35.299999999999997,35.299999999999997,35.299999999999997,35.4,35.299999999999997,35.4,35.4]
["CP-E2L114C3","CP",6,"E2L114C3",801,"E/L Ratio, Privately-Owned, FLAT - OTHER",1.96803545951843,1.8138242959976201,1.89014327526093,1.6978739500045801,1.92610323429108,1.8529250621795701,2.01574802398682,1.8531625270843499,1.8507330417633101,1.9592944369063801,1.9016959798994999,1.9744565217391301,2.0442477876106202,2.09179869524697,2.0707232452628799,2.06301229508197]
[{"$f":"B2754&\"-\"&D2754","v":"CP-E2L114C9"},"CP",6,"E2L114C9",807,"CD per Industry Switch, FLAT - OTHER",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L114C10","CP",6,"E2L114C10",808,"CD per Interchange Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L114C13","CP",6,"E2L114C13",811,"CD per I&I Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CP-E2L114C16","CP",6,"E2L114C16",814,"CD per Load & Unload Interterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L114C20","CP",6,"E2L114C20",818,"CM per Interterminal Switch, FLAT - OTHER",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CP-E2L114C23","CP",6,"E2L114C23",821,"Average Miles between I&I Switches, FLAT - OTHER",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CP-E2L114C26","CP",6,"E2L114C26",824,"SEMs per Interchange Switch, FLAT - OTHER",9.6163663864135707,7.3418779373168901,7.1906185150146502,7.3261818885803196,7.9760451316833496,5.3282766342163104,4.9850816726684597,4.3014254570007298,3.6566739082336399,3.5316050050079499,3.0390987766999098,2.5307421327422102,2.3734704051529998,2.20201569116526,1.9810598700348101,1.8398208185996101]
["CP-E2L114C28","CP",6,"E2L114C28",826,"SEMs per Interterminal Switch, FLAT - OTHER",20.981159210205099,16.018642425537099,15.688621520996101,15.9843969345093,17.402280807495099,11.6253318786621,10.8765420913696,9.3849277496337908,7.9781985282897896,7.7053200109264504,6.6307609673452603,5.5216191987102796,5.1784808839701899,4.8043978716332996,4.3223124437123204,4.0141545133082399]
["CP-E2L115C5","CP",6,"E2L115C5",832,"Local circuity, TANK <22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["CP-E2L115C6","CP",6,"E2L115C6",833,"Interline circuity, TANK <22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["CP-E2L115C9","CP",6,"E2L115C9",836,"CD per Industry Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CP-E2L115C12","CP",6,"E2L115C12",839,"CD per Interterminal Switch, TANK <22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CP-E2L115C16","CP",6,"E2L115C16",843,"CD per Load & Unload Interterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L115C19","CP",6,"E2L115C19",846,"CM per Intraterminal Switch, TANK <22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CP-E2L115C24","CP",6,"E2L115C24",851,"Average Miles between Interchange Switches, TANK <22,000 GAL",101986.0625,182420.625,199143.5625,210475.84375,1561124.25,459.48693847656301,403.26596069335898,401.96896362304699,377.63934326171898,551.22543442767699,488.69864339857997,422.32971349055703,445.85456819885502,355.27388329756701,429.582213119443,416.54966932937498]
["CP-E2L115C27","CP",6,"E2L115C27",854,"SEMs per Intraterminal Switch, TANK <22,000 GAL",26.2264499664307,20.0233039855957,19.610774993896499,19.980493545532202,21.752849578857401,14.531662940979,13.5956773757935,11.731158256530801,9.9727468490600604,9.6316500136580601,8.2884512091815807,6.9020239983878504,6.4731011049627396,6.0054973395416296,5.4028905546403996,5.0176931416353003]
["CP-E2L116C1","CP",6,"E2L116C1",857,"Average Tare Weight, TANK >=22,000 GAL",38.9,39.200000000000003,38.9,38.9,39,38.9,38.9,39.1,39.5,40.1,40.4,40.700000000000003,41,41.4,41.7,41.9]
["CP-E2L116C2","CP",6,"E2L116C2",858,"E/L Ratio, Railroad-Owned, TANK >=22,000 GAL",1.70715832710266,2.38509321212769,2.1198978424072301,2.3008849620819101,2.1308410167694101,2.0604982376098602,2.15936255455017,2.4518072605133101,2.1798942089080802,2.6967741935483902,2.6842105263157898,3,2.5087719298245599,2.89230769230769,3.1458333333333299,2.4090909090909101]
["CP-E2L116C5","CP",6,"E2L116C5",861,"Local circuity, TANK >=22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["CP-E2L116C8","CP",6,"E2L116C8",864,"Spotted-to-Pulled Ratio, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L116C12","CP",6,"E2L116C12",868,"CD per Interterminal Switch, TANK >=22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
[{"$f":"B2818&\"-\"&D2818","v":"CP-E2L116C15"},"CP",6,"E2L116C15",871,"CD per Load & Unload Intraterminal Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L116C20","CP",6,"E2L116C20",876,"CM per Interterminal Switch, TANK >=22,000 GAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CP-E2L116C23","CP",6,"E2L116C23",879,"Average Miles between I&I Switches, TANK >=22,000 GAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CP-E2L116C26","CP",6,"E2L116C26",882,"SEMs per Interchange Switch, TANK >=22,000 GAL",9.6163654327392596,7.3418779373168901,7.1906180381774902,7.3261818885803196,7.9760451316833496,5.3282761573791504,4.9850821495056197,4.3014249801635698,3.6566739082336399,3.5316050050079602,3.0390987766999098,2.5307421327422102,2.3734704051529998,2.20201569116526,1.9810598700348101,1.8398208185996101]
["CP-E2L116C27","CP",6,"E2L116C27",883,"SEMs per Intraterminal Switch, TANK >=22,000 GAL",26.2264499664307,20.0233039855957,19.610774993896499,19.980493545532202,21.752849578857401,14.531662940979,13.5956773757935,11.731158256530801,9.9727468490600604,9.6316500136580601,8.2884512091815807,6.9020239983878504,6.4731011049627396,6.0054973395416296,5.4028905546403996,5.0176931416353003]
["CP-E2L117C1","CP",6,"E2L117C1",886,"Average Tare Weight, ALL OTHER FREIGHT CARS",36.799999237060497,39.200000762939503,36.5,36.599998474121101,36.700000762939503,36.599998474121101,36.799999237060497,37.099998474121101,37.5,38.1,38.4,38.6,38.9,39.299999999999997,39.6,39.799999999999997]
["CP-E2L117C4","CP",6,"E2L117C4",889,"E/L Ratio, All Freight Cars, ALL OTHER FREIGHT CAR",2.0145115852356001,1.9891719818115201,1.97410333156586,1.98173391819,2.0044467449188201,2.02124691009521,2.00268602371216,2.1058266162872301,2.1201436519622798,2.0117429881498201,2.0030935173017999,2.0017368021131099,1.98818637850418,2.0044828602567701,1.9966145102441799,1.99211591732367]
["CP-E2L117C8","CP",6,"E2L117C8",893,"Spotted-to-Pulled Ratio, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L117C11","CP",6,"E2L117C11",896,"CD per Intraterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L117C16","CP",6,"E2L117C16",901,"CD per Load & Unload Interterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CP-E2L117C19","CP",6,"E2L117C19",904,"CM per Intraterminal Switch, ALL OTHER FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CP-E2L117C22","CP",6,"E2L117C22",907,"Average CM per CD, Railroad-Owned, ALL OTHER FREIGHT CARS",794.16223144531295,704.79339599609398,662.05426025390602,708.21771240234398,572.548095703125,552.27032470703102,658.933349609375,697.05426025390602,501.30465698242199,679.54669551331597,701.72396178223403,716.35840094921502,607.54568750537499,736.13795584933098,763.82806884259105,713.16588025175702]
["CP-E2L117C23","CP",6,"E2L117C23",908,"Average Miles between I&I Switches, ALL OTHER FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CP-E2L117C26","CP",6,"E2L117C26",911,"SEMs per Interchange Switch, ALL OTHER FREIGHT CARS",9.6163654327392596,7.3418779373168901,7.1906180381774902,7.3261818885803196,7.9760451316833496,5.3282761573791504,4.9850821495056197,4.3014249801635698,3.6566739082336399,3.5316050050079602,3.0390987766999098,2.5307421327422102,2.3734704051529998,2.20201569116526,1.9810598700348101,1.8398208185996101]
["CP-E2L118C1","CP",6,"E2L118C1",915,"Average Tare Weight, AVERAGE ALL FREIGHT CARS",34.400001525878899,34.400001525878899,34.299999237060497,34.299999237060497,34.299999237060497,34.299999237060497,34.200000762939503,34.299999237060497,34.400001525878899,34.6,34.799999999999997,34.799999999999997,34.9,35.200000000000003,35.299999999999997,35.4]
["CP-E2L118C4","CP",6,"E2L118C4",918,"E/L Ratio, All Freight Cars, AVERAGE ALL FREIGHT CARS",1.7178049087524401,1.6941720247268699,1.7167621850967401,1.7386442422866799,1.7921164035797099,1.79960441589355,1.8368233442306501,1.88795101642609,1.8777377605438199,1.86456681640807,1.8243464725054901,1.83162016882696,1.8283786260634001,1.8423320009878299,1.8335379199030499,1.8372266154091299]
["CP-E2L118C8","CP",6,"E2L118C8",922,"Spotted-to-Pulled Ratio, AVERAGE ALL FREIGHT CARS",1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.9,1.9,1.9,1.9,1.9,1.9,1.9]
["CP-E2L118C12","CP",6,"E2L118C12",926,"CD per Interterminal Switch, AVERAGE ALL FREIGHT CARS",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CP-E2L118C15","CP",6,"E2L118C15",929,"CD per Load & Unload Intraterminal Switch, AVERAGE ALL FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CP-E2L118C18","CP",6,"E2L118C18",932,"CM per Interchange Switch, AVERAGE ALL FREIGHT CAR",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CP-E2L118C19","CP",6,"E2L118C19",933,"CM per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CP-E2L118C22","CP",6,"E2L118C22",936,"Average CM per CD, Railroad-Owned, AVERAGE ALL FREIGHT CARS",794.16223144531295,704.79345703125,662.05426025390602,708.21771240234398,572.548095703125,552.27032470703102,658.933349609375,697.05432128906295,501.30462646484398,679.54669551331597,701.72396178223403,716.35840094921502,607.54568750537396,736.13795584933098,763.82806884259105,713.16588025175702]
["CP-E2L118C26","CP",6,"E2L118C26",940,"SEMs per Interchange Switch, AVERAGE ALL FREIGHT CARS",9.6163644790649396,7.3418779373168901,7.1906185150146502,7.3261818885803196,7.9760451316833496,5.3282756805419904,4.9850821495056197,4.3014245033264196,3.6566739082336399,3.5316050050079499,3.0390987766999098,2.5307421327422102,2.3734704051529998,2.20201569116526,1.9810598700348101,1.8398208185996101]
["CP-E2L118C29","CP",6,"E2L118C29",943,"SEMs per I&I Switch, AVERAGE ALL FREIGHT CARS",4.3710746765136701,3.3372170925140399,3.2684626579284699,3.3300824165344198,3.6254746913909899,2.4219439029693599,2.2659461498260498,1.9551931619644201,1.6621243953704801,1.60527500227634,1.3814085348636,1.15033733306464,1.0788501841604601,1.00091622325694,0.900481759106733,0.83628219027255102]
["CP-E2L204C1","CP",6,"E2L204C1",947,"Average Tare Weight - Non-Refrigerated TCU",5,5,5,4.9000000953674299,4.9000000953674299,4.9000000953674299,4.9000000953674299,5,5,5,4.9000000000000004,4.7,4.9000000000000004,4.9000000000000004,4.8,4.8]
["CP-E2L208C1","CP",6,"E2L208C1",951,"Average Locomotive Units - Unit Train",1.9679303169250499,2.07448434829712,2.07189989089966,2.1593587398529102,2.3530569076538099,2.4013445377349898,2.3489573001861599,2.24843525886536,2.2014224529266402,2.4388451815626002,2.48548708876671,2.2476257576302601,2.3454581298583399,2.2590952929812498,2.179072095495,2.2763811541554801]
["CP-E2L211C1","CP",6,"E2L211C1",954,"Average Gross Tons - Unit Train",7887.6083984375,8617.5107421875,8763.943359375,8652.744140625,8071.1708984375,7734.63232421875,7624.345703125,7591.265625,8238.70703125,8282.8578995863008,9093.8521131485195,8983.9425178856309,9747.9289054532401,9403.1429261383801,9658.7839064648506,10023.817250575001]
["CP-E2L212C1","CP",6,"E2L212C1",955,"Average Gross Tons - Way Train",1856.54016113281,1795.58557128906,1645.35607910156,2033.15173339844,1856.11853027344,1794.89196777344,1753.02136230469,2245.9462890625,3148.88818359375,3532.4486712770599,3817.1722789329201,3861.58055816347,4228.2672770034897,3280.7366501574002,3464.7247964159201,4044.6278006899302]
["CP-E2L215C1","CP",6,"E2L215C1",958,"Train Crews (Excl Train Switching)",20550.4453125,18669.15234375,19867.595703125,16594.83203125,32524.8046875,42013.62109375,38613.24609375,34705.46484375,40141.375,39127.110065507601,26880.068800791501,30445.075328757099,38179.626675662497,38089.501773767101,27007.5040934192,29527.395700607001]
["CP-E2L218C1","CP",6,"E2L218C1",961,"Average Crew Wages (Assigned To TM-Crew)",4.9501380920410201,4.8070836067199698,5.4241809844970703,5.1871018409729004,5.6775574684143102,6.9482049942016602,6.5420861244201696,6.0360307693481401,7.7216796875,8.4041459717393092,8.3908870660134696,8.7054334247154603,9.4857468734890595,9.1909841535704206,8.1760552675255393,8.9600113130650207]
["CP-E2L301C2","CP",6,"E2L301C2",965,"Residual Factor, Industry Switching, Privately-Owned",37.801302263265498,27.687771938270501,30.143657099970898,36.006309526621202,45.504111668752202,31.266062169781598,36.930159898163502,25.329353741429347,33.507538965830399,33.571514149187102,30.894518745114599,34.268259245785899,41.445092507235302,44.256160742330302,38.776267717413873,30.201239387420401]
["CP-E2L303C1","CP",6,"E2L303C1",968,"Residual Factor, Interchange Switching, Railroad-Owned",7.7414136570118499,5.9053923195994402,5.9700357304152396,7.9719716174207402,15.1161161421938,14.969579087062099,18.363612746259399,10.240291638581972,10.5121326304427,10.111424740472399,9.1169330124515895,10.1595896849076,11.333934523543901,8.3380123175634893,6.6911279105846333,6.1893316465796797]
["CP-E2L305C1","CP",6,"E2L305C1",972,"Residual Factor, Mileage, Railroad-Owned",-2.0759069329684099,-2.9284863669458301,-2.5707423700798602,-3.48437498748785,-0.63023414601510797,-0.52943879505047697,1.4588638432447301,4.1390544486310663,3.1416633015266,-2.8797933486022398,-5.7510136814769899,-9.1570292047222406,-15.7358635556206,-6.11786723804431,-5.5209570939094856,-7.2625595311815596]
["CSXT-E1L101C3","CSXT",3,"E1L101C3",3,"Gross Ton Mile (GTM), ROI Expense",1.53397466056049E-3,1.92356610205024E-3,2.1516219712793801E-3,2.2436215076595501E-3,2.1877738181501601E-3,2.3441433440893901E-3,2.3444110993295899E-3,2.4474845267832301E-3,2.2103912197053402E-3,2.2708393490987501E-3,2.3382644114845401E-3,2.72162852397392E-3,3.2756065007348901E-3,2.6140928716678999E-3,2.4344121664023502E-3,3.1496314344912099E-3]
["CSXT-E1L102C3","CSXT",3,"E1L102C3",6,"Car Mile (CM) - Other Than Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L103C1","CSXT",3,"E1L103C1",7,"Train Mile (TM) - Other Than Crew, OPR Expense",0.667716205120087,0.755532026290894,0.671375691890717,0.74740248918533303,0.77305936813354503,0.73541390895843495,0.74300372600555398,0.78907793760299705,0.849778532981873,0.93743564987508698,0.91691162815141303,0.84366800871225101,0.89085646067678104,0.86323112017937698,0.91875626093412999,0.89937343843585105]
["CSXT-E1L104C1","CSXT",3,"E1L104C1",10,"Train Mile (TM) - Crew, OPR Expense",7.7999839782714799,7.8036117553710902,7.8502445220947301,8.6934099197387695,8.6892051696777308,8.4880962371826207,8.4018449783325195,8.48968505859375,9.4926691055297905,11.2587816820859,11.4860708918262,10.781512699494399,10.405593367631999,10.7980250067077,11.2107363096244,11.2768702395985]
["CSXT-E1L105C1","CSXT",3,"E1L105C1",13,"Locomotive Unit Mile (LUM), OPR Expense",4.3358473777770996,5.0367064476013201,6.6226711273193404,4.50347805023193,5.4916901588439897,6.7196855545043901,6.6861166954040501,6.7958068847656303,6.74066162109375,4.8852508510492596,4.3666826813024402,5.1452339232537696,5.87757389125691,6.2663645285053704,4.7802631706392802,6.72338923181126]
["CSXT-E1L106C2","CSXT",3,"E1L106C2",17,"CLOR (Carloads Handled) - Other, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L107C2","CSXT",3,"E1L107C2",20,"CLOR (Carloads Handled) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L108C3","CSXT",3,"E1L108C3",24,"CLOT (Carloads Orig Or Term) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L110C1","CSXT",3,"E1L110C1",28,"Car Mile (CM) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L111C1","CSXT",3,"E1L111C1",31,"Switch Engine Minutes (SEM), OPR Expense",4.6547985076904297,4.0039348602294904,4.0997447967529297,3.80589079856873,4.0369939804077104,4.1657671928405797,4.2998642921447798,4.2100529670715297,4.3225145339965803,4.2162609497478796,3.8838836965757202,4.0698144170059001,4.1719402594209596,4.0738468736205498,4.0856784806370099,4.3172180277406396]
["CSXT-E1L111C2","CSXT",3,"E1L111C2",32,"Switch Engine Minutes (SEM), DRL Expense",0.36206150054931602,0.31266731023788502,0.338023781776428,0.43591091036796598,0.43800413608550998,0.42576926946639998,0.46599462628364602,0.47763782739639299,0.47401800751686102,0.48473260209636998,0.540039206535053,0.55155896126951898,0.65444457138167,0.76269925090076995,0.78242538110511906,0.72123452423572698]
["CSXT-E1L112C2","CSXT",3,"E1L112C2",35,"Ton Miles In Lake Transfer Service, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L113C2","CSXT",3,"E1L113C2",38,"Tons Handled at Coal Terminals, DRL Expense",0.13256028294563299,9.0477995574474293E-2,8.6520001292228699E-2,0.139605388045311,0.13993327319622001,0.111873395740986,7.6256096363067599E-2,8.17299485206604E-2,8.1310369074344593E-2,0.13225628655837099,0.139575822067661,0.15479098450030801,0.13611339605758599,0.16291231282830801,0.202959687922977,0.174865868593096]
["CSXT-E1L114C3","CSXT",3,"E1L114C3",42,"Tons Handled at Ore Terminals, ROI Expense",0.35153737664222701,0.434928238391876,0.59264057874679599,0.29925242066383401,0.371218472719193,0.33371841907501198,0.24079014360904699,0.203999012708664,0.138323783874512,0.15213519118920699,0.120922046959115,3.8596089559744299E-5,0,0,0,0]
["CSXT-E1L115C3","CSXT",3,"E1L115C3",45,"Tons Handled at Other Marine Terminals, ROI Expense",0.81985563039779696,0.52581351995468095,0.68187510967254605,0.74958926439285301,0.455452620983124,0.47291532158851601,1.5128298997878999,2.3642215728759801,6.20481300354004,14.3745610678441,0.22083147653951099,0.30462109939112297,0.40624600803732502,0.32736321815480002,0.31122307859833598,0.57187182744070397]
["CSXT-E1L117C2","CSXT",3,"E1L117C2",50,"Protective Service Reefer TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L118C2","CSXT",3,"E1L118C2",53,"Refrigerated TCU Days, DRL Expense",0,0,0,0,3.6736492067575503E-2,1.8970418022945499E-3,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L119C2","CSXT",3,"E1L119C2",56,"Other (Non-Refrigerated) TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L119C3","CSXT",3,"E1L119C3",57,"Other (Non-Refrigerated) TCU Days, ROI Expense",7.3991425335407299E-2,9.7246080636978094E-2,0.10226321965456001,9.3269459903240204E-2,8.8887266814708696E-2,8.5343405604362502E-2,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L120C3","CSXT",3,"E1L120C3",60,"TCUs Loaded And Unloaded (L&UL), ROI Expense",0.763233482837677,0.97329902648925803,1.0251537561416599,1.52150571346283,1.2880820035934399,1.2336076498031601,0.60678106546402,0.53169924020767201,0.43671882152557401,0.34492840279553,0.29509163104834302,0.33860308820690799,0.33431084257970101,0.24513181298560499,0.17307317691125501,0.19463182312911301]
["CSXT-E1L121C3","CSXT",3,"E1L121C3",63,"MVUs Loaded And Unloaded (L&UL), ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L201C1","CSXT",3,"E1L201C1",67,"CM(R), OPR Expense, Railroad-Owned, BOX - 40 FT",4.1952601168304698E-4,4.0757839451543998E-4,3.8914923788979698E-4,4.6507240040227798E-4,1.4225544873625001E-3,1.5205638483166699E-3,1.9360057776793801E-3,1.0344192851334799E-3,1.8921545706689399E-3,3.1275010955518498E-3,4.1459065181139098E-3,4.5256735405287598E-3,3.9434614681841404E-3,3.0471471478525402E-3,2.0306566134087102E-3,1.46017834503287E-3]
["CSXT-E1L201C4","CSXT",3,"E1L201C4",70,"CM(Y), OPR Expense, Railroad-Owned, BOX - 40 FT",1.09076732769608E-3,1.0597043437883299E-3,1.0117866331711401E-3,1.2091911630704999E-3,3.6986407358199401E-3,3.9534671232104301E-3,5.0336145795881696E-3,2.6894924230873602E-3,4.9196025356650396E-3,8.1315028484348004E-3,1.07793569470962E-2,1.1766751205374799E-2,1.02529998172787E-2,7.9225825844166098E-3,5.2797071948626597E-3,3.79646369708546E-3]
["CSXT-E1L201C9","CSXT",3,"E1L201C9",75,"CD(R), ROI Expense, Railroad-Owned, BOX - 40 FT",17.368688583373999,26.573501586914102,32.494094848632798,15.9998273849487,11.6895446777344,12.634325027465801,17.548591613769499,6.99806833267212,-7.1763247251510606E-2,0.22508509014804901,0.101778448644837,0.101814980177693,6.2718915356614002E-2,3.08941315136896E-2,2.1015475077363701E-2,1.64047538401756E-2]
["CSXT-E1L201C12","CSXT",3,"E1L201C12",78,"CD(Y), ROI Expense, Railroad-Owned, BOX - 40 FT",17.368686676025401,26.573501586914102,32.494094848632798,15.999831199646,11.689543724060099,12.634325027465801,17.548589706420898,6.9980673789978001,-7.1763254702091203E-2,0.22508509014804901,0.101778448644837,0.101814980177693,6.2718915356614002E-2,3.08941315136896E-2,2.1015475077363701E-2,1.64047538401756E-2]
["CSXT-E1L202C2","CSXT",3,"E1L202C2",81,"CM(R), DRL Expense, Railroad-Owned, BOX - 50 FT",0.17859320342540699,0.18583309650421101,0.197329431772232,6.7223109304904896E-2,6.9771744310855893E-2,5.57223670184612E-2,6.2153246253728901E-2,6.4334727823734297E-2,6.5188057720661205E-2,6.1788230235483299E-2,6.5122456687343594E-2,6.2272371896479703E-2,6.2225805451556301E-2,6.4562536921941804E-2,7.3342367144435594E-2,6.9652431440688195E-2]
["CSXT-E1L202C3","CSXT",3,"E1L202C3",82,"CM(R), ROI Expense, Railroad-Owned, BOX - 50 FT",9.4792082905769307E-2,0.14105446636676799,0.16630123555660201,7.8650340437889099E-2,5.8747455477714497E-2,6.4173094928264604E-2,8.8884472846984905E-2,3.5753890872001599E-2,-3.6736525362357503E-4,1.1580572894081601E-3,5.3208479657902805E-4,4.9182802727646595E-4,3.2050588015425098E-4,1.6423078620329601E-4,1.12693589424145E-4,8.6177813536216405E-5]
["CSXT-E1L202C6","CSXT",3,"E1L202C6",85,"CM(Y), ROI Expense, Railroad-Owned, BOX - 50 FT",0.24645973742008201,0.36674195528030401,0.432382702827454,0.20449107885360701,0.15274301171302801,0.166849941015244,0.23109945654869099,9.2959992587566403E-2,-9.5514854183420496E-4,3.01094895246121E-3,1.3834204711054799E-3,1.2787528709187999E-3,8.3331528840105396E-4,4.2700004412857002E-4,2.9300333250277598E-4,2.24062315194163E-4]
["CSXT-E1L202C9","CSXT",3,"E1L202C9",88,"CD(R), ROI Expense, Railroad-Owned, BOX - 50 FT",17.368688583373999,26.573501586914102,32.494094848632798,15.9998273849487,11.6895446777344,12.634325027465801,17.548591613769499,6.99806833267212,-7.1763247251510606E-2,0.22508509014804901,0.101778448644837,0.101814980177693,6.2718915356614002E-2,3.08941315136896E-2,2.1015475077363701E-2,1.64047538401756E-2]
["CSXT-E1L202C13","CSXT",3,"E1L202C13",92,"CM(R), DRL Expense, Privately-Owned, BOX - 50 FT",0.19232641160488101,0.45417258143424999,0.46134582161903398,0.71812909841537498,0.216695711016655,0.243293762207031,0.25977295637130698,0.26844891905784601,0.29895675182342502,0.28424138012929601,0.32956257605961897,0.30553618446150199,0.29031731748613998,0.30780711900736302,0.24837225917794301,0.30718625775104302]
["CSXT-E1L203C3","CSXT",3,"E1L203C3",95,"CM(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED",1.58081594854593E-2,1.9793659448623699E-2,2.7478884905576699E-2,3.1268879771232598E-2,3.2831404358148603E-2,3.5650268197059597E-2,3.8693290203809703E-2,3.70111577212811E-2,1.0876651853323E-2,3.8384136152675298E-3,1.13359423843503E-2,1.27710619573596E-2,1.2670964926107199E-2,1.27390611246029E-2,1.10271209767929E-2,1.2746212085624599E-2]
["CSXT-E1L203C8","CSXT",3,"E1L203C8",100,"CD(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED",14.6307420730591,15.3153276443481,14.815259933471699,13.7856187820435,12.3184213638306,12.9594535827637,12.408504486084,12.6162252426147,15.278359413146999,14.7237254260633,15.0719603363794,18.606338315115799,14.1293699962162,15.150496624040001,17.300943319916499,18.128062030855801]
["CSXT-E1L203C11","CSXT",3,"E1L203C11",103,"CD(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED",14.6307430267334,15.3153276443481,14.815258979797401,13.7856187820435,12.3184213638306,12.9594535827637,12.408505439758301,12.616224288940399,15.278358459472701,14.7237254260633,15.0719603363794,18.606338315115799,14.1293699962162,15.150496624040001,17.300943319916499,18.128062030855801]
["CSXT-E1L204C1","CSXT",3,"E1L204C1",106,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",7.4333599768578998E-3,8.1494767218828201E-3,7.9152230173349398E-3,1.27510754391551E-2,1.7880028113722801E-2,2.10953932255507E-2,2.3708859458565702E-2,2.22231857478619E-2,3.0525242909789099E-2,3.8058599924546202E-2,4.4353079921579198E-2,3.8071953447525203E-2,3.1354177197285699E-2,2.87223004375479E-2,2.6100570460808999E-2,2.4529498667582601E-2]
["CSXT-E1L204C2","CSXT",3,"E1L204C2",107,"CM(R), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",8.6788674816489202E-3,8.1489617004990595E-3,8.67988169193268E-3,1.5843983739614501E-2,1.12311458215117E-2,8.9406780898570997E-3,7.8106890432536602E-3,7.4470001272857198E-3,1.7266811802983301E-2,3.3378971493269703E-2,3.8219406306021997E-2,1.9533599721187799E-2,1.87863308305522E-2,1.8847874537338601E-2,2.9022151914457901E-2,2.29888422326745E-2]
["CSXT-E1L204C5","CSXT",3,"E1L204C5",110,"CM(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",2.25650388747454E-2,2.1187286823987999E-2,2.25676745176315E-2,4.1194345802068703E-2,2.9200961813330699E-2,2.3245735093951201E-2,2.0307779312133799E-2,1.9362181425094601E-2,4.48937118053436E-2,8.6785325882501305E-2,9.9370456395657406E-2,5.0787359275088297E-2,4.8844460159435797E-2,4.9004473797080401E-2,7.54575949775904E-2,5.97709898049536E-2]
["CSXT-E1L204C9","CSXT",3,"E1L204C9",114,"CD(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",0.88003700971603405,1.08619892597198,1.50093221664429,3.4481167793273899,3.1502096652984601,2.9000985622406001,2.6602506637573198,2.5956223011016801,7.7702269554138201,9.7844546435483597,8.9664145485309295,7.9684696236583603,8.3950696285013802,6.9416856218400902,7.5651967205748596,8.4588251237074399]
["CSXT-E1L204C12","CSXT",3,"E1L204C12",117,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",0.88003700971603405,1.08619892597198,1.50093221664429,3.4481167793273899,3.1502096652984601,2.9000988006591801,2.66025042533875,2.5956223011016801,7.7702269554138201,9.7844546435483597,8.9664145485309295,7.9684696236583603,8.3950696285013802,6.9416856218400902,7.5651967205748596,8.4588251237074399]
["CSXT-E1L205C2","CSXT",3,"E1L205C2",120,"CM(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",1.04194050654769E-2,1.21282702311873E-2,1.3210855424404099E-2,4.9837097525596598E-2,3.2590720802545499E-2,2.5939304381609001E-2,3.6448385566473E-2,3.48563008010387E-2,2.4087512865662599E-2,3.2538239664644503E-2,4.33426825208858E-2,2.3762576364767599E-2,2.5857814138518499E-2,2.4335323937274399E-2,4.8825732242506401E-2,3.7532672449822002E-2]
["CSXT-E1L205C7","CSXT",3,"E1L205C7",125,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.1180379390716602,2.4941391944885298,2.91811871528625,4.7872352600097701,5.2655172348022496,5.1369862556457502,4.8658614158630398,4.63242530822754,5.49554347991943,6.1763423287489401,6.7687148651149904,6.8850222756153903,6.5984300466575503,6.7157788226615196,5.7851713064526802,5.0595244228185798]
["CSXT-E1L205C10","CSXT",3,"E1L205C10",128,"CD(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.1180379390716602,2.4941391944885298,2.9181184768676798,4.7872357368469203,5.2655172348022496,5.1369862556457502,4.8658614158630398,4.63242530822754,5.49554347991943,6.1763423287489401,6.7687148651149904,6.8850222756153903,6.5984300466575503,6.7157788226615196,5.7851713064526802,5.0595244228185798]
["CSXT-E1L205C13","CSXT",3,"E1L205C13",131,"CM(R), DRL Expense, Privately-Owned, GONDOLA - EQUIPPED",2.7681680876412398E-5,7.8803830547258299E-5,4.8591810627840497E-4,8.6011298000812503E-2,5.5639434605836903E-2,2.8492972254753099E-2,3.21288369596004E-2,3.0367339029908201E-2,3.6550533026456798E-2,5.2234840638868303E-2,3.4584273145188797E-2,2.14949571287931E-2,6.5015665066368699E-3,4.1393627745684499E-4,2.1330550917492501E-3,1.1479456672574199E-3]
["CSXT-E1L206C1","CSXT",3,"E1L206C1",132,"CM(R), OPR Expense, Railroad-Owned, HOPPER - COVERED",3.6135349422693301E-2,3.7684187293052701E-2,3.6892548203468302E-2,4.6022944152355201E-2,4.3929245322942699E-2,3.6867149174213402E-2,3.4483838826417902E-2,5.0172671675682103E-2,5.2082698792219197E-2,5.6002490792959402E-2,3.8131483405361502E-2,4.6447867668440702E-2,4.88693921519699E-2,5.2013843549578102E-2,4.5007424715248302E-2,3.9192783104491702E-2]
["CSXT-E1L206C4","CSXT",3,"E1L206C4",135,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",9.3951873481273707E-2,9.7978807985782596E-2,9.5920518040657002E-2,0.119659647345543,0.114215895533562,9.5854580402374295E-2,8.9657962322235094E-2,0.13044896721839899,0.135414808988571,0.145606476061694,9.9141856853939905E-2,0.12076445593794601,0.12706041959512199,0.13523599322890301,0.117019304259645,0.101901236071678]
["CSXT-E1L206C8","CSXT",3,"E1L206C8",139,"CD(R), DRL Expense, Railroad-Owned, HOPPER - COVERED",7.97186374664307,7.6213178634643599,7.8387522697448704,7.5047888755798304,5.4062685966491699,5.7502741813659703,5.46065425872803,4.9313201904296902,5.9156146049499503,7.0338476534414998,9.0753109407455401,10.253567980142201,7.6657769332431096,11.182001025558201,8.5644954511998304,5.7487956613308198]
["CSXT-E1L206C10","CSXT",3,"E1L206C10",141,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",3.7037713527679399,4.0163435935974103,4.0672230720520002,5.1992115974426296,5.00115966796875,4.2441921234130904,4.0078601837158203,5.8877191543579102,6.0499186515808097,6.4671966054836698,4.4400732310666804,5.5788460447253803,5.8688998725135599,6.1940383712932103,5.27884472469208,4.63742700501827]
["CSXT-E1L207C2","CSXT",3,"E1L207C2",146,"CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",4.7938182950019802E-2,4.8278681933879901E-2,4.8942454159259803E-2,3.4927848726511002E-2,2.7466665953397799E-2,3.4686900675296797E-2,5.1822572946548497E-2,5.04811443388462E-2,3.9985731244087198E-2,3.9920508358602502E-2,5.9468216714117297E-2,7.4925267831105202E-2,5.1401803088753403E-2,4.2362694799223201E-2,5.4527403009836502E-2,4.3182917777091101E-2]
["CSXT-E1L207C6","CSXT",3,"E1L207C6",150,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",0.13358636200428001,0.16205233335495001,0.234119638800621,0.138981103897095,0.14678083360195199,0.22039607167243999,0.29963847994804399,0.30221250653266901,0.278554856777191,0.33658815056208202,0.46222867404224499,0.373335159193527,0.34286785765064898,0.25695547302477001,0.24114554359983301,0.27583124522125202]
["CSXT-E1L207C9","CSXT",3,"E1L207C9",153,"CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",5.5655460357665998,6.7880926132202104,10.2099857330322,6.0370168685913104,5.9101638793945304,9.2013702392578107,12.620265007019,13.2168569564819,10.8563280105591,12.5493312962674,18.577411251555102,15.9312049360675,12.622346462987601,10.3737206081708,10.684385757399999,12.9962452222347]
[{"$f":"B3074&\"-\"&D3074","v":"CSXT-E1L207C10"},"CSXT",3,"E1L207C10",154,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.54891073703766,1.6243761777877801,1.6201857328414899,2.39696073532104,2.5707380771636998,2.73738718032837,2.7687580585479701,2.5558414459228498,2.7476148605346702,2.3776597685153802,2.5811374439736099,2.1720468747564299,1.8799597257153899,1.6422188436031799,1.3505264009984299,1.29665382601948]
["CSXT-E1L207C13","CSXT",3,"E1L207C13",157,"CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - GENERAL",2.1721285520470701E-5,3.9766197005519603E-5,2.9689277653233101E-5,5.8888420462608303E-3,1.82594452053308E-2,5.2113435231149197E-3,7.0227761752903496E-3,9.4829490408301405E-3,6.4027407206594901E-3,6.0995729036495399E-3,5.7068165951983897E-3,2.2506069524651701E-3,1.29551491461536E-3,1.8356538818569001E-4,1.01592312858056E-5,6.1360996982716104E-6]
["CSXT-E1L208C3","CSXT",3,"E1L208C3",160,"CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.5345372036099399E-2,3.2561622560024303E-2,4.3901190161705003E-2,9.5564872026443495E-2,0.11610709875822101,0.13587854802608501,0.149192914366722,0.12988817691803001,9.0394720435142503E-2,9.0289027049138895E-2,0.111574026638235,0.12276522430207901,0.14265482123165299,0.112421972565888,0.101702407364232,0.12507282905474501]
["CSXT-E1L208C7","CSXT",3,"E1L208C7",164,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.70250147581100497,0.77317517995834395,0.79587256908416704,1.21408987045288,1.5426844358444201,1.8491634130477901,2.16185474395752,2.1873092651367201,2.4680619239807098,3.3676587950259398,3.9003882922641901,4.5583858777385302,4.3851286936726996,4.3149989251235201,3.64323543376097,3.2244577027347301]
["CSXT-E1L208C9","CSXT",3,"E1L208C9",166,"CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.5233739614486701,1.9618383646011399,2.7784802913665798,5.6746387481689498,6.2692184448242196,6.7786788940429696,7.06632328033447,6.4543948173522896,4.4883327484130904,4.5250998060386696,5.4375186820307198,6.54423397345652,8.1254091077206994,5.9607786775464202,5.3061044253212497,6.99283058192312]
["CSXT-E1L209C1","CSXT",3,"E1L209C1",171,"CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",0,0,0,5.3450901759788405E-4,1.1691303225234201E-3,1.4009380247443899E-3,1.6185572603717401E-3,1.75076152663678E-3,2.2149637807160599E-3,2.2935685135693998E-3,2.1206969631635099E-3,2.0691365336115799E-3,1.9890272657914999E-3,2.0378877665856898E-3,1.87132310649992E-3,2.0073298718561502E-3]
["CSXT-E1L209C5","CSXT",3,"E1L209C5",175,"CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",0.332193583250046,0.33837080001831099,0.31572696566581698,0.34068095684051503,0.33319297432899497,0.27298071980476402,0.33604222536086997,0.37149795889854398,0.38640683889388999,0.35027715791148001,0.33713301751305003,0.34833970817377402,0.34330299711270201,0.37746695719255002,0.410244869357271,0.38840052212933401]
["CSXT-E1L209C8","CSXT",3,"E1L209C8",178,"CD(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",34.463939666747997,31.5871677398682,30.972904205322301,36.396141052246101,33.157215118408203,28.124469757080099,30.494672775268601,33.231128692627003,40.466392517089801,40.8584817690721,41.292156647424299,46.764229538779098,38.437928544991699,44.695809857999201,51.192001640136603,70.3274770534602]
["CSXT-E1L209C9","CSXT",3,"E1L209C9",179,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",0,0,0,5.9937157630920401,5.6314511299133301,6.3188762664794904,6.2800946235656703,6.3314528465270996,0.27081361413001998,0.27418403323549601,0.27922829946670602,0.32607785907793202,0.29681189671712099,0.27536867401224802,0.27238635477229201,0.37858929085575899]
["CSXT-E1L209C12","CSXT",3,"E1L209C12",182,"CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",0,0,0,5.9937162399292001,5.6314506530761701,6.3188762664794904,6.2800946235656703,6.3314533233642596,0.27081361413001998,0.27418403323549601,0.27922829946670602,0.32607785907793202,0.29681189671712099,0.27536867401224802,0.27238635477229201,0.37858929085575899]
["CSXT-E1L210C2","CSXT",3,"E1L210C2",185,"CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",4.5679133385419797E-2,4.9945987761020702E-2,5.0198238343000398E-2,4.9631748348474503E-2,4.9582686275243801E-2,4.9342952668666798E-2,5.2196156233549097E-2,5.2206285297870601E-2,0.239917442202568,4.17725766739451E-2,3.6583692536889097E-2,5.5163423589978902E-2,6.0120963659145599E-2,5.7230042904719503E-2,9.1733230421701603E-2,8.6767951537693594E-2]
["CSXT-E1L210C6","CSXT",3,"E1L210C6",189,"CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",4.0323063731193501E-2,7.4358537793159499E-2,0.114921443164349,9.9544795230030996E-3,1.0648315772414201E-2,1.26063423231244E-2,1.80476177483797E-2,2.16285567730665E-2,-1.85773577541113E-2,-1.75316366185117E-2,2.3355589729524999E-2,2.9509565779211201E-2,2.8124292109730699E-2,2.52311110553862E-2,2.4867691948799401E-2,2.9202357725915701E-2]
["CSXT-E1L210C8","CSXT",3,"E1L210C8",191,"CD(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",12.1787977218628,13.6792459487915,14.4307355880737,16.404058456420898,17.157457351684599,18.2819633483887,18.505966186523398,16.804878234863299,63.517215728759801,17.335396989514098,15.5751667621492,19.676449764819498,18.1945837046683,17.393402761180301,28.581147922910802,27.809759500502999]
["CSXT-E1L210C13","CSXT",3,"E1L210C13",196,"CM(R), DRL Expense, Privately-Owned, REFRIGERATED - NON-MECH",2.9705124907195598E-3,2.0205448381602799E-3,2.4513114476576399E-4,6.0224084882065697E-4,1.30967330187559E-3,1.0516141541302201E-2,1.8505442887544601E-2,1.28209334798157E-3,3.3699097111821201E-3,1.0189270516069401E-3,4.5024843412803202E-4,2.8814301511837799E-4,4.2206856909553301E-4,2.7405929836366998E-4,2.6121506914516998E-4,1.4992614048417601E-4]
["CSXT-E1L211C4","CSXT",3,"E1L211C4",200,"CM(Y), OPR Expense, Railroad-Owned, FLAT - TOFC",0,0,0,9.1718859039247003E-4,1.5578608727082599E-3,2.33118096366525E-3,2.6331115514040002E-3,2.5830913800746198E-3,2.34812125563622E-3,1.6245911848103999E-3,1.2510646731363701E-3,1.03164940563284E-3,9.9113099098998105E-4,1.0605187414452E-3,8.9829703675154099E-4,8.4523547485960602E-4]
["CSXT-E1L211C7","CSXT",3,"E1L211C7",203,"CD(R), OPR Expense, Railroad-Owned, FLAT - TOFC",0,0,0,3.3407736569643E-2,5.4912805557250997E-2,8.0259010195732103E-2,8.9440532028675093E-2,8.7747916579246493E-2,7.8031204640865298E-2,5.3419350353587101E-2,4.1025940133552798E-2,3.4406708880765302E-2,3.3832782308825998E-2,3.6500863118126899E-2,3.1421449922382903E-2,2.86669064654906E-2]
["CSXT-E1L211C8","CSXT",3,"E1L211C8",204,"CD(R), DRL Expense, Railroad-Owned, FLAT - TOFC",0,0,0,0.33839607238769498,13.5269060134888,19.8314018249512,12.888343811035201,13.306097984314,14.331096649169901,12.890765865153,13.321739291906599,14.6039778978881,16.083136262854399,14.914276953411299,14.4495299529253,18.815973115493499]
["CSXT-E1L211C11","CSXT",3,"E1L211C11",207,"CD(Y), DRL Expense, Railroad-Owned, FLAT - TOFC",0,0,0,0.33839607238769498,13.5269060134888,19.8314018249512,12.8883419036865,13.306097984314,14.3310956954956,12.890765865153,13.321739291906599,14.6039778978881,16.083136262854399,14.914276953411299,14.4495299529253,18.815973115493499]
["CSXT-E1L212C1","CSXT",3,"E1L212C1",210,"CM(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",0.20963788032531699,0.22240823507308999,0.22583769261837,0.25394123792648299,0.226562410593033,0.22254973649978599,0.248420596122742,0.236876040697098,0.21889321506023399,0.22721600331679701,0.230221842218261,0.240115454827383,0.214942452622882,0.23742136686086701,0.22052315639342601,0.22558848046194099]
["CSXT-E1L212C7","CSXT",3,"E1L212C7",216,"CD(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",22.3227939605713,23.955532073974599,24.3398532867432,27.728294372558601,24.845832824706999,24.634803771972699,27.526100158691399,26.207561492919901,23.943252563476602,24.681944825032399,25.0452716189005,26.848947756067499,24.177472428522002,26.788871887265898,24.319651798620701,24.869848799987501]
[{"$f":"B3138&\"-\"&D3138","v":"CSXT-E1L212C9"},"CSXT",3,"E1L212C9",218,"CD(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",20.111944198608398,26.431449890136701,36.861526489257798,70.320556640625,56.712497711181598,66.908905029296903,60.184226989746101,49.321788787841797,36.854179382324197,49.079106470639402,38.091802295817899,44.334962891526096,39.795979566380197,29.4719194971691,33.339121758854297,49.8609249696649]
["CSXT-E1L212C13","CSXT",3,"E1L212C13",222,"CM(R), DRL Expense, Privately-Owned, FLAT - MULTILEVEL",0.13063292205333699,0.13549561798572499,0.15772764384746599,0.22016510367393499,0.18977333605289501,0.18986251950263999,0.16810254752636,0.17453993856906899,0.18580384552478801,0.17958284443957001,0.19011880322289601,0.217982400321384,0.189246185278065,0.18587627296217701,0.248895113945867,0.28431347901938198]
["CSXT-E1L213C3","CSXT",3,"E1L213C3",225,"CM(R), ROI Expense, Railroad-Owned, FLAT - GENERAL",5.8265496045351001E-2,4.1237890720367397E-2,9.7128473222255707E-2,0,0,0,0,0,2.7199259493499999E-3,3.8085069126152999E-3,4.3275830240902396E-3,3.8608543798445097E-2,4.3693649301364601E-2,3.3433275192128298E-2,2.27566570901775E-3,3.4535957821273098E-3]
["CSXT-E1L213C6","CSXT",3,"E1L213C6",228,"CM(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL",0.15149022638797799,0.107218533754349,0.25253355503082298,0,0,0,0,0,7.0718098431825603E-3,9.9021179727997802E-3,1.12517158626346E-2,0.100382213875957,0.113603488183548,8.6926515499533397E-2,5.9167308434461396E-3,8.9793490335309794E-3]
["CSXT-E1L213C7","CSXT",3,"E1L213C7",229,"CD(R), OPR Expense, Railroad-Owned, FLAT - GENERAL",0,0,0,0,0,0,0,0,0,0,0,536.88065934276403,533.78144833540102,530.16765902993097,0,0]
["CSXT-E1L213C10","CSXT",3,"E1L213C10",232,"CD(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL",0,0,0,0,0,0,0,0,0,0,0,536.88065934276403,533.78144833540102,530.16765902993097,0,0]
["CSXT-E1L213C13","CSXT",3,"E1L213C13",235,"CM(R), DRL Expense, Privately-Owned, FLAT - GENERAL",0.30732518434524497,0.40977552533149703,0.33768284320831299,0.366513311862946,1.0375219583511399,1.8161705732345601,3.1956722736358598,9.9351830780506106E-2,3.37144899368286,4.4953327574955397E-2,6.8741532461777499E-2,6.3298686816013203E-3,0.103368887486539,0.19822317537360901,0.27682835861053501,8.7373971220519694E-2]
["CSXT-E1L214C6","CSXT",3,"E1L214C6",241,"CM(Y), ROI Expense, Railroad-Owned, FLAT - OTHER",1.05358948931098E-2,1.35584827512503E-2,2.0172905176878E-2,2.1880839020013799E-2,2.26048845797777E-2,2.8558177873492199E-2,2.9722733423113799E-2,2.6773018762469299E-2,4.3788637965917601E-2,8.0073032343617706E-2,6.8075288288227301E-2,7.7458889665868794E-2,9.1931937358359903E-2,6.3040569614528294E-2,5.5584682825677099E-2,6.8791240959386296E-2]
["CSXT-E1L214C8","CSXT",3,"E1L214C8",243,"CD(R), DRL Expense, Railroad-Owned, FLAT - OTHER",18.274877548217798,17.739048004150401,16.9767246246338,17.195184707641602,17.064008712768601,11.378318786621101,15.366035461425801,15.501523971557599,20.712596893310501,23.4183811377886,27.115319608282501,27.354010672387801,22.328591224627999,20.9762465946175,20.7028467105837,22.940547844559699]
["CSXT-E1L214C12","CSXT",3,"E1L214C12",247,"CD(Y), ROI Expense, Railroad-Owned, FLAT - OTHER",0.64944577217102095,0.868588507175446,1.2771669626236,1.39215040206909,1.39846587181091,1.7178076505661,1.83606469631195,1.6421189308166499,2.7876627445220898,5.7160061129711996,5.3292546855450604,6.2173817021072404,6.7544831451711502,4.6454753029516898,4.1618806135064501,5.0972820322666497]
["CSXT-E1L215C2","CSXT",3,"E1L215C2",250,"CM(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,3.7509130779653801E-3,0,2.5262583512812901E-3,2.43039382155214E-3,2.1895651314997899E-3,1.62213160292911E-3,1.62969603258616E-3,1.9756147903464802E-3,1.6293537444077399E-3,1.1280280974125E-3]
["CSXT-E1L215C5","CSXT",3,"E1L215C5",253,"CM(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L215C6","CSXT",3,"E1L215C6",254,"CM(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L215C9","CSXT",3,"E1L215C9",257,"CD(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L215C13","CSXT",3,"E1L215C13",261,"CM(R), DRL Expense, Privately-Owned, TANK <22,000 GAL",2.3276435211300898E-2,1.7070950940251399E-2,1.1907698586583099E-2,6.5929060801863696E-3,9.4089312478900008E-3,4.9899271689355399E-3,3.7509130779653801E-3,2.7956871781498198E-3,2.5262583512812901E-3,2.43039382155214E-3,2.1895651314997899E-3,1.62213160292911E-3,1.62969603258616E-3,1.9756147903464802E-3,1.6293537444077399E-3,1.1280280974125E-3]
["CSXT-E1L216C5","CSXT",3,"E1L216C5",266,"CM(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L216C7","CSXT",3,"E1L216C7",268,"CD(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L216C11","CSXT",3,"E1L216C11",272,"CD(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L217C1","CSXT",3,"E1L217C1",275,"CM(R), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.33439859747886702,0.38355129957199102,0.38750836253166199,0.32311126589775102,7.7154949307441698E-2,4.7798696323297902E-4,5.6609127204865196E-4,0.265881568193436,0.30766624212264998,0.221188341411337,1.0810550045196399E-3,1.5944851604345501E-3,1.7846520307577499E-3,2.0125146349131299E-3,1.84738770547075E-3,1.4968360872960099E-3]
["CSXT-E1L217C4","CSXT",3,"E1L217C4",278,"CM(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.86943602561950695,0.99723142385482799,1.0075216293335001,0.84008908271789595,0.20060274004936199,1.24276790302247E-3,1.4718394959345499E-3,0.69129168987274203,0.79993176460266102,0.57508968766947599,2.8107430117510599E-3,4.1456614171298299E-3,4.6400952799701602E-3,5.2325380507741298E-3,4.8032080342239403E-3,3.8917738269696402E-3]
["CSXT-E1L217C5","CSXT",3,"E1L217C5",279,"CM(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.199443429708481,0.230209931731224,9.5425650477409404E-2,0.122853025794029,2.78472620993853E-2,0.123442940413952,0.26741069555282598,0.24283082783222201,6.5714098513126401E-2,3.2647183137221099E-2,3.6215987818964498E-2,9.1257383391039101E-2,-4.4442804253116003E-2,5.4277401281462703E-2,4.1937983262999301E-2,2.3526787264906402E-3]
[{"$f":"B3202&\"-\"&D3202","v":"CSXT-E1L217C8"},"CSXT",3,"E1L217C8",282,"CD(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",12.9425706863403,14.2888174057007,8.7363119125366193,10.4412536621094,3.6241507530212398,9.1759233474731392,14.534014701843301,10.3860569000244,5.6309223175048801,2.5847847762396698,4.4192724512451802,4.9881871198286101,-0.52658325361042801,2.7695314491444898,1.71302861984559,0.51465771614191702]
["CSXT-E1L217C12","CSXT",3,"E1L217C12",286,"CD(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",21.252799987793001,29.307878494262699,24.083183288574201,18.413568496704102,7.5670051574706996,22.185234069824201,29.560979843139599,25.420469284057599,1.45681381225586,7.1004942309335997,4.4650102747911298,4.2482154419210501,5.1909037985476401,3.3512698358108599,2.5885573074490398,2.2642767631743101]
["CSXT-E1L218C4","CSXT",3,"E1L218C4",291,"CM(Y), OPR Expense, Railroad-Owned, AUTO RACKS",6.2191719189286197E-3,0.578260958194733,0.58717846870422397,0.65433317422866799,0.54326927661895796,0.49322494864463801,0.52337044477462802,0.503290235996246,0.45341685414314298,0.467701252334843,0.47256259565061898,0.53724913496554205,0.49112685216741903,0.56126255730957697,0.49680360110341298,0.51261543100019702]
["CSXT-E1L218C6","CSXT",3,"E1L218C6",293,"CM(Y), ROI Expense, Railroad-Owned, AUTO RACKS",0.15362644195556599,0.42519104480743403,0.60098767280578602,1.05816662311554,0.85877209901809703,1.0129475593566899,0.90253919363021895,0.74766075611114502,0.47035396099090598,0.706268337845668,0.59780321164172201,0.66587232562091003,0.62427488353897498,0.46073214399330997,0.53842162607487098,0.78534462391621696]
["CSXT-E1L218C10","CSXT",3,"E1L218C10",297,"CD(Y), OPR Expense, Railroad-Owned, AUTO RACKS",0.10575807839632,23.955532073974599,24.3398532867432,27.479957580566399,22.914381027221701,20.9987602233887,22.304559707641602,21.416601181030298,19.075454711914102,19.5404988005589,19.772665374479399,23.105189394205301,21.247558236898001,24.3571991558928,21.0724261146398,21.735746154661999]
["CSXT-E1L218C13","CSXT",3,"E1L218C13",300,"CM(R), DRL Expense, Privately-Owned, AUTO RACKS",1.6569355502724599E-2,1.7995601519942301E-2,2.4581553414464E-2,1.89069344196469E-3,2.5866871699690801E-2,1.1874490417540099E-2,8.4810778498649597E-3,8.6317807435989397E-3,1.0816371999680999E-2,1.30104974844034E-2,1.6457750961105199E-2,1.6917391034244299E-2,1.3742329326082299E-2,1.4560430010472801E-2,2.3258389121373801E-2,1.3781132495121501E-2]
["CSXT-E1L219C3","CSXT",3,"E1L219C3",303,"CM(R), ROI Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L219C4","CSXT",3,"E1L219C4",304,"CM(Y), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L219C7","CSXT",3,"E1L219C7",307,"CD(R), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L219C12","CSXT",3,"E1L219C12",312,"CD(Y), ROI Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E1L220C2","CSXT",3,"E1L220C2",315,"CM(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.85320261120796E-2,4.03918102383614E-2,4.01770509779453E-2,4.30838465690613E-2,3.8508348166942603E-2,3.8522429764270803E-2,4.06341888010502E-2,4.0449362248182297E-2,4.2565055191516897E-2,4.57090984672004E-2,5.0716134194547097E-2,4.5703663973519902E-2,4.4010951075268499E-2,4.7577785298011099E-2,5.5999428570298299E-2,4.7633698320471603E-2]
["CSXT-E1L220C5","CSXT",3,"E1L220C5",318,"CM(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",9.3837656080722795E-2,9.6126332879066495E-2,0.101357504725456,0.109392330050468,9.4403110444545704E-2,9.2039361596107497E-2,9.8519526422023801E-2,9.5640689134597806E-2,9.5844671130180401E-2,0.10913658271700299,0.12566048274191599,0.108510802072497,0.106677286817994,0.106871717821469,0.13729296878071301,0.11768571871139299]
["CSXT-E1L220C9","CSXT",3,"E1L220C9",322,"CD(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.14995265007019,4.2056412696838397,6.0037183761596697,6.9695057868957502,6.5311303138732901,7.2505931854248002,7.7079510688781703,7.2160172462463397,6.3675236701965297,7.3051072116381999,7.72511042991162,8.7289619233466507,9.1933990214046997,7.3616608227393199,7.0723472387572004,8.7119239074276003]
["CSXT-E1L220C12","CSXT",3,"E1L220C12",325,"CD(Y), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",2.8556668758392298,3.7653532028198198,5.4908676147460902,6.57668256759644,6.1720890998840297,6.7297496795654297,7.1180005073547399,6.7359085083007804,6.5027604103088397,7.4366283351287699,7.7331416583236896,8.4431514845188094,9.1516692990292903,7.2756218507270196,7.0640059637753296,8.5500004517752597]
["CSXT-E1L220C13","CSXT",3,"E1L220C13",326,"CM(R), DRL Expense, Privately-Owned, AVERAGE ALL FREIGHT CARS",3.6228612065315198E-2,3.4776881337165798E-2,3.3229313790798201E-2,4.2095545679330798E-2,4.1526123881339999E-2,5.4751981049776098E-2,5.76149746775627E-2,5.66123388707638E-2,5.8876410126686103E-2,6.0437757832226303E-2,6.65405357510402E-2,6.8453296599131699E-2,6.5962526828133097E-2,6.4670094776012294E-2,7.0687000816999399E-2,7.6630215261916504E-2]
["CSXT-E1L221C3","CSXT",3,"E1L221C3",329,"CM(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.126747071743011,0.16354763507843001,0.231168478727341,0.42379122972488398,0.34428396821022,0.406324833631516,0.36215418577194203,0.30023080110549899,0.23148944973945601,0.30256842449754001,0.23028736199230701,0.256402191512627,0.24039163646376799,0.17741220028667601,0.20744607931037701,0.302505347075744]
["CSXT-E1L221C6","CSXT",3,"E1L221C6",332,"CM(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.32954192161560097,0.42522409558296198,0.60103791952133201,1.10185635089874,0.89513820409774802,1.05644595623016,0.94159978628158603,0.78060019016265902,0.60187220573425304,0.78667790369360002,0.59874714118000105,0.66664569793283301,0.62501825480579698,0.46127172074535899,0.53935980620697999,0.78651390239693597]
["CSXT-E1L221C11","CSXT",3,"E1L221C11",337,"CD(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",52.184123992919901,51.228233337402301,111.654083251953,98.863883972167997,72.238830566406307,46.0145874023438,55.425857543945298,40.379322052002003,52.9688911437988,48.667604524240602,71.928152336832298,74.490927642856704,57.261217743901,66.577008436657493,70.793068341978596,61.092175393203298]
["CSXT-E1L301C1","CSXT",3,"E1L301C1",340,"L&D Expense, FARM PRODUCTS",6.0479726642370203E-2,4.3492771685123402E-2,5.2238646894693402E-2,5.0968628376722301E-2,3.09725925326347E-2,5.8702994138002403E-2,3.9931595325469998E-2,4.0919195860624299E-2,5.5300697684287997E-2,4.0740445742439298E-2,3.0235172829172E-2,4.2640386857255498E-2,3.0764167073179E-2,3.9305223656339899E-2,2.3084220232348799E-2,3.2991514790269003E-2]
["CSXT-E1L304C1","CSXT",3,"E1L304C1",343,"L&D Expense, FRESH FRUITS",0.302319556474686,8.5989952087402302E-2,0.58841019868850697,8.6072228848934201E-2,1.4460543170571299E-2,0.126831129193306,0.49312025308608998,0.52817994356155396,0.16668255627155301,8.2599028253724796E-2,9.9674777409128404E-2,0.43295957620681202,8.8434329739041695E-2,0.85901773298737005,1.1195029946875601,0.48971047651869798]
["CSXT-E1L308C1","CSXT",3,"E1L308C1",347,"L&D Expense, COAL",3.01631726324558E-3,3.2460147049277999E-3,3.05656832642853E-3,4.3408023193478602E-3,3.2279870938509698E-3,3.3305299002677198E-3,4.0287571027874903E-3,3.9105019532144096E-3,2.7237308677285901E-3,2.14346200941452E-3,2.0286106009389702E-3,4.8588212337537899E-3,4.4838032093151596E-3,3.9408800824081098E-3,1.5177075802263499E-3,2.1313169653889401E-3]
["CSXT-E1L311C1","CSXT",3,"E1L311C1",350,"L&D Expense, FRESH MEATS",0,0,0,0,6.0307089239358902E-2,0.14437814056873299,0.18296842277049999,0,0,0,0,0,0,0,0,0]
["CSXT-E1L312C1","CSXT",3,"E1L312C1",351,"L&D Expense, DAIRY PRODUCTS",0.26197466254234297,1.34666740894318,1.7574552297592201,0.46422058343887301,0.35715392231941201,0.464790970087051,0.49275985360145602,0.75572431087493896,1.05871522426605,2.0809273501940702,0.96986246387669905,0.98166953399452095,2.6580326093429498,4.3113833540049997,3.8502678120262801,1.82206074815941]
["CSXT-E1L315C1","CSXT",3,"E1L315C1",354,"L&D Expense, FLOUR",3.2923668622970602E-2,7.6696105301380199E-2,8.2328729331493405E-2,4.6068139374256099E-2,6.2322694808244698E-2,7.4686713516712203E-2,7.1782425045967102E-2,5.7252213358879103E-2,2.7048252522945401E-2,5.3978262161745102E-2,8.1389778583540101E-2,2.0658939350466098E-2,5.6218799270150201E-2,4.7762989723968197E-2,5.6966833978788899E-2,5.6377434374590599E-2]
["CSXT-E1L318C1","CSXT",3,"E1L318C1",357,"L&D Expense, RICE",0.18275606632232699,0.20021592080593101,0.26043739914894098,0.49083593487739602,0.26900073885917702,0.26474368572235102,0.105855084955692,0.30795875191688499,0.195555880665779,0.171957354616004,0.217271284411443,0.20353585332434401,0.10460667322949101,0.201985129218855,0.18705377019309699,0.27474099401881502]
["CSXT-E1L323C1","CSXT",3,"E1L323C1",362,"L&D Expense, WINES",0.84492164850234996,8.3208911120891599E-2,1.34687983989716,0.44220030307769798,0.205625951290131,6.3485205173492404E-2,0.24367405474185899,0.51581692695617698,0.34035617113113398,1.35427260144433,0.24422654004494099,0.105158524452878,0.36028833717952002,0.267506679227699,0.16329456182654101,0.12703334188972801]
["CSXT-E1L326C1","CSXT",3,"E1L326C1",365,"L&D Expense, ALL OTHER FOOD PRODUCTS",9.1888576745986897E-2,7.9573296010494204E-2,0.12117470800876599,6.5014228224754306E-2,3.6592349410057103E-2,4.3420534580946003E-2,0.141043856739998,5.3964279592037201E-2,5.3006786853075E-2,7.9923448269122996E-2,9.9097557048061696E-2,8.1842532444312499E-2,0.19285248625642101,0.17873068167745801,0.111427994915152,8.3245180810300995E-2]
["CSXT-E1L329C1","CSXT",3,"E1L329C1",368,"L&D Expense, LUMBER/DIMENSION STOCK",6.9662675261497498E-2,6.6921301186084706E-2,5.0744507461786298E-2,4.2644336819648701E-2,2.0643839612603201E-2,7.3353521525859805E-2,1.56366545706987E-2,3.8499526679515797E-2,2.4210380390286401E-2,6.5480499825039798E-2,6.5441979456708904E-2,6.6382032559786502E-2,9.6643513669763995E-2,3.5730563075364201E-2,7.45180514067776E-2,0.18957337341988301]
["CSXT-E1L333C1","CSXT",3,"E1L333C1",372,"L&D Expense, PULP, PAPER AND ALLIED PRODUCTS",0.26838248968124401,0.28085958957672102,0.29805308580398598,0.29972025752067599,0.20974843204021501,0.18133181333541901,0.162495583295822,0.17467743158340501,0.16834378242492701,0.12844722302166001,0.153450512751615,0.17213338337717099,0.106044886035222,0.12062119539989299,8.5510400889075799E-2,0.144576608542514]
["CSXT-E1L336C1","CSXT",3,"E1L336C1",375,"L&D Expense, FIBREBD/PAPERDB/PULPDB",0.247822120785713,0.201040908694267,0.26354819536209101,0.315349161624908,0.22802263498306299,0.206928014755249,0.15028686821460699,0.219723805785179,0.196718350052834,0.13845131328341401,0.14237568256028199,0.14370424430854201,9.1790883821594699E-2,8.6933569886294401E-2,7.6629285275818401E-2,0.17068400098040601]
["CSXT-E1L337C1","CSXT",3,"E1L337C1",376,"L&D Expense, COV PAPER/PAPERBOARD",0.14351396262645699,2.3441700264811498E-2,5.0217267125844997E-2,4.3607987463474301E-2,3.0316181480884601E-2,3.9156388491392101E-2,6.6796630620956393E-2,3.8177575916051899E-2,0.123719930648804,8.9984059162479299E-2,4.7553798615383003E-2,9.2495401211793692E-3,6.3031332334864496E-3,3.4192846214227003E-2,6.3265511684125697E-2,8.0745058269087004E-3]
["CSXT-E1L340C1","CSXT",3,"E1L340C1",379,"L&D Expense, CHEMICALS",5.11742942035198E-2,4.20025512576103E-2,3.6974240094423301E-2,4.2966037988662699E-2,3.3213671296834897E-2,4.8909343779087101E-2,5.0282698124647099E-2,3.2089069485664402E-2,3.1751915812492398E-2,3.2152053773539503E-2,4.5385256484858798E-2,3.7555629213460701E-2,3.01283549154009E-2,4.3525262911993302E-2,4.1050292308664603E-2,4.8456104800754497E-2]
["CSXT-E1L344C1","CSXT",3,"E1L344C1",383,"L&D Expense, MISC CHEMICALS PRODUCTS",4.3860375881195103E-2,5.9413857758045197E-2,5.3479108959436403E-2,6.6045254468917805E-2,5.3832165896892499E-2,6.0841087251901599E-2,1.3048115186393301E-2,3.7528481334447902E-2,7.7735278755426398E-3,5.2866308194148698E-2,6.3770333647115898E-3,9.4641084932867905E-3,5.7108239653403999E-3,4.0468951069907904E-3,3.7185460949404302E-2,2.3238877916688001E-2]
["CSXT-E1L348C1","CSXT",3,"E1L348C1",387,"L&D Expense, RUBBER TIRES/INNER TUBES",0.134509116411209,8.9131239801645296E-3,1.7789637669920901E-2,4.3709573219530301E-4,6.3215277623385202E-4,0.12824502587318401,0.20823356509208699,0.172246068716049,0.101569473743439,5.1709465437767201E-2,4.1918087269156301E-3,3.8097494457809397E-2,6.2541206245703999E-3,5.4441562535281901E-2,7.61084379992156E-2,9.8839377049493804E-2]
["CSXT-E1L351C1","CSXT",3,"E1L351C1",390,"L&D Expense, FLAT GLASS",7.9960972070693997E-2,0,0,4.9382718279957797E-3,0,0,0,0,0.24076983332634,7.4834149668299293E-2,0,0,0,2.46638667305578E-3,0,1.26070110068464E-2]
["CSXT-E1L355C1","CSXT",3,"E1L355C1",394,"L&D Expense, PRIMARY IRON/STEEL PRODUCTS",3.4884344786405598E-2,5.3362432867288603E-2,3.6286663264036199E-2,9.7192518413066906E-2,4.7952342778444297E-2,4.3800264596939101E-2,2.8834400698542598E-2,3.0930418521165799E-2,4.0773164480924599E-2,4.32040643335612E-2,3.8559282806765002E-2,6.04644823038471E-2,4.9514510216627401E-2,7.8182518416237898E-2,1.5334172940485001E-2,4.9781753141333498E-2]
["CSXT-E1L358C1","CSXT",3,"E1L358C1",397,"L&D Expense, FABRICATED METAL PRODUCTS",0.29441612958908098,8.34800750017166E-2,0.120782092213631,0.57032650709152199,0.127834737300873,0.121632412075996,0.10238241404295,0.34850579500198398,2.4500768631696701E-2,4.4205237424147302E-2,4.1813711219508103E-2,0.13085792181979899,5.4769202978317402E-2,0.17031496412081801,3.3467763128923302E-3,0.226221318634625]
["CSXT-E1L361C1","CSXT",3,"E1L361C1",400,"L&D Expense, MACHINERY EXCEPT ELECTRICAL",0.56518673896789595,0.32207629084587103,0.48734244704246499,0.78966307640075695,0.41966882348060602,0.16947755217552199,0.53890877962112405,0.47151488065719599,0.35861149430275002,0.237905620493821,0.107907509116882,0.111111250301434,0.57319507395133296,0.40923914491589602,4.4424753803321601E-2,0.24683393968713699]
["CSXT-E1L362C1","CSXT",3,"E1L362C1",401,"L&D Expense, ENGINES/TURBINES",0,0,0,0.65623474121093806,0.37552052736282299,3.18804383277893E-2,0.92005145549774203,0.18546940386295299,0.75826698541641202,0.10592373868414701,1.7432681007613301E-2,0.11374880081262601,0.19588503448769101,0.627909057749931,-6.83448356503671E-4,0.166006178271392]
["CSXT-E1L365C1","CSXT",3,"E1L365C1",404,"L&D Expense, ALL OTHER MACHINERY EXCEPT ELECTRICAL",0.51521039009094205,0.112866580486298,0.80271893739700295,0.47596234083175698,0.30874112248420699,4.8945009708404499E-2,0.31174495816230802,0.42183950543403598,4.2986869812011701E-3,0.15186131419488499,9.5799168819499E-2,2.66155263257274E-3,0.14928714522905701,0.14762019602208301,5.02985279069205E-2,3.62333789688866E-2]
["CSXT-E1L369C1","CSXT",3,"E1L369C1",408,"L&D Expense, RADIO OR TV SETS",6.56506299972534,7.9000549316406303,11.099229812622101,2.6888911724090598,3.2490937709808398,1.53677189350128,5.8817706108093297,24.248622894287099,3.8644213676452601,1.0204034771199,2.4656724349818999,0.16968987712112299,0.212309300578224,0.93635726795096297,0.93072368421052598,7.9683165020530504]
["CSXT-E1L373C1","CSXT",3,"E1L373C1",412,"L&D Expense, MOTOR TRUCKS",2.1043250560760498,1.26811671257019,1.65900325775146,1.4032484292984,0.97844052314758301,0.82795894145965598,2.6402244567871098,2.5844602584838898,5.3508419990539604,2.3972440890440101,2.5053101151001802,3.01905989333518,4.5072670290018699,1.8358317475753301,1.9620481392513101,6.0876948799235704]
["CSXT-E1L376C1","CSXT",3,"E1L376C1",415,"L&D Expense, FREIGHT FORWARDER TRAFFIC",3.4748416393995299E-2,0.119148962199688,0.133060157299042,6.0009412467479699E-2,2.6239469647407501E-2,5.6703973561525303E-2,0.39763507246971103,0.102938175201416,0.42134848237037698,0.183535784884371,6.4649280290004899E-2,1.21218522459901E-2,9.2906133987932099E-3,3.4791419592622302E-2,1.53999961012668E-2,7.4345374257392599E-2]
["CSXT-E1L380C1","CSXT",3,"E1L380C1",419,"L&D Expense, ALL OTHER MIXED SHIPMENTS",0.16601713001728099,0.88630723953247104,1.4442171668633799E-3,0.87179607152938798,0.75372087955474898,0.13352239131927501,3.1231531873345399E-2,9.3002393841743497E-2,1.03999447822571,0.416805851183083,0.345811739282818,0.14978310418351601,0.18150323928185,3.82302116571379,1.53221325354683,0.10334428935010299]
["CSXT-E2L101C1","CSXT",3,"E2L101C1",422,"Average Tare Weight, BOX - 40 FT",26.200000762939499,26.200000762939499,25.899999618530298,25.299999237060501,26,25.700000762939499,29,28.5,28.5,28.5,27.9,27.5,29,29,29.2,29.2]
["CSXT-E2L101C4","CSXT",3,"E2L101C4",425,"E/L Ratio, All Freight Cars, BOX - 40 FT",1.67222952842712,1.7296861410141,1.7342956066131601,1.85379791259766,1.78199315071106,1.6999477148055999,1.7269216775894201,1.70006310939789,1.73571705818176,1.8313538270454901,1.82924685824765,1.74804255319149,1.82117800620003,1.98231756574814,1.95330067646373,1.8980000702963]
["CSXT-E2L101C5","CSXT",3,"E2L101C5",426,"Local circuity, BOX - 40 FT",1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999]
["CSXT-E2L101C8","CSXT",3,"E2L101C8",429,"Spotted-to-Pulled Ratio, BOX - 40 FT",1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.8,1.8,1.8,1.8,1.8,1.8,1.8]
["CSXT-E2L101C12","CSXT",3,"E2L101C12",433,"CD per Interterminal Switch, BOX - 40 FT",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CSXT-E2L101C16","CSXT",3,"E2L101C16",437,"CD per Load & Unload Interterminal Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L101C19","CSXT",3,"E2L101C19",440,"CM per Intraterminal Switch, BOX - 40 FT",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CSXT-E2L101C23","CSXT",3,"E2L101C23",444,"Average Miles between I&I Switches, BOX - 40 FT",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CSXT-E2L101C26","CSXT",3,"E2L101C26",447,"SEMs per Interchange Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E2L101C29","CSXT",3,"E2L101C29",450,"SEMs per I&I Switch, BOX - 40 FT",0,2.08750319480896,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["CSXT-E2L102C1","CSXT",3,"E2L102C1",451,"Average Tare Weight, BOX - 50 FT",33.5,33.900001525878899,34.099998474121101,34.200000762939503,34.5,34.299999237060497,32.599998474121101,32.700000762939503,32.799999237060497,32.799999999999997,32.9,33,33.200000000000003,33.4,33.6,34]
["CSXT-E2L102C4","CSXT",3,"E2L102C4",454,"E/L Ratio, All Freight Cars, BOX - 50 FT",1.67222952842712,1.7296861410141,1.7342956066131601,1.85379791259766,1.78199315071106,1.6999477148055999,1.7269216775894201,1.70006310939789,1.73571705818176,1.8313538270454901,1.82924685824765,1.74804255319149,1.82117800620003,1.98231756574814,1.95330067646373,1.8980000702963]
["CSXT-E2L102C8","CSXT",3,"E2L102C8",458,"Spotted-to-Pulled Ratio, BOX - 50 FT",1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.8,1.8,1.8,1.8,1.8,1.8,1.8]
["CSXT-E2L102C12","CSXT",3,"E2L102C12",462,"CD per Interterminal Switch, BOX - 50 FT",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CSXT-E2L102C15","CSXT",3,"E2L102C15",465,"CD per Load & Unload Intraterminal Switch, BOX - 50 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L102C19","CSXT",3,"E2L102C19",469,"CM per Intraterminal Switch, BOX - 50 FT",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CSXT-E2L102C22","CSXT",3,"E2L102C22",472,"Average CM per CD, Railroad-Owned, BOX - 50 FT",513.59899902343795,575.00164794921898,565.24432373046898,603.20428466796898,572.982666015625,547.36187744140602,607.225341796875,596.57702636718795,526.75726318359398,560.81578840141697,610.86960076797095,775.55981155753705,604.06281591185302,605.17228800243402,612.39455265867798,642.46511684267296]
["CSXT-E2L102C25","CSXT",3,"E2L102C25",475,"SEMs per Industry Switch, BOX - 50 FT",5.7464227676391602,8.3500127792358398,9.0052804946899396,8.9962663650512695,8.7556381225585902,9.1123256683349592,9.1233806610107404,8.8767271041870099,8.8498840332031303,9.3611594740446709,9.1945340497318107,8.80232545825044,6.9356966831961904,6.6890275426386303,6.7289582072708303,6.6922747502017703]
["CSXT-E2L102C26","CSXT",3,"E2L102C26",476,"SEMs per Interchange Switch, BOX - 50 FT",3.16053247451782,4.59250736236572,4.9529051780700701,4.9479470252990696,4.8156008720397896,5.01177883148193,5.0178594589233398,4.8822007179260298,4.8674373626709002,5.1486377107245698,5.0569937273525003,4.8412790020377399,3.8146331757579102,3.6789651484512498,3.7009270139989501,3.6807511126109702]
["CSXT-E2L102C29","CSXT",3,"E2L102C29",479,"SEMs per I&I Switch, BOX - 50 FT",1.4366055727005,2.08750319480896,2.2513201236724898,2.24906706809998,2.1889095306396502,2.2780811786651598,2.28084516525269,2.2191820144653298,2.2124712467193599,2.3402898685111699,2.29863351243295,2.20058136456261,1.73392417079905,1.67225688565966,1.68223955181771,1.6730686875504399]
["CSXT-E2L103C5","CSXT",3,"E2L103C5",484,"Local circuity, BOX - EQUIPPED",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["CSXT-E2L103C8","CSXT",3,"E2L103C8",487,"Spotted-to-Pulled Ratio, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L103C11","CSXT",3,"E2L103C11",490,"CD per Intraterminal Switch, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L103C15","CSXT",3,"E2L103C15",494,"CD per Load & Unload Intraterminal Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L103C18","CSXT",3,"E2L103C18",497,"CM per Interchange Switch, BOX - EQUIPPED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CSXT-E2L103C19","CSXT",3,"E2L103C19",498,"CM per Intraterminal Switch, BOX - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CSXT-E2L103C22","CSXT",3,"E2L103C22",501,"Average CM per CD, Railroad-Owned, BOX - EQUIPPED",513.59899902343795,575.001708984375,565.24432373046898,603.20428466796898,572.982666015625,547.36187744140602,607.22540283203102,596.57702636718795,526.75720214843795,560.81578840141697,610.86960076797095,775.55981155753705,604.06281591185302,605.17228800243402,612.39455265867798,642.46511684267296]
["CSXT-E2L103C25","CSXT",3,"E2L103C25",504,"SEMs per Industry Switch, BOX - EQUIPPED",5.7464222908020002,8.3500127792358398,9.0052795410156303,8.9962673187255895,8.7556371688842791,9.1123256683349592,9.1233806610107404,8.8767271041870099,8.8498849868774396,9.3611594740446797,9.1945340497318107,8.80232545825044,6.9356966831961904,6.6890275426386303,6.7289582072708196,6.6922747502017703]
["CSXT-E2L104C1","CSXT",3,"E2L104C1",509,"Average Tare Weight, GONDOLA - PLAIN",26,25.899999618530298,25.799999237060501,25.600000381469702,25.5,25.600000381469702,25.299999237060501,25.700000762939499,25.700000762939499,25.6,25.6,25.6,25.7,25.9,26.1,26.3]
["CSXT-E2L104C4","CSXT",3,"E2L104C4",512,"E/L Ratio, All Freight Cars, GONDOLA - PLAIN",1.94184374809265,1.9501478672027599,1.94076192378998,1.94345366954803,1.9335247278213501,1.9324022531509399,1.95818996429443,1.9332925081253101,1.92976987361908,1.94936580167016,1.90156995081845,1.85805818765502,1.8446561619009301,1.9224194844709801,1.90704566643996,1.9393742707989099]
["CSXT-E2L104C7","CSXT",3,"E2L104C7",515,"Average circuity, GONDOLA - PLAIN",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["CSXT-E2L104C11","CSXT",3,"E2L104C11",519,"CD per Intraterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L104C14","CSXT",3,"E2L104C14",522,"CD per Load & Unload Industry Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L104C15","CSXT",3,"E2L104C15",523,"CD per Load & Unload Intraterminal Switch, GONDOLA - PLAIN",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L104C18","CSXT",3,"E2L104C18",526,"CM per Interchange Switch, GONDOLA - PLAIN",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CSXT-E2L104C21","CSXT",3,"E2L104C21",529,"CM per I&I Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L104C26","CSXT",3,"E2L104C26",534,"SEMs per Interchange Switch, GONDOLA - PLAIN",3.1605322360992401,4.59250688552856,4.9529047012329102,4.9479470252990696,4.8156008720397896,5.01177883148193,5.0178594589233398,4.8822007179260298,4.8674373626709002,5.1486377107245698,5.0569937273525003,4.8412790020377399,3.8146331757579102,3.6789651484512498,3.7009270139989501,3.6807511126109702]
["CSXT-E2L104C29","CSXT",3,"E2L104C29",537,"SEMs per I&I Switch, GONDOLA - PLAIN",1.43660569190979,2.08750319480896,2.25132036209106,2.24906706809998,2.1889095306396502,2.2780814170837398,2.28084492683411,2.2191822528839098,2.2124714851379399,2.3402898685111699,2.29863351243295,2.20058136456261,1.73392417079905,1.67225688565966,1.68223955181771,1.6730686875504399]
["CSXT-E2L105C3","CSXT",3,"E2L105C3",540,"E/L Ratio, Privately-Owned, GONDOLA - EQUIPPED",1.9073221683502199,1.8378714323043801,1.8012015819549601,1.7848308086395299,1.7364959716796899,1.71204102039337,1.5138645172119101,1.5109457969665501,1.5537592172622701,1.7684039538259499,1.8201480374847201,1.7757891202149101,1.7311220889202501,1.8347312718240401,1.85822533228438,1.8395230806412599]
["CSXT-E2L105C7","CSXT",3,"E2L105C7",544,"Average circuity, GONDOLA - EQUIPPED",1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.119,1.119,1.119,1.119,1.119,1.119,1.119]
["CSXT-E2L105C10","CSXT",3,"E2L105C10",547,"CD per Interchange Switch, GONDOLA - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CSXT-E2L105C11","CSXT",3,"E2L105C11",548,"CD per Intraterminal Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L105C14","CSXT",3,"E2L105C14",551,"CD per Load & Unload Industry Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L105C17","CSXT",3,"E2L105C17",554,"CM per Industry Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L105C22","CSXT",3,"E2L105C22",559,"Average CM per CD, Railroad-Owned, GONDOLA - EQUIPPED",513.59906005859398,575.001708984375,565.24432373046898,603.204345703125,572.98260498046898,547.36193847656295,607.225341796875,596.57708740234398,526.75720214843795,560.81578840141697,610.86960076797095,775.55981155753705,604.06281591185302,605.17228800243402,612.39455265867798,642.46511684267296]
["CSXT-E2L105C25","CSXT",3,"E2L105C25",562,"SEMs per Industry Switch, GONDOLA - EQUIPPED",5.7464227676391602,8.3500137329101598,9.0052804946899396,8.9962663650512695,8.7556381225585902,9.1123256683349592,9.1233797073364293,8.8767271041870099,8.8498849868774396,9.3611594740446797,9.1945340497318107,8.80232545825044,6.9356966831961904,6.6890275426386303,6.7289582072708196,6.6922747502017703]
["CSXT-E2L105C29","CSXT",3,"E2L105C29",566,"SEMs per I&I Switch, GONDOLA - EQUIPPED",1.4366055727005,2.08750319480896,2.2513201236724898,2.2490668296814,2.1889095306396502,2.2780814170837398,2.28084516525269,2.2191822528839098,2.2124714851379399,2.3402898685111699,2.29863351243295,2.20058136456261,1.73392417079905,1.67225688565966,1.68223955181771,1.6730686875504399]
["CSXT-E2L106C3","CSXT",3,"E2L106C3",569,"E/L Ratio, Privately-Owned, HOPPER - COVERED",1.8931734561920199,1.8716782331466699,1.8553496599197401,1.8305957317352299,1.83714735507965,1.84734106063843,1.8717007637023899,1.8919922113418599,1.89180648326874,1.8953324190291001,1.8672427983539099,1.8847157301120301,1.93050162028978,1.9409983732404801,1.91554645546375,1.92826833809761]
["CSXT-E2L106C6","CSXT",3,"E2L106C6",572,"Interline circuity, HOPPER - COVERED",1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999]
["CSXT-E2L106C7","CSXT",3,"E2L106C7",573,"Average circuity, HOPPER - COVERED",1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999]
["CSXT-E2L106C13","CSXT",3,"E2L106C13",579,"CD per I&I Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CSXT-E2L106C14","CSXT",3,"E2L106C14",580,"CD per Load & Unload Industry Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L106C18","CSXT",3,"E2L106C18",584,"CM per Interchange Switch, HOPPER - COVERED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CSXT-E2L106C21","CSXT",3,"E2L106C21",587,"CM per I&I Switch, HOPPER - COVERED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L106C25","CSXT",3,"E2L106C25",591,"SEMs per Industry Switch, HOPPER - COVERED",5.7464227676391602,8.3500137329101598,9.0052804946899396,8.9962663650512695,8.7556381225585902,9.1123266220092791,9.1233806610107404,8.8767280578613299,8.8498840332031303,9.3611594740446797,9.1945340497318107,8.80232545825044,6.9356966831961904,6.6890275426386303,6.7289582072708196,6.6922747502017703]
["CSXT-E2L106C28","CSXT",3,"E2L106C28",594,"SEMs per Interterminal Switch, HOPPER - COVERED",6.8957071304321298,10.020017623901399,10.806337356567401,10.7955207824707,10.506767272949199,10.934791564941399,10.948057174682599,10.6520748138428,10.6198635101318,11.233391368853599,11.033440859678199,10.5627905499005,8.3228360198354299,8.0268330511663599,8.0747498487249896,8.0307297002421194]
["CSXT-E2L107C2","CSXT",3,"E2L107C2",597,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.97876036167145,1.9558192491531401,1.9483001232147199,1.9741958379745499,1.9431337118148799,1.97130823135376,1.9711490869522099,2.0191061496734601,1.99875152111053,2.0111487961315002,2.0770744846161802,1.9603667445938,1.9827720247535501,2.0326198772191799,2.0152101452051601,2.02417574717074]
["CSXT-E2L107C3","CSXT",3,"E2L107C3",598,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - GENERAL",1.9520561695098899,1.9490705728530899,1.93299531936646,1.9715451002121001,1.9568904638290401,1.9151200056076001,1.85185706615448,1.85193395614624,1.82805180549622,1.84155792849424,1.7927899686520401,1.7950060243466699,1.83352360879365,1.87993741554655,1.89696803151049,1.9067683147731]
["CSXT-E2L107C9","CSXT",3,"E2L107C9",604,"CD per Industry Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L107C11","CSXT",3,"E2L107C11",606,"CD per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L107C14","CSXT",3,"E2L107C14",609,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L107C17","CSXT",3,"E2L107C17",612,"CM per Industry Switch, HOPPER - OPEN TOP - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L107C21","CSXT",3,"E2L107C21",616,"CM per I&I Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L107C24","CSXT",3,"E2L107C24",619,"Average Miles between Interchange Switches, HOPPER - OPEN TOP - GENERAL",2724.77026367188,2636.962890625,2812.25512695313,3193.82592773438,5515.97802734375,5548.537109375,2800.68530273438,3594.44848632813,5399.88623046875,6033.70870758208,6207.9254887900197,4217.1177146466398,4264.3402555268804,2190.3803382689298,2349.9490073644702,2482.00521034137]
["CSXT-E2L107C27","CSXT",3,"E2L107C27",622,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",8.6196336746215803,12.5250196456909,13.507922172546399,13.4944000244141,13.1334581375122,13.6684894561768,13.685070991516101,13.315092086791999,13.274828910827599,14.041739211067,13.7918010745977,13.203488187375701,10.403545024794299,10.033541313957899,10.0934373109062,10.038412125302701]
["CSXT-E2L107C28","CSXT",3,"E2L107C28",623,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",6.8957071304321298,10.020015716552701,10.806337356567401,10.795519828796399,10.5067682266235,10.9347925186157,10.948057174682599,10.6520738601685,10.6198625564575,11.233391368853599,11.033440859678199,10.5627905499005,8.3228360198354299,8.0268330511663599,8.0747498487249896,8.0307297002421194]
["CSXT-E2L108C5","CSXT",3,"E2L108C5",629,"Local circuity, HOPPER - OPEN TOP - SPECIAL",1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.202,1.202,1.202,1.202,1.202,1.202,1.202]
["CSXT-E2L108C7","CSXT",3,"E2L108C7",631,"Average circuity, HOPPER - OPEN TOP - SPECIAL",1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001]
["CSXT-E2L108C10","CSXT",3,"E2L108C10",634,"CD per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CSXT-E2L108C13","CSXT",3,"E2L108C13",637,"CD per I&I Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CSXT-E2L108C17","CSXT",3,"E2L108C17",641,"CM per Industry Switch, HOPPER - OPEN TOP - SPECIAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L108C20","CSXT",3,"E2L108C20",644,"CM per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CSXT-E2L108C23","CSXT",3,"E2L108C23",647,"Average Miles between I&I Switches, HOPPER - OPEN TOP - SPECIAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CSXT-E2L108C26","CSXT",3,"E2L108C26",650,"SEMs per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",3.1605322360992401,4.59250736236572,4.9529051780700701,4.9479470252990696,4.8156008720397896,5.0117783546447798,5.0178589820861799,4.8822007179260298,4.8674368858337402,5.1486377107245698,5.0569937273525003,4.8412790020377399,3.8146331757579102,3.6789651484512498,3.7009270139989501,3.6807511126109702]
["CSXT-E2L108C28","CSXT",3,"E2L108C28",652,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",6.8957066535949698,10.020016670227101,10.806337356567401,10.795519828796399,10.5067682266235,10.934791564941399,10.948056221008301,10.6520748138428,10.6198625564575,11.233391368853599,11.033440859678199,10.5627905499005,8.3228360198354299,8.0268330511663599,8.0747498487249896,8.0307297002421194]
["CSXT-E2L109C3","CSXT",3,"E2L109C3",656,"E/L Ratio, Privately-Owned, REFRIGERATED - MECH",1.6282999515533401,1.62934958934784,1.60412085056305,1.5534814596176101,1.51224660873413,1.5032607316970801,1.4403727054595901,1.4527713060378999,1.3982121944427499,1.39787998403335,1.41289189867068,1.3495729350575001,1.3125727025979099,1.2164285714285701,1.2070363399449799,1.22956587636679]
["CSXT-E2L109C6","CSXT",3,"E2L109C6",659,"Interline circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["CSXT-E2L109C9","CSXT",3,"E2L109C9",662,"CD per Industry Switch, REFRIGERATED - MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
[{"$f":"B3586&\"-\"&D3586","v":"CSXT-E2L109C13"},"CSXT",3,"E2L109C13",666,"CD per I&I Switch, REFRIGERATED - MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CSXT-E2L109C16","CSXT",3,"E2L109C16",669,"CD per Load & Unload Interterminal Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L109C17","CSXT",3,"E2L109C17",670,"CM per Industry Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L109C22","CSXT",3,"E2L109C22",675,"Average CM per CD, Railroad-Owned, REFRIGERATED - MECH",513.59906005859398,575.001708984375,565.244384765625,603.20428466796898,572.982666015625,547.36187744140602,607.225341796875,596.57702636718795,526.75720214843795,560.81578840141697,610.86960076797095,775.55981155753705,604.06281591185302,605.17228800243402,612.39455265867798,642.46511684267296]
["CSXT-E2L109C24","CSXT",3,"E2L109C24",677,"Average Miles between Interchange Switches, REFRIGERATED - MECH",1309.06591796875,1348.15209960938,1573.84484863281,1697.28625488281,2150.55102539063,2422.35668945313,1247.79516601563,1357.96533203125,1473.26062011719,1384.21565759963,1278.01120983795,1306.24362701669,1238.77493423333,1194.0493133094701,1163.95693002284,1120.22044097506]
["CSXT-E2L109C28","CSXT",3,"E2L109C28",681,"SEMs per Interterminal Switch, REFRIGERATED - MECH",6.8957066535949698,10.020015716552701,10.806337356567401,10.795519828796399,10.5067682266235,10.934790611267101,10.948056221008301,10.652075767517101,10.6198635101318,11.233391368853599,11.033440859678199,10.5627905499005,8.3228360198354299,8.0268330511663599,8.0747498487249896,8.0307297002421194]
["CSXT-E2L110C2","CSXT",3,"E2L110C2",684,"E/L Ratio, Railroad-Owned, REFRIGERATED - NON-MECH",1.96744585037231,1.9809812307357799,2.0348472595214799,1.9998418092727701,2.0089743137359601,1.99385643005371,2.0106964111328098,1.94227302074432,1.93613493442535,2.03864311942647,1.9571505088377099,1.98770355599867,2.0044905008635601,1.99754601226994,1.95040871934605,1.96946564885496]
["CSXT-E2L110C5","CSXT",3,"E2L110C5",687,"Local circuity, REFRIGERATED - NON-MECH",1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001]
["CSXT-E2L110C9","CSXT",3,"E2L110C9",691,"CD per Industry Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L110C12","CSXT",3,"E2L110C12",694,"CD per Interterminal Switch, REFRIGERATED - NON-MECH",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CSXT-E2L110C13","CSXT",3,"E2L110C13",695,"CD per I&I Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CSXT-E2L110C18","CSXT",3,"E2L110C18",700,"CM per Interchange Switch, REFRIGERATED - NON-MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CSXT-E2L110C20","CSXT",3,"E2L110C20",702,"CM per Interterminal Switch, REFRIGERATED - NON-MECH",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CSXT-E2L110C24","CSXT",3,"E2L110C24",706,"Average Miles between Interchange Switches, REFRIGERATED - NON-MECH",1255.13854980469,1390.02331542969,1025.70397949219,1105.11608886719,1517.52075195313,1729.35986328125,1093.33312988281,1006.69067382813,1226.0302734375,1228.12323612418,1265.1982047609299,1041.21422558923,1021.05787776915,959.399226389354,1033.72119742729,1272.3689969438301]
["CSXT-E2L110C27","CSXT",3,"E2L110C27",709,"SEMs per Intraterminal Switch, REFRIGERATED - NON-MECH",8.6196336746215803,12.5250196456909,13.5079202651978,13.4943990707397,13.1334571838379,13.6684875488281,13.6850700378418,13.315091133117701,13.274827003479,14.041739211067,13.7918010745977,13.203488187375701,10.403545024794299,10.033541313957899,10.0934373109062,10.038412125302701]
["CSXT-E2L111C2","CSXT",3,"E2L111C2",713,"E/L Ratio, Railroad-Owned, FLAT - TOFC",1.1986788511276201,1.1692043542861901,1.1380541324615501,1.10578513145447,1.0865228176116899,1.12581598758698,1.1331865787506099,1.1456332206726101,1.10938549041748,1.1036859294807699,1.1160335335006499,1.1146472921036901,1.10195021651765,1.0932455413596101,1.1030057230408701,1.0997684391971201]
["CSXT-E2L111C5","CSXT",3,"E2L111C5",716,"Local circuity, FLAT - TOFC",1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.069,1.069,1.069,1.069,1.069,1.069,1.069]
["CSXT-E2L111C8","CSXT",3,"E2L111C8",719,"Spotted-to-Pulled Ratio, FLAT - TOFC",1.17796170711517,1.1532630920410201,1.1331744194030799,1.10098648071289,1.07988500595093,1.1102989912033101,1.11265456676483,1.11915147304535,1.10285556316376,1.0999691070931501,1.0969488255601401,1.09264013021549,1.08979697977228,1.0864663585002601,1.0881558021708699,1.09569539046412]
["CSXT-E2L111C9","CSXT",3,"E2L111C9",720,"CD per Industry Switch, FLAT - TOFC",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L111C14","CSXT",3,"E2L111C14",725,"CD per Load & Unload Industry Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L111C16","CSXT",3,"E2L111C16",727,"CD per Load & Unload Interterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L111C20","CSXT",3,"E2L111C20",731,"CM per Interterminal Switch, FLAT - TOFC",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["CSXT-E2L111C23","CSXT",3,"E2L111C23",734,"Average Miles between I&I Switches, FLAT - TOFC",4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162]
["CSXT-E2L111C27","CSXT",3,"E2L111C27",738,"SEMs per Intraterminal Switch, FLAT - TOFC",8.6196336746215803,12.5250196456909,13.507921218872101,13.4944000244141,13.1334590911865,13.6684894561768,13.6850700378418,13.315091133117701,13.274827957153301,14.041739211067,13.7918010745977,13.203488187375701,10.403545024794299,10.033541313957899,10.0934373109062,10.038412125302701]
["CSXT-E2L112C1","CSXT",3,"E2L112C1",741,"Average Tare Weight, FLAT - MULTILEVEL",54.299999237060497,54.299999237060497,54.200000762939503,54.400001525878899,54.900001525878899,54.5,54,54,53.799999237060497,53.6,53.6,53.4,53.3,53.1,53.1,53.1]
["CSXT-E2L112C4","CSXT",3,"E2L112C4",744,"E/L Ratio, All Freight Cars, FLAT - MULTILEVEL",1.5364578962326001,1.53766930103302,1.5408681631088299,1.5881867408752399,1.5674979686737101,1.5495356321334799,1.5506317615509,1.5705636739730799,1.5400861501693699,1.5076492873895,1.4767124649334,1.5299370047104,1.55134793287544,1.5743886825689399,1.57123260171306,1.57714209449239]
["CSXT-E2L112C6","CSXT",3,"E2L112C6",746,"Interline circuity, FLAT - MULTILEVEL",1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999]
["CSXT-E2L112C9","CSXT",3,"E2L112C9",749,"CD per Industry Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L112C12","CSXT",3,"E2L112C12",752,"CD per Interterminal Switch, FLAT - MULTILEVEL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CSXT-E2L112C16","CSXT",3,"E2L112C16",756,"CD per Load & Unload Interterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L112C19","CSXT",3,"E2L112C19",759,"CM per Intraterminal Switch, FLAT - MULTILEVEL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CSXT-E2L112C23","CSXT",3,"E2L112C23",763,"Average Miles between I&I Switches, FLAT - MULTILEVEL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CSXT-E2L112C26","CSXT",3,"E2L112C26",766,"SEMs per Interchange Switch, FLAT - MULTILEVEL",3.1605322360992401,4.59250736236572,4.9529051780700701,4.9479465484619096,4.8156013488769496,5.01177883148193,5.0178594589233398,4.8822002410888699,4.8674368858337402,5.1486377107245698,5.0569937273525003,4.8412790020377399,3.8146331757579102,3.6789651484512498,3.7009270139989501,3.6807511126109702]
["CSXT-E2L112C29","CSXT",3,"E2L112C29",769,"SEMs per I&I Switch, FLAT - MULTILEVEL",1.4366055727005,2.08750319480896,2.2513198852539098,2.24906706809998,2.1889095306396502,2.2780811786651598,2.28084492683411,2.2191820144653298,2.2124714851379399,2.3402898685111699,2.29863351243295,2.20058136456261,1.73392417079905,1.67225688565966,1.68223955181771,1.6730686875504399]
["CSXT-E2L113C2","CSXT",3,"E2L113C2",771,"E/L Ratio, Railroad-Owned, FLAT - GENERAL",1.72102999687195,1.9842271804809599,1.89247310161591,1.9051988124847401,2.1049382686614999,1.9390244483947801,1.9530200958252,1.88145899772644,2.0662982463836701,2.0238095238095202,1.91588785046729,1.8217054263565899,1.95744680851064,2.1025641025641,1.9328358208955201,1.9734513274336301]
["CSXT-E2L113C5","CSXT",3,"E2L113C5",774,"Local circuity, FLAT - GENERAL",1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001]
["CSXT-E2L113C9","CSXT",3,"E2L113C9",778,"CD per Industry Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L113C12","CSXT",3,"E2L113C12",781,"CD per Interterminal Switch, FLAT - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["CSXT-E2L113C15","CSXT",3,"E2L113C15",784,"CD per Load & Unload Intraterminal Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L113C19","CSXT",3,"E2L113C19",788,"CM per Intraterminal Switch, FLAT - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CSXT-E2L113C22","CSXT",3,"E2L113C22",791,"Average CM per CD, Railroad-Owned, FLAT - GENERAL",513.59899902343795,575.00164794921898,565.24426269531295,603.204345703125,572.982666015625,547.36193847656295,607.225341796875,596.57702636718795,526.75720214843795,560.81578840141697,610.86960076797095,775.55981155753705,604.06281591185302,605.17228800243402,612.39455265867798,642.46511684267296]
[{"$f":"B3714&\"-\"&D3714","v":"CSXT-E2L113C25"},"CSXT",3,"E2L113C25",794,"SEMs per Industry Switch, FLAT - GENERAL",5.7464222908020002,8.3500127792358398,9.0052804946899396,8.9962663650512695,8.7556381225585902,9.1123256683349592,9.1233806610107404,8.8767271041870099,8.8498849868774396,9.3611594740446797,9.1945340497318107,8.80232545825044,6.9356966831961904,6.6890275426386303,6.7289582072708303,6.6922747502017703]
["CSXT-E2L113C27","CSXT",3,"E2L113C27",796,"SEMs per Intraterminal Switch, FLAT - GENERAL",8.6196336746215803,12.5250186920166,13.507922172546399,13.4943990707397,13.1334581375122,13.668488502502401,13.6850700378418,13.315091133117701,13.274827003479,14.041739211067,13.7918010745977,13.203488187375701,10.403545024794299,10.033541313957899,10.0934373109062,10.038412125302701]
["CSXT-E2L114C1","CSXT",3,"E2L114C1",799,"Average Tare Weight, FLAT - OTHER",34.599998474121101,34.599998474121101,34.700000762939503,34.700000762939503,34.700000762939503,34.700000762939503,35.099998474121101,35.200000762939503,35.200000762939503,35.299999999999997,35.299999999999997,35.299999999999997,35.4,35.299999999999997,35.4,35.4]
["CSXT-E2L114C5","CSXT",3,"E2L114C5",803,"Local circuity, FLAT - OTHER",1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001]
["CSXT-E2L114C8","CSXT",3,"E2L114C8",806,"Spotted-to-Pulled Ratio, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L114C11","CSXT",3,"E2L114C11",809,"CD per Intraterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L114C15","CSXT",3,"E2L114C15",813,"CD per Load & Unload Intraterminal Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L114C18","CSXT",3,"E2L114C18",816,"CM per Interchange Switch, FLAT - OTHER",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CSXT-E2L114C19","CSXT",3,"E2L114C19",817,"CM per Intraterminal Switch, FLAT - OTHER",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CSXT-E2L114C23","CSXT",3,"E2L114C23",821,"Average Miles between I&I Switches, FLAT - OTHER",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["CSXT-E2L114C26","CSXT",3,"E2L114C26",824,"SEMs per Interchange Switch, FLAT - OTHER",3.1605319976806601,4.59250736236572,4.9529047012329102,4.9479465484619096,4.8156013488769496,5.01177883148193,5.0178594589233398,4.8822007179260298,4.8674368858337402,5.1486377107245698,5.0569937273525003,4.8412790020377399,3.8146331757579102,3.6789651484512498,3.7009270139989501,3.6807511126109702]
["CSXT-E2L115C1","CSXT",3,"E2L115C1",828,"Average Tare Weight, TANK <22,000 GAL",31.7,32.700000000000003,32.6,32.6,32.6,32.6,32.6,32.6,32.6,32.700000000000003,32.700000000000003,32.799999999999997,32.799999999999997,32.9,32.9,32.9]
["CSXT-E2L115C4","CSXT",3,"E2L115C4",831,"E/L Ratio, All Freight Cars, TANK <22,000 GAL",1.96557712554932,1.97780108451843,1.97714984416962,1.98369693756104,1.97300565242767,1.9765878915786701,2.0074985027313201,1.99693095684052,1.97824418544769,1.9789780363940701,1.9749070230996899,1.9765520004674599,1.97993558456556,1.97287586238829,1.9673315635983,1.9658173733064599]
["CSXT-E2L115C7","CSXT",3,"E2L115C7",834,"Average circuity, TANK <22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["CSXT-E2L115C11","CSXT",3,"E2L115C11",838,"CD per Intraterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L115C14","CSXT",3,"E2L115C14",841,"CD per Load & Unload Industry Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L115C15","CSXT",3,"E2L115C15",842,"CD per Load & Unload Intraterminal Switch, TANK <22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L115C19","CSXT",3,"E2L115C19",846,"CM per Intraterminal Switch, TANK <22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["CSXT-E2L115C22","CSXT",3,"E2L115C22",849,"Average CM per CD, Railroad-Owned, TANK <22,000 GAL",513.59906005859398,575.00164794921898,565.24426269531295,603.20428466796898,572.98260498046898,547.36187744140602,607.225341796875,596.57702636718795,526.75726318359398,560.81578840141697,610.86960076797095,775.55981155753705,604.06281591185302,605.17228800243402,612.39455265867798,642.46511684267296]
["CSXT-E2L115C26","CSXT",3,"E2L115C26",853,"SEMs per Interchange Switch, TANK <22,000 GAL",3.1605322360992401,4.59250736236572,4.9529047012329102,4.9479470252990696,4.8156013488769496,5.01177883148193,5.0178594589233398,4.8822007179260298,4.8674368858337402,5.1486377107245698,5.0569937273525003,4.8412790020377399,3.8146331757579102,3.6789651484512498,3.7009270139989501,3.6807511126109702]
["CSXT-E2L115C29","CSXT",3,"E2L115C29",856,"SEMs per I&I Switch, TANK <22,000 GAL",1.43660569190979,2.08750319480896,2.2513201236724898,2.2490668296814,2.1889095306396502,2.2780811786651598,2.28084492683411,2.2191822528839098,2.2124714851379399,2.3402898685111699,2.29863351243295,2.20058136456261,1.73392417079905,1.67225688565966,1.68223955181771,1.6730686875504399]
["CSXT-E2L116C3","CSXT",3,"E2L116C3",859,"E/L Ratio, Privately-Owned, TANK >=22,000 GAL",1.99648225307465,2.0104773044586199,1.99414598941803,1.99218821525574,1.97075247764587,1.97182881832123,1.99861299991608,1.9930397272110001,1.96980535984039,1.95796969755203,1.9900064638178501,1.9811442483675701,1.98112887913236,1.9892325015583201,1.9864472645998701,1.9814917507471399]
["CSXT-E2L116C7","CSXT",3,"E2L116C7",863,"Average circuity, TANK >=22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["CSXT-E2L116C10","CSXT",3,"E2L116C10",866,"CD per Interchange Switch, TANK >=22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CSXT-E2L116C11","CSXT",3,"E2L116C11",867,"CD per Intraterminal Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L116C15","CSXT",3,"E2L116C15",871,"CD per Load & Unload Intraterminal Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L116C18","CSXT",3,"E2L116C18",874,"CM per Interchange Switch, TANK >=22,000 GAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CSXT-E2L116C22","CSXT",3,"E2L116C22",878,"Average CM per CD, Railroad-Owned, TANK >=22,000 GAL",513.59906005859398,575.00164794921898,565.24426269531295,603.20428466796898,572.98260498046898,547.36187744140602,607.225341796875,596.57702636718795,526.75726318359398,560.81578840141697,610.86960076797095,775.55981155753705,604.06281591185302,605.17228800243402,612.39455265867798,642.46511684267296]
["CSXT-E2L116C25","CSXT",3,"E2L116C25",881,"SEMs per Industry Switch, TANK >=22,000 GAL",5.7464227676391602,8.3500127792358398,9.0052804946899396,8.9962663650512695,8.7556371688842791,9.1123256683349592,9.1233806610107404,8.8767271041870099,8.8498849868774396,9.3611594740446709,9.1945340497318107,8.80232545825044,6.9356966831962001,6.6890275426386303,6.7289582072708303,6.6922747502017703]
["CSXT-E2L116C29","CSXT",3,"E2L116C29",885,"SEMs per I&I Switch, TANK >=22,000 GAL",1.43660569190979,2.08750319480896,2.2513201236724898,2.2490668296814,2.1889095306396502,2.2780811786651598,2.28084492683411,2.2191822528839098,2.2124714851379399,2.3402898685111699,2.29863351243295,2.20058136456261,1.73392417079905,1.67225688565966,1.68223955181771,1.6730686875504399]
["CSXT-E2L117C3","CSXT",3,"E2L117C3",888,"E/L Ratio, Privately-Owned, ALL OTHER FREIGHT CARS",1.5799312591552701,1.6321169137954701,1.70113790035248,1.38680839538574,1.5632858276367201,1.22984111309052,1.2080103158950799,1.1804586648941,1.19218194484711,1.3299232736572899,1.3820005989817301,1.39218114275606,1.5868621064060799,1.5889285714285699,1.5476067936181199,1.5734250698774499]
["CSXT-E2L117C6","CSXT",3,"E2L117C6",891,"Interline circuity, ALL OTHER FREIGHT CARS",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["CSXT-E2L117C7","CSXT",3,"E2L117C7",892,"Average circuity, ALL OTHER FREIGHT CARS",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["CSXT-E2L117C11","CSXT",3,"E2L117C11",896,"CD per Intraterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L117C14","CSXT",3,"E2L117C14",899,"CD per Load & Unload Industry Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L117C18","CSXT",3,"E2L117C18",903,"CM per Interchange Switch, ALL OTHER FREIGHT CARS",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["CSXT-E2L117C21","CSXT",3,"E2L117C21",906,"CM per I&I Switch, ALL OTHER FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L117C25","CSXT",3,"E2L117C25",910,"SEMs per Industry Switch, ALL OTHER FREIGHT CARS",5.7464227676391602,8.3500127792358398,9.0052804946899396,8.9962663650512695,8.7556371688842791,9.1123256683349592,9.1233806610107404,8.8767271041870099,8.8498849868774396,9.3611594740446709,9.1945340497318107,8.80232545825044,6.9356966831962001,6.6890275426386303,6.7289582072708303,6.6922747502017703]
["CSXT-E2L117C28","CSXT",3,"E2L117C28",913,"SEMs per Interterminal Switch, ALL OTHER FREIGHT CARS",6.8957066535949698,10.020016670227101,10.8063364028931,10.7955207824707,10.506767272949199,10.934790611267101,10.948056221008301,10.6520748138428,10.6198635101318,11.233391368853599,11.033440859678199,10.5627905499005,8.3228360198354299,8.0268330511663599,8.0747498487249896,8.0307297002421194]
["CSXT-E2L118C3","CSXT",3,"E2L118C3",917,"E/L Ratio, Privately-Owned, AVERAGE ALL FREIGHT CARS",1.7294389009475699,1.7462234497070299,1.75147116184235,1.74990487098694,1.7200893163680999,1.7099683284759499,1.68423187732697,1.6935223340988199,1.6813155412673999,1.66854953182324,1.6445097768922801,1.66582680750227,1.67117490638569,1.71469124474918,1.7002864465551,1.7193744390747501]
["CSXT-E2L118C4","CSXT",3,"E2L118C4",918,"E/L Ratio, All Freight Cars, AVERAGE ALL FREIGHT CARS",1.77560269832611,1.7867248058319101,1.78703117370605,1.78599500656128,1.75515902042389,1.7446697950363199,1.7331683635711701,1.73755538463593,1.7177300453186,1.7071454303801299,1.67828224381035,1.6952752235172801,1.6944690296057101,1.7386550271282399,1.7244754951577299,1.74440823094743]
["CSXT-E2L118C7","CSXT",3,"E2L118C7",921,"Average circuity, AVERAGE ALL FREIGHT CARS",1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.135,1.135,1.135,1.135,1.135,1.135,1.135]
["CSXT-E2L118C10","CSXT",3,"E2L118C10",924,"CD per Interchange Switch, AVERAGE ALL FREIGHT CAR",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["CSXT-E2L118C14","CSXT",3,"E2L118C14",928,"CD per Load & Unload Industry Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["CSXT-E2L118C17","CSXT",3,"E2L118C17",931,"CM per Industry Switch, AVERAGE ALL FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["CSXT-E2L118C21","CSXT",3,"E2L118C21",935,"CM per I&I Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["CSXT-E2L118C24","CSXT",3,"E2L118C24",938,"Average Miles between Interchange Switches, AVERAGE ALL FREIGHT CARS",2556.44458007813,2498.76049804688,2522.59252929688,2639.54052734375,2963.89575195313,2910.58618164063,1711.25500488281,1752.24792480469,1726.08850097656,1868.98564802082,1868.8976550816301,2027.9057781868901,1941.1202095558201,1769.3011393649599,1737.16632671906,1681.7869371510401]
["CSXT-E2L118C28","CSXT",3,"E2L118C28",942,"SEMs per Interterminal Switch, AVERAGE ALL FREIGHT CARS",6.8957066535949698,10.020017623901399,10.806337356567401,10.7955226898193,10.506767272949199,10.9347925186157,10.948057174682599,10.652075767517101,10.6198635101318,11.233391368853599,11.033440859678199,10.5627905499005,8.3228360198354405,8.0268330511663599,8.0747498487249896,8.0307297002421194]
["CSXT-E2L118C29","CSXT",3,"E2L118C29",943,"SEMs per I&I Switch, AVERAGE ALL FREIGHT CARS",1.4366055727005,2.08750319480896,2.2513201236724898,2.2490668296814,2.1889095306396502,2.2780814170837398,2.28084492683411,2.2191820144653298,2.2124714851379399,2.3402898685111699,2.29863351243295,2.20058136456261,1.73392417079905,1.67225688565966,1.68223955181771,1.6730686875504399]
["CSXT-E2L203C1","CSXT",3,"E2L203C1",946,"Average Tare Weight - Refrigerated TCU",7.3000001907348597,7.3000001907348597,7.1999998092651403,7.0999999046325701,7,7.0999999046325701,6.9000000953674299,6.9000000953674299,6.9000000953674299,6.9,6.9,6.8,6.9,6.9,7.1,7.1]
["CSXT-E2L207C1","CSXT",3,"E2L207C1",950,"L/E Ratio - Refrigerated/Non-Refrigerated - TCU",1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33,1.33,1.33,1.33,1.33,1.33,1.33]
["CSXT-E2L210C1","CSXT",3,"E2L210C1",953,"Average Locomotive Units - Through Train",2.5516529083252002,2.5229566097259499,2.5387344360351598,2.5306301116943399,2.5126411914825399,2.4860711097717298,2.4842209815978999,2.44139456748962,2.4427752494811998,2.5903318520041601,2.6583696228458802,2.4965857844712001,2.4400489224993498,2.1566192264007098,2.22300091519261,2.20169534413031]
["CSXT-E2L213C1","CSXT",3,"E2L213C1",956,"Average Gross Tons - Through Train",4828.728515625,4868.4755859375,4951.59716796875,5172.91552734375,5267.84326171875,4937.9794921875,4769.25146484375,4960.26123046875,5248.03076171875,5509.5661347886698,6173.1441668571297,6202.0249054431597,6655.2583356996201,6640.9998381776904,7540.2103477099299,7787.4300981507904]
["CSXT-E2L217C1","CSXT",3,"E2L217C1",960,"Train Miles - Running",97268.8359375,92910.7109375,89363.6015625,73891.5234375,78965.078125,82646.859375,83119.3828125,83853.375,86046.453125,79714.472999999998,67611.811000000002,67619.831999999995,64389.798999999999,61671.368000000002,52903.362000000001,53019.754999999997]
["CSXT-E2L220C1","CSXT",3,"E2L220C1",963,"Constant Cost Markup Ratio",1.4039988517761199,1.39784467220306,1.38793349266052,1.4479384422302199,1.41917312145233,1.38268601894379,1.3738545179367101,1.3775217533111599,1.3716006278991699,1.3901513588748899,1.406293253599,1.4212475386474701,1.4389224342772899,1.4318180526867501,1.4654006678153999,1.4666669523521201]
["CSXT-E2L302C2","CSXT",3,"E2L302C2",967,"Residual Factor, Station Clerical, Privately-Owned",2.9622011609224601,3.9872704961030201,4.7208652820290498,5.4579956322926799,4.5567444836390898,4.7429474665180296,4.1470643972189301,4.6434095471941861,4.8865998338534604,3.1961080546751899,3.2630791472364198,2.9793293678278001,2.4347860006274402,3.72126319939151,2.3798496029162228,2.0450630128260898]
["CSXT-E2L303C1","CSXT",3,"E2L303C1",968,"Residual Factor, Interchange Switching, Railroad-Owned",5.2861327762911801,6.9955494257434001,7.5931312211075301,8.3364167906493503,7.4632752703764602,8.2470868594541002,7.4383113272722499,8.5160659759271056,11.2620566719006,10.9743097447301,8.7132852739338293,8.2408558592547205,6.7028558460381298,6.22006507457845,6.3654768333068077,6.6701792142740004]
["CSXT-E2L304C2","CSXT",3,"E2L304C2",971,"Residual Factor, I&I Switching, Privately-Owned",28.749138415797798,38.203164467647902,45.489293849940999,51.771409751200302,50.5292175028396,50.989066238229299,43.659992455702998,42.641957567951913,48.512103919612002,43.975248404022501,35.441117987529097,33.424695003677101,29.4386146944742,25.898899304272899,23.13189972145371,23.262308197461]
["EAST-E1L101C2","EAST",8,"E1L101C2",2,"Gross Ton Mile (GTM), DRL Expense",8.8091992074623704E-4,9.50137502513826E-4,9.8456896375864701E-4,1.21120945550501E-3,1.0933541925624E-3,1.10231433063745E-3,1.2160019250586601E-3,1.16154574789107E-3,1.14883983042091E-3,1.2449528881579199E-3,1.4004073380556299E-3,1.3822096084742299E-3,1.4138551152026099E-3,1.50910739397405E-3,1.73004531518911E-3,1.6996869206180099E-3]
["EAST-E1L102C2","EAST",8,"E1L102C2",5,"Car Mile (CM) - Other Than Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L103C2","EAST",8,"E1L103C2",8,"Train Mile (TM) - Other Than Crew, DRL Expense",4.7652637585997599E-3,4.64695319533348E-3,4.4082347303628904E-3,3.8302873726934199E-3,2.8872641269117598E-3,3.06407897733152E-3,3.2112565822899298E-3,2.5560527574270998E-3,2.0297530572861398E-3,5.1503476828025901E-4,6.0365549392981299E-4,1.3448568017140801E-3,1.1815787156133799E-3,2.0257218486669001E-3,1.1270517411956899E-3,-7.3566659384587601E-5]
["EAST-E1L104C3","EAST",8,"E1L104C3",12,"Train Mile (TM) - Crew, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L105C3","EAST",8,"E1L105C3",15,"Locomotive Unit Mile (LUM), ROI Expense",0.575414478778839,0.75032073259353604,0.90585750341415405,0.92376846075057995,0.924013912677765,0.94674700498580899,0.95568263530731201,0.93385756015777599,0.91480731964111295,0.92699764070375101,1.0464940571360699,1.2488894450581001,1.5511287953680799,1.3570955565743501,1.30966515242115,1.8162318614985999]
["EAST-E1L107C1","EAST",8,"E1L107C1",19,"CLOR (Carloads Handled) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L107C2","EAST",8,"E1L107C2",20,"CLOR (Carloads Handled) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L108C2","EAST",8,"E1L108C2",23,"CLOT (Carloads Orig Or Term) - Other, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L109C3","EAST",8,"E1L109C3",27,"CLOT (Carloads Orig Or Term) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L110C3","EAST",8,"E1L110C3",30,"Car Mile (CM) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L111C3","EAST",8,"E1L111C3",33,"Switch Engine Minutes (SEM), ROI Expense",1.0902738571167001,1.10986864566803,1.1937328577041599,1.3342529535293599,1.4161679744720499,1.4396226406097401,1.432732462883,1.5149393081664999,1.4136253595352199,1.34163945715794,1.3679530202211601,1.5747938405480799,1.8830575239334999,1.55632120295164,1.50919585805866,2.0057367489228199]
["EAST-E1L113C1","EAST",8,"E1L113C1",37,"Tons Handled at Coal Terminals, OPR Expense",1.4208467006683301,1.47167491912842,1.6112157106399501,1.80966985225677,1.5917432308196999,1.77073574066162,2.0600607395172101,2.0109825134277299,2.2549247741699201,2.7035427252052,2.4738466845876501,2.2278710212195398,1.8462387743213899,2.1042063617777398,1.92763020873292,2.0285855457055799]
["EAST-E1L114C1","EAST",8,"E1L114C1",40,"Tons Handled at Ore Terminals, OPR Expense",0.90506565570831299,0.83270150423049905,0.80333673954009999,1.1158304214477499,4.3264307975768999,5.1262702941894496,0.85121041536331199,1.27582335472107,1.30250799655914,1.30213491851249,1.52584270128415,0.88389914291577998,0.912449038722151,0.81463240234242495,0.70741711223569503,0.65748893908537598]
["EAST-E1L114C3","EAST",8,"E1L114C3",42,"Tons Handled at Ore Terminals, ROI Expense",0.17888127267360701,0.20866499841213201,0.27359920740127602,0.37800744175911,0.25970014929771401,0.30404397845268299,0.32936251163482699,0.337456345558167,0.31936538219451899,0.34070401153696001,0.28808826568171703,0.25038655331427201,0.235246906243543,0.15598144801483399,0.14104980587447999,0.13048142697966]
["EAST-E1L115C3","EAST",8,"E1L115C3",45,"Tons Handled at Other Marine Terminals, ROI Expense",0.14305019378662101,0.150401040911675,0.165297776460648,0.3101666867733,0.170025110244751,0.18691097199916801,0.884981989860535,0.828557670116425,1.08246302604675,0.85915817732046496,0.22501709457406599,0.313117838754842,0.40146550996778801,0.34855023702146698,0.18265609942210601,0.25627199085570701]
["EAST-E1L116C3","EAST",8,"E1L116C3",48,"Refrigerated Car Miles, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L118C1","EAST",8,"E1L118C1",52,"Refrigerated TCU Days, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L119C1","EAST",8,"E1L119C1",55,"Other (Non-Refrigerated) TCU Days, OPR Expense",3.4202032089233398,3.82561182975769,5.1321034431457502,4.3333373069763201,3.7116899490356401,3.4992372989654501,3.4074635505676301,3.3369789123535201,3.25893235206604,3.1808780250514199,3.12657899571292,3.6242794562591598,3.7033715796056299,3.70702749542549,3.23155517553755,3.5238806685994999]
["EAST-E1L120C1","EAST",8,"E1L120C1",58,"TCUs Loaded And Unloaded (L&UL), OPR Expense",34.490646362304702,35.4869995117188,50.368251800537102,37.009567260742202,59.679523468017599,109.689483642578,114.558486938477,109.47713470459,103.24137878418,98.638457573275204,101.83258952585901,96.2000058679548,94.264687889953507,100.65645638293999,93.732143249067803,95.753278872665206]
["EAST-E1L121C2","EAST",8,"E1L121C2",62,"MVUs Loaded And Unloaded (L&UL), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L122C2","EAST",8,"E1L122C2",65,"TCUs Picked Up and Delivered (PU&D), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L201C1","EAST",8,"E1L201C1",67,"CM(R), OPR Expense, Railroad-Owned, BOX - 40 FT",1.90927069634199E-2,6.2973671592771998E-3,7.5599798001348998E-3,1.26231098547578E-2,1.63268037140369E-2,1.94918476045132E-2,1.9149050116539001E-2,1.9068850204348599E-2,1.8148085102438899E-2,2.0522178638088698E-2,2.2176655877091101E-2,2.2261952055891099E-2,1.9516902785043699E-2,1.6163782884431599E-2,1.38527386262153E-2,1.2408754156967501E-2]
["EAST-E1L201C4","EAST",8,"E1L201C4",70,"CM(Y), OPR Expense, Railroad-Owned, BOX - 40 FT",4.9641050398349797E-2,1.6373159363865901E-2,1.9655957818031301E-2,3.2820105552673298E-2,4.2449768632650403E-2,5.0678897649049801E-2,4.9787536263465902E-2,4.95790541172028E-2,4.71849851310253E-2,5.3357664459030799E-2,5.7659305280437001E-2,5.78810753453168E-2,5.0743947241113703E-2,4.2025835499522102E-2,3.601712042816E-2,3.2262760808115402E-2]
["EAST-E1L201C7","EAST",8,"E1L201C7",73,"CD(R), OPR Expense, Railroad-Owned, BOX - 40 FT",2.3279886245727499,0.77002650499343905,0.94257891178131104,1.5879892110824601,2.0698201656341602,2.4577054977417001,2.4156017303466801,2.4055032730102499,2.2687449455261199,2.5490102319241101,2.74764887695477,2.8240541918644801,2.5449851297641302,2.165575025966,1.88309601358127,1.71860719766855]
[{"$f":"B3970&\"-\"&D3970","v":"EAST-E1L201C11"},"EAST",8,"E1L201C11",77,"CD(Y), DRL Expense, Railroad-Owned, BOX - 40 FT",114.36208343505901,76.141914367675795,87.511505126953097,62.329051971435497,53.166210174560497,51.727634429931598,43.912300109863303,30.453620910644499,37.289009094238303,38.417408920719502,33.126309702771302,35.648777400850499,50.452400579139599,53.888838540464498,50.916595369132203,53.636584931774003]
["EAST-E1L202C1","EAST",8,"E1L202C1",80,"CM(R), OPR Expense, Railroad-Owned, BOX - 50 FT",1.90927069634199E-2,6.2973671592771998E-3,7.5599798001348998E-3,1.26231098547578E-2,1.63268037140369E-2,1.94918476045132E-2,1.9149050116539001E-2,1.9068850204348599E-2,1.8148085102438899E-2,2.0522178638088698E-2,2.2176655877091101E-2,2.2261952055891099E-2,1.9516902785043699E-2,1.6163782884431599E-2,1.38527386262153E-2,1.2408754156967501E-2]
["EAST-E1L202C5","EAST",8,"E1L202C5",84,"CM(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",0.56627780199050903,0.36093232035636902,0.41116973757743802,0.21536169946193701,0.220783621072769,0.21017549932002999,0.21140247583389299,0.17237316071987199,0.21029540896415699,0.23663533105655299,0.207009688171432,0.209372784909649,0.23092932344389899,0.196793121132018,0.19403098430653801,0.19845478297209501]
["EAST-E1L202C8","EAST",8,"E1L202C8",87,"CD(R), DRL Expense, Railroad-Owned, BOX - 50 FT",114.36208343505901,76.141921997070298,87.511505126953097,62.329051971435497,53.166206359863303,51.727634429931598,43.912303924560497,30.453619003295898,37.289012908935497,38.417408920719502,33.126309702771302,35.648777400850499,50.452400579139599,53.888838540464498,50.916595369132203,53.636584931774003]
["EAST-E1L202C11","EAST",8,"E1L202C11",90,"CD(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",114.36208343505901,76.141914367675795,87.511505126953097,62.329051971435497,53.166210174560497,51.727634429931598,43.912300109863303,30.453620910644499,37.289009094238303,38.417408920719502,33.126309702771302,35.648777400850499,50.452400579139599,53.888838540464498,50.916595369132203,53.636584931774003]
["EAST-E1L202C13","EAST",8,"E1L202C13",92,"CM(R), DRL Expense, Privately-Owned, BOX - 50 FT",0.521784126758575,0.48545575141906699,0.53531265258789096,0.84295159578323398,0.44607910513877902,0.475842446088791,0.54120123386383101,0.571602642536163,0.54070335626602195,0.53421858723121696,0.69438094707430797,0.76434363700330299,0.75342774502748699,0.99324295597262002,0.98136653224862702,0.91619023950951795]
["EAST-E1L203C3","EAST",8,"E1L203C3",95,"CM(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED",2.06557139754295E-2,2.7247117832302999E-2,3.3858913928270298E-2,3.8910508155822802E-2,4.0403347462415702E-2,4.48110140860081E-2,4.69247028231621E-2,4.2434126138687099E-2,3.0467130243778201E-2,2.39870967088117E-2,2.64983430142453E-2,3.0139649022851499E-2,3.4296458016688902E-2,3.0573313061652101E-2,2.7351279492351398E-2,3.4419243401697899E-2]
["EAST-E1L203C6","EAST",8,"E1L203C6",98,"CM(Y), ROI Expense, Railroad-Owned, BOX - EQUIPPED",5.3704891353845603E-2,7.0842534303665203E-2,8.8033109903335599E-2,0.10116732120513899,0.105048730969429,0.116508565843105,0.12200430035591101,0.110328786075115,7.9214565455913502E-2,6.2366451442910503E-2,6.8895691837038101E-2,7.8363087459413699E-2,8.9170790843391204E-2,7.9490613960295498E-2,7.1113326680113706E-2,8.9490032844414397E-2]
["EAST-E1L203C10","EAST",8,"E1L203C10",102,"CD(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED",4.6512155532836896,4.6197738647460902,4.9871253967285201,5.4195404052734402,5.18412113189697,5.0698771476745597,5.5022644996643102,5.8327584266662598,6.0349636077880904,6.4133315936163298,6.3794127664302298,6.9048961275559204,6.2204724525930901,5.9471519438287199,4.9588076429113102,5.1275117667711196]
["EAST-E1L203C13","EAST",8,"E1L203C13",105,"CM(R), DRL Expense, Privately-Owned, BOX - EQUIPPED",0.33356142044067399,0.194173023104668,0.187669932842255,0.18948450684547399,0.183773458003998,0.19099274277687101,0.195416644215584,0.20674593746662101,0.24449484050273901,0.21341578626135899,0.21844921191661301,0.21369776858811601,0.19459162670354299,0.18118508472573999,0.18434157467594101,0.208438496536929]
["EAST-E1L204C4","EAST",8,"E1L204C4",109,"CM(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",5.6253235787153202E-2,5.2746698260307298E-2,6.0108393430709797E-2,6.7532740533351898E-2,6.7950487136840806E-2,6.3738428056240096E-2,6.2644943594932598E-2,6.7314162850379902E-2,9.4437554478645297E-2,0.12775398811767499,0.129857036394807,0.114830646627904,9.7774141535355699E-2,0.102662441212952,9.1796558512940996E-2,7.5721225373887396E-2]
["EAST-E1L204C6","EAST",8,"E1L204C6",111,"CM(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",4.8648934811353697E-2,6.8756990134716006E-2,6.5605863928794902E-2,8.7993994355201693E-2,8.0446541309356703E-2,7.8169763088226304E-2,9.4356715679168701E-2,8.9648187160491902E-2,0.15916812419891399,0.20106932465003299,0.195939275741772,0.16626301542149899,0.18866213117578501,0.163627779182977,0.17137054840157601,0.185064920289219]
["EAST-E1L204C11","EAST",8,"E1L204C11",116,"CD(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",4.4740576744079599,4.1261100769043004,4.0442013740539604,4.1799883842468297,2.8205628395080602,2.3566083908081099,1.4357035160064699,0.41651025414466902,1.0019713640212999,4.9828615595766399,3.1527410904716202,1.9754373316898099,2.0116280971956502,2.18400557067039,3.1734423843787098,2.6579030410542202]
["EAST-E1L204C12","EAST",8,"E1L204C12",117,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",1.9427474737167401,2.8177838325500502,2.92523169517517,3.83229279518127,3.55774593353271,3.51909351348877,3.6329600811004599,3.6934945583343501,6.4641981124877903,8.0590483740066396,7.8076596268638401,7.2095284752819797,7.8066066907294003,6.6944784039420098,6.9225988035026296,7.6106814619852798]
["EAST-E1L205C2","EAST",8,"E1L205C2",120,"CM(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",1.7880410887301001E-3,4.3497318401932699E-3,2.4514473043382198E-3,1.6067085787653899E-2,5.2050622180104299E-3,3.0092836823314398E-3,9.3634491786360706E-3,1.6246797516942E-2,1.48505577817559E-2,2.1352350701976702E-2,2.5219526291817299E-2,1.35257411573212E-2,1.46226018940278E-2,1.5986176022824601E-2,3.1669886218994497E-2,3.12930330723422E-2]
["EAST-E1L205C5","EAST",8,"E1L205C5",123,"CM(Y), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",4.64890105649829E-3,1.13093089312315E-2,6.3737612217664701E-3,4.1774395853281E-2,1.3533147983253E-2,7.8241378068924002E-3,2.4344986304640801E-2,4.2241688817739501E-2,3.8611501455307E-2,5.5516111825139297E-2,6.5570768358725107E-2,3.5166927009035301E-2,3.8018764924472301E-2,4.1564057659343998E-2,8.2341704169385896E-2,8.1361885988089799E-2]
["EAST-E1L205C9","EAST",8,"E1L205C9",127,"CD(R), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.682284116745,3.6911988258361799,5.2730145454406703,9.3161993026733398,7.4066410064697301,7.3879380226135298,8.9083108901977504,8.8168573379516602,7.7671823501586896,9.7365117185428804,10.438260736922899,11.0987737886164,12.5806750161679,10.6769495915542,10.080715892020701,10.6507179770582]
["EAST-E1L205C12","EAST",8,"E1L205C12",130,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.682284116745,3.6911988258361799,5.2730140686035201,9.3161983489990199,7.4066410064697301,7.3879380226135298,8.9083118438720703,8.8168563842773402,7.7671818733215297,9.7365117185428698,10.438260736922899,11.0987737886164,12.5806750161679,10.6769495915542,10.080715892020701,10.6507179770582]
["EAST-E1L206C3","EAST",8,"E1L206C3",134,"CM(R), ROI Expense, Railroad-Owned, HOPPER - COVERED",1.8258929252624501E-2,2.1602917462587402E-2,2.7731643989682201E-2,3.4249857068061801E-2,3.3030416816473E-2,4.7256067395210301E-2,5.23861199617386E-2,4.5034158974885899E-2,4.0136143565177897E-2,4.0312851617575599E-2,4.43860393733519E-2,5.4090286593775398E-2,6.7305809819063298E-2,5.2766889410084998E-2,4.7539127356857898E-2,5.8655719448569898E-2]
["EAST-E1L206C5","EAST",8,"E1L206C5",136,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",6.8674147129058796E-2,4.8919063061475802E-2,4.9995638430118602E-2,4.9733538180589697E-2,4.2623762041330303E-2,4.9412600696086897E-2,5.6073654443025603E-2,4.9107484519481701E-2,5.6331183761358303E-2,7.4397954162837399E-2,7.6839275647499303E-2,8.1542671211879997E-2,7.87660367069484E-2,0.101283658684634,8.2846769174473298E-2,6.7591884943002195E-2]
[{"$f":"B4034&\"-\"&D4034","v":"EAST-E1L206C10"},"EAST",8,"E1L206C10",141,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",4.02738285064697,3.91769170761108,4.1582179069518999,5.12561130523682,5.4966015815734899,5.5094704627990696,5.0663366317748997,5.83569431304932,5.9792160987854004,6.4664192796240503,5.6569541983798199,6.4663850528013596,6.6550953687569399,6.99829543123339,6.54661709715075,6.6688620598123904]
["EAST-E1L206C11","EAST",8,"E1L206C11",142,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",9.9817695617675799,8.4453525543212908,9.3621606826782209,10.225048065185501,7.4210066795349103,7.6809449195861799,5.2171201705932599,4.3346490859985396,4.7862224578857404,6.3440068127412603,7.0860230001767004,7.5648359683542203,6.80519456336605,7.7740773824255003,6.0840801805023403,5.5057902015951203]
["EAST-E1L207C1","EAST",8,"E1L207C1",145,"CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.8268218040466302E-2,2.8636299073696098E-2,3.0679928138852099E-2,3.7109695374965702E-2,3.5413604229688603E-2,3.6135181784629801E-2,3.7324402481317499E-2,3.7364557385444599E-2,3.7669777870178202E-2,3.9633481427829097E-2,4.16651800100949E-2,4.1757447495054403E-2,3.6352528465841097E-2,3.6917543748055698E-2,3.3058565359963099E-2,2.9621301516463201E-2]
["EAST-E1L207C5","EAST",8,"E1L207C5",149,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",8.45529660582542E-2,0.105915024876595,0.104354538023472,0.10393890738487201,7.7732302248477894E-2,9.3212381005287198E-2,0.13972221314907099,0.117993913590908,0.115026667714119,0.13284146455812301,0.11352847363882899,0.122574737707979,0.113556547879229,0.12559921771419699,0.18662204359308901,0.122149962385374]
["EAST-E1L207C8","EAST",8,"E1L207C8",152,"CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",5.0155110359191903,5.6197824478149396,5.0988717079162598,6.05759620666504,3.81275081634521,4.3115220069885298,7.15364742279053,6.9052248001098597,4.6632628440856898,4.7542439137618704,4.4655076992936804,4.86844056620098,5.0535246482834104,5.8831676779447601,8.5822723946148098,5.0027802640770496]
["EAST-E1L207C11","EAST",8,"E1L207C11",155,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",5.0155110359191903,5.6197829246520996,5.0988721847534197,6.05759572982788,3.8127510547637899,4.3115220069885298,7.15364742279053,6.9052248001098597,4.6632628440856898,4.7542439137618704,4.4655076992936804,4.86844056620098,5.0535246482834104,5.8831676779447601,8.5822723946148098,5.0027802640770496]
["EAST-E1L208C2","EAST",8,"E1L208C2",159,"CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.6439912617206601E-2,2.5039833039045299E-2,2.6104327291250201E-2,3.5241268575191498E-2,2.6309572160243998E-2,2.5815427303314199E-2,3.1423565000295597E-2,2.1771173924207701E-2,1.7132014036178599E-2,2.1877461008520602E-2,2.8090580301009901E-2,2.62191541061737E-2,3.0704729198077901E-2,2.0337014324105201E-2,3.1864795388753302E-2,3.1549043273986298E-2]
["EAST-E1L208C4","EAST",8,"E1L208C4",161,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",7.5889766216278104E-2,6.9213636219501495E-2,7.4834614992141696E-2,9.4681978225707994E-2,0.10061090439558,0.10901518166065199,0.11140982061624501,0.10907970368862201,0.11615387350320799,0.14882036514972399,0.181507627910103,0.226491363912453,0.22546552999066799,0.24168296870548001,0.21180433074281799,0.214506063161195]
["EAST-E1L208C9","EAST",8,"E1L208C9",166,"CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.4661829471588099,1.77094054222107,2.51761817932129,3.1313953399658199,2.4911580085754399,2.67580246925354,2.9710986614227299,2.6334896087646502,2.0533487796783398,2.33380299215644,2.6016560256260601,2.70425943546332,3.13212739807968,2.3381707658455402,2.0363684626216001,2.5199384388616299]
["EAST-E1L208C10","EAST",8,"E1L208C10",167,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.0394936800003101,0.93780881166458097,1.0184066295623799,1.2182326316833501,1.1755459308624301,1.15125036239624,1.0720572471618699,1.0510104894638099,1.1218237876892101,1.5172833682451301,1.88436767158937,2.28464676943929,2.18324178491266,2.23134663006062,1.8969483341676701,1.9338338043963299]
["EAST-E1L208C13","EAST",8,"E1L208C13",170,"CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - SPECIAL",4.7244720917660701E-6,9.9036760730086792E-6,7.2794355219230098E-6,8.2155445124953996E-4,5.1881329454772598E-6,1.3324297469807799E-6,4.9811533244792399E-5,3.08459675579797E-5,5.2639719797298301E-4,6.5708676698200698E-6,3.9152668947337397E-6,1.8120022004226901E-6,1.9008679556000599E-6,6.1782877190938502E-6,9.9605842709842395E-6,5.3202893594181596E-6]
["EAST-E1L209C4","EAST",8,"E1L209C4",174,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",5.4594123503193303E-4,-5.0480797654017795E-4,6.8034767173230596E-3,1.4567892067134399E-2,1.6947306692600299E-2,1.29725988954306E-2,1.0064262896776199E-2,9.6266753971576708E-3,9.7364895045757294E-3,9.4991168784474694E-3,1.2522780992523699E-2,1.5762531299078401E-2,1.8205282107376299E-2,2.0355634162968698E-2,2.1181170852292801E-2,2.9580706333852999E-2]
["EAST-E1L209C7","EAST",8,"E1L209C7",177,"CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",2.7862910181283999E-2,-2.5733582675457001E-2,0.34935721755027799,0.75979810953140303,0.89996093511581399,0.693842232227325,0.53789651393890403,0.51484042406082198,0.525240838527679,0.51815999642308297,0.67648996416506602,0.84912535508318499,0.96404715046828204,1.08625339007301,1.1286068151731301,1.58399561712591]
["EAST-E1L209C10","EAST",8,"E1L209C10",180,"CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",2.7862908318638802E-2,-2.5733582675457001E-2,0.34935721755027799,0.75979804992675803,0.89996093511581399,0.693842232227325,0.53789657354354903,0.51484042406082198,0.525240778923035,0.51815999642308297,0.67648996416506602,0.84912535508318499,0.96404715046828204,1.08625339007301,1.1286068151731301,1.58399561712591]
["EAST-E1L210C1","EAST",8,"E1L210C1",184,"CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",1.48957679048181E-2,1.50746339932084E-2,1.6519524157047299E-2,1.6746647655963901E-2,1.33242141455412E-2,8.52350704371929E-3,9.0015558525919897E-3,8.6558777838945406E-3,8.6494013667106594E-3,6.7456256085183103E-3,7.0006631732569104E-3,7.4484895825319402E-3,9.6040006892544605E-3,1.1223337242587599E-2,1.1343961989299E-2,1.14738790071841E-2]
["EAST-E1L210C3","EAST",8,"E1L210C3",186,"CM(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",1.24378195032477E-2,2.1192545071244202E-2,3.3152308315038702E-2,5.7810512371361299E-3,3.2612239010631999E-3,7.0591690018773096E-3,8.6650699377059902E-3,9.3826502561569197E-3,2.1238583140075198E-3,1.70983705469197E-3,7.6992781250123498E-3,1.03513822856075E-2,1.11503519528667E-2,9.1185469543635708E-3,8.6133348385384594E-3,7.9687604131861208E-3]
["EAST-E1L210C6","EAST",8,"E1L210C6",189,"CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",3.2338257879018797E-2,5.5100589990615803E-2,8.6195953190326705E-2,1.5030715614557299E-2,8.4791816771030391E-3,1.8353858962655099E-2,2.2529199719428999E-2,2.43948772549629E-2,5.5220411159098096E-3,4.4455763421991298E-3,2.0018123125032102E-2,2.6913593942579299E-2,2.89909150774534E-2,2.3708222081345199E-2,2.2394670580200001E-2,2.0718777074283899E-2]
["EAST-E1L210C9","EAST",8,"E1L210C9",192,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",2.5615379810333301,4.3493847846984899,6.8555727005004901,1.22183585166931,0.68771690130233798,1.54036664962769,1.94213247299194,2.1167340278625502,0.29190778732299799,0.39154328117522202,1.8118118965591801,2.5109522236864001,2.7818502345519098,2.3534091548181499,2.2083609243607398,2.1865267412861802]
["EAST-E1L210C12","EAST",8,"E1L210C12",195,"CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",2.5615379810333301,4.3493838310241699,6.8555722236633301,1.22183585166931,0.68771690130233798,1.54036688804626,1.94213247299194,2.1167345046997101,0.29190778732299799,0.39154328117522202,1.8118118965591801,2.5109522236864001,2.7818502345519098,2.3534091548181499,2.2083609243607398,2.1865267412861802]
["EAST-E1L211C3","EAST",8,"E1L211C3",199,"CM(R), ROI Expense, Railroad-Owned, FLAT - TOFC",2.1003530127927699E-4,2.2257692762650501E-4,2.0776517339982101E-4,1.5960184391588001E-3,1.7870339797809701E-3,1.74862868152559E-3,1.8164970679208599E-3,1.62975862622261E-3,1.36676465626806E-3,9.6034434796405798E-4,9.860675061366161E-4,1.18314292288732E-3,1.34455445067429E-3,6.4414194456376196E-5,8.1058788107479798E-5,1.6295010477426899E-4]
["EAST-E1L211C6","EAST",8,"E1L211C6",202,"CM(Y), ROI Expense, Railroad-Owned, FLAT - TOFC",5.4609164362773299E-4,5.7870079763233705E-4,5.4018985247239503E-4,4.1496478952467398E-3,4.64628683403134E-3,4.5464402064681097E-3,4.7228951007127797E-3,4.2373719625174999E-3,3.5535872448235798E-3,2.4968953047065502E-3,2.5637755159552099E-3,3.0761715995070199E-3,3.49584157175316E-3,1.6747690558657801E-4,2.10752849079447E-4,4.2367027241310001E-4]
[{"$f":"B4098&\"-\"&D4098","v":"EAST-E1L211C9"},"EAST",8,"E1L211C9",205,"CD(R), ROI Expense, Railroad-Owned, FLAT - TOFC",1.7498513683676699E-2,1.7748428508639301E-2,1.54898148030043E-2,0.13393715023994399,0.12963695824146301,0.130202576518059,0.18106380105018599,0.15756587684154499,0.12589161098003401,8.6320029347173005E-2,9.2590669137126394E-2,0.105438128238666,0.11859932089927699,2.5655778117336498E-3,4.2450666485107803E-3,9.0548568613027895E-3]
["EAST-E1L211C11","EAST",8,"E1L211C11",207,"CD(Y), DRL Expense, Railroad-Owned, FLAT - TOFC",4.9351215362548801,3.0264914035797101,3.0556483268737802,3.1208872795104998,5.5239772796630904,7.5302481651306197,6.1624999046325701,7.0402712821960396,7.5871233940124503,7.1641001424395796,6.7509942642612302,5.4661329311045703,5.1872578628694201,4.3232222317883702,5.1610469053091803,7.42756089928492]
["EAST-E1L212C4","EAST",8,"E1L212C4",213,"CM(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",0.366265118122101,0.46643015742301902,0.55372327566146895,0.63149857521057096,0.419312834739685,0.42092990875244102,0.47288843989372298,0.45491689443588301,0.44066721200942999,0.43801373846806702,0.43679465892811398,0.45123242632099397,0.39434721316515298,0.41088119630697201,0.35864187627355998,0.37266556903255599]
["EAST-E1L212C5","EAST",8,"E1L212C5",214,"CM(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",0.50449240207672097,0.45322859287262002,0.535367012023926,0.63532841205596902,0.50783127546310403,0.52718788385391202,0.54507279396057096,0.47210991382598899,0.47124570608138999,0.485193776615651,0.46677541079909202,0.50003177072171801,0.42447402188091099,0.39216669913028102,0.47366330087789399,0.45549655125462701]
["EAST-E1L212C8","EAST",8,"E1L212C8",217,"CD(R), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",3.98824119567871,14.151939392089799,37.269882202148402,46.464939117431598,34.388790130615199,19.823539733886701,51.834983825683601,16.452417373657202,20.776588439941399,20.300954977353101,27.169381245488101,18.9854036797839,18.1693560541487,15.7515896203665,16.065610620726002,35.418436986340097]
["EAST-E1L212C11","EAST",8,"E1L212C11",220,"CD(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",3.9882392883300799,14.151939392089799,37.2698783874512,46.464939117431598,34.3887939453125,19.823539733886701,51.834983825683601,16.452417373657202,20.776588439941399,20.300954977353101,27.169381245488101,18.9854036797839,18.1693560541487,15.7515896203665,16.065610620726002,35.418436986340097]
["EAST-E1L213C2","EAST",8,"E1L213C2",224,"CM(R), DRL Expense, Railroad-Owned, FLAT - GENERAL",2.95426771044731E-2,1.63084305822849E-2,1.42230642959476E-2,0.19428823888301799,0.24239678680896801,0.43714857101440402,0.442850321531296,0.47617655992507901,0.46975195407867398,0.68334881249963297,1.2769317629002099,-0.22798245575322601,3.0783194437460701,3.2951544242967499,4.7673455069413304,5.9898800719233103]
["EAST-E1L213C5","EAST",8,"E1L213C5",227,"CM(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",7.6810896396637005E-2,4.2401958256959901E-2,3.6979965865612002E-2,0.50514894723892201,0.63023173809051503,1.13658440113068,1.1514099836349501,1.23805844783783,1.2213557958602901,1.77670691249904,3.3200225835405202,-0.59275438495838495,8.0036305537397592,8.5674015031715207,12.3950983180475,15.573688187000601]
["EAST-E1L213C8","EAST",8,"E1L213C8",230,"CD(R), DRL Expense, Railroad-Owned, FLAT - GENERAL",-26.8680725097656,-5.8445386886596697,-7.8087892532348597,101.144340515137,25.609086990356399,54.801761627197301,67.101959228515597,74.489585876464801,114.49871063232401,212.15050502045301,443.71008929439898,183.93187869026499,766.27785542472805,779.38106019298698,858.81561704035198,1071.9787948861999]
["EAST-E1L213C10","EAST",8,"E1L213C10",232,"CD(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL",35.3252983093262,10.9610252380371,8.1972150802612305,9.2406778335571307,13.1117763519287,18.4469394683838,93.459495544433594,116.05934143066401,96.478263854980497,15.601980772787901,2.8696538306059298,138.819666485178,155.42466544253799,186.612676670871,3.2563058164592098,3.3495094852867702]
["EAST-E1L214C3","EAST",8,"E1L214C3",238,"CM(R), ROI Expense, Railroad-Owned, FLAT - OTHER",1.06660882011056E-2,1.37710738927126E-2,1.8786389380693401E-2,1.43231656402349E-2,1.29836359992623E-2,1.48485386744142E-2,1.48679688572884E-2,1.2910353019833599E-2,1.37310838326812E-2,1.6695036310407901E-2,1.32391864858012E-2,1.5337965386214601E-2,1.7557750656786601E-2,1.26759621730556E-2,1.13379402967835E-2,1.3555308312014999E-2]
["EAST-E1L214C4","EAST",8,"E1L214C4",239,"CM(Y), OPR Expense, Railroad-Owned, FLAT - OTHER",4.8003405332565301E-2,5.4466221481561702E-2,6.0636714100837701E-2,7.7173098921775804E-2,9.7921781241893796E-2,0.11491481214761699,0.137999147176743,0.147248759865761,0.16078856587410001,0.16089682428562099,0.14503806320739701,0.14516811803987201,0.13215009673848099,0.14320118750414401,0.129450744736887,0.12980252536499401]
["EAST-E1L214C7","EAST",8,"E1L214C7",242,"CD(R), OPR Expense, Railroad-Owned, FLAT - OTHER",2.1185750961303702,2.43356513977051,2.6896538734436,3.4324305057525599,4.2832946777343803,5.0010452270507804,6.0870409011840803,6.5155949592590297,7.2263765335082999,7.3430788046718396,6.89365766791963,7.0974499318168798,6.4912010650424596,6.9678159098786896,6.3216865376767597,6.4319135417235298]
["EAST-E1L214C10","EAST",8,"E1L214C10",245,"CD(Y), OPR Expense, Railroad-Owned, FLAT - OTHER",2.1185750961303702,2.43356513977051,2.68965411186218,3.4324305057525599,4.2832946777343803,5.0010452270507804,6.0870409011840803,6.5155949592590297,7.2263765335082999,7.3430788046718396,6.89365766791963,7.0974499318168798,6.4912010650424596,6.9678159098786896,6.3216865376767597,6.4319135417235298]
["EAST-E1L215C1","EAST",8,"E1L215C1",249,"CM(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L215C4","EAST",8,"E1L215C4",252,"CM(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L215C8","EAST",8,"E1L215C8",256,"CD(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L215C9","EAST",8,"E1L215C9",257,"CD(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L216C2","EAST",8,"E1L216C2",263,"CM(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,1.0543582029640701E-2,0,7.4272528290748596E-3,6.4300410176499102E-3,6.6299190049544801E-3,6.3173500711627998E-3,6.1162004258980499E-3,4.8286719475096399E-3,4.2403841720874197E-3,3.7101758080977602E-3]
["EAST-E1L216C3","EAST",8,"E1L216C3",264,"CM(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L216C6","EAST",8,"E1L216C6",267,"CM(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L216C9","EAST",8,"E1L216C9",270,"CD(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L216C13","EAST",8,"E1L216C13",274,"CM(R), DRL Expense, Privately-Owned, TANK >=22,000 GAL",5.8673989027738599E-2,2.6461226865649199E-2,2.18772776424885E-2,1.7512649297714199E-2,1.73372458666563E-2,1.5107460319995899E-2,1.0543582029640701E-2,8.5642607882618904E-3,7.4272528290748596E-3,6.4300410176499102E-3,6.6299190049544801E-3,6.3173500711627998E-3,6.1162004258980499E-3,4.8286719475096399E-3,4.2403841720874197E-3,3.7101758080977602E-3]
["EAST-E1L217C3","EAST",8,"E1L217C3",277,"CM(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",1.0791831649839901E-2,1.2579454109072701E-2,1.5013515949249301E-2,1.19014289230108E-2,9.6028652042150497E-3,1.07568129897118E-2,1.1144431307911901E-2,1.04910973459482E-2,5.9550791047513502E-3,8.5298145355474503E-3,1.0320174388297101E-2,9.8646462643313896E-3,-6.58925831885701E-3,2.1833307696293301E-3,8.8950187332619002E-3,1.26762610875037E-2]
["EAST-E1L217C8","EAST",8,"E1L217C8",282,"CD(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-3.27627778053284,-0.23439286649227101,2.5834683328867E-2,1.56600737571716,0.15386247634887701,0.61223077774047896,0.25593721866607699,-0.72303795814514205,-2.6456649303436302,5.4567985800764198,-10.1832893095649,-19.467117098201498,-26.2720959941574,-26.165659508684399,-27.7488570038456,-29.687762564778598]
["EAST-E1L217C11","EAST",8,"E1L217C11",285,"CD(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-3.27627801895142,-0.23439286649227101,2.5834558531641998E-2,1.56600737571716,0.15386235713958701,0.61223077774047896,0.25593733787536599,-0.72303783893585205,-2.6456651687622101,5.4567985800764198,-10.1832893095649,-19.467117098201498,-26.2720959941574,-26.165659508684399,-27.7488570038456,-29.687762564778598]
["EAST-E1L218C1","EAST",8,"E1L218C1",288,"CM(R), OPR Expense, Railroad-Owned, AUTO RACKS",0.12159825861454,0.16511395573616,0.19195520877838099,0.21506404876709001,0.123944312334061,0.117163822054863,0.13300859928131101,0.12929649651050601,0.11965861171484,0.115064700602086,0.112732628670117,0.12906877239520501,0.118064786551517,0.12903039048300799,0.104504177483192,0.10676331207027299]
["EAST-E1L218C2","EAST",8,"E1L218C2",289,"CM(R), DRL Expense, Railroad-Owned, AUTO RACKS",0.14496593177318601,0.145406574010849,0.16875000298023199,0.22843436896801,0.156289607286453,0.16672413051128401,0.15112566947937001,0.119387663900852,0.109577469527721,0.116526783194408,0.11457861817804001,0.12866946193797399,0.10883252832603101,0.10088876394526999,0.13513487614633499,0.12897153650802001]
["EAST-E1L218C5","EAST",8,"E1L218C5",292,"CM(Y), DRL Expense, Railroad-Owned, AUTO RACKS",0.37691134214401201,0.37805685400962802,0.43875032663345298,0.59392893314361594,0.40635228157043501,0.433482766151428,0.39292666316032399,0.31040778756141701,0.28490144014358498,0.30296963630546198,0.29790440726290301,0.33454060103873101,0.28296457364768102,0.26231078625769999,0.35135067798046998,0.33532599492085202]
["EAST-E1L218C8","EAST",8,"E1L218C8",295,"CD(R), DRL Expense, Railroad-Owned, AUTO RACKS",14.778052330017101,18.868534088134801,41.575466156005902,40.620426177978501,30.877378463745099,30.612993240356399,31.8052978515625,13.475725173950201,16.060907363891602,17.446445895022801,29.634591090949499,25.5256634613811,23.833956181756601,20.315877775455199,11.0193187510976,29.7265174958291]
["EAST-E1L218C12","EAST",8,"E1L218C12",299,"CD(Y), ROI Expense, Railroad-Owned, AUTO RACKS",17.430082321166999,20.744125366210898,30.6048908233643,47.388835906982401,38.804347991943402,42.367439270019503,41.6718940734863,36.322563171386697,29.082017898559599,34.775120204395201,31.050765143983199,34.871290281401002,32.594984806440998,26.395999482592298,27.645516619062398,36.144454120755697]
["EAST-E1L219C2","EAST",8,"E1L219C2",302,"CM(R), DRL Expense, Railroad-Owned, ACCESSORIAL",2.2305919264908899E-4,2.6125641306862203E-4,3.1437579309567798E-4,4.7133781481534199E-4,1.9210859318263799E-4,1.67667065397836E-4,1.6009916726034099E-4,6.9968657044228193E-5,6.0071433836128603E-5,7.1363910929109895E-5,-2.55569674616011E-7,2.3512388228467899E-5,1.15530465941411E-4,1.01958193186682E-4,1.32083191581404E-4,1.08092311724864E-4]
["EAST-E1L219C7","EAST",8,"E1L219C7",307,"CD(R), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L219C10","EAST",8,"E1L219C10",310,"CD(Y), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L219C13","EAST",8,"E1L219C13",313,"CM(R), DRL Expense, Privately-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E1L220C1","EAST",8,"E1L220C1",314,"CM(R), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.5830099135637297E-2,3.8495421409606899E-2,4.2018439620733303E-2,5.38810640573502E-2,4.3691266328096397E-2,3.9077233523130403E-2,4.3094601482152897E-2,4.5606505125760997E-2,4.8816170543432201E-2,5.6000426022066903E-2,5.7994447042511103E-2,5.6222135912981301E-2,5.20437090737026E-2,5.7525257483059901E-2,5.5009988594636801E-2,4.8161472057931899E-2]
["EAST-E1L220C4","EAST",8,"E1L220C4",317,"CM(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",9.11004394292831E-2,9.7365863621234894E-2,0.106582224369049,0.135344699025154,0.106086015701294,9.7465291619300801E-2,0.10912268608808499,0.11407259106636,0.12184024602174801,0.14483502229171999,0.15305651779860099,0.14793348737670001,0.136881956085148,0.15290464582896901,0.145058479041663,0.12953806118529701]
["EAST-E1L220C8","EAST",8,"E1L220C8",321,"CD(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",9.2270698547363299,7.6757979393005398,8.4355964660644496,9.7301158905029297,7.7184820175170898,7.2063574790954599,7.1758742332458496,6.3837757110595703,7.4759755134582502,9.1484993975515696,9.5175691608862998,8.3560287016265598,8.6178845570573106,8.9905157003957505,10.1284842452781,11.409862252407301]
["EAST-E1L220C11","EAST",8,"E1L220C11",324,"CD(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",7.1805729866027797,6.2040123939514196,6.7666716575622603,7.6686577796936,5.9367494583129901,5.6219902038574201,5.4547882080078098,5.0240898132324201,5.5668845176696804,6.9567762470517298,7.1612988437989298,6.06664221479764,6.2045506248387001,6.1834156129866296,6.9362875971861104,7.6952191746369101]
["EAST-E1L221C1","EAST",8,"E1L221C1",327,"CM(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.1408711373806,0.17939640581607799,0.212970405817032,0.242883905768394,0.16127409040927901,0.16189613938331601,0.18188032507896401,0.17496806383132901,0.16948744654655501,0.16846682248771799,0.167997945741582,0.17355093320038201,0.15167200506351999,0.15803122934883601,0.13793918318213799,0.14333291116636801]
["EAST-E1L221C6","EAST",8,"E1L221C6",332,"CM(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.36962771415710399,0.44502103328704801,0.63606882095336903,0.90815085172653198,0.74340951442718495,0.82136559486389205,0.75693148374557495,0.654959976673126,0.58634489774704002,0.64851639761208202,0.53580300905142997,0.595552370432468,0.57679346549288002,0.46775438994132501,0.48291649023035899,0.62259799149362804]
["EAST-E1L221C9","EAST",8,"E1L221C9",335,"CD(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",19.538587570190401,23.229181289672901,33.542747497558601,49.440803527832003,41.2504692077637,44.975208282470703,44.147251129150398,38.432754516601598,34.185596466064503,38.124578130981298,31.870324992894599,35.750418290391202,33.483576831088101,26.9439120965862,28.177453602353101,36.783351125730398]
["EAST-E1L221C12","EAST",8,"E1L221C12",338,"CD(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",19.5385856628418,23.229179382324201,33.542747497558601,49.440799713134801,41.250465393066399,44.975208282470703,44.147247314453097,38.432750701904297,34.185592651367202,38.124578130981298,31.870324992894599,35.750418290391202,33.483576831088101,26.9439120965862,28.177453602353101,36.783351125730398]
["EAST-E1L221C13","EAST",8,"E1L221C13",339,"CM(R), DRL Expense, Privately-Owned, TOTAL FLAT, MULTILEVEL",0.29265728592872597,0.174065947532654,0.217188775539398,0.27947828173637401,0.23359996080398601,0.22402092814445501,0.19530099630355799,0.19358460605144501,0.205410450696945,0.20495403248158001,0.21803210369180401,0.23265965511032799,0.21662632887723901,0.22030921172468301,0.29036232936707701,0.29215968003051002]
["EAST-E1L303C1","EAST",8,"E1L303C1",342,"L&D Expense, POTATOES OTHER THAN SWEET",3.6799578666686998,3.1860339641571001,1.57116758823395,2.0286219120025599,0.46845808625221302,0.59124863147735596,0.76070266962051403,0.51356053352356001,1.9531569480896001,2.51130048867766,2.4820239734348402,1.5628554724856101,1.5738487949622999,4.7855950282905102,2.6763798404894299,1.6733272275745501]
["EAST-E1L307C1","EAST",8,"E1L307C1",346,"L&D Expense, METALLIC ORES",1.6947247087955499E-2,7.1331090293824699E-3,3.3462069928646102E-2,7.0100501179695102E-2,4.2934261262416798E-2,3.86384478770196E-3,4.2152050882577896E-3,8.2664601504802704E-3,2.1994682028889699E-3,1.2440038637219399E-2,8.2511941540468301E-4,0,0,5.0977125450342798E-3,1.33905395969415E-4,0]
["EAST-E1L310C1","EAST",8,"E1L310C1",349,"L&D Expense, FOOD AND KINDRED PRODUCTS",0.112814217805862,0.10337255895137799,0.15115562081337,0.103318996727467,7.9335421323776203E-2,8.1889294087886796E-2,0.113200463354588,0.10237280279398001,0.105734661221504,0.155869352854069,0.14200791172845001,0.110538880168726,0.16084816368765401,0.19031238664048999,0.105766987771637,0.100991336079819]
["EAST-E1L313C1","EAST",8,"E1L313C1",352,"L&D Expense, CANNED FRUITS/VEG",0.61201786994934104,0.45836937427520802,0.54955309629440297,0.46772405505180398,0.268973708152771,0.44812881946563698,0.364413142204285,0.32465270161628701,0.30047565698623702,0.54309701066336802,0.60036280662191399,0.59926710243978698,0.57379621654754098,0.79501823483980005,0.40052818960853498,0.33041247966923698]
["EAST-E1L318C1","EAST",8,"E1L318C1",357,"L&D Expense, RICE",0.18275606632232699,0.20021592080593101,0.26043739914894098,0.49083593487739602,0.26900073885917702,0.26474368572235102,0.105855084955692,0.30795875191688499,0.195555880665779,0.171957354616004,0.217271284411443,0.20353585332434401,0.10460667322949101,0.201985129218855,0.18705377019309699,0.27474099401881502]
["EAST-E1L321C1","EAST",8,"E1L321C1",360,"L&D Expense, REFINED SUGAR",2.7943493798375098E-2,0.16404953598976099,3.96022871136665E-2,0.10142989456653601,3.3815246075391797E-2,7.3806062340736403E-2,0.14849175512790699,8.2387849688529996E-2,0.25767901539802601,0.19669764508510401,3.2387171869427901E-3,4.3898923629163901E-2,7.3782916037265098E-2,3.3899308291411599E-2,1.4090874839876401E-2,0.11818608416618399]
["EAST-E1L322C1","EAST",8,"E1L322C1",361,"L&D Expense, BEER",0.21311140060424799,0.13795143365859999,0.11230556666851001,0.209407404065132,0.334010690450668,0.38553339242935197,0.90072369575500499,0.90642565488815297,0.56750947237014804,1.0174552404741599,1.7311441019848299,1.9743613882701201,3.1530590569508399,8.7245439934215394,2.5082539988572998,1.4391021304396601]
["EAST-E1L325C1","EAST",8,"E1L325C1",364,"L&D Expense, MISC FOOD PREPARATIONS",4.9347322434186901E-2,3.9073646068572998E-2,6.88051283359528E-2,4.7288753092288999E-2,7.3226988315582303E-2,4.44420874118805E-2,5.8179348707199097E-2,6.4795158803462996E-2,6.5988443791866302E-2,4.7256400580346102E-2,0.10027194560448401,5.8322594141169803E-2,4.7792372956870097E-2,4.0860279141872603E-2,3.6097560727487002E-2,5.5607518381965003E-2]
["EAST-E1L328C1","EAST",8,"E1L328C1",367,"L&D Expense, LUMBER AND WOOD EX FURNITURE",6.4082108438014998E-2,6.3597209751606001E-2,4.2465981096029302E-2,5.5317327380180401E-2,2.6106728240847601E-2,4.5685745775699602E-2,2.36855149269104E-2,3.1761787831783302E-2,2.2764811292290701E-2,5.5634208764431099E-2,6.8785233747138505E-2,4.2106313382289699E-2,5.85751816640947E-2,5.6718723912763502E-2,5.8628574900259398E-2,0.141446267912923]
["EAST-E1L332C1","EAST",8,"E1L332C1",371,"L&D Expense, FURNITURE AND FIXTURES",1.01506423950195,4.2289190292358398,3.8702409267425502,1.72642862796783,1.0335067510604901,0.56756269931793202,1.8485848903655999,0.51095122098922696,0.77477347850799605,0.87920951704397499,0.29486340670581901,0.40993634402058698,0.171194339057925,0.29584487614604099,0.37153646834541698,2.0288792699200302]
["EAST-E1L335C1","EAST",8,"E1L335C1",374,"L&D Expense, PRINTING PAPER",0.45069688558578502,0.77085703611373901,0.80805128812789895,0.78840303421020497,0.60578840970992998,0.33505225181579601,0.42516347765922502,0.31435161828994801,0.37708187103271501,0.39925658646490703,0.66945896095312996,1.11723782584026,0.58951542221150599,0.19435054877364999,0.121608076937136,0.190232288385774]
["EAST-E1L339C1","EAST",8,"E1L339C1",378,"L&D Expense, ALL OTHER PULP, PAPER & ALLIED PRODUCTS",0.17567807435989399,0.195987403392792,0.152946561574936,0.107534527778625,7.8239731490612002E-2,8.5699714720249204E-2,0.122758314013481,8.2997627556324005E-2,7.0808172225952107E-2,5.6488843821234702E-2,7.3495363821740795E-2,3.9105518177458103E-2,5.0811760324324599E-2,0.14501322871120401,0.100518870925555,0.10260932363021701]
["EAST-E1L343C1","EAST",8,"E1L343C1",382,"L&D Expense, SYN FIBRES/RESINS/RUBBER",0.14274440705776201,6.1173558235168499E-2,8.7265506386756897E-2,0.10607888549566299,8.5183314979076399E-2,0.12817049026489299,0.132741883397102,9.0175598859787001E-2,0.100434817373753,8.3801154952120302E-2,0.11696684497985201,0.106955975079934,5.2621767832795201E-2,0.10260436617034099,6.5752737420087498E-2,0.139082763813134]
["EAST-E1L346C1","EAST",8,"E1L346C1",385,"L&D Expense, PETROLEUM OR COAL PRODUCTS",5.6120855733752303E-3,2.0458623766899098E-2,1.4187679626047601E-2,1.6730939969420398E-2,9.0988166630268097E-3,2.5490145199000801E-3,7.7201277017593401E-3,7.4020400643348703E-3,7.5389896519482101E-3,2.8806192440008001E-3,3.97382980853935E-3,1.3481022730943801E-2,7.8551231896560793E-3,6.7912819925897497E-3,5.4264531937212798E-3,1.17302843534858E-2]
["EAST-E1L347C1","EAST",8,"E1L347C1",386,"L&D Expense, RUBBER AND MISC PLASTICS",0.121731825172901,8.4463320672512096E-2,5.7188738137483597E-2,2.3528395220637301E-2,1.31647260859609E-2,7.10021182894707E-2,0.156284719705582,9.4427227973938002E-2,0.101616881787777,2.8642241838434401E-2,2.2199691128442101E-2,1.54454766150119E-2,6.0183038438072003E-3,9.8465346002906795E-2,4.7641514960962097E-2,3.8674507534544302E-2]
["EAST-E1L350C1","EAST",8,"E1L350C1",389,"L&D Expense, STONE, CLAY AND GLASS PRODUCTS",2.8050996363163001E-2,2.94760055840015E-2,2.3014681413769701E-2,2.2323321551084501E-2,1.25137800350785E-2,2.0365133881568898E-2,1.3885203748941401E-2,1.2379656545817901E-2,2.0123468711972198E-2,1.8672422852622099E-2,1.5618687233242201E-2,7.1743035945493697E-3,1.00761913642266E-2,1.1213559823315599E-2,1.4322538640667201E-2,1.0220925283838099E-2]
["EAST-E1L353C1","EAST",8,"E1L353C1",392,"L&D Expense, ALL OTHER STONE & CLAY, GLASS PRODUCTS",2.3819899186492001E-2,2.95029655098915E-2,1.7426427453756301E-2,1.5901990234851799E-2,9.0113366022705997E-3,1.7641941085457798E-2,1.0626674629747901E-2,8.8174836710095406E-3,1.7466975376009899E-2,1.6213023466090899E-2,8.0123522222395605E-3,7.0282422645380101E-3,8.5392018813610897E-3,1.00639728338627E-2,1.8205648733177902E-2,8.8792988187615506E-3]
["EAST-E1L357C1","EAST",8,"E1L357C1",396,"L&D Expense, ALL OTHER PRIMARY METAL PRODUCTS",2.12727766484022E-2,9.5122657716274303E-2,0.135312050580978,4.1251994669437402E-2,3.5979904234409298E-2,3.8908191025257097E-2,5.8396480977535199E-2,1.43697401508689E-2,1.95995084941387E-2,2.3422915187733099E-2,3.1688528748677502E-2,3.7337457772167501E-2,8.8837298846552505E-4,7.0970671331329699E-2,0.279650607967111,9.53012962841015E-2]
["EAST-E1L360C1","EAST",8,"E1L360C1",399,"L&D Expense, ALL OTHER FAB METAL PRODUCTS",8.2236602902412401E-2,4.22826893627644E-2,0.12317106872797,0.57348483800888095,0.11085592955350899,0.104633316397667,0.104206696152687,0.41068261861801098,2.90865134447813E-2,2.6793860444710701E-2,1.17116840125649E-2,6.1026978151819303E-2,8.3779653724611707E-3,1.9695008077359299E-2,2.3129155730127701E-3,8.2394414457267903E-2]
["EAST-E1L364C1","EAST",8,"E1L364C1",403,"L&D Expense, CONST MIN/MAT HAND MACHINERY",5.3824152797460598E-2,0.14556503295898399,0.225022718310356,0.24387198686599701,0.111423380672932,1.9659049808979E-2,9.3566169962286897E-3,0.25835311412811302,9.0812714770436304E-3,2.4417359235743799E-2,0.226980429468987,0.123886814731048,5.6786413195415104,5.5626533761732502E-2,0.50608937133810405,2.0688925659798598]
["EAST-E1L368C1","EAST",8,"E1L368C1",407,"L&D Expense, HOUSEHOLD APPLIANCES",0.205303609371185,0.23462562263011899,0.17131142318248699,0.277806997299194,0.25822886824607799,8.2644179463386494E-2,0.297059416770935,0.38408657908439597,0.13108573853969599,0.40999757319887098,0.15451085360087599,7.3435426620840294E-2,0.14930913105378599,0.247363305660388,7.2794077869062196E-2,8.71202277086814E-2]
["EAST-E1L371C1","EAST",8,"E1L371C1",410,"L&D Expense, TRANSPORTAION EQUIPMENT",1.3006241321563701,1.08988153934479,1.35968601703644,1.2409585714340201,0.75661820173263605,1.0195336341857899,1.6047393083572401,1.7275034189224201,2.29360747337341,1.4390260176603999,1.53309053496067,2.5685685982062201,2.42239663922193,2.64924837876096,2.5732802744444401,3.2399183966489802]
["EAST-E1L372C1","EAST",8,"E1L372C1",411,"L&D Expense, MOTOR PASSENGER CARS",1.6142339706420901,1.60462009906769,2.0916264057159402,1.80427742004395,1.1449105739593499,1.8661357164382899,2.4315426349639901,2.3879089355468799,2.9647860527038601,2.2775114836972699,2.3379065129382699,4.7704088395188302,3.82250992141388,3.6264625356952398,4.5673487040649103,7.7164689836323603]
["EAST-E1L375C1","EAST",8,"E1L375C1",414,"L&D Expense, ALL OTHER TRANSPORTATION EQUIPMENT",2.6227355003356899E-2,0.10049141198396699,3.2508585602045101E-2,6.5525375306606307E-2,0.26267328858375499,3.3132839947938898E-2,5.0899308174848598E-2,6.18039257824421E-2,9.2528991401195498E-2,3.1585700434175697E-2,7.6281476545512997E-2,0.119202553620429,7.6049686090451901E-2,4.0474509693458502,2.3140971066584299,1.6999942051205801E-2]
["EAST-E1L378C1","EAST",8,"E1L378C1",417,"L&D Expense, MISC MIXED SHIPMENTS",9.1315463185310405E-2,0.11395051330328,0.119482338428497,7.6815418899059296E-2,6.5753631293773707E-2,4.5803453773260103E-2,6.1025261878967299E-2,5.9127628803253202E-2,6.1889201402664198E-2,4.37200018110191E-2,7.5652365651906694E-2,3.3229987868641203E-2,3.2905317083349601E-2,3.0981519923329901E-2,4.4879455499843499E-2,4.5587054201045099E-2]
["EAST-E1L382C1","EAST",8,"E1L382C1",421,"L&D Expense, ALL OTHER COMMODITIES",3.7811581045389203E-2,0.571766257286072,0.50435817241668701,0.395120829343796,0.34854763746261602,0.28982281684875499,1.35337150096893,0.27479436993598899,2.1931312978267701E-2,0.35576115206112802,1.58875264111078,0.37422378104875798,0.25508157108880503,0.88390067928004001,0.16117152606319499,2.4966038048811998]
["EAST-E2L101C3","EAST",8,"E2L101C3",424,"E/L Ratio, Privately-Owned, BOX - 40 FT",1.6135851144790601,1.6772884130477901,1.6839191913604701,1.96958231925964,1.8478095531463601,1.71988105773926,1.79961144924164,1.77097940444946,1.7686024904251101,1.8076899377657301,1.8684433334677299,1.75281151596941,1.77128306226384,1.93790739220704,1.9228182711706601,1.86100070972321]
["EAST-E2L101C7","EAST",8,"E2L101C7",428,"Average circuity, BOX - 40 FT",1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999]
["EAST-E2L101C11","EAST",8,"E2L101C11",432,"CD per Intraterminal Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L101C14","EAST",8,"E2L101C14",435,"CD per Load & Unload Industry Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L101C15","EAST",8,"E2L101C15",436,"CD per Load & Unload Intraterminal Switch, BOX - 40 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L101C18","EAST",8,"E2L101C18",439,"CM per Interchange Switch, BOX - 40 FT",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["EAST-E2L101C21","EAST",8,"E2L101C21",442,"CM per I&I Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L101C25","EAST",8,"E2L101C25",446,"SEMs per Industry Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E2L101C28","EAST",8,"E2L101C28",449,"SEMs per Interterminal Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["EAST-E2L102C3","EAST",8,"E2L102C3",453,"E/L Ratio, Privately-Owned, BOX - 50 FT",1.6135851144790601,1.6772884130477901,1.6839191913604701,1.96958231925964,1.8478095531463601,1.71988105773926,1.79961144924164,1.77097940444946,1.7686024904251101,1.8076899377657301,1.8684433334677299,1.75281151596941,1.77128306226384,1.93790739220704,1.9228182711706601,1.86100070972321]
["EAST-E2L102C7","EAST",8,"E2L102C7",457,"Average circuity, BOX - 50 FT",1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999]
["EAST-E2L102C10","EAST",8,"E2L102C10",460,"CD per Interchange Switch, BOX - 50 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
[{"$f":"B4354&\"-\"&D4354","v":"EAST-E2L102C11"},"EAST",8,"E2L102C11",461,"CD per Intraterminal Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L102C14","EAST",8,"E2L102C14",464,"CD per Load & Unload Industry Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L102C18","EAST",8,"E2L102C18",468,"CM per Interchange Switch, BOX - 50 FT",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["EAST-E2L102C21","EAST",8,"E2L102C21",471,"CM per I&I Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L102C24","EAST",8,"E2L102C24",474,"Average Miles between Interchange Switches, BOX - 50 FT",969.75531005859398,855.52178955078102,804.59808349609398,881.60919189453102,891.96746826171898,897.69329833984398,721.10607910156295,740.75744628906295,757.94616699218795,726.804319406231,682.70271736713903,717.70232788110002,751.93750911379004,735.46519867115205,735.75055572725705,725.29223275448601]
["EAST-E2L102C29","EAST",8,"E2L102C29",479,"SEMs per I&I Switch, BOX - 50 FT",1.59511983394623,1.87213134765625,1.9836724996566799,1.95497357845306,1.8518542051315301,1.89151871204376,1.99306428432465,1.8959367275237999,1.8616740703582799,1.92025334789622,1.8480989943294299,1.7709429116779001,1.61139185111617,1.5669282747439901,1.5600285854879901,1.4618621611831699]
["EAST-E2L103C3","EAST",8,"E2L103C3",482,"E/L Ratio, Privately-Owned, BOX - EQUIPPED",1.87950587272644,1.8234215974807699,1.8102401494979901,1.78766334056854,1.8041347265243499,1.73530280590057,1.7978030443191499,1.74810290336609,1.66328680515289,1.7473182002310499,1.7449466792463599,1.8041439913303701,1.7580003357129499,1.77546107857812,1.73756451268927,1.72171028089308]
["EAST-E2L103C6","EAST",8,"E2L103C6",485,"Interline circuity, BOX - EQUIPPED",1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999]
["EAST-E2L103C7","EAST",8,"E2L103C7",486,"Average circuity, BOX - EQUIPPED",1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999]
["EAST-E2L103C10","EAST",8,"E2L103C10",489,"CD per Interchange Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L103C14","EAST",8,"E2L103C14",493,"CD per Load & Unload Industry Switch, BOX - EQUIPP",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L103C17","EAST",8,"E2L103C17",496,"CM per Industry Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L103C20","EAST",8,"E2L103C20",499,"CM per Interterminal Switch, BOX - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["EAST-E2L103C25","EAST",8,"E2L103C25",504,"SEMs per Industry Switch, BOX - EQUIPPED",6.3804793357849103,7.488525390625,7.9346904754638699,7.8198938369751003,7.4074163436889604,7.5660753250122097,7.9722566604614302,7.5837464332580602,7.4466958045959499,7.6810133915848597,7.3923959773177303,7.0837716467115897,6.44556740446468,6.2677130989759799,6.2401143419519798,5.8474486447326699]
["EAST-E2L103C28","EAST",8,"E2L103C28",507,"SEMs per Interterminal Switch, BOX - EQUIPPED",7.6565747261047399,8.9862298965454102,9.5216293334960902,9.3838720321655291,8.8888998031616193,9.0792903900146502,9.5667095184326207,9.1004962921142596,8.93603610992432,9.2172160699018306,8.8708751727812807,8.5005259760539094,7.7346808853576103,7.5212557187711697,7.4881372103423702,7.0169383736792099]
["EAST-E2L104C2","EAST",8,"E2L104C2",510,"E/L Ratio, Railroad-Owned, GONDOLA - PLAIN",1.89685547351837,1.89614057540894,1.89870989322662,1.9290174245834399,1.91076076030731,1.91645860671997,1.94087421894073,1.96307384967804,1.96169292926788,2.00442220758748,1.95663827370812,1.90637218716514,1.8989643726590699,1.9525440229551301,1.9730211725471001,1.97528588995262]
["EAST-E2L104C3","EAST",8,"E2L104C3",511,"E/L Ratio, Privately-Owned, GONDOLA - PLAIN",1.98779773712158,1.9813580513000499,1.97496545314789,1.95970118045807,1.9418649673461901,1.9436582326889,1.9596022367477399,1.9236878156662001,1.9240527153015099,1.99430035977974,1.93947188795632,1.97894441861502,1.93437782464598,1.9613936719166001,1.9116111146928001,1.89807879535276]
["EAST-E2L104C6","EAST",8,"E2L104C6",514,"Interline circuity, GONDOLA - PLAIN",1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.151,1.151,1.151,1.151,1.151,1.151,1.151]
["EAST-E2L104C10","EAST",8,"E2L104C10",518,"CD per Interchange Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L104C13","EAST",8,"E2L104C13",521,"CD per I&I Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L104C16","EAST",8,"E2L104C16",524,"CD per Load & Unload Interterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L104C21","EAST",8,"E2L104C21",529,"CM per I&I Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L104C24","EAST",8,"E2L104C24",532,"Average Miles between Interchange Switches, GONDOLA - PLAIN",2356.06176757813,2169.83276367188,2040.29113769531,1947.57836914063,2147.54760742188,2342.61010742188,1694.51098632813,1757.92504882813,1315.06921386719,1114.6904956619701,1281.6233269214399,2013.78055123183,1973.4005378664499,1848.73561937404,1842.6288284581201,1813.1355636385499]
["EAST-E2L104C25","EAST",8,"E2L104C25",533,"SEMs per Industry Switch, GONDOLA - PLAIN",6.3804788589477504,7.488525390625,7.9346895217895499,7.8198943138122603,7.4074163436889604,7.5660748481750497,7.9722576141357404,7.5837459564209002,7.4466958045959499,7.6810133915848597,7.3923959773177303,7.0837716467115897,6.44556740446468,6.2677130989759702,6.2401143419519798,5.8474486447326699]
["EAST-E2L104C28","EAST",8,"E2L104C28",536,"SEMs per Interterminal Switch, GONDOLA - PLAIN",7.6565756797790501,8.9862298965454102,9.5216274261474592,9.3838729858398402,8.8889007568359393,9.0792903900146502,9.5667095184326207,9.1004962921142596,8.93603610992432,9.2172160699018306,8.8708751727812807,8.5005259760539005,7.7346808853576103,7.5212557187711697,7.4881372103423702,7.0169383736792099]
["EAST-E2L105C2","EAST",8,"E2L105C2",539,"E/L Ratio, Railroad-Owned, GONDOLA - EQUIPPED",1.8813490867614699,1.9022618532180799,1.9513148069381701,2.20249724388123,1.9769754409789999,1.9197372198104901,2.0015203952789302,1.9861202239990201,1.8590629100799601,2.0024587802573999,1.93964251791728,1.8935517096507499,1.8225901098370001,1.9481477223267001,1.9843763688929099,1.8542405847091299]
["EAST-E2L105C6","EAST",8,"E2L105C6",543,"Interline circuity, GONDOLA - EQUIPPED",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["EAST-E2L105C8","EAST",8,"E2L105C8",545,"Spotted-to-Pulled Ratio, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L105C13","EAST",8,"E2L105C13",550,"CD per I&I Switch, GONDOLA - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L105C17","EAST",8,"E2L105C17",554,"CM per Industry Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L105C20","EAST",8,"E2L105C20",557,"CM per Interterminal Switch, GONDOLA - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["EAST-E2L105C21","EAST",8,"E2L105C21",558,"CM per I&I Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L105C24","EAST",8,"E2L105C24",561,"Average Miles between Interchange Switches, GONDOLA - EQUIPPED",1315.20324707031,1044.10559082031,1018.17681884766,1001.25317382813,1057.36389160156,984.20147705078102,964.14617919921898,929.501953125,823.63641357421898,790.96147965249997,722.98161405047995,688.24872934861105,635.83920851519395,556.56158147999201,573.314790215578,534.51609316679298]
["EAST-E2L105C27","EAST",8,"E2L105C27",564,"SEMs per Intraterminal Switch, GONDOLA - EQUIPPED",9.5707187652587908,11.2327890396118,11.9020347595215,11.729841232299799,11.1111249923706,11.349113464355501,11.958387374877899,11.375617980956999,11.1700439453125,11.521520087377301,11.0885939659766,10.6256574700674,9.6683511066970205,9.4015696484639601,9.3601715129279697,8.7711729670990106]
["EAST-E2L106C2","EAST",8,"E2L106C2",568,"E/L Ratio, Railroad-Owned, HOPPER - COVERED",2.0314056873321502,2.0421829223632799,2.0606315135955802,2.0576088428497301,2.0554513931274401,2.0679728984832799,2.0566661357879599,2.06537961959839,2.0317237377166699,2.07272218608116,2.07214129572669,2.0356526715130498,2.0218340611353698,2.0352210044562198,2.0130553984072401,2.0249062850936599]
["EAST-E2L106C4","EAST",8,"E2L106C4",570,"E/L Ratio, All Freight Cars, HOPPER - COVERED",1.9921084642410301,1.9860272407531701,1.99670398235321,1.9798725843429601,1.9846447706222501,1.9949380159378101,1.9906636476516699,1.9965463876724201,1.98763847351074,2.0062906758063699,1.9926768722327299,1.97955899090192,1.9966585530704299,2.00463432097302,1.98367907155547,2.0005992444227298]
["EAST-E2L106C9","EAST",8,"E2L106C9",575,"CD per Industry Switch, HOPPER - COVERED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L106C13","EAST",8,"E2L106C13",579,"CD per I&I Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L106C16","EAST",8,"E2L106C16",582,"CD per Load & Unload Interterminal Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L106C17","EAST",8,"E2L106C17",583,"CM per Industry Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L106C20","EAST",8,"E2L106C20",586,"CM per Interterminal Switch, HOPPER - COVERED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
[{"$f":"B4482&\"-\"&D4482","v":"EAST-E2L106C23"},"EAST",8,"E2L106C23",589,"Average Miles between I&I Switches, HOPPER - COVERED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["EAST-E2L106C27","EAST",8,"E2L106C27",593,"SEMs per Intraterminal Switch, HOPPER - COVERED",9.5707187652587908,11.2327871322632,11.902035713195801,11.729840278625501,11.1111249923706,11.349114418029799,11.958386421203601,11.3756189346313,11.1700429916382,11.521520087377301,11.0885939659766,10.6256574700674,9.6683511066970205,9.4015696484639601,9.3601715129279697,8.7711729670990106]
["EAST-E2L106C29","EAST",8,"E2L106C29",595,"SEMs per I&I Switch, HOPPER - COVERED",1.59511971473694,1.87213122844696,1.9836723804473899,1.95497334003448,1.8518540859222401,1.89151883125305,1.99306440353394,1.8959366083145099,1.8616740703582799,1.92025334789622,1.8480989943294299,1.7709429116779001,1.61139185111617,1.5669282747439901,1.5600285854879901,1.4618621611831699]
["EAST-E2L107C6","EAST",8,"E2L107C6",601,"Interline circuity, HOPPER - OPEN TOP - GENERAL",1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.137,1.137,1.137,1.137,1.137,1.137,1.137]
["EAST-E2L107C9","EAST",8,"E2L107C9",604,"CD per Industry Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L107C12","EAST",8,"E2L107C12",607,"CD per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["EAST-E2L107C13","EAST",8,"E2L107C13",608,"CD per I&I Switch, HOPPER - OPEN TOP - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L107C16","EAST",8,"E2L107C16",611,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L107C19","EAST",8,"E2L107C19",614,"CM per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["EAST-E2L107C23","EAST",8,"E2L107C23",618,"Average Miles between I&I Switches, HOPPER - OPEN TOP - GENERAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["EAST-E2L107C25","EAST",8,"E2L107C25",620,"SEMs per Industry Switch, HOPPER - OPEN TOP - GENERAL",6.3804788589477504,7.48852634429932,7.9346899986267099,7.8198943138122603,7.4074168205261204,7.5660758018493697,7.9722566604614302,7.5837464332580602,7.4466962814331099,7.6810133915848597,7.3923959773177303,7.0837716467115897,6.44556740446468,6.2677130989759799,6.2401143419519798,5.8474486447326699]
["EAST-E2L108C2","EAST",8,"E2L108C2",626,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.0151662826538099,2.04326391220093,2.01946973800659,2.0467939376831099,2.0274884700775102,2.02526879310608,2.0630149841308598,2.0558326244354199,2.0116026401519802,2.0330924984390299,2.0615613364320202,2.0115328630612499,2.00601958302116,2.0438204756056702,2.0193142497640801,2.0024272525745701]
["EAST-E2L108C5","EAST",8,"E2L108C5",629,"Local circuity, HOPPER - OPEN TOP - SPECIAL",1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.202,1.202,1.202,1.202,1.202,1.202,1.202]
["EAST-E2L108C8","EAST",8,"E2L108C8",632,"Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L108C9","EAST",8,"E2L108C9",633,"CD per Industry Switch, HOPPER - OPEN TOP - SPECIAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L108C12","EAST",8,"E2L108C12",636,"CD per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["EAST-E2L108C16","EAST",8,"E2L108C16",640,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L108C21","EAST",8,"E2L108C21",645,"CM per I&I Switch, HOPPER - OPEN TOP - SPECIAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L108C23","EAST",8,"E2L108C23",647,"Average Miles between I&I Switches, HOPPER - OPEN TOP - SPECIAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["EAST-E2L108C27","EAST",8,"E2L108C27",651,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",9.5707178115844709,11.2327880859375,11.9020347595215,11.729841232299799,11.1111249923706,11.349113464355501,11.958386421203601,11.3756189346313,11.1700439453125,11.521520087377301,11.0885939659766,10.6256574700674,9.6683511066970205,9.4015696484639601,9.3601715129279697,8.7711729670990106]
["EAST-E2L109C1","EAST",8,"E2L109C1",654,"Average Tare Weight, REFRIGERATED - MECH",46.099998474121101,46.099998474121101,46.400001525878899,46.599998474121101,46.599998474121101,46.5,46.599998474121101,47,47.200000762939503,47.5,48.2,48.3,48.4,48.6,48.9,49.2]
["EAST-E2L109C4","EAST",8,"E2L109C4",657,"E/L Ratio, All Freight Cars, REFRIGERATED - MECH",1.7898223400116,1.75989973545074,1.75008344650269,1.75052726268768,1.72956347465515,1.71917247772217,1.71847283840179,1.70225262641907,1.6810462474823,1.6780799582599599,1.6671504470649201,1.6380476556495001,1.6531642390758401,1.56964562510022,1.4904352057419199,1.53499887463426]
["EAST-E2L109C5","EAST",8,"E2L109C5",658,"Local circuity, REFRIGERATED - MECH",1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.079,1.079,1.079,1.079,1.079,1.079,1.079]
["EAST-E2L109C8","EAST",8,"E2L109C8",661,"Spotted-to-Pulled Ratio, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L109C12","EAST",8,"E2L109C12",665,"CD per Interterminal Switch, REFRIGERATED - MECH",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["EAST-E2L109C17","EAST",8,"E2L109C17",670,"CM per Industry Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L109C19","EAST",8,"E2L109C19",672,"CM per Intraterminal Switch, REFRIGERATED - MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["EAST-E2L109C23","EAST",8,"E2L109C23",676,"Average Miles between I&I Switches, REFRIGERATED - MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["EAST-E2L109C26","EAST",8,"E2L109C26",679,"SEMs per Interchange Switch, REFRIGERATED - MECH",3.5092635154724099,4.1186895370483398,4.3640794754028303,4.30094194412231,4.07407903671265,4.1613416671752903,4.3847417831420898,4.17106056213379,4.0956826210021999,4.2245573653716697,4.0658177875247503,3.8960744056913699,3.5450620724555701,3.4472422044367899,3.4320628880735899,3.2160967546029702]
["EAST-E2L109C29","EAST",8,"E2L109C29",682,"SEMs per I&I Switch, REFRIGERATED - MECH",1.59511983394623,1.87213134765625,1.9836724996566799,1.95497345924377,1.8518542051315301,1.89151871204376,1.99306428432465,1.8959367275237999,1.8616739511489899,1.92025334789622,1.8480989943294299,1.7709429116779001,1.61139185111617,1.5669282747439901,1.5600285854879901,1.4618621611831699]
["EAST-E2L110C1","EAST",8,"E2L110C1",683,"Average Tare Weight, REFRIGERATED - NON-MECH",42.799999237060497,42.900001525878899,43.099998474121101,43.299999237060497,43.799999237060497,43.400001525878899,44,44.099998474121101,44.099998474121101,44.2,44.2,44.2,44.2,44.2,44.6,45.2]
["EAST-E2L110C4","EAST",8,"E2L110C4",686,"E/L Ratio, All Freight Cars, REFRIGERATED - NON-MECH",1.9366227388382,1.94895911216736,1.96491026878357,1.94960260391235,1.95335292816162,1.94834649562836,1.9522725343704199,1.9154791831970199,1.8887038230896001,1.9373784519642201,1.9270034181542,1.94175715695953,1.9432429880064199,1.9688444305512101,1.9313736971542299,1.9276776489495999]
["EAST-E2L110C8","EAST",8,"E2L110C8",690,"Spotted-to-Pulled Ratio, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L110C13","EAST",8,"E2L110C13",695,"CD per I&I Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L110C15","EAST",8,"E2L110C15",697,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - NON-MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L110C19","EAST",8,"E2L110C19",701,"CM per Intraterminal Switch, REFRIGERATED - NON-MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["EAST-E2L110C22","EAST",8,"E2L110C22",704,"Average CM per CD, Railroad-Owned, REFRIGERATED - NON-MECH",551.6376953125,586.05944824218795,578.45819091796898,613.00054931640602,571.51953125,560.348388671875,606.06268310546898,600.37634277343795,549.49572753906295,569.779600758588,594.31474828005503,639.35367377627995,568.48227593219599,584.28734233248201,595.38320590636295,594.72694897019699]
["EAST-E2L110C23","EAST",8,"E2L110C23",705,"Average Miles between I&I Switches, REFRIGERATED - NON-MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["EAST-E2L110C26","EAST",8,"E2L110C26",708,"SEMs per Interchange Switch, REFRIGERATED - NON-MECH",3.5092635154724099,4.1186895370483398,4.3640794754028303,4.30094194412231,4.07407903671265,4.1613416671752903,4.3847413063049299,4.17106056213379,4.0956830978393599,4.2245573653716697,4.0658177875247503,3.8960744056913699,3.5450620724555701,3.4472422044367899,3.4320628880735899,3.2160967546029702]
["EAST-E2L110C29","EAST",8,"E2L110C29",711,"SEMs per I&I Switch, REFRIGERATED - NON-MECH",1.59511971473694,1.87213122844696,1.9836726188659699,1.95497345924377,1.8518543243408201,1.89151883125305,1.99306440353394,1.8959366083145099,1.8616739511489899,1.92025334789621,1.8480989943294299,1.7709429116779001,1.61139185111617,1.5669282747439901,1.5600285854879901,1.4618621611831699]
["EAST-E2L111C5","EAST",8,"E2L111C5",716,"Local circuity, FLAT - TOFC",1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.069,1.069,1.069,1.069,1.069,1.069,1.069]
["EAST-E2L111C8","EAST",8,"E2L111C8",719,"Spotted-to-Pulled Ratio, FLAT - TOFC",1.14663481712341,1.1496064662933301,1.1334854364395099,1.1141271591186499,1.08945596218109,1.11075079441071,1.1093608140945399,1.10583400726318,1.0946965217590301,1.09727881240261,1.1051722646522699,1.09816622324584,1.08410658300038,1.08773746193578,1.1102588199032599,1.0915186609502701]
["EAST-E2L111C11","EAST",8,"E2L111C11",722,"CD per Intraterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L111C15","EAST",8,"E2L111C15",726,"CD per Load & Unload Intraterminal Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L111C18","EAST",8,"E2L111C18",729,"CM per Interchange Switch, FLAT - TOFC",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["EAST-E2L111C19","EAST",8,"E2L111C19",730,"CM per Intraterminal Switch, FLAT - TOFC",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["EAST-E2L111C22","EAST",8,"E2L111C22",733,"Average CM per CD, Railroad-Owned, FLAT - TOFC",551.6376953125,586.05938720703102,578.45819091796898,613.00054931640602,571.51953125,560.348388671875,606.062744140625,600.37628173828102,549.49578857421898,569.779600758588,594.31474828005503,639.35367377627995,568.48227593219599,584.28734233248201,595.38320590636295,594.72694897019699]
["EAST-E2L111C25","EAST",8,"E2L111C25",736,"SEMs per Industry Switch, FLAT - TOFC",6.3804788589477504,7.48852586746216,7.9346904754638699,7.8198938369751003,7.4074168205261204,7.5660748481750497,7.9722571372985804,7.5837464332580602,7.4466958045959499,7.6810133915848597,7.3923959773177303,7.0837716467115897,6.44556740446468,6.2677130989759799,6.2401143419519798,5.8474486447326699]
["EAST-E2L112C1","EAST",8,"E2L112C1",741,"Average Tare Weight, FLAT - MULTILEVEL",54.299999237060497,54.299999237060497,54.200000762939503,54.400001525878899,54.900001525878899,54.5,54,54,53.799999237060497,53.6,53.6,53.4,53.3,53.1,53.1,53.1]
["EAST-E2L112C4","EAST",8,"E2L112C4",744,"E/L Ratio, All Freight Cars, FLAT - MULTILEVEL",1.54029512405396,1.5534850358962999,1.5316956043243399,1.5506743192672701,1.57530033588409,1.55896997451782,1.5788543224334699,1.60300588607788,1.58562028408051,1.5763990221828901,1.5823511124123499,1.60293990155376,1.60267024507928,1.63783496770464,1.61369201454755,1.61898919163207]
["EAST-E2L112C7","EAST",8,"E2L112C7",747,"Average circuity, FLAT - MULTILEVEL",1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999]
["EAST-E2L112C11","EAST",8,"E2L112C11",751,"CD per Intraterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L112C14","EAST",8,"E2L112C14",754,"CD per Load & Unload Industry Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L112C15","EAST",8,"E2L112C15",755,"CD per Load & Unload Intraterminal Switch, FLAT - MULTILEVEL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L112C18","EAST",8,"E2L112C18",758,"CM per Interchange Switch, FLAT - MULTILEVEL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["EAST-E2L112C21","EAST",8,"E2L112C21",761,"CM per I&I Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L112C26","EAST",8,"E2L112C26",766,"SEMs per Interchange Switch, FLAT - MULTILEVEL",3.5092635154724099,4.1186895370483398,4.3640794754028303,4.30094242095947,4.0740795135498002,4.1613416671752903,4.3847417831420898,4.1710610389709499,4.0956830978393599,4.2245573653716697,4.0658177875247503,3.8960744056913699,3.5450620724555701,3.4472422044367899,3.4320628880735899,3.2160967546029702]
["EAST-E2L112C29","EAST",8,"E2L112C29",769,"SEMs per I&I Switch, FLAT - MULTILEVEL",1.59511971473694,1.87213122844696,1.9836726188659699,1.95497334003448,1.8518542051315301,1.89151871204376,1.99306440353394,1.8959367275237999,1.8616739511489899,1.92025334789622,1.8480989943294299,1.7709429116779001,1.61139185111617,1.5669282747439901,1.5600285854879901,1.4618621611831699]
["EAST-E2L113C4","EAST",8,"E2L113C4",773,"E/L Ratio, All Freight Cars, FLAT - GENERAL",2.6085059642791699,2.44644379615784,2.3362832069396999,2.2747380733489999,3.1010363101959202,3.31125831604004,2.8089330196380602,2.2170939445495601,2.2870543003082302,2.1153846153846199,2.1206349206349202,1.88241206030151,2.0758620689655198,2.0625782227784701,2.0493066255778101,2.3490304709141299]
["EAST-E2L113C7","EAST",8,"E2L113C7",776,"Average circuity, FLAT - GENERAL",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["EAST-E2L113C10","EAST",8,"E2L113C10",779,"CD per Interchange Switch, FLAT - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L113C11","EAST",8,"E2L113C11",780,"CD per Intraterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L113C14","EAST",8,"E2L113C14",783,"CD per Load & Unload Industry Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L113C17","EAST",8,"E2L113C17",786,"CM per Industry Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L113C22","EAST",8,"E2L113C22",791,"Average CM per CD, Railroad-Owned, FLAT - GENERAL",551.6376953125,586.05938720703102,578.458251953125,613.00061035156295,571.51959228515602,560.34844970703102,606.062744140625,600.37634277343795,549.49578857421898,569.779600758588,594.31474828005503,639.35367377627995,568.48227593219599,584.28734233248201,595.38320590636295,594.72694897019699]
["EAST-E2L113C25","EAST",8,"E2L113C25",794,"SEMs per Industry Switch, FLAT - GENERAL",6.3804793357849103,7.48852491378784,7.9346899986267099,7.8198943138122603,7.4074163436889604,7.5660758018493697,7.9722576141357404,7.5837464332580602,7.4466962814331099,7.6810133915848597,7.3923959773177303,7.0837716467115897,6.44556740446468,6.2677130989759799,6.2401143419519798,5.8474486447326699]
["EAST-E2L113C29","EAST",8,"E2L113C29",798,"SEMs per I&I Switch, FLAT - GENERAL",1.59511959552765,1.87213134765625,1.9836724996566799,1.95497334003448,1.8518542051315301,1.89151883125305,1.99306428432465,1.8959367275237999,1.8616740703582799,1.92025334789622,1.8480989943294299,1.7709429116779001,1.61139185111617,1.5669282747439901,1.5600285854879901,1.4618621611831699]
["EAST-E2L114C3","EAST",8,"E2L114C3",801,"E/L Ratio, Privately-Owned, FLAT - OTHER",1.84089696407318,1.8235940933227499,1.9440286159515401,1.9936060905456501,1.91689813137054,1.9013133049011199,1.9425401687622099,1.9202581644058201,1.8681793212890601,1.9091351794054501,1.90577202691584,1.89250062914185,1.88251774569556,1.99553741785033,1.9750511680429099,1.85823258945951]
["EAST-E2L114C6","EAST",8,"E2L114C6",804,"Interline circuity, FLAT - OTHER",1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.17,1.17,1.17,1.17,1.17,1.17,1.17]
["EAST-E2L114C7","EAST",8,"E2L114C7",805,"Average circuity, FLAT - OTHER",1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.155,1.155,1.155,1.155,1.155,1.155,1.155]
["EAST-E2L114C10","EAST",8,"E2L114C10",808,"CD per Interchange Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L114C14","EAST",8,"E2L114C14",812,"CD per Load & Unload Industry Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L114C18","EAST",8,"E2L114C18",816,"CM per Interchange Switch, FLAT - OTHER",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["EAST-E2L114C21","EAST",8,"E2L114C21",819,"CM per I&I Switch, FLAT - OTHER",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L114C25","EAST",8,"E2L114C25",823,"SEMs per Industry Switch, FLAT - OTHER",6.3804788589477504,7.48852586746216,7.9346899986267099,7.8198943138122603,7.4074163436889604,7.5660753250122097,7.9722571372985804,7.5837459564209002,7.44669532775879,7.6810133915848597,7.3923959773177303,7.0837716467115897,6.44556740446468,6.2677130989759702,6.2401143419519798,5.8474486447326699]
["EAST-E2L114C28","EAST",8,"E2L114C28",826,"SEMs per Interterminal Switch, FLAT - OTHER",7.6565752029418901,8.9862308502197301,9.5216283798217791,9.3838720321655291,8.8888998031616193,9.0792894363403303,9.5667085647583008,9.1004972457885707,8.93603515625,9.2172160699018306,8.8708751727812807,8.5005259760539094,7.7346808853576103,7.5212557187711697,7.4881372103423702,7.0169383736792099]
["EAST-E2L115C2","EAST",8,"E2L115C2",829,"E/L Ratio, Railroad-Owned, TANK <22,000 GAL",1.02510797977448,1.0210472345352199,1.03611016273499,1.0205540657043499,1.07265508174896,1.03137135505676,1.01525223255157,1.0158883333206199,1.0186020135879501,1.0283225612672799,1.06525540572351,1.0695725193213801,1.07595190380762,1.0781267589778201,1.0590608765824401,1.0907866956335499]
["EAST-E2L115C3","EAST",8,"E2L115C3",830,"E/L Ratio, Privately-Owned, TANK <22,000 GAL",2.0045475959777801,2.0103015899658199,2.0317757129669198,2.0331730842590301,2.01846480369568,2.0211806297302202,2.0288643836975102,2.02212333679199,2.0120668411254901,2.0161859629942001,2.01270883631096,2.0063554579154901,2.0121783006967502,2.01955674148225,2.0271508613918399,2.0184005513899601]
["EAST-E2L115C6","EAST",8,"E2L115C6",833,"Interline circuity, TANK <22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["EAST-E2L115C10","EAST",8,"E2L115C10",837,"CD per Interchange Switch, TANK <22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L115C14","EAST",8,"E2L115C14",841,"CD per Load & Unload Industry Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L115C17","EAST",8,"E2L115C17",844,"CM per Industry Switch, TANK <22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L115C21","EAST",8,"E2L115C21",848,"CM per I&I Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L115C24","EAST",8,"E2L115C24",851,"Average Miles between Interchange Switches, TANK <22,000 GAL",1248.86511230469,1352.88598632813,1525.43298339844,1672.83874511719,1802.70361328125,1710.06909179688,1311.46630859375,1203.17016601563,1195.83032226563,1569.8656869419699,1064.98326703773,1114.0077629575401,1159.12894405053,1123.15553216801,1117.9277163924501,1162.21941662166]
["EAST-E2L115C27","EAST",8,"E2L115C27",854,"SEMs per Intraterminal Switch, TANK <22,000 GAL",9.5707178115844709,11.2327880859375,11.9020347595215,11.729841232299799,11.1111240386963,11.349114418029799,11.958387374877899,11.3756189346313,11.1700439453125,11.521520087377301,11.0885939659766,10.6256574700674,9.6683511066970205,9.4015696484639601,9.3601715129279697,8.7711729670990106]
["EAST-E2L115C28","EAST",8,"E2L115C28",855,"SEMs per Interterminal Switch, TANK <22,000 GAL",7.6565747261047399,8.9862308502197301,9.5216274261474592,9.3838720321655291,8.8889007568359393,9.0792903900146502,9.5667095184326207,9.1004972457885707,8.93603610992432,9.2172160699018306,8.8708751727812807,8.5005259760539094,7.7346808853576103,7.5212557187711697,7.4881372103423702,7.0169383736792099]
["EAST-E2L116C2","EAST",8,"E2L116C2",858,"E/L Ratio, Railroad-Owned, TANK >=22,000 GAL",1.02510797977448,1.0210472345352199,1.03611016273499,1.0205540657043499,1.07265508174896,1.03137135505676,1.01525223255157,1.0158883333206199,1.0186020135879501,1.0283225612672799,1.06525540572351,1.0695725193213801,1.07595190380762,1.0781267589778201,1.0590608765824401,1.0907866956335499]
["EAST-E2L116C6","EAST",8,"E2L116C6",862,"Interline circuity, TANK >=22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["EAST-E2L116C10","EAST",8,"E2L116C10",866,"CD per Interchange Switch, TANK >=22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L116C13","EAST",8,"E2L116C13",869,"CD per I&I Switch, TANK >=22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L116C17","EAST",8,"E2L116C17",873,"CM per Industry Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L116C20","EAST",8,"E2L116C20",876,"CM per Interterminal Switch, TANK >=22,000 GAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["EAST-E2L116C21","EAST",8,"E2L116C21",877,"CM per I&I Switch, TANK >=22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L116C24","EAST",8,"E2L116C24",880,"Average Miles between Interchange Switches, TANK >=22,000 GAL",1248.86511230469,1352.88598632813,1525.43298339844,1672.83874511719,1802.70361328125,1710.06909179688,1311.46630859375,1203.17016601563,1195.83032226563,1569.8656869419699,1064.98326703773,1114.0077629575401,1159.12894405053,1123.15553216801,1117.9277163924501,1162.21941662166]
["EAST-E2L116C27","EAST",8,"E2L116C27",883,"SEMs per Intraterminal Switch, TANK >=22,000 GAL",9.5707178115844709,11.2327880859375,11.9020347595215,11.729841232299799,11.1111240386963,11.349114418029799,11.958387374877899,11.3756189346313,11.1700439453125,11.521520087377301,11.0885939659766,10.6256574700674,9.6683511066970205,9.4015696484639601,9.3601715129279697,8.7711729670990106]
["EAST-E2L117C2","EAST",8,"E2L117C2",887,"E/L Ratio, Railroad-Owned, ALL OTHER FREIGHT CARS",1.02510797977448,1.0210472345352199,1.03611016273499,1.0205540657043499,1.07265508174896,1.03137135505676,1.01525223255157,1.0158883333206199,1.0186020135879501,1.0283225612672799,1.06525540572351,1.0695725193213801,1.07595190380762,1.0781267589778201,1.0590608765824401,1.0907866956335499]
["EAST-E2L117C6","EAST",8,"E2L117C6",891,"Interline circuity, ALL OTHER FREIGHT CARS",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["EAST-E2L117C9","EAST",8,"E2L117C9",894,"CD per Industry Switch, ALL OTHER FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L117C13","EAST",8,"E2L117C13",898,"CD per I&I Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L117C16","EAST",8,"E2L117C16",901,"CD per Load & Unload Interterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L117C17","EAST",8,"E2L117C17",902,"CM per Industry Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["EAST-E2L117C20","EAST",8,"E2L117C20",905,"CM per Interterminal Switch, ALL OTHER FREIGHT CARS",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["EAST-E2L117C23","EAST",8,"E2L117C23",908,"Average Miles between I&I Switches, ALL OTHER FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["EAST-E2L117C28","EAST",8,"E2L117C28",913,"SEMs per Interterminal Switch, ALL OTHER FREIGHT CARS",7.6565747261047399,8.9862308502197301,9.5216274261474592,9.3838720321655291,8.8889007568359393,9.0792903900146502,9.5667095184326207,9.1004972457885707,8.93603610992432,9.2172160699018306,8.8708751727812807,8.5005259760539094,7.7346808853576103,7.5212557187711697,7.4881372103423702,7.0169383736792099]
["EAST-E2L118C2","EAST",8,"E2L118C2",916,"E/L Ratio, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.79027247428894,1.78958344459534,1.7894258499145499,1.7804994583129901,1.76683497428894,1.76168549060822,1.7680983543396001,1.7734432220459,1.7525115013122601,1.76946407182896,1.7933189653936801,1.78123950234568,1.7540066759269499,1.77407506616107,1.7562356811787601,1.7725525130969499]
["EAST-E2L118C6","EAST",8,"E2L118C6",920,"Interline circuity, AVERAGE ALL FREIGHT CARS",1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.157,1.157,1.157,1.157,1.157,1.157,1.157]
["EAST-E2L118C9","EAST",8,"E2L118C9",923,"CD per Industry Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["EAST-E2L118C12","EAST",8,"E2L118C12",926,"CD per Interterminal Switch, AVERAGE ALL FREIGHT CARS",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["EAST-E2L118C13","EAST",8,"E2L118C13",927,"CD per I&I Switch, AVERAGE ALL FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["EAST-E2L118C16","EAST",8,"E2L118C16",930,"CD per Load & Unload Interterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["EAST-E2L118C19","EAST",8,"E2L118C19",933,"CM per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["EAST-E2L118C24","EAST",8,"E2L118C24",938,"Average Miles between Interchange Switches, AVERAGE ALL FREIGHT CARS",1369.09533691406,1344.37463378906,1377.44128417969,1451.49011230469,1501.04748535156,1509.22143554688,1244.36828613281,1235.64916992188,1229.57885742188,1161.94485653169,1126.85649165118,1155.34835828732,1151.54982142929,1125.7989018507999,1153.89140381063,1146.4407348228201]
["EAST-E2L118C27","EAST",8,"E2L118C27",941,"SEMs per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",9.5707187652587908,11.2327880859375,11.902035713195801,11.729841232299799,11.111125946044901,11.3491106033325,11.958387374877899,11.375617980956999,11.170042037963899,11.521520087377301,11.0885939659766,10.6256574700674,9.6683511066970205,9.4015696484639601,9.3601715129279697,8.7711729670990106]
["EAST-E2L202C1","EAST",8,"E2L202C1",945,"Average TCUs Per Flat Car",4.1900000000000004,4.12,4.12,4.0999999999999996,4.57,4.53,4.4000000000000004,4.32,4.4400000000000004,4.6018590000000001,4.4826079999999999,4.399114,4.5770600000000004,4.6159309999999998,4.5059690000000003,4.5779800000000002]
["EAST-E2L205C1","EAST",8,"E2L205C1",948,"Linehaul Miles Per TCU Day",343,343,343,343,343,343,343,343,343,343,343,343,343,343,343,343]
["EAST-E2L208C1","EAST",8,"E2L208C1",951,"Average Locomotive Units - Unit Train",2.2273113727569598,2.24293041229248,2.3166477680206299,2.3147726058960001,2.3056218624114999,2.2829296588897701,2.3305742740631099,2.3721907138824498,2.3426361083984402,2.4189428699448099,2.4815399683122101,2.4040024548166099,2.4288296093944499,2.3712985431334501,2.30290012557237,2.2243691662801499]
["EAST-E2L209C1","EAST",8,"E2L209C1",952,"Average Locomotive Units - Way Train",1.5174362659454299,1.5141737461090099,1.53072190284729,1.50337266921997,1.5249670743942301,1.5223257541656501,1.5618268251419101,1.55205237865448,1.5532763004303001,1.5492666357373099,1.4524961720618901,1.4419462718724401,1.71242380667182,1.63278657083467,1.63541331323161,1.6149281565756299]
["EAST-E2L212C1","EAST",8,"E2L212C1",955,"Average Gross Tons - Way Train",1654.09143066406,1641.36145019531,1671.30847167969,1646.26892089844,1863.48022460938,1829.11218261719,1702.57531738281,1782.90100097656,1880.88635253906,1786.48438910971,1947.2151959416101,2151.8947793570701,2418.0265395146398,2262.75014734253,2315.6267099294,2488.1115729676999]
["EAST-E2L215C1","EAST",8,"E2L215C1",958,"Train Crews (Excl Train Switching)",675911.375,654282.75,705776.9375,585976.875,662604.1875,733011.1875,729599.9375,699717.9375,778883.25,808529.47526984301,724587.00160801003,719826.33088990604,708066.47043182596,664746.48197685496,532605.86918847496,570423.368007891]
["EAST-E2L220C1","EAST",8,"E2L220C1",963,"Constant Cost Markup Ratio",1.38632571697235,1.4070796966552701,1.3950209617614699,1.46003365516663,1.4319832324981701,1.40364730358124,1.3967037200927701,1.3992321491241499,1.39308428764343,1.41278195871158,1.4280088701397999,1.4340931768168099,1.4370689506059899,1.4326405776856499,1.4744494818282801,1.46862803067548]
["EAST-E2L302C1","EAST",8,"E2L302C1",966,"Residual Factor, Station Clerical, Railroad-Owned",18.8254886503011,21.654789895260599,19.039551374067099,25.065657973914298,19.546033222461499,19.0529114567269,26.798506740785999,30.104026995496632,26.014923179206299,24.840380494622899,22.745819294518999,23.447850008688899,22.829382739269899,26.9061424557311,25.230426572411144,22.7789672927663]
["EAST-E2L304C1","EAST",8,"E2L304C1",970,"Residual Factor, I&I Switching, Railroad-Owned",21.4490899818238,25.1837813082461,28.2808558748455,25.380976474179299,26.615704252688499,30.005778913412001,28.9905993459782,37.099961135077095,33.299864588376003,31.0789451841245,30.624689785768901,34.4616575479467,33.800330043937102,29.7460123306189,32.495249995008905,34.2283223975504]
[{"$f":"B4866&\"-\"&D4866","v":"EAST-E2L305C2"},"EAST",8,"E2L305C2",973,"Residual Factor, Mileage, Privately-Owned",-0.50794373940540405,-0.40351417158707897,-1.49540654608315,-0.37273534079847898,-1.1976440151638901,-1.4705518341271899,-1.63329008191534,-0.8056559906911589,-2.2627087627956599,-1.1557248270134199,-1.11176490053991,-2.06035708526016,-2.1714323734609899,-0.60058361756144196,-1.594195744916173,-1.7041701505892399]
["KCS-E1L101C3","KCS",5,"E1L101C3",3,"Gross Ton Mile (GTM), ROI Expense",1.6018775058910301E-3,1.0701542487368001E-3,2.0039051305502701E-3,2.2847787477076101E-3,2.7434707153588499E-3,3.1763694714754798E-3,3.2641240395605599E-3,3.6807970609515901E-3,3.7003736943006498E-3,3.7776609641063399E-3,3.68627278954523E-3,3.8734323213751799E-3,4.8544220992127298E-3,3.5847644187907901E-3,3.3341721690671698E-3,3.9441716841912599E-3]
["KCS-E1L102C1","KCS",5,"E1L102C1",4,"Car Mile (CM) - Other Than Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L104C1","KCS",5,"E1L104C1",10,"Train Mile (TM) - Crew, OPR Expense",9.2487163543701207,9.9810380935668892,8.87207126617432,10.0166311264038,9.37921142578125,9.6949443817138707,10.4321393966675,10.7770385742188,11.8414916992188,12.918189068843301,13.840043613319001,13.853539631633399,13.256704599219701,14.8243646850209,17.779499617234801,19.043327644405899]
["KCS-E1L104C3","KCS",5,"E1L104C3",12,"Train Mile (TM) - Crew, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L105C3","KCS",5,"E1L105C3",15,"Locomotive Unit Mile (LUM), ROI Expense",0.233833938837051,0.34373530745506298,0.40220305323600802,0.35968279838562001,0.35255479812622098,0.53346508741378795,0.56762194633483898,1.1851876974105799,1.7828609943389899,1.7376032494696301,1.62076135423345,1.7460454679062201,2.1451714315221602,1.6802575173343699,1.52541529965677,1.8422849879659799]
["KCS-E1L106C3","KCS",5,"E1L106C3",18,"CLOR (Carloads Handled) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L108C1","KCS",5,"E1L108C1",22,"CLOT (Carloads Orig Or Term) - Other, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L109C1","KCS",5,"E1L109C1",25,"CLOT (Carloads Orig Or Term) - Clerical, OPR Expense",10.2326354980469,9.2003107070922905,10.279279708862299,8.5873289108276403,6.2873334884643599,6.5101680755615199,7.4406299591064498,8.1274890899658203,6.8073620796203604,5.7841314217192199,9.3102343368066904,6.2301547482651198,3.8817027719828401,4.3942597337789397,4.3667286146996203,3.7325175677389599]
["KCS-E1L110C1","KCS",5,"E1L110C1",28,"Car Mile (CM) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L110C2","KCS",5,"E1L110C2",29,"Car Mile (CM) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L112C2","KCS",5,"E1L112C2",35,"Ton Miles In Lake Transfer Service, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L113C1","KCS",5,"E1L113C1",37,"Tons Handled at Coal Terminals, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L114C1","KCS",5,"E1L114C1",40,"Tons Handled at Ore Terminals, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L115C1","KCS",5,"E1L115C1",43,"Tons Handled at Other Marine Terminals, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L116C2","KCS",5,"E1L116C2",47,"Refrigerated Car Miles, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L117C2","KCS",5,"E1L117C2",50,"Protective Service Reefer TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L118C2","KCS",5,"E1L118C2",53,"Refrigerated TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L118C3","KCS",5,"E1L118C3",54,"Refrigerated TCU Days, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L120C3","KCS",5,"E1L120C3",60,"TCUs Loaded And Unloaded (L&UL), ROI Expense",2.7205016613006601,2.6390411853790301,6.7513012886047399,4.6135015487670898,3.9372298717498802,5.3001251220703098,4.8453269004821804,4.7864465713501003,4.1962866783142099,8.4789530232656602,8.7462538981765405,9.0214940111026305,8.8225716971257597,7.0123025927872504,5.7580025938121802,6.47566888940041]
["KCS-E1L121C2","KCS",5,"E1L121C2",62,"MVUs Loaded And Unloaded (L&UL), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L122C2","KCS",5,"E1L122C2",65,"TCUs Picked Up and Delivered (PU&D), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L201C2","KCS",5,"E1L201C2",68,"CM(R), DRL Expense, Railroad-Owned, BOX - 40 FT",9.2020742595195798E-2,6.9540366530418396E-2,9.0952031314373002E-2,7.0064477622509003E-2,6.0325361788272899E-2,6.4686179161071805E-2,6.5431423485279097E-2,7.5201779603958102E-2,3.3898785710334799E-2,-4.3851461934191302E-2,-9.2292643100108901E-2,-0.115897504619475,-9.6640927620318895E-2,-7.3821267606956203E-2,-0.10981907782151901,-7.4820347953160102E-2]
["KCS-E1L201C6","KCS",5,"E1L201C6",72,"CM(Y), ROI Expense, Railroad-Owned, BOX - 40 FT",8.3158016204833998E-2,8.6915396153926794E-2,0.116884484887123,1.36028160341084E-3,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L201C9","KCS",5,"E1L201C9",75,"CD(R), ROI Expense, Railroad-Owned, BOX - 40 FT",5.1892619132995597,4.65960788726807,8.5319957733154297,6.1203345656395E-2,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L201C10","KCS",5,"E1L201C10",76,"CD(Y), OPR Expense, Railroad-Owned, BOX - 40 FT",1.3244321346282999,2.4284441471099898,2.7746875286102299,1.39817690849304,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L201C13","KCS",5,"E1L201C13",79,"CM(R), DRL Expense, Privately-Owned, BOX - 40 FT",0.40923479199409502,0.39594233036041299,0.34801954030990601,0.38102772831916798,0.29335319995880099,0.329200148582459,0.32030877470970198,0.49586102366447399,0.32844176888465898,0.38004504558704999,0.39817845696736598,0.386193020069245,0.39378887532808898,0.42837191295606802,0.40643786399193299,0.398909408193722]
["KCS-E1L202C6","KCS",5,"E1L202C6",85,"CM(Y), ROI Expense, Railroad-Owned, BOX - 50 FT",8.3158016204833998E-2,8.6915396153926794E-2,0.116884484887123,1.36028160341084E-3,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L202C8","KCS",5,"E1L202C8",87,"CD(R), DRL Expense, Railroad-Owned, BOX - 50 FT",81.653610229492202,113.62245941162099,29.237270355224599,23.1266784667969,20.534734725952099,22.538249969482401,24.272565841674801,25.834373474121101,12.88649559021,-11.3704425618608,-20.7943490130436,-30.971031097830998,-26.8251115844384,-21.6653854728239,-31.725682318049099,-31.364898034809201]
["KCS-E1L202C11","KCS",5,"E1L202C11",90,"CD(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",81.653610229492202,113.62245941162099,29.237270355224599,23.126680374145501,20.534734725952099,22.538249969482401,24.272565841674801,25.834375381469702,12.8864946365356,-11.3704425618608,-20.7943490130436,-30.971031097830998,-26.8251115844384,-21.6653854728239,-31.725682318049099,-31.364898034809201]
["KCS-E1L203C1","KCS",5,"E1L203C1",93,"CM(R), OPR Expense, Railroad-Owned, BOX - EQUIPPED",3.0803740024566699E-2,3.6588434129953398E-2,2.2771995514631299E-2,1.85540746897459E-2,1.38046480715275E-2,2.04384047538042E-2,2.18543577939272E-2,2.00162827968597E-2,4.74718883633614E-2,2.18945037902766E-2,3.7472283043989599E-2,6.5857881683367994E-2,8.4931490837096807E-2,0.178789590978607,0.127616279633635,0.121289577715028]
["KCS-E1L203C5","KCS",5,"E1L203C5",97,"CM(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED",-4.9615394324064303E-2,-6.2574334442615495E-2,-6.2652356922626495E-2,-4.1513081640005098E-2,-3.8307607173919699E-2,-5.2576392889022799E-2,-2.9643336310982701E-2,-1.8845064565539402E-2,-8.06010738015175E-2,-9.8070161937481401E-2,-8.8232496327128804E-2,-6.5677401641543495E-2,-7.6836515081414897E-2,-9.9234024428106499E-2,-0.107257830072697,-0.14058069843933699]
["KCS-E1L203C8","KCS",5,"E1L203C8",100,"CD(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED",8.2403888702392596,1.0191063880920399,13.1963500976563,19.3370265960693,12.8700160980225,11.649838447570801,14.5495195388794,15.197033882141101,5.19881296157837,3.6448042733502799,0.40323131229055698,-1.8380025875397199,0.13667027290354999,-1.3531768948685901,0.31516980146822299,-11.0783515331347]
["KCS-E1L203C9","KCS",5,"E1L203C9",101,"CD(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED",1.5012636184692401,1.9533764123916599,1.9777466058731099,2.4559972286224401,2.29849028587341,2.3654696941375701,3.0463449954986599,10.0771675109863,6.7316136360168501,-0.62526895897106105,8.0034304178826492,16.755662368721001,11.9399950971801,8.9037725914643104,7.9327202542156696,10.088308873852]
["KCS-E1L204C1","KCS",5,"E1L204C1",106,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",1.5833041397854701E-3,1.4259834773838499E-2,4.1824571788310998E-2,4.2785108089447001E-2,3.3194925636053099E-2,1.3799852458760099E-3,2.5041000917553902E-3,4.1101728565990899E-3,1.36576015502214E-2,6.3904686146225697E-3,1.7852965647439299E-2,4.1074906329383098E-2,5.33524247529217E-2,0.107037910069522,0.103133573497452,0.11206127025330501]
["KCS-E1L204C3","KCS",5,"E1L204C3",108,"CM(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",1.5114255947992199E-3,1.90250761806965E-3,1.7054511699825499E-3,2.5542546063661601E-3,1.87051855027676E-3,3.1595479231327798E-3,8.3531765267252905E-3,9.74688678979874E-3,5.1723085343837703E-2,0.106021822272461,7.2049059723494305E-2,6.9756589079911502E-2,6.8667267510071503E-2,3.2633658017350901E-2,3.4723259009779399E-2,4.2330105840903499E-2]
["KCS-E1L204C7","KCS",5,"E1L204C7",112,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",0.12966559827327701,1.2419971227645901,3.7920298576354998,3.9693737030029301,3.1397957801818799,0.12781120836734799,0.23178519308567,0.36948290467262301,1.15451407432556,0.52736502107716399,1.48790806447721,3.24725853754676,4.2233594066913902,8.8238249753665308,8.1026776964932505,8.8704184946437294]
["KCS-E1L204C10","KCS",5,"E1L204C10",115,"CD(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",0.12966559827327701,1.2419971227645901,3.7920296192169198,3.9693734645843501,3.1397957801818799,0.12781125307083099,0.23178519308567,0.36948287487030002,1.15451407432556,0.52736502107716399,1.48790806447721,3.24725853754676,4.2233594066913902,8.8238249753665308,8.1026776964932505,8.8704184946437294]
["KCS-E1L205C1","KCS",5,"E1L205C1",119,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",1.8502820283174501E-2,2.6056071743369099E-2,3.1333088874816901E-2,3.0794754624366798E-2,2.36766245216131E-2,1.0698864236474001E-2,9.6806967630982399E-3,8.2431305199861492E-3,1.4560363255441199E-2,7.1476095952076402E-3,4.3397910307427399E-3,2.3516875203486698E-3,0,0,0,0]
["KCS-E1L205C4","KCS",5,"E1L205C4",122,"CM(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",4.8107333481311798E-2,6.77457749843597E-2,8.1466078758239704E-2,8.0066271126270294E-2,6.15592002868652E-2,2.7817010879516602E-2,2.51698140054941E-2,2.1432146430015599E-2,3.7856921553611797E-2,1.8583784947539799E-2,1.1283456679931201E-2,6.1143875529065502E-3,0,0,0,0]
["KCS-E1L205C7","KCS",5,"E1L205C7",125,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",1.00076484680176,1.55664670467377,2.28835821151733,2.4823622703552202,2.0518348217010498,0.92821592092514005,0.84833937883377097,0.732200026512146,1.34920883178711,0.66417562672667896,0.40102688973989797,0.21507953148085901,0,0,0,0]
["KCS-E1L205C8","KCS",5,"E1L205C8",126,"CD(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",12.547401428222701,17.009569168090799,12.7738027572632,22.397600173950199,19.233470916748001,19.1343994140625,20.789981842041001,17.773921966552699,15.4291286468506,13.9577931059835,15.2705293516751,14.9708309671714,10.2672479808363,13.4346516867798,17.613103906083499,11.147047969274601]
["KCS-E1L205C13","KCS",5,"E1L205C13",131,"CM(R), DRL Expense, Privately-Owned, GONDOLA - EQUIPPED",2.7681680876412398E-5,3.5568948078434901E-5,8.2971462688874494E-5,3.4044427593471503E-5,1.38630193760036E-5,1.9341140985488899E-2,1.0583487892290599E-5,2.2593452740693499E-5,1.24448060887516E-5,3.0376113618873601E-2,2.01543513424523E-2,1.23657013363603E-2,3.7489955819157098E-3,4.4740396217598502E-4,1.3307655451925699E-3,4.8533010004884898E-5]
["KCS-E1L206C2","KCS",5,"E1L206C2",133,"CM(R), DRL Expense, Railroad-Owned, HOPPER - COVERED",7.3712915182113604E-3,-1.41210982110351E-3,-1.12988837063313E-2,-1.46683305501938E-2,-3.9131855592131597E-3,7.6383474515751004E-4,1.8591230036690801E-3,2.97430064529181E-3,-5.3281104192137701E-3,-6.3879997022634003E-3,-1.36341716905888E-2,-1.4491479871799001E-2,-1.4611097307053801E-2,-2.2506317278485601E-2,-2.62152400087656E-2,-2.7933938829585399E-2]
["KCS-E1L206C6","KCS",5,"E1L206C6",137,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED",2.1849682554602599E-2,2.6633938774466501E-2,1.6596462577581399E-2,1.6972247511148501E-2,1.7319316044449799E-2,1.9959177821874601E-2,5.0628274679184002E-2,9.9270872771740001E-2,0.13141310214996299,0.25231431248629399,0.161763242587178,0.178807279157042,0.281900263689838,0.186546835150005,0.14903483868914799,0.17327971562953501]
["KCS-E1L206C9","KCS",5,"E1L206C9",140,"CD(R), ROI Expense, Railroad-Owned, HOPPER - COVERED",1.1326754093170199,1.4978152513503999,1.08879423141479,1.08204853534698,1.04000055789948,1.0660378932952901,3.1068806648254399,5.99387407302856,8.1774129867553693,15.849456105953101,10.887827094545599,11.9144251433713,18.576883931979999,13.109640140174401,10.6730475585343,12.2711408110862]
["KCS-E1L206C13","KCS",5,"E1L206C13",144,"CM(R), DRL Expense, Privately-Owned, HOPPER - COVERED",1.5994032844901099E-2,1.12053751945496E-2,1.0525012388825399E-2,8.5746385157108307E-3,5.7697361335158296E-3,4.6382294967770602E-3,3.0512579251080799E-3,3.3705960959196099E-3,3.3880607225000902E-3,6.6601886783651304E-4,8.3877469251156201E-4,1.0156570912284501E-4,3.62543657882511E-4,8.6287545637281704E-5,2.3065124688367501E-2,7.2458588767041095E-4]
["KCS-E1L207C3","KCS",5,"E1L207C3",147,"CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",7.0304092951118903E-3,2.3089138790965101E-2,1.95108465850353E-2,4.3327488005161299E-2,4.1722208261489903E-2,1.13955745473504E-2,5.3090403525857302E-5,3.9900700357975398E-5,0.35599619150161699,0.29284963688076499,0.41124615230609701,0.38360277751042599,0.221420755783933,9.8051697185344497E-2,0.132304934523747,0.18505371882472299]
["KCS-E1L207C6","KCS",5,"E1L207C6",150,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.82790532708168E-2,6.0031782835721997E-2,5.0728242844343199E-2,0.11265131086111101,0.108477808535099,2.96285003423691E-2,1.3803500041831301E-4,1.0374198609497399E-4,0.925589740276337,0.76140905588998997,1.0692399959958501,0.99736722152710899,0.57569396503822501,0.25493441268189598,0.343992829761741,0.48113966894427701]
["KCS-E1L207C7","KCS",5,"E1L207C7",151,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",0.72272068262100198,1.5648610591888401,28.794054031372099,39.2085151672363,57.236953735351598,0.11467894166707999,7.4615642428398105E-2,6.1055719852447503E-2,0.275881737470627,0.13181090716270999,0.83108209344587503,1.7140957263376599,1.7338355886461001,73.807932678685802,117.196961362138,202.69552248974199]
["KCS-E1L207C12","KCS",5,"E1L207C12",156,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",0.57615894079208396,2.0069651603698699,1.77150225639343,4.2210097312927202,4.0578098297119096,1.14883232116699,4.2879050597548502E-3,3.7567385006695999E-3,43.143386840820298,36.143355914787698,37.413135273268303,36.264143808234003,21.998173137915199,15.7491963779936,19.116383674016799,26.676594707204099]
["KCS-E1L208C1","KCS",5,"E1L208C1",158,"CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.57313551753759E-2,2.21202876418829E-2,1.8454590812325498E-2,1.7525661736726799E-2,1.31708234548569E-2,1.3025392778217799E-2,1.15739908069372E-2,2.6262030005455E-3,1.9867308437824202E-3,4.1263943651280201E-3,2.4220820700600601E-3,1.63001709716015E-3,0,0,0,0]
["KCS-E1L208C5","KCS",5,"E1L208C5",162,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",3.7268653512001003E-2,5.3968325257301303E-2,4.8360843211412402E-2,5.50031065940857E-2,6.5373830497264904E-2,9.2615067958831801E-2,0.13735577464103699,0.106534525752068,7.0760130882263197E-2,3.2917830623774402E-2,3.9276244863006002E-2,1.3272511763761499E-2,1.9399353836308499E-2,2.26985723045116E-2,9.9474786225882909E-3,7.8163681660734698E-3]
["KCS-E1L208C8","KCS",5,"E1L208C8",165,"CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",10.421949386596699,2.81578922271729,6.4689292907714799,14.0274648666382,17.627315521240199,28.569297790527301,55.404525756835902,32.1980171203613,7.0844855308532697,2.45201187777915,1.6224798523294199,1.16260608980822,1.2996719208936001,0.79273842382693505,0.61066526625699302,0.36963565662235298]
["KCS-E1L208C12","KCS",5,"E1L208C12",169,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.19075195491313901,4.8369374126195901E-2,4.3634671717882198E-2,2.2448293864726999E-2,3.2989457249641398E-2,2.85482052713633E-2,3.00475284457207E-2,5.9096035547554502E-3,7.2861328953877102E-4,1.459019486745E-3,7.65844687387478E-4,5.9212273138874096E-4,0,0,0,0]
["KCS-E1L209C2","KCS",5,"E1L209C2",172,"CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",0.111177273094654,0.12823377549648299,0.118160702288151,0.16489455103874201,0.148522779345512,0.12535253167152399,0.123830862343311,8.0544471740722698E-2,0.12745569646358501,0.119310904100634,0,0,0,0,0,0]
["KCS-E1L209C5","KCS",5,"E1L209C5",175,"CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",0.289061099290848,0.33340790867805498,0.30721798539161699,0.42872601747512801,0.38615921139717102,0.325916558504105,0.32196030020713801,0.20941562950611101,0.331384778022766,0.31020835066164798,0,0,0,0,0,0]
["KCS-E1L209C7","KCS",5,"E1L209C7",177,"CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",0.25549408793449402,1.1986734867095901,83.123825073242202,99.708206176757798,129.55905151367199,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L209C10","KCS",5,"E1L209C10",180,"CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",0.25549408793449402,1.1986734867095901,83.123825073242202,99.708206176757798,129.55905151367199,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L210C1","KCS",5,"E1L210C1",184,"CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",7.9323453828692402E-3,2.42971628904343E-2,3.39764952659607E-2,1.32829369977117E-2,6.2614148482680303E-3,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L210C4","KCS",5,"E1L210C4",187,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",2.0624110475182499E-2,6.3172571361064897E-2,8.8338807225227398E-2,3.4535661339759799E-2,1.62797085940838E-2,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L210C7","KCS",5,"E1L210C7",190,"CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",0.92006516456604004,2.9422569274902299,4.8733620643615696,2.1934361457824698,1.1668313741684,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L210C11","KCS",5,"E1L210C11",194,"CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",103.728713989258,51.649879455566399,57.746963500976598,81.7994384765625,66.789924621582003,64.135955810546903,72.731025695800795,84.960960388183594,30.073310852050799,26.935872533543499,0,0,17.8712169798413,0,0,0]
["KCS-E1L211C1","KCS",5,"E1L211C1",197,"CM(R), OPR Expense, Railroad-Owned, FLAT - TOFC",7.3457378894090696E-3,2.0413611084222801E-2,1.94127503782511E-2,1.7617167904972999E-2,5.89641531405505E-5,0,1.3600963029603E-5,2.3269587472896098E-5,8.0371049989480498E-5,3.9706086299703497E-5,2.4622618237259901E-5,1.3588480711161199E-5,0,0,0,0]
["KCS-E1L211C4","KCS",5,"E1L211C4",200,"CM(Y), OPR Expense, Railroad-Owned, FLAT - TOFC",1.9098917022347499E-2,5.3075402975082397E-2,5.0473194569349303E-2,4.58046719431877E-2,1.5330690075643401E-4,0,3.5362565540708601E-5,6.0500835388665999E-5,2.0896470232401E-4,1.0323582437922899E-4,6.4018807416875705E-5,3.5330049849019202E-5,0,0,0,0]
["KCS-E1L211C6","KCS",5,"E1L211C6",202,"CM(Y), ROI Expense, Railroad-Owned, FLAT - TOFC",4.9356920644640897E-3,1.71595741994679E-3,1.6154986806213899E-3,5.3366271458798999E-5,5.17204352945555E-6,0,1.20079630505643E-6,2.60353908743127E-6,4.5767310439259703E-6,4.3120306514138797E-6,2.6605453615461799E-6,1.4976625330866301E-6,0,0,0,0]
["KCS-E1L211C9","KCS",5,"E1L211C9",205,"CD(R), ROI Expense, Railroad-Owned, FLAT - TOFC",0.258689165115356,5.8234602212905898E-2,5.1809515804052401E-2,-1.52777563780546E-2,1.7157589900307401E-4,0,5.2877418056596098E-5,9.4587587227579206E-5,1.4218999422155299E-4,1.2653953268870399E-4,8.1991643601800701E-5,4.56870452147509E-5,0,0,0,0]
["KCS-E1L211C13","KCS",5,"E1L211C13",209,"CM(R), DRL Expense, Privately-Owned, FLAT - TOFC",0.12925280630588501,0.174183815717697,0.17897963523864699,0.192753776907921,0.16789130866527599,0.172544971108437,0.14746807515621199,0.13750495016574901,0.14700134098529799,0.14920878694712,0.152527352160369,0.147420821467561,0.16492845706656001,0.169922417078579,0.17650511800762,0.19685347836102399]
["KCS-E1L212C3","KCS",5,"E1L212C3",212,"CM(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",4.1895047761499899E-3,4.2702131904661699E-3,2.5725089013576501E-2,1.7124036327004401E-2,5.6998855434358103E-3,1.7583980225026601E-3,1.63027225062251E-3,1.87423880561255E-4,1.8513162136077901,2.0226535318521202,2.4456201683213301,1.9486772556084699,2.3720684002641601,1.4918481920417801,1.9096029027194099,1.21694215475405]
["KCS-E1L212C6","KCS",5,"E1L212C6",215,"CM(Y), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",1.08927134424448E-2,1.11025478690863E-2,6.6885218024253804E-2,4.4522453099489198E-2,1.48197039961815E-2,4.5718322508037099E-3,4.2387084104120697E-3,4.87302400870249E-4,4.8134241104126003,5.2588991828155001,6.3586124376354496,5.0665608645820202,6.1673778406868101,3.8788052993086199,4.9649675470704597,3.1640496023605298]
["KCS-E1L212C10","KCS",5,"E1L212C10",219,"CD(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",5.7424068450927699,6.4501271247863796,58.979427337646499,57.123687744140597,22.537427902221701,6.6556066274642903E-2,0.162965297698975,0.24559333920478801,1.0178319215774501,0.73087299832794395,0.51723841871086995,0.30878354707269201,0,0,0,0]
["KCS-E1L212C13","KCS",5,"E1L212C13",222,"CM(R), DRL Expense, Privately-Owned, FLAT - MULTILEVEL",1.2661064863205,1.7265820503234901,0.67501068115234397,0.60770672559738204,0.394404917955399,0.210764020681381,0.15285032987594599,0.13987348973751099,0.26439762115478499,0.32801772986168198,0.38280640124141502,0.39890975492773201,0.44896913040000103,0.46257604078690601,0.42269922032343099,0.41382346771134898]
["KCS-E1L213C1","KCS",5,"E1L213C1",223,"CM(R), OPR Expense, Railroad-Owned, FLAT - GENERAL",9.5126600936055201E-3,1.25337038189173E-2,2.2478168830275501E-2,3.7414841353893301E-2,0.54436451196670499,1.6257904767990099,3.1981663703918501,2.4463350772857702,5.2609176635742196,2.1045132042907202,2.2044357802771599,9.7271091020814797,5.4905718193822803,16.928607623764499,8.9109006758376204,9.0494212712401598]
["KCS-E1L213C5","KCS",5,"E1L213C5",227,"CM(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",0.153132408857346,0.22795960307121299,0.54608875513076804,0.75441604852676403,0.457380920648575,0.190707236528397,0.53763514757156405,0.21155296266078899,0.65822583436965898,1.3361259004997701,0.53403682742832603,3.58498978939922,0.54015066223341102,0.54871108045752504,0.54076553875252498,0.48336533281850402]
["KCS-E1L213C8","KCS",5,"E1L213C8",230,"CD(R), DRL Expense, Railroad-Owned, FLAT - GENERAL",34.227325439453097,92.194526672363295,86.689208984375,943.002197265625,533.24853515625,247.96855163574199,401.26864624023398,189.99778747558599,248.40090942382801,348.415877177124,204.34964977908601,2251.7365421571899,361.24879674200503,298.55595876614802,173.67603968495399,198.16280781591999]
["KCS-E1L213C12","KCS",5,"E1L213C12",234,"CD(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL",-0.31583982706069902,0.216911941766739,7.5584582984447493E-2,0.45515665411949202,5.4912796020507804,11.4360866546631,29.264024734497099,14.356956481933601,20.575035095214801,15.4606329004844,16.490370052129499,267.67871813478502,45.742302176944598,54.239675168080304,31.538119741068599,45.240428633119301]
["KCS-E1L214C2","KCS",5,"E1L214C2",237,"CM(R), DRL Expense, Railroad-Owned, FLAT - OTHER",2.1777989342808699E-2,3.3962719142437002E-2,2.8057798743248E-2,1.8961558118462601E-2,7.2609940543770799E-3,6.54155761003494E-3,1.3761795125901701E-2,2.8024276718497301E-2,3.4983605146408102E-2,2.4559982418245099E-2,2.86731471273056E-2,1.1259780559588199E-2,1.48267119651202E-2,3.1468024715905797E-2,1.36420283269129E-2,6.3624966496640496E-3]
["KCS-E1L214C5","KCS",5,"E1L214C5",240,"CM(Y), DRL Expense, Railroad-Owned, FLAT - OTHER",5.6622806936502498E-2,8.8303036987781497E-2,7.2950229048728901E-2,4.9300044775009197E-2,1.8878588452935201E-2,1.7008066177368199E-2,3.5780638456344598E-2,7.2863079607486697E-2,9.0957306325435597E-2,6.3855954287437205E-2,7.4550182530994505E-2,2.9275429454929201E-2,3.8549451109312502E-2,8.1816864261354899E-2,3.5469273649973397E-2,1.6542491289126601E-2]
["KCS-E1L214C9","KCS",5,"E1L214C9",244,"CD(R), ROI Expense, Railroad-Owned, FLAT - OTHER",2.2123942375183101,2.6850626468658398,2.7561850547790501,1.8408391475677499,1.5910302400589,2.2044579982757599,3.2027463912963898,11.9325294494629,10.6845693588257,10.1210144423366,8.6619607395866307,10.680048287397399,12.575241925395,7.2111511844473704,7.1157263505227997,6.60330573674565]
["KCS-E1L214C12","KCS",5,"E1L214C12",247,"CD(Y), ROI Expense, Railroad-Owned, FLAT - OTHER",2.2123942375183101,2.6850626468658398,2.7561850547790501,1.8408389091491699,1.5910302400589,2.20445775985718,3.2027466297149698,11.9325304031372,10.6845693588257,10.1210144423366,8.6619607395866307,10.680048287397399,12.575241925395,7.2111511844473704,7.1157263505227997,6.60330573674565]
["KCS-E1L214C13","KCS",5,"E1L214C13",248,"CM(R), DRL Expense, Privately-Owned, FLAT - OTHER",0.37992724776268,0.39934393763542197,0.34177491068839999,0.34640285372734098,0.35683345794677701,0.40779903531074502,0.26444396376609802,0.242894262075424,0.26402613520622298,0.34887914339157899,0.36836427725201698,0.39081185979738298,0.402027839622634,0.613523643570826,0.63284522871399096,0.467542856246843]
["KCS-E1L215C4","KCS",5,"E1L215C4",252,"CM(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L215C7","KCS",5,"E1L215C7",255,"CD(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L215C11","KCS",5,"E1L215C11",259,"CD(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L216C1","KCS",5,"E1L216C1",262,"CM(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L216C4","KCS",5,"E1L216C4",265,"CM(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L216C8","KCS",5,"E1L216C8",269,"CD(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L216C11","KCS",5,"E1L216C11",272,"CD(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L216C12","KCS",5,"E1L216C12",273,"CD(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L217C3","KCS",5,"E1L217C3",277,"CM(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",7.5704893097281499E-3,5.5170994251966497E-2,0.27832531929016102,0.89300471544265703,0.69940549135208097,0.45948836207389798,0.63146305084228505,3.0133304595947301,3.83738661184907E-3,8.9596412362567296E-2,4.0125780299981196E-3,9.1484396927028894E-3,0.30897867295942399,0.26461436173845199,1.0878218952469199E-2,8.0772663975089906E-3]
["KCS-E1L217C6","KCS",5,"E1L217C6",280,"CM(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",1.9683275371789901E-2,0.14344456791877699,0.72364610433578502,2.3218116760253902,1.8184549808502199,1.19466984272003,1.6418036222457899,7.8346571922302202,9.9772075191140192E-3,0.23295067214267501,1.0432702877995101E-2,2.3785943201027501E-2,0.80334454969450297,0.68799734051997397,2.8283369276420101E-2,2.1000892633523401E-2]
["KCS-E1L217C10","KCS",5,"E1L217C10",284,"CD(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",4.0328102111816397,5.7563800811767596,9.2877693176269496,3.18991899490356,5.9663429260253897,0.73129630088806197,0.49328449368476901,0.244536057114601,0.437265634536743,8.2522499471377006E-2,0.40635245177706097,2.2905087903716201,3.33092098137065,6.2145013614853601,3.0001662163532101,1.5051323801448999]
["KCS-E1L217C13","KCS",5,"E1L217C13",287,"CM(R), DRL Expense, Privately-Owned, ALL OTHER FREIGHT CARS",3.5113706253468999E-3,0,1.2133617419749501E-3,8.3498518506530699E-5,2.0253703405614899E-4,3.60885006375611E-3,9.5382994040846807E-3,1.12817017361522E-2,7.3358290828764404E-3,0,2.7272776629487598E-4,0,0,0,3.6406961096743698E-5,0]
["KCS-E1L218C4","KCS",5,"E1L218C4",291,"CM(Y), OPR Expense, Railroad-Owned, AUTO RACKS",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L218C7","KCS",5,"E1L218C7",294,"CD(R), OPR Expense, Railroad-Owned, AUTO RACKS",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L218C10","KCS",5,"E1L218C10",297,"CD(Y), OPR Expense, Railroad-Owned, AUTO RACKS",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L218C11","KCS",5,"E1L218C11",298,"CD(Y), DRL Expense, Railroad-Owned, AUTO RACKS",674.18841552734398,474.00604248046898,0,0,0,0,0,0,42.818595886230497,59.932355494228901,81.130527596041802,71.430393792958299,87.752986182820905,38.476103561403797,84.1314178748746,41.603561372648798]
["KCS-E1L219C2","KCS",5,"E1L219C2",302,"CM(R), DRL Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,1.08840169559699E-4,1.19551074552249E-4,2.94254883533105E-4,0,0,1.6934443508823501E-4,2.09212673763225E-4,1.7835371465320699E-4]
["KCS-E1L219C5","KCS",5,"E1L219C5",305,"CM(Y), DRL Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,2.8298402321524902E-4,3.1083279383584697E-4,7.6506269718607401E-4,0,0,4.4029553122941001E-4,5.4395295178438503E-4,4.63719658098338E-4]
["KCS-E1L219C9","KCS",5,"E1L219C9",309,"CD(R), ROI Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,1.5703454613685601E-2,1.2563669046617701E-2,2.2967691160197201E-2,0,0,2.7817627779050998E-2,2.9252846876820501E-2,3.2304297442863297E-2]
["KCS-E1L219C12","KCS",5,"E1L219C12",312,"CD(Y), ROI Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,1.57034527510405E-2,1.2563669046617701E-2,2.2967691160197201E-2,0,0,2.7817627779050998E-2,2.9252846876820501E-2,3.2304297442863297E-2]
["KCS-E1L220C3","KCS",5,"E1L220C3",316,"CM(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",9.2709967866540007E-3,1.2611855752766099E-2,1.0840758681297301E-2,1.0699782520532599E-2,9.8091037943959201E-3,1.04247778654099E-2,1.6726627945900002E-2,4.7939896583557101E-2,6.1437759548425702E-2,7.8284572474295294E-2,7.8937989579828005E-2,9.8252377080644507E-2,0.120919918187263,8.2868365717089804E-2,7.1059275003733297E-2,8.4826223904613501E-2]
["KCS-E1L220C6","KCS",5,"E1L220C6",319,"CM(Y), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",2.4382339790463399E-2,3.6550313234329203E-2,3.2901056110858903E-2,2.96926274895668E-2,2.6770681142807E-2,4.4794954359531403E-2,6.4488083124160794E-2,0.19473661482334101,0.207346141338348,0.275937915076996,0.27976001207453,0.32640141471440498,0.37198622791846297,0.230417953520483,0.17226302623259901,0.178914596074879]
["KCS-E1L220C9","KCS",5,"E1L220C9",322,"CD(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.19688856601715,1.61900067329407,1.5205727815628101,1.5015275478362999,1.40252077579498,1.2580913305282599,2.3271429538726802,6.0827050209045401,8.0119180679321307,10.548775194668201,10.712258834951299,13.2518808017695,16.8931582175777,12.486669329030899,11.8057935938475,14.458999712510799]
["KCS-E1L220C10","KCS",5,"E1L220C10",323,"CD(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.70327520370483,2.5525853633880602,2.9174530506134002,3.2186481952667201,2.8388113975524898,2.3529355525970499,2.6724495887756299,2.3000237941741899,4.8715286254882804,2.5845720585065401,2.4413566817301899,2.7158285259952901,2.4748101868764198,4.7861184670319199,3.6254002567081298,3.4669675354567699]
["KCS-E1L221C1","KCS",5,"E1L221C1",327,"CM(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.121390819549561,0.149405732750893,1.0953239202499401,0.79970896244049094,0.32037031650543202,1.0711348149925501E-3,2.7658969629555902E-3,4.19213064014912E-3,1.6192007809877399E-2,1.20381689520492E-2,8.4351091308495097E-3,5.0829422643643898E-3,0,0,0,0]
["KCS-E1L221C4","KCS",5,"E1L221C4",330,"CM(Y), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.31561619043350198,0.38845473527908297,2.8478419780731201,2.0792429447174099,0.83296328783035301,2.7849504258483601E-3,7.1913343854248498E-3,1.08995456248522E-2,4.2099222540855401E-2,3.1299239275327899E-2,2.19312837402088E-2,1.32156498873474E-2,0,0,0,0]
["KCS-E1L221C8","KCS",5,"E1L221C8",334,"CD(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",423.85546875,261.70422363281301,359.25189208984398,766.79626464843795,237.919509887695,60.447891235351598,57.828327178955099,45.794223785400398,42.724620819091797,50.915876299082399,72.748424977509003,87.678896299590704,51.891836819145198,-35.6617199317825,-76.174567770867597,21.824008759225599]
["KCS-E1L221C11","KCS",5,"E1L221C11",337,"CD(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",423.85534667968801,261.70422363281301,359.25189208984398,766.79638671875,237.919509887695,60.447891235351598,57.828323364257798,45.794219970703097,42.724620819091797,50.915876299082399,72.748424977509003,87.678896299590704,51.891836819145297,-35.6617199317825,-76.174567770867696,21.824008759225599]
["KCS-E1L302C1","KCS",5,"E1L302C1",341,"L&D Expense, GRAIN",2.6387264952063599E-2,2.4945870041847201E-2,3.6727432161569602E-2,3.52221131324768E-2,2.7508964762091598E-2,4.8060111701488502E-2,2.2179268300533302E-2,3.1123021617531801E-2,3.6137115210294703E-2,3.1673053208722303E-2,2.06520373319149E-2,3.17940606104282E-2,2.12862621972436E-2,1.6299519112691799E-2,1.6646101782829398E-2,1.6986060104260001E-2]
["KCS-E1L305C1","KCS",5,"E1L305C1",344,"L&D Expense, FRESH VEGETABLES",0.60301697254180897,0.243790358304977,0.41229620575904802,0.19410522282123599,7.3158152401447296E-2,0.65559387207031306,0.35545039176940901,0.20792415738105799,0.48678919672965998,0.41470897303029602,0.34160943933107601,0.389577076844837,0.26595492810377602,0.63672310190342996,0.200726594272612,0.51497044391303703]
["KCS-E1L308C1","KCS",5,"E1L308C1",347,"L&D Expense, COAL",3.01631726324558E-3,3.2460147049277999E-3,3.05656832642853E-3,4.3408023193478602E-3,3.2279870938509698E-3,3.3305299002677198E-3,4.0287571027874903E-3,3.9105019532144096E-3,2.7237308677285901E-3,2.14346200941452E-3,2.0286106009389702E-3,4.8588212337537899E-3,4.4838032093151596E-3,3.9408800824081098E-3,1.5177075802263499E-3,2.1313169653889401E-3]
["KCS-E1L309C1","KCS",5,"E1L309C1",348,"L&D Expense, NONMETALLIC MINERALS",6.1751324683427802E-3,6.0367635451257203E-3,6.24764291569591E-3,1.1238164268434001E-2,1.2882996350526799E-2,1.0773151181638199E-2,1.14579824730754E-2,5.6324019096791701E-3,5.2316985093057199E-3,7.1841635102270198E-3,1.9460853891206499E-3,2.9566385317463602E-3,2.6945083219701502E-3,3.9923515321203399E-3,1.2879584932098101E-3,2.5697714472261999E-3]
["KCS-E1L313C1","KCS",5,"E1L313C1",352,"L&D Expense, CANNED FRUITS/VEG",0.61201786994934104,0.45836937427520802,0.54955309629440297,0.46772405505180398,0.268973708152771,0.44812881946563698,0.364413142204285,0.32465270161628701,0.30047565698623702,0.54309701066336802,0.60036280662191399,0.59926710243978698,0.57379621654754098,0.79501823483980005,0.40052818960853498,0.33041247966923698]
["KCS-E1L317C1","KCS",5,"E1L317C1",356,"L&D Expense, CEREALS",0.13801950216293299,0.150457173585892,0.113301411271095,0.12655127048492401,0.114000834524632,5.6761432439088801E-2,2.6986366137862199E-2,9.9266923964023604E-2,4.1428942233324099E-2,2.69035785859623E-2,7.1618623461894307E-2,1.92697768762677E-2,5.9594076037541001E-2,1.39432972578182E-3,9.1593963957775203E-4,6.4883822884699701E-3]
["KCS-E1L320C1","KCS",5,"E1L320C1",359,"L&D Expense, CORN PRODUCTS",1.34091908112168E-2,3.9376903325319297E-2,4.7181513160467099E-2,2.6431472972035401E-2,2.73294728249311E-2,3.8074269890785203E-2,3.7078451365232502E-2,1.75428669899702E-2,2.01527439057827E-2,4.1817161674595404E-3,1.34790764147741E-2,4.3508653131181197E-3,9.0233417435583996E-3,3.9086462228574504E-3,3.02978423330987E-5,2.0180023840311999E-2]
["KCS-E1L323C1","KCS",5,"E1L323C1",362,"L&D Expense, WINES",0.84492164850234996,8.3208911120891599E-2,1.34687983989716,0.44220030307769798,0.205625951290131,6.3485205173492404E-2,0.24367405474185899,0.51581692695617698,0.34035617113113398,1.35427260144433,0.24422654004494099,0.105158524452878,0.36028833717952002,0.267506679227699,0.16329456182654101,0.12703334188972801]
["KCS-E1L327C1","KCS",5,"E1L327C1",366,"L&D Expense, TOBACCO PRODUCTS",0,0,0,0,3.18567967414856,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E1L330C1","KCS",5,"E1L330C1",369,"L&D Expense, PLYWOOD OR VENEER",7.4905700981617002E-2,4.27759401500225E-2,8.9939765632152599E-2,0.12727469205856301,8.0512069165706607E-2,9.6415840089321095E-2,4.3528910726308802E-2,3.7447415292263003E-2,2.03599594533443E-2,0.12145549472462901,0.216664798239351,2.9783990826895802E-2,7.0972097170494602E-2,6.9536828674594306E-2,6.8338321410531103E-2,0.117691760964366]
["KCS-E1L334C1","KCS",5,"E1L334C1",373,"L&D Expense, NEWSPRINT",0.386345565319061,0.26457613706588701,0.24139791727066001,0.40231353044509899,0.33147549629211398,0.257203638553619,0.141914248466492,8.8899778202176094E-3,0.17850668728351601,0.192825144881663,9.4011005829416405E-2,0.20472030566705901,3.1076594371090002E-2,1.2324784383151699,2.51977665787704E-2,0.16148795459672499]
["KCS-E1L335C1","KCS",5,"E1L335C1",374,"L&D Expense, PRINTING PAPER",0.45069688558578502,0.77085703611373901,0.80805128812789895,0.78840303421020497,0.60578840970992998,0.33505225181579601,0.42516347765922502,0.31435161828994801,0.37708187103271501,0.39925658646490703,0.66945896095312996,1.11723782584026,0.58951542221150599,0.19435054877364999,0.121608076937136,0.190232288385774]
["KCS-E1L338C1","KCS",5,"E1L338C1",377,"L&D Expense, SANITARY TISSUES",0.122947245836258,3.0709726270288199E-3,6.65031932294369E-3,6.80103600025177E-2,1.2522803619503999E-2,0,0.10232835263013799,1.07538355514407E-2,9.4120344147086091E-3,2.9207028751322198E-2,1.1900797086969101E-3,1.39013832183855E-2,0,5.0166042535151603E-3,1.23663771402875E-3,4.3280785841464898E-3]
["KCS-E1L342C1","KCS",5,"E1L342C1",381,"L&D Expense, POTASSIUM OR SODIUM",2.7809889987111099E-2,1.60602275282145E-2,1.1788333766162401E-2,1.4397126622498001E-2,2.13480275124311E-2,1.2410043738782401E-2,9.0565774589776993E-3,7.6568066142499404E-3,1.3412986882031E-2,8.5684775629813106E-3,2.6314574467900101E-2,1.10570170436835E-2,1.12225187459802E-2,1.60371523159329E-2,1.1939958424653599E-2,5.9931752529763698E-3]
[{"$f":"B5250&\"-\"&D5250","v":"KCS-E1L345C1"},"KCS",5,"E1L345C1",384,"L&D Expense, ALL OTHER CHEMICALS",2.6043361052870799E-2,0.102892324328423,5.1314171403646497E-2,5.8835830539464999E-2,4.2031995952129399E-2,1.8057033419609101E-2,2.5860302150249499E-2,7.7346088364720301E-3,2.08973791450262E-2,2.2599386791942899E-2,5.1338501809845997E-2,4.6916238257755201E-4,7.0031947197344305E-2,9.0754973556344501E-2,0.11058293551930599,1.91782433824856E-2]
["KCS-E1L348C1","KCS",5,"E1L348C1",387,"L&D Expense, RUBBER TIRES/INNER TUBES",0.134509116411209,8.9131239801645296E-3,1.7789637669920901E-2,4.3709573219530301E-4,6.3215277623385202E-4,0.12824502587318401,0.20823356509208699,0.172246068716049,0.101569473743439,5.1709465437767201E-2,4.1918087269156301E-3,3.8097494457809397E-2,6.2541206245703999E-3,5.4441562535281901E-2,7.61084379992156E-2,9.8839377049493804E-2]
["KCS-E1L352C1","KCS",5,"E1L352C1",391,"L&D Expense, NONMETALLIC EARTH/MIN",3.5418793559074402E-2,2.9506977647542999E-2,3.24249938130379E-2,3.4120228141546201E-2,1.8458276987075799E-2,2.4468347430229201E-2,2.0480075851082798E-2,2.0243378356099101E-2,2.5672337040305099E-2,2.5089518608720399E-2,3.77997396445496E-2,7.6303684431867002E-3,1.4583935379803001E-2,1.4303699383296E-2,4.0311754906339203E-3,1.3603944578531899E-2]
["KCS-E1L355C1","KCS",5,"E1L355C1",394,"L&D Expense, PRIMARY IRON/STEEL PRODUCTS",3.4884344786405598E-2,5.3362432867288603E-2,3.6286663264036199E-2,9.7192518413066906E-2,4.7952342778444297E-2,4.3800264596939101E-2,2.8834400698542598E-2,3.0930418521165799E-2,4.0773164480924599E-2,4.32040643335612E-2,3.8559282806765002E-2,6.04644823038471E-2,4.9514510216627401E-2,7.8182518416237898E-2,1.5334172940485001E-2,4.9781753141333498E-2]
["KCS-E1L359C1","KCS",5,"E1L359C1",398,"L&D Expense, FAB STRUC METAL PRODUCTS",1.3789104223251301,0.26735174655914301,0.109357416629791,0.55470359325408902,0.24174544215202301,0.26759335398674,8.8351674377918202E-2,2.4079890921711901E-2,1.6526019899174599E-3,0.13177579165119599,0.176593743188519,0.36042406768129098,0.20247041874306199,0.685889247456412,6.71721725659165E-3,0.61904499763286203]
["KCS-E1L360C1","KCS",5,"E1L360C1",399,"L&D Expense, ALL OTHER FAB METAL PRODUCTS",8.2236602902412401E-2,4.22826893627644E-2,0.12317106872797,0.57348483800888095,0.11085592955350899,0.104633316397667,0.104206696152687,0.41068261861801098,2.90865134447813E-2,2.6793860444710701E-2,1.17116840125649E-2,6.1026978151819303E-2,8.3779653724611707E-3,1.9695008077359299E-2,2.3129155730127701E-3,8.2394414457267903E-2]
["KCS-E1L363C1","KCS",5,"E1L363C1",402,"L&D Expense, FARM MACHINERY",2.4298570156097399,1.5298203229904199,1.5081578493118299,2.9845852851867698,1.5362756252288801,0.99220669269561801,0.70848298072814897,1.0776067972183201,0.70382529497146595,1.3448171672090701,0.559861487070207,0.61976011384427698,0.13272710665462301,0.15808913426766,0,0.16933120027486401]
["KCS-E1L367C1","KCS",5,"E1L367C1",406,"L&D Expense, ELECTRICAL TRANS/DIST EQUIPMENT",4.9571437835693404,1.3843834400177,1.5912679433822601,0.52243554592132602,0.95162492990493797,1.35360562801361,0.46107843518257102,0.55019402503967296,0.73037481307983398,2.4718954756265998,0.72087862382857204,0.437231102871734,8.2663145076920408,0,1.4978214029207599,2.3871011726206701]
["KCS-E1L370C1","KCS",5,"E1L370C1",409,"L&D Expense, ALL OTHER ELECTRICAL MACHINERY",0.72443789243698098,0.124912194907665,1.22650158405304,2.0479607582092298,1.4720858335495,2.7940336614847201E-2,2.5568239390850098E-2,0.79280191659927401,0.32959437370300299,0.11638569092668601,0.15527288252874599,0.20274542735457399,3.8295146556108502E-2,0.100668737420884,0.10349523579893,6.5650136035665803]
["KCS-E1L373C1","KCS",5,"E1L373C1",412,"L&D Expense, MOTOR TRUCKS",2.1043250560760498,1.26811671257019,1.65900325775146,1.4032484292984,0.97844052314758301,0.82795894145965598,2.6402244567871098,2.5844602584838898,5.3508419990539604,2.3972440890440101,2.5053101151001802,3.01905989333518,4.5072670290018699,1.8358317475753301,1.9620481392513101,6.0876948799235704]
["KCS-E1L377C1","KCS",5,"E1L377C1",416,"L&D Expense, SHIPPER ASSOCIATION TRAFFIC",6.9035097956657396E-2,4.24118414521217E-2,0,0,0,0,0.15256458520889299,0,0,0,0,3.9752304352468099E-2,0,1.2640222416189799E-2,0,0]
["KCS-E1L380C1","KCS",5,"E1L380C1",419,"L&D Expense, ALL OTHER MIXED SHIPMENTS",0.16601713001728099,0.88630723953247104,1.4442171668633799E-3,0.87179607152938798,0.75372087955474898,0.13352239131927501,3.1231531873345399E-2,9.3002393841743497E-2,1.03999447822571,0.416805851183083,0.345811739282818,0.14978310418351601,0.18150323928185,3.82302116571379,1.53221325354683,0.10334428935010299]
["KCS-E2L101C2","KCS",5,"E2L101C2",423,"E/L Ratio, Railroad-Owned, BOX - 40 FT",1.9375342130661,1.98747062683105,2.0183515548706099,1.9474798440933201,1.73396396636963,1.7323247194290201,1.9003558158874501,1.8031582832336399,1.7764493227005,1.79788039364118,1.8042180660565099,1.87970615243343,1.8244746600741699,1.8778386844166,1.814011676397,1.87747035573123]
["KCS-E2L101C3","KCS",5,"E2L101C3",424,"E/L Ratio, Privately-Owned, BOX - 40 FT",1.2072404623031601,1.24586045742035,1.26481997966766,1.46746742725372,1.4366424083709699,1.2629648447036701,1.33602154254913,1.4502470493316699,1.46832811832428,1.28900949796472,1.6194724592707499,1.4145587408656499,1.4745412251227701,1.7921022067363499,2.0916993830622501,1.9555002763958]
["KCS-E2L101C6","KCS",5,"E2L101C6",427,"Interline circuity, BOX - 40 FT",1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.192999958992,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001,1.1930000000000001]
["KCS-E2L101C10","KCS",5,"E2L101C10",431,"CD per Interchange Switch, BOX - 40 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L101C13","KCS",5,"E2L101C13",434,"CD per I&I Switch, BOX - 40 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L101C16","KCS",5,"E2L101C16",437,"CD per Load & Unload Interterminal Switch, BOX - 40 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L101C20","KCS",5,"E2L101C20",441,"CM per Interterminal Switch, BOX - 40 FT",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["KCS-E2L101C23","KCS",5,"E2L101C23",444,"Average Miles between I&I Switches, BOX - 40 FT",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["KCS-E2L101C25","KCS",5,"E2L101C25",446,"SEMs per Industry Switch, BOX - 40 FT",8.7567062377929705,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E2L101C28","KCS",5,"E2L101C28",449,"SEMs per Interterminal Switch, BOX - 40 FT",10.5080480575562,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["KCS-E2L102C2","KCS",5,"E2L102C2",452,"E/L Ratio, Railroad-Owned, BOX - 50 FT",1.9375342130661,1.98747062683105,2.0183515548706099,1.9474798440933201,1.73396396636963,1.7323247194290201,1.9003558158874501,1.8031582832336399,1.7764493227005,1.79788039364118,1.8042180660565099,1.87970615243343,1.8244746600741699,1.8778386844166,1.814011676397,1.87747035573123]
["KCS-E2L102C6","KCS",5,"E2L102C6",456,"Interline circuity, BOX - 50 FT",1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001]
["KCS-E2L102C9","KCS",5,"E2L102C9",459,"CD per Industry Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L102C13","KCS",5,"E2L102C13",463,"CD per I&I Switch, BOX - 50 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L102C16","KCS",5,"E2L102C16",466,"CD per Load & Unload Interterminal Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L102C19","KCS",5,"E2L102C19",469,"CM per Intraterminal Switch, BOX - 50 FT",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["KCS-E2L102C21","KCS",5,"E2L102C21",471,"CM per I&I Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L102C24","KCS",5,"E2L102C24",474,"Average Miles between Interchange Switches, BOX - 50 FT",187.67051696777301,81.770416259765597,258.9755859375,252.14675903320301,193.032791137695,248.90556335449199,260.04580688476602,223.31735229492199,336.17672729492199,268.31036113420902,308.807405150845,400.342842726274,320.111454538418,335.55225733539697,395.85467486244301,423.49080286538702]
["KCS-E2L102C27","KCS",5,"E2L102C27",477,"SEMs per Intraterminal Switch, BOX - 50 FT",13.1350603103638,12.768383979797401,11.484691619873001,10.2740364074707,10.2223415374756,10.8923845291138,11.218360900878899,11.138505935668899,10.6885375976563,10.548979298740001,10.4307736286619,9.2535174475933797,9.63453681464574,8.9524845356580904,8.7129714124508499,8.1824438032959996]
["KCS-E2L103C2","KCS",5,"E2L103C2",481,"E/L Ratio, Railroad-Owned, BOX - EQUIPPED",1.8129259347915601,1.8469585180282599,1.9106365442276001,1.92492604255676,1.8311469554901101,1.8070307970046999,1.8741215467453001,1.79079973697662,1.78360378742218,1.81731457873779,1.92458127917986,1.95048607080673,1.9133532615372,1.9490135432775699,1.8804221582588501,1.89440466719703]
["KCS-E2L103C5","KCS",5,"E2L103C5",484,"Local circuity, BOX - EQUIPPED",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["KCS-E2L103C9","KCS",5,"E2L103C9",488,"CD per Industry Switch, BOX - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L103C12","KCS",5,"E2L103C12",491,"CD per Interterminal Switch, BOX - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["KCS-E2L103C15","KCS",5,"E2L103C15",494,"CD per Load & Unload Intraterminal Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["KCS-E2L103C17","KCS",5,"E2L103C17",496,"CM per Industry Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["KCS-E2L103C20","KCS",5,"E2L103C20",499,"CM per Interterminal Switch, BOX - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["KCS-E2L103C23","KCS",5,"E2L103C23",502,"Average Miles between I&I Switches, BOX - EQUIPPED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["KCS-E2L103C27","KCS",5,"E2L103C27",506,"SEMs per Intraterminal Switch, BOX - EQUIPPED",13.135062217712401,12.768383979797401,11.484691619873001,10.274035453796399,10.2223405838013,10.892383575439499,11.218360900878899,11.138505935668899,10.6885375976563,10.548979298740001,10.4307736286619,9.2535174475933708,9.63453681464574,8.9524845356580904,8.7129714124508499,8.1824438032959996]
["KCS-E2L104C1","KCS",5,"E2L104C1",509,"Average Tare Weight, GONDOLA - PLAIN",26,25.899999618530298,25.799999237060501,25.600000381469702,25.5,25.600000381469702,25.299999237060501,25.700000762939499,25.700000762939499,25.6,25.6,25.6,25.7,25.9,26.1,26.3]
["KCS-E2L104C5","KCS",5,"E2L104C5",513,"Local circuity, GONDOLA - PLAIN",1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.093,1.093,1.093,1.093,1.093,1.093,1.093]
["KCS-E2L104C8","KCS",5,"E2L104C8",516,"Spotted-to-Pulled Ratio, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L104C11","KCS",5,"E2L104C11",519,"CD per Intraterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L104C13","KCS",5,"E2L104C13",521,"CD per I&I Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L104C16","KCS",5,"E2L104C16",524,"CD per Load & Unload Interterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L104C20","KCS",5,"E2L104C20",528,"CM per Interterminal Switch, GONDOLA - PLAIN",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["KCS-E2L104C23","KCS",5,"E2L104C23",531,"Average Miles between I&I Switches, GONDOLA - PLAIN",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["KCS-E2L104C26","KCS",5,"E2L104C26",534,"SEMs per Interchange Switch, GONDOLA - PLAIN",4.8161888122558603,4.68174076080322,4.2110538482665998,3.7671461105346702,3.7481915950775102,3.9938747882843,4.1133995056152299,4.0841193199157697,3.9191303253173801,3.8679590762046798,3.82461699717601,3.3929563974509001,3.5326634987034402,3.2825776630746302,3.1947561845653101,3.0002293945418699]
["KCS-E2L105C1","KCS",5,"E2L105C1",538,"Average Tare Weight, GONDOLA - EQUIPPED",33.099998474121101,33.200000762939503,33.400001525878899,33.299999237060497,33.299999237060497,33.299999237060497,33.299999237060497,33.099998474121101,33.099998474121101,33.200000000000003,33.200000000000003,33.1,33.1,33.1,33.1,33.1]
["KCS-E2L105C3","KCS",5,"E2L105C3",540,"E/L Ratio, Privately-Owned, GONDOLA - EQUIPPED",2.0417933464050302,2.0554745197296098,2.1184062957763699,2.1051259040832502,2.0360307693481401,2.0488119125366202,2.0177352428436302,2.04023408889771,2.0176656246185298,2.0308239478363999,2.03859857482185,2.0299785867237699,2.0606868956318798,1.96665566193463,2.0171037628278201,2.0353227771011002]
["KCS-E2L105C8","KCS",5,"E2L105C8",545,"Spotted-to-Pulled Ratio, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L105C9","KCS",5,"E2L105C9",546,"CD per Industry Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L105C12","KCS",5,"E2L105C12",549,"CD per Interterminal Switch, GONDOLA - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["KCS-E2L105C16","KCS",5,"E2L105C16",553,"CD per Load & Unload Interterminal Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L105C19","KCS",5,"E2L105C19",556,"CM per Intraterminal Switch, GONDOLA - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["KCS-E2L105C22","KCS",5,"E2L105C22",559,"Average CM per CD, Railroad-Owned, GONDOLA - EQUIPPED",478.25125122070301,558.17974853515602,575.27001953125,682.88665771484398,568.424560546875,399.16067504882801,512.25146484375,445.99636840820301,365.51055908203102,358.90958784072802,392.22637853440102,381.794031804817,349.84331025776498,394.25519355420403,443.57288994839899,374.97712559015099]
["KCS-E2L105C26","KCS",5,"E2L105C26",563,"SEMs per Interchange Switch, GONDOLA - EQUIPPED",4.8161888122558603,4.68174076080322,4.2110538482665998,3.7671463489532502,3.7481915950775102,3.99387454986572,4.1133999824523899,4.0841188430786097,3.9191300868988002,3.8679590762046798,3.82461699717601,3.3929563974509001,3.5326634987034402,3.2825776630746302,3.1947561845653101,3.0002293945418699]
["KCS-E2L105C28","KCS",5,"E2L105C28",565,"SEMs per Interterminal Switch, GONDOLA - EQUIPPED",10.5080480575562,10.2147064208984,9.1877536773681605,8.2192296981811506,8.1778736114502006,8.7139081954956108,8.9746885299682599,8.9108057022094709,8.5508298873901403,8.4391834389920408,8.3446189029294793,7.4028139580746997,7.7076294517166,7.1619876285264699,6.9703771299606796,6.5459550426368001]
["KCS-E2L106C2","KCS",5,"E2L106C2",568,"E/L Ratio, Railroad-Owned, HOPPER - COVERED",2.0210092067718501,2.0482132434845002,2.0465517044067401,2.0144855976104701,1.99640488624573,1.99723184108734,2.05106401443481,2.0098576545715301,2.0074312686920202,1.99671047454159,1.9805015538050199,1.9395915640251,1.9149119981257501,1.96733290350312,1.96588713438604,1.98348025779687]
["KCS-E2L106C5","KCS",5,"E2L106C5",571,"Local circuity, HOPPER - COVERED",1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999]
["KCS-E2L106C8","KCS",5,"E2L106C8",574,"Spotted-to-Pulled Ratio, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L106C12","KCS",5,"E2L106C12",578,"CD per Interterminal Switch, HOPPER - COVERED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["KCS-E2L106C15","KCS",5,"E2L106C15",581,"CD per Load & Unload Intraterminal Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["KCS-E2L106C18","KCS",5,"E2L106C18",584,"CM per Interchange Switch, HOPPER - COVERED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["KCS-E2L106C22","KCS",5,"E2L106C22",588,"Average CM per CD, Railroad-Owned, HOPPER - COVERED",478.25128173828102,558.17980957031295,575.27001953125,682.88677978515602,568.424560546875,399.16067504882801,512.25140380859398,445.99636840820301,365.51055908203102,358.90958784072802,392.22637853440102,381.794031804817,349.84331025776498,394.25519355420403,443.57288994839899,374.97712559015099]
["KCS-E2L106C24","KCS",5,"E2L106C24",590,"Average Miles between Interchange Switches, HOPPER - COVERED",404.96267700195301,424.46398925781301,318.63131713867199,330.46356201171898,310.85995483398398,318.70620727539102,265.06747436523398,348.33670043945301,430.173583984375,364.15771799751599,347.00882635601999,405.83938486643598,382.38399973741201,454.87832157340102,429.036307967239,441.21727725865202]
["KCS-E2L106C27","KCS",5,"E2L106C27",593,"SEMs per Intraterminal Switch, HOPPER - COVERED",13.1350603103638,12.768383979797401,11.484691619873001,10.2740364074707,10.2223405838013,10.8923845291138,11.2183618545532,11.138506889343301,10.6885375976563,10.548979298740001,10.4307736286619,9.2535174475933797,9.63453681464574,8.9524845356580904,8.7129714124508499,8.1824438032959996]
["KCS-E2L107C1","KCS",5,"E2L107C1",596,"Average Tare Weight, HOPPER - OPEN TOP - GENERAL",29.799999237060501,29.700000762939499,29.600000381469702,29.600000381469702,29.5,29.600000381469702,29.399999618530298,29.200000762939499,29,28.9,28.8,28.8,28.7,28.5,28.4,28.3]
["KCS-E2L107C4","KCS",5,"E2L107C4",599,"E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - GENERAL",2.0547170639038099,1.9710763692855799,2.04761910438538,2.0284757614135698,2.0161178112029998,1.98449611663818,1.9974160194396999,2.0052585601806601,2.0135416984558101,2.00472589792061,2.0064205457463902,2.03074141048825,1.99055330634278,2.0391489361702102,1.9913258983891,1.96216768916155]
["KCS-E2L107C8","KCS",5,"E2L107C8",603,"Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L107C11","KCS",5,"E2L107C11",606,"CD per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L107C14","KCS",5,"E2L107C14",609,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L107C16","KCS",5,"E2L107C16",611,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L107C22","KCS",5,"E2L107C22",617,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",478.25128173828102,558.17980957031295,575.26995849609398,682.88677978515602,568.42462158203102,399.16067504882801,512.25146484375,445.99636840820301,365.51055908203102,358.90958784072802,392.22637853440102,381.794031804817,349.84331025776498,394.25519355420403,443.57288994839899,374.97712559015099]
["KCS-E2L107C23","KCS",5,"E2L107C23",618,"Average Miles between I&I Switches, HOPPER - OPEN TOP - GENERAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["KCS-E2L107C26","KCS",5,"E2L107C26",621,"SEMs per Interchange Switch, HOPPER - OPEN TOP - GENERAL",4.8161888122558603,4.68174076080322,4.2110538482665998,3.7671465873718302,3.7481915950775102,3.99387454986572,4.1133995056152299,4.0841188430786097,3.9191300868988002,3.8679590762046798,3.82461699717601,3.3929563974509001,3.5326634987034402,3.2825776630746302,3.1947561845653101,3.0002293945418699]
["KCS-E2L107C29","KCS",5,"E2L107C29",624,"SEMs per I&I Switch, HOPPER - OPEN TOP - GENERAL",2.18917679786682,2.1280639171600302,1.9141151905059799,1.7123394012451201,1.70372354984283,1.81539750099182,1.8697268962860101,1.85641777515411,1.78142297267914,1.7581632164566701,1.73846227144364,1.54225290793223,1.60575613577429,1.49208075594301,1.45216190207514,1.3637406338826701]
["KCS-E2L108C4","KCS",5,"E2L108C4",628,"E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - SPECIAL",1.9942097663879399,1.97850358486176,1.9937618970871001,2.0079870223999001,1.9955642223358201,1.9098562002182,1.97920918464661,1.9405703544616699,1.97504866123199,1.9266047188797999,2.0049213680853399,1.9407080138855399,2.0007979722117901,1.83353101234912,1.88613068545804,1.8930695928385799]
["KCS-E2L108C7","KCS",5,"E2L108C7",631,"Average circuity, HOPPER - OPEN TOP - SPECIAL",1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001]
["KCS-E2L108C11","KCS",5,"E2L108C11",635,"CD per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L108C12","KCS",5,"E2L108C12",636,"CD per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["KCS-E2L108C18","KCS",5,"E2L108C18",642,"CM per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["KCS-E2L108C19","KCS",5,"E2L108C19",643,"CM per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["KCS-E2L108C22","KCS",5,"E2L108C22",646,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",478.25131225585898,558.17974853515602,575.27001953125,682.88671875,568.42462158203102,399.16067504882801,512.25146484375,445.99636840820301,365.51055908203102,358.90958784072802,392.22637853440102,381.794031804817,349.84331025776498,394.25519355420403,443.57288994839899,374.97712559015099]
["KCS-E2L108C25","KCS",5,"E2L108C25",649,"SEMs per Industry Switch, HOPPER - OPEN TOP - SPECIAL",8.7567071914672905,8.5122556686401403,7.6564612388610804,6.8493571281433097,6.8148932456970197,7.2615895271301296,7.4789075851440403,7.4256711006164604,7.1256914138793901,7.0326528658266998,6.9538490857745696,6.1690116317289201,6.42302454309716,5.9683230237720597,5.8086476083005696,5.4549625355306697]
["KCS-E2L108C29","KCS",5,"E2L108C29",653,"SEMs per I&I Switch, HOPPER - OPEN TOP - SPECIAL",2.18917679786682,2.1280641555786102,1.9141153097152701,1.7123392820358301,1.70372354984283,1.81539762020111,1.8697267770767201,1.85641777515411,1.78142273426056,1.7581632164566701,1.73846227144364,1.54225290793223,1.60575613577429,1.49208075594301,1.45216190207514,1.3637406338826701]
["KCS-E2L109C3","KCS",5,"E2L109C3",656,"E/L Ratio, Privately-Owned, REFRIGERATED - MECH",2.06168484687805,2.1109426021575901,2.17184686660767,2,2,2,2,1.94405949115753,1.9011980295181301,1.86375486454831,2,1.88782658864255,1.84661023981412,1.8886063489459399,1.9152630526105201,1.92901119788438]
["KCS-E2L109C7","KCS",5,"E2L109C7",660,"Average circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["KCS-E2L109C8","KCS",5,"E2L109C8",661,"Spotted-to-Pulled Ratio, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L109C14","KCS",5,"E2L109C14",667,"CD per Load & Unload Industry Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L109C15","KCS",5,"E2L109C15",668,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["KCS-E2L109C18","KCS",5,"E2L109C18",671,"CM per Interchange Switch, REFRIGERATED - MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["KCS-E2L109C22","KCS",5,"E2L109C22",675,"Average CM per CD, Railroad-Owned, REFRIGERATED - MECH",478.25128173828102,558.17974853515602,575.27001953125,682.88671875,568.42462158203102,399.16067504882801,512.25140380859398,445.99636840820301,365.51058959960898,358.90958784072802,0,0,349.84331025776498,394.25519355420403,0,0]
["KCS-E2L109C25","KCS",5,"E2L109C25",678,"SEMs per Industry Switch, REFRIGERATED - MECH",8.7567071914672905,8.5122556686401403,7.6564607620239302,6.8493571281433097,6.8148937225341797,7.2615895271301296,7.4789071083068803,7.4256711006164604,7.1256918907165501,7.0326528658266998,6.9538490857745696,0,0,0,5.8086476083005696,0]
["KCS-E2L109C28","KCS",5,"E2L109C28",681,"SEMs per Interterminal Switch, REFRIGERATED - MECH",10.5080480575562,10.2147064208984,9.1877527236938494,8.2192296981811506,8.1778726577758807,8.7139091491699201,8.9746894836425799,8.9108057022094709,8.5508308410644496,8.4391834389920408,8.3446189029294793,0,0,0,6.9703771299606796,0]
["KCS-E2L110C3","KCS",5,"E2L110C3",685,"E/L Ratio, Privately-Owned, REFRIGERATED - NON-MECH",2.0414018630981401,2.0714960098266602,2.0409078598022501,2.0481255054473899,2,1.9125388860702499,1.93333327770233,2.11764717102051,2,1.9,2.1666666666666701,3,2.5,1.99803891989742,2.01223491027732,1.9966545454545499]
["KCS-E2L110C4","KCS",5,"E2L110C4",686,"E/L Ratio, All Freight Cars, REFRIGERATED - NON-MECH",2.5942029953002899,2.8399999141693102,2.3225805759429901,2.0571429729461701,1.57407402992249,1.8709677457809399,1.9166666269302399,2.1666667461395299,2.0454545021057098,2.16,3,4,5.6,0,0,0]
["KCS-E2L110C10","KCS",5,"E2L110C10",692,"CD per Interchange Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L110C11","KCS",5,"E2L110C11",693,"CD per Intraterminal Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L110C14","KCS",5,"E2L110C14",696,"CD per Load & Unload Industry Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L110C18","KCS",5,"E2L110C18",700,"CM per Interchange Switch, REFRIGERATED - NON-MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["KCS-E2L110C21","KCS",5,"E2L110C21",703,"CM per I&I Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L110C24","KCS",5,"E2L110C24",706,"Average Miles between Interchange Switches, REFRIGERATED - NON-MECH",547.61901855468795,584.409423828125,1029.9501953125,2405.51904296875,2869.67578125,456.37344360351602,5484.3046875,1917.06982421875,3384.615234375,576.92307692307702,2000,128.30730610224899,309.53383672335701,0,0,0]
["KCS-E2L110C29","KCS",5,"E2L110C29",711,"SEMs per I&I Switch, REFRIGERATED - NON-MECH",2.18917679786682,2.1280639171600302,1.9141149520873999,1.7123394012451201,1.70372343063354,1.81539738178253,1.8697268962860101,1.8564178943634,1.78142285346985,1.7581632164566701,1.73846227144364,1.54225290793223,1.60575613577429,1.49208075594302,0,1.3637406338826701]
["KCS-E2L111C3","KCS",5,"E2L111C3",714,"E/L Ratio, Privately-Owned, FLAT - TOFC",1.0703715085983301,1.1012428998947099,1.10537910461426,1.0875848531723,1.08359086513519,1.0663417577743499,1.0532578229904199,1.03776347637177,1.0287349224090601,1.0334564943765501,1.03507668279138,1.03141398216345,1.0260139609004999,1.0419034262639899,1.0375208949466399,1.0275066758040501]
["KCS-E2L111C6","KCS",5,"E2L111C6",717,"Interline circuity, FLAT - TOFC",1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.107,1.107,1.107,1.107,1.107,1.107,1.107]
["KCS-E2L111C7","KCS",5,"E2L111C7",718,"Average circuity, FLAT - TOFC",1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.085,1.085,1.085,1.085,1.085,1.085,1.085]
["KCS-E2L111C10","KCS",5,"E2L111C10",721,"CD per Interchange Switch, FLAT - TOFC",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L111C14","KCS",5,"E2L111C14",725,"CD per Load & Unload Industry Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L111C17","KCS",5,"E2L111C17",728,"CM per Industry Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["KCS-E2L111C20","KCS",5,"E2L111C20",731,"CM per Interterminal Switch, FLAT - TOFC",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["KCS-E2L111C25","KCS",5,"E2L111C25",736,"SEMs per Industry Switch, FLAT - TOFC",8.7567062377929705,8.5122556686401403,7.6564617156982404,6.8493566513061497,6.8148932456970197,7.2615895271301296,7.4789066314697301,7.4256711006164604,7.1256914138793901,7.0326528658266998,6.9538490857745696,6.1690116317289201,6.42302454309716,5.9683230237720597,5.8086476083005696,5.4549625355306697]
["KCS-E2L111C28","KCS",5,"E2L111C28",739,"SEMs per Interterminal Switch, FLAT - TOFC",10.5080480575562,10.2147073745728,9.1877536773681605,8.2192296981811506,8.1778726577758807,8.7139091491699201,8.9746894836425799,8.9108057022094709,8.5508298873901403,8.4391834389920408,8.3446189029294793,7.4028139580746997,7.7076294517165902,7.1619876285264699,6.9703771299606796,6.5459550426368001]
["KCS-E2L111C29","KCS",5,"E2L111C29",740,"SEMs per I&I Switch, FLAT - TOFC",2.18917679786682,2.1280639171600302,1.9141150712966899,1.7123392820358301,1.70372343063354,1.81539750099182,1.8697267770767201,1.85641777515411,1.78142285346985,1.7581632164566701,1.73846227144364,1.54225290793223,1.60575613577429,1.49208075594301,1.45216190207514,1.3637406338826701]
["KCS-E2L112C3","KCS",5,"E2L112C3",743,"E/L Ratio, Privately-Owned, FLAT - MULTILEVEL",1.4619047641754199,1.10977447032928,1.7183246612548799,1.3934611082077,1.17898833751678,1.13443326950073,1.15790390968323,1.19489562511444,1.1632059812545801,1.0635856744584999,1.29194906551653,1.3752763819095499,1.4206170052671201,1.4111534108447401,1.47311196003526,1.3366294067067901]
["KCS-E2L112C6","KCS",5,"E2L112C6",746,"Interline circuity, FLAT - MULTILEVEL",1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999]
["KCS-E2L112C10","KCS",5,"E2L112C10",750,"CD per Interchange Switch, FLAT - MULTILEVEL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L112C13","KCS",5,"E2L112C13",753,"CD per I&I Switch, FLAT - MULTILEVEL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L112C16","KCS",5,"E2L112C16",756,"CD per Load & Unload Interterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L112C21","KCS",5,"E2L112C21",761,"CM per I&I Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L112C24","KCS",5,"E2L112C24",764,"Average Miles between Interchange Switches, FLAT - MULTILEVEL",183.22515869140599,146.70307922363301,222.15013122558599,394.58792114257801,354.25274658203102,371.27911376953102,321.69558715820301,396.89151000976602,462.88751220703102,331.763640824297,320.01696621789898,277.16026874554302,277.79252229187,466.18195750385303,347.69471652848,435.809157926588]
["KCS-E2L112C25","KCS",5,"E2L112C25",765,"SEMs per Industry Switch, FLAT - MULTILEVEL",8.7567071914672905,8.5122556686401403,7.6564612388610804,6.8493566513061497,6.8148937225341797,7.2615900039672896,7.4789075851440403,7.4256711006164604,7.1256909370422399,7.0326528658266998,6.9538490857745696,6.1690116317289201,6.42302454309716,5.9683230237720597,5.8086476083005696,5.4549625355306697]
[{"$f":"B5634&\"-\"&D5634","v":"KCS-E2L112C28"},"KCS",5,"E2L112C28",768,"SEMs per Interterminal Switch, FLAT - MULTILEVEL",10.5080480575562,10.2147064208984,9.1877536773681605,8.2192296981811506,8.1778726577758807,8.7139091491699201,8.9746885299682599,8.9108047485351598,8.5508308410644496,8.4391834389920408,8.3446189029294793,7.4028139580746997,7.7076294517165902,7.1619876285264699,6.9703771299606796,6.5459550426368001]
["KCS-E2L113C2","KCS",5,"E2L113C2",771,"E/L Ratio, Railroad-Owned, FLAT - GENERAL",1.59090912342072,4,5.2105264663696298,1.72727274894714,4.1666665077209499,2.125,2,12.199999809265099,22,3.8461538461538498,12.5,1.5,2.3636363636363602,1.875,1.8125,1.2777777777777799]
["KCS-E2L113C6","KCS",5,"E2L113C6",775,"Interline circuity, FLAT - GENERAL",1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.177,1.177,1.177,1.177,1.177,1.177,1.177]
["KCS-E2L113C9","KCS",5,"E2L113C9",778,"CD per Industry Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L113C12","KCS",5,"E2L113C12",781,"CD per Interterminal Switch, FLAT - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["KCS-E2L113C17","KCS",5,"E2L113C17",786,"CM per Industry Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["KCS-E2L113C20","KCS",5,"E2L113C20",789,"CM per Interterminal Switch, FLAT - GENERAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["KCS-E2L113C21","KCS",5,"E2L113C21",790,"CM per I&I Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L113C24","KCS",5,"E2L113C24",793,"Average Miles between Interchange Switches, FLAT - GENERAL",846.15380859375,269.93099975585898,93.242118835449205,3628.89770507813,0,1272.96313476563,685.5380859375,1711.66943359375,1999.99987792969,2401.2652806583901,0,1283.07306102249,3404.8722039569302,10413.598111155699,4832.7669139073196,3106.7787303689902]
["KCS-E2L113C27","KCS",5,"E2L113C27",796,"SEMs per Intraterminal Switch, FLAT - GENERAL",13.1350603103638,12.768383026123001,11.484691619873001,10.2740364074707,0,10.8923854827881,11.2183618545532,11.138506889343301,10.6885375976563,10.548979298740001,0,9.2535174475933797,9.63453681464574,8.9524845356580904,8.7129714124508499,8.1824438032959996]
["KCS-E2L114C2","KCS",5,"E2L114C2",800,"E/L Ratio, Railroad-Owned, FLAT - OTHER",2.0667195320129399,2.0298092365264901,2.0798027515411399,2.08564352989197,2.00990962982178,1.9612015485763501,2.0300247669220002,1.9540435075759901,1.9651519060134901,2.0094773118897198,1.9897907095456899,2.03235294117647,1.9914931064828401,2.0763636363636402,2.0088748019017402,2.0361083249749199]
["KCS-E2L114C5","KCS",5,"E2L114C5",803,"Local circuity, FLAT - OTHER",1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001]
["KCS-E2L114C9","KCS",5,"E2L114C9",807,"CD per Industry Switch, FLAT - OTHER",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L114C13","KCS",5,"E2L114C13",811,"CD per I&I Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L114C16","KCS",5,"E2L114C16",814,"CD per Load & Unload Interterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L114C17","KCS",5,"E2L114C17",815,"CM per Industry Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["KCS-E2L114C20","KCS",5,"E2L114C20",818,"CM per Interterminal Switch, FLAT - OTHER",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["KCS-E2L114C23","KCS",5,"E2L114C23",821,"Average Miles between I&I Switches, FLAT - OTHER",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["KCS-E2L114C27","KCS",5,"E2L114C27",825,"SEMs per Intraterminal Switch, FLAT - OTHER",13.1350612640381,12.768383979797401,11.484691619873001,10.274035453796399,10.2223405838013,10.892383575439499,11.218360900878899,11.138506889343301,10.6885385513306,10.548979298740001,10.4307736286619,9.2535174475933708,9.63453681464574,8.9524845356580904,8.7129714124508499,8.1824438032959996]
["KCS-E2L115C1","KCS",5,"E2L115C1",828,"Average Tare Weight, TANK <22,000 GAL",32.700000000000003,32.700000000000003,32.6,32.6,32.6,32.6,32.6,32.6,32.6,32.700000000000003,32.700000000000003,32.799999999999997,32.799999999999997,32.9,32.9,32.9]
[{"$f":"B5698&\"-\"&D5698","v":"KCS-E2L115C5"},"KCS",5,"E2L115C5",832,"Local circuity, TANK <22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["KCS-E2L115C9","KCS",5,"E2L115C9",836,"CD per Industry Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L115C12","KCS",5,"E2L115C12",839,"CD per Interterminal Switch, TANK <22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["KCS-E2L115C13","KCS",5,"E2L115C13",840,"CD per I&I Switch, TANK <22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["KCS-E2L115C16","KCS",5,"E2L115C16",843,"CD per Load & Unload Interterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L115C20","KCS",5,"E2L115C20",847,"CM per Interterminal Switch, TANK <22,000 GAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["KCS-E2L115C23","KCS",5,"E2L115C23",850,"Average Miles between I&I Switches, TANK <22,000 GAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["KCS-E2L115C26","KCS",5,"E2L115C26",853,"SEMs per Interchange Switch, TANK <22,000 GAL",4.8161888122558603,4.68174076080322,4.2110533714294398,3.7671465873718302,3.7481915950775102,3.99387454986572,4.1133995056152299,4.0841188430786097,3.9191303253173801,3.8679590762046798,3.82461699717601,3.3929563974509001,3.5326634987034402,3.2825776630746302,3.1947561845653101,3.0002293945418699]
["KCS-E2L116C1","KCS",5,"E2L116C1",857,"Average Tare Weight, TANK >=22,000 GAL",39.799999999999997,39.200000000000003,38.9,38.9,39,38.9,38.9,39.1,39.5,40.1,40.4,40.700000000000003,41,41.4,41.7,41.9]
["KCS-E2L116C5","KCS",5,"E2L116C5",861,"Local circuity, TANK >=22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["KCS-E2L116C8","KCS",5,"E2L116C8",864,"Spotted-to-Pulled Ratio, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L116C9","KCS",5,"E2L116C9",865,"CD per Industry Switch, TANK >=22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["KCS-E2L116C12","KCS",5,"E2L116C12",868,"CD per Interterminal Switch, TANK >=22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["KCS-E2L116C16","KCS",5,"E2L116C16",872,"CD per Load & Unload Interterminal Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L116C19","KCS",5,"E2L116C19",875,"CM per Intraterminal Switch, TANK >=22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["KCS-E2L116C22","KCS",5,"E2L116C22",878,"Average CM per CD, Railroad-Owned, TANK >=22,000 GAL",478.25131225585898,558.17974853515602,575.27001953125,682.88671875,568.42462158203102,399.16067504882801,512.25140380859398,445.99639892578102,365.51058959960898,358.90958784072802,392.22637853440102,381.794031804817,349.84331025776498,394.25519355420403,443.57288994839899,374.97712559015099]
["KCS-E2L116C27","KCS",5,"E2L116C27",883,"SEMs per Intraterminal Switch, TANK >=22,000 GAL",13.1350612640381,12.768384933471699,11.484691619873001,10.2740364074707,10.2223405838013,10.8923845291138,11.2183618545532,11.138505935668899,10.6885375976563,10.548979298740001,10.4307736286619,9.2535174475933708,9.63453681464574,8.9524845356580904,8.7129714124508499,8.1824438032959996]
["KCS-E2L117C1","KCS",5,"E2L117C1",886,"Average Tare Weight, ALL OTHER FREIGHT CARS",36.799999237060497,39.200000762939503,36.5,36.599998474121101,36.700000762939503,36.599998474121101,36.799999237060497,37.099998474121101,37.5,38.1,38.4,38.6,38.9,39.299999999999997,39.6,39.799999999999997]
["KCS-E2L117C4","KCS",5,"E2L117C4",889,"E/L Ratio, All Freight Cars, ALL OTHER FREIGHT CAR",2.0443646907806401,2.0304868221282999,2.0800049304962198,2.04930448532104,2.0273380279540998,2.0145013332366899,2.02449631690979,1.99918365478516,2.0030982494354199,2.0466343958352402,2.0499626834729199,2.02523222428644,2.03681006493506,2.0591714444717701,2.0467537302746499,2.0575677032936102]
["KCS-E2L117C5","KCS",5,"E2L117C5",890,"Local circuity, ALL OTHER FREIGHT CARS",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["KCS-E2L117C8","KCS",5,"E2L117C8",893,"Spotted-to-Pulled Ratio, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L117C12","KCS",5,"E2L117C12",897,"CD per Interterminal Switch, ALL OTHER FREIGHT CARS",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["KCS-E2L117C15","KCS",5,"E2L117C15",900,"CD per Load & Unload Intraterminal Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["KCS-E2L117C18","KCS",5,"E2L117C18",903,"CM per Interchange Switch, ALL OTHER FREIGHT CARS",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["KCS-E2L117C23","KCS",5,"E2L117C23",908,"Average Miles between I&I Switches, ALL OTHER FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["KCS-E2L117C26","KCS",5,"E2L117C26",911,"SEMs per Interchange Switch, ALL OTHER FREIGHT CARS",4.8161888122558603,4.68174076080322,4.2110533714294398,3.7671465873718302,3.7481915950775102,3.99387454986572,4.1133995056152299,4.0841188430786097,3.9191303253173801,3.8679590762046798,3.82461699717601,3.3929563974509001,3.5326634987034402,3.2825776630746302,3.1947561845653101,3.0002293945418699]
["KCS-E2L117C27","KCS",5,"E2L117C27",912,"SEMs per Intraterminal Switch, ALL OTHER FREIGHT CARS",13.1350612640381,12.768384933471699,11.484691619873001,10.2740364074707,10.2223405838013,10.8923845291138,11.2183618545532,11.138505935668899,10.6885375976563,10.548979298740001,10.4307736286619,9.2535174475933708,9.63453681464574,8.9524845356580904,8.7129714124508499,8.1824438032959996]
["KCS-E2L118C1","KCS",5,"E2L118C1",915,"Average Tare Weight, AVERAGE ALL FREIGHT CARS",34.400001525878899,34.400001525878899,34.299999237060497,34.299999237060497,34.299999237060497,34.299999237060497,34.200000762939503,34.299999237060497,34.400001525878899,34.6,34.799999999999997,34.799999999999997,34.9,35.200000000000003,35.299999999999997,35.4]
["KCS-E2L118C4","KCS",5,"E2L118C4",918,"E/L Ratio, All Freight Cars, AVERAGE ALL FREIGHT CARS",1.8673075437545801,1.89904749393463,1.93076360225677,1.9089107513427701,1.8745934963226301,1.82916867733002,1.8268445730209399,1.78404653072357,1.7833515405654901,1.77836201571851,1.79868575296779,1.80426986844499,1.7968359896983299,1.8169288736118501,1.8138238416866701,1.8185397707744999]
["KCS-E2L118C8","KCS",5,"E2L118C8",922,"Spotted-to-Pulled Ratio, AVERAGE ALL FREIGHT CARS",1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.9,1.9,1.9,1.9,1.9,1.9,1.9]
["KCS-E2L118C11","KCS",5,"E2L118C11",925,"CD per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L118C14","KCS",5,"E2L118C14",928,"CD per Load & Unload Industry Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["KCS-E2L118C19","KCS",5,"E2L118C19",933,"CM per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["KCS-E2L118C22","KCS",5,"E2L118C22",936,"Average CM per CD, Railroad-Owned, AVERAGE ALL FREIGHT CARS",478.25128173828102,558.17980957031295,575.27001953125,682.88671875,568.424560546875,399.16067504882801,512.25140380859398,445.99639892578102,365.51058959960898,358.90958784072802,392.22637853440102,381.794031804817,349.84331025776498,394.25519355420403,443.57288994839899,374.97712559015099]
["KCS-E2L118C23","KCS",5,"E2L118C23",937,"Average Miles between I&I Switches, AVERAGE ALL FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["KCS-E2L118C26","KCS",5,"E2L118C26",940,"SEMs per Interchange Switch, AVERAGE ALL FREIGHT CARS",4.8161883354187003,4.68174076080322,4.2110533714294398,3.7671463489532502,3.7481915950775102,3.99387502670288,4.1133990287780797,4.0841197967529297,3.9191296100616499,3.8679590762046798,3.82461699717601,3.3929563974509001,3.5326634987034402,3.2825776630746302,3.1947561845653101,3.0002293945418699]
["KCS-E2L118C29","KCS",5,"E2L118C29",943,"SEMs per I&I Switch, AVERAGE ALL FREIGHT CARS",2.18917679786682,2.1280639171600302,1.9141151905059799,1.7123392820358301,1.70372354984283,1.81539750099182,1.8697268962860101,1.85641777515411,1.78142285346985,1.7581632164566701,1.73846227144364,1.54225290793223,1.60575613577429,1.49208075594301,1.45216190207514,1.3637406338826701]
["KCS-E2L204C1","KCS",5,"E2L204C1",947,"Average Tare Weight - Non-Refrigerated TCU",5,5,5,4.9000000953674299,4.9000000953674299,4.9000000953674299,4.9000000953674299,5,5,5,4.9000000000000004,4.7,4.9000000000000004,4.9000000000000004,4.8,4.8]
["KCS-E2L207C1","KCS",5,"E2L207C1",950,"L/E Ratio - Refrigerated/Non-Refrigerated - TCU",1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.48,1.48,1.48,1.48,1.48,1.48,1.48]
["KCS-E2L210C1","KCS",5,"E2L210C1",953,"Average Locomotive Units - Through Train",2.6940734386444101,2.89255666732788,2.89302325248718,2.8698022365570099,2.7101202011108398,2.8839650154113801,2.71827244758606,2.8164212703704798,2.68285131454468,2.6584479809430599,2.8359759992497602,2.7546073695812701,2.7841655475229699,2.4699154763292301,2.9540310481260699,2.81242240787298]
["KCS-E2L215C1","KCS",5,"E2L215C1",958,"Train Crews (Excl Train Switching)",36992.078125,35825.2734375,33565.515625,30717.1171875,33233.61328125,37153.9921875,38161.66796875,38502.90234375,46776.2265625,44535.855250444001,40630.259318225799,44805.915671333401,45838.833131180203,47061.194994955702,40148.593319253901,48277.490345810496]
["KCS-E2L218C1","KCS",5,"E2L218C1",961,"Average Crew Wages (Assigned To TM-Crew)",7.5133228302001998,7.6112685203552202,7.1006875038146999,7.1576957702636701,7.42513132095337,8.1404733657836896,8.3329124450683594,8.5945596694946307,9.3741712570190394,9.6032843331400404,9.2711698226870798,9.4628764057199799,9.7783319047741895,10.1639317616168,10.260261221340899,10.840076123895599]
["KCS-E2L219C1","KCS",5,"E2L219C1",962,"General Overhead Ratio",1.1270829439163199,1.1440182924270601,1.11242759227753,1.1337797641754199,1.13282489776611,1.1066381931304901,1.11226558685303,1.10683810710907,1.0931702852249101,1.0893988809811599,1.11473076407575,1.1175846760043,1.1034260558537901,1.13732314914116,1.1858739672781,1.21886196263772]
["KCS-E2L301C2","KCS",5,"E2L301C2",965,"Residual Factor, Industry Switching, Privately-Owned",13.2507653045376,38.708041371441901,28.3942379465703,32.087852790185103,25.6613878039166,22.7792495059375,22.376608707560599,18.40588970544573,18.020394734507999,16.862701427037901,17.069845473480399,15.8837277407049,12.5156879917634,14.502655779195701,11.91410876606937,16.5880976694528]
["KCS-E2L303C1","KCS",5,"E2L303C1",968,"Residual Factor, Interchange Switching, Railroad-Owned",2.9942854097485401,7.4293470756878799,8.3176760683695594,11.195254640137099,8.6347210625413098,7.5194689792277103,8.2668476688235693,7.5296631218124226,8.9432404710616105,9.6799909130011095,9.2662505889940405,9.3990402441260095,9.4680814753446292,9.6149651371826295,10.463072795729527,11.384583582264501]
["KCS-E2L305C1","KCS",5,"E2L305C1",972,"Residual Factor, Mileage, Railroad-Owned",-0.649684115061817,-1.09869069163544,2.4483250649806099,1.2362434751834901,-0.45140726042298301,-6.2028965564065697,0.49294578237990799,-4.1064032530953645,-0.14970937150972599,-1.0894605357519,-1.1196889409747399,-7.9801263942377796,-9.5965679903438392,-6.4737206420918696,-9.0093457493644884,-5.9012102037835401]
["NS-E1L101C1","NS",2,"E1L101C1",1,"Gross Ton Mile (GTM), OPR Expense",2.6648973580449798E-3,2.7200023178011201E-3,3.40578425675631E-3,2.5547416880726801E-3,2.9828022234141801E-3,3.5927817225456199E-3,3.7041448522359098E-3,3.7654081825166902E-3,3.6254457663744701E-3,2.9040417542131399E-3,2.6555880112242398E-3,2.8801320781751002E-3,3.12100611903453E-3,3.0153994877419698E-3,2.7662605135994099E-3,2.7503900816658201E-3]
["NS-E1L103C1","NS",2,"E1L103C1",7,"Train Mile (TM) - Other Than Crew, OPR Expense",0.64191710948944103,0.74692136049270597,0.66245692968368497,0.71147596836090099,0.77762472629547097,0.72947740554809604,0.746864974498749,0.87255007028579701,0.69109201431274403,0.74784219377309202,0.67766557303302399,0.58543418928914204,0.61324164640766998,0.67764990066065101,0.62800480974161399,0.57609494581292997]
["NS-E1L104C1","NS",2,"E1L104C1",10,"Train Mile (TM) - Crew, OPR Expense",8.6396532058715803,8.1957769393920898,8.8786325454711896,8.9094877243041992,9.8325462341308594,10.4100961685181,9.6722545623779297,9.69189453125,10.051073074340801,11.2617761346963,11.737643027389099,12.401424489133699,12.5141174067561,12.0303817037865,12.548667028682701,12.716199652135099]
["NS-E1L105C1","NS",2,"E1L105C1",13,"Locomotive Unit Mile (LUM), OPR Expense",4.3334889411926296,4.5630197525024396,5.9910411834716797,3.8772671222686799,5.0620484352111799,6.5825934410095197,6.5073866844177202,6.8552002906799299,6.6377749443054199,4.6784908380105801,4.06932276047326,4.8140069201144504,5.8249111644032903,5.4110641719186097,5.38692698237048,5.7908949366698996]
["NS-E1L105C2","NS",2,"E1L105C2",14,"Locomotive Unit Mile (LUM), DRL Expense",0.43994641304016102,0.42040392756462103,0.44018584489822399,0.52030742168426503,0.46431353688240101,0.475950807332993,0.46113231778144798,0.473748028278351,0.44541454315185502,0.47740193875974202,0.570888890044431,0.62574806463627197,0.78043762373328196,0.70499093023995896,0.82170632183428505,0.94431243546903798]
["NS-E1L106C2","NS",2,"E1L106C2",17,"CLOR (Carloads Handled) - Other, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L107C2","NS",2,"E1L107C2",20,"CLOR (Carloads Handled) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L108C3","NS",2,"E1L108C3",24,"CLOT (Carloads Orig Or Term) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L109C2","NS",2,"E1L109C2",26,"CLOT (Carloads Orig Or Term) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L111C2","NS",2,"E1L111C2",32,"Switch Engine Minutes (SEM), DRL Expense",0.21085204184055301,0.20973366498947099,0.19947303831577301,0.24189914762973799,0.22126865386962899,0.21970754861831701,0.21814295649528501,0.20750954747200001,0.20272459089756001,0.211548362604845,0.255819235019561,0.25188084966111102,0.253328185994255,0.28484010279882599,0.31293937628234803,0.37805337803649303]
["NS-E1L112C2","NS",2,"E1L112C2",35,"Ton Miles In Lake Transfer Service, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L113C2","NS",2,"E1L113C2",38,"Tons Handled at Coal Terminals, DRL Expense",0.18035778403282199,0.162788510322571,0.13727293908596,0.17750105261802701,0.150655537843704,0.109926328063011,0.179133921861649,0.21159549057483701,0.25930765271186801,0.35953692934713299,0.45385535603728699,0.27923050864619697,0.25224701089812801,0.31139529417248002,0.39936901093007399,0.40978083794905301]
["NS-E1L113C3","NS",2,"E1L113C3",39,"Tons Handled at Coal Terminals, ROI Expense",0.194725856184959,0.20382101833820301,0.20103286206722301,0.22649437189102201,0.222923904657364,0.25357800722122198,0.312366813421249,0.28627073764800998,0.35856372117996199,0.42446804583219,0.42609946937879001,0.32518999604349502,0.32821090549815601,0.30381361733530898,0.38483535123462298,0.48974345692430998]
["NS-E1L114C3","NS",2,"E1L114C3",42,"Tons Handled at Ore Terminals, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L116C1","NS",2,"E1L116C1",46,"Refrigerated Car Miles, OPR Expense",8.2542441785335499E-2,4.5571729540824897E-2,0.218623861670494,6.5670065581798595E-2,7.9211898148059803E-2,0.123459815979004,0.10656899958849,9.5871344208717305E-2,0.11401587724685699,0.106378884830039,9.6523896375776894E-2,4.9178473680402401E-2,7.4637152475366494E-2,3.80898945058116E-2,3.1777408882440003E-2,5.1573959222204403E-2]
["NS-E1L117C1","NS",2,"E1L117C1",49,"Protective Service Reefer TCU Days, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B5890&\"-\"&D5890","v":"NS-E1L117C3"},"NS",2,"E1L117C3",51,"Protective Service Reefer TCU Days, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L119C3","NS",2,"E1L119C3",57,"Other (Non-Refrigerated) TCU Days, ROI Expense",0.71079707145690896,1.0351874828338601,1.49441885948181,1.3666456937789899,1.4955592155456501,3.3519382476806601,3.7034137248992902,3.5961844921112101,3.8100750446319598,3.807328124384,3.22565433809193,3.3370214414955202,4.2623280879439696,3.3741980474226798,2.7367662490470699,3.4107298660346301]
["NS-E1L120C3","NS",2,"E1L120C3",60,"TCUs Loaded And Unloaded (L&UL), ROI Expense",3.0386672019958501,3.6607031822204599,5.0993227958679199,5.1959099769592303,4.7507286071777299,4.9610309600830096,5.1331086158752397,5.0584268569946298,4.6839222908020002,4.3149022981323899,3.8961700534750001,4.5112555586073002,5.0490240925710799,4.2190299988945696,3.6911757716769902,5.4103808401610296]
["NS-E1L121C3","NS",2,"E1L121C3",63,"MVUs Loaded And Unloaded (L&UL), ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L122C1","NS",2,"E1L122C1",64,"TCUs Picked Up and Delivered (PU&D), OPR Expense",808.27008056640602,1087.56970214844,651.05944824218795,1210.08581542969,730.6337890625,730.65783691406295,623.82940673828102,697.32946777343795,207.32247924804699,184.110205855347,184.11645752528099,152.26842326484601,131.383345489817,141.650627853294,208.85328453063801,172.51397279084699]
["NS-E1L201C1","NS",2,"E1L201C1",67,"CM(R), OPR Expense, Railroad-Owned, BOX - 40 FT",1.6515545547008501E-2,1.36955222114921E-2,1.7338979989290199E-2,2.8159564360976198E-2,3.5810805857181501E-2,4.46583926677704E-2,4.1520241647958797E-2,4.0503550320863703E-2,3.7515003234147998E-2,4.1509587053931603E-2,4.4197853760476399E-2,4.7045712745921502E-2,4.4886145859844399E-2,3.9508783299617503E-2,3.2511490016592502E-2,2.9485985121053201E-2]
["NS-E1L201C5","NS",2,"E1L201C5",71,"CM(Y), DRL Expense, Railroad-Owned, BOX - 40 FT",0.89266765117645297,0.30589973926544201,0.31685516238212602,0.27391695976257302,0.28080624341964699,0.285829067230225,0.26833310723304699,0.18597106635570501,0.25905728340148898,0.31317205488942002,0.24535075672648601,0.28650752686064401,0.36840492014025,0.30967093351867597,0.270328381348308,0.29961653927592602]
["NS-E1L201C10","NS",2,"E1L201C10",76,"CD(Y), OPR Expense, Railroad-Owned, BOX - 40 FT",1.9801095724105799,1.6223280429840099,2.0771338939666699,3.3192710876464799,4.2203497886657697,5.2806906700134304,5.0274505615234402,4.9509530067443803,4.5230417251586896,4.9461933958693498,5.2535892701042801,5.5826241793484002,5.3973921796965003,4.8451460724770898,4.0381380209735198,3.7290944695988402]
["NS-E1L201C12","NS",2,"E1L201C12",78,"CD(Y), ROI Expense, Railroad-Owned, BOX - 40 FT",-13.2499351501465,-15.7915182113647,-18.373756408691399,-18.965328216552699,0.36033087968826299,0.363272905349731,0.37858772277831998,0.310319423675537,0.27263092994689903,0.31074900735530497,0.24031923832862001,0.28019513115559702,0.31650623103321202,0.123180459647459,8.2031819926576599E-2,9.4172213787655099E-2]
["NS-E1L202C3","NS",2,"E1L202C3",82,"CM(R), ROI Expense, Railroad-Owned, BOX - 50 FT",-7.2932094335556003E-2,-8.8993959128856701E-2,-0.10191920399665801,-0.10880161821842201,2.2466478403657701E-3,2.24639871157706E-3,2.3070140741765499E-3,1.9744788296520701E-3,1.8149144016206299E-3,2.0425682732107399E-3,1.6296793785673001E-3,1.9295044908052301E-3,2.1382806338822499E-3,9.1037850550940201E-4,6.3708878115241604E-4,6.79772036015293E-4]
["NS-E1L202C6","NS",2,"E1L202C6",85,"CM(Y), ROI Expense, Railroad-Owned, BOX - 50 FT",-0.18962329626083399,-0.23138411343097701,-0.264989674091339,-0.28288453817367598,5.8412835933268096E-3,5.8406400494277503E-3,5.9982328675687296E-3,5.1336516626179201E-3,4.7187828458845598E-3,5.3106775103479303E-3,4.23716638427499E-3,5.0167116760935901E-3,5.55952964809385E-3,2.36698411432444E-3,1.65643083099629E-3,1.76740729363977E-3]
["NS-E1L202C9","NS",2,"E1L202C9",88,"CD(R), ROI Expense, Railroad-Owned, BOX - 50 FT",-13.249936103820801,-15.7915191650391,-18.373756408691399,-18.965328216552699,0.36033093929290799,0.363272935152054,0.37858772277831998,0.310319423675537,0.27263092994689903,0.31074900735530497,0.24031923832862001,0.28019513115559702,0.31650623103321202,0.123180459647459,8.2031819926576599E-2,9.4172213787655099E-2]
["NS-E1L202C10","NS",2,"E1L202C10",89,"CD(Y), OPR Expense, Railroad-Owned, BOX - 50 FT",1.9801095724105799,1.6223280429840099,2.0771338939666699,3.3192710876464799,4.2203497886657697,5.2806906700134304,5.0274505615234402,4.9509530067443803,4.5230417251586896,4.9461933958693498,5.2535892701042801,5.5826241793484002,5.3973921796965003,4.8451460724770898,4.0381380209735198,3.7290944695988402]
["NS-E1L202C13","NS",2,"E1L202C13",92,"CM(R), DRL Expense, Privately-Owned, BOX - 50 FT",1.03821849822998,0.53365314006805398,0.63786906003952004,1.0356638431549099,0.77112054824829102,0.839707851409912,1.0349757671356199,1.33490037918091,1.0307861566543599,0.98750677591734004,1.5970983034626201,1.73812305542582,1.5247403672326001,2.2712133045883802,2.1151458036749999,1.931654183679]
["NS-E1L203C4","NS",2,"E1L203C4",96,"CM(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED",0.150692269206047,0.13234038650989499,0.148851618170738,0.158545017242432,0.159519478678703,0.17392072081565901,0.1964181214571,0.23141571879386899,0.25367155671119701,0.25332654464839399,0.23832891628794201,0.249375433283999,0.21350493580191099,0.17924391198474299,0.123206747081271,0.139047856387331]
["NS-E1L203C9","NS",2,"E1L203C9",101,"CD(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED",3.4641997814178498,3.9536192417144802,4.8397116661071804,5.0233612060546902,6.2612981796264604,6.56475925445557,5.8482308387756303,4.2602844238281303,4.1569838523864702,3.56367407611598,3.2666625822636299,3.5436776769894398,3.9813110813211701,3.1305099720640999,2.8088679426096399,3.8440789708555498]
["NS-E1L203C11","NS",2,"E1L203C11",103,"CD(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED",14.232450485229499,9.3698997497558594,9.8780012130737305,10.6737670898438,9.0740766525268608,9.1414651870727504,6.5732378959655797,9.1286144256591797,10.625679969787599,11.1368326136683,11.628832381854799,13.635771266468,18.509694509477299,17.997618638171101,20.114489642426701,30.238076096039499]
["NS-E1L204C2","NS",2,"E1L204C2",107,"CM(R), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",3.6400526762008702E-2,3.2271154224872603E-2,2.8986930847168E-2,3.8504078984260601E-2,3.0305083841085399E-2,2.67568547278643E-2,1.7913613468408598E-2,5.4295076988637404E-3,4.2892443016171499E-3,8.4953335605092595E-3,1.7330219061886001E-2,1.2414078333459999E-2,1.4780398586488301E-2,1.2349707516131901E-2,1.90989135576114E-2,1.5945537978818699E-2]
["NS-E1L204C5","NS",2,"E1L204C5",110,"CM(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",9.4641402363777202E-2,8.3904907107353197E-2,7.5366005301475497E-2,0.100110530853271,7.8793220221996293E-2,6.9567799568176297E-2,4.6575400978326797E-2,1.4116710983216801E-2,1.11520392820239E-2,2.20878672573241E-2,4.5058569560903497E-2,3.2276603666996001E-2,3.8429036324869603E-2,3.2109239541942898E-2,4.9657175249789798E-2,4.1458398744928598E-2]
["NS-E1L204C6","NS",2,"E1L204C6",111,"CM(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",6.02658353745937E-2,8.5239313542842907E-2,8.2465328276157407E-2,9.0665116906166104E-2,8.2550495862960802E-2,8.5245475172996493E-2,0.132141083478928,0.116868153214455,0.13123264908790599,0.16875997229342099,0.174171052193376,0.16241460538001601,0.19149626855390101,0.166654500293059,0.16536507033120801,0.175251730642208]
["NS-E1L204C9","NS",2,"E1L204C9",114,"CD(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",2.5836737155914302,3.7358944416046098,3.9439926147460902,4.2532486915588397,3.97241139411926,4.30916404724121,4.6726312637329102,4.7238717079162598,5.5965290069580096,7.2221746531572499,7.5226363917405497,6.8577464175762204,7.8110313775517799,6.77892869592604,6.8191127432455696,7.2522846379635402]
["NS-E1L204C12","NS",2,"E1L204C12",117,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",2.5836734771728498,3.7358944416046098,3.9439930915832502,4.2532491683959996,3.97241187095642,4.30916452407837,4.6726317405700701,4.7238717079162598,5.5965285301208496,7.2221746531572499,7.5226363917405497,6.8577464175762204,7.8110313775517799,6.77892869592604,6.8191127432455696,7.2522846379635499]
["NS-E1L205C3","NS",2,"E1L205C3",121,"CM(R), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.7308419346809401E-2,3.3721420913934701E-2,4.0288660675287198E-2,4.93549667298794E-2,4.8357769846916199E-2,4.7297492623329197E-2,4.9762558192014701E-2,5.2650086581707001E-2,5.8001715689897503E-2,8.2983740575184498E-2,7.9967211441266603E-2,8.1685296433797294E-2,0.100208628522235,9.1233708886194198E-2,8.88230305565922E-2,9.1211328286753393E-2]
["NS-E1L205C8","NS",2,"E1L205C8",126,"CD(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",3.8612914085388201,4.1680493354797399,5.12213134765625,8.7000789642334002,4.8604383468627903,2.50761818885803,-2.83464574813843,7.9641566276550302,7.1144771575927699,8.0767643053891494,6.3020170876239501,5.0047671825606601,5.3511058098513802,6.0421569164576496,8.2282107402151095,6.7453261501879096]
["NS-E1L205C10","NS",2,"E1L205C10",128,"CD(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",6.39792680740356,6.7733883857727104,8.0770998001098597,8.4804973602294904,6.7296242713928196,5.6855449676513699,7.4577841758728001,8.8564414978027308,8.5334186553955096,6.0451796030192,4.7136617610854303,4.7768919551249196,5.0931281381152802,5.8302933387438101,5.79083236741074,5.6468986305108704]
["NS-E1L206C1","NS",2,"E1L206C1",132,"CM(R), OPR Expense, Railroad-Owned, HOPPER - COVERED",4.9565207213163397E-2,4.1980441659688998E-2,4.5168418437242501E-2,5.2932139486074399E-2,6.2045831233263002E-2,6.7530915141105693E-2,6.13999143242836E-2,5.7698391377925901E-2,5.5700160562992103E-2,5.6190175088698897E-2,5.5581656016692502E-2,5.8550402498230902E-2,6.2696494142636602E-2,6.4832843649081498E-2,6.5782385734893006E-2,8.49588644515753E-2]
["NS-E1L206C4","NS",2,"E1L206C4",135,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",0.128869518637657,0.109149292111397,0.117437809705734,0.13762369751930201,0.16131915152072901,0.17558047175407401,0.15963985025882699,0.15001575648784601,0.14482045173645,0.14609445523061701,0.14451230564340101,0.15223104649540001,0.16301088477085501,0.16856539348761199,0.17103420291072199,0.220893047574095]
["NS-E1L206C5","NS",2,"E1L206C5",136,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",0.112717792391777,4.93178591132164E-2,4.70436736941338E-2,4.5524049550294897E-2,3.83947305381298E-2,4.0702704340219498E-2,6.43949955701828E-2,4.21487353742123E-2,4.7905985265970202E-2,5.0931789968171499E-2,4.9515117537395202E-2,5.3413794067707798E-2,5.9697675767203598E-2,5.8901521963815498E-2,5.7188637505494001E-2,6.0928271620738203E-2]
["NS-E1L206C8","NS",2,"E1L206C8",139,"CD(R), DRL Expense, Railroad-Owned, HOPPER - COVERED",18.0482997894287,10.514940261840801,11.0188493728638,11.080681800842299,7.8171129226684597,8.7898292541503906,4.2875828742981001,3.2418086528778098,4.1620788574218803,5.3414950058591302,4.6512764507131301,5.2836586937493699,5.9990301379238504,4.22524178691401,3.8025794548356102,4.4196389004269099]
["NS-E1L206C11","NS",2,"E1L206C11",142,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",18.048297882080099,10.514940261840801,11.0188493728638,11.080681800842299,7.8171129226684597,8.7898292541503906,4.2875828742981001,3.2418086528778098,4.1620793342590297,5.3414950058591302,4.6512764507131301,5.2836586937493699,5.9990301379238504,4.22524178691401,3.8025794548356102,4.4196389004269099]
["NS-E1L207C2","NS",2,"E1L207C2",146,"CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.1057687699794801E-2,3.00276353955269E-2,3.0120616778731301E-2,4.2854178696870797E-2,2.7263410389423402E-2,2.60606203228235E-2,4.07533198595047E-2,2.5167901068925899E-2,2.8249314054846798E-2,2.8375803165368502E-2,5.1505969150491496E-3,4.5152811854761703E-3,1.1830261390411399E-2,1.2645185905223E-2,2.18434281840095E-2,1.3654491781033401E-2]
["NS-E1L207C7","NS",2,"E1L207C7",151,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.2940368652343799,2.09904217720032,2.0639121532440199,1.98938012123108,1.59307289123535,1.57266545295715,2.0247876644134499,2.5552711486816402,2.5975768566131601,2.8964070718003798,2.80098415639304,2.9705529807404898,2.3906226105261998,2.6758205714785901,2.9035163085070401,3.0732951678397198]
["NS-E1L207C10","NS",2,"E1L207C10",154,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.2940368652343799,2.09904217720032,2.0639121532440199,1.9893798828125,1.59307277202606,1.57266545295715,2.0247876644134499,2.5552711486816402,2.5975768566131601,2.8964070718003798,2.8009841563930502,2.9705529807404898,2.3906226105261998,2.6758205714785999,2.9035163085070401,3.0732951678397198]
["NS-E1L207C13","NS",2,"E1L207C13",157,"CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - GENERAL",1.40643416671082E-4,2.0545510051306299E-4,1.49737315950915E-4,1.4800779172219301E-4,1.4420115621760501E-4,3.78737786377314E-5,4.7959863877622397E-5,5.4207666835281998E-5,1.26850776723586E-4,5.6967547006541203E-5,2.9591377765201399E-5,5.35892322690826E-5,4.8416402202633501E-5,2.3787815623372401E-5,3.2542772740372898E-5,2.9419275639018399E-5]
["NS-E1L208C3","NS",2,"E1L208C3",160,"CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",6.9666951894760104E-2,7.0850633084774003E-2,9.4818659126758603E-2,9.1670647263526903E-2,8.1020310521125793E-2,8.5420005023479503E-2,0.135483458638191,9.1940268874168396E-2,8.0676518380641896E-2,7.8196917898538498E-2,8.0608987469833596E-2,0.115195024603567,0.17060446332058701,0.12656480979684401,0.133992984021822,0.191849367387843]
["NS-E1L208C4","NS",2,"E1L208C4",161,"CM(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.17843092978000599,0.14268259704113001,0.13795302808284801,0.13710018992424,0.13215523958206199,0.12900322675705,0.13279266655445099,0.12776164710521701,0.119337275624275,0.110973738463935,0.126156869325939,0.16729165911469701,0.21932754285593201,0.36458899366212399,0.365022065242672,0.47488324248991098]
["NS-E1L208C7","NS",2,"E1L208C7",164,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",3.47120141983032,2.8903100490570099,2.80392622947693,2.76710033416748,2.58344697952271,2.4632472991943399,2.2753481864929199,2.1825926303863499,1.9359073638916,1.88844905299948,2.1537022596811699,2.7061662581292398,3.1741887726131899,5.2877897883625202,5.4664462076793603,7.4105843871074004]
["NS-E1L208C10","NS",2,"E1L208C10",167,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",3.47120141983032,2.89030981063843,2.80392646789551,2.76710057258606,2.5834472179412802,2.4632475376129199,2.2753481864929199,2.1825931072235099,1.9359073638916,1.88844905299948,2.1537022596811699,2.7061662581292398,3.1741887726131899,5.2877897883625202,5.4664462076793603,7.4105843871074004]
["NS-E1L209C2","NS",2,"E1L209C2",172,"CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",0.30314245820045499,0.120159082114697,0.124204881489277,9.7864970564842196E-2,0.111682295799255,0.100696839392185,0.112453930079937,0.110403127968311,0.114873066544533,0.119583223326776,0.112753957906396,0.110655073851792,0.106203668490623,0.101132806321653,9.6295544979024303E-2,9.3647778450619307E-2]
["NS-E1L209C5","NS",2,"E1L209C5",175,"CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",0.78817176818847701,0.31241384148597701,0.32293239235878002,0.25444924831390398,0.29037368297576899,0.26181149482727101,0.29238015413284302,0.28704801201820401,0.29867064952850297,0.31091638064961802,0.29316029055663001,0.28770319201465899,0.27612953807562002,0.26294529643629799,0.25036841694546302,0.24348422397161101]
[{"$f":"B6018&\"-\"&D6018","v":"NS-E1L209C9"},"NS",2,"E1L209C9",179,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",-2.78627965599298E-3,-1.4702554326504499E-3,2.4507958441972701E-2,5.4363679140806198E-2,6.8591482937335996E-2,4.1415255516767502E-2,3.0658008530736001E-2,3.2472603023052202E-2,2.5529857724905E-2,2.3320993025992699E-2,5.02025428108872E-2,6.6752248079962995E-2,8.8849000468633005E-2,9.1495128269105094E-2,0.135648856548999,0.13274325112905699]
["NS-E1L209C12","NS",2,"E1L209C12",182,"CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",-2.78627965599298E-3,-1.4702553162351301E-3,2.4507960304617899E-2,5.43636903166771E-2,6.8591482937335996E-2,4.14152592420578E-2,3.0658008530736001E-2,3.24726067483425E-2,2.55298558622599E-2,2.3320993025992699E-2,5.02025428108872E-2,6.6752248079962995E-2,8.8849000468633005E-2,9.1495128269105094E-2,0.135648856548999,0.13274325112905699]
["NS-E1L210C2","NS",2,"E1L210C2",185,"CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",0.15069688856601701,6.3940532505512196E-2,7.0862837135791806E-2,6.7528985440730993E-2,8.3390660583972903E-2,8.5955843329429599E-2,6.5845310688018799E-2,6.5301090478897095E-2,6.5383218228817E-2,6.4563663509943997E-2,6.2259110516926203E-2,6.1543087618987698E-2,5.8197642986521497E-2,5.5688409164786297E-2,5.2285063310576203E-2,5.3596470404127003E-2]
["NS-E1L210C3","NS",2,"E1L210C3",186,"CM(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",4.2451596818864302E-3,1.6018589667510201E-4,1.4776189345866401E-4,7.1459820901509401E-5,1.0824739001691299E-4,9.8040494776796604E-5,8.9883207692764699E-5,1.0770474909804799E-4,1.00015487987548E-4,5.89952726451858E-5,7.4846617824402296E-5,1.2506356720193699E-4,2.2270521126486901E-4,2.2366490327013601E-4,2.7196465440540701E-4,2.5638834151510702E-4]
["NS-E1L210C6","NS",2,"E1L210C6",189,"CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",1.10374204814434E-2,4.1648396290838702E-4,3.84180922992527E-4,1.85795754077844E-4,2.8144315001554798E-4,2.54905433394015E-4,2.33696424402297E-4,2.8003207989968397E-4,2.6004086248576598E-4,1.53387708877484E-4,1.9460120634344599E-4,3.2516527472503703E-4,5.7903354928865597E-4,5.8152874850235297E-4,7.0710810145406099E-4,6.6660968793927399E-4]
["NS-E1L210C9","NS",2,"E1L210C9",192,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",0.856833815574646,2.0924283191561699E-2,1.94452181458473E-2,9.6476469188928604E-3,1.42542980611324E-2,1.3932984322309499E-2,1.39357224106789E-2,1.7107659950852401E-2,1.5814209356903999E-2,9.3571528323564603E-3,1.1767239495800601E-2,2.0806581001970099E-2,4.1284110198334903E-2,4.4424028074533099E-2,5.0645395461976203E-2,5.3404878714207703E-2]
["NS-E1L211C1","NS",2,"E1L211C1",197,"CM(R), OPR Expense, Railroad-Owned, FLAT - TOFC",4.3822275474667497E-3,3.2991489861160499E-3,4.1561024263501202E-3,6.5271803177893196E-3,9.3322768807411194E-3,1.1089157313108401E-2,1.00846672430634E-2,9.0316319838166202E-3,9.6959779039025307E-3,8.7479743382454997E-3,1.15258847929372E-2,1.23771205004026E-2,1.4359127215498001E-2,1.2813432317068701E-2,1.2062306839359599E-2,1.6712733235289299E-2]
["NS-E1L211C4","NS",2,"E1L211C4",200,"CM(Y), OPR Expense, Railroad-Owned, FLAT - TOFC",1.1393794789910301E-2,8.5777938365936297E-3,1.08058648183942E-2,1.6970690339803699E-2,2.4263912811875302E-2,2.8831809759140001E-2,2.6220142841339101E-2,2.348224632442E-2,2.52095106989145E-2,2.2744733279438299E-2,2.99673004616367E-2,3.2180513301046799E-2,3.7333730760294698E-2,3.3314924024378599E-2,3.1361997782335102E-2,4.34531064117522E-2]
["NS-E1L211C8","NS",2,"E1L211C8",204,"CD(R), DRL Expense, Railroad-Owned, FLAT - TOFC",11.0364179611206,4.8201370239257804,4.8815412521362296,5.1068787574768102,2.89802026748657,3.3255305290222199,3.9042024612426798,7.07397556304932,7.4763655662536603,7.0907476762880197,6.3924241739539198,3.0159639273455201,1.73667793812019,1.4314555265011399,4.5787451318896002,6.0461613655743696]
["NS-E1L211C11","NS",2,"E1L211C11",207,"CD(Y), DRL Expense, Railroad-Owned, FLAT - TOFC",11.0364179611206,4.8201370239257804,4.8815412521362296,5.1068787574768102,2.8980200290679901,3.3255310058593799,3.9042024612426798,7.073974609375,7.4763655662536603,7.0907476762880197,6.3924241739539198,3.0159639273455201,1.73667793812019,1.4314555265011299,4.57874513188961,6.0461613655743696]
["NS-E1L212C1","NS",2,"E1L212C1",210,"CM(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",6.3484422862529796E-2,0.17154812812805201,0.232190862298012,0.27331361174583402,9.1306596994399997E-2,7.3420606553554493E-2,9.4344437122344998E-2,0.10015986859798399,0.106252759695053,9.6652276478251795E-2,9.4436999427298801E-2,9.5672660405714802E-2,7.2264504910366303E-2,5.65751094393106E-2,3.9871519056934902E-2,5.2708833516615199E-2]
["NS-E1L212C2","NS",2,"E1L212C2",211,"CM(R), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",0.13020865619182601,0.13003450632095301,0.16987796127796201,0.19685381650924699,0.19498470425605799,0.212840095162392,0.231890469789505,0.19743329286575301,0.219369322061539,0.234609075248084,0.226603799909601,0.23229975210794301,0.19563317321252799,0.187375629216639,0.220738231406297,0.205286368227896]
["NS-E1L212C5","NS",2,"E1L212C5",214,"CM(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",0.33854204416275002,0.33808961510658297,0.44168215990066501,0.51181983947753895,0.50695997476577803,0.553383529186249,0.60291588306427002,0.51332676410675004,0.57036066055297896,0.60998359564501703,0.58916987976496304,0.60397935548065196,0.50864625035257305,0.48717663596326199,0.57391940165637401,0.53374455739253202]
["NS-E1L212C9","NS",2,"E1L212C9",218,"CD(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",18.736557006835898,20.554517745971701,30.726100921630898,36.671535491943402,33.256893157958999,32.141815185546903,34.085777282714801,34.002655029296903,39.063674926757798,36.826729728309601,34.219657549019601,37.072949355818899,35.349018789506303,29.408673298645201,28.6504623333879,32.3334032919919]
["NS-E1L212C13","NS",2,"E1L212C13",222,"CM(R), DRL Expense, Privately-Owned, FLAT - MULTILEVEL",0.46392804384231601,0.201277300715446,0.245327919721603,0.32228949666023299,0.28007996082305903,0.25574907660484297,0.21550366282463099,0.20581428706645999,0.21692362427711501,0.21839031579455001,0.227340605368128,0.23442486651956601,0.24140286756766299,0.24630463071718001,0.308768812585342,0.29739353334785701]
["NS-E1L213C3","NS",2,"E1L213C3",225,"CM(R), ROI Expense, Railroad-Owned, FLAT - GENERAL",3.6217886954546002E-2,3.6126069724559798E-2,4.0575016289949403E-2,2.3950442671775801E-2,9.6093937754631001E-2,0.10632648319005999,0.120049111545086,0.10407442599535,3.5188477486372001E-2,5.3813509776714898E-3,-8.0766125294899401E-3,-1.1901962296952701E-2,-8.6028777632422802E-3,4.26454878880673E-3,4.5780071947762804E-3,6.38250273139899E-3]
["NS-E1L213C7","NS",2,"E1L213C7",229,"CD(R), OPR Expense, Railroad-Owned, FLAT - GENERAL",7.3377933502197301,6.0587711334228498,11.1685781478882,13.1103363037109,21.203619003295898,32.183589935302699,175.38984680175801,217.62156677246099,166.64703369140599,24.3637613459059,1.8426983265266299,2.08056320993493,3.4718206057249099,5.18382305643647,5.91659763937131,7.3835496474876203]
["NS-E1L213C10","NS",2,"E1L213C10",232,"CD(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL",7.3377933502197301,6.0587711334228498,11.1685781478882,13.1103363037109,21.203617095947301,32.183586120605497,175.38984680175801,217.62158203125,166.64703369140599,24.3637613459059,1.8426983265266299,2.08056320993493,3.4718206057249099,5.18382305643647,5.91659763937131,7.3835496474876203]
["NS-E1L213C13","NS",2,"E1L213C13",235,"CM(R), DRL Expense, Privately-Owned, FLAT - GENERAL",1.54694271087646,0.34194892644882202,0.44269943237304699,0.70088434219360396,4.9060511589050302,4.8850240707397496,13.053590774536101,7.9642825126647896,8.2999124526977504,7.1821590741866803,0.38950561782995702,0.27750125655789498,0.24104693443990899,0.242638284411688,0.57557049883107902,0.32061661487323001]
["NS-E1L214C1","NS",2,"E1L214C1",236,"CM(R), OPR Expense, Railroad-Owned, FLAT - OTHER",3.0272217467427299E-2,2.60850638151169E-2,2.9797460883855799E-2,4.1762150824069998E-2,6.1915453523397397E-2,7.0949897170066806E-2,8.4914460778236403E-2,9.1108486056327806E-2,8.8748499751091003E-2,6.7320088060291494E-2,4.9015271757034601E-2,5.0659439720570701E-2,4.7553377956086898E-2,5.2211022940164803E-2,5.1773255350497198E-2,6.3035214856126107E-2]
["NS-E1L214C4","NS",2,"E1L214C4",239,"CM(Y), OPR Expense, Railroad-Owned, FLAT - OTHER",7.8707695007324205E-2,6.7821130156517001E-2,7.7473394572734805E-2,0.108581587672234,0.160980254411697,0.18446987867355299,0.220777958631516,0.236882343888283,0.230746060609818,0.17503222895675799,0.12743970656829001,0.131714543273484,0.123638782685826,0.135748659644428,0.134610463911293,0.163891558625928]
[{"$f":"B6082&\"-\"&D6082","v":"NS-E1L214C8"},"NS",2,"E1L214C8",243,"CD(R), DRL Expense, Railroad-Owned, FLAT - OTHER",42.738029479980497,18.342445373535199,21.170978546142599,24.0077304840088,25.125932693481399,28.747142791748001,20.381156921386701,15.4322805404663,16.839311599731399,15.447261491978001,15.157740582629801,13.4385227680729,14.7011347374349,9.3969999802970303,9.8998512956705405,15.333978453217799]
["NS-E1L214C12","NS",2,"E1L214C12",247,"CD(Y), ROI Expense, Railroad-Owned, FLAT - OTHER",2.7759451866149898,3.1932015419006299,5.1296758651733398,6.4521126747131303,5.6207327842712402,6.4021635055542001,7.8785824775695801,5.1996598243713397,4.55580711364746,4.1415207192838999,3.09366171600933,3.3526287971570699,3.5964794106556401,2.41148133112209,2.4036571275137901,2.8479649312426099]
["NS-E1L215C2","NS",2,"E1L215C2",250,"CM(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,1.7899323254823699E-2,0,1.2456899508833901E-2,1.0959975386746401E-2,1.3238035996574899E-2,1.36054295740281E-2,1.2881843056756799E-2,1.5188784319622801E-2,1.6649225262665299E-2,1.3176693126679E-2]
["NS-E1L215C6","NS",2,"E1L215C6",254,"CM(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L215C9","NS",2,"E1L215C9",257,"CD(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L215C12","NS",2,"E1L215C12",260,"CD(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L215C13","NS",2,"E1L215C13",261,"CM(R), DRL Expense, Privately-Owned, TANK <22,000 GAL",0.13425613939762099,4.8544075340032598E-2,4.5850787311792401E-2,4.3012391775846502E-2,3.38187552988529E-2,3.19103710353374E-2,1.7899323254823699E-2,1.47406319156289E-2,1.2456899508833901E-2,1.0959975386746401E-2,1.3238035996574899E-2,1.36054295740281E-2,1.2881843056756799E-2,1.5188784319622801E-2,1.6649225262665299E-2,1.3176693126679E-2]
["NS-E1L216C3","NS",2,"E1L216C3",264,"CM(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L216C7","NS",2,"E1L216C7",268,"CD(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L216C11","NS",2,"E1L216C11",272,"CD(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L217C1","NS",2,"E1L217C1",275,"CM(R), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",1.1109246872365501E-2,8.8051389902830107E-3,1.2016911059618E-2,1.6921589151024801E-2,2.0969774574041401E-2,2.32891347259283E-2,1.90199632197618E-2,1.78862269967794E-2,1.87246799468994E-2,2.23807703677192E-2,5.3666279749142898E-2,8.1052387814536594E-2,0.136198145157785,0.136711516071991,0.14347580937631099,0.20751057729484301]
["NS-E1L217C5","NS",2,"E1L217C5",279,"CM(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",7.1844775229692502E-3,1.2889129109680699E-2,1.38183571398258E-2,1.5238586813211399E-2,1.5555795282125501E-2,1.48296970874071E-2,1.1656348593532999E-2,8.2673253491520899E-3,9.1277826577425003E-3,9.7044502944460306E-2,2.8574815422140801E-2,9.7758602159021195E-4,1.05695529459113E-2,1.15490928513178E-2,1.7874251475879999E-2,2.2580525203154098E-2]
["NS-E1L217C8","NS",2,"E1L217C8",282,"CD(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",-7.2603478431701696,-1.1253237724304199,-1.0130188465118399,0.87568086385726895,-0.64253079891204801,-0.14698851108551,-0.88720166683196999,-1.8592264652252199,-3.8426241874694802,6.3902354549379101,-23.369774782694201,-41.352051270321702,-52.486847379173,-57.0817471418342,-59.734241730732997,-80.953864544675497]
["NS-E1L217C9","NS",2,"E1L217C9",283,"CD(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",2.2077085971832302,2.55399823188782,3.1354143619537398,2.8508644104003902,2.2768528461456299,2.1507844924926798,2.1635613441467298,1.99651098251343,1.95524001121521,1.34135260736129,1.63755677603759,1.74670358953591,1.9336281833531499,1.64429074392654,1.66716486252544,2.6305700245516301]
["NS-E1L217C12","NS",2,"E1L217C12",286,"CD(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",2.2077085971832302,2.5539979934692401,3.1354141235351598,2.8508641719818102,2.2768533229827899,2.1507842540740998,2.1635611057281499,1.9965112209320099,1.9552401304245,1.34135260736129,1.63755677603759,1.74670358953591,1.9336281833531499,1.64429074392654,1.66716486252544,2.6305700245516301]
["NS-E1L218C2","NS",2,"E1L218C2",289,"CM(R), DRL Expense, Railroad-Owned, AUTO RACKS",5.75377456843853E-2,0.143042787909508,0.180376946926117,0.26619252562522899,0.19509999454021501,0.20171061158180201,0.17282558977603901,0.132831886410713,0.149841904640198,0.16117463212052599,0.147588524340896,0.154771075760918,0.129284377914096,0.12938503445054,0.16836474493228001,0.15371364505489299]
["NS-E1L218C6","NS",2,"E1L218C6",293,"CM(Y), ROI Expense, Railroad-Owned, AUTO RACKS",0.15362644195556599,0.400862246751785,0.60483235120773304,0.72295796871185303,0.58038192987442005,0.57580751180648804,0.53091812133789096,0.53116422891616799,0.61076706647872903,0.57064673698469504,0.53412550609853104,0.59688549867057095,0.56778100534072695,0.47479097313884799,0.46207450550637102,0.51893315865663803]
["NS-E1L218C10","NS",2,"E1L218C10",297,"CD(Y), OPR Expense, Railroad-Owned, AUTO RACKS",0.10575807839632,12.419109344482401,16.4658107757568,19.034297943115199,3.1771757602691699,1.4660274982452399,4.5418763160705602,5.4054527282714799,6.0208387374877903,5.3640402682981101,4.7433232278144803,5.0063580904184404,3.2188704230696001,2.0324391598849698,0.12312721531318301,0.18185401462263701]
["NS-E1L218C13","NS",2,"E1L218C13",300,"CM(R), DRL Expense, Privately-Owned, AUTO RACKS",1.6569355502724599E-2,1.7995601519942301E-2,2.4581553414464E-2,9.921002201735969E-4,2.5866871699690801E-2,1.1874490417540099E-2,8.4810778498649597E-3,8.6317807435989397E-3,1.0816371999680999E-2,1.30104974844034E-2,1.6457750961105199E-2,1.6917391034244299E-2,1.3742329326082299E-2,1.4560430010472801E-2,2.3258389121373801E-2,1.3781132495121501E-2]
["NS-E1L219C4","NS",2,"E1L219C4",304,"CM(Y), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B6146&\"-\"&D6146","v":"NS-E1L219C7"},"NS",2,"E1L219C7",307,"CD(R), OPR Expense, Railroad-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E1L219C8","NS",2,"E1L219C8",308,"CD(R), DRL Expense, Railroad-Owned, ACCESSORIAL",6.3792258501052898E-2,7.1792371571063995E-2,8.3010278642177596E-2,0.125197052955627,4.9119062721729299E-2,4.4295206665992702E-2,4.8821140080690398E-2,2.1134080365300199E-2,1.82056855410337E-2,2.22311168320392E-2,6.4286898243602901E-4,7.4968441050081202E-3,3.38403237561491E-2,3.0752870298719901E-2,4.0853699372449599E-2,3.3081616923418898E-2]
["NS-E1L219C11","NS",2,"E1L219C11",311,"CD(Y), DRL Expense, Railroad-Owned, ACCESSORIAL",6.3792258501052898E-2,7.1792371571063995E-2,8.3010271191596999E-2,0.125197052955627,4.9119062721729299E-2,4.4295206665992702E-2,4.8821140080690398E-2,2.1134080365300199E-2,1.82056855410337E-2,2.22311168320392E-2,6.4286898243602901E-4,7.4968441050081202E-3,3.38403237561491E-2,3.0752870298719901E-2,4.0853699372449599E-2,3.3081616923418898E-2]
["NS-E1L220C1","NS",2,"E1L220C1",314,"CM(R), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",4.4279471039771999E-2,4.43535819649696E-2,4.9303263425826999E-2,5.8261070400476497E-2,4.8188146203756298E-2,4.4308912009000799E-2,4.9572736024856602E-2,5.2717633545398698E-2,5.5235624313354499E-2,5.9787938738432397E-2,6.1234256375151203E-2,5.9396273120653098E-2,5.7132558473117302E-2,6.2714128266316796E-2,5.93412316087445E-2,5.7557168711642397E-2]
["NS-E1L220C5","NS",2,"E1L220C5",318,"CM(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",0.109281934797764,6.9942444562912001E-2,6.93618208169937E-2,8.2459680736064897E-2,6.4222820103168501E-2,6.18491843342781E-2,6.7627929151058197E-2,4.9082417041063302E-2,5.4916985332965899E-2,6.84696114464933E-2,6.6097220634082507E-2,6.0181078404467798E-2,6.8863553501606695E-2,7.2120124616145295E-2,8.9692656377525298E-2,8.7653852108802804E-2]
["NS-E1L220C9","NS",2,"E1L220C9",322,"CD(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",2.7740502357482901,3.3056795597076398,4.1624894142150897,4.4956016540527299,4.6923842430114702,5.39992380142212,6.3043565750122097,5.7418260574340803,5.7829856872558603,6.2072184541649698,6.4875627373732003,6.8166685185276501,7.9228458374519501,6.7406790996778199,6.4947724818443202,7.6333985482698203]
["NS-E1L220C13","NS",2,"E1L220C13",326,"CM(R), DRL Expense, Privately-Owned, AVERAGE ALL FREIGHT CARS",0.18776464462280301,7.2813294827938094E-2,7.4681825935840607E-2,7.82877951860428E-2,7.2990640997886699E-2,7.4538752436637906E-2,7.5475782155990601E-2,7.0992916822433499E-2,7.4058890342712402E-2,7.6238155195267804E-2,8.1051855797551906E-2,8.2948041810218101E-2,8.4785323178122401E-2,8.31655409507224E-2,9.6612093844070004E-2,8.8766793478692999E-2]
["NS-E1L221C3","NS",2,"E1L221C3",329,"CM(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.145402401685715,0.164439842104912,0.24240431189537001,0.28868687152862499,0.245470985770226,0.242838844656944,0.22188393771648399,0.21899370849132499,0.24884846806526201,0.23197491946594301,0.21534350934528801,0.24050573860952101,0.23083303124670801,0.19061214431901499,0.18537275580389601,0.208453591209211]
["NS-E1L221C6","NS",2,"E1L221C6",332,"CM(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.37804576754570002,0.42754399776458701,0.63025104999542203,0.75058603286743197,0.63822376728057895,0.63138014078140303,0.57689917087554898,0.56938338279724099,0.64700752496719405,0.60313479061145303,0.55989312429774696,0.625314920384754,0.60016588124144299,0.49559157522943798,0.48196916509012899,0.54197933714394797]
["NS-E1L221C7","NS",2,"E1L221C7",333,"CD(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",5.3770332336425799,14.464547157287599,19.7280578613281,23.159408569335898,8.0050745010375994,6.50671434402466,9.0408372879028303,10.0001316070557,11.1132469177246,10.262079569306801,10.0941558823639,10.167877635089001,7.6071518782738696,5.93459337419627,4.1894395179876502,5.57316069073413]
["NS-E1L221C10","NS",2,"E1L221C10",336,"CD(Y), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",5.3770332336425799,14.464547157287599,19.7280578613281,23.1594123840332,8.0050745010375994,6.5067138671875,9.0408372879028303,10.0001316070557,11.1132469177246,10.262079569306801,10.0941558823639,10.167877635089001,7.6071518782738696,5.93459337419627,4.18943951798766,5.57316069073413]
["NS-E1L221C13","NS",2,"E1L221C13",339,"CM(R), DRL Expense, Privately-Owned, TOTAL FLAT, MULTILEVEL",0.46392804384231601,0.201277300715446,0.245327919721603,0.32228949666023299,0.28007996082305903,0.25574907660484297,0.21550366282463099,0.20581428706645999,0.21692362427711501,0.21839031579455001,0.227340605368128,0.23442486651956601,0.24140286756766299,0.24630463071718001,0.308768812585342,0.29739353334785701]
["NS-E1L305C1","NS",2,"E1L305C1",344,"L&D Expense, FRESH VEGETABLES",0.60301697254180897,0.243790358304977,0.41229620575904802,0.19410522282123599,7.3158152401447296E-2,0.65559387207031306,0.35545039176940901,0.20792415738105799,0.48678919672965998,0.41470897303029602,0.34160943933107601,0.389577076844837,0.26595492810377602,0.63672310190342996,0.200726594272612,0.51497044391303703]
["NS-E1L308C1","NS",2,"E1L308C1",347,"L&D Expense, COAL",3.01631726324558E-3,3.2460147049277999E-3,3.05656832642853E-3,4.3408023193478602E-3,3.2279870938509698E-3,3.3305299002677198E-3,4.0287571027874903E-3,3.9105019532144096E-3,2.7237308677285901E-3,2.14346200941452E-3,2.0286106009389702E-3,4.8588212337537899E-3,4.4838032093151596E-3,3.9408800824081098E-3,1.5177075802263499E-3,2.1313169653889401E-3]
["NS-E1L312C1","NS",2,"E1L312C1",351,"L&D Expense, DAIRY PRODUCTS",0.26197466254234297,1.34666740894318,1.7574552297592201,0.46422058343887301,0.35715392231941201,0.464790970087051,0.49275985360145602,0.75572431087493896,1.05871522426605,2.0809273501940702,0.96986246387669905,0.98166953399452095,2.6580326093429498,4.3113833540049997,3.8502678120262801,1.82206074815941]
["NS-E1L315C1","NS",2,"E1L315C1",354,"L&D Expense, FLOUR",3.2923668622970602E-2,7.6696105301380199E-2,8.2328729331493405E-2,4.6068139374256099E-2,6.2322694808244698E-2,7.4686713516712203E-2,7.1782425045967102E-2,5.7252213358879103E-2,2.7048252522945401E-2,5.3978262161745102E-2,8.1389778583540101E-2,2.0658939350466098E-2,5.6218799270150201E-2,4.7762989723968197E-2,5.6966833978788899E-2,5.6377434374590599E-2]
["NS-E1L318C1","NS",2,"E1L318C1",357,"L&D Expense, RICE",0.18275606632232699,0.20021592080593101,0.26043739914894098,0.49083593487739602,0.26900073885917702,0.26474368572235102,0.105855084955692,0.30795875191688499,0.195555880665779,0.171957354616004,0.217271284411443,0.20353585332434401,0.10460667322949101,0.201985129218855,0.18705377019309699,0.27474099401881502]
["NS-E1L319C1","NS",2,"E1L319C1",358,"L&D Expense, PREPARED FLOUR",0.37972217798232999,0.44714790582656899,0.31831541657447798,0.25416249036788902,0.14075364172458599,4.0416184812784202E-2,0.17804516851902,0,0,0,0,0,0,0,0,0]
["NS-E1L322C1","NS",2,"E1L322C1",361,"L&D Expense, BEER",0.21311140060424799,0.13795143365859999,0.11230556666851001,0.209407404065132,0.334010690450668,0.38553339242935197,0.90072369575500499,0.90642565488815297,0.56750947237014804,1.0174552404741599,1.7311441019848299,1.9743613882701201,3.1530590569508399,8.7245439934215394,2.5082539988572998,1.4391021304396601]
["NS-E1L325C1","NS",2,"E1L325C1",364,"L&D Expense, MISC FOOD PREPARATIONS",4.9347322434186901E-2,3.9073646068572998E-2,6.88051283359528E-2,4.7288753092288999E-2,7.3226988315582303E-2,4.44420874118805E-2,5.8179348707199097E-2,6.4795158803462996E-2,6.5988443791866302E-2,4.7256400580346102E-2,0.10027194560448401,5.8322594141169803E-2,4.7792372956870097E-2,4.0860279141872603E-2,3.6097560727487002E-2,5.5607518381965003E-2]
["NS-E1L330C1","NS",2,"E1L330C1",369,"L&D Expense, PLYWOOD OR VENEER",7.4905700981617002E-2,4.27759401500225E-2,8.9939765632152599E-2,0.12727469205856301,8.0512069165706607E-2,9.6415840089321095E-2,4.3528910726308802E-2,3.7447415292263003E-2,2.03599594533443E-2,0.12145549472462901,0.216664798239351,2.9783990826895802E-2,7.0972097170494602E-2,6.9536828674594306E-2,6.8338321410531103E-2,0.117691760964366]
["NS-E1L333C1","NS",2,"E1L333C1",372,"L&D Expense, PULP, PAPER AND ALLIED PRODUCTS",0.26838248968124401,0.28085958957672102,0.29805308580398598,0.29972025752067599,0.20974843204021501,0.18133181333541901,0.162495583295822,0.17467743158340501,0.16834378242492701,0.12844722302166001,0.153450512751615,0.17213338337717099,0.106044886035222,0.12062119539989299,8.5510400889075799E-2,0.144576608542514]
["NS-E1L337C1","NS",2,"E1L337C1",376,"L&D Expense, COV PAPER/PAPERBOARD",0.14351396262645699,2.3441700264811498E-2,5.0217267125844997E-2,4.3607987463474301E-2,3.0316181480884601E-2,3.9156388491392101E-2,6.6796630620956393E-2,3.8177575916051899E-2,0.123719930648804,8.9984059162479299E-2,4.7553798615383003E-2,9.2495401211793692E-3,6.3031332334864496E-3,3.4192846214227003E-2,6.3265511684125697E-2,8.0745058269087004E-3]
["NS-E1L340C1","NS",2,"E1L340C1",379,"L&D Expense, CHEMICALS",5.11742942035198E-2,4.20025512576103E-2,3.6974240094423301E-2,4.2966037988662699E-2,3.3213671296834897E-2,4.8909343779087101E-2,5.0282698124647099E-2,3.2089069485664402E-2,3.1751915812492398E-2,3.2152053773539503E-2,4.5385256484858798E-2,3.7555629213460701E-2,3.01283549154009E-2,4.3525262911993302E-2,4.1050292308664603E-2,4.8456104800754497E-2]
["NS-E1L343C1","NS",2,"E1L343C1",382,"L&D Expense, SYN FIBRES/RESINS/RUBBER",0.14274440705776201,6.1173558235168499E-2,8.7265506386756897E-2,0.10607888549566299,8.5183314979076399E-2,0.12817049026489299,0.132741883397102,9.0175598859787001E-2,0.100434817373753,8.3801154952120302E-2,0.11696684497985201,0.106955975079934,5.2621767832795201E-2,0.10260436617034099,6.5752737420087498E-2,0.139082763813134]
["NS-E1L344C1","NS",2,"E1L344C1",383,"L&D Expense, MISC CHEMICALS PRODUCTS",4.3860375881195103E-2,5.9413857758045197E-2,5.3479108959436403E-2,6.6045254468917805E-2,5.3832165896892499E-2,6.0841087251901599E-2,1.3048115186393301E-2,3.7528481334447902E-2,7.7735278755426398E-3,5.2866308194148698E-2,6.3770333647115898E-3,9.4641084932867905E-3,5.7108239653403999E-3,4.0468951069907904E-3,3.7185460949404302E-2,2.3238877916688001E-2]
["NS-E1L347C1","NS",2,"E1L347C1",386,"L&D Expense, RUBBER AND MISC PLASTICS",0.121731825172901,8.4463320672512096E-2,5.7188738137483597E-2,2.3528395220637301E-2,1.31647260859609E-2,7.10021182894707E-2,0.156284719705582,9.4427227973938002E-2,0.101616881787777,2.8642241838434401E-2,2.2199691128442101E-2,1.54454766150119E-2,6.0183038438072003E-3,9.8465346002906795E-2,4.7641514960962097E-2,3.8674507534544302E-2]
["NS-E1L350C1","NS",2,"E1L350C1",389,"L&D Expense, STONE, CLAY AND GLASS PRODUCTS",2.8050996363163001E-2,2.94760055840015E-2,2.3014681413769701E-2,2.2323321551084501E-2,1.25137800350785E-2,2.0365133881568898E-2,1.3885203748941401E-2,1.2379656545817901E-2,2.0123468711972198E-2,1.8672422852622099E-2,1.5618687233242201E-2,7.1743035945493697E-3,1.00761913642266E-2,1.1213559823315599E-2,1.4322538640667201E-2,1.0220925283838099E-2]
["NS-E1L355C1","NS",2,"E1L355C1",394,"L&D Expense, PRIMARY IRON/STEEL PRODUCTS",3.4884344786405598E-2,5.3362432867288603E-2,3.6286663264036199E-2,9.7192518413066906E-2,4.7952342778444297E-2,4.3800264596939101E-2,2.8834400698542598E-2,3.0930418521165799E-2,4.0773164480924599E-2,4.32040643335612E-2,3.8559282806765002E-2,6.04644823038471E-2,4.9514510216627401E-2,7.8182518416237898E-2,1.5334172940485001E-2,4.9781753141333498E-2]
["NS-E1L358C1","NS",2,"E1L358C1",397,"L&D Expense, FABRICATED METAL PRODUCTS",0.29441612958908098,8.34800750017166E-2,0.120782092213631,0.57032650709152199,0.127834737300873,0.121632412075996,0.10238241404295,0.34850579500198398,2.4500768631696701E-2,4.4205237424147302E-2,4.1813711219508103E-2,0.13085792181979899,5.4769202978317402E-2,0.17031496412081801,3.3467763128923302E-3,0.226221318634625]
["NS-E1L362C1","NS",2,"E1L362C1",401,"L&D Expense, ENGINES/TURBINES",0,0,0,0.65623474121093806,0.37552052736282299,3.18804383277893E-2,0.92005145549774203,0.18546940386295299,0.75826698541641202,0.10592373868414701,1.7432681007613301E-2,0.11374880081262601,0.19588503448769101,0.627909057749931,-6.83448356503671E-4,0.166006178271392]
["NS-E1L365C1","NS",2,"E1L365C1",404,"L&D Expense, ALL OTHER MACHINERY EXCEPT ELECTRICAL",0.51521039009094205,0.112866580486298,0.80271893739700295,0.47596234083175698,0.30874112248420699,4.8945009708404499E-2,0.31174495816230802,0.42183950543403598,4.2986869812011701E-3,0.15186131419488499,9.5799168819499E-2,2.66155263257274E-3,0.14928714522905701,0.14762019602208301,5.02985279069205E-2,3.62333789688866E-2]
["NS-E1L368C1","NS",2,"E1L368C1",407,"L&D Expense, HOUSEHOLD APPLIANCES",0.205303609371185,0.23462562263011899,0.17131142318248699,0.277806997299194,0.25822886824607799,8.2644179463386494E-2,0.297059416770935,0.38408657908439597,0.13108573853969599,0.40999757319887098,0.15451085360087599,7.3435426620840294E-2,0.14930913105378599,0.247363305660388,7.2794077869062196E-2,8.71202277086814E-2]
["NS-E1L369C1","NS",2,"E1L369C1",408,"L&D Expense, RADIO OR TV SETS",6.56506299972534,7.9000549316406303,11.099229812622101,2.6888911724090598,3.2490937709808398,1.53677189350128,5.8817706108093297,24.248622894287099,3.8644213676452601,1.0204034771199,2.4656724349818999,0.16968987712112299,0.212309300578224,0.93635726795096297,0.93072368421052598,7.9683165020530504]
["NS-E1L372C1","NS",2,"E1L372C1",411,"L&D Expense, MOTOR PASSENGER CARS",1.6142339706420901,1.60462009906769,2.0916264057159402,1.80427742004395,1.1449105739593499,1.8661357164382899,2.4315426349639901,2.3879089355468799,2.9647860527038601,2.2775114836972699,2.3379065129382699,4.7704088395188302,3.82250992141388,3.6264625356952398,4.5673487040649103,7.7164689836323603]
["NS-E1L375C1","NS",2,"E1L375C1",414,"L&D Expense, ALL OTHER TRANSPORTATION EQUIPMENT",2.6227355003356899E-2,0.10049141198396699,3.2508585602045101E-2,6.5525375306606307E-2,0.26267328858375499,3.3132839947938898E-2,5.0899308174848598E-2,6.18039257824421E-2,9.2528991401195498E-2,3.1585700434175697E-2,7.6281476545512997E-2,0.119202553620429,7.6049686090451901E-2,4.0474509693458502,2.3140971066584299,1.6999942051205801E-2]
["NS-E1L380C1","NS",2,"E1L380C1",419,"L&D Expense, ALL OTHER MIXED SHIPMENTS",0.16601713001728099,0.88630723953247104,1.4442171668633799E-3,0.87179607152938798,0.75372087955474898,0.13352239131927501,3.1231531873345399E-2,9.3002393841743497E-2,1.03999447822571,0.416805851183083,0.345811739282818,0.14978310418351601,0.18150323928185,3.82302116571379,1.53221325354683,0.10334428935010299]
["NS-E2L101C1","NS",2,"E2L101C1",422,"Average Tare Weight, BOX - 40 FT",26.200000762939499,26.200000762939499,25.899999618530298,25.299999237060501,26,25.700000762939499,29,28.5,28.5,28.5,27.9,27.5,29,29,29.2,29.2]
["NS-E2L101C5","NS",2,"E2L101C5",426,"Local circuity, BOX - 40 FT",1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999856948899,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999,1.1399999999999999]
["NS-E2L101C8","NS",2,"E2L101C8",429,"Spotted-to-Pulled Ratio, BOX - 40 FT",1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.8,1.8,1.8,1.8,1.8,1.8,1.8]
["NS-E2L101C9","NS",2,"E2L101C9",430,"CD per Industry Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["NS-E2L101C12","NS",2,"E2L101C12",433,"CD per Interterminal Switch, BOX - 40 FT",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["NS-E2L101C18","NS",2,"E2L101C18",439,"CM per Interchange Switch, BOX - 40 FT",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["NS-E2L101C20","NS",2,"E2L101C20",441,"CM per Interterminal Switch, BOX - 40 FT",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["NS-E2L101C23","NS",2,"E2L101C23",444,"Average Miles between I&I Switches, BOX - 40 FT",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["NS-E2L101C26","NS",2,"E2L101C26",447,"SEMs per Interchange Switch, BOX - 40 FT",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["NS-E2L102C1","NS",2,"E2L102C1",451,"Average Tare Weight, BOX - 50 FT",33.5,33.900001525878899,34.099998474121101,34.200000762939503,34.5,34.299999237060497,32.599998474121101,32.700000762939503,32.799999237060497,32.799999999999997,32.9,33,33.200000000000003,33.4,33.6,34]
["NS-E2L102C4","NS",2,"E2L102C4",454,"E/L Ratio, All Freight Cars, BOX - 50 FT",1.8010500669479399,1.90346539020538,1.92928802967072,2.2033638954162602,2.0792210102081299,1.9658389091491699,2.1013298034668,2.09385466575623,1.94921779632568,1.89973698053656,2.04897110489711,1.9103912219972601,1.8135263157894701,1.87742387119356,1.9065762351220199,1.86807973757255]
["NS-E2L102C5","NS",2,"E2L102C5",455,"Local circuity, BOX - 50 FT",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["NS-E2L102C8","NS",2,"E2L102C8",458,"Spotted-to-Pulled Ratio, BOX - 50 FT",1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.79999995231628,1.8,1.8,1.8,1.8,1.8,1.8,1.8]
["NS-E2L102C14","NS",2,"E2L102C14",464,"CD per Load & Unload Industry Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L102C16","NS",2,"E2L102C16",466,"CD per Load & Unload Interterminal Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L102C19","NS",2,"E2L102C19",469,"CM per Intraterminal Switch, BOX - 50 FT",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["NS-E2L102C22","NS",2,"E2L102C22",472,"Average CM per CD, Railroad-Owned, BOX - 50 FT",562.25256347656295,565.11291503906295,562.05926513671898,580.63195800781295,533.62518310546898,541.47662353515602,577.70440673828102,578.30383300781295,541.52429199218795,548.24383515701595,555.61441377984499,534.453212527598,516.31512513141104,542.10456880957599,549.60304612458401,523.27424532518501]
["NS-E2L102C26","NS",2,"E2L102C26",476,"SEMs per Interchange Switch, BOX - 50 FT",3.8144278526306201,3.8931212425231898,4.15873050689697,4.1730580329895002,4.0252885818481401,4.0373163223266602,4.7107481956481898,4.4231705665588397,4.3516521453857404,4.5098960028236101,4.2608485099979703,4.1327752402438902,4.3307349404828601,4.2439109775633499,4.30551998464815,3.74821200698785]
["NS-E2L102C29","NS",2,"E2L102C29",479,"SEMs per I&I Switch, BOX - 50 FT",1.73383092880249,1.7696003913879399,1.89033174514771,1.89684450626373,1.8296765089035001,1.83514368534088,2.1412491798400901,2.0105321407318102,1.9780238866805999,2.0499527285561898,1.9367493227263499,1.87853420011086,1.96851588203767,1.92905044434698,1.95705453847643,1.70373273044902]
["NS-E2L103C1","NS",2,"E2L103C1",480,"Average Tare Weight, BOX - EQUIPPED",36.099998474121101,36.099998474121101,36.200000762939503,36.099998474121101,36.200000762939503,36.200000762939503,36.400001525878899,36.5,36.5,36.5,36.6,36.700000000000003,36.799999999999997,37,37.1,37.299999999999997]
["NS-E2L103C4","NS",2,"E2L103C4",483,"E/L Ratio, All Freight Cars, BOX - EQUIPPED",2.0295879840850799,2.0273768901825,2.0152735710143999,2.03553438186646,2.0011451244354199,2.0159239768981898,2.03893947601318,2.0125505924224898,1.94433689117432,1.9582120167124399,1.9745998129710101,1.9163206487225799,1.8735055463541599,1.8752922245499,1.83454627759593,1.8237705981575201]
["NS-E2L103C10","NS",2,"E2L103C10",489,"CD per Interchange Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["NS-E2L103C12","NS",2,"E2L103C12",491,"CD per Interterminal Switch, BOX - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["NS-E2L103C15","NS",2,"E2L103C15",494,"CD per Load & Unload Intraterminal Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L103C19","NS",2,"E2L103C19",498,"CM per Intraterminal Switch, BOX - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["NS-E2L103C22","NS",2,"E2L103C22",501,"Average CM per CD, Railroad-Owned, BOX - EQUIPPED",562.25256347656295,565.113037109375,562.059326171875,580.63195800781295,533.625244140625,541.47662353515602,577.70446777343795,578.30383300781295,541.52423095703102,548.24383515701595,555.61441377984499,534.453212527598,516.31512513141104,542.10456880957599,549.60304612458401,523.27424532518501]
["NS-E2L103C25","NS",2,"E2L103C25",504,"SEMs per Industry Switch, BOX - EQUIPPED",6.9353232383728001,7.0784020423889196,7.5613284111022896,7.5873780250549299,7.3187055587768599,7.340576171875,8.5649967193603498,8.0421285629272496,7.9120960235595703,8.1998109142247397,7.7469972909054103,7.5141368004434304,7.8740635281506597,7.7162017773879201,7.8282181539057296,6.8149309217960896]
["NS-E2L103C26","NS",2,"E2L103C26",505,"SEMs per Interchange Switch, BOX - EQUIPPED",3.8144280910491899,3.8931214809417698,4.15873003005981,4.1730580329895002,4.0252885818481401,4.0373163223266602,4.7107477188110396,4.4231705665588397,4.3516526222229004,4.5098960028236101,4.26084850999798,4.1327752402438902,4.3307349404828601,4.2439109775633499,4.30551998464815,3.74821200698785]
["NS-E2L104C2","NS",2,"E2L104C2",510,"E/L Ratio, Railroad-Owned, GONDOLA - PLAIN",1.8781882524490401,1.8701947927475,1.88200891017914,1.89772260189056,1.8666918277740501,1.8804360628128101,1.8899683952331501,1.9409083127975499,1.9486652612686199,2.02834323617996,1.99852916725287,1.9746231357514199,1.95092099315921,1.9691928411464701,1.98639220615965,1.94789447706136]
["NS-E2L104C4","NS",2,"E2L104C4",512,"E/L Ratio, All Freight Cars, GONDOLA - PLAIN",1.91049492359161,1.9039403200149501,1.90991711616516,1.93013203144073,1.90200519561768,1.9117773771286,1.9221655130386399,1.9613672494888299,1.96897315979004,2.0378279552797798,2.0084250769938801,1.99987779029579,1.97694103579929,1.9913543497016499,2.0010994606855999,1.95778974977654]
["NS-E2L104C8","NS",2,"E2L104C8",516,"Spotted-to-Pulled Ratio, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L104C11","NS",2,"E2L104C11",519,"CD per Intraterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L104C15","NS",2,"E2L104C15",523,"CD per Load & Unload Intraterminal Switch, GONDOLA - PLAIN",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L104C18","NS",2,"E2L104C18",526,"CM per Interchange Switch, GONDOLA - PLAIN",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["NS-E2L104C21","NS",2,"E2L104C21",529,"CM per I&I Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["NS-E2L104C22","NS",2,"E2L104C22",530,"Average CM per CD, Railroad-Owned, GONDOLA - PLAIN",562.25256347656295,565.11291503906295,562.059326171875,580.63201904296898,533.62518310546898,541.47668457031295,577.70440673828102,578.30389404296898,541.52423095703102,548.24383515701595,555.61441377984499,534.453212527598,516.31512513141104,542.10456880957702,549.60304612458401,523.27424532518501]
["NS-E2L104C27","NS",2,"E2L104C27",535,"SEMs per Intraterminal Switch, GONDOLA - PLAIN",10.4029846191406,10.617603302001999,11.341991424560501,11.381067276001,10.9780597686768,11.0108633041382,12.847495079040501,12.0631914138794,11.868143081665,12.2997163713371,11.6204959363581,11.2712052006652,11.811095292226,11.5743026660819,11.742327230858599,10.2223963826941]
["NS-E2L104C29","NS",2,"E2L104C29",537,"SEMs per I&I Switch, GONDOLA - PLAIN",1.73383092880249,1.7696005105972299,1.89033162593842,1.89684450626373,1.8296765089035001,1.83514392375946,2.1412491798400901,2.0105321407318102,1.9780240058898899,2.0499527285561898,1.9367493227263499,1.87853420011086,1.96851588203767,1.92905044434698,1.95705453847643,1.70373273044902]
["NS-E2L105C4","NS",2,"E2L105C4",541,"E/L Ratio, All Freight Cars, GONDOLA - EQUIPPED",1.9010044336319001,1.9375227689743,1.9965174198150599,2.23772168159485,1.9790726900100699,1.9129824638366699,2.0036242008209202,1.9776308536529501,1.83506202697754,1.9357015908322699,1.89343760406484,1.89334171121856,1.8681647449336101,1.93209099407915,1.9353522993779999,1.84930956046228]
["NS-E2L105C7","NS",2,"E2L105C7",544,"Average circuity, GONDOLA - EQUIPPED",1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.119,1.119,1.119,1.119,1.119,1.119,1.119]
["NS-E2L105C11","NS",2,"E2L105C11",548,"CD per Intraterminal Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L105C14","NS",2,"E2L105C14",551,"CD per Load & Unload Industry Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L105C17","NS",2,"E2L105C17",554,"CM per Industry Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L105C18","NS",2,"E2L105C18",555,"CM per Interchange Switch, GONDOLA - EQUIPPED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["NS-E2L105C23","NS",2,"E2L105C23",560,"Average Miles between I&I Switches, GONDOLA - EQUIPPED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
[{"$f":"B6402&\"-\"&D6402","v":"NS-E2L105C26"},"NS",2,"E2L105C26",563,"SEMs per Interchange Switch, GONDOLA - EQUIPPED",3.8144278526306201,3.89312076568604,4.15873050689697,4.1730575561523402,4.0252881050109899,4.0373163223266602,4.7107486724853498,4.4231705665588397,4.3516526222229004,4.5098960028236101,4.2608485099979703,4.1327752402438902,4.3307349404828601,4.2439109775633499,4.30551998464815,3.74821200698785]
["NS-E2L105C29","NS",2,"E2L105C29",566,"SEMs per I&I Switch, GONDOLA - EQUIPPED",1.7338308095932,1.7696005105972299,1.89033186435699,1.89684450626373,1.8296765089035001,1.83514392375946,2.1412494182586701,2.0105321407318102,1.9780238866805999,2.0499527285561898,1.9367493227263499,1.87853420011086,1.96851588203767,1.92905044434698,1.95705453847643,1.70373273044902]
["NS-E2L106C3","NS",2,"E2L106C3",569,"E/L Ratio, Privately-Owned, HOPPER - COVERED",2.0323371887207,2.02807593345642,2.03924512863159,2.0415403842925999,2.0301287174224898,2.0328726768493701,2.0274190902710001,2.02379298210144,2.01027178764343,2.0263198278648602,2.0345410327987801,2.0056374240038699,2.01338370059461,2.0205433324772399,2.0157476759114101,2.0094652621173301]
["NS-E2L106C7","NS",2,"E2L106C7",573,"Average circuity, HOPPER - COVERED",1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999]
["NS-E2L106C10","NS",2,"E2L106C10",576,"CD per Interchange Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["NS-E2L106C13","NS",2,"E2L106C13",579,"CD per I&I Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["NS-E2L106C14","NS",2,"E2L106C14",580,"CD per Load & Unload Industry Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L106C19","NS",2,"E2L106C19",585,"CM per Intraterminal Switch, HOPPER - COVERED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["NS-E2L106C22","NS",2,"E2L106C22",588,"Average CM per CD, Railroad-Owned, HOPPER - COVERED",562.25250244140602,565.11291503906295,562.059326171875,580.63201904296898,533.625244140625,541.47662353515602,577.70440673828102,578.30377197265602,541.52429199218795,548.24383515701595,555.61441377984499,534.453212527598,516.31512513141104,542.10456880957702,549.60304612458401,523.27424532518501]
["NS-E2L106C25","NS",2,"E2L106C25",591,"SEMs per Industry Switch, HOPPER - COVERED",6.9353227615356401,7.0784025192260698,7.5613279342651403,7.5873780250549299,7.3187050819396999,7.34057569503784,8.5649967193603498,8.0421285629272496,7.9120960235595703,8.1998109142247397,7.7469972909054103,7.5141368004434304,7.8740635281506597,7.7162017773879201,7.8282181539057296,6.8149309217960896]
["NS-E2L106C28","NS",2,"E2L106C28",594,"SEMs per Interterminal Switch, HOPPER - COVERED",8.3223896026611293,8.4940824508666992,9.0735940933227504,9.1048536300659197,8.7824468612670898,8.8086910247802699,10.277996063232401,9.6505546569824201,9.4945144653320295,9.8397730970696902,9.2963967490864903,9.0169641605321207,9.4488762337807906,9.2594421328654999,9.3938617846868695,8.1779171061553004]
["NS-E2L107C3","NS",2,"E2L107C3",598,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - GENERAL",2.0604126453399698,2.0466272830963099,2.0318067073821999,2.0502738952636701,2.0449891090393102,2.0452606678009002,2.0514364242553702,2.0225884914398198,2.00434350967407,2.0347698334965698,2.0630847827334802,2.0626751063609001,2.04020030602309,2.0228911319394398,2.0299401197604801,2.02398055033705]
["NS-E2L107C6","NS",2,"E2L107C6",601,"Interline circuity, HOPPER - OPEN TOP - GENERAL",1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.137,1.137,1.137,1.137,1.137,1.137,1.137]
["NS-E2L107C7","NS",2,"E2L107C7",602,"Average circuity, HOPPER - OPEN TOP - GENERAL",1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001]
["NS-E2L107C11","NS",2,"E2L107C11",606,"CD per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L107C14","NS",2,"E2L107C14",609,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L107C18","NS",2,"E2L107C18",613,"CM per Interchange Switch, HOPPER - OPEN TOP - GENERAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["NS-E2L107C21","NS",2,"E2L107C21",616,"CM per I&I Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["NS-E2L107C24","NS",2,"E2L107C24",619,"Average Miles between Interchange Switches, HOPPER - OPEN TOP - GENERAL",1483.9658203125,892.75531005859398,957.86175537109398,1176.68225097656,1525.32531738281,1417.59033203125,1172.28173828125,1076.75268554688,1125.01257324219,1086.1219599976801,797.61666091119298,1008.67596559452,1013.582777616,1212.1767137935799,807.69394497592896,1173.20089139896]
["NS-E2L107C28","NS",2,"E2L107C28",623,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",8.32238864898682,8.4940814971923793,9.0735931396484393,9.1048536300659197,8.7824468612670898,8.8086919784545898,10.277996063232401,9.6505546569824201,9.4945154190063494,9.8397730970696902,9.2963967490864903,9.0169641605321207,9.4488762337807906,9.2594421328654999,9.3938617846868695,8.1779171061553004]
["NS-E2L108C2","NS",2,"E2L108C2",626,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.0639383792877202,2.0647816658020002,2.0258529186248802,2.0627205371856698,2.04598045349121,2.0782520771026598,2.1887392997741699,2.1019909381866499,2.0472040176391602,2.0566327089495,2.0807312207117299,2.0687322162504,2.04810084591143,2.1107250617171101,2.0422946605911898,2.0076903023983301]
[{"$f":"B6466&\"-\"&D6466","v":"NS-E2L108C3"},"NS",2,"E2L108C3",627,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - SPECIAL",2.01297903060913,2.0165319442749001,2.0128338336944598,2.00859427452087,2.0167686939239502,2.0046632289886501,2.0221755504608199,2.0316920280456499,1.9995689392089799,2.0009487976443601,2.0096608948014301,2.01635799206128,1.9999117085499201,2.0064193792581402,2.0317522625667901,1.9955327744852001]
["NS-E2L108C7","NS",2,"E2L108C7",631,"Average circuity, HOPPER - OPEN TOP - SPECIAL",1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001]
["NS-E2L108C10","NS",2,"E2L108C10",634,"CD per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["NS-E2L108C14","NS",2,"E2L108C14",638,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L108C17","NS",2,"E2L108C17",641,"CM per Industry Switch, HOPPER - OPEN TOP - SPECIAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L108C20","NS",2,"E2L108C20",644,"CM per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["NS-E2L108C24","NS",2,"E2L108C24",648,"Average Miles between Interchange Switches, HOPPER - OPEN TOP - SPECIAL",2187.42431640625,1166.13452148438,985.24053955078102,1144.32922363281,1006.0556640625,1008.38629150391,671.47106933593795,706.27978515625,678.71765136718795,564.31825783536794,739.37780957613404,582.30731892876702,608.40646114831998,628.30106382900703,579.428673793646,515.22359200076505]
["NS-E2L108C27","NS",2,"E2L108C27",651,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",10.4029865264893,10.617603302001999,11.341991424560501,11.381066322326699,10.978058815002401,11.0108633041382,12.8474931716919,12.0631923675537,11.8681449890137,12.2997163713371,11.6204959363581,11.2712052006652,11.811095292226,11.5743026660819,11.742327230858599,10.2223963826941]
["NS-E2L108C28","NS",2,"E2L108C28",652,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",8.3223896026611293,8.4940814971923793,9.0735931396484393,9.1048536300659197,8.7824478149414098,8.8086910247802699,10.277996063232401,9.6505537033081108,9.4945144653320295,9.8397730970696902,9.2963967490864903,9.0169641605321207,9.4488762337807906,9.2594421328654999,9.3938617846868695,8.1779171061553004]
["NS-E2L109C3","NS",2,"E2L109C3",656,"E/L Ratio, Privately-Owned, REFRIGERATED - MECH",1.9724497795105,1.9805046319961499,1.95984888076782,1.9916387796402,2.01099824905396,1.9666998386383101,1.9876741170883201,1.99743723869324,1.97289443016052,2.02109872611465,2.0307497893850002,1.9987951807228901,2.0236734693877501,2.0435356200527699,1.9393665158371001,1.9845910707230301]
["NS-E2L109C6","NS",2,"E2L109C6",659,"Interline circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["NS-E2L109C10","NS",2,"E2L109C10",663,"CD per Interchange Switch, REFRIGERATED - MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["NS-E2L109C13","NS",2,"E2L109C13",666,"CD per I&I Switch, REFRIGERATED - MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["NS-E2L109C17","NS",2,"E2L109C17",670,"CM per Industry Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L109C20","NS",2,"E2L109C20",673,"CM per Interterminal Switch, REFRIGERATED - MECH",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["NS-E2L109C23","NS",2,"E2L109C23",676,"Average Miles between I&I Switches, REFRIGERATED - MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["NS-E2L109C24","NS",2,"E2L109C24",677,"Average Miles between Interchange Switches, REFRIGERATED - MECH",717.23791503906295,724.24475097656295,737.753173828125,778.76922607421898,796.67376708984398,789.92327880859398,778.74279785156295,795.01605224609398,857.05316162109398,920.182748750663,777.89888044487702,836.29055305829695,866.40156979603898,824.31394240411896,821.34315803014101,850.00825647894305]
["NS-E2L109C28","NS",2,"E2L109C28",681,"SEMs per Interterminal Switch, REFRIGERATED - MECH",8.32238864898682,8.4940824508666992,9.0735940933227504,9.1048545837402308,8.7824468612670898,8.8086910247802699,10.277997016906699,9.6505537033081108,9.4945154190063494,9.8397730970696902,9.2963967490864903,9.0169641605321207,9.4488762337807906,9.2594421328654999,9.3938617846868695,8.1779171061553004]
["NS-E2L110C2","NS",2,"E2L110C2",684,"E/L Ratio, Railroad-Owned, REFRIGERATED - NON-MECH",1.85350978374481,1.88082146644592,1.83316278457642,1.85119152069092,1.8388353586196899,1.8619734048843399,1.8754683732986499,1.8693716526031501,1.8195275068283101,1.84438081603436,1.87667009249743,1.84146069917613,1.8261648745519701,1.8418688230008999,1.8211636079656399,1.89465648854962]
["NS-E2L110C6","NS",2,"E2L110C6",688,"Interline circuity, REFRIGERATED - NON-MECH",1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.159,1.159,1.159,1.159,1.159,1.159,1.159]
[{"$f":"B6530&\"-\"&D6530","v":"NS-E2L110C9"},"NS",2,"E2L110C9",691,"CD per Industry Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["NS-E2L110C13","NS",2,"E2L110C13",695,"CD per I&I Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["NS-E2L110C16","NS",2,"E2L110C16",698,"CD per Load & Unload Interterminal Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L110C19","NS",2,"E2L110C19",701,"CM per Intraterminal Switch, REFRIGERATED - NON-MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["NS-E2L110C20","NS",2,"E2L110C20",702,"CM per Interterminal Switch, REFRIGERATED - NON-MECH",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["NS-E2L110C24","NS",2,"E2L110C24",706,"Average Miles between Interchange Switches, REFRIGERATED - NON-MECH",937.03643798828102,850.33166503906295,840.25891113281295,780.63116455078102,857.02648925781295,1765.345703125,1938.74365234375,2193.97216796875,2406.39501953125,2101.90395039339,2155.5830743727402,2166.6634280079102,2871.93814787068,2152.12568207711,1507.6895516919999,4757.3869733268602]
["NS-E2L110C27","NS",2,"E2L110C27",709,"SEMs per Intraterminal Switch, REFRIGERATED - NON-MECH",10.402985572814901,10.617603302001999,11.3419904708862,11.381066322326699,10.978058815002401,11.0108633041382,12.847495079040501,12.0631923675537,11.8681440353394,12.2997163713371,11.6204959363581,11.2712052006652,11.811095292226,11.5743026660819,11.742327230858599,10.2223963826941]
["NS-E2L111C2","NS",2,"E2L111C2",713,"E/L Ratio, Railroad-Owned, FLAT - TOFC",1.1636943817138701,1.1833610534668,1.1561467647552499,1.1343410015106199,1.0873329639434799,1.11013042926788,1.1176780462264999,1.12461745738983,1.09918248653412,1.1093335425522799,1.1408381254456199,1.12348045633065,1.0984546143995599,1.10288691250562,1.14300505511907,1.0969160003704499]
["NS-E2L111C5","NS",2,"E2L111C5",716,"Local circuity, FLAT - TOFC",1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.069,1.069,1.069,1.069,1.069,1.069,1.069]
["NS-E2L111C9","NS",2,"E2L111C9",720,"CD per Industry Switch, FLAT - TOFC",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["NS-E2L111C12","NS",2,"E2L111C12",723,"CD per Interterminal Switch, FLAT - TOFC",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["NS-E2L111C15","NS",2,"E2L111C15",726,"CD per Load & Unload Intraterminal Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L111C16","NS",2,"E2L111C16",727,"CD per Load & Unload Interterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L111C20","NS",2,"E2L111C20",731,"CM per Interterminal Switch, FLAT - TOFC",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["NS-E2L111C24","NS",2,"E2L111C24",735,"Average Miles between Interchange Switches, FLAT - TOFC",1015.73107910156,1142.01306152344,1222.44360351563,1429.3603515625,1350.41638183594,1372.65771484375,2639.12109375,2572.19506835938,2503.3828125,2458.9826974819498,2343.2130864802798,2302.7330118599798,2092.5376745106601,1981.41595167129,1858.7560673975399,1748.8216347551599]
["NS-E2L111C27","NS",2,"E2L111C27",738,"SEMs per Intraterminal Switch, FLAT - TOFC",10.402985572814901,10.617603302001999,11.341991424560501,11.381067276001,10.978058815002401,11.0108633041382,12.8474941253662,12.0631914138794,11.868143081665,12.2997163713371,11.6204959363581,11.2712052006652,11.811095292226,11.5743026660819,11.742327230858599,10.2223963826941]
["NS-E2L112C1","NS",2,"E2L112C1",741,"Average Tare Weight, FLAT - MULTILEVEL",54.299999237060497,54.299999237060497,54.200000762939503,54.400001525878899,54.900001525878899,54.5,54,54,53.799999237060497,53.6,53.6,53.4,53.3,53.1,53.1,53.1]
["NS-E2L112C5","NS",2,"E2L112C5",745,"Local circuity, FLAT - MULTILEVEL",1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999]
["NS-E2L112C8","NS",2,"E2L112C8",748,"Spotted-to-Pulled Ratio, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L112C11","NS",2,"E2L112C11",751,"CD per Intraterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L112C12","NS",2,"E2L112C12",752,"CD per Interterminal Switch, FLAT - MULTILEVEL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["NS-E2L112C16","NS",2,"E2L112C16",756,"CD per Load & Unload Interterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L112C20","NS",2,"E2L112C20",760,"CM per Interterminal Switch, FLAT - MULTILEVEL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["NS-E2L112C23","NS",2,"E2L112C23",763,"Average Miles between I&I Switches, FLAT - MULTILEVEL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["NS-E2L112C26","NS",2,"E2L112C26",766,"SEMs per Interchange Switch, FLAT - MULTILEVEL",3.8144280910491899,3.89312076568604,4.15873050689697,4.1730580329895002,4.0252881050109899,4.0373163223266602,4.7107481956481898,4.4231705665588397,4.3516521453857404,4.5098960028236101,4.26084850999798,4.1327752402438902,4.3307349404828601,4.2439109775633499,4.30551998464815,3.74821200698785]
["NS-E2L113C1","NS",2,"E2L113C1",770,"Average Tare Weight, FLAT - GENERAL",33.599998474121101,34.099998474121101,34,32.900001525878899,32.200000762939503,33,32.200000762939503,32.799999237060497,32.799999237060497,32.5,32.4,32.200000000000003,32.1,32.200000000000003,32.299999999999997,32.299999999999997]
["NS-E2L113C4","NS",2,"E2L113C4",773,"E/L Ratio, All Freight Cars, FLAT - GENERAL",3.1571125984191899,2.7632849216461199,2.6537215709686302,2.7530863285064702,4.6199998855590803,4.5,3.86335396766663,2.6649215221404998,2.3108973503112802,2.1559633027522902,2.1857506361323198,2.0895196506550202,2.1033868092691601,2.06201550387597,2.06486486486487,2.1231671554252198]
["NS-E2L113C8","NS",2,"E2L113C8",777,"Spotted-to-Pulled Ratio, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L113C9","NS",2,"E2L113C9",778,"CD per Industry Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["NS-E2L113C12","NS",2,"E2L113C12",781,"CD per Interterminal Switch, FLAT - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["NS-E2L113C16","NS",2,"E2L113C16",785,"CD per Load & Unload Interterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L113C19","NS",2,"E2L113C19",788,"CM per Intraterminal Switch, FLAT - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["NS-E2L113C22","NS",2,"E2L113C22",791,"Average CM per CD, Railroad-Owned, FLAT - GENERAL",562.25250244140602,565.11291503906295,562.059326171875,580.63201904296898,533.62518310546898,541.47668457031295,577.70440673828102,578.30377197265602,541.52423095703102,548.24383515701595,555.61441377984499,534.45321252759697,516.31512513141104,542.10456880957599,549.60304612458401,523.27424532518501]
["NS-E2L113C26","NS",2,"E2L113C26",795,"SEMs per Interchange Switch, FLAT - GENERAL",3.8144278526306201,3.8931210041046098,4.15873050689697,4.1730575561523402,4.0252881050109899,4.0373167991638201,4.7107481956481898,4.4231705665588397,4.3516526222229004,4.5098960028236101,4.26084850999798,4.1327752402438902,4.3307349404828601,4.2439109775633499,4.30551998464815,3.74821200698785]
["NS-E2L113C29","NS",2,"E2L113C29",798,"SEMs per I&I Switch, FLAT - GENERAL",1.73383092880249,1.7696003913879399,1.89033186435699,1.89684438705444,1.8296765089035001,1.83514392375946,2.1412491798400901,2.0105321407318102,1.9780237674713099,2.0499527285561898,1.9367493227263499,1.87853420011086,1.96851588203767,1.92905044434698,1.95705453847643,1.70373273044902]
["NS-E2L114C4","NS",2,"E2L114C4",802,"E/L Ratio, All Freight Cars, FLAT - OTHER",2.0226387977600102,2.0298047065734899,2.0916671752929701,2.1655538082122798,2.1315050125122101,2.1323535442352299,2.09743309020996,2.1040050983428999,2.08897137641907,2.1629864412748701,2.17845309587906,2.0922863191320502,2.0497675023574899,2.0745908042218502,2.0764963012777402,2.0441988950276202]
["NS-E2L114C5","NS",2,"E2L114C5",803,"Local circuity, FLAT - OTHER",1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001]
["NS-E2L114C8","NS",2,"E2L114C8",806,"Spotted-to-Pulled Ratio, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L114C12","NS",2,"E2L114C12",810,"CD per Interterminal Switch, FLAT - OTHER",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["NS-E2L114C15","NS",2,"E2L114C15",813,"CD per Load & Unload Intraterminal Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L114C18","NS",2,"E2L114C18",816,"CM per Interchange Switch, FLAT - OTHER",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["NS-E2L114C22","NS",2,"E2L114C22",820,"Average CM per CD, Railroad-Owned, FLAT - OTHER",562.25250244140602,565.11291503906295,562.059326171875,580.63201904296898,533.62518310546898,541.47662353515602,577.70446777343795,578.30383300781295,541.52423095703102,548.24383515701595,555.61441377984499,534.453212527598,516.31512513141104,542.10456880957599,549.60304612458401,523.27424532518501]
["NS-E2L114C25","NS",2,"E2L114C25",823,"SEMs per Industry Switch, FLAT - OTHER",6.9353232383728001,7.0784025192260698,7.5613279342651403,7.5873780250549299,7.3187050819396999,7.34057569503784,8.5649967193603498,8.0421276092529297,7.9120960235595703,8.1998109142247397,7.7469972909054103,7.5141368004434304,7.8740635281506597,7.7162017773879201,7.8282181539057296,6.8149309217960896]
["NS-E2L114C29","NS",2,"E2L114C29",827,"SEMs per I&I Switch, FLAT - OTHER",1.7338308095932,1.7696003913879399,1.89033174514771,1.89684438705444,1.8296765089035001,1.83514380455017,2.1412489414215101,2.0105321407318102,1.9780240058898899,2.0499527285561898,1.9367493227263499,1.87853420011086,1.96851588203767,1.92905044434698,1.95705453847643,1.70373273044902]
["NS-E2L115C1","NS",2,"E2L115C1",828,"Average Tare Weight, TANK <22,000 GAL",32.700000000000003,32.700000000000003,32.6,32.6,32.6,32.6,32.6,32.6,32.6,32.700000000000003,32.700000000000003,32.799999999999997,32.799999999999997,32.9,32.9,32.9]
["NS-E2L115C4","NS",2,"E2L115C4",831,"E/L Ratio, All Freight Cars, TANK <22,000 GAL",2.0355470180511501,2.0324151515960698,2.06805491447449,2.08592748641968,2.0456373691558798,2.0466837882995601,2.03549456596375,2.0465850830078098,2.03995680809021,2.0452254164376802,2.0434375435869798,2.02950813101811,2.0341726618705001,2.0675856381911801,2.09630695080561,2.0717086900710102]
["NS-E2L115C8","NS",2,"E2L115C8",835,"Spotted-to-Pulled Ratio, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L115C11","NS",2,"E2L115C11",838,"CD per Intraterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L115C15","NS",2,"E2L115C15",842,"CD per Load & Unload Intraterminal Switch, TANK <22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L115C18","NS",2,"E2L115C18",845,"CM per Interchange Switch, TANK <22,000 GAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["NS-E2L115C21","NS",2,"E2L115C21",848,"CM per I&I Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["NS-E2L115C25","NS",2,"E2L115C25",852,"SEMs per Industry Switch, TANK <22,000 GAL",6.9353227615356401,7.0784020423889196,7.5613274574279803,7.5873780250549299,7.3187055587768599,7.340576171875,8.5649967193603498,8.0421285629272496,7.9120960235595703,8.1998109142247397,7.7469972909054103,7.5141368004434304,7.8740635281506597,7.7162017773879201,7.8282181539057296,6.8149309217960896]
["NS-E2L115C26","NS",2,"E2L115C26",853,"SEMs per Interchange Switch, TANK <22,000 GAL",3.8144276142120401,3.8931210041046098,4.15873050689697,4.1730575561523402,4.0252885818481401,4.0373163223266602,4.7107481956481898,4.4231705665588397,4.3516530990600604,4.5098960028236101,4.2608485099979703,4.1327752402438902,4.3307349404828601,4.2439109775633499,4.30551998464815,3.74821200698785]
["NS-E2L115C29","NS",2,"E2L115C29",856,"SEMs per I&I Switch, TANK <22,000 GAL",1.73383104801178,1.7696005105972299,1.89033162593842,1.89684438705444,1.8296765089035001,1.83514380455017,2.1412494182586701,2.0105321407318102,1.9780240058898899,2.0499527285561898,1.9367493227263499,1.87853420011086,1.96851588203767,1.92905044434698,1.95705453847643,1.70373273044902]
["NS-E2L116C4","NS",2,"E2L116C4",860,"E/L Ratio, All Freight Cars, TANK >=22,000 GAL",2.0420544147491499,2.0434093475341801,2.0419347286224401,2.0713336467742902,2.03969526290894,2.0491907596588099,2.022127866745,2.0348548889160201,2.0232064723968501,2.03372755554315,2.0560990774024299,2.0582640851399101,2.0435216235935099,2.0452972436366901,2.0431514025082498,2.02726370717324]
["NS-E2L116C7","NS",2,"E2L116C7",863,"Average circuity, TANK >=22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["NS-E2L116C11","NS",2,"E2L116C11",867,"CD per Intraterminal Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L116C14","NS",2,"E2L116C14",870,"CD per Load & Unload Industry Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L116C17","NS",2,"E2L116C17",873,"CM per Industry Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L116C19","NS",2,"E2L116C19",875,"CM per Intraterminal Switch, TANK >=22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["NS-E2L116C22","NS",2,"E2L116C22",878,"Average CM per CD, Railroad-Owned, TANK >=22,000 GAL",562.25256347656295,565.11297607421898,562.059326171875,580.63201904296898,533.62518310546898,541.47662353515602,577.70446777343795,578.30383300781295,541.52429199218795,548.24383515701595,555.61441377984499,534.45321252759697,516.31512513141104,542.10456880957599,549.60304612458401,523.27424532518501]
["NS-E2L116C26","NS",2,"E2L116C26",882,"SEMs per Interchange Switch, TANK >=22,000 GAL",3.8144276142120401,3.8931210041046098,4.15873050689697,4.1730575561523402,4.0252885818481401,4.0373163223266602,4.7107481956481898,4.4231705665588397,4.3516530990600604,4.5098960028236101,4.2608485099979703,4.1327752402438902,4.3307349404828601,4.2439109775633499,4.30551998464815,3.74821200698785]
["NS-E2L116C29","NS",2,"E2L116C29",885,"SEMs per I&I Switch, TANK >=22,000 GAL",1.73383104801178,1.7696005105972299,1.89033162593842,1.89684438705444,1.8296765089035001,1.83514380455017,2.1412494182586701,2.0105321407318102,1.9780240058898899,2.0499527285561898,1.9367493227263499,1.87853420011086,1.96851588203767,1.92905044434698,1.95705453847643,1.70373273044902]
["NS-E2L117C3","NS",2,"E2L117C3",888,"E/L Ratio, Privately-Owned, ALL OTHER FREIGHT CARS",2.0593900680542001,2.01417183876038,2.06801462173462,2.2151544094085698,2.07774806022644,2.0577595233917201,2.0847043991088898,2.14598536491394,2.2488927841186501,1.82018618324351,2.2343572241183201,2.04412565825313,2.0274814096346598,2.0438470155224802,2.0564102564102602,2.1574657280474301]
["NS-E2L117C7","NS",2,"E2L117C7",892,"Average circuity, ALL OTHER FREIGHT CARS",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["NS-E2L117C10","NS",2,"E2L117C10",895,"CD per Interchange Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["NS-E2L117C13","NS",2,"E2L117C13",898,"CD per I&I Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["NS-E2L117C15","NS",2,"E2L117C15",900,"CD per Load & Unload Intraterminal Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["NS-E2L117C18","NS",2,"E2L117C18",903,"CM per Interchange Switch, ALL OTHER FREIGHT CARS",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["NS-E2L117C22","NS",2,"E2L117C22",907,"Average CM per CD, Railroad-Owned, ALL OTHER FREIGHT CARS",562.25256347656295,565.11297607421898,562.059326171875,580.63201904296898,533.62518310546898,541.47662353515602,577.70446777343795,578.30383300781295,541.52429199218795,548.24383515701595,555.61441377984499,534.45321252759697,516.31512513141104,542.10456880957599,549.60304612458401,523.27424532518501]
["NS-E2L117C25","NS",2,"E2L117C25",910,"SEMs per Industry Switch, ALL OTHER FREIGHT CARS",6.9353227615356401,7.0784020423889196,7.5613274574279803,7.5873780250549299,7.3187055587768599,7.340576171875,8.5649967193603498,8.0421285629272496,7.9120960235595703,8.1998109142247397,7.7469972909054103,7.5141368004434304,7.8740635281506597,7.7162017773879201,7.8282181539057296,6.8149309217960896]
["NS-E2L117C28","NS",2,"E2L117C28",913,"SEMs per Interterminal Switch, ALL OTHER FREIGHT CARS",8.3223896026611293,8.4940834045410192,9.0735940933227504,9.1048536300659197,8.7824468612670898,8.8086910247802699,10.277996063232401,9.6505546569824201,9.4945144653320295,9.8397730970696902,9.2963967490864903,9.0169641605321207,9.4488762337807906,9.2594421328654999,9.3938617846868695,8.1779171061553004]
["NS-E2L118C3","NS",2,"E2L118C3",917,"E/L Ratio, Privately-Owned, AVERAGE ALL FREIGHT CARS",1.7276903390884399,1.7634458541870099,1.7632807493209799,1.7586907148361199,1.73840856552124,1.7223470211029099,1.7116957902908301,1.7141200304031401,1.704185962677,1.72051693143111,1.7212019473503199,1.7083204583817599,1.6879649220116399,1.7108621619700799,1.69457735952522,1.68075796175909]
["NS-E2L118C6","NS",2,"E2L118C6",920,"Interline circuity, AVERAGE ALL FREIGHT CARS",1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.157,1.157,1.157,1.157,1.157,1.157,1.157]
["NS-E2L118C9","NS",2,"E2L118C9",923,"CD per Industry Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["NS-E2L118C11","NS",2,"E2L118C11",925,"CD per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L118C14","NS",2,"E2L118C14",928,"CD per Load & Unload Industry Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["NS-E2L118C18","NS",2,"E2L118C18",932,"CM per Interchange Switch, AVERAGE ALL FREIGHT CAR",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["NS-E2L118C21","NS",2,"E2L118C21",935,"CM per I&I Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["NS-E2L118C24","NS",2,"E2L118C24",938,"Average Miles between Interchange Switches, AVERAGE ALL FREIGHT CARS",1337.87744140625,1262.63427734375,1304.49768066406,1399.58825683594,1387.39526367188,1445.03381347656,1322.88134765625,1286.41589355469,1311.10888671875,1384.2841313228,1352.61407269405,1315.5539579225599,1371.4759838633299,1416.85176553069,1511.7601462166399,1473.36892247265]
["NS-E2L118C28","NS",2,"E2L118C28",942,"SEMs per Interterminal Switch, AVERAGE ALL FREIGHT CARS",8.32238864898682,8.4940824508666992,9.0735940933227504,9.1048536300659197,8.7824468612670898,8.8086910247802699,10.277996063232401,9.6505527496337908,9.4945144653320295,9.8397730970696902,9.2963967490864903,9.0169641605321207,9.4488762337807906,9.2594421328654999,9.3938617846868695,8.1779171061553004]
["NS-E2L201C1","NS",2,"E2L201C1",944,"Average Distance Per Car In Way Trains",26.898715972900401,26.256818771362301,27.162345886230501,27.3393955230713,27.989322662353501,25.854442596435501,25.220607757568398,23.877418518066399,23.889764785766602,22.870086213380901,22.245272835519099,20.509956192294698,19.6936568653847,17.066919864256899,14.6504356188471,17.4535227242717]
[{"$f":"B6786&\"-\"&D6786","v":"NS-E2L204C1"},"NS",2,"E2L204C1",947,"Average Tare Weight - Non-Refrigerated TCU",5,5,5,4.9000000953674299,4.9000000953674299,4.9000000953674299,4.9000000953674299,5,5,5,4.9000000000000004,4.7,4.9000000000000004,4.9000000000000004,4.8,4.8]
["NS-E2L207C1","NS",2,"E2L207C1",950,"L/E Ratio - Refrigerated/Non-Refrigerated - TCU",1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33000004291534,1.33,1.33,1.33,1.33,1.33,1.33,1.33]
["NS-E2L210C1","NS",2,"E2L210C1",953,"Average Locomotive Units - Through Train",2.3304095268249498,2.3592896461486799,2.3744933605194101,2.3708844184875502,2.3473465442657502,2.3540298938751198,2.3825821876525901,2.3995895385742201,2.3898172378539999,2.3737404631591801,2.4751714318961602,2.42637956179269,2.2925921977944101,2.3628530205858,2.3542101271424798,2.2967228726342799]
["NS-E2L214C1","NS",2,"E2L214C1",957,"Engine Crews (Excl Train Switching)",308674.53125,293804.4375,332758.28125,231724.578125,286831.875,331393.59375,314595.625,321309.6875,339388.53125,352267.04432664701,329457.016354469,360890.398373759,384918.87678001699,341023.60440660198,272538.60464986501,292650.01588417398]
["NS-E2L217C1","NS",2,"E2L217C1",960,"Train Miles - Running",84159.671875,81855.1015625,79990.8515625,67460.21875,72566.9140625,75689.046875,76271.90625,74795.671875,74822.15625,75604.994999999995,71650.066999999995,72279.497000000003,73177.858999999997,70588.361999999994,58584.639000000003,56243.718000000001]
["NS-E2L220C1","NS",2,"E2L220C1",963,"Constant Cost Markup Ratio",1.3352421522140501,1.3755120038986199,1.3647662401199301,1.42659020423889,1.41025650501251,1.38884472846985,1.3900225162506099,1.39059281349182,1.3886147737503101,1.4049626560003701,1.4219666786074401,1.4221419403529201,1.4145830271507001,1.4161785497223101,1.46352365330551,1.45083622556173]
["NS-E2L302C2","NS",2,"E2L302C2",967,"Residual Factor, Station Clerical, Privately-Owned",1.0555746016370799,1.0694047188073399,1.13684565247989,1.36834889668496,1.30106184691351,1.2644763173846501,1.25146133697623,1.0856203936050797,0.99085944487786204,1.03101969998072,0.71780851946503799,0.70513933386093097,0.73347866316157895,0.70630581971064998,0.53124587232944698,0.50098275359073297]
["NS-E2L303C2","NS",2,"E2L303C2",969,"Residual Factor, Interchange Switching, Privately-Owned",5.1579890676945102,5.1226346451272802,5.8004478258532401,5.9106616780692196,6.1891348272723796,7.2813332401307598,7.9766803818287304,8.3839237736871048,8.4761686879239306,5.8847887887770796,4.42922737309806,5.0981106123860398,5.6451470976759799,5.9452573865694003,4.460859730244958,4.28279666100455]
["NS-E2L305C1","NS",2,"E2L305C1",972,"Residual Factor, Mileage, Railroad-Owned",-2.9280342952605101,-2.7647681379360098,-3.6046657830920199,-1.9569166053983601E-2,-3.17538003639392,-1.4598914775042,8.0100598496825895E-2,2.9068997787650903,0.96523841592217796,4.8201786509874696,3.9201064051852201,1.9900414289233599,-5.8139627772733004E-4,1.6755436005662001,1.7638691339146091,-2.4523914692311202]
["UP-E1L101C2","UP",7,"E1L101C2",2,"Gross Ton Mile (GTM), DRL Expense",6.44498853944242E-4,6.9406413240358201E-4,7.3929940117523096E-4,8.8603468611836401E-4,8.6103600915521405E-4,8.6592289153486501E-4,9.31045855395496E-4,9.6189253963530096E-4,9.4682280905544801E-4,1.0087164255612299E-3,1.0947223384225699E-3,1.0607738834039499E-3,1.0466267127055601E-3,1.1448218817123499E-3,1.2232545422282499E-3,1.15906579639585E-3]
["UP-E1L102C2","UP",7,"E1L102C2",5,"Car Mile (CM) - Other Than Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L103C3","UP",7,"E1L103C3",9,"Train Mile (TM) - Other Than Crew, ROI Expense",2.3346820380538702E-3,2.4782735854387301E-3,2.4163716007024102E-3,2.1290676668286302E-3,1.84652651660144E-3,1.55451835598797E-3,1.16452225483954E-3,1.4773357543162999E-4,3.2533987541683002E-4,4.4491921084775798E-4,2.7339247109376399E-3,3.2048050452849E-4,2.4600776063505398E-4,1.03562027809076E-4,-4.3318630992484204E-6,-1.9360858989580999E-4]
["UP-E1L104C3","UP",7,"E1L104C3",12,"Train Mile (TM) - Crew, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L105C3","UP",7,"E1L105C3",15,"Locomotive Unit Mile (LUM), ROI Expense",0.31147900223732,0.347525775432587,0.39037278294563299,0.51634943485259999,0.48714014887809798,0.505273938179016,0.55740201473236095,0.56746125221252397,0.59401309490203902,0.66113191577893504,0.65967516335683896,0.75250265098756097,0.85606838130496299,0.78139760937895797,0.76598250539664503,0.91451222299394397]
["UP-E1L107C1","UP",7,"E1L107C1",19,"CLOR (Carloads Handled) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L107C3","UP",7,"E1L107C3",21,"CLOR (Carloads Handled) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L108C3","UP",7,"E1L108C3",24,"CLOT (Carloads Orig Or Term) - Other, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L109C3","UP",7,"E1L109C3",27,"CLOT (Carloads Orig Or Term) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L110C3","UP",7,"E1L110C3",30,"Car Mile (CM) - Clerical, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L112C1","UP",7,"E1L112C1",34,"Ton Miles In Lake Transfer Service, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L113C1","UP",7,"E1L113C1",37,"Tons Handled at Coal Terminals, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L114C2","UP",7,"E1L114C2",41,"Tons Handled at Ore Terminals, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L115C2","UP",7,"E1L115C2",44,"Tons Handled at Other Marine Terminals, DRL Expense",0,0,0,0,0,0,0,4.8435111530125098E-3,4.5210421085357701E-3,5.6262864499715499E-3,8.6410951414681407E-3,1.03693773816785E-2,1.03824513745354E-2,9.8157787177833907E-3,1.25820379226177E-2,1.5428961848300201E-2]
["UP-E1L116C1","UP",7,"E1L116C1",46,"Refrigerated Car Miles, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L117C1","UP",7,"E1L117C1",49,"Protective Service Reefer TCU Days, OPR Expense",0,0,0,0,1.3620258569717401,1.52048444747925,1.7379560470581099,1.9058136940002399,1.8541504144668599,1.05031834518884,0.898752001368469,0.72452288822425803,0.35204518138576602,0.20596905143543801,6.9349800127370496E-3,-6.8041289682117898E-3]
["UP-E1L118C1","UP",7,"E1L118C1",52,"Refrigerated TCU Days, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L119C1","UP",7,"E1L119C1",55,"Other (Non-Refrigerated) TCU Days, OPR Expense",2.5991015434265101,2.0533220767974898,2.54784083366394,2.6058645248413099,1.8152859210968,1.14864385128021,0,0,0,0,0,0,0,0,0,0]
["UP-E1L120C2","UP",7,"E1L120C2",59,"TCUs Loaded And Unloaded (L&UL), DRL Expense",1.37043428421021,1.4831014871597299,1.70604801177979,2.0893645286560099,1.86820733547211,2.1534759998321502,2.1680390834808398,2.2310562133789098,2.0929436683654798,2.1361396024127899,2.4679774264116099,2.57180914456807,2.6343170840494299,2.9172836317309101,3.1188254020959598,2.8082958229514201]
["UP-E1L121C2","UP",7,"E1L121C2",62,"MVUs Loaded And Unloaded (L&UL), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L122C3","UP",7,"E1L122C3",66,"TCUs Picked Up and Delivered (PU&D), ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L201C1","UP",7,"E1L201C1",67,"CM(R), OPR Expense, Railroad-Owned, BOX - 40 FT",1.2384160421788699E-2,1.0943965986371E-2,1.72191765159369E-2,1.7504068091511699E-2,1.31017491221428E-2,9.5544848591089205E-4,1.2970975367352399E-3,1.1308222310617601E-3,3.2342397607862902E-3,6.38511789454337E-3,1.9192261714590798E-2,3.2950088900967102E-2,4.1054074066493897E-2,4.0675377545166598E-2,3.5202583543772897E-2,2.5303562288748301E-2]
["UP-E1L201C7","UP",7,"E1L201C7",73,"CD(R), OPR Expense, Railroad-Owned, BOX - 40 FT",1.7322018146514899,1.5763347148895299,2.5285415649414098,2.63787817955017,1.98377692699432,0.145493254065514,0.198145061731339,0.17290334403514901,0.491123527288437,0.95912294393187902,2.9001045052427599,4.97100084769402,6.1657171946107301,5.9546050803755897,5.16419131515282,3.6758064942131101]
["UP-E1L201C8","UP",7,"E1L201C8",74,"CD(R), DRL Expense, Railroad-Owned, BOX - 40 FT",46.157115936279297,41.806156158447301,44.889427185058601,42.904502868652301,40.8184623718262,42.464080810546903,42.059028625488303,29.165683746337901,28.9990425109863,31.049802224200999,27.3955681201396,25.341783102655501,23.732314962179299,23.928769864880699,23.696331639730701,23.200113262705301]
["UP-E1L201C11","UP",7,"E1L201C11",77,"CD(Y), DRL Expense, Railroad-Owned, BOX - 40 FT",46.1571235656738,41.806156158447301,44.889430999755902,42.904502868652301,40.8184623718262,42.464080810546903,42.059028625488303,29.1656818389893,28.999036788940401,31.049802224200999,27.3955681201396,25.341783102655501,23.732314962179299,23.928769864880699,23.696331639730701,23.200113262705301]
["UP-E1L202C2","UP",7,"E1L202C2",81,"CM(R), DRL Expense, Railroad-Owned, BOX - 50 FT",0.156650990247726,0.147349253296852,0.16843438148498499,0.160150587558746,0.14517450332641599,0.140864372253418,0.138121977448463,9.1636538505554199E-2,8.1383362412452698E-2,6.3888803221821694E-2,5.4819768242523097E-2,4.53852000861137E-2,4.3802866557380603E-2,5.3830961052467E-2,5.2510228074334503E-2,4.6439962834855499E-2]
["UP-E1L202C5","UP",7,"E1L202C5",84,"CM(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",0.40729278326034501,0.383107930421829,0.43792924284934998,0.416391551494598,0.37745413184165999,0.36624684929847701,0.359117090702057,0.238254889845848,0.21159666776657099,0.16611088837673699,0.14253139743055901,0.118001520223896,0.11388745304919,0.139960498736414,0.13652659299327,0.120743903370624]
["UP-E1L202C8","UP",7,"E1L202C8",87,"CD(R), DRL Expense, Railroad-Owned, BOX - 50 FT",46.157115936279297,41.806156158447301,44.889427185058601,42.904502868652301,40.8184623718262,42.464080810546903,42.059028625488303,29.165683746337901,28.9990425109863,31.049802224200999,27.3955681201396,25.341783102655501,23.732314962179299,23.928769864880699,23.696331639730701,23.200113262705301]
["UP-E1L202C12","UP",7,"E1L202C12",91,"CD(Y), ROI Expense, Railroad-Owned, BOX - 50 FT",13.6830024719238,14.2155981063843,15.5752725601196,13.5880641937256,12.009860038757299,12.3803653717041,13.096941947936999,13.790132522583001,10.662045478820801,7.9035923770298799,6.3626300962781599,7.3498118568379001,7.9997057268106602,6.6534386908423304,5.6811921477282796,5.9409922581301702]
["UP-E1L202C13","UP",7,"E1L202C13",92,"CM(R), DRL Expense, Privately-Owned, BOX - 50 FT",0.212218478322029,0.233134791254997,0.229180157184601,0.23359155654907199,0.17389422655105599,0.20231449604034399,0.202124163508415,0.187271818518639,0.190546944737434,0.190538198173554,0.235520531368279,0.230580362763147,0.218857960025853,0.239773839740824,0.213537268594335,0.183831273218233]
["UP-E1L203C6","UP",7,"E1L203C6",98,"CM(Y), ROI Expense, Railroad-Owned, BOX - EQUIPPED",1.90914012491703E-2,2.0476624369621301E-2,2.0063685253262499E-2,1.9844034686684602E-2,1.8449196591973301E-2,1.5508774667978301E-2,1.3208080083131801E-2,1.44876344129443E-2,1.3422211632132501E-2,1.15503716883476E-2,9.9196429458791799E-3,1.23609058634722E-2,1.51618509937528E-2,1.19070147810128E-2,1.0102442986634701E-2,1.2971266476749999E-2]
["UP-E1L203C7","UP",7,"E1L203C7",99,"CD(R), OPR Expense, Railroad-Owned, BOX - EQUIPPED",4.3373265266418501,4.3849930763244602,5.5800108909606898,6.6174964904785201,5.5206875801086399,4.2557272911071804,4.6530122756957999,5.0850071907043501,5.2774233818054199,5.5096715923681501,5.9291979787819402,7.2775199793983996,8.4364056519589994,9.0101072871950105,8.4625338788907207,6.4236058786771197]
[{"$f":"B6914&\"-\"&D6914","v":"UP-E1L203C10"},"UP",7,"E1L203C10",102,"CD(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED",4.3373265266418501,4.3849930763244602,5.5800108909606898,6.6174964904785201,5.5206875801086399,4.2557272911071804,4.6530122756957999,5.0850071907043501,5.2774229049682599,5.5096715923681501,5.92919797878195,7.2775199793984102,8.4364056519589994,9.0101072871950105,8.4625338788907207,6.4236058786771197]
["UP-E1L204C1","UP",7,"E1L204C1",106,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",2.3277448490262E-2,2.4263184517622001E-2,2.39626746624708E-2,2.5139980018138899E-2,2.6006223633885401E-2,2.67166737467051E-2,3.0917726457118998E-2,2.70775575190783E-2,3.1060865148901901E-2,3.5512171758095699E-2,3.8044851481707297E-2,3.7817016867601701E-2,3.4766909669599499E-2,3.3603797857587103E-2,3.2933093766071203E-2,2.80485168922361E-2]
["UP-E1L204C4","UP",7,"E1L204C4",109,"CM(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",6.0521300882101101E-2,6.3084259629249601E-2,6.2302965670824099E-2,6.5364055335521698E-2,6.7616194486618E-2,6.9463193416595501E-2,8.0386042594909696E-2,7.0401668548583998E-2,8.0758295953273801E-2,9.2331646571049003E-2,9.8916613852438898E-2,9.8324243855764701E-2,9.0393965140958404E-2,8.7369874429726505E-2,8.56260437917854E-2,7.2926143919813904E-2]
["UP-E1L204C7","UP",7,"E1L204C7",112,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",2.7099125385284402,2.89102363586426,2.8793644905090301,3.07277512550354,3.1828880310058598,3.2591648101806601,3.7156403064727801,3.2045328617095898,3.5451314449310298,3.9471320632202298,4.0476151523432202,4.0748293181031503,3.73994698569707,3.5976309109603299,3.3404556503228502,2.6205352855503401]
["UP-E1L204C11","UP",7,"E1L204C11",116,"CD(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",7.6002078056335396,6.2854561805725098,6.5019216537475604,7.5315804481506303,7.3450183868408203,7.3565912246704102,8.8550872802734393,9.1306562423706108,7.2992448806762704,8.4308844925000894,7.7941777454967598,8.1653080961121791,8.5453188706718493,9.8290950921877709,10.601211220829001,8.6013636841718402]
["UP-E1L204C12","UP",7,"E1L204C12",117,"CD(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",1.3824479579925499,1.06940233707428,0.94545418024063099,0.83920758962631203,0.83997935056686401,1.4815751314163199,2.0492918491363499,2.1297807693481401,2.5718371868133501,2.8326065077107998,2.9763504519911699,2.9887807328954499,4.5013019874855598,4.33005045333379,4.1728823810337703,4.61872676985372]
["UP-E1L205C5","UP",7,"E1L205C5",123,"CM(Y), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",0.10575365275144601,0.108635254204273,0.134456902742386,0.152602419257164,0.12816643714904799,0.114268578588963,0.125282302498817,0.12764233350753801,0.111880645155907,0.13365726698550101,0.125013224407892,0.117509257076492,0.119939131995363,0.12913525487907301,0.144057385532781,0.106929022252362]
["UP-E1L205C6","UP",7,"E1L205C6",124,"CM(Y), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",2.3749480023980099E-2,2.6502449065446899E-2,2.5502501055598301E-2,3.8805358111858403E-2,2.78476607054472E-2,2.5347627699375201E-2,2.98858005553484E-2,3.9644114673137699E-2,3.3317755907773999E-2,3.6446015605471602E-2,3.02730468090683E-2,3.08718786628631E-2,3.4075614534090901E-2,2.40568870409874E-2,2.16936915029626E-2,4.4314798402248799E-2]
["UP-E1L205C9","UP",7,"E1L205C9",127,"CD(R), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED",1.2568676471710201,1.52174949645996,1.41531598567963,2.3559660911560099,1.72015285491943,1.5977908372878999,2.0449459552764901,2.7433769702911399,2.2431273460388201,2.47633897715024,2.0711173033908601,2.1427544363514701,2.3353234651416299,1.66663306972033,1.56602425435285,3.0548629433343999]
["UP-E1L205C13","UP",7,"E1L205C13",131,"CM(R), DRL Expense, Privately-Owned, GONDOLA - EQUIPPED",3.9000868127914098E-5,5.98869373789057E-5,2.15441705222474E-5,3.4044427593471503E-5,0,1.9341140985488899E-2,1.0583487892290599E-5,2.29811084864195E-5,1.24448060887516E-5,3.0376113618873601E-2,2.01543513424523E-2,1.23657013363603E-2,3.7489955819157098E-3,4.4740396217598502E-4,1.3307655451925699E-3,4.8533010004884898E-5]
["UP-E1L206C3","UP",7,"E1L206C3",134,"CM(R), ROI Expense, Railroad-Owned, HOPPER - COVERED",1.1693967506289499E-2,1.3790857046842599E-2,1.57790537923574E-2,1.61567032337189E-2,1.6587074846029299E-2,1.8610823899507498E-2,2.2790171205997498E-2,2.48733256012201E-2,1.98725331574678E-2,2.0068540624218999E-2,1.8712911930857199E-2,2.41446552511007E-2,3.1249971973700299E-2,2.51911416009836E-2,1.8359221084492301E-2,2.28019686986103E-2]
["UP-E1L206C6","UP",7,"E1L206C6",137,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED",3.04043386131525E-2,3.5856258124113097E-2,4.1025545448064797E-2,4.2007435113191598E-2,4.31263744831085E-2,4.8388104885816602E-2,5.9254352003336001E-2,6.4670719206333202E-2,5.16685396432877E-2,5.2178205622969598E-2,4.8653571020228603E-2,6.2776103652861903E-2,8.1249927131620603E-2,6.5496968162557498E-2,4.7733974819680003E-2,5.9285118616387203E-2]
["UP-E1L206C10","UP",7,"E1L206C10",141,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",5.9545249938964799,6.7873120307922399,7.1270709037780797,8.6698570251464808,8.0502185821533203,8.5659770965576207,9.3085651397705096,8.9690999984741193,8.3815507888793892,7.9526551718092398,7.2299893482695596,6.8978761116320904,6.2280079832834003,5.8159400154521999,5.2487583410434899,4.5813526772493898]
["UP-E1L206C11","UP",7,"E1L206C11",142,"CD(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED",15.9693241119385,17.0752277374268,18.51003074646,21.551189422607401,17.757369995117202,17.410535812377901,20.9049892425537,17.388523101806602,13.5935573577881,14.5149068411397,13.142881585315701,13.4435477175873,11.889860023510099,9.9097683672684003,8.8201054612992493,6.7888297148894097]
["UP-E1L207C2","UP",7,"E1L207C2",146,"CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",4.9044606275856504E-3,4.4445991516113299E-3,4.9148863181471799E-3,1.1208305135369301E-2,6.4054173417389402E-3,5.2024801261722998E-3,4.33950684964657E-3,-9.7835878841579004E-4,-6.9706491194665399E-4,1.5774032023233499E-3,7.02087155637998E-3,3.8693106203767898E-3,7.5967416275531894E-5,1.2208348166620499E-2,1.2580805641651E-2,1.3509093119978E-2]
["UP-E1L207C5","UP",7,"E1L207C5",149,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.2751570902764801E-2,1.15559594705701E-2,1.2778709642589099E-2,2.9141582548618299E-2,1.6654072329402001E-2,1.35264592245221E-2,1.12827206030488E-2,-2.54373578354716E-3,-1.8123661866411599E-3,4.1012483260406997E-3,1.8254266046587898E-2,1.00602076129797E-2,1.97515282316347E-4,3.1741705233213298E-2,3.2710094668292597E-2,3.5123642111942903E-2]
["UP-E1L207C8","UP",7,"E1L207C8",152,"CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.9642896652221702,2.5079436302185099,2.2343199253082302,5.2244911193847701,3.9193012714386,3.3109552860260001,2.7000868320465101,2.0237720012664799,2.00649785995483,1.9164416625023699,1.9971047007793601,1.37280763787255,0.59081020114579796,2.38169974113144,2.20932747058905,0.68818101713063795]
["UP-E1L207C12","UP",7,"E1L207C12",156,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.53684782981873,1.73386967182159,1.52394139766693,2.3999190330505402,1.9600111246109,1.30747735500336,0.88841801881790206,1.1564983129501301,1.17829036712646,1.9449558304839001,2.0181796530462801,2.0871338204828098,2.4771232345012599,2.25830904765143,2.2057367233212801,2.9637842294630499]
["UP-E1L208C2","UP",7,"E1L208C2",159,"CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",5.90624893084168E-3,5.0225700251758099E-3,4.6621230430901103E-3,2.12017726153135E-3,2.00459966436028E-3,1.2221916113048801E-3,1.7884089611470699E-3,1.3417316367849699E-3,1.27346208319068E-3,1.54990238575178E-3,1.02025415608472E-3,1.41200319367247E-3,6.4308152267538398E-4,1.5241981056178301E-3,5.0217155838637199E-3,3.7091438319457899E-3]
["UP-E1L208C5","UP",7,"E1L208C5",162,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.53562361374497E-2,1.30586856976151E-2,1.21215283870697E-2,5.5124629288911802E-3,5.2119600586593203E-3,3.1776956748217301E-3,4.64986776933074E-3,3.4884978085756302E-3,3.3110047224909102E-3,4.02974620295462E-3,2.6526608058202701E-3,3.6712083035484299E-3,1.6720119589559901E-3,3.9629150746063602E-3,1.3056460518045701E-2,9.6437739630590592E-3]
["UP-E1L208C10","UP",7,"E1L208C10",167,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.7032206058502202,3.5511825084686302,3.64688372612,3.54871726036072,2.0468232631683398,0.97161346673965499,1.1788688898086499,1.4186147451400799,2.2194173336029102,2.6507589250460701,2.7816093576368401,2.42743045416033,2.3853668055706199,2.27804658126633,2.5419070504757801,2.28227307944627]
["UP-E1L208C13","UP",7,"E1L208C13",170,"CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - SPECIAL",2.3465699996450002E-6,5.5661694204900397E-6,4.9080636017606602E-6,7.9880774137564003E-6,2.8451197522372202E-6,6.4407847821712505E-4,7.0607209636364105E-5,1.842957090048E-6,8.1460241926833998E-4,5.7882804829342501E-4,3.9152668947337397E-6,1.8120022004226901E-6,1.9008679556000599E-6,6.1782877190938502E-6,9.9605842709842395E-6,5.3202893594181596E-6]
["UP-E1L209C1","UP",7,"E1L209C1",171,"CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",0.140214458107948,7.3323637247085599E-2,2.8051709756255198E-2,3.8034632802009603E-2,6.3274249434471103E-2,8.8011309504509E-2,8.0504775047302204E-2,9.1180257499218001E-2,0.13204020261764499,0.18851261584525,0.189583780331635,0.163053217550299,0.143033769924441,0.160571457302778,0.17840835854645101,0.128232487696361]
["UP-E1L209C4","UP",7,"E1L209C4",174,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",0.36455789208412198,0.19064146280288699,7.2934336960315704E-2,9.8890051245689406E-2,0.16451333463192,0.228829696774483,0.20931296050548601,0.23706856369972201,0.343304753303528,0.49013280119765101,0.49291782886225399,0.42393836563077802,0.37188780180354503,0.41748578898722,0.46386173222077098,0.33340446801053802]
["UP-E1L209C7","UP",7,"E1L209C7",177,"CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",22.875715255737301,12.0216817855835,4.5411286354064897,6.2457466125488299,10.524885177612299,14.8097143173218,13.557558059692401,15.319200515747101,22.193473815918001,31.598356142387701,31.733481837492199,27.2762747303682,23.827695880228902,26.5787749457469,29.4696174734311,20.867825320104298]
["UP-E1L209C11","UP",7,"E1L209C11",181,"CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",10.8364515304565,12.233996391296399,11.6847839355469,16.893459320068398,13.780325889587401,13.5613956451416,15.7545309066772,18.077966690063501,13.3088331222534,14.5243580557933,19.452842763576498,18.326121940817,16.689609208296801,17.577300145500701,26.8425093746099,18.982155807986398]
["UP-E1L210C1","UP",7,"E1L210C1",184,"CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",1.1562411673366999E-2,1.2370322830975101E-2,1.4638265594839999E-2,3.0331894755363499E-2,5.0992917269468301E-2,7.59871080517769E-2,7.3882453143596594E-2,7.8142240643501296E-2,9.2840194702148396E-2,0.112224116363006,9.6941409932954095E-2,8.7388384496353499E-2,8.6091715542995897E-2,9.5791658659943907E-2,8.2323548523145093E-2,7.16004441336031E-2]
["UP-E1L210C4","UP",7,"E1L210C4",187,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",3.0062267556786499E-2,3.2162819057702997E-2,3.80594693124294E-2,7.8863091766834301E-2,0.132581457495689,0.19756641983985901,0.19209413230419201,0.20316970348358199,0.24138395488262199,0.291782702543816,0.25204766582568,0.22720979969051899,0.22383846041178901,0.249058312515855,0.21404122616017801,0.186161154747369]
["UP-E1L210C9","UP",7,"E1L210C9",192,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",4.82247066497803,6.4110217094421396,6.2439951896667498,6.4969577789306596,6.8293962478637704,6.6139574050903303,6.4048275947570801,2.8967387676239,2.0463423728942902,0.97846282862460499,0.70767436809736495,1.0242273512467699,1.4155468080012099,1.29212908671379,2.33289215109843,3.9131329307926901]
["UP-E1L210C12","UP",7,"E1L210C12",195,"CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH",4.82247114181519,6.4110221862793004,6.2439951896667498,6.4969577789306596,6.8293967247009304,6.6139574050903303,6.4048271179199201,2.89673852920532,2.0463423728942902,0.97846282862460499,0.70767436809736495,1.0242273512467699,1.4155468080012099,1.29212908671379,2.33289215109843,3.9131329307926901]
["UP-E1L210C13","UP",7,"E1L210C13",196,"CM(R), DRL Expense, Privately-Owned, REFRIGERATED - NON-MECH",4.1941492818295999E-3,1.5235770260915199E-3,1.9599697552621399E-3,2.45218770578504E-3,5.13438647612929E-3,5.8047985658049601E-3,7.4246870353817896E-3,7.7305953018367299E-3,2.8920527547597898E-3,2.40920321612306E-4,4.5024843412803202E-4,2.8814301511837799E-4,4.2206856909553301E-4,2.7405929836366998E-4,2.6121506914516998E-4,1.4992614048417601E-4]
["UP-E1L211C3","UP",7,"E1L211C3",199,"CM(R), ROI Expense, Railroad-Owned, FLAT - TOFC",2.2240016551222701E-4,2.0813944865949501E-4,1.55683330376633E-4,1.2528109073173301E-4,7.3843228165060295E-5,5.2891056839143898E-5,2.5504234145046202E-5,2.2816275304649001E-5,-9.1091220610906E-7,-2.89605843194427E-6,-3.7352740207141202E-6,-7.58716837792213E-6,-3.2243185047741102E-6,-2.5429634047875499E-8,2.2829707652807399E-6,7.3630579794647001E-6]
["UP-E1L211C6","UP",7,"E1L211C6",202,"CM(Y), ROI Expense, Railroad-Owned, FLAT - TOFC",5.7824002578854604E-4,5.4116267710924105E-4,4.0477589936926999E-4,3.2572998316027202E-4,1.91991595784202E-4,1.37517359689809E-4,6.6311011323705302E-5,5.9322373999748399E-5,-2.36837672673573E-6,-7.5297519230550704E-6,-9.7117124538567297E-6,-1.9726637782597599E-5,-8.3832281124126693E-6,-6.6117048524476803E-8,5.9357239897299098E-6,1.9143950746608299E-5]
["UP-E1L211C10","UP",7,"E1L211C10",206,"CD(Y), OPR Expense, Railroad-Owned, FLAT - TOFC",1.6339430585503599E-2,1.82498283684254E-2,1.3762948103249101E-2,0.114187695086002,0.16512048244476299,0.24215461313724501,0.13283519446849801,8.3096429705619798E-2,4.6298592351377002E-3,4.1727138377090902E-3,1.6672391409977699E-4,3.2739728871995202E-4,3.3191884684747903E-4,3.5081685954437702E-4,2.11373111398618E-4,2.59591670048147E-4]
["UP-E1L211C13","UP",7,"E1L211C13",209,"CM(R), DRL Expense, Privately-Owned, FLAT - TOFC",0.295021802186966,0.33488842844963101,0.32586628198623702,0.30542838573455799,0.32935786247253401,0.30214172601699801,0.29903179407119801,0.15242658555507699,0.153845429420471,0.16976517932875601,0.172897792251931,0.18079827836128601,0.184209198969389,0.179219533033631,0.16662838184547199,0.159295337090057]
["UP-E1L212C4","UP",7,"E1L212C4",213,"CM(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",5.2262567915022399E-3,0,0,3.9600502699613599E-2,6.8111404776573195E-2,0.106853023171425,0.10349879413843199,8.57430770993233E-2,6.5147124230861705E-2,4.3560546684316498E-2,3.5366476713694098E-2,3.26555504203438E-2,2.2688015933434998E-2,1.6249176357185199E-2,1.5072638940964E-2,1.38677697180859E-2]
["UP-E1L212C8","UP",7,"E1L212C8",217,"CD(R), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",7.9394435882568404,3.6536157131195099,3.93187379837036,13.895545959472701,3.8924753665924099,2.48433637619019,3.6857278347015399,3.66235446929932,11.1495161056519,17.0849874298837,23.852473742766499,26.794455302657902,34.351049423210497,31.9804909980726,38.082057032447999,35.325344015084298]
["UP-E1L212C11","UP",7,"E1L212C11",220,"CD(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL",7.9394435882568404,3.6536159515380899,3.93187379837036,13.895545959472701,3.8924751281738299,2.4843370914459202,3.6857278347015399,3.6623549461364702,11.1495170593262,17.0849874298837,23.852473742766499,26.794455302657902,34.351049423210497,31.9804909980726,38.082057032447999,35.325344015084298]
["UP-E1L212C12","UP",7,"E1L212C12",221,"CD(Y), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",3.6202867031097399,5.1140766143798801,6.7723932266235396,8.2847108840942401,5.92460012435913,5.9584879875183097,5.2185339927673304,6.7556819915771502,6.4338483810424796,6.0939145460475803,6.1002467009846102,6.43166389524999,7.3969612547333803,6.4913768067011901,5.9702333850843301,7.5007581427593797]
["UP-E1L213C2","UP",7,"E1L213C2",224,"CM(R), DRL Expense, Railroad-Owned, FLAT - GENERAL",0.13958030939102201,0.13687463104724901,0.14364522695541401,0.150820627808571,0.32846292853355402,0.27860310673713701,0.33161342144012501,-0.127739667892456,-0.14542064070701599,-1.45870064224506E-2,-0.27683958281374998,5.5759088406639103E-2,5.38929606961508E-2,6.22514084198275E-2,6.52905517025196E-2,6.8808552434238293E-2]
["UP-E1L213C5","UP",7,"E1L213C5",227,"CM(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",0.36290901899337802,0.355873733758926,0.37347760796546903,0.39213362336158802,0.85400331020355202,0.72436785697937001,0.86219531297683705,-0.33212241530418402,-0.37809386849403398,-3.7926216698371103E-2,-0.71978291531575,0.144973629857262,0.14012169780999301,0.16185366189155101,0.169755434426551,0.17890223632902]
["UP-E1L213C9","UP",7,"E1L213C9",231,"CD(R), ROI Expense, Railroad-Owned, FLAT - GENERAL",10.072217941284199,14.1725568771362,15.0191431045532,16.267978668212901,20.532058715820298,14.5066480636597,12.840674400329601,2.3242483139038099,6.6416940689086896,5.4671124773133402,14.072622853490399,7.5953421344561898,9.5650801918613002,7.1704728421138197,4.6983055731635801,7.9001129616685803]
["UP-E1L213C12","UP",7,"E1L213C12",234,"CD(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL",10.072217941284199,14.1725568771362,15.0191440582275,16.267980575561499,20.532058715820298,14.5066480636597,12.8406734466553,2.3242483139038099,6.6416940689086896,5.4671124773133402,14.072622853490399,7.5953421344561898,9.5650801918613002,7.1704728421138197,4.6983055731635801,7.9001129616685803]
["UP-E1L214C3","UP",7,"E1L214C3",238,"CM(R), ROI Expense, Railroad-Owned, FLAT - OTHER",7.30311870574951E-3,9.4006732106208801E-3,1.07075134292245E-2,1.1586531996727E-2,1.15263313055038E-2,1.21304374188185E-2,1.1717859655618701E-2,1.0701376013457799E-2,8.8109802454710007E-3,6.6809851742771504E-3,6.0141410264185303E-3,7.6647918139510001E-3,9.3687514954717901E-3,6.2702832064164002E-3,5.1174416442091603E-3,6.5224851834995998E-3]
["UP-E1L214C7","UP",7,"E1L214C7",242,"CD(R), OPR Expense, Railroad-Owned, FLAT - OTHER",1.3191504478454601,1.1905734539032,1.40649497509003,1.6965138912200901,1.38771140575409,1.5341892242431601,2.34390449523926,3.0675201416015598,3.7430667877197301,4.1570459685363197,4.7197261799890402,4.6897120767152298,4.24553713442491,3.40928754684521,2.86474957870715,2.1501156577691201]
["UP-E1L214C10","UP",7,"E1L214C10",245,"CD(Y), OPR Expense, Railroad-Owned, FLAT - OTHER",1.3191504478454601,1.1905734539032,1.40649497509003,1.6965140104293801,1.38771152496338,1.5341891050338701,2.34390425682068,3.0675203800201398,3.7430665493011501,4.1570459685363197,4.7197261799890402,4.6897120767152298,4.24553713442491,3.40928754684521,2.86474957870715,2.1501156577691201]
["UP-E1L214C11","UP",7,"E1L214C11",246,"CD(Y), DRL Expense, Railroad-Owned, FLAT - OTHER",20.803916931152301,18.8527717590332,18.862964630126999,20.396772384643601,16.272212982177699,17.0008869171143,14.802526473999,18.390211105346701,17.4098205566406,17.691666554137498,18.592157930967399,19.3352198453005,20.074284701454001,17.5423853484963,14.281980745620499,13.020755704513199]
["UP-E1L215C1","UP",7,"E1L215C1",249,"CM(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L215C5","UP",7,"E1L215C5",253,"CM(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L215C8","UP",7,"E1L215C8",256,"CD(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L215C11","UP",7,"E1L215C11",259,"CD(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L216C2","UP",7,"E1L216C2",263,"CM(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,1.8385049770586201E-4,0,7.4272528290748596E-3,1.4013680941529999E-4,2.4451077950018898E-4,1.70175261717922E-4,2.4363774554402801E-5,4.8286719475096399E-3,3.00148372572208E-6,2.8308021814053801E-6]
["UP-E1L216C6","UP",7,"E1L216C6",267,"CM(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L216C9","UP",7,"E1L216C9",270,"CD(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L216C10","UP",7,"E1L216C10",271,"CD(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L216C13","UP",7,"E1L216C13",274,"CM(R), DRL Expense, Privately-Owned, TANK >=22,000 GAL",1.14438962191343E-2,1.2561650946736301E-3,2.18772776424885E-2,1.7512649297714199E-2,1.73372458666563E-2,1.5107460319995899E-2,1.8385049770586201E-4,2.4943033349700299E-4,7.4272528290748596E-3,1.4013680941529999E-4,2.4451077950018898E-4,1.70175261717922E-4,2.4363774554402801E-5,4.8286719475096399E-3,3.00148372572208E-6,2.8308021814053801E-6]
["UP-E1L217C4","UP",7,"E1L217C4",278,"CM(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",1.08261788263917E-2,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L217C7","UP",7,"E1L217C7",281,"CD(R), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.343480825424194,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L217C10","UP",7,"E1L217C10",284,"CD(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.343480825424194,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L218C1","UP",7,"E1L218C1",288,"CM(R), OPR Expense, Railroad-Owned, AUTO RACKS",2.0100986585021002E-3,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L218C5","UP",7,"E1L218C5",292,"CM(Y), DRL Expense, Railroad-Owned, AUTO RACKS",0.172003239393234,0.19333478808403001,0.28249195218086198,0.39747968316078203,0.204507917165756,0.203741669654846,0.17157092690467801,7.2534412145614596E-2,8.3773359656333896E-2,0.10130327206277601,0.29929492392127499,0.29853029941106002,0.23778103354492899,0.15690906863034099,0.19337399522526799,0.2029983149781]
["UP-E1L218C8","UP",7,"E1L218C8",295,"CD(R), DRL Expense, Railroad-Owned, AUTO RACKS",2.38200163841248,-1.1318047046661399,-2.6114225387573198,3.8718597888946502,-2.2936828136444101,-1.686638712883,8.96231457591057E-3,-2.3857011795043901,4.9776034355163601,10.9175376193611,17.089291147719901,19.201138349145101,22.663744818426299,17.917354237359199,21.234117541022499,20.387025618839001]
["UP-E1L218C9","UP",7,"E1L218C9",296,"CD(R), ROI Expense, Railroad-Owned, AUTO RACKS",3.3568041324615501,4.8359727859497097,6.4169411659240696,7.8351130485534703,5.6188001632690403,5.6873669624328604,5.0377554893493697,6.5146565437316903,6.20967674255371,5.9435429390767398,6.0021375261683101,6.3439115024471198,7.3487589274947096,6.4750188541730003,5.9597570980276497,7.4757117847808301]
["UP-E1L218C12","UP",7,"E1L218C12",299,"CD(Y), ROI Expense, Railroad-Owned, AUTO RACKS",3.3568041324615501,4.8359723091125497,6.4169402122497603,7.8351144790649396,5.6188001632690403,5.6873669624328604,5.0377554893493697,6.5146565437316903,6.20967721939087,5.9435429390767398,6.0021375261683101,6.3439115024471198,7.3487589274947096,6.4750188541730003,5.9597570980276497,7.4757117847808301]
["UP-E1L219C3","UP",7,"E1L219C3",303,"CM(R), ROI Expense, Railroad-Owned, ACCESSORIAL",1.5509084914810999E-4,1.39321593451314E-4,1.4482728147413601E-4,6.9043468101881404E-5,5.48072202946059E-5,5.2308652811916498E-5,1.1970305422437401E-6,3.4951415273099E-7,2.6913340889222999E-7,2.0869286400716101E-7,1.13346451566296E-7,7.8356504328299295E-8,-6.8872036828515404E-9,-1.7247244993904701E-7,-2.5952548686965299E-7,-3.0117127977442298E-7]
["UP-E1L219C6","UP",7,"E1L219C6",306,"CM(Y), ROI Expense, Railroad-Owned, ACCESSORIAL",4.0323607390746501E-4,3.6223602364771101E-4,3.7655179039575197E-4,1.7951289191842101E-4,1.4249865489546199E-4,1.36002548970282E-4,3.1122790460358399E-6,9.0873624003506795E-7,6.9974657890270496E-7,5.4260144641861899E-7,2.9470077407236903E-7,2.03726911253578E-7,-1.7906729575414001E-8,-4.48428369841522E-7,-6.7476626586109497E-7,-7.83045327413501E-7]
["UP-E1L219C9","UP",7,"E1L219C9",309,"CD(R), ROI Expense, Railroad-Owned, ACCESSORIAL",2.76779569685459E-2,2.58390530943871E-2,2.7233412489294999E-2,1.3634226284921201E-2,1.07131330296397E-2,1.0293697007000399E-2,1.6748507914598999E-4,5.7247129007009803E-5,4.2778057832038003E-5,3.2569904822364901E-5,1.7787512251016301E-5,1.20802105586733E-5,-2.1076608096729802E-6,-2.85575169149558E-5,-4.2022794252639303E-5,-4.6707579599750402E-5]
["UP-E1L219C13","UP",7,"E1L219C13",313,"CM(R), DRL Expense, Privately-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["UP-E1L220C4","UP",7,"E1L220C4",317,"CM(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",8.7990649044513702E-2,9.4782173633575398E-2,0.10474406927824,0.149611607193947,0.108939379453659,9.7327508032321902E-2,9.8018750548362704E-2,0.10432491451501801,9.9482141435146304E-2,0.11233316423942399,0.11134725987322699,0.102374235741251,9.3453581451641607E-2,9.5863798527969404E-2,8.8426408561048997E-2,6.9096456966396505E-2]
["UP-E1L220C5","UP",7,"E1L220C5",318,"CM(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",9.2847004532813998E-2,9.7012951970100403E-2,0.101583071053028,0.108110204339027,9.1536328196525601E-2,8.6687147617340102E-2,8.84115025401115E-2,8.1516526639461503E-2,7.6571218669414506E-2,8.9504208138958694E-2,0.114219372578831,0.108177325062663,9.7921851569467602E-2,9.5954649674796999E-2,0.101212970309091,9.7670428587373501E-2]
["UP-E1L220C8","UP",7,"E1L220C8",321,"CD(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",12.4186849594116,11.5825204849243,11.812228202819799,13.962363243103001,12.4146881103516,12.2269830703735,12.3640842437744,12.9432163238525,11.6408748626709,13.672651676405399,14.2493564093977,13.7391337274483,13.7674514344943,13.163210557672601,12.7603655904382,10.256640447685999]
["UP-E1L220C11","UP",7,"E1L220C11",324,"CD(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",11.912299156189,11.0035562515259,11.4130096435547,14.180782318115201,11.920225143432599,11.628069877624499,11.4719400405884,11.872830390930201,11.0811262130737,13.0984639124068,14.175410927705601,14.1785166523323,14.8455501906148,14.137601939874401,13.951198046621901,12.1068191046644]
["UP-E1L221C2","UP",7,"E1L221C2",328,"CM(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.12906461954116799,0.14307302236557001,0.17700988054275499,0.21128720045089699,0.133779317140579,0.125801786780357,0.110686957836151,6.3794247806072193E-2,6.7422270774841295E-2,7.9305315520540806E-2,0.166358175695074,0.16168402785219399,0.12934848576878399,9.8264684496902899E-2,0.114897200574771,0.11494422104656001]
["UP-E1L221C5","UP",7,"E1L221C5",331,"CM(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.33556807041168202,0.371989786624908,0.46022552251815801,0.54934668540954601,0.34782624244689903,0.32708442211151101,0.287786215543747,0.165865033864975,0.175297901034355,0.206193820353406,0.43253125680719201,0.42037847241570397,0.33630606299884003,0.25548817969194798,0.29873272149440599,0.29885497472105599]
["UP-E1L221C8","UP",7,"E1L221C8",334,"CD(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",7.9394435882568404,3.6536157131195099,3.93187379837036,13.895545959472701,3.8924753665924099,2.48433637619019,3.6857278347015399,3.66235446929932,11.1495161056519,17.0849874298837,23.852473742766499,26.794455302657902,34.351049423210497,31.9804909980726,38.082057032447999,35.325344015084298]
["UP-E1L221C13","UP",7,"E1L221C13",339,"CM(R), DRL Expense, Privately-Owned, TOTAL FLAT, MULTILEVEL",0.11130332946777299,0.125895485281944,0.15740978717803999,0.24382610619068101,0.16130723059177399,0.146173596382141,0.135339811444283,0.145507231354713,0.141860380768776,0.14039323371421,0.13953621641484101,0.151950108498902,0.16852843197449799,0.15177107236072901,0.178318082985198,0.190209183513603]
["UP-E1L303C1","UP",7,"E1L303C1",342,"L&D Expense, POTATOES OTHER THAN SWEET",3.6799578666686998,3.1860339641571001,1.57116758823395,2.0286219120025599,0.46845808625221302,0.59124863147735596,0.76070266962051403,0.51356053352356001,1.9531569480896001,2.51130048867766,2.4820239734348402,1.5628554724856101,1.5738487949622999,4.7855950282905102,2.6763798404894299,1.6733272275745501]
["UP-E1L304C1","UP",7,"E1L304C1",343,"L&D Expense, FRESH FRUITS",0.302319556474686,8.5989952087402302E-2,0.58841019868850697,8.6072228848934201E-2,1.4460543170571299E-2,0.126831129193306,0.49312025308608998,0.52817994356155396,0.16668255627155301,8.2599028253724796E-2,9.9674777409128404E-2,0.43295957620681202,8.8434329739041695E-2,0.85901773298737005,1.1195029946875601,0.48971047651869798]
["UP-E1L307C1","UP",7,"E1L307C1",346,"L&D Expense, METALLIC ORES",1.6947247087955499E-2,7.1331090293824699E-3,3.3462069928646102E-2,7.0100501179695102E-2,4.2934261262416798E-2,3.86384478770196E-3,4.2152050882577896E-3,8.2664601504802704E-3,2.1994682028889699E-3,1.2440038637219399E-2,8.2511941540468301E-4,0,0,5.0977125450342798E-3,1.33905395969415E-4,0]
["UP-E1L310C1","UP",7,"E1L310C1",349,"L&D Expense, FOOD AND KINDRED PRODUCTS",0.112814217805862,0.10337255895137799,0.15115562081337,0.103318996727467,7.9335421323776203E-2,8.1889294087886796E-2,0.113200463354588,0.10237280279398001,0.105734661221504,0.155869352854069,0.14200791172845001,0.110538880168726,0.16084816368765401,0.19031238664048999,0.105766987771637,0.100991336079819]
["UP-E1L314C1","UP",7,"E1L314C1",353,"L&D Expense, GRAIN MILL PRODUCTS",3.1477384269237497E-2,6.5411634743213695E-2,8.0874219536781297E-2,6.5766513347625705E-2,5.2350562065839802E-2,5.79447709023952E-2,4.7625388950109503E-2,4.8314291983842898E-2,3.0080657452344901E-2,3.5506442073018903E-2,4.5023558881849897E-2,2.2275958202964401E-2,3.7569787654383499E-2,3.02891444533398E-2,2.6234808790303401E-2,6.1752196822825997E-2]
["UP-E1L317C1","UP",7,"E1L317C1",356,"L&D Expense, CEREALS",0.13801950216293299,0.150457173585892,0.113301411271095,0.12655127048492401,0.114000834524632,5.6761432439088801E-2,2.6986366137862199E-2,9.9266923964023604E-2,4.1428942233324099E-2,2.69035785859623E-2,7.1618623461894307E-2,1.92697768762677E-2,5.9594076037541001E-2,1.39432972578182E-3,9.1593963957775203E-4,6.4883822884699701E-3]
["UP-E1L320C1","UP",7,"E1L320C1",359,"L&D Expense, CORN PRODUCTS",1.34091908112168E-2,3.9376903325319297E-2,4.7181513160467099E-2,2.6431472972035401E-2,2.73294728249311E-2,3.8074269890785203E-2,3.7078451365232502E-2,1.75428669899702E-2,2.01527439057827E-2,4.1817161674595404E-3,1.34790764147741E-2,4.3508653131181197E-3,9.0233417435583996E-3,3.9086462228574504E-3,3.02978423330987E-5,2.0180023840311999E-2]
["UP-E1L325C1","UP",7,"E1L325C1",364,"L&D Expense, MISC FOOD PREPARATIONS",4.9347322434186901E-2,3.9073646068572998E-2,6.88051283359528E-2,4.7288753092288999E-2,7.3226988315582303E-2,4.44420874118805E-2,5.8179348707199097E-2,6.4795158803462996E-2,6.5988443791866302E-2,4.7256400580346102E-2,0.10027194560448401,5.8322594141169803E-2,4.7792372956870097E-2,4.0860279141872603E-2,3.6097560727487002E-2,5.5607518381965003E-2]
["UP-E1L328C1","UP",7,"E1L328C1",367,"L&D Expense, LUMBER AND WOOD EX FURNITURE",6.4082108438014998E-2,6.3597209751606001E-2,4.2465981096029302E-2,5.5317327380180401E-2,2.6106728240847601E-2,4.5685745775699602E-2,2.36855149269104E-2,3.1761787831783302E-2,2.2764811292290701E-2,5.5634208764431099E-2,6.8785233747138505E-2,4.2106313382289699E-2,5.85751816640947E-2,5.6718723912763502E-2,5.8628574900259398E-2,0.141446267912923]
["UP-E1L329C1","UP",7,"E1L329C1",368,"L&D Expense, LUMBER/DIMENSION STOCK",6.9662675261497498E-2,6.6921301186084706E-2,5.0744507461786298E-2,4.2644336819648701E-2,2.0643839612603201E-2,7.3353521525859805E-2,1.56366545706987E-2,3.8499526679515797E-2,2.4210380390286401E-2,6.5480499825039798E-2,6.5441979456708904E-2,6.6382032559786502E-2,9.6643513669763995E-2,3.5730563075364201E-2,7.45180514067776E-2,0.18957337341988301]
["UP-E1L332C1","UP",7,"E1L332C1",371,"L&D Expense, FURNITURE AND FIXTURES",1.01506423950195,4.2289190292358398,3.8702409267425502,1.72642862796783,1.0335067510604901,0.56756269931793202,1.8485848903655999,0.51095122098922696,0.77477347850799605,0.87920951704397499,0.29486340670581901,0.40993634402058698,0.171194339057925,0.29584487614604099,0.37153646834541698,2.0288792699200302]
["UP-E1L335C1","UP",7,"E1L335C1",374,"L&D Expense, PRINTING PAPER",0.45069688558578502,0.77085703611373901,0.80805128812789895,0.78840303421020497,0.60578840970992998,0.33505225181579601,0.42516347765922502,0.31435161828994801,0.37708187103271501,0.39925658646490703,0.66945896095312996,1.11723782584026,0.58951542221150599,0.19435054877364999,0.121608076937136,0.190232288385774]
["UP-E1L339C1","UP",7,"E1L339C1",378,"L&D Expense, ALL OTHER PULP, PAPER & ALLIED PRODUCTS",0.17567807435989399,0.195987403392792,0.152946561574936,0.107534527778625,7.8239731490612002E-2,8.5699714720249204E-2,0.122758314013481,8.2997627556324005E-2,7.0808172225952107E-2,5.6488843821234702E-2,7.3495363821740795E-2,3.9105518177458103E-2,5.0811760324324599E-2,0.14501322871120401,0.100518870925555,0.10260932363021701]
["UP-E1L342C1","UP",7,"E1L342C1",381,"L&D Expense, POTASSIUM OR SODIUM",2.7809889987111099E-2,1.60602275282145E-2,1.1788333766162401E-2,1.4397126622498001E-2,2.13480275124311E-2,1.2410043738782401E-2,9.0565774589776993E-3,7.6568066142499404E-3,1.3412986882031E-2,8.5684775629813106E-3,2.6314574467900101E-2,1.10570170436835E-2,1.12225187459802E-2,1.60371523159329E-2,1.1939958424653599E-2,5.9931752529763698E-3]
["UP-E1L345C1","UP",7,"E1L345C1",384,"L&D Expense, ALL OTHER CHEMICALS",2.6043361052870799E-2,0.102892324328423,5.1314171403646497E-2,5.8835830539464999E-2,4.2031995952129399E-2,1.8057033419609101E-2,2.5860302150249499E-2,7.7346088364720301E-3,2.08973791450262E-2,2.2599386791942899E-2,5.1338501809845997E-2,4.6916238257755201E-4,7.0031947197344305E-2,9.0754973556344501E-2,0.11058293551930599,1.91782433824856E-2]
["UP-E1L350C1","UP",7,"E1L350C1",389,"L&D Expense, STONE, CLAY AND GLASS PRODUCTS",2.8050996363163001E-2,2.94760055840015E-2,2.3014681413769701E-2,2.2323321551084501E-2,1.25137800350785E-2,2.0365133881568898E-2,1.3885203748941401E-2,1.2379656545817901E-2,2.0123468711972198E-2,1.8672422852622099E-2,1.5618687233242201E-2,7.1743035945493697E-3,1.00761913642266E-2,1.1213559823315599E-2,1.4322538640667201E-2,1.0220925283838099E-2]
["UP-E1L353C1","UP",7,"E1L353C1",392,"L&D Expense, ALL OTHER STONE & CLAY, GLASS PRODUCTS",2.3819899186492001E-2,2.95029655098915E-2,1.7426427453756301E-2,1.5901990234851799E-2,9.0113366022705997E-3,1.7641941085457798E-2,1.0626674629747901E-2,8.8174836710095406E-3,1.7466975376009899E-2,1.6213023466090899E-2,8.0123522222395605E-3,7.0282422645380101E-3,8.5392018813610897E-3,1.00639728338627E-2,1.8205648733177902E-2,8.8792988187615506E-3]
["UP-E1L354C1","UP",7,"E1L354C1",393,"L&D Expense, PRIMARY METAL PRODUCTS",3.4512434154748903E-2,5.7771623134613002E-2,4.6246688812971101E-2,0.105558961629868,4.7241918742656701E-2,4.59798015654087E-2,3.2263457775116001E-2,3.3330846577882801E-2,3.9058309048414203E-2,4.5040043560047503E-2,3.8303111795328998E-2,5.8488123741768101E-2,4.45886648461584E-2,8.2227833513675699E-2,4.9633379412000397E-2,6.0209103013003903E-2]
["UP-E1L357C1","UP",7,"E1L357C1",396,"L&D Expense, ALL OTHER PRIMARY METAL PRODUCTS",2.12727766484022E-2,9.5122657716274303E-2,0.135312050580978,4.1251994669437402E-2,3.5979904234409298E-2,3.8908191025257097E-2,5.8396480977535199E-2,1.43697401508689E-2,1.95995084941387E-2,2.3422915187733099E-2,3.1688528748677502E-2,3.7337457772167501E-2,8.8837298846552505E-4,7.0970671331329699E-2,0.279650607967111,9.53012962841015E-2]
["UP-E1L360C1","UP",7,"E1L360C1",399,"L&D Expense, ALL OTHER FAB METAL PRODUCTS",8.2236602902412401E-2,4.22826893627644E-2,0.12317106872797,0.57348483800888095,0.11085592955350899,0.104633316397667,0.104206696152687,0.41068261861801098,2.90865134447813E-2,2.6793860444710701E-2,1.17116840125649E-2,6.1026978151819303E-2,8.3779653724611707E-3,1.9695008077359299E-2,2.3129155730127701E-3,8.2394414457267903E-2]
["UP-E1L364C1","UP",7,"E1L364C1",403,"L&D Expense, CONST MIN/MAT HAND MACHINERY",5.3824152797460598E-2,0.14556503295898399,0.225022718310356,0.24387198686599701,0.111423380672932,1.9659049808979E-2,9.3566169962286897E-3,0.25835311412811302,9.0812714770436304E-3,2.4417359235743799E-2,0.226980429468987,0.123886814731048,5.6786413195415104,5.5626533761732502E-2,0.50608937133810405,2.0688925659798598]
["UP-E1L366C1","UP",7,"E1L366C1",405,"L&D Expense, ELECTRICAL MACHINERY",0.67479163408279397,0.47035461664199801,0.76611125469207797,0.65651184320449796,0.56727981567382801,0.21725417673587799,0.49147397279739402,0.91961038112640403,0.289804667234421,0.44987594767502198,0.21864727922893701,0.110947990600422,0.399700701714716,0.218458461333112,0.13409182722392801,1.67087861140951]
["UP-E1L372C1","UP",7,"E1L372C1",411,"L&D Expense, MOTOR PASSENGER CARS",1.6142339706420901,1.60462009906769,2.0916264057159402,1.80427742004395,1.1449105739593499,1.8661357164382899,2.4315426349639901,2.3879089355468799,2.9647860527038601,2.2775114836972699,2.3379065129382699,4.7704088395188302,3.82250992141388,3.6264625356952398,4.5673487040649103,7.7164689836323603]
["UP-E1L375C1","UP",7,"E1L375C1",414,"L&D Expense, ALL OTHER TRANSPORTATION EQUIPMENT",2.6227355003356899E-2,0.10049141198396699,3.2508585602045101E-2,6.5525375306606307E-2,0.26267328858375499,3.3132839947938898E-2,5.0899308174848598E-2,6.18039257824421E-2,9.2528991401195498E-2,3.1585700434175697E-2,7.6281476545512997E-2,0.119202553620429,7.6049686090451901E-2,4.0474509693458502,2.3140971066584299,1.6999942051205801E-2]
["UP-E1L378C1","UP",7,"E1L378C1",417,"L&D Expense, MISC MIXED SHIPMENTS",9.1315463185310405E-2,0.11395051330328,0.119482338428497,7.6815418899059296E-2,6.5753631293773707E-2,4.5803453773260103E-2,6.1025261878967299E-2,5.9127628803253202E-2,6.1889201402664198E-2,4.37200018110191E-2,7.5652365651906694E-2,3.3229987868641203E-2,3.2905317083349601E-2,3.0981519923329901E-2,4.4879455499843499E-2,4.5587054201045099E-2]
["UP-E1L379C1","UP",7,"E1L379C1",418,"L&D Expense, MISC MIXED SHIPMENTS NEC INC TOFC",9.1119572520256001E-2,0.112067364156246,0.119818732142448,7.3888465762138394E-2,6.1532124876975999E-2,4.5287456363439602E-2,6.1175230890512501E-2,5.8978945016860997E-2,5.8081496506929398E-2,4.2502426273880303E-2,7.4517811883176202E-2,3.2837985738498998E-2,3.2487919273463603E-2,1.9547644020149899E-2,3.9562979823806702E-2,4.5379167595824103E-2]
["UP-E1L382C1","UP",7,"E1L382C1",421,"L&D Expense, ALL OTHER COMMODITIES",3.7811581045389203E-2,0.571766257286072,0.50435817241668701,0.395120829343796,0.34854763746261602,0.28982281684875499,1.35337150096893,0.27479436993598899,2.1931312978267701E-2,0.35576115206112802,1.58875264111078,0.37422378104875798,0.25508157108880503,0.88390067928004001,0.16117152606319499,2.4966038048811998]
["UP-E2L101C4","UP",7,"E2L101C4",425,"E/L Ratio, All Freight Cars, BOX - 40 FT",1.4350563287735001,1.6781082153320299,1.5271072387695299,1.69590079784393,1.6346670389175399,1.6496042013168299,1.6738587617874101,1.64361536502838,1.54510951042175,1.53013860879029,1.58620340356564,1.62602403551193,1.6814540178931201,1.8036124432684699,1.78084668014306,1.7500720023040699]
["UP-E2L101C7","UP",7,"E2L101C7",428,"Average circuity, BOX - 40 FT",1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999]
["UP-E2L101C9","UP",7,"E2L101C9",430,"CD per Industry Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L101C15","UP",7,"E2L101C15",436,"CD per Load & Unload Intraterminal Switch, BOX - 40 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L101C18","UP",7,"E2L101C18",439,"CM per Interchange Switch, BOX - 40 FT",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["UP-E2L101C21","UP",7,"E2L101C21",442,"CM per I&I Switch, BOX - 40 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L101C22","UP",7,"E2L101C22",443,"Average CM per CD, Railroad-Owned, BOX - 40 FT",626.09124755859398,638.89947509765602,0,0,0,707.66638183593795,0,0,650.09063720703102,0,0,0,0,0,0,0]
["UP-E2L101C25","UP",7,"E2L101C25",446,"SEMs per Industry Switch, BOX - 40 FT",6.95050001144409,6.7008547782897896,6.0523476600646999,0,0,0,5.1721048355102504,0,0,0,5.0032109906049298,0,0,0,0,0]
["UP-E2L101C29","UP",7,"E2L101C29",450,"SEMs per I&I Switch, BOX - 40 FT",1.7376250028610201,1.6752138137817401,0,0,1.31425368785858,1.3278380632400499,0,0,1.2830847501754801,0,0,0,0,0,0,0]
["UP-E2L102C3","UP",7,"E2L102C3",453,"E/L Ratio, Privately-Owned, BOX - 50 FT",1.35681188106537,1.59989833831787,1.3776000738143901,1.5804842710495,1.5334554910659799,1.5609977245330799,1.6095232963562001,1.57289862632751,1.46113693714142,1.45160525067215,1.5120050639542499,1.5656458244718601,1.6349021188148201,1.79590910237333,1.74858467676713,1.69596954769369]
["UP-E2L102C5","UP",7,"E2L102C5",455,"Local circuity, BOX - 50 FT",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["UP-E2L102C11","UP",7,"E2L102C11",461,"CD per Intraterminal Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L102C14","UP",7,"E2L102C14",464,"CD per Load & Unload Industry Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L102C17","UP",7,"E2L102C17",467,"CM per Industry Switch, BOX - 50 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L102C18","UP",7,"E2L102C18",468,"CM per Interchange Switch, BOX - 50 FT",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["UP-E2L102C21","UP",7,"E2L102C21",471,"CM per I&I Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L102C25","UP",7,"E2L102C25",475,"SEMs per Industry Switch, BOX - 50 FT",6.95050001144409,6.7008547782897896,6.0523476600646999,5.7136745452880904,5.2570147514343297,5.3113522529602104,5.1721048355102504,5.2846555709838903,5.1323385238647496,4.9400372401710904,5.0032109906049298,4.9524509594886998,4.9163413700590297,4.8746082817399898,4.48371336478984,4.3741292642868501]
["UP-E2L102C28","UP",7,"E2L102C28",478,"SEMs per Interterminal Switch, BOX - 50 FT",8.3406009674072301,8.0410261154174805,7.26281690597534,6.8564105033874503,6.3084182739257804,6.3736238479614302,6.2065258026123002,6.3415875434875497,6.1588077545165998,5.9280446882053104,6.0038531887259197,5.9429411513864396,5.8996096440708303,5.8495299380879899,5.3804560377478099,5.2489551171442201]
["UP-E2L103C1","UP",7,"E2L103C1",480,"Average Tare Weight, BOX - EQUIPPED",36.099998474121101,36.099998474121101,36.200000762939503,36.099998474121101,36.200000762939503,36.200000762939503,36.400001525878899,36.5,36.5,36.5,36.6,36.700000000000003,36.799999999999997,37,37.1,37.299999999999997]
[{"$f":"B7298&\"-\"&D7298","v":"UP-E2L103C7"},"UP",7,"E2L103C7",486,"Average circuity, BOX - EQUIPPED",1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999]
["UP-E2L103C10","UP",7,"E2L103C10",489,"CD per Interchange Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L103C11","UP",7,"E2L103C11",490,"CD per Intraterminal Switch, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L103C14","UP",7,"E2L103C14",493,"CD per Load & Unload Industry Switch, BOX - EQUIPP",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L103C17","UP",7,"E2L103C17",496,"CM per Industry Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L103C21","UP",7,"E2L103C21",500,"CM per I&I Switch, BOX - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L103C26","UP",7,"E2L103C26",505,"SEMs per Interchange Switch, BOX - EQUIPPED",3.82277488708496,3.6854703426361102,3.3287913799285902,3.1425216197967498,2.89135813713074,2.9212441444396999,2.8446574211120601,2.9065604209899898,2.82278633117676,2.7170204820941,2.7517660448327099,2.72384802771878,2.7039877535324699,2.6810345549569998,2.4660423506344098,2.4057710953577698]
["UP-E2L103C28","UP",7,"E2L103C28",507,"SEMs per Interterminal Switch, BOX - EQUIPPED",8.3406009674072301,8.0410270690918004,7.26281690597534,6.8564105033874503,6.3084177970886204,6.3736233711242702,6.2065262794494602,6.3415865898132298,6.1588072776794398,5.9280446882053104,6.0038531887259197,5.9429411513864396,5.8996096440708303,5.8495299380879899,5.3804560377478099,5.2489551171442201]
["UP-E2L104C3","UP",7,"E2L104C3",511,"E/L Ratio, Privately-Owned, GONDOLA - PLAIN",2.3969848155975302,2.3795516490936302,2.2978887557983398,2.30961966514587,2.3102962970733598,2.2888960838317902,2.3156373500824001,1.9914087057113601,1.9870234727859499,1.9847457771846599,1.98073010305796,1.99368723714703,1.9930344279977601,1.9906688834889401,1.9974783392934901,1.9963720450316]
["UP-E2L104C6","UP",7,"E2L104C6",514,"Interline circuity, GONDOLA - PLAIN",1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.151,1.151,1.151,1.151,1.151,1.151,1.151]
["UP-E2L104C7","UP",7,"E2L104C7",515,"Average circuity, GONDOLA - PLAIN",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["UP-E2L104C10","UP",7,"E2L104C10",518,"CD per Interchange Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L104C13","UP",7,"E2L104C13",521,"CD per I&I Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L104C17","UP",7,"E2L104C17",525,"CM per Industry Switch, GONDOLA - PLAIN",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L104C22","UP",7,"E2L104C22",530,"Average CM per CD, Railroad-Owned, GONDOLA - PLAIN",626.09118652343795,638.89953613281295,668.76696777343795,786.42926025390602,733.56066894531295,707.66638183593795,729.85687255859398,720.34368896484398,650.09063720703102,643.09421058408304,665.54871430049695,612.93755803264196,587.48292339771103,562.83978931581396,611.17092098456101,574.88279583356996]
["UP-E2L104C25","UP",7,"E2L104C25",533,"SEMs per Industry Switch, GONDOLA - PLAIN",6.95049953460693,6.7008547782897896,6.0523476600646999,5.7136745452880904,5.2570152282714799,5.3113522529602104,5.1721048355102504,5.2846550941467303,5.1323394775390598,4.9400372401710904,5.0032109906049298,4.9524509594886998,4.9163413700590297,4.8746082817399898,4.48371336478984,4.3741292642868501]
["UP-E2L104C28","UP",7,"E2L104C28",536,"SEMs per Interterminal Switch, GONDOLA - PLAIN",8.3406009674072301,8.0410270690918004,7.26281690597534,6.8564105033874503,6.3084182739257804,6.3736238479614302,6.2065262794494602,6.3415870666503897,6.1588077545165998,5.9280446882053104,6.0038531887259197,5.9429411513864396,5.8996096440708303,5.8495299380879899,5.3804560377478099,5.2489551171442201]
["UP-E2L105C2","UP",7,"E2L105C2",539,"E/L Ratio, Railroad-Owned, GONDOLA - EQUIPPED",1.90046334266663,2.1030845642089799,1.9378196001052901,2.1022365093231201,2.0476381778717001,1.9501868486404399,2.0250477790832502,2.00736308097839,1.9340859651565601,2.0532483839464302,2.03658517559324,2.0526386125382401,1.9276708692767099,2.04844654343652,2.09929429837897,1.9255249530529801]
["UP-E2L105C3","UP",7,"E2L105C3",540,"E/L Ratio, Privately-Owned, GONDOLA - EQUIPPED",1.97204697132111,1.9891659021377599,1.9534212350845299,1.95558226108551,2.0093421936035201,1.94736635684967,1.99269890785217,1.9784749746322601,1.9871344566345199,1.9824199372991,1.9281301283907699,1.87379378127234,1.9192908274915601,1.9602151923200799,2.0086905605719698,1.9807427373465101]
["UP-E2L105C6","UP",7,"E2L105C6",543,"Interline circuity, GONDOLA - EQUIPPED",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["UP-E2L105C9","UP",7,"E2L105C9",546,"CD per Industry Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
[{"$f":"B7362&\"-\"&D7362","v":"UP-E2L105C13"},"UP",7,"E2L105C13",550,"CD per I&I Switch, GONDOLA - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L105C18","UP",7,"E2L105C18",555,"CM per Interchange Switch, GONDOLA - EQUIPPED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["UP-E2L105C21","UP",7,"E2L105C21",558,"CM per I&I Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L105C24","UP",7,"E2L105C24",561,"Average Miles between Interchange Switches, GONDOLA - EQUIPPED",989.254638671875,906.23156738281295,874.42266845703102,1065.63806152344,983.196044921875,1003.93933105469,962.34100341796898,1094.31689453125,1108.09558105469,1248.97691196242,1128.49875244697,1038.66329471172,1058.55427537421,1262.2297161608999,1239.42650140725,1228.6666039576701]
["UP-E2L105C27","UP",7,"E2L105C27",564,"SEMs per Intraterminal Switch, GONDOLA - EQUIPPED",10.4257488250732,10.0512838363647,9.0785207748413104,8.5705127716064506,7.8855218887329102,7.9670286178588903,7.75815677642822,7.9269833564758301,7.69850873947144,7.4100558602566302,7.5048164859073996,7.4286764392330502,7.3745120550885401,7.3119124226099901,6.7255700471847701,6.5611938964302796]
["UP-E2L105C28","UP",7,"E2L105C28",565,"SEMs per Interterminal Switch, GONDOLA - EQUIPPED",8.3406009674072301,8.0410261154174805,7.2628173828125,6.8564109802246103,6.3084182739257804,6.3736233711242702,6.2065262794494602,6.3415875434875497,6.1588072776794398,5.9280446882053104,6.0038531887259197,5.9429411513864396,5.8996096440708303,5.8495299380879899,5.3804560377478099,5.2489551171442201]
["UP-E2L106C2","UP",7,"E2L106C2",568,"E/L Ratio, Railroad-Owned, HOPPER - COVERED",2.0287399291992201,2.0362322330474898,2.0469868183136,2.0935070514678999,2.0643842220306401,2.0352492332458501,2.0263962745666499,2.0414202213287398,2.0005838871002202,2.0046624219882698,2.0565956964607199,2.0692136313591898,2.0723346330793602,2.0741432269585198,2.0757454815697098,2.0709209010875398]
["UP-E2L106C5","UP",7,"E2L106C5",571,"Local circuity, HOPPER - COVERED",1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999]
["UP-E2L106C9","UP",7,"E2L106C9",575,"CD per Industry Switch, HOPPER - COVERED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L106C14","UP",7,"E2L106C14",580,"CD per Load & Unload Industry Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L106C17","UP",7,"E2L106C17",583,"CM per Industry Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L106C20","UP",7,"E2L106C20",586,"CM per Interterminal Switch, HOPPER - COVERED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["UP-E2L106C23","UP",7,"E2L106C23",589,"Average Miles between I&I Switches, HOPPER - COVERED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["UP-E2L106C24","UP",7,"E2L106C24",590,"Average Miles between Interchange Switches, HOPPER - COVERED",1227.02502441406,1271.29211425781,1245.92932128906,1381.91394042969,1431.83117675781,1537.541015625,1525.52001953125,1538.68737792969,1630.86059570313,1579.3096325669401,1752.9117693084499,1986.85398899913,1992.20461486917,1960.23206055529,1885.4881654185799,2065.4864414119202]
["UP-E2L106C27","UP",7,"E2L106C27",593,"SEMs per Intraterminal Switch, HOPPER - COVERED",10.4257507324219,10.051282882690399,9.0785207748413104,8.5705118179321307,7.8855218887329102,7.9670290946960396,7.75815725326538,7.9269833564758301,7.69850873947144,7.4100558602566302,7.5048164859073996,7.4286764392330502,7.3745120550885401,7.3119124226099901,6.7255700471847701,6.5611938964302796]
["UP-E2L107C2","UP",7,"E2L107C2",597,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.0366942882537802,2.0185384750366202,2.0296857357025102,2.0283181667327899,2.0436372756957999,2.05406618118286,2.0386898517608598,2.0383753776550302,2.0381314754486102,2.0550566968341801,2.0841087012320298,2.0767441860465099,2.1017719931002001,2.06064298770653,2.0642730708510699,2.0496423425928301]
["UP-E2L107C6","UP",7,"E2L107C6",601,"Interline circuity, HOPPER - OPEN TOP - GENERAL",1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.137,1.137,1.137,1.137,1.137,1.137,1.137]
["UP-E2L107C9","UP",7,"E2L107C9",604,"CD per Industry Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L107C13","UP",7,"E2L107C13",608,"CD per I&I Switch, HOPPER - OPEN TOP - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L107C16","UP",7,"E2L107C16",611,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
[{"$f":"B7426&\"-\"&D7426","v":"UP-E2L107C19"},"UP",7,"E2L107C19",614,"CM per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["UP-E2L107C20","UP",7,"E2L107C20",615,"CM per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["UP-E2L107C23","UP",7,"E2L107C23",618,"Average Miles between I&I Switches, HOPPER - OPEN TOP - GENERAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["UP-E2L107C27","UP",7,"E2L107C27",622,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",10.425749778747599,10.0512838363647,9.0785217285156303,8.5705127716064506,7.8855218887329102,7.9670286178588903,7.75815725326538,7.9269838333129901,7.69850826263428,7.4100558602566302,7.5048164859073996,7.4286764392330502,7.3745120550885401,7.3119124226099901,6.7255700471847604,6.5611938964302796]
["UP-E2L108C2","UP",7,"E2L108C2",626,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",2.0254976749420202,2.0158145427703902,2.01138114929199,2.0219175815582302,2.0264554023742698,2.0194275379180899,2.0026261806488002,1.92483127117157,1.95124292373657,1.9563660909080001,2.02382233952043,2.0322605529498898,2.0272471268741898,2.0508178575820901,2.0692683810213701,2.00635765737551]
["UP-E2L108C5","UP",7,"E2L108C5",629,"Local circuity, HOPPER - OPEN TOP - SPECIAL",1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.202,1.202,1.202,1.202,1.202,1.202,1.202]
["UP-E2L108C9","UP",7,"E2L108C9",633,"CD per Industry Switch, HOPPER - OPEN TOP - SPECIAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L108C12","UP",7,"E2L108C12",636,"CD per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["UP-E2L108C13","UP",7,"E2L108C13",637,"CD per I&I Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L108C16","UP",7,"E2L108C16",640,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L108C19","UP",7,"E2L108C19",643,"CM per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["UP-E2L108C23","UP",7,"E2L108C23",647,"Average Miles between I&I Switches, HOPPER - OPEN TOP - SPECIAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["UP-E2L108C27","UP",7,"E2L108C27",651,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",10.425749778747599,10.0512838363647,9.0785217285156303,8.5705127716064506,7.8855214118957502,7.9670286178588903,7.75815773010254,7.9269833564758301,7.69850778579712,7.4100558602566302,7.5048164859073996,7.4286764392330502,7.3745120550885401,7.3119124226099901,6.7255700471847701,6.5611938964302796]
["UP-E2L109C1","UP",7,"E2L109C1",654,"Average Tare Weight, REFRIGERATED - MECH",46.099998474121101,46.099998474121101,46.400001525878899,46.599998474121101,46.599998474121101,46.5,46.599998474121101,47,47.200000762939503,47.5,48.2,48.3,48.4,48.6,48.9,49.2]
["UP-E2L109C5","UP",7,"E2L109C5",658,"Local circuity, REFRIGERATED - MECH",1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.079,1.079,1.079,1.079,1.079,1.079,1.079]
["UP-E2L109C8","UP",7,"E2L109C8",661,"Spotted-to-Pulled Ratio, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L109C9","UP",7,"E2L109C9",662,"CD per Industry Switch, REFRIGERATED - MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L109C12","UP",7,"E2L109C12",665,"CD per Interterminal Switch, REFRIGERATED - MECH",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["UP-E2L109C15","UP",7,"E2L109C15",668,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L109C19","UP",7,"E2L109C19",672,"CM per Intraterminal Switch, REFRIGERATED - MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["UP-E2L109C23","UP",7,"E2L109C23",676,"Average Miles between I&I Switches, REFRIGERATED - MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["UP-E2L109C26","UP",7,"E2L109C26",679,"SEMs per Interchange Switch, REFRIGERATED - MECH",3.82277512550354,3.6854705810546902,3.3287913799285902,3.1425218582153298,2.89135789871216,2.9212439060211199,2.8446576595306401,2.9065604209899898,2.82278633117676,2.7170204820941,2.7517660448327099,2.72384802771878,2.7039877535324699,2.6810345549569998,2.4660423506344098,2.4057710953577698]
["UP-E2L110C1","UP",7,"E2L110C1",683,"Average Tare Weight, REFRIGERATED - NON-MECH",42.799999237060497,42.900001525878899,43.099998474121101,43.299999237060497,43.799999237060497,43.400001525878899,44,44.099998474121101,44.099998474121101,44.2,44.2,44.2,44.2,44.2,44.6,45.2]
["UP-E2L110C4","UP",7,"E2L110C4",686,"E/L Ratio, All Freight Cars, REFRIGERATED - NON-MECH",1.9523948431014999,2.1389715671539302,2.0070152282714799,1.8656034469604501,1.93338918685913,2.0089797973632799,2.1027779579162602,2.0006184577941899,2.0231897830963099,2.06031324418392,1.9791324949881499,2.0143740902474501,2.1629510825982399,2.1354735580125199,2.2653790521568999,2.2255164664188798]
["UP-E2L110C5","UP",7,"E2L110C5",687,"Local circuity, REFRIGERATED - NON-MECH",1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001]
["UP-E2L110C8","UP",7,"E2L110C8",690,"Spotted-to-Pulled Ratio, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L110C11","UP",7,"E2L110C11",693,"CD per Intraterminal Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L110C15","UP",7,"E2L110C15",697,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - NON-MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L110C19","UP",7,"E2L110C19",701,"CM per Intraterminal Switch, REFRIGERATED - NON-MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["UP-E2L110C23","UP",7,"E2L110C23",705,"Average Miles between I&I Switches, REFRIGERATED - NON-MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["UP-E2L110C26","UP",7,"E2L110C26",708,"SEMs per Interchange Switch, REFRIGERATED - NON-MECH",3.82277536392212,3.6854703426361102,3.3287913799285902,3.1425216197967498,2.89135813713074,2.9212441444396999,2.8446576595306401,2.9065606594085698,2.82278633117676,2.7170204820941,2.7517660448327099,2.72384802771878,2.7039877535324699,2.6810345549569998,2.4660423506344098,2.4057710953577698]
["UP-E2L110C29","UP",7,"E2L110C29",711,"SEMs per I&I Switch, REFRIGERATED - NON-MECH",1.7376250028610201,1.6752138137817401,1.5130867958068801,1.4284188747405999,1.31425356864929,1.3278380632400499,1.2930262088775599,1.3211638927459699,1.2830847501754801,1.2350093100427699,1.25080274765123,1.2381127398721701,1.2290853425147601,1.2186520704349999,1.12092834119746,1.0935323160717101]
["UP-E2L111C1","UP",7,"E2L111C1",712,"Average Tare Weight, FLAT - TOFC",58.299999237060497,59.700000762939503,59.400001525878899,59.5,59.099998474121101,59.299999237060497,58.200000762939503,57.799999237060497,57.799999237060497,58.3,58.6,58.6,58.5,58.9,58.7,58.6]
["UP-E2L111C4","UP",7,"E2L111C4",715,"E/L Ratio, All Freight Cars, FLAT - TOFC",1.1678380966186499,1.15844810009003,1.1538546085357699,1.16184782981873,1.12437903881073,1.12450683116913,1.12377941608429,1.0489094257354701,1.05144715309143,1.0545217231525701,1.04089083447012,1.0430079103508201,1.04377395235611,1.03571224802391,1.02817193957558,1.0277683555398101]
["UP-E2L111C7","UP",7,"E2L111C7",718,"Average circuity, FLAT - TOFC",1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.085,1.085,1.085,1.085,1.085,1.085,1.085]
["UP-E2L111C11","UP",7,"E2L111C11",722,"CD per Intraterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L111C15","UP",7,"E2L111C15",726,"CD per Load & Unload Intraterminal Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L111C19","UP",7,"E2L111C19",730,"CM per Intraterminal Switch, FLAT - TOFC",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["UP-E2L111C22","UP",7,"E2L111C22",733,"Average CM per CD, Railroad-Owned, FLAT - TOFC",626.09112548828102,638.89953613281295,668.76690673828102,786.42919921875,733.56060791015602,707.66638183593795,729.85687255859398,720.34368896484398,650.09063720703102,643.09421058408304,665.54871430049695,612.93755803264196,587.48292339771103,562.83978931581396,611.17092098455998,574.88279583356996]
["UP-E2L111C25","UP",7,"E2L111C25",736,"SEMs per Industry Switch, FLAT - TOFC",6.95049953460693,6.7008547782897896,6.05234718322754,5.7136750221252397,5.2570152282714799,5.3113527297973597,5.1721048355102504,5.2846550941467303,5.1323394775390598,4.9400372401710904,5.0032109906049298,4.9524509594886998,4.9163413700590297,4.8746082817399898,4.48371336478984,4.3741292642868501]
["UP-E2L111C26","UP",7,"E2L111C26",737,"SEMs per Interchange Switch, FLAT - TOFC",3.82277536392212,3.6854705810546902,3.3287911415100102,3.1425216197967498,2.89135789871216,2.9212439060211199,2.8446578979492201,2.9065604209899898,2.82278633117676,2.7170204820941,2.7517660448327099,2.72384802771878,2.7039877535324699,2.6810345549569998,2.4660423506344098,2.4057710953577698]
["UP-E2L111C29","UP",7,"E2L111C29",740,"SEMs per I&I Switch, FLAT - TOFC",1.7376250028610201,1.6752139329910301,1.5130867958068801,1.4284189939498899,1.31425380706787,1.3278380632400499,1.2930262088775599,1.3211638927459699,1.2830846309661901,1.2350093100427699,1.25080274765123,1.2381127398721701,1.2290853425147601,1.2186520704349999,1.12092834119746,1.0935323160717101]
["UP-E2L112C3","UP",7,"E2L112C3",743,"E/L Ratio, Privately-Owned, FLAT - MULTILEVEL",1.37015068531036,1.3654258251190201,1.3269906044006301,1.3540611267089799,1.35878133773804,1.3853628635406501,1.3780049085617101,1.37900578975677,1.3909322023391699,1.40169616835248,1.36525176710632,1.3536361958601699,1.3508103878242199,1.3767337645448601,1.37136623399039,1.3100660906286701]
["UP-E2L112C7","UP",7,"E2L112C7",747,"Average circuity, FLAT - MULTILEVEL",1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999]
["UP-E2L112C11","UP",7,"E2L112C11",751,"CD per Intraterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L112C15","UP",7,"E2L112C15",755,"CD per Load & Unload Intraterminal Switch, FLAT - MULTILEVEL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L112C18","UP",7,"E2L112C18",758,"CM per Interchange Switch, FLAT - MULTILEVEL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["UP-E2L112C21","UP",7,"E2L112C21",761,"CM per I&I Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L112C22","UP",7,"E2L112C22",762,"Average CM per CD, Railroad-Owned, FLAT - MULTILEVEL",626.09118652343795,638.89947509765602,668.76690673828102,786.42919921875,733.56060791015602,707.66638183593795,729.85681152343795,720.34362792968795,650.09063720703102,643.09421058408304,665.54871430049695,612.93755803264196,587.48292339771103,562.83978931581396,611.17092098455998,574.88279583356996]
["UP-E2L112C25","UP",7,"E2L112C25",765,"SEMs per Industry Switch, FLAT - MULTILEVEL",6.95050001144409,6.7008547782897896,6.0523476600646999,5.7136750221252397,5.2570147514343297,5.3113522529602104,5.1721048355102504,5.2846555709838903,5.1323390007018999,4.9400372401710904,5.0032109906049298,4.9524509594886998,4.9163413700590297,4.8746082817399898,4.48371336478984,4.3741292642868501]
["UP-E2L112C28","UP",7,"E2L112C28",768,"SEMs per Interterminal Switch, FLAT - MULTILEVEL",8.3406009674072301,8.0410270690918004,7.2628173828125,6.8564109802246103,6.3084182739257804,6.3736238479614302,6.2065258026123002,6.3415875434875497,6.1588068008422896,5.9280446882053104,6.0038531887259197,5.9429411513864396,5.8996096440708303,5.8495299380879899,5.3804560377478099,5.2489551171442201]
["UP-E2L113C4","UP",7,"E2L113C4",773,"E/L Ratio, All Freight Cars, FLAT - GENERAL",1.9948717355728101,1.8360248804092401,1.9543379545211801,1.9963898658752399,1.87834548950195,1.86918604373932,2.2360060214996298,1.9678111076355,1.7822580337524401,1.56242707117853,1.99356223175966,1.84838160136286,2.0400890868596901,1.94933333333333,1.8179723502304099,2.0098684210526301]
["UP-E2L113C7","UP",7,"E2L113C7",776,"Average circuity, FLAT - GENERAL",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["UP-E2L113C11","UP",7,"E2L113C11",780,"CD per Intraterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L113C14","UP",7,"E2L113C14",783,"CD per Load & Unload Industry Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L113C17","UP",7,"E2L113C17",786,"CM per Industry Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L113C18","UP",7,"E2L113C18",787,"CM per Interchange Switch, FLAT - GENERAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["UP-E2L113C21","UP",7,"E2L113C21",790,"CM per I&I Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L113C24","UP",7,"E2L113C24",793,"Average Miles between Interchange Switches, FLAT - GENERAL",865.08758544921898,648.651123046875,713.35504150390602,666.66668701171898,656.54949951171898,747.01416015625,726.37365722656295,650.83795166015602,744.25921630859398,824.83156881616901,744.40894568690101,5513.4518518518498,610.054347826087,2440.5653836691799,676.01246105918995,690.90909090909099]
["UP-E2L113C29","UP",7,"E2L113C29",798,"SEMs per I&I Switch, FLAT - GENERAL",1.7376248836517301,1.6752136945724501,1.5130869150161701,1.4284188747405999,1.31425368785858,1.3278380632400499,1.2930262088775599,1.3211638927459699,1.2830847501754801,1.2350093100427699,1.25080274765123,1.2381127398721701,1.2290853425147601,1.2186520704349999,1.12092834119746,1.0935323160717101]
["UP-E2L114C3","UP",7,"E2L114C3",801,"E/L Ratio, Privately-Owned, FLAT - OTHER",1.9585890769958501,1.9788457155227701,1.94232285022736,1.93731093406677,1.84672296047211,1.85872662067413,1.8780425786971999,1.8886147737503101,1.8497232198715201,1.88986128772201,1.8720514518112199,1.8944836047826401,1.9437262252604901,1.9400198450336299,1.90567582060907,1.9045446290747301]
["UP-E2L114C7","UP",7,"E2L114C7",805,"Average circuity, FLAT - OTHER",1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.155,1.155,1.155,1.155,1.155,1.155,1.155]
["UP-E2L114C10","UP",7,"E2L114C10",808,"CD per Interchange Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L114C11","UP",7,"E2L114C11",809,"CD per Intraterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L114C14","UP",7,"E2L114C14",812,"CD per Load & Unload Industry Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L114C17","UP",7,"E2L114C17",815,"CM per Industry Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L114C20","UP",7,"E2L114C20",818,"CM per Interterminal Switch, FLAT - OTHER",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["UP-E2L114C25","UP",7,"E2L114C25",823,"SEMs per Industry Switch, FLAT - OTHER",6.95050048828125,6.7008547782897896,6.05234718322754,5.7136750221252397,5.2570152282714799,5.3113527297973597,5.1721043586731001,5.2846550941467303,5.1323390007018999,4.9400372401710904,5.0032109906049298,4.9524509594886998,4.9163413700590297,4.8746082817399898,4.48371336478984,4.3741292642868501]
["UP-E2L114C28","UP",7,"E2L114C28",826,"SEMs per Interterminal Switch, FLAT - OTHER",8.3406009674072301,8.0410261154174805,7.26281642913818,6.8564100265502903,6.3084182739257804,6.3736238479614302,6.2065262794494602,6.3415875434875497,6.1588072776794398,5.9280446882053104,6.0038531887259197,5.9429411513864396,5.8996096440708303,5.8495299380879899,5.3804560377478099,5.2489551171442201]
["UP-E2L115C3","UP",7,"E2L115C3",830,"E/L Ratio, Privately-Owned, TANK <22,000 GAL",2.0748350620269802,2.0653743743896502,2.0800139904022199,2.0378584861755402,2.00978350639343,2.0786166191101101,2.06017971038818,1.98925304412842,2.0004615783691402,2.0055311939406,2.0081591843284401,2.0067335719293098,2.0026391742638299,2.0267260305141699,2.0400776814319102,2.0143530520857902]
["UP-E2L115C6","UP",7,"E2L115C6",833,"Interline circuity, TANK <22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["UP-E2L115C7","UP",7,"E2L115C7",834,"Average circuity, TANK <22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["UP-E2L115C10","UP",7,"E2L115C10",837,"CD per Interchange Switch, TANK <22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L115C16","UP",7,"E2L115C16",843,"CD per Load & Unload Interterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L115C18","UP",7,"E2L115C18",845,"CM per Interchange Switch, TANK <22,000 GAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["UP-E2L115C21","UP",7,"E2L115C21",848,"CM per I&I Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L115C24","UP",7,"E2L115C24",851,"Average Miles between Interchange Switches, TANK <22,000 GAL",1126.22583007813,1156.65515136719,1124.38122558594,1185.73278808594,1251.25659179688,1340.88720703125,1218.39074707031,1315.70764160156,1451.10290527344,1573.4495387568199,1535.88583016289,1724.26138631139,1853.81868069956,1899.87167686714,1995.8525970932601,2104.4189041784398]
["UP-E2L115C28","UP",7,"E2L115C28",855,"SEMs per Interterminal Switch, TANK <22,000 GAL",8.3406009674072301,8.0410261154174805,7.26281690597534,6.8564100265502903,6.3084177970886204,6.3736243247985804,6.2065262794494602,6.3415870666503897,6.1588072776794398,5.9280446882053104,6.0038531887259197,5.9429411513864396,5.8996096440708303,5.8495299380879899,5.3804560377478099,5.2489551171442201]
["UP-E2L116C2","UP",7,"E2L116C2",858,"E/L Ratio, Railroad-Owned, TANK >=22,000 GAL",1.1206567287445099,1.12803566455841,1.12975549697876,1.0656725168228101,1.0839644670486499,1.0771785974502599,1.0933152437210101,1.79481136798859,1.79600882530212,1.6352140077821,1.5305832147937399,1.7327586206896599,1.5489130434782601,1.47684605757197,1.7683397683397699,1.5956790123456801]
["UP-E2L116C3","UP",7,"E2L116C3",859,"E/L Ratio, Privately-Owned, TANK >=22,000 GAL",2.04571533203125,2.0228207111358598,2.0742216110229501,2.0566809177398699,2.0675735473632799,2.0860216617584202,2.0088129043579102,1.9879137277603101,1.9914255142211901,2.0069144467604398,2.0278427912638199,2.0236782705452199,2.0097057485989902,2.0187603050124201,2.0408281258369998,2.0286539004316801]
["UP-E2L116C6","UP",7,"E2L116C6",862,"Interline circuity, TANK >=22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["UP-E2L116C12","UP",7,"E2L116C12",868,"CD per Interterminal Switch, TANK >=22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
[{"$f":"B7682&\"-\"&D7682","v":"UP-E2L116C14"},"UP",7,"E2L116C14",870,"CD per Load & Unload Industry Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L116C17","UP",7,"E2L116C17",873,"CM per Industry Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L116C21","UP",7,"E2L116C21",877,"CM per I&I Switch, TANK >=22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L116C24","UP",7,"E2L116C24",880,"Average Miles between Interchange Switches, TANK >=22,000 GAL",1126.22583007813,1156.65515136719,1124.38122558594,1185.73278808594,1251.25659179688,1340.88720703125,1218.39074707031,1315.70764160156,1451.10290527344,1573.4495387568199,1535.88583016289,1724.26138631139,1853.81868069956,1899.87167686714,1995.8525970932601,2104.4189041784398]
["UP-E2L116C27","UP",7,"E2L116C27",883,"SEMs per Intraterminal Switch, TANK >=22,000 GAL",10.425749778747599,10.051282882690399,9.0785207748413104,8.5705127716064506,7.8855209350585902,7.9670286178588903,7.75815725326538,7.92698431015015,7.69850778579712,7.4100558602566302,7.5048164859073996,7.4286764392330502,7.3745120550885401,7.3119124226099901,6.7255700471847604,6.5611938964302796]
["UP-E2L116C28","UP",7,"E2L116C28",884,"SEMs per Interterminal Switch, TANK >=22,000 GAL",8.3406009674072301,8.0410261154174805,7.26281690597534,6.8564100265502903,6.3084177970886204,6.3736243247985804,6.2065262794494602,6.3415870666503897,6.1588072776794398,5.9280446882053104,6.0038531887259197,5.9429411513864396,5.8996096440708303,5.8495299380879899,5.3804560377478099,5.2489551171442201]
["UP-E2L117C2","UP",7,"E2L117C2",887,"E/L Ratio, Railroad-Owned, ALL OTHER FREIGHT CARS",1.1206567287445099,1.12803566455841,1.12975549697876,1.0656725168228101,1.0839644670486499,1.0771785974502599,1.0933152437210101,1.79481136798859,1.79600882530212,1.6352140077821,1.5305832147937399,1.7327586206896599,1.5489130434782601,1.47684605757197,1.7683397683397699,1.5956790123456801]
["UP-E2L117C8","UP",7,"E2L117C8",893,"Spotted-to-Pulled Ratio, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L117C10","UP",7,"E2L117C10",895,"CD per Interchange Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L117C13","UP",7,"E2L117C13",898,"CD per I&I Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L117C17","UP",7,"E2L117C17",902,"CM per Industry Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["UP-E2L117C20","UP",7,"E2L117C20",905,"CM per Interterminal Switch, ALL OTHER FREIGHT CARS",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["UP-E2L117C23","UP",7,"E2L117C23",908,"Average Miles between I&I Switches, ALL OTHER FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["UP-E2L117C24","UP",7,"E2L117C24",909,"Average Miles between Interchange Switches, ALL OTHER FREIGHT CARS",1126.22583007813,1156.65515136719,1124.38122558594,1185.73278808594,1251.25659179688,1340.88720703125,1218.39074707031,1315.70764160156,1451.10290527344,1573.4495387568199,1535.88583016289,1724.26138631139,1853.81868069956,1899.87167686714,1995.8525970932601,2104.4189041784398]
["UP-E2L117C27","UP",7,"E2L117C27",912,"SEMs per Intraterminal Switch, ALL OTHER FREIGHT CARS",10.425749778747599,10.051282882690399,9.0785207748413104,8.5705127716064506,7.8855209350585902,7.9670286178588903,7.75815725326538,7.92698431015015,7.69850778579712,7.4100558602566302,7.5048164859073996,7.4286764392330502,7.3745120550885401,7.3119124226099901,6.7255700471847604,6.5611938964302796]
["UP-E2L118C4","UP",7,"E2L118C4",918,"E/L Ratio, All Freight Cars, AVERAGE ALL FREIGHT CARS",1.82564973831177,1.83270907402039,1.8268946409225499,1.8381775617599501,1.79009509086609,1.79565346240997,1.7807048559188801,1.7183419466018699,1.7108733654022199,1.69418819746633,1.67065266554082,1.6913611224109599,1.68898658237762,1.68599420127697,1.67273619606891,1.6703248218322599]
["UP-E2L118C6","UP",7,"E2L118C6",920,"Interline circuity, AVERAGE ALL FREIGHT CARS",1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.157,1.157,1.157,1.157,1.157,1.157,1.157]
["UP-E2L118C9","UP",7,"E2L118C9",923,"CD per Industry Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["UP-E2L118C13","UP",7,"E2L118C13",927,"CD per I&I Switch, AVERAGE ALL FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["UP-E2L118C16","UP",7,"E2L118C16",930,"CD per Load & Unload Interterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["UP-E2L118C19","UP",7,"E2L118C19",933,"CM per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
[{"$f":"B7746&\"-\"&D7746","v":"UP-E2L118C20"},"UP",7,"E2L118C20",934,"CM per Interterminal Switch, AVERAGE ALL FREIGHT CARS",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["UP-E2L118C25","UP",7,"E2L118C25",939,"SEMs per Industry Switch, AVERAGE ALL FREIGHT CARS",6.95050001144409,6.7008547782897896,6.05234718322754,5.7136750221252397,5.2570152282714799,5.3113522529602104,5.1721048355102504,5.2846555709838903,5.1323390007018999,4.9400372401710904,5.0032109906049298,4.9524509594886998,4.9163413700590297,4.8746082817399898,4.48371336478984,4.3741292642868501]
["UP-E2L118C28","UP",7,"E2L118C28",942,"SEMs per Interterminal Switch, AVERAGE ALL FREIGHT CARS",8.3406009674072301,8.0410270690918004,7.2628154754638699,6.8564090728759801,6.3084182739257804,6.3736233711242702,6.2065262794494602,6.3415865898132298,6.1588087081909197,5.9280446882053104,6.0038531887259197,5.9429411513864396,5.8996096440708303,5.8495299380879899,5.3804560377478099,5.2489551171442201]
["UP-E2L202C1","UP",7,"E2L202C1",945,"Average TCUs Per Flat Car",4.8,4.9000000000000004,5.2,5,5,4.9000000000000004,4.8,4.5999999999999996,4.5999999999999996,4.7,4.5999999999999996,4.5,4.5999999999999996,4.5999999999999996,4.5999999999999996,4.5]
["UP-E2L205C1","UP",7,"E2L205C1",948,"Linehaul Miles Per TCU Day",478,478,478,478,478,478,478,478,478,478,478,478,478,478,478,478]
["UP-E2L209C1","UP",7,"E2L209C1",952,"Average Locomotive Units - Way Train",2.2683022022247301,2.2288522720336901,2.1897602081298801,2.1446566581726101,2.16823077201843,2.19650101661682,2.1785149574279798,2.1902434825897199,2.2308363914489702,2.1601638618209198,2.07658270460733,2.1012606903236501,2.1440838097243402,2.0408014343918599,1.87097952474373,1.99202897621682]
["UP-E2L212C1","UP",7,"E2L212C1",955,"Average Gross Tons - Way Train",2104.146484375,1980.28833007813,1931.39514160156,1837.41003417969,2083.75512695313,2110.47485351563,2057.26708984375,2134.75219726563,2166.07495117188,2108.4972639817502,1915.20273539563,2141.6825770683399,2206.7776727349101,2237.2874728101401,2168.3456647491298,2365.6504355407101]
["UP-E2L215C1","UP",7,"E2L215C1",958,"Train Crews (Excl Train Switching)",520893.125,508438.0625,468685.875,379847.125,429694.875,467252.4375,466910,485397.625,535870.25,497736.29377568502,423875.94068211003,434380.89147465699,471163.42176967202,441378.83641197003,366439.36469658301,372855.63264096802]
["UP-E2L216C1","UP",7,"E2L216C1",959,"Total Crew Wages (Excl Train Switching)",1238628.625,1244282.5,1172640,930677.0625,1017886,1099733.75,1108787.75,1131465.5,1249180.25,1181681.3705887501,1012450.46669093,1034867.36729844,1132907.4862717399,1054311.4981674601,880259.90641463106,893002.45024824201]
["UP-E2L301C1","UP",7,"E2L301C1",964,"Residual Factor, Industry Switching, Railroad-Owned",64.613145051565894,70.056927872869494,72.534386588359197,96.432171061863897,89.887635629936298,87.906134540900794,82.692229850478299,80.130048979369519,80.962134604659596,71.603845279093207,66.580642188933595,71.923521807729998,72.827897135432906,64.802916928920098,61.111149679486616,65.608375855223997]
["UP-E2L302C2","UP",7,"E2L302C2",967,"Residual Factor, Station Clerical, Privately-Owned",4.9880564742363198,7.2940459385192202,7.7434675182322996,9.2306890626907503,8.3389948557982994,7.96703696425792,7.7022670857076596,6.9511223804129996,7.5652799324239401,5.05684446399398,4.3754191138360596,4.05196629550223,2.6253534630019901,2.1458980983282601,1.653056859117616,2.6274840901823899]
["UP-E2L304C1","UP",7,"E2L304C1",970,"Residual Factor, I&I Switching, Railroad-Owned",91.419865383711297,98.505578449444201,104.487683575072,136.339033570467,124.133146830803,126.534079452648,116.028790023376,103.76805086163068,104.717518731059,82.315757106194596,75.891693533976195,83.050272842069305,80.345866719677005,67.5269759027465,64.386469353223049,65.600614418545106]
["UP-E2L305C2","UP",7,"E2L305C2",973,"Residual Factor, Mileage, Privately-Owned",14.833838319761201,14.2512117858805,13.3865832847279,15.904264905423,16.674244228026499,18.5093816825852,16.589788430833,-0.7920146794182753,-1.4684888726246801,-0.84091153405300501,-7.4228014041275506E-2,0.42907954414255201,0.36389328529498499,0.46844821009271298,1.3278340241456346,0.91242586780964696]
["WEST-E1L102C1","WEST",9,"E1L102C1",4,"Car Mile (CM) - Other Than Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L103C1","WEST",9,"E1L103C1",7,"Train Mile (TM) - Other Than Crew, OPR Expense",0.44628298282623302,0.48417994379997298,0.50037336349487305,0.497776418924332,0.48278281092643699,0.51629412174224898,0.49699553847312899,0.47951835393905601,0.51189255714416504,0.74799488556456395,0.66357763513999002,0.65346840082284496,0.73211768344833805,0.753007584560763,0.74295990095860598,0.63688697269414296]
["WEST-E1L103C2","WEST",9,"E1L103C2",8,"Train Mile (TM) - Other Than Crew, DRL Expense",4.69148857519031E-3,1.1382878292352E-3,1.6458153259009099E-3,2.9714882839471102E-3,4.0598371997475598E-3,4.4753965921700001E-3,4.1459589265286896E-3,1.44549843389541E-3,-2.7500942815095202E-4,-1.7284623887297999E-3,-2.7757944801895502E-4,-2.9261079292305101E-4,-3.2935035333690402E-4,-1.4774871057089E-3,-2.46006694659317E-4,-3.4287390173140699E-4]
["WEST-E1L104C2","WEST",9,"E1L104C2",11,"Train Mile (TM) - Crew, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L106C1","WEST",9,"E1L106C1",16,"CLOR (Carloads Handled) - Other, OPR Expense",2.35501980781555,2.39695024490356,2.3835704326629599,2.3308396339416499,2.69218826293945,2.49186062812805,2.8084588050842298,2.8022871017456099,2.6880407333374001,3.00157512984579,3.3703098412868102,3.23347101680312,2.8719218510406099,3.0662994823721101,2.8853114783028202,1.6930165994223101]
["WEST-E1L107C1","WEST",9,"E1L107C1",19,"CLOR (Carloads Handled) - Clerical, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L108C1","WEST",9,"E1L108C1",22,"CLOT (Carloads Orig Or Term) - Other, OPR Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"B7810&\"-\"&D7810","v":"WEST-E1L109C1"},"WEST",9,"E1L109C1",25,"CLOT (Carloads Orig Or Term) - Clerical, OPR Expense",11.6525764465332,14.135794639587401,15.099609375,14.764284133911101,14.337231636047401,13.3128509521484,13.3545026779175,12.6697187423706,14.0340366363525,11.6361482896999,11.480227688734001,9.83691611224687,7.4576087429914697,7.0872424343162104,6.2329267855393597,6.92833589137242]
["WEST-E1L110C2","WEST",9,"E1L110C2",29,"Car Mile (CM) - Clerical, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L111C2","WEST",9,"E1L111C2",32,"Switch Engine Minutes (SEM), DRL Expense",0.51731932163238503,0.66012072563171398,0.72954010963439897,0.972709000110626,0.97433638572692904,0.85073655843734697,0.91725116968154896,0.92933666706085205,0.94314241409301802,1.0246886602420699,1.13974909064014,1.2827145944482199,1.3019774133738,1.37254734481876,1.6502100772421899,1.65613308535255]
["WEST-E1L111C3","WEST",9,"E1L111C3",33,"Switch Engine Minutes (SEM), ROI Expense",1.4769196510314899,1.9151957035064699,2.2631311416625999,2.5899350643157999,2.80517506599426,2.7934885025024401,2.7778782844543501,3.0191226005554199,3.0725023746490501,3.34943895888276,3.62120115526734,4.1617737914733901,4.6966681756673099,3.7787397631261901,3.81837847265485,5.0243142132773198]
["WEST-E1L112C3","WEST",9,"E1L112C3",36,"Ton Miles In Lake Transfer Service, ROI Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L114C2","WEST",9,"E1L114C2",41,"Tons Handled at Ore Terminals, DRL Expense",1.2806853279471399E-2,1.3413079082965899E-2,1.4731374569237199E-2,8.8819116353988606E-2,2.4932460859417901E-2,2.0664826035499601E-2,2.9142785817384699E-2,4.5924749225378002E-2,6.76768124103546E-2,8.1136633473998201E-2,0.106957735234173,7.4115015743916102E-2,8.8509106284016301E-2,0.104561229357307,0.17141793813845699,9.6472164292256996E-2]
["WEST-E1L115C2","WEST",9,"E1L115C2",44,"Tons Handled at Other Marine Terminals, DRL Expense",0,0,0,0,0,0,0,8.6281942203640903E-3,8.5788695141673105E-3,1.05425295632282E-2,1.40166630335817E-2,1.5902320113039301E-2,1.51476995384086E-2,1.42500386773137E-2,1.8086612061500501E-2,2.2577126511475198E-2]
["WEST-E1L116C2","WEST",9,"E1L116C2",47,"Refrigerated Car Miles, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L117C2","WEST",9,"E1L117C2",50,"Protective Service Reefer TCU Days, DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L118C3","WEST",9,"E1L118C3",54,"Refrigerated TCU Days, ROI Expense",1.32764307782054E-2,2.07981858402491E-2,2.0024033263325702E-2,1.2293346226215401E-2,1.04976240545511E-2,4.6795718371868099E-3,3.2840105704963199E-3,3.1751592177897703E-4,0.142886817455292,0.131235130055217,0,0.15608446014226901,0.16295078893282,0.123629145595253,8.8461079223372194E-2,0.12710384705993]
["WEST-E1L119C3","WEST",9,"E1L119C3",57,"Other (Non-Refrigerated) TCU Days, ROI Expense",5.1111932843923603E-2,5.50198368728161E-2,6.4802795648574801E-2,6.9819770753383595E-2,5.2277226001024198E-2,4.8244468867778799E-2,3.1731039285659797E-2,2.8679884970188099E-2,6.7171123810112502E-3,5.2833815965519504E-3,4.47639299035167E-2,4.94336491792633E-3,6.0319412498777798E-3,4.3145732525518799E-3,3.6128145229899298E-3,5.4417137735754996E-3]
["WEST-E1L120C1","WEST",9,"E1L120C1",58,"TCUs Loaded And Unloaded (L&UL), OPR Expense",40.959239959716797,43.226730346679702,46.677215576171903,45.064220428466797,45.918212890625,46.351432800292997,47.398181915283203,51.822044372558601,51.548721313476598,53.580176601703798,49.735032398416102,51.9985340719468,53.191562964814501,54.370002386920198,53.806423557498199,56.656876044055501]
["WEST-E1L121C2","WEST",9,"E1L121C2",62,"MVUs Loaded And Unloaded (L&UL), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L122C2","WEST",9,"E1L122C2",65,"TCUs Picked Up and Delivered (PU&D), DRL Expense",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L201C3","WEST",9,"E1L201C3",69,"CM(R), ROI Expense, Railroad-Owned, BOX - 40 FT",3.9450705051422098E-2,4.1769005358219098E-2,4.6374958008527797E-2,3.3283572643995299E-2,3.0054869130253799E-2,2.8917910531163198E-2,2.8656508773565299E-2,3.0695362016558599E-2,2.51835323870182E-2,1.8980010357755199E-2,1.46965859076163E-2,1.8024233169918601E-2,2.0059161028031298E-2,1.6264237127074699E-2,1.37651375221957E-2,1.4984951931502399E-2]
["WEST-E1L201C6","WEST",9,"E1L201C6",72,"CM(Y), ROI Expense, Railroad-Owned, BOX - 40 FT",0.102571949362755,0.108599588274956,0.1205750182271,8.6537130177020999E-2,7.8142561018466894E-2,7.5186595320701599E-2,7.4506819248199505E-2,7.9807922244072002E-2,6.5477132797241197E-2,4.9348026930163401E-2,3.82111233598025E-2,4.6863006241788498E-2,5.2153818672881401E-2,4.22870165303941E-2,3.5789357557708797E-2,3.8960875021906198E-2]
["WEST-E1L201C10","WEST",9,"E1L201C10",76,"CD(Y), OPR Expense, Railroad-Owned, BOX - 40 FT",6.2275519371032697,5.9619197845459002,4.0004863739013699,4.0078654289245597,3.3195121288299601,2.52933669090271,2.7068560123443599,2.8508059978485099,3.2230570316314702,3.6625506102235201,3.6428494643459901,4.5325840807274096,5.1929454465612199,5.7618426141613801,5.4524873969549104,4.2909576057243903]
["WEST-E1L201C13","WEST",9,"E1L201C13",79,"CM(R), DRL Expense, Privately-Owned, BOX - 40 FT",0.241152718663216,0.25780263543129001,0.25665453076362599,0.26563096046447798,0.188191428780556,0.21946595609188099,0.21286860108375499,0.20125770568847701,0.20840331912040699,0.203861420725585,0.242697665177146,0.23841931552640699,0.232453173450754,0.25032030071101902,0.22858040032093099,0.201540791350522]
["WEST-E1L202C3","WEST",9,"E1L202C3",82,"CM(R), ROI Expense, Railroad-Owned, BOX - 50 FT",3.9450705051422098E-2,4.1769005358219098E-2,4.6374958008527797E-2,3.3283572643995299E-2,3.0054869130253799E-2,2.8917910531163198E-2,2.8656508773565299E-2,3.0695362016558599E-2,2.51835323870182E-2,1.8980010357755199E-2,1.46965859076163E-2,1.8024233169918601E-2,2.0059161028031298E-2,1.6264237127074699E-2,1.37651375221957E-2,1.4984951931502399E-2]
["WEST-E1L202C4","WEST",9,"E1L202C4",83,"CM(Y), OPR Expense, Railroad-Owned, BOX - 50 FT",0.123526744544506,0.117112003266811,7.7364176511764499E-2,7.6545946300029796E-2,6.2691465020179707E-2,4.7953158617019702E-2,5.1581144332885701E-2,5.4754313081502901E-2,6.2737852334976196E-2,7.1409341427546305E-2,6.9484996438186702E-2,8.5138655723665899E-2,9.7586570082345295E-2,0.110710161232521,0.105235602233099,8.3654420955203895E-2]
["WEST-E1L202C8","WEST",9,"E1L202C8",87,"CD(R), DRL Expense, Railroad-Owned, BOX - 50 FT",38.864711761474602,44.6516304016113,28.996721267700199,25.017196655273398,28.6526889801025,29.571022033691399,28.395042419433601,24.570020675659201,23.1791172027588,21.020236807589502,17.773114987784201,12.984198902178001,13.5427319760299,14.2905089846889,13.759004618714799,14.617752062116301]
["WEST-E1L202C11","WEST",9,"E1L202C11",90,"CD(Y), DRL Expense, Railroad-Owned, BOX - 50 FT",38.864711761474602,44.6516304016113,28.996721267700199,25.017196655273398,28.6526889801025,29.57102394104,28.395040512085,24.570022583007798,23.179115295410199,21.020236807589502,17.773114987784201,12.984198902178001,13.5427319760299,14.2905089846889,13.759004618714799,14.617752062116301]
["WEST-E1L203C2","WEST",9,"E1L203C2",94,"CM(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED",4.0779016911983497E-2,4.24895472824574E-2,4.5804940164089203E-2,5.08489497005939E-2,4.9552291631698601E-2,4.7583319246769E-2,4.5372039079666103E-2,4.81592118740082E-2,4.2558401823043802E-2,4.01687724904728E-2,3.3801131905137602E-2,3.0185111608362899E-2,2.6254824329016199E-2,2.73409269231361E-2,2.61147143995599E-2,2.0711743639556301E-2]
["WEST-E1L203C5","WEST",9,"E1L203C5",97,"CM(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED",0.106025472283363,0.110472939908504,0.119092755019665,0.13220724463462799,0.12883584201335899,0.123716503381729,0.117967449128628,0.12521396577358199,0.110651783645153,0.104438808475229,8.7882942953357801E-2,7.8481290181743504E-2,6.8262543255442107E-2,7.1086410000153602E-2,6.7898257438855206E-2,5.3850533462846302E-2]
["WEST-E1L203C9","WEST",9,"E1L203C9",101,"CD(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED",1.6522744894027701,1.6193976402282699,1.61142194271088,1.8603665828704801,2.1543278694152801,1.8184461593627901,2.4005417823791499,2.94694852828979,2.3201220035553001,1.3522471461969501,2.06639183911996,3.12230280700261,2.9682511800786502,2.6832544778991099,2.3892105058199902,2.5859440999602299]
["WEST-E1L203C12","WEST",9,"E1L203C12",104,"CD(Y), ROI Expense, Railroad-Owned, BOX - EQUIPPED",1.6522746086120601,1.6193976402282699,1.61142194271088,1.8603667020797701,2.1543278694152801,1.8184460401535001,2.4005417823791499,2.9469482898712198,2.3201220035553001,1.3522471461969501,2.06639183911996,3.12230280700261,2.9682511800786502,2.6832544778991099,2.3892105058199902,2.5859440999602299]
["WEST-E1L204C2","WEST",9,"E1L204C2",107,"CM(R), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",5.1404945552349099E-3,5.5810865014791497E-3,5.2719158120453401E-3,4.2555374093353696E-3,4.05670842155814E-3,4.2507406324148204E-3,3.2347384840249998E-3,5.2002994343638403E-3,7.0897494442760901E-3,7.2617501802482304E-3,8.0464265564752502E-3,5.9482533151689202E-3,4.5978664697790799E-4,8.4530560658001193E-3,3.4481732515365899E-3,1.8757145033716999E-3]
["WEST-E1L204C3","WEST",9,"E1L204C3",108,"CM(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN",6.3580060377717001E-3,5.5274330079555503E-3,5.4237581789493604E-3,4.2859376408159698E-3,4.0542595088481903E-3,5.7745561935007598E-3,7.4039688333868998E-3,8.9850518852472305E-3,1.1738082394003899E-2,1.0709596422396999E-2,1.1034734336768E-2,1.09482713477851E-2,1.3103102213930601E-2,1.2021972228100201E-2,1.1531897663933401E-2,1.49225139117441E-2]
["WEST-E1L204C7","WEST",9,"E1L204C7",112,"CD(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN",3.7077522277832,3.7072632312774698,4.1550846099853498,4.3986392021179199,4.4790573120117196,4.6694102287292498,5.3308420181274396,5.1278505325317401,5.2155470848083496,5.4493138804734,5.3466463154617596,4.8666490175956998,4.3051296470800704,4.7878360643227396,5.4522645132824401,5.0599012551205202]
["WEST-E1L204C11","WEST",9,"E1L204C11",116,"CD(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN",3.0706701278686501,2.9237656593322798,3.1189935207366899,3.1280221939086901,2.8628089427947998,3.0266540050506601,3.5806872844696001,3.9578583240509002,3.378262758255,3.2921615535233499,3.0214494034706698,2.8772363536421199,2.1122590039139202,2.9254354064502199,2.9143394194945702,2.7163250101039602]
["WEST-E1L205C1","WEST",9,"E1L205C1",119,"CM(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",4.9481686204671901E-2,5.7043988257646602E-2,5.8918830007314703E-2,6.7975617945194203E-2,5.7623855769634198E-2,5.5350363254547098E-2,5.2403029054403298E-2,4.8335779458284399E-2,4.5619305223226499E-2,5.0538746051245802E-2,5.1642042633999199E-2,5.0726022467766599E-2,4.5458034249470002E-2,4.4000054856382802E-2,4.4200556045309203E-2,4.1864556015760598E-2]
["WEST-E1L205C4","WEST",9,"E1L205C4",122,"CM(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED",0.12865214049816101,0.14831449091434501,0.15318888425826999,0.17673648893833199,0.14982183277607,0.14391088485717801,0.136247873306274,0.12567305564880399,0.11861017346382099,0.13140073973323901,0.13426931084839799,0.13188765841619299,0.118190889048622,0.11440014262659499,0.11492144571780399,0.10884784564097801]
["WEST-E1L205C8","WEST",9,"E1L205C8",126,"CD(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",16.471559524536101,18.8919467926025,18.278413772583001,24.5241394042969,20.174085617065401,18.680934906005898,22.9874458312988,24.0026245117188,23.281471252441399,28.492149666108102,24.686798552748201,19.891204931876,19.603480965250501,20.990167252998301,19.841800740253898,17.615122481509701]
["WEST-E1L205C11","WEST",9,"E1L205C11",129,"CD(Y), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED",16.4715576171875,18.891944885253899,18.278415679931602,24.5241374969482,20.174085617065401,18.680934906005898,22.9874458312988,24.002620697021499,23.281471252441399,28.492149666108102,24.686798552748201,19.891204931876,19.603480965250501,20.990167252998301,19.841800740253898,17.615122481509601]
["WEST-E1L206C1","WEST",9,"E1L206C1",132,"CM(R), OPR Expense, Railroad-Owned, HOPPER - COVERED",3.5339180380106E-2,3.9406705647706999E-2,4.2414236813783597E-2,4.7693438827991499E-2,4.3455645442009E-2,4.4488709419965702E-2,4.5905210077762597E-2,4.6219341456890099E-2,4.6809889376163497E-2,4.7397226398394499E-2,4.4137525510314399E-2,4.1119594816250701E-2,3.7444272089040498E-2,3.7893780171579697E-2,3.62631717628236E-2,3.3299107981417601E-2]
["WEST-E1L206C2","WEST",9,"E1L206C2",133,"CM(R), DRL Expense, Railroad-Owned, HOPPER - COVERED",1.41375069506466E-3,1.1083009885624101E-3,2.8101750649511801E-3,3.6098973359912599E-3,2.8865510830655699E-4,2.8692060150206102E-3,3.8929176516830899E-3,3.95352346822619E-3,2.5635540951043402E-3,2.28301231674741E-3,2.0853538181066899E-3,2.4622873084083801E-3,2.12522284073856E-4,-1.8777597681932099E-3,-2.8826622959303599E-3,-9.4949203518043801E-4]
["WEST-E1L206C6","WEST",9,"E1L206C6",137,"CM(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED",3.1918555498123197E-2,4.29964624345303E-2,4.4757440686225898E-2,4.5285318046808201E-2,4.2762670665979399E-2,4.9695670604705797E-2,5.7165000587701797E-2,6.3787333667278304E-2,5.6300450116395999E-2,5.7445808224148798E-2,4.7279421127060801E-2,5.6435888235567201E-2,7.2665867231439196E-2,6.3510694311867899E-2,4.9409390293334299E-2,6.1750325680933901E-2]
["WEST-E1L206C10","WEST",9,"E1L206C10",141,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED",3.92578029632568,4.4444866180419904,4.8413343429565403,5.5333600044250497,5.0743455886840803,5.2146525382995597,5.3771605491638201,5.3877191543579102,5.4624600410461399,5.5794631434709103,5.2789996578921699,4.98821393178374,4.6318850096094897,4.7080482125836696,4.5950054527544504,4.1926106668546304]
["WEST-E1L206C13","WEST",9,"E1L206C13",144,"CM(R), DRL Expense, Privately-Owned, HOPPER - COVERED",3.75213623046875E-2,3.8303494453430197E-2,3.6039788275957101E-2,3.8291528820991502E-2,3.2202415168285398E-2,3.1184025108814201E-2,3.04815582931042E-2,2.9764834791421901E-2,2.59022898972034E-2,2.69815193495225E-2,2.6999837507642999E-2,2.2584208775490201E-2,2.1880977336752899E-2,2.4540876056971899E-2,2.3065124688367501E-2,2.33260527862378E-2]
["WEST-E1L207C3","WEST",9,"E1L207C3",147,"CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",1.3638587668538101E-2,1.5157662332058E-2,1.43781462684274E-2,2.0306847989559201E-2,1.68187227100134E-2,1.2494202703237501E-2,9.3492176383733697E-3,1.09952567145228E-2,1.28806876018643E-2,2.28249239045131E-2,2.5090104743865201E-2,2.3989462275018199E-2,2.6231889171349498E-2,2.8415626533093801E-2,2.9864302770229501E-2,3.6428448535503997E-2]
["WEST-E1L207C7","WEST",9,"E1L207C7",151,"CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",4.6657142639160201,5.7310376167297399,7.3667082786560103,8.3374404907226598,7.1967134475707999,4.9122815132141104,4.6083412170410201,4.8805184364318803,5.0149393081665004,4.8605808216280604,4.1335147259788103,3.7161302759648098,3.5079596498587202,3.9861507999225898,4.6321986385482203,5.00986693481331]
["WEST-E1L207C10","WEST",9,"E1L207C10",154,"CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",4.6657147407531703,5.7310376167297399,7.3667082786560103,8.3374404907226598,7.1967139244079599,4.9122815132141104,4.6083407402038601,4.8805179595947301,5.0149402618408203,4.8605808216280604,4.1335147259788103,3.7161302759648098,3.5079596498587202,3.9861507999225898,4.6321986385482301,5.00986693481331]
["WEST-E1L207C13","WEST",9,"E1L207C13",157,"CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - GENERAL",7.3341056122444597E-5,3.9766197005519603E-5,2.9689277653233101E-5,1.0363461115048301E-5,7.9588580410927502E-4,3.42062849085778E-4,9.9958782084286191E-4,1.0718958219513299E-3,8.7139179231598995E-4,8.3894785460358098E-4,4.31395714574894E-3,1.64065537815164E-3,9.3327893101443E-4,1.38157796186714E-4,1.4640909045006899E-5,6.1360996982716104E-6]
["WEST-E1L208C1","WEST",9,"E1L208C1",158,"CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",3.1243290752172501E-2,3.4871473908424398E-2,3.3686518669128397E-2,3.6721911281347303E-2,2.97226421535015E-2,2.6497144252061799E-2,2.6030749082565301E-2,2.8579343110323001E-2,3.5293009132146801E-2,3.9153295703585299E-2,3.78637936423913E-2,3.3563454940299997E-2,3.0151353756634702E-2,3.1687191878460703E-2,3.4860529732518998E-2,3.6474222122875002E-2]
["WEST-E1L208C5","WEST",9,"E1L208C5",162,"CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",6.9308327510953002E-3,9.8708271980285592E-3,2.8359554708004002E-3,-1.66289061307907E-2,-1.73400025814772E-2,-1.08685716986656E-2,2.31566443108022E-3,7.0312106981873504E-3,6.8059605546295599E-3,7.3660042163287802E-3,1.1069453768988199E-2,5.9544584669586698E-3,-1.90339410033925E-3,-2.8037481929174802E-3,2.3008178784786801E-3,5.6517223704236402E-3]
["WEST-E1L208C9","WEST",9,"E1L208C9",166,"CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.60432636737823497,0.74291521310806297,0.75707131624221802,0.90210843086242698,0.96477264165878296,1.1856005191803001,1.7759807109832799,1.64932060241699,1.5436041355133101,1.77191088324012,1.8093269099910301,1.71143591073938,1.9588684112855801,1.2541595735362101,1.5925314928157299,1.6680870991285299]
["WEST-E1L208C12","WEST",9,"E1L208C12",169,"CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",0.60432636737823497,0.74291515350341797,0.75707131624221802,0.90210843086242698,0.96477276086807295,1.1856003999710101,1.7759807109832799,1.6493204832077,1.5436041355133101,1.77191088324012,1.8093269099910301,1.71143591073938,1.9588684112855801,1.2541595735362101,1.5925314928157299,1.6680870991285299]
["WEST-E1L209C2","WEST",9,"E1L209C2",172,"CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH",-2.5972103700041799E-2,-2.6261273771524402E-2,-2.49313414096832E-2,-2.6002027094364201E-2,-2.96895485371351E-2,-2.4675171822309501E-2,-2.3114614188671102E-2,-2.34259404242039E-2,-1.7827792093157799E-2,-1.0209002185749501E-2,1.06235643639378E-2,1.04470693755499E-2,3.3322498524994298E-3,8.0248837307856005E-3,2.0452185986336101E-2,3.5179946301864398E-2]
["WEST-E1L209C6","WEST",9,"E1L209C6",176,"CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",2.8997544199228301E-2,2.2523032501339899E-2,2.0079547539353398E-2,1.6593430191278499E-2,2.4123059585690498E-2,3.6363899707794203E-2,4.8225805163383498E-2,0.11424165964126599,0.118488021194935,0.16276177495584199,0.19455296195816099,0.21482501777361099,0.235060112608211,0.18594776762703399,0.27567812090452198,0.39963052215743899]
["WEST-E1L209C9","WEST",9,"E1L209C9",179,"CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - MECH",2.3195042610168501,1.82400298118591,1.6327427625656099,1.4187932014465301,2.0268471240997301,2.9660894870758101,4.1517171859741202,9.6981401443481392,9.6765375137329102,13.986389435234599,17.020503729742,18.473546228379998,20.595849887428301,15.992136161926901,24.394786649933501,34.318603688539703]
["WEST-E1L209C10","WEST",9,"E1L209C10",180,"CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH",16.5186672210693,9.6719875335693395,5.0944809913635298,6.2844257354736301,9.7568922042846697,13.004005432128899,12.035825729370099,13.246542930603001,18.5515251159668,25.3082941771357,26.363531031065101,23.063296406688401,20.957335325739798,22.936631739712301,23.693265287432901,17.2307147951689]
["WEST-E1L209C13","WEST",9,"E1L209C13",183,"CM(R), DRL Expense, Privately-Owned, REFRIGERATED - MECH",7.12515180930495E-3,1.1036193463951299E-3,3.21391550824046E-3,5.0343276234343605E-4,9.8361819982528708E-4,7.1189895970746896E-4,8.8639213936403405E-4,3.4781752037815798E-4,1.32896902505308E-3,3.9134411713082301E-4,4.6815473544930403E-4,6.5648843278026095E-4,7.02276994498786E-4,6.7938145774834298E-4,7.6907352627534199E-4,6.0245595957216197E-4]
["WEST-E1L210C4","WEST",9,"E1L210C4",187,"CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH",3.3316586166620303E-2,3.5059161484241499E-2,3.9115708321332897E-2,5.6731402873992899E-2,8.0196738243103E-2,0.110903710126877,0.111555270850658,0.116075083613396,0.13497056066989899,0.149211395983186,0.134123229918228,0.121638760225149,0.126935376579799,0.14391864227408399,0.12626630228136701,0.109110066491274]
["WEST-E1L210C8","WEST",9,"E1L210C8",191,"CD(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",9.9615230560302699,8.9916362762451207,10.7489070892334,13.9053544998169,17.951845169067401,16.514625549316399,19.280015945434599,17.299415588378899,13.3293600082397,14.7364801833359,16.874147519091402,16.191758573587901,25.5866709291668,31.112828141736902,16.322751297463,13.4263060185525]
["WEST-E1L210C11","WEST",9,"E1L210C11",194,"CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH",9.9615230560302699,8.9916353225708008,10.7489070892334,13.9053544998169,17.951845169067401,16.514625549316399,19.280015945434599,17.299415588378899,13.3293600082397,14.7364801833359,16.874147519091402,16.191758573587901,25.5866709291668,31.112828141736902,16.322751297463,13.4263060185525]
["WEST-E1L211C1","WEST",9,"E1L211C1",197,"CM(R), OPR Expense, Railroad-Owned, FLAT - TOFC",8.3244899287819897E-3,8.0517465248704009E-3,8.0235181376338005E-3,9.1630490496754594E-3,8.3051249384880101E-3,7.7913478016853298E-3,6.88176462426782E-3,6.7695928737521198E-3,7.6533309184014797E-3,9.7903349846761092E-3,1.0863710144705699E-2,1.27175277114926E-2,1.56451142458876E-2,1.9230873590971399E-2,2.18247328188616E-2,2.2776746344264898E-2]
["WEST-E1L211C5","WEST",9,"E1L211C5",201,"CM(Y), DRL Expense, Railroad-Owned, FLAT - TOFC",3.54720316827297E-2,3.36704179644585E-2,3.51080521941185E-2,3.5769723355770097E-2,3.8071282207965899E-2,3.4960325807332999E-2,3.3883802592754399E-2,5.4227545857429497E-2,6.03297613561153E-2,6.4664046853430704E-2,6.1277158042707301E-2,5.43725695015288E-2,2.1982671983252499E-2,3.2620534600622197E-2,3.4112616923289901E-2,3.0935496214206801E-2]
["WEST-E1L211C8","WEST",9,"E1L211C8",204,"CD(R), DRL Expense, Railroad-Owned, FLAT - TOFC",14.1609554290771,14.243920326232899,14.623663902282701,16.363632202148398,14.3900699615479,13.6710157394409,12.168206214904799,15.394788742065399,11.3719425201416,8.7906091259927006,7.3883070507194502,4.5155220806887204,9.5898114227319002,9.4341295143146198,9.0257198703298105,8.1402035532288703]
["WEST-E1L211C9","WEST",9,"E1L211C9",205,"CD(R), ROI Expense, Railroad-Owned, FLAT - TOFC",0.10936726629734,0.132526114583015,0.36105254292488098,0.96155744791030895,0.80600827932357799,1.58223092556,1.73767185211182,2.08140897750854,1.8449083566665601,1.68417309631074,1.60612246191451,2.2090656879335402,2.8974642035178402,2.21974783752436,1.8758444686769,2.6780419323396298]
["WEST-E1L211C12","WEST",9,"E1L211C12",208,"CD(Y), ROI Expense, Railroad-Owned, FLAT - TOFC",0.10936726629734,0.132526099681854,0.36105257272720298,0.96155756711959794,0.80600827932357799,1.58223104476929,1.73767185211182,2.08140897750854,1.8449083566665601,1.68417309631074,1.60612246191451,2.2090656879335402,2.8974642035178402,2.21974783752436,1.8758444686769,2.6780419323396298]
["WEST-E1L212C3","WEST",9,"E1L212C3",212,"CM(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL",6.45885840058327E-2,7.8489765524864197E-2,0.107714936137199,0.12997125089168499,0.128752276301384,0.125866174697876,0.104144036769867,0.10460782796144499,0.144369706511497,0.147870048044147,0.166982440368625,0.173764732257151,0.18532582685978399,0.13771709440580501,0.13385060871051499,0.18069998022577599]
["WEST-E1L212C7","WEST",9,"E1L212C7",216,"CD(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",0.27420276403427102,0.23306095600128199,0.35544613003730802,0.96528512239456199,1.2951914072036701,1.62542057037354,1.67331659793854,2.23657321929932,2.5645833015441899,2.6558402314710401,2.4597925989884701,2.4058539440927,2.1524320117137901,2.2397786582122801,2.2605343415550201,2.3551585646806901]
["WEST-E1L212C10","WEST",9,"E1L212C10",219,"CD(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL",0.27420276403427102,0.23306095600128199,0.35544613003730802,0.96528506278991699,1.2951914072036701,1.62542057037354,1.67331671714783,2.23657298088074,2.5645830631256099,2.6558402314710401,2.4597925989884701,2.4058539440927,2.1524320117137901,2.2397786582122801,2.2605343415550201,2.3551585646806901]
["WEST-E1L212C13","WEST",9,"E1L212C13",222,"CM(R), DRL Expense, Privately-Owned, FLAT - MULTILEVEL",0.12524877488613101,0.13883304595947299,0.17170687019825001,0.23439812660217299,0.17726399004459401,0.15763662755489299,0.141272813081741,0.15551437437534299,0.166743978857994,0.16138755002961799,0.175532718696507,0.19269736245556399,0.200446500711572,0.19881814251254301,0.23656812945758901,0.22984145298303699]
["WEST-E1L213C4","WEST",9,"E1L213C4",226,"CM(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL",2.1439685821533199,2.8601014614105198,3.3451592922210698,4.9166784286498997,6.0262937545776403,6.8168630599975604,6.04260158538818,2.89455914497375,1.4249418973922701,0.212062536017499,0.231334674821144,0.308632606535509,0.35860080315133902,0.58032384823746996,0.67873484089151603,0.68386526393463898]
["WEST-E1L213C7","WEST",9,"E1L213C7",229,"CD(R), OPR Expense, Railroad-Owned, FLAT - GENERAL",97.313941955566406,131.66954040527301,157.66227722168,226.790115356445,261.73568725585898,269.5341796875,225.67822265625,110.42254638671901,55.5662841796875,9.1455933350942402,10.646203842254,14.959728738944801,17.435110434577901,26.965687455813502,30.4370434474646,29.895884070522001]
["WEST-E1L213C11","WEST",9,"E1L213C11",233,"CD(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL",18.372888565063501,19.7739067077637,26.942438125610401,24.195907592773398,27.4114875793457,23.630126953125,22.7754306793213,2.0450375080108598,7.9922208786010698,12.7867945303596,-11.9587108663479,18.343426404728401,25.693644857247001,26.280233823457401,17.467723524715801,17.227613552418401]
["WEST-E1L213C12","WEST",9,"E1L213C12",234,"CD(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL",11.6537408828735,13.9135847091675,14.0259799957275,15.6149740219116,15.459551811218301,14.123682975769,11.437793731689499,6.9785580635070801,6.9187746047973597,6.2013478851478601,7.9979365369441098,7.8470405813923803,8.3967284831756803,198.00314915445901,4.8779170900150204,6.16848754695169]
["WEST-E1L214C2","WEST",9,"E1L214C2",237,"CM(R), DRL Expense, Railroad-Owned, FLAT - OTHER",4.0678407996892901E-2,3.9814475923776599E-2,4.5665752142667798E-2,4.7265000641345999E-2,3.9605263620614999E-2,4.1171927005052601E-2,4.0771782398223898E-2,3.6907304078340503E-2,2.94522270560265E-2,3.2309933448184898E-2,3.4016244590083997E-2,3.3045192697381501E-2,3.4599286194345699E-2,3.5942014476739101E-2,3.5959636977184198E-2,3.1735165959255102E-2]
["WEST-E1L214C6","WEST",9,"E1L214C6",241,"CM(Y), ROI Expense, Railroad-Owned, FLAT - OTHER",2.1973581984639199E-2,4.27035205066204E-2,4.9450092017650597E-2,3.42120751738548E-2,2.51802019774914E-2,3.93259674310684E-2,2.41397880017757E-2,3.1035957857966399E-2,2.6710269972681999E-2,2.1942333113811E-2,1.85462254546797E-2,2.2097334452789E-2,2.81910490340085E-2,2.4362086087956699E-2,2.1191081700188401E-2,2.5118173128390001E-2]
["WEST-E1L214C9","WEST",9,"E1L214C9",244,"CD(R), ROI Expense, Railroad-Owned, FLAT - OTHER",1.4383901357650799,2.7770950794220002,3.1966173648834202,2.3828365802764901,1.5609258413314799,2.3445508480071999,1.3393689393997199,1.8713915348053001,1.6487399339675901,1.4470571595391,1.2910724711030801,1.4883554757392401,1.90734945159755,1.6822991064867601,1.42954139342672,1.49315002819009]
["WEST-E1L214C13","WEST",9,"E1L214C13",248,"CM(R), DRL Expense, Privately-Owned, FLAT - OTHER",1.8780918791890099E-2,0.207417592406273,0.22997313737869299,0.26374202966690102,0.24186284840107,0.23153719305992099,0.22729532420635201,0.23234805464744601,0.237826153635979,0.24095616653304,0.234778860123699,0.25371473854034299,0.26359784782273199,0.313421161317539,0.27381054362380602,0.26185006873011002]
["WEST-E1L215C3","WEST",9,"E1L215C3",251,"CM(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L215C6","WEST",9,"E1L215C6",254,"CM(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L215C10","WEST",9,"E1L215C10",258,"CD(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L215C11","WEST",9,"E1L215C11",259,"CD(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L216C1","WEST",9,"E1L216C1",262,"CM(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L216C5","WEST",9,"E1L216C5",266,"CM(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L216C8","WEST",9,"E1L216C8",269,"CD(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L216C12","WEST",9,"E1L216C12",273,"CD(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L217C2","WEST",9,"E1L217C2",276,"CM(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",5.1810233853757399E-3,1.1401622556149999E-2,2.09347754716873E-2,1.3852537609636799E-2,4.0541337803006198E-3,5.5918092839419798E-3,4.07369947060943E-3,9.8146107047796197E-3,8.9376969262957608E-3,6.4598572592909506E-2,9.0728242215758398E-2,7.7616272780208995E-2,5.4018226161798702E-2,0.108777059906791,0.185238370712005,0.12652572971475301]
["WEST-E1L217C5","WEST",9,"E1L217C5",279,"CM(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",1.3470657169818901E-2,2.9644226655363998E-2,5.4430413991212803E-2,3.6016587167978301E-2,1.05407442897558E-2,1.4538702555000799E-2,1.0591615922748999E-2,2.5517987087369E-2,2.3238006979227101E-2,0.16795628874156501,0.235893429760972,0.201802309228543,0.14044738802067699,0.28282035575765502,0.48161976385121202,0.32896689725835698]
["WEST-E1L217C9","WEST",9,"E1L217C9",283,"CD(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",0.38524600863456698,0.769140005111694,1.1602022647857699,0.94522231817245495,0.53990006446838401,0.456368267536163,0.46435335278510997,1.33242511749268,1.0095076560974099,1.09110282006651,0.34850073112712598,0.32291700872078399,0.33587076316756398,0.77640080819375201,0.55839035584936703,0.73810591487715305]
["WEST-E1L217C10","WEST",9,"E1L217C10",284,"CD(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS",5.8668532371520996,7.3299212455749503,9.5682392120361293,11.205692291259799,8.3426256179809606,6.70818996429443,5.9125270843505904,6.1796622276306197,7.1789140701293901,8.2063397500692705,8.5401103794888105,7.9410384606012601,7.1501292928145697,10.611768248385101,15.5340593541122,27.948471143889101]
["WEST-E1L218C1","WEST",9,"E1L218C1",288,"CM(R), OPR Expense, Railroad-Owned, AUTO RACKS",2.3919898085296202E-3,1.1364703532308301E-3,1.5848026378080199E-3,3.62268439494073E-3,3.1959475018084002E-3,2.29087681509554E-3,0,0,0,0,0,0,4.4691771424739801E-4,1.3135790843924E-3,1.6454435365259501E-3,1.4186293226074701E-3]
["WEST-E1L218C4","WEST",9,"E1L218C4",291,"CM(Y), OPR Expense, Railroad-Owned, AUTO RACKS",6.2191719189286197E-3,2.9548224993050098E-3,4.1204853914678097E-3,9.4189764931797999E-3,8.3094667643308605E-3,5.9562781825661703E-3,0,0,0,0,0,0,1.16198605704323E-3,3.4153056194202399E-3,4.2781531949674604E-3,3.6884362387794301E-3]
["WEST-E1L218C7","WEST",9,"E1L218C7",294,"CD(R), OPR Expense, Railroad-Owned, AUTO RACKS",0.10575807094574,5.07092475891113E-2,7.1391046047210693E-2,0.173939108848572,0.157831445336342,0.114931546151638,0,0,0,0,0,0,2.6618069989264099E-2,8.3550772388942707E-2,0.109278251555479,9.1978884447345796E-2]
["WEST-E1L218C11","WEST",9,"E1L218C11",298,"CD(Y), DRL Expense, Railroad-Owned, AUTO RACKS",8.5294666290283203,6.1657543182373002,5.4071478843689,14.5077409744263,4.9339704513549796,4.5473694801330602,5.4402136802673304,4.28717041015625,11.6884098052979,16.303258968376799,24.524296874475802,26.5875917767349,22.834661199254501,14.588582450442299,17.933678520904799,18.034068542542499]
["WEST-E1L219C1","WEST",9,"E1L219C1",301,"CM(R), OPR Expense, Railroad-Owned, ACCESSORIAL",3.19763748848345E-5,5.7458430092083297E-5,7.0127389335539206E-5,7.8843644587323097E-5,4.1012965084519197E-5,4.2710093111963902E-5,7.5241056038066704E-5,1.01131707197055E-4,1.07294872577768E-4,1.03946356414612E-4,9.4497459147668101E-5,6.5466295211800602E-5,2.51752908590738E-5,3.2778099599331902E-6,0,0]
["WEST-E1L219C4","WEST",9,"E1L219C4",304,"CM(Y), OPR Expense, Railroad-Owned, ACCESSORIAL",8.3138562331441803E-5,1.4939166430849601E-4,1.8233133596368099E-4,2.04993251827545E-4,1.06633626273833E-4,1.1104618897661601E-4,1.9562672241590901E-4,2.6294242707081101E-4,2.7896658866666301E-4,2.7026052667798999E-4,2.4569339378393797E-4,1.7021236755068099E-4,6.5455756233591904E-5,8.5223058958263006E-6,0,0]
["WEST-E1L219C6","WEST",9,"E1L219C6",306,"CM(Y), ROI Expense, Railroad-Owned, ACCESSORIAL",3.5498061333782998E-4,5.1580340368673205E-4,8.2230591215193304E-4,4.9861770821735295E-4,1.8557631410658401E-3,1.87522557098418E-3,1.78959767799824E-3,2.16639693826437E-3,2.1952253300696598E-3,2.29486274095431E-3,2.3035866280960702E-3,2.7445646435904402E-3,2.4764573027187698E-3,2.1171747754578402E-3,1.75852348568479E-3,2.3888578186325301E-3]
["WEST-E1L219C9","WEST",9,"E1L219C9",309,"CD(R), ROI Expense, Railroad-Owned, ACCESSORIAL",2.2752886638045301E-2,3.4126859158277498E-2,5.4701801389455802E-2,3.4482907503843301E-2,0.129058763384819,0.12786966562271099,0.120465964078903,0.137649595737457,0.13496108353138001,0.146586050435767,0.15038613501412601,0.17698869897762701,0.163227890423746,0.136857741607807,0.11724451852309301,0.15188159942736401]
["WEST-E1L219C13","WEST",9,"E1L219C13",313,"CM(R), DRL Expense, Privately-Owned, ACCESSORIAL",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L220C3","WEST",9,"E1L220C3",316,"CM(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.0149234905838999E-2,1.19794504716992E-2,1.26455305144191E-2,1.31427962332964E-2,1.26156732439995E-2,1.42447454854846E-2,1.5646373853087401E-2,1.9943738356232601E-2,1.99708566069603E-2,2.0163039018020499E-2,1.90988121745309E-2,2.2067612726978499E-2,2.7209649915601299E-2,2.3318712506568001E-2,2.03757104094189E-2,2.61183395648815E-2]
["WEST-E1L220C6","WEST",9,"E1L220C6",319,"CM(Y), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.5480540245771401E-2,4.3095897883176797E-2,4.6039368957281099E-2,4.6377908438444103E-2,4.6966359019279501E-2,4.9878675490617801E-2,5.1899634301662403E-2,6.3591599464416504E-2,6.4528226852417006E-2,7.9145748890076098E-2,6.9961842909499805E-2,7.5329781535116699E-2,8.8055470157575699E-2,7.2529354997773396E-2,6.35432799611136E-2,8.2587780282381298E-2]
["WEST-E1L220C10","WEST",9,"E1L220C10",323,"CD(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS",3.63403272628784,4.0015673637390101,4.5449976921081499,6.0187625885009801,4.7480616569518999,4.4441761970520002,4.6499147415161097,4.9180703163146999,4.9974088668823198,5.4330080601608204,5.4228503208685197,5.0011830610885797,4.8246643163492697,5.2527357839952904,5.4223729961671703,4.6537900433610604]
["WEST-E1L220C13","WEST",9,"E1L220C13",326,"CM(R), DRL Expense, Privately-Owned, AVERAGE ALL FREIGHT CARS",4.5696020126342801E-2,4.3885484337806702E-2,4.2518414556980098E-2,4.1107874363660799E-2,4.0357585996389403E-2,4.0804199874401099E-2,4.2570598423481001E-2,4.22210358083248E-2,4.3962951749563203E-2,4.6214450886888303E-2,5.1139030290882702E-2,5.3079813743837502E-2,5.4993798844046503E-2,5.6022320210770103E-2,6.0314465589979799E-2,5.87865454229674E-2]
["WEST-E1L221C3","WEST",9,"E1L221C3",329,"CM(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",6.45885840058327E-2,7.8489765524864197E-2,0.107714936137199,0.12997125089168499,0.128752276301384,0.125866174697876,0.104144036769867,0.10460782796144499,0.144369706511497,0.147870048044147,0.166982440368625,0.173764732257151,0.18532582685978399,0.13771709440580501,0.13385060871051499,0.18069998022577599]
["WEST-E1L221C5","WEST",9,"E1L221C5",331,"CM(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",0.24250075221061701,0.27387788891792297,0.28863298892974898,0.341759532690048,0.235037371516228,0.218890905380249,0.16647991538047799,0.11657588183879899,0.14562700688839,0.21631382906874699,0.32868977079029299,0.33779812649285201,0.27114422135688099,0.21071786609339199,0.23145320652672599,0.240548323791584]
["WEST-E1L221C8","WEST",9,"E1L221C8",334,"CD(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",13.430402755737299,11.0383453369141,13.7644605636597,25.786808013916001,13.574755668640099,11.0293884277344,10.994553565979,12.118522644043001,19.142940521240199,17.606202123951199,30.453585978788499,34.611098870153,29.648698366251999,20.130481354089799,25.3637720935698,26.626046025023602]
["WEST-E1L221C12","WEST",9,"E1L221C12",338,"CD(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL",4.1286535263061497,5.19968461990356,7.5926394462585396,10.3661251068115,9.2618455886840803,9.2474937438964808,7.7635250091552699,10.857215881347701,13.7437906265259,13.373060081569999,13.570995856484799,14.897711927360399,17.955470541814002,13.6464353427685,13.4234287557942,16.3393740595391]
["WEST-E1L302C1","WEST",9,"E1L302C1",341,"L&D Expense, GRAIN",2.6387264952063599E-2,2.4945870041847201E-2,3.6727432161569602E-2,3.52221131324768E-2,2.7508964762091598E-2,4.8060111701488502E-2,2.2179268300533302E-2,3.1123021617531801E-2,3.6137115210294703E-2,3.1673053208722303E-2,2.06520373319149E-2,3.17940606104282E-2,2.12862621972436E-2,1.6299519112691799E-2,1.6646101782829398E-2,1.6986060104260001E-2]
["WEST-E1L305C1","WEST",9,"E1L305C1",344,"L&D Expense, FRESH VEGETABLES",0.60301697254180897,0.243790358304977,0.41229620575904802,0.19410522282123599,7.3158152401447296E-2,0.65559387207031306,0.35545039176940901,0.20792415738105799,0.48678919672965998,0.41470897303029602,0.34160943933107601,0.389577076844837,0.26595492810377602,0.63672310190342996,0.200726594272612,0.51497044391303703]
["WEST-E1L309C1","WEST",9,"E1L309C1",348,"L&D Expense, NONMETALLIC MINERALS",6.1751324683427802E-3,6.0367635451257203E-3,6.24764291569591E-3,1.1238164268434001E-2,1.2882996350526799E-2,1.0773151181638199E-2,1.14579824730754E-2,5.6324019096791701E-3,5.2316985093057199E-3,7.1841635102270198E-3,1.9460853891206499E-3,2.9566385317463602E-3,2.6945083219701502E-3,3.9923515321203399E-3,1.2879584932098101E-3,2.5697714472261999E-3]
["WEST-E1L312C1","WEST",9,"E1L312C1",351,"L&D Expense, DAIRY PRODUCTS",0.26197466254234297,1.34666740894318,1.7574552297592201,0.46422058343887301,0.35715392231941201,0.464790970087051,0.49275985360145602,0.75572431087493896,1.05871522426605,2.0809273501940702,0.96986246387669905,0.98166953399452095,2.6580326093429498,4.3113833540049997,3.8502678120262801,1.82206074815941]
["WEST-E1L315C1","WEST",9,"E1L315C1",354,"L&D Expense, FLOUR",3.2923668622970602E-2,7.6696105301380199E-2,8.2328729331493405E-2,4.6068139374256099E-2,6.2322694808244698E-2,7.4686713516712203E-2,7.1782425045967102E-2,5.7252213358879103E-2,2.7048252522945401E-2,5.3978262161745102E-2,8.1389778583540101E-2,2.0658939350466098E-2,5.6218799270150201E-2,4.7762989723968197E-2,5.6966833978788899E-2,5.6377434374590599E-2]
["WEST-E1L317C1","WEST",9,"E1L317C1",356,"L&D Expense, CEREALS",0.13801950216293299,0.150457173585892,0.113301411271095,0.12655127048492401,0.114000834524632,5.6761432439088801E-2,2.6986366137862199E-2,9.9266923964023604E-2,4.1428942233324099E-2,2.69035785859623E-2,7.1618623461894307E-2,1.92697768762677E-2,5.9594076037541001E-2,1.39432972578182E-3,9.1593963957775203E-4,6.4883822884699701E-3]
["WEST-E1L320C1","WEST",9,"E1L320C1",359,"L&D Expense, CORN PRODUCTS",1.34091908112168E-2,3.9376903325319297E-2,4.7181513160467099E-2,2.6431472972035401E-2,2.73294728249311E-2,3.8074269890785203E-2,3.7078451365232502E-2,1.75428669899702E-2,2.01527439057827E-2,4.1817161674595404E-3,1.34790764147741E-2,4.3508653131181197E-3,9.0233417435583996E-3,3.9086462228574504E-3,3.02978423330987E-5,2.0180023840311999E-2]
["WEST-E1L324C1","WEST",9,"E1L324C1",363,"L&D Expense, WHISKEY",0.15329632163047799,4.5956458896398503E-2,1.3157946057617701E-2,0.17441810667514801,0.113551504909992,6.6947758197784396E-2,9.6811883151531206E-2,5.2685525268316297E-2,0.73190534114837602,0.41291941120203002,0.301251651267823,2.16556871024641E-2,2.35566983096023E-2,8.2224230857488294E-3,0.14673836468771501,6.9431467804815294E-2]
["WEST-E1L327C1","WEST",9,"E1L327C1",366,"L&D Expense, TOBACCO PRODUCTS",0,0,0,0,3.18567967414856,0,0,0,0,0,0,0,0,0,0,0]
["WEST-E1L330C1","WEST",9,"E1L330C1",369,"L&D Expense, PLYWOOD OR VENEER",7.4905700981617002E-2,4.27759401500225E-2,8.9939765632152599E-2,0.12727469205856301,8.0512069165706607E-2,9.6415840089321095E-2,4.3528910726308802E-2,3.7447415292263003E-2,2.03599594533443E-2,0.12145549472462901,0.216664798239351,2.9783990826895802E-2,7.0972097170494602E-2,6.9536828674594306E-2,6.8338321410531103E-2,0.117691760964366]
["WEST-E1L334C1","WEST",9,"E1L334C1",373,"L&D Expense, NEWSPRINT",0.386345565319061,0.26457613706588701,0.24139791727066001,0.40231353044509899,0.33147549629211398,0.257203638553619,0.141914248466492,8.8899778202176094E-3,0.17850668728351601,0.192825144881663,9.4011005829416405E-2,0.20472030566705901,3.1076594371090002E-2,1.2324784383151699,2.51977665787704E-2,0.16148795459672499]
["WEST-E1L337C1","WEST",9,"E1L337C1",376,"L&D Expense, COV PAPER/PAPERBOARD",0.14351396262645699,2.3441700264811498E-2,5.0217267125844997E-2,4.3607987463474301E-2,3.0316181480884601E-2,3.9156388491392101E-2,6.6796630620956393E-2,3.8177575916051899E-2,0.123719930648804,8.9984059162479299E-2,4.7553798615383003E-2,9.2495401211793692E-3,6.3031332334864496E-3,3.4192846214227003E-2,6.3265511684125697E-2,8.0745058269087004E-3]
["WEST-E1L340C1","WEST",9,"E1L340C1",379,"L&D Expense, CHEMICALS",5.11742942035198E-2,4.20025512576103E-2,3.6974240094423301E-2,4.2966037988662699E-2,3.3213671296834897E-2,4.8909343779087101E-2,5.0282698124647099E-2,3.2089069485664402E-2,3.1751915812492398E-2,3.2152053773539503E-2,4.5385256484858798E-2,3.7555629213460701E-2,3.01283549154009E-2,4.3525262911993302E-2,4.1050292308664603E-2,4.8456104800754497E-2]
["WEST-E1L342C1","WEST",9,"E1L342C1",381,"L&D Expense, POTASSIUM OR SODIUM",2.7809889987111099E-2,1.60602275282145E-2,1.1788333766162401E-2,1.4397126622498001E-2,2.13480275124311E-2,1.2410043738782401E-2,9.0565774589776993E-3,7.6568066142499404E-3,1.3412986882031E-2,8.5684775629813106E-3,2.6314574467900101E-2,1.10570170436835E-2,1.12225187459802E-2,1.60371523159329E-2,1.1939958424653599E-2,5.9931752529763698E-3]
["WEST-E1L345C1","WEST",9,"E1L345C1",384,"L&D Expense, ALL OTHER CHEMICALS",2.6043361052870799E-2,0.102892324328423,5.1314171403646497E-2,5.8835830539464999E-2,4.2031995952129399E-2,1.8057033419609101E-2,2.5860302150249499E-2,7.7346088364720301E-3,2.08973791450262E-2,2.2599386791942899E-2,5.1338501809845997E-2,4.6916238257755201E-4,7.0031947197344305E-2,9.0754973556344501E-2,0.11058293551930599,1.91782433824856E-2]
["WEST-E1L349C1","WEST",9,"E1L349C1",388,"L&D Expense, ALL OTHER RUBBER PRODUCTS",0.11405962705612201,0.128890320658684,8.23671519756317E-2,3.9198044687509502E-2,2.3228943347930901E-2,2.2845545783638999E-2,0.11083518713712701,3.211560100317E-2,0.101654149591923,1.32252519852178E-2,3.40125415840088E-2,1.0177256724421E-3,5.8682357893787302E-3,0.123604358744922,3.6994674618663702E-2,1.0509528840878701E-2]
["WEST-E1L352C1","WEST",9,"E1L352C1",391,"L&D Expense, NONMETALLIC EARTH/MIN",3.5418793559074402E-2,2.9506977647542999E-2,3.24249938130379E-2,3.4120228141546201E-2,1.8458276987075799E-2,2.4468347430229201E-2,2.0480075851082798E-2,2.0243378356099101E-2,2.5672337040305099E-2,2.5089518608720399E-2,3.77997396445496E-2,7.6303684431867002E-3,1.4583935379803001E-2,1.4303699383296E-2,4.0311754906339203E-3,1.3603944578531899E-2]
["WEST-E1L356C1","WEST",9,"E1L356C1",395,"L&D Expense, ALUMINUM BASIC SHAPES",0.11286199837923,0.15163244307041199,0.19129206240177199,0.99977880716323897,9.2738665640354198E-2,0.365030497312546,0.13654950261116,0.40275806188583402,4.6725824475288398E-2,0.427446876899923,7.1842447765894907E-2,6.1801981514728398E-2,2.36256029762279E-4,0.97019829399741397,1.4380682533099101,1.67692641734201]
["WEST-E1L359C1","WEST",9,"E1L359C1",398,"L&D Expense, FAB STRUC METAL PRODUCTS",1.3789104223251301,0.26735174655914301,0.109357416629791,0.55470359325408902,0.24174544215202301,0.26759335398674,8.8351674377918202E-2,2.4079890921711901E-2,1.6526019899174599E-3,0.13177579165119599,0.176593743188519,0.36042406768129098,0.20247041874306199,0.685889247456412,6.71721725659165E-3,0.61904499763286203]
["WEST-E1L361C1","WEST",9,"E1L361C1",400,"L&D Expense, MACHINERY EXCEPT ELECTRICAL",0.56518673896789595,0.32207629084587103,0.48734244704246499,0.78966307640075695,0.41966882348060602,0.16947755217552199,0.53890877962112405,0.47151488065719599,0.35861149430275002,0.237905620493821,0.107907509116882,0.111111250301434,0.57319507395133296,0.40923914491589602,4.4424753803321601E-2,0.24683393968713699]
["WEST-E1L364C1","WEST",9,"E1L364C1",403,"L&D Expense, CONST MIN/MAT HAND MACHINERY",5.3824152797460598E-2,0.14556503295898399,0.225022718310356,0.24387198686599701,0.111423380672932,1.9659049808979E-2,9.3566169962286897E-3,0.25835311412811302,9.0812714770436304E-3,2.4417359235743799E-2,0.226980429468987,0.123886814731048,5.6786413195415104,5.5626533761732502E-2,0.50608937133810405,2.0688925659798598]
["WEST-E1L367C1","WEST",9,"E1L367C1",406,"L&D Expense, ELECTRICAL TRANS/DIST EQUIPMENT",4.9571437835693404,1.3843834400177,1.5912679433822601,0.52243554592132602,0.95162492990493797,1.35360562801361,0.46107843518257102,0.55019402503967296,0.73037481307983398,2.4718954756265998,0.72087862382857204,0.437231102871734,8.2663145076920408,0,1.4978214029207599,2.3871011726206701]
[{"$f":"B8194&\"-\"&D8194","v":"WEST-E1L370C1"},"WEST",9,"E1L370C1",409,"L&D Expense, ALL OTHER ELECTRICAL MACHINERY",0.72443789243698098,0.124912194907665,1.22650158405304,2.0479607582092298,1.4720858335495,2.7940336614847201E-2,2.5568239390850098E-2,0.79280191659927401,0.32959437370300299,0.11638569092668601,0.15527288252874599,0.20274542735457399,3.8295146556108502E-2,0.100668737420884,0.10349523579893,6.5650136035665803]
["WEST-E1L374C1","WEST",9,"E1L374C1",413,"L&D Expense, MOTOR VECHICLE PARTS",0.17642442882060999,0.27078187465667702,0.25748610496521002,0.82535320520401001,0.14550699293613401,0.17560070753097501,0.17617671191692399,0.84027493000030495,0.21214038133621199,8.8219921107315594E-2,0.393716560465393,0.212999234670077,0.10576437246174999,0.119489105755487,4.6983042073175697E-3,5.2852034619368202E-2]
["WEST-E1L377C1","WEST",9,"E1L377C1",416,"L&D Expense, SHIPPER ASSOCIATION TRAFFIC",6.9035097956657396E-2,4.24118414521217E-2,0,0,0,0,0.15256458520889299,0,0,0,0,3.9752304352468099E-2,0,1.2640222416189799E-2,0,0]
["WEST-E1L381C1","WEST",9,"E1L381C1",420,"L&D Expense, HAZARDOUS MATERIALS",3.3822157420218E-3,4.38846610486507E-2,6.9866083562374101E-2,4.1437070816755302E-2,3.1556442379951498E-2,2.9638551175594299E-2,1.43746230751276E-2,2.3880230262875599E-2,1.29652125760913E-2,2.8145488342284499E-2,1.9073883682287199E-2,6.4705703700832298E-3,1.8164087945304101E-2,3.0475595834185201E-2,1.6340194747313699E-2,2.5929638549913699E-2]
["WEST-E2L101C2","WEST",9,"E2L101C2",423,"E/L Ratio, Railroad-Owned, BOX - 40 FT",1.8218299150466899,1.87522161006927,1.8492568731307999,1.8628079891204801,1.7838646173477199,1.8092288970947299,1.88639605045319,1.8504165410995499,1.8136303424835201,1.8339691347321001,1.83838821490468,1.8371298405467,1.7968027384290399,1.8390003519887399,1.83654439243859,1.8247067342505401]
["WEST-E2L101C4","WEST",9,"E2L101C4",425,"E/L Ratio, All Freight Cars, BOX - 40 FT",1.46511578559875,1.66671931743622,1.5838713645935101,1.72836124897003,1.66820240020752,1.6243766546249401,1.6838968992233301,1.6763818264007599,1.6042726039886499,1.60016064446781,1.6536897372297701,1.6427126455260399,1.6736445836118601,1.8075208913648999,1.8109839688890099,1.7643683405964099]
["WEST-E2L101C7","WEST",9,"E2L101C7",428,"Average circuity, BOX - 40 FT",1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.182000041008,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999,1.1819999999999999]
["WEST-E2L101C10","WEST",9,"E2L101C10",431,"CD per Interchange Switch, BOX - 40 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L101C13","WEST",9,"E2L101C13",434,"CD per I&I Switch, BOX - 40 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L101C17","WEST",9,"E2L101C17",438,"CM per Industry Switch, BOX - 40 FT",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L101C20","WEST",9,"E2L101C20",441,"CM per Interterminal Switch, BOX - 40 FT",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L101C24","WEST",9,"E2L101C24",445,"Average Miles between Interchange Switches, BOX - 40 FT",1225.31860351563,743.51361083984398,1038.95397949219,845.85144042968795,880.20086669921898,993.81658935546898,1120.53662109375,1024.18115234375,1218.03503417969,1074.4221772369599,1117.7495946701799,1078.69517237795,1101.8101032868601,1055.41052365007,932.37036247475999,1065.18825585285]
["WEST-E2L101C27","WEST",9,"E2L101C27",448,"SEMs per Intraterminal Switch, BOX - 40 FT",8.8392734527587908,8.8682355880737305,8.3601112365722692,7.8566813468933097,7.5806179046630904,0,7.5752749443054199,7.5999903678893999,7.3342633247375497,0,7.0890597910869397,6.8900803499824601,0,0,6.8227779061994998,0]
["WEST-E2L101C29","WEST",9,"E2L101C29",450,"SEMs per I&I Switch, BOX - 40 FT",1.47321224212646,1.47803914546967,1.3933517932891799,1.3094469308853101,1.2634361982345601,1.27491998672485,0,0,1.2223773002624501,1.1791417475439201,1.18150996518116,0,0,0,0,0]
["WEST-E2L102C3","WEST",9,"E2L102C3",453,"E/L Ratio, Privately-Owned, BOX - 50 FT",1.34876692295074,1.5571423768997199,1.39674496650696,1.5797306299209599,1.5780956745147701,1.5228080749511701,1.59264612197876,1.6018089056014999,1.52073431015015,1.5125911253267501,1.5669103358934,1.5522311875454,1.61513977304179,1.78848446147297,1.7949459305634601,1.72516138746165]
["WEST-E2L102C6","WEST",9,"E2L102C6",456,"Interline circuity, BOX - 50 FT",1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.18700003623962,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001,1.1870000000000001]
["WEST-E2L102C10","WEST",9,"E2L102C10",460,"CD per Interchange Switch, BOX - 50 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L102C13","WEST",9,"E2L102C13",463,"CD per I&I Switch, BOX - 50 FT",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L102C16","WEST",9,"E2L102C16",466,"CD per Load & Unload Interterminal Switch, BOX - 50 FT",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L102C20","WEST",9,"E2L102C20",470,"CM per Interterminal Switch, BOX - 50 FT",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L102C21","WEST",9,"E2L102C21",471,"CM per I&I Switch, BOX - 50 FT",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L102C25","WEST",9,"E2L102C25",475,"SEMs per Industry Switch, BOX - 50 FT",5.8928489685058603,5.9121565818786603,5.5734071731567401,5.2377877235412598,5.0537457466125497,5.0996809005737296,5.0501842498779297,5.0666599273681596,4.88950872421265,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L102C26","WEST",9,"E2L102C26",476,"SEMs per Interchange Switch, BOX - 50 FT",3.24106669425964,3.2516863346099898,3.0653741359710698,2.8807830810546902,2.7795603275299099,2.8048243522643999,2.7776014804840101,2.7866628170013401,2.68922996520996,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L102C27","WEST",9,"E2L102C27",477,"SEMs per Intraterminal Switch, BOX - 50 FT",8.8392734527587908,8.8682346343994105,8.3601102828979492,7.8566808700561497,7.5806183815002397,7.6495208740234402,7.5752754211425799,7.5999898910522496,7.3342633247375497,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L102C28","WEST",9,"E2L102C28",478,"SEMs per Interterminal Switch, BOX - 50 FT",7.0714197158813503,7.0945878028869602,6.68808889389038,6.2853460311889604,6.0644941329956099,6.1196165084838903,6.06022071838379,6.0799922943115199,5.86741018295288,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L102C29","WEST",9,"E2L102C29",479,"SEMs per I&I Switch, BOX - 50 FT",1.47321224212646,1.47803914546967,1.3933516740798999,1.3094469308853101,1.2634361982345601,1.27492010593414,1.26254594326019,1.2666651010513299,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L103C1","WEST",9,"E2L103C1",480,"Average Tare Weight, BOX - EQUIPPED",36.099998474121101,36.099998474121101,36.200000762939503,36.099998474121101,36.200000762939503,36.200000762939503,36.400001525878899,36.5,36.5,36.5,36.6,36.700000000000003,36.799999999999997,37,37.1,37.299999999999997]
["WEST-E2L103C2","WEST",9,"E2L103C2",481,"E/L Ratio, Railroad-Owned, BOX - EQUIPPED",1.8093556165695199,1.8667608499527,1.8105696439743,1.8203775882720901,1.7817368507385301,1.78959035873413,1.83778619766235,1.8168412446975699,1.7787117958068801,1.8087098366746599,1.7118306599136399,1.7217742482677401,1.7426018656528901,1.7620788757904999,1.80236332720746,1.79124628980259]
["WEST-E2L103C3","WEST",9,"E2L103C3",482,"E/L Ratio, Privately-Owned, BOX - EQUIPPED",1.67722415924072,1.6694347858428999,1.5413959026336701,1.56041359901428,1.56234586238861,1.62052655220032,1.64427709579468,1.5856084823608401,1.5315735340118399,1.5316847217034,1.5110709901061601,1.53130952455791,1.53439591048312,1.57794069317693,1.5781548427747301,1.5153387963090501]
["WEST-E2L103C4","WEST",9,"E2L103C4",483,"E/L Ratio, All Freight Cars, BOX - EQUIPPED",1.7931162118911701,1.84008300304413,1.7694067955017101,1.77059614658356,1.74088978767395,1.7615532875061,1.7988201379776001,1.7629576921462999,1.7181156873703001,1.7383240193770799,1.6603759266286,1.66434006543803,1.6710954566113001,1.69236555887769,1.7102109605614799,1.6701755976325099]
["WEST-E2L103C5","WEST",9,"E2L103C5",484,"Local circuity, BOX - EQUIPPED",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["WEST-E2L103C6","WEST",9,"E2L103C6",485,"Interline circuity, BOX - EQUIPPED",1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.18400001525879,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999,1.1839999999999999]
["WEST-E2L103C7","WEST",9,"E2L103C7",486,"Average circuity, BOX - EQUIPPED",1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999990463299,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999,1.1759999999999999]
["WEST-E2L103C8","WEST",9,"E2L103C8",487,"Spotted-to-Pulled Ratio, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L103C9","WEST",9,"E2L103C9",488,"CD per Industry Switch, BOX - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L103C10","WEST",9,"E2L103C10",489,"CD per Interchange Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L103C11","WEST",9,"E2L103C11",490,"CD per Intraterminal Switch, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L103C12","WEST",9,"E2L103C12",491,"CD per Interterminal Switch, BOX - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L103C13","WEST",9,"E2L103C13",492,"CD per I&I Switch, BOX - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L103C14","WEST",9,"E2L103C14",493,"CD per Load & Unload Industry Switch, BOX - EQUIPP",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L103C15","WEST",9,"E2L103C15",494,"CD per Load & Unload Intraterminal Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L103C16","WEST",9,"E2L103C16",495,"CD per Load & Unload Interterminal Switch, BOX - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L103C17","WEST",9,"E2L103C17",496,"CM per Industry Switch, BOX - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L103C18","WEST",9,"E2L103C18",497,"CM per Interchange Switch, BOX - EQUIPPED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L103C19","WEST",9,"E2L103C19",498,"CM per Intraterminal Switch, BOX - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L103C20","WEST",9,"E2L103C20",499,"CM per Interterminal Switch, BOX - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L103C21","WEST",9,"E2L103C21",500,"CM per I&I Switch, BOX - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L103C22","WEST",9,"E2L103C22",501,"Average CM per CD, Railroad-Owned, BOX - EQUIPPED",507.32382202148398,537.491943359375,546.41351318359398,622.742919921875,574.45928955078102,533.28082275390602,579.116943359375,533.37854003906295,460.41842651367199,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L103C23","WEST",9,"E2L103C23",502,"Average Miles between I&I Switches, BOX - EQUIPPED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L103C24","WEST",9,"E2L103C24",503,"Average Miles between Interchange Switches, BOX - EQUIPPED",1058.80590820313,1027.71325683594,1053.60888671875,1090.12731933594,1009.89056396484,840.55059814453102,881.41955566406295,819.166259765625,826.28240966796898,786.00358684703997,883.21768129105897,803.15059390617603,757.24832703624895,1237.3623571150899,1319.90035081058,1377.4636650029299]
["WEST-E2L103C25","WEST",9,"E2L103C25",504,"SEMs per Industry Switch, BOX - EQUIPPED",5.8928489685058603,5.9121561050415004,5.5734071731567401,5.2377877235412598,5.0537452697753897,5.0996809005737296,5.0501842498779297,5.0666599273681596,4.8895092010498002,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L103C26","WEST",9,"E2L103C26",505,"SEMs per Interchange Switch, BOX - EQUIPPED",3.24106669425964,3.2516863346099898,3.0653741359710698,2.8807833194732702,2.7795603275299099,2.8048245906829798,2.7776012420654301,2.7866628170013401,2.68923020362854,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L103C27","WEST",9,"E2L103C27",506,"SEMs per Intraterminal Switch, BOX - EQUIPPED",8.8392734527587908,8.8682355880737305,8.3601112365722692,7.8566813468933097,7.5806179046630904,7.6495208740234402,7.5752754211425799,7.5999898910522496,7.3342633247375497,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.5047952272936502]
["WEST-E2L103C28","WEST",9,"E2L103C28",507,"SEMs per Interterminal Switch, BOX - EQUIPPED",7.0714192390441903,7.0945878028869602,6.68808841705322,6.2853460311889604,6.0644946098327601,6.1196169853210396,6.06022071838379,6.0799927711486799,5.86741065979004,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L103C29","WEST",9,"E2L103C29",508,"SEMs per I&I Switch, BOX - EQUIPPED",1.47321212291718,1.47803926467896,1.3933517932891799,1.3094469308853101,1.2634363174438501,1.27492010593414,1.2625458240509,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L104C1","WEST",9,"E2L104C1",509,"Average Tare Weight, GONDOLA - PLAIN",26,25.899999618530298,25.799999237060501,25.600000381469702,25.5,25.600000381469702,25.299999237060501,25.700000762939499,25.700000762939499,25.6,25.6,25.6,25.7,25.9,26.1,26.3]
["WEST-E2L104C2","WEST",9,"E2L104C2",510,"E/L Ratio, Railroad-Owned, GONDOLA - PLAIN",2.00466108322144,2.0166893005371098,2.0260770320892298,2.0169763565063499,1.9979054927825901,1.9621063470840501,1.8837763071060201,1.90579569339752,1.94879770278931,1.97586947028052,1.9796508866029201,1.94737215477228,1.9381056195337101,1.96069462631553,1.9573409845035701,1.9077607718071601]
["WEST-E2L104C3","WEST",9,"E2L104C3",511,"E/L Ratio, Privately-Owned, GONDOLA - PLAIN",2.18774461746216,2.1797463893890399,2.1617903709411599,2.1452286243438698,2.13473272323608,2.1360235214233398,2.13194704055786,2.0006351470947301,2.0008096694946298,1.99740302411527,2.0049718894937398,2.0078392794300202,2.0078267695820902,2.0051618983580002,2.0129738809714102,2.0108203489663499]
["WEST-E2L104C4","WEST",9,"E2L104C4",512,"E/L Ratio, All Freight Cars, GONDOLA - PLAIN",2.1506814956664999,2.1413450241088898,2.1302824020385698,2.11541771888733,2.1029491424560498,2.1001837253570601,2.0828444957733199,1.9836183786392201,1.9923913478851301,1.9936308350271501,2.0001576479797198,1.9958562079558,1.99459757243589,1.9970620746468299,2.0019685121323398,1.9913578582507301]
["WEST-E2L104C5","WEST",9,"E2L104C5",513,"Local circuity, GONDOLA - PLAIN",1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.09300005435944,1.093,1.093,1.093,1.093,1.093,1.093,1.093]
["WEST-E2L104C6","WEST",9,"E2L104C6",514,"Interline circuity, GONDOLA - PLAIN",1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.15100002288818,1.151,1.151,1.151,1.151,1.151,1.151,1.151]
["WEST-E2L104C7","WEST",9,"E2L104C7",515,"Average circuity, GONDOLA - PLAIN",1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.13399994373322,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999,1.1339999999999999]
["WEST-E2L104C8","WEST",9,"E2L104C8",516,"Spotted-to-Pulled Ratio, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L104C9","WEST",9,"E2L104C9",517,"CD per Industry Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L104C10","WEST",9,"E2L104C10",518,"CD per Interchange Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L104C11","WEST",9,"E2L104C11",519,"CD per Intraterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L104C12","WEST",9,"E2L104C12",520,"CD per Interterminal Switch, GONDOLA - PLAIN",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L104C13","WEST",9,"E2L104C13",521,"CD per I&I Switch, GONDOLA - PLAIN",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L104C14","WEST",9,"E2L104C14",522,"CD per Load & Unload Industry Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L104C15","WEST",9,"E2L104C15",523,"CD per Load & Unload Intraterminal Switch, GONDOLA - PLAIN",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L104C16","WEST",9,"E2L104C16",524,"CD per Load & Unload Interterminal Switch, GONDOLA - PLAIN",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L104C17","WEST",9,"E2L104C17",525,"CM per Industry Switch, GONDOLA - PLAIN",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L104C18","WEST",9,"E2L104C18",526,"CM per Interchange Switch, GONDOLA - PLAIN",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L104C19","WEST",9,"E2L104C19",527,"CM per Intraterminal Switch, GONDOLA - PLAIN",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L104C20","WEST",9,"E2L104C20",528,"CM per Interterminal Switch, GONDOLA - PLAIN",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L104C21","WEST",9,"E2L104C21",529,"CM per I&I Switch, GONDOLA - PLAIN",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L104C22","WEST",9,"E2L104C22",530,"Average CM per CD, Railroad-Owned, GONDOLA - PLAIN",507.32376098632801,537.49188232421898,546.41351318359398,622.74298095703102,574.45928955078102,533.28076171875,579.11706542968795,533.37854003906295,460.41845703125,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L104C23","WEST",9,"E2L104C23",531,"Average Miles between I&I Switches, GONDOLA - PLAIN",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L104C24","WEST",9,"E2L104C24",532,"Average Miles between Interchange Switches, GONDOLA - PLAIN",1540.19152832031,1634.07690429688,1658.08129882813,1734.95520019531,1985.28955078125,1776.17858886719,1703.41540527344,2015.75134277344,2266.1630859375,2113.9031138201299,2223.4139181590199,2994.59843062564,2558.3572135448599,2428.87338193907,2848.4857133240598,2639.2018130441202]
["WEST-E2L104C25","WEST",9,"E2L104C25",533,"SEMs per Industry Switch, GONDOLA - PLAIN",5.8928484916687003,5.9121565818786603,5.5734071731567401,5.2377877235412598,5.0537457466125497,5.0996809005737296,5.0501842498779297,5.0666604042053196,4.88950872421265,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L104C26","WEST",9,"E2L104C26",534,"SEMs per Interchange Switch, GONDOLA - PLAIN",3.24106669425964,3.2516863346099898,3.0653741359710698,2.8807833194732702,2.7795600891113299,2.8048245906829798,2.7776012420654301,2.7866628170013401,2.68922996520996,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L104C27","WEST",9,"E2L104C27",535,"SEMs per Intraterminal Switch, GONDOLA - PLAIN",8.8392744064331108,8.8682355880737305,8.3601112365722692,7.8566813468933097,7.5806188583373997,7.6495208740234402,7.5752754211425799,7.5999903678893999,7.3342638015747097,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L104C28","WEST",9,"E2L104C28",536,"SEMs per Interterminal Switch, GONDOLA - PLAIN",7.0714197158813503,7.0945878028869602,6.68808841705322,6.2853455543518102,6.0644946098327601,6.1196169853210396,6.06022024154663,6.0799932479858398,5.86741065979004,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
[{"$f":"B8322&\"-\"&D8322","v":"WEST-E2L104C29"},"WEST",9,"E2L104C29",537,"SEMs per I&I Switch, GONDOLA - PLAIN",1.47321212291718,1.47803914546967,1.3933517932891799,1.3094470500946001,1.2634363174438501,1.27491998672485,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L105C1","WEST",9,"E2L105C1",538,"Average Tare Weight, GONDOLA - EQUIPPED",33.099998474121101,33.200000762939503,33.400001525878899,33.299999237060497,33.299999237060497,33.299999237060497,33.299999237060497,33.099998474121101,33.099998474121101,33.200000000000003,33.200000000000003,33.1,33.1,33.1,33.1,33.1]
["WEST-E2L105C2","WEST",9,"E2L105C2",539,"E/L Ratio, Railroad-Owned, GONDOLA - EQUIPPED",1.89289367198944,2.0464074611663801,1.9507800340652499,2.0906279087066699,2.0113601684570299,1.93816518783569,1.99631023406982,2.0018756389617902,1.9390565156936601,2.07278560250391,2.0223515124576301,2.0121780371628302,1.9182355622027201,2.0043394182654302,2.0205127824680602,1.90096465591276]
["WEST-E2L105C3","WEST",9,"E2L105C3",540,"E/L Ratio, Privately-Owned, GONDOLA - EQUIPPED",2.0381987094879199,2.0598835945129399,2.0217642784118701,2.0009028911590598,2.0160684585571298,2.0064604282379199,2.00225734710693,2.01650094985962,2.0344827175140399,2.0273722200089099,1.9794398259220001,1.94821949502062,1.98334869554763,1.99389392557291,2.0110793174442501,1.98966274481798]
["WEST-E2L105C4","WEST",9,"E2L105C4",541,"E/L Ratio, All Freight Cars, GONDOLA - EQUIPPED",1.93648433685303,2.0495474338531499,1.9618127346038801,2.0735182762146001,2.01215767860413,1.9508410692214999,1.9975013732910201,2.00501680374146,1.9574348926544201,2.0614180711088701,2.01284657640901,1.9985114969397,1.93403339896449,2.0015915924739698,2.0176983779957101,1.9250557656871301]
["WEST-E2L105C5","WEST",9,"E2L105C5",542,"Local circuity, GONDOLA - EQUIPPED",1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000143051101,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001,1.1100000000000001]
["WEST-E2L105C6","WEST",9,"E2L105C6",543,"Interline circuity, GONDOLA - EQUIPPED",1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1219999790191699,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001,1.1220000000000001]
["WEST-E2L105C7","WEST",9,"E2L105C7",544,"Average circuity, GONDOLA - EQUIPPED",1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.1189999580383301,1.119,1.119,1.119,1.119,1.119,1.119,1.119]
["WEST-E2L105C8","WEST",9,"E2L105C8",545,"Spotted-to-Pulled Ratio, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L105C9","WEST",9,"E2L105C9",546,"CD per Industry Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L105C10","WEST",9,"E2L105C10",547,"CD per Interchange Switch, GONDOLA - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L105C11","WEST",9,"E2L105C11",548,"CD per Intraterminal Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L105C12","WEST",9,"E2L105C12",549,"CD per Interterminal Switch, GONDOLA - EQUIPPED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L105C13","WEST",9,"E2L105C13",550,"CD per I&I Switch, GONDOLA - EQUIPPED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L105C14","WEST",9,"E2L105C14",551,"CD per Load & Unload Industry Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L105C15","WEST",9,"E2L105C15",552,"CD per Load & Unload Intraterminal Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L105C16","WEST",9,"E2L105C16",553,"CD per Load & Unload Interterminal Switch, GONDOLA - EQUIPPED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L105C17","WEST",9,"E2L105C17",554,"CM per Industry Switch, GONDOLA - EQUIPPED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L105C18","WEST",9,"E2L105C18",555,"CM per Interchange Switch, GONDOLA - EQUIPPED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L105C19","WEST",9,"E2L105C19",556,"CM per Intraterminal Switch, GONDOLA - EQUIPPED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L105C20","WEST",9,"E2L105C20",557,"CM per Interterminal Switch, GONDOLA - EQUIPPED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L105C21","WEST",9,"E2L105C21",558,"CM per I&I Switch, GONDOLA - EQUIPPED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L105C22","WEST",9,"E2L105C22",559,"Average CM per CD, Railroad-Owned, GONDOLA - EQUIPPED",507.32376098632801,537.491943359375,546.41351318359398,622.742919921875,574.459228515625,533.28076171875,579.11700439453102,533.37860107421898,460.41845703125,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L105C23","WEST",9,"E2L105C23",560,"Average Miles between I&I Switches, GONDOLA - EQUIPPED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L105C24","WEST",9,"E2L105C24",561,"Average Miles between Interchange Switches, GONDOLA - EQUIPPED",1224.09130859375,890.67010498046898,793.81994628906295,983.20916748046898,885.79754638671898,885.597900390625,834.62451171875,849.602783203125,848.61267089843795,887.74658447012996,876.71595655945396,926.27591027830499,1018.99210768956,1117.2026737743199,1196.4134525503,1075.26097243291]
["WEST-E2L105C25","WEST",9,"E2L105C25",562,"SEMs per Industry Switch, GONDOLA - EQUIPPED",5.8928484916687003,5.9121565818786603,5.5734066963195801,5.2377882003784197,5.0537457466125497,5.0996809005737296,5.0501842498779297,5.0666599273681596,4.8895092010498002,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L105C26","WEST",9,"E2L105C26",563,"SEMs per Interchange Switch, GONDOLA - EQUIPPED",3.24106669425964,3.2516863346099898,3.0653736591339098,2.8807833194732702,2.7795600891113299,2.8048243522643999,2.7776012420654301,2.7866628170013401,2.68922996520996,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L105C27","WEST",9,"E2L105C27",564,"SEMs per Intraterminal Switch, GONDOLA - EQUIPPED",8.8392734527587908,8.8682355880737305,8.3601112365722692,7.8566818237304696,7.5806183815002397,7.6495213508606001,7.5752758979797399,7.5999898910522496,7.3342628479003897,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L105C28","WEST",9,"E2L105C28",565,"SEMs per Interterminal Switch, GONDOLA - EQUIPPED",7.0714192390441903,7.0945873260498002,6.68808841705322,6.2853460311889604,6.0644941329956099,6.1196165084838903,6.0602211952209499,6.0799927711486799,5.86741065979004,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L105C29","WEST",9,"E2L105C29",566,"SEMs per I&I Switch, GONDOLA - EQUIPPED",1.47321224212646,1.47803914546967,1.3933517932891799,1.30944716930389,1.2634361982345601,1.27491998672485,1.26254594326019,1.2666649818420399,1.2223771810531601,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714199,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L106C1","WEST",9,"E2L106C1",567,"Average Tare Weight, HOPPER - COVERED",31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.399999618530298,31.200000762939499,31.100000381469702,31,30.8,30.8,30.8,30.8,30.8,30.8,30.9]
["WEST-E2L106C2","WEST",9,"E2L106C2",568,"E/L Ratio, Railroad-Owned, HOPPER - COVERED",1.99489569664001,1.9894942045211801,1.99264681339264,2.0017292499542201,1.99688196182251,1.9905012845993,2.00821828842163,2.0224072933196999,1.9763224124908401,2.0001113822295999,1.9948052802906,2.0192404336276799,2.0060908084163902,2.0168911281731901,1.98244664571561,1.9769228108307599]
["WEST-E2L106C3","WEST",9,"E2L106C3",569,"E/L Ratio, Privately-Owned, HOPPER - COVERED",2.0042583942413299,2.00533223152161,2.0178759098053001,2.0196394920349099,2.0018606185913099,1.9912738800048799,1.9931451082229601,1.9913963079452499,1.97444415092468,1.9964945292128,1.99611871104151,1.99698624677907,2.0034923628640402,2.0172631504875,2.0032871633332801,1.99243084043054]
["WEST-E2L106C4","WEST",9,"E2L106C4",570,"E/L Ratio, All Freight Cars, HOPPER - COVERED",1.99958872795105,1.9974403381347701,2.0050637722015399,2.01069855690002,1.99931263923645,1.9908797740936299,2.0002555847168,2.0049586296081499,1.9752655029296899,1.9981223266249399,1.9955002328273601,2.0064011182361701,2.0046171972390501,2.01709766217042,1.9928174723712899,1.9849506657559299]
["WEST-E2L106C5","WEST",9,"E2L106C5",571,"Local circuity, HOPPER - COVERED",1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1260000467300399,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999,1.1259999999999999]
["WEST-E2L106C6","WEST",9,"E2L106C6",572,"Interline circuity, HOPPER - COVERED",1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1640000343322801,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999,1.1639999999999999]
["WEST-E2L106C7","WEST",9,"E2L106C7",573,"Average circuity, HOPPER - COVERED",1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.14800000190735,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999,1.1479999999999999]
["WEST-E2L106C8","WEST",9,"E2L106C8",574,"Spotted-to-Pulled Ratio, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L106C9","WEST",9,"E2L106C9",575,"CD per Industry Switch, HOPPER - COVERED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L106C10","WEST",9,"E2L106C10",576,"CD per Interchange Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L106C11","WEST",9,"E2L106C11",577,"CD per Intraterminal Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L106C12","WEST",9,"E2L106C12",578,"CD per Interterminal Switch, HOPPER - COVERED",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L106C13","WEST",9,"E2L106C13",579,"CD per I&I Switch, HOPPER - COVERED",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L106C14","WEST",9,"E2L106C14",580,"CD per Load & Unload Industry Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L106C15","WEST",9,"E2L106C15",581,"CD per Load & Unload Intraterminal Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L106C16","WEST",9,"E2L106C16",582,"CD per Load & Unload Interterminal Switch, HOPPER - COVERED",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L106C17","WEST",9,"E2L106C17",583,"CM per Industry Switch, HOPPER - COVERED",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L106C18","WEST",9,"E2L106C18",584,"CM per Interchange Switch, HOPPER - COVERED",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L106C19","WEST",9,"E2L106C19",585,"CM per Intraterminal Switch, HOPPER - COVERED",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L106C20","WEST",9,"E2L106C20",586,"CM per Interterminal Switch, HOPPER - COVERED",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L106C21","WEST",9,"E2L106C21",587,"CM per I&I Switch, HOPPER - COVERED",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L106C22","WEST",9,"E2L106C22",588,"Average CM per CD, Railroad-Owned, HOPPER - COVERED",507.32373046875,537.49188232421898,546.41357421875,622.74298095703102,574.45928955078102,533.28070068359398,579.11706542968795,533.37860107421898,460.41845703125,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L106C23","WEST",9,"E2L106C23",589,"Average Miles between I&I Switches, HOPPER - COVERED",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L106C24","WEST",9,"E2L106C24",590,"Average Miles between Interchange Switches, HOPPER - COVERED",1246.73388671875,1338.00366210938,1337.8955078125,1485.73510742188,1406.2099609375,1391.30200195313,1357.09167480469,1428.35986328125,1525.12609863281,1370.57755949281,1599.0394941797199,1625.9628032657199,1749.2033475011399,1849.2238409111001,1832.77576694595,1900.4198779763999]
["WEST-E2L106C25","WEST",9,"E2L106C25",591,"SEMs per Industry Switch, HOPPER - COVERED",5.8928484916687003,5.9121565818786603,5.5734071731567401,5.2377882003784197,5.0537452697753897,5.0996809005737296,5.0501842498779297,5.0666599273681596,4.88950872421265,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L106C26","WEST",9,"E2L106C26",592,"SEMs per Interchange Switch, HOPPER - COVERED",3.24106645584106,3.2516863346099898,3.0653738975524898,2.8807830810546902,2.7795600891113299,2.8048243522643999,2.7776012420654301,2.7866630554199201,2.68923020362854,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L106C27","WEST",9,"E2L106C27",593,"SEMs per Intraterminal Switch, HOPPER - COVERED",8.8392744064331108,8.8682355880737305,8.3601112365722692,7.8566803932189897,7.5806179046630904,7.6495203971862802,7.5752754211425799,7.5999903678893999,7.3342633247375497,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L106C28","WEST",9,"E2L106C28",594,"SEMs per Interterminal Switch, HOPPER - COVERED",7.0714197158813503,7.0945873260498002,6.68808841705322,6.2853460311889604,6.0644941329956099,6.1196169853210396,6.06022024154663,6.0799927711486799,5.86741065979004,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L106C29","WEST",9,"E2L106C29",595,"SEMs per I&I Switch, HOPPER - COVERED",1.47321236133575,1.47803926467896,1.3933519124984699,1.3094470500946001,1.2634363174438501,1.27491998672485,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714199,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L107C1","WEST",9,"E2L107C1",596,"Average Tare Weight, HOPPER - OPEN TOP - GENERAL",29.799999237060501,29.700000762939499,29.600000381469702,29.600000381469702,29.5,29.600000381469702,29.399999618530298,29.200000762939499,29,28.9,28.8,28.8,28.7,28.5,28.4,28.3]
["WEST-E2L107C2","WEST",9,"E2L107C2",597,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",2.0377345085143999,2.04338932037354,2.0217442512512198,2.0546886920928999,2.0440485477447501,2.0850663185119598,2.0940279960632302,2.0999495983123802,2.09499907493591,2.1176097992641201,2.1462417691638702,2.10570043849527,2.12403947342295,2.1433359002880699,2.16072372672267,2.1305871879520799]
["WEST-E2L107C3","WEST",9,"E2L107C3",598,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - GENERAL",2.1490967273712198,2.1529743671417201,2.0190336704254199,2.0302288532257098,1.99888455867767,2.1784749031066899,2.1723897457122798,1.99474084377289,1.9812102317810101,1.9962119304043,1.9979588777287001,1.9943307655272,1.9879889835262901,2.0135435775340502,2.0025442611104398,1.99642075411957]
["WEST-E2L107C4","WEST",9,"E2L107C4",599,"E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - GENERAL",2.0648787021636998,2.0707662105560298,2.0210237503051798,2.0466861724853498,2.0300247669220002,2.1127774715423602,2.1135725975036599,2.0677752494811998,2.0534546375274698,2.0592893027577999,2.0693392023061201,2.0538378754077802,2.0644808377150401,2.0754634826683001,2.07129786455363,2.05357975331663]
["WEST-E2L107C5","WEST",9,"E2L107C5",600,"Local circuity, HOPPER - OPEN TOP - GENERAL",1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.07599997520447,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001,1.0760000000000001]
[{"$f":"B8386&\"-\"&D8386","v":"WEST-E2L107C6"},"WEST",9,"E2L107C6",601,"Interline circuity, HOPPER - OPEN TOP - GENERAL",1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.1369999647140501,1.137,1.137,1.137,1.137,1.137,1.137,1.137]
["WEST-E2L107C7","WEST",9,"E2L107C7",602,"Average circuity, HOPPER - OPEN TOP - GENERAL",1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1059999465942401,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001,1.1060000000000001]
["WEST-E2L107C8","WEST",9,"E2L107C8",603,"Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L107C9","WEST",9,"E2L107C9",604,"CD per Industry Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L107C10","WEST",9,"E2L107C10",605,"CD per Interchange Switch, HOPPER - OPEN TOP - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L107C11","WEST",9,"E2L107C11",606,"CD per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L107C12","WEST",9,"E2L107C12",607,"CD per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L107C13","WEST",9,"E2L107C13",608,"CD per I&I Switch, HOPPER - OPEN TOP - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L107C14","WEST",9,"E2L107C14",609,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L107C15","WEST",9,"E2L107C15",610,"CD per Load & Unload Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L107C16","WEST",9,"E2L107C16",611,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L107C17","WEST",9,"E2L107C17",612,"CM per Industry Switch, HOPPER - OPEN TOP - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L107C18","WEST",9,"E2L107C18",613,"CM per Interchange Switch, HOPPER - OPEN TOP - GENERAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L107C19","WEST",9,"E2L107C19",614,"CM per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L107C20","WEST",9,"E2L107C20",615,"CM per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L107C21","WEST",9,"E2L107C21",616,"CM per I&I Switch, HOPPER - OPEN TOP - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L107C22","WEST",9,"E2L107C22",617,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - GENERAL",507.32376098632801,537.49188232421898,546.41357421875,622.742919921875,574.45928955078102,533.28076171875,579.11700439453102,533.37860107421898,460.41845703125,517.68365917384403,559.033501284561,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L107C23","WEST",9,"E2L107C23",618,"Average Miles between I&I Switches, HOPPER - OPEN TOP - GENERAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L107C24","WEST",9,"E2L107C24",619,"Average Miles between Interchange Switches, HOPPER - OPEN TOP - GENERAL",738.81091308593795,779.63372802734398,934.2353515625,1101.708984375,1010.13336181641,1277.23620605469,1509.26416015625,1429.41174316406,1348.95666503906,1185.9015603192399,2183.02745275179,2560.7329936759802,2854.7069749717198,3308.22973343785,2897.2480090797599,3132.7923788815101]
["WEST-E2L107C25","WEST",9,"E2L107C25",620,"SEMs per Industry Switch, HOPPER - OPEN TOP - GENERAL",5.8928484916687003,5.9121565818786603,5.5734071731567401,5.2377882003784197,5.0537457466125497,5.0996804237365696,5.0501842498779297,5.0666599273681596,4.88950872421265,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L107C26","WEST",9,"E2L107C26",621,"SEMs per Interchange Switch, HOPPER - OPEN TOP - GENERAL",3.24106693267822,3.2516863346099898,3.0653741359710698,2.8807833194732702,2.7795600891113299,2.8048241138458301,2.7776012420654301,2.7866628170013401,2.68922996520996,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L107C27","WEST",9,"E2L107C27",622,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL",8.8392744064331108,8.8682355880737305,8.3601112365722692,7.8566818237304696,7.5806179046630904,7.6495218276977504,7.5752758979797399,7.5999898910522496,7.3342628479003897,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.5047952272936502]
["WEST-E2L107C28","WEST",9,"E2L107C28",623,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - GENERAL",7.0714192390441903,7.0945882797241202,6.68808794021606,6.2853455543518102,6.0644941329956099,6.1196174621581996,6.06022024154663,6.0799922943115199,5.8674111366271999,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L107C29","WEST",9,"E2L107C29",624,"SEMs per I&I Switch, HOPPER - OPEN TOP - GENERAL",1.47321224212646,1.47803914546967,1.3933517932891799,1.3094470500946001,1.2634361982345601,1.27492010593414,1.2625458240509,1.2666651010513299,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714199,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L108C1","WEST",9,"E2L108C1",625,"Average Tare Weight, HOPPER - OPEN TOP - SPECIAL",27.299999237060501,27.399999618530298,26.899999618530298,26.799999237060501,26.700000762939499,26.799999237060501,26.5,26.5,26.399999618530298,26.4,26.4,26.2,26.1,26.1,26,26]
["WEST-E2L108C2","WEST",9,"E2L108C2",626,"E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",1.98437964916229,2.0081048011779798,2.0049881935119598,2.0327100753784202,2.0210368633270299,2.0464529991149898,2.0933897495269802,2.0279903411865199,1.9905433654785201,2.0034085737690002,2.0168688042744001,2.0137925806125501,2.0112271434559399,2.0187040542551,2.0157145680964601,2.0108338222652802]
["WEST-E2L108C3","WEST",9,"E2L108C3",627,"E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - SPECIAL",2.0643999576568599,2.04887843132019,2.0530838966369598,2.06439256668091,2.0819256305694598,2.0436136722564702,2.0407626628875701,2.00639772415161,2.00506544113159,1.9952002855564399,2.00561879028005,2.0014770691329402,2.0146062933226898,2.0297730513730099,2.0043077839548902,2.00225103364482]
["WEST-E2L108C4","WEST",9,"E2L108C4",628,"E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - SPECIAL",2.05063700675964,2.0408475399017298,2.04390621185303,2.0591897964477499,2.0710868835449201,2.0440940856933598,2.0506715774536102,2.01048803329468,2.0022056102752699,1.9966822530114801,2.0074286480702499,2.00359894844178,2.0138741182801101,2.0275783291477101,2.0061480283657001,2.0036741374883098]
["WEST-E2L108C5","WEST",9,"E2L108C5",629,"Local circuity, HOPPER - OPEN TOP - SPECIAL",1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.2020000219345099,1.202,1.202,1.202,1.202,1.202,1.202,1.202]
["WEST-E2L108C6","WEST",9,"E2L108C6",630,"Interline circuity, HOPPER - OPEN TOP - SPECIAL",1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.15600001811981,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999,1.1559999999999999]
["WEST-E2L108C7","WEST",9,"E2L108C7",631,"Average circuity, HOPPER - OPEN TOP - SPECIAL",1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.18299996852875,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001,1.1830000000000001]
["WEST-E2L108C8","WEST",9,"E2L108C8",632,"Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L108C9","WEST",9,"E2L108C9",633,"CD per Industry Switch, HOPPER - OPEN TOP - SPECIAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L108C10","WEST",9,"E2L108C10",634,"CD per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L108C11","WEST",9,"E2L108C11",635,"CD per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L108C12","WEST",9,"E2L108C12",636,"CD per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L108C13","WEST",9,"E2L108C13",637,"CD per I&I Switch, HOPPER - OPEN TOP - SPECIAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L108C14","WEST",9,"E2L108C14",638,"CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L108C15","WEST",9,"E2L108C15",639,"CD per Load & Unload Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L108C16","WEST",9,"E2L108C16",640,"CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L108C17","WEST",9,"E2L108C17",641,"CM per Industry Switch, HOPPER - OPEN TOP - SPECIAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L108C18","WEST",9,"E2L108C18",642,"CM per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L108C19","WEST",9,"E2L108C19",643,"CM per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L108C20","WEST",9,"E2L108C20",644,"CM per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L108C21","WEST",9,"E2L108C21",645,"CM per I&I Switch, HOPPER - OPEN TOP - SPECIAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L108C22","WEST",9,"E2L108C22",646,"Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL",507.32376098632801,537.491943359375,546.41351318359398,622.74298095703102,574.459228515625,533.28076171875,579.11700439453102,533.37860107421898,460.41842651367199,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L108C23","WEST",9,"E2L108C23",647,"Average Miles between I&I Switches, HOPPER - OPEN TOP - SPECIAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L108C24","WEST",9,"E2L108C24",648,"Average Miles between Interchange Switches, HOPPER - OPEN TOP - SPECIAL",1769.98828125,1402.38488769531,1323.37316894531,1310.99731445313,1377.95495605469,1547.34411621094,1844.51818847656,1977.98596191406,1873.92504882813,2304.5667944655202,1716.1475702387499,1484.39383936642,1639.3629602840299,1228.6335117702399,1012.44518093133,1082.84517069803]
["WEST-E2L108C25","WEST",9,"E2L108C25",649,"SEMs per Industry Switch, HOPPER - OPEN TOP - SPECIAL",5.8928484916687003,5.9121565818786603,5.5734071731567401,5.2377882003784197,5.0537452697753897,5.0996809005737296,5.0501842498779297,5.0666599273681596,4.88950872421265,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L108C26","WEST",9,"E2L108C26",650,"SEMs per Interchange Switch, HOPPER - OPEN TOP - SPECIAL",3.24106669425964,3.2516860961914098,3.0653741359710698,2.8807830810546902,2.7795603275299099,2.8048245906829798,2.7776014804840101,2.7866628170013401,2.68922996520996,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L108C27","WEST",9,"E2L108C27",651,"SEMs per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL",8.8392744064331108,8.8682355880737305,8.3601112365722692,7.8566808700561497,7.5806179046630904,7.6495208740234402,7.5752754211425799,7.5999903678893999,7.3342628479003897,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.5047952272936502]
["WEST-E2L108C28","WEST",9,"E2L108C28",652,"SEMs per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL",7.0714192390441903,7.0945873260498002,6.68808841705322,6.2853460311889604,6.0644936561584499,6.1196169853210396,6.06022071838379,6.0799927711486799,5.8674111366271999,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L108C29","WEST",9,"E2L108C29",653,"SEMs per I&I Switch, HOPPER - OPEN TOP - SPECIAL",1.47321212291718,1.47803902626038,1.3933516740798999,1.3094470500946001,1.2634361982345601,1.27492010593414,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L109C1","WEST",9,"E2L109C1",654,"Average Tare Weight, REFRIGERATED - MECH",46.099998474121101,46.099998474121101,46.400001525878899,46.599998474121101,46.599998474121101,46.5,46.599998474121101,47,47.200000762939503,47.5,48.2,48.3,48.4,48.6,48.9,49.2]
["WEST-E2L109C2","WEST",9,"E2L109C2",655,"E/L Ratio, Railroad-Owned, REFRIGERATED - MECH",1.76497149467468,1.7138966321945199,1.6718657016754199,1.6738101243972801,1.69289326667786,1.6413005590438801,1.7374846935272199,1.7462629079818699,1.77023673057556,1.85640607411151,1.76999665638816,1.7694529241136501,1.8267022373127999,1.8916655725268801,1.8665181939006401,1.8878013343784099]
["WEST-E2L109C3","WEST",9,"E2L109C3",656,"E/L Ratio, Privately-Owned, REFRIGERATED - MECH",2.06168484687805,2.1109426021575901,2.17184686660767,2.1229696273803702,2.1806282997131299,2.2464129924774201,2.3253514766693102,1.94405949115753,1.9011980295181301,1.86375486454831,1.87674818025681,1.88782658864255,1.84661023981412,1.8886063489459399,1.9152630526105201,1.92901119788438]
["WEST-E2L109C4","WEST",9,"E2L109C4",657,"E/L Ratio, All Freight Cars, REFRIGERATED - MECH",1.8000916242599501,1.76494157314301,1.7372181415557899,1.74459493160248,1.76569676399231,1.71953749656677,1.8230941295623799,1.78629267215729,1.79569888114929,1.85811935696983,1.7948101325982599,1.7972832879579099,1.8312047819681501,1.8908629168505,1.88162086447758,1.9008364919618399]
["WEST-E2L109C5","WEST",9,"E2L109C5",658,"Local circuity, REFRIGERATED - MECH",1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.0789999961853001,1.079,1.079,1.079,1.079,1.079,1.079,1.079]
["WEST-E2L109C6","WEST",9,"E2L109C6",659,"Interline circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["WEST-E2L109C7","WEST",9,"E2L109C7",660,"Average circuity, REFRIGERATED - MECH",1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0779999494552599,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001,1.0780000000000001]
["WEST-E2L109C8","WEST",9,"E2L109C8",661,"Spotted-to-Pulled Ratio, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L109C9","WEST",9,"E2L109C9",662,"CD per Industry Switch, REFRIGERATED - MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L109C10","WEST",9,"E2L109C10",663,"CD per Interchange Switch, REFRIGERATED - MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L109C11","WEST",9,"E2L109C11",664,"CD per Intraterminal Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
[{"$f":"B8450&\"-\"&D8450","v":"WEST-E2L109C12"},"WEST",9,"E2L109C12",665,"CD per Interterminal Switch, REFRIGERATED - MECH",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L109C13","WEST",9,"E2L109C13",666,"CD per I&I Switch, REFRIGERATED - MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L109C14","WEST",9,"E2L109C14",667,"CD per Load & Unload Industry Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L109C15","WEST",9,"E2L109C15",668,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L109C16","WEST",9,"E2L109C16",669,"CD per Load & Unload Interterminal Switch, REFRIGERATED - MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L109C17","WEST",9,"E2L109C17",670,"CM per Industry Switch, REFRIGERATED - MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L109C18","WEST",9,"E2L109C18",671,"CM per Interchange Switch, REFRIGERATED - MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L109C19","WEST",9,"E2L109C19",672,"CM per Intraterminal Switch, REFRIGERATED - MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L109C20","WEST",9,"E2L109C20",673,"CM per Interterminal Switch, REFRIGERATED - MECH",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L109C21","WEST",9,"E2L109C21",674,"CM per I&I Switch, REFRIGERATED - MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L109C22","WEST",9,"E2L109C22",675,"Average CM per CD, Railroad-Owned, REFRIGERATED - MECH",507.32379150390602,537.49182128906295,546.41351318359398,622.742919921875,574.459228515625,533.28076171875,579.11700439453102,533.37860107421898,460.41848754882801,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L109C23","WEST",9,"E2L109C23",676,"Average Miles between I&I Switches, REFRIGERATED - MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L109C24","WEST",9,"E2L109C24",677,"Average Miles between Interchange Switches, REFRIGERATED - MECH",1650.09167480469,1552.22814941406,1597.59411621094,1957.30310058594,2022.20727539063,1871.16772460938,1688.87841796875,1666.83532714844,1865.28747558594,1721.3853084454199,1706.7734708006701,1817.3300663144901,1891.8466463356001,1762.79335686389,1719.92554986185,1558.5952308890901]
["WEST-E2L109C25","WEST",9,"E2L109C25",678,"SEMs per Industry Switch, REFRIGERATED - MECH",5.8928489685058603,5.9121565818786603,5.5734071731567401,5.2377882003784197,5.0537452697753897,5.0996813774108896,5.0501842498779297,5.0666599273681596,4.88950872421265,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L109C26","WEST",9,"E2L109C26",679,"SEMs per Interchange Switch, REFRIGERATED - MECH",3.24106669425964,3.2516863346099898,3.0653741359710698,2.8807833194732702,2.7795600891113299,2.8048245906829798,2.7776014804840101,2.7866628170013401,2.68922996520996,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L109C27","WEST",9,"E2L109C27",680,"SEMs per Intraterminal Switch, REFRIGERATED - MECH",8.8392744064331108,8.8682346343994105,8.3601112365722692,7.8566808700561497,7.5806179046630904,7.6495203971862802,7.5752754211425799,7.5999903678893999,7.3342628479003897,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.5047952272936502]
["WEST-E2L109C28","WEST",9,"E2L109C28",681,"SEMs per Interterminal Switch, REFRIGERATED - MECH",7.0714192390441903,7.0945873260498002,6.68808841705322,6.2853450775146502,6.0644946098327601,6.1196165084838903,6.0602211952209499,6.0799922943115199,5.86741065979004,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L109C29","WEST",9,"E2L109C29",682,"SEMs per I&I Switch, REFRIGERATED - MECH",1.47321224212646,1.47803914546967,1.3933517932891799,1.3094469308853101,1.2634361982345601,1.27492010593414,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714199,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L110C1","WEST",9,"E2L110C1",683,"Average Tare Weight, REFRIGERATED - NON-MECH",42.799999237060497,42.900001525878899,43.099998474121101,43.299999237060497,43.799999237060497,43.400001525878899,44,44.099998474121101,44.099998474121101,44.2,44.2,44.2,44.2,44.2,44.6,45.2]
["WEST-E2L110C2","WEST",9,"E2L110C2",684,"E/L Ratio, Railroad-Owned, REFRIGERATED - NON-MECH",1.7891362905502299,1.87827455997467,1.7914344072341899,1.7445770502090501,1.8388812541961701,1.8821341991424601,1.91862988471985,1.84857642650604,1.8573625087737999,1.87949195802779,1.8347155570050799,1.8631709433494501,1.8808775605214201,1.91179114675105,2.03453737515949,2.0161191749427001]
["WEST-E2L110C3","WEST",9,"E2L110C3",685,"E/L Ratio, Privately-Owned, REFRIGERATED - NON-MECH",2.0414018630981401,2.0714960098266602,2.0409078598022501,2.0481255054473899,2.04822897911072,1.9125388860702499,1.95646440982819,1.96411025524139,1.92742455005646,1.9908318425760301,1.9590584878744699,1.9901324682346599,1.9944903581267199,1.99803891989742,2.01223491027732,1.9966545454545499]
["WEST-E2L110C4","WEST",9,"E2L110C4",686,"E/L Ratio, All Freight Cars, REFRIGERATED - NON-MECH",1.7999128103256199,1.88655698299408,1.8024554252624501,1.76055824756622,1.8517637252807599,1.8838402032852199,1.92065966129303,1.85431480407715,1.86156725883484,1.88874029495895,1.8521707785966,1.8828483439130199,1.9006918420293999,1.9283930541843299,2.0290842612597602,2.0120707911057298]
["WEST-E2L110C5","WEST",9,"E2L110C5",687,"Local circuity, REFRIGERATED - NON-MECH",1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000305175799,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001,1.1180000000000001]
["WEST-E2L110C6","WEST",9,"E2L110C6",688,"Interline circuity, REFRIGERATED - NON-MECH",1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.1590000391006501,1.159,1.159,1.159,1.159,1.159,1.159,1.159]
["WEST-E2L110C7","WEST",9,"E2L110C7",689,"Average circuity, REFRIGERATED - NON-MECH",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["WEST-E2L110C8","WEST",9,"E2L110C8",690,"Spotted-to-Pulled Ratio, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L110C9","WEST",9,"E2L110C9",691,"CD per Industry Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L110C10","WEST",9,"E2L110C10",692,"CD per Interchange Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L110C11","WEST",9,"E2L110C11",693,"CD per Intraterminal Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L110C12","WEST",9,"E2L110C12",694,"CD per Interterminal Switch, REFRIGERATED - NON-MECH",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L110C13","WEST",9,"E2L110C13",695,"CD per I&I Switch, REFRIGERATED - NON-MECH",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L110C14","WEST",9,"E2L110C14",696,"CD per Load & Unload Industry Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L110C15","WEST",9,"E2L110C15",697,"CD per Load & Unload Intraterminal Switch, REFRIGERATED - NON-MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L110C16","WEST",9,"E2L110C16",698,"CD per Load & Unload Interterminal Switch, REFRIGERATED - NON-MECH",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L110C17","WEST",9,"E2L110C17",699,"CM per Industry Switch, REFRIGERATED - NON-MECH",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L110C18","WEST",9,"E2L110C18",700,"CM per Interchange Switch, REFRIGERATED - NON-MECH",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L110C19","WEST",9,"E2L110C19",701,"CM per Intraterminal Switch, REFRIGERATED - NON-MECH",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L110C20","WEST",9,"E2L110C20",702,"CM per Interterminal Switch, REFRIGERATED - NON-MECH",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L110C21","WEST",9,"E2L110C21",703,"CM per I&I Switch, REFRIGERATED - NON-MECH",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L110C22","WEST",9,"E2L110C22",704,"Average CM per CD, Railroad-Owned, REFRIGERATED - NON-MECH",507.32376098632801,537.491943359375,546.41357421875,622.742919921875,574.459228515625,533.28076171875,579.11700439453102,533.37854003906295,460.41842651367199,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L110C23","WEST",9,"E2L110C23",705,"Average Miles between I&I Switches, REFRIGERATED - NON-MECH",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L110C24","WEST",9,"E2L110C24",706,"Average Miles between Interchange Switches, REFRIGERATED - NON-MECH",1341.08081054688,1544.11010742188,1667.91540527344,1694.30004882813,2126.42309570313,2399.01538085938,2616.21337890625,2764.52905273438,2713.0625,2854.8133796971701,3104.5641658341901,3078.9575051761099,3787.89952442804,3960.5664354436399,3257.5534019829802,2394.6140704305799]
["WEST-E2L110C25","WEST",9,"E2L110C25",707,"SEMs per Industry Switch, REFRIGERATED - NON-MECH",5.8928484916687003,5.9121565818786603,5.5734071731567401,5.2377877235412598,5.0537452697753897,5.0996809005737296,5.0501837730407697,5.0666599273681596,4.88950872421265,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L110C26","WEST",9,"E2L110C26",708,"SEMs per Interchange Switch, REFRIGERATED - NON-MECH",3.24106645584106,3.2516860961914098,3.0653741359710698,2.8807833194732702,2.7795600891113299,2.8048243522643999,2.7776012420654301,2.7866630554199201,2.68923020362854,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L110C27","WEST",9,"E2L110C27",709,"SEMs per Intraterminal Switch, REFRIGERATED - NON-MECH",8.8392744064331108,8.8682346343994105,8.3601112365722692,7.8566813468933097,7.5806179046630904,7.6495213508606001,7.5752758979797399,7.5999894142150897,7.3342628479003897,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L110C28","WEST",9,"E2L110C28",710,"SEMs per Interterminal Switch, REFRIGERATED - NON-MECH",7.0714192390441903,7.0945878028869602,6.68808841705322,6.2853455543518102,6.0644946098327601,6.1196165084838903,6.06022024154663,6.0799927711486799,5.8674111366271999,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L110C29","WEST",9,"E2L110C29",711,"SEMs per I&I Switch, REFRIGERATED - NON-MECH",1.47321224212646,1.47803914546967,1.3933517932891799,1.3094469308853101,1.2634363174438501,1.27491998672485,1.2625458240509,1.2666649818420399,1.2223774194717401,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L111C1","WEST",9,"E2L111C1",712,"Average Tare Weight, FLAT - TOFC",58.299999237060497,59.700000762939503,59.400001525878899,59.5,59.099998474121101,59.299999237060497,58.200000762939503,57.799999237060497,57.799999237060497,58.3,58.6,58.6,58.5,58.9,58.7,58.6]
["WEST-E2L111C2","WEST",9,"E2L111C2",713,"E/L Ratio, Railroad-Owned, FLAT - TOFC",1.1000177860260001,1.07684278488159,1.0764616727828999,1.0833165645599401,1.0732345581054701,1.0715790987014799,1.0719610452652,1.08132183551788,1.07545673847198,1.1070562835103099,1.0993413583114,1.1031681808638001,1.09847037668434,1.1072686125145199,1.1000340850366701,1.12676732803188]
["WEST-E2L111C3","WEST",9,"E2L111C3",714,"E/L Ratio, Privately-Owned, FLAT - TOFC",1.2276200056076001,1.208988904953,1.1980181932449301,1.1924748420715301,1.1736546754837001,1.1607689857482899,1.1602703332901001,1.07436227798462,1.07371270656586,1.0842609898904401,1.06528586460738,1.0730450829445799,1.0769669304664999,1.0739384918811501,1.0688893453435999,1.0932544412955401]
["WEST-E2L111C4","WEST",9,"E2L111C4",715,"E/L Ratio, All Freight Cars, FLAT - TOFC",1.1662838459014899,1.1367934942245499,1.1299811601638801,1.1307740211486801,1.1173011064529399,1.11232566833496,1.11265480518341,1.0766400098800699,1.0742161273956301,1.09065218084611,1.07511859073755,1.0811275409929899,1.0824145495593001,1.0831497771807199,1.07782932074588,1.10129352431054]
["WEST-E2L111C5","WEST",9,"E2L111C5",716,"Local circuity, FLAT - TOFC",1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.0690000057220499,1.069,1.069,1.069,1.069,1.069,1.069,1.069]
["WEST-E2L111C6","WEST",9,"E2L111C6",717,"Interline circuity, FLAT - TOFC",1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.10699999332428,1.107,1.107,1.107,1.107,1.107,1.107,1.107]
["WEST-E2L111C7","WEST",9,"E2L111C7",718,"Average circuity, FLAT - TOFC",1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.08500003814697,1.085,1.085,1.085,1.085,1.085,1.085,1.085]
["WEST-E2L111C8","WEST",9,"E2L111C8",719,"Spotted-to-Pulled Ratio, FLAT - TOFC",1.1662838459014899,1.1367934942245499,1.1299811601638801,1.1307740211486801,1.1173011064529399,1.11232566833496,1.11265480518341,1.0766400098800699,1.0742161273956301,1.09065218084611,1.07511859073755,1.0811275409929899,1.0824145495593001,1.0831497771807199,1.07782932074588,1.10129352431054]
["WEST-E2L111C9","WEST",9,"E2L111C9",720,"CD per Industry Switch, FLAT - TOFC",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L111C10","WEST",9,"E2L111C10",721,"CD per Interchange Switch, FLAT - TOFC",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L111C11","WEST",9,"E2L111C11",722,"CD per Intraterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L111C12","WEST",9,"E2L111C12",723,"CD per Interterminal Switch, FLAT - TOFC",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L111C13","WEST",9,"E2L111C13",724,"CD per I&I Switch, FLAT - TOFC",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L111C14","WEST",9,"E2L111C14",725,"CD per Load & Unload Industry Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L111C15","WEST",9,"E2L111C15",726,"CD per Load & Unload Intraterminal Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L111C16","WEST",9,"E2L111C16",727,"CD per Load & Unload Interterminal Switch, FLAT - TOFC",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L111C17","WEST",9,"E2L111C17",728,"CM per Industry Switch, FLAT - TOFC",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
[{"$f":"B8514&\"-\"&D8514","v":"WEST-E2L111C18"},"WEST",9,"E2L111C18",729,"CM per Interchange Switch, FLAT - TOFC",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L111C19","WEST",9,"E2L111C19",730,"CM per Intraterminal Switch, FLAT - TOFC",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L111C20","WEST",9,"E2L111C20",731,"CM per Interterminal Switch, FLAT - TOFC",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L111C21","WEST",9,"E2L111C21",732,"CM per I&I Switch, FLAT - TOFC",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L111C22","WEST",9,"E2L111C22",733,"Average CM per CD, Railroad-Owned, FLAT - TOFC",507.32373046875,537.49188232421898,546.41351318359398,622.74298095703102,574.45928955078102,533.28076171875,579.11706542968795,533.37854003906295,460.41845703125,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L111C23","WEST",9,"E2L111C23",734,"Average Miles between I&I Switches, FLAT - TOFC",4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162,4162]
["WEST-E2L111C24","WEST",9,"E2L111C24",735,"Average Miles between Interchange Switches, FLAT - TOFC",9805.5546875,12219.4130859375,14676.7021484375,13432.8115234375,11039.03515625,12082.201171875,6579.45654296875,6201.14208984375,5814.93359375,5356.92381056051,5591.2515659866704,5462.1261321404399,5006.0870311714998,4008.3080470973,4075.6411380723098,4113.48294821319]
["WEST-E2L111C25","WEST",9,"E2L111C25",736,"SEMs per Industry Switch, FLAT - TOFC",5.8928489685058603,5.9121561050415004,5.5734071731567401,5.2377877235412598,5.0537457466125497,5.0996809005737296,5.0501842498779297,5.0666604042053196,4.8895092010498002,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L111C26","WEST",9,"E2L111C26",737,"SEMs per Interchange Switch, FLAT - TOFC",3.24106669425964,3.2516863346099898,3.0653741359710698,2.8807830810546902,2.7795603275299099,2.8048245906829798,2.7776010036468501,2.7866630554199201,2.68923020362854,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L111C27","WEST",9,"E2L111C27",738,"SEMs per Intraterminal Switch, FLAT - TOFC",8.8392744064331108,8.8682355880737305,8.3601102828979492,7.8566818237304696,7.5806179046630904,7.6495213508606001,7.5752754211425799,7.5999898910522496,7.3342633247375497,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L111C28","WEST",9,"E2L111C28",739,"SEMs per Interterminal Switch, FLAT - TOFC",7.0714197158813503,7.0945878028869602,6.68808889389038,6.2853455543518102,6.0644946098327601,6.1196169853210396,6.06022024154663,6.0799927711486799,5.8674111366271999,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L111C29","WEST",9,"E2L111C29",740,"SEMs per I&I Switch, FLAT - TOFC",1.47321224212646,1.47803914546967,1.3933519124984699,1.30944716930389,1.2634363174438501,1.27491998672485,1.2625458240509,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L112C1","WEST",9,"E2L112C1",741,"Average Tare Weight, FLAT - MULTILEVEL",54.299999237060497,54.299999237060497,54.200000762939503,54.400001525878899,54.900001525878899,54.5,54,54,53.799999237060497,53.6,53.6,53.4,53.3,53.1,53.1,53.1]
["WEST-E2L112C2","WEST",9,"E2L112C2",742,"E/L Ratio, Railroad-Owned, FLAT - MULTILEVEL",1.3452216386795,1.3326047658920299,1.3299137353897099,1.3709254264831501,1.34403860569,1.35062909126282,1.3762795925140401,1.3746989965438801,1.3898005485534699,1.39834477401235,1.3753146397704701,1.3708173804271599,1.3300785806167801,1.3556140003702499,1.38738703215936,1.32112523972989]
["WEST-E2L112C3","WEST",9,"E2L112C3",743,"E/L Ratio, Privately-Owned, FLAT - MULTILEVEL",1.3376481533050499,1.3237333297729501,1.2949962615966799,1.31907522678375,1.3083466291427599,1.3312281370162999,1.3582787513732899,1.36157119274139,1.37260186672211,1.3744226814740901,1.3464264599474101,1.3408653670230899,1.31362055923454,1.3282925741154501,1.3447539186812001,1.28501532550479]
["WEST-E2L112C4","WEST",9,"E2L112C4",744,"E/L Ratio, All Freight Cars, FLAT - MULTILEVEL",1.33857321739197,1.32482898235321,1.2994967699050901,1.32631504535675,1.3129848241805999,1.33363926410675,1.36058020591736,1.36374771595001,1.3751016855239899,1.3775702955311599,1.3496437077913801,1.34433918800495,1.31596275348036,1.3325557350694199,1.35129416461508,1.29034448557875]
["WEST-E2L112C5","WEST",9,"E2L112C5",745,"Local circuity, FLAT - MULTILEVEL",1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999895095801,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999,1.0609999999999999]
["WEST-E2L112C6","WEST",9,"E2L112C6",746,"Interline circuity, FLAT - MULTILEVEL",1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.16600000858307,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999,1.1659999999999999]
["WEST-E2L112C7","WEST",9,"E2L112C7",747,"Average circuity, FLAT - MULTILEVEL",1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.15199995040894,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999,1.1519999999999999]
["WEST-E2L112C8","WEST",9,"E2L112C8",748,"Spotted-to-Pulled Ratio, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L112C9","WEST",9,"E2L112C9",749,"CD per Industry Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L112C10","WEST",9,"E2L112C10",750,"CD per Interchange Switch, FLAT - MULTILEVEL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L112C11","WEST",9,"E2L112C11",751,"CD per Intraterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L112C12","WEST",9,"E2L112C12",752,"CD per Interterminal Switch, FLAT - MULTILEVEL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L112C13","WEST",9,"E2L112C13",753,"CD per I&I Switch, FLAT - MULTILEVEL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L112C14","WEST",9,"E2L112C14",754,"CD per Load & Unload Industry Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L112C15","WEST",9,"E2L112C15",755,"CD per Load & Unload Intraterminal Switch, FLAT - MULTILEVEL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L112C16","WEST",9,"E2L112C16",756,"CD per Load & Unload Interterminal Switch, FLAT - MULTILEVEL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L112C17","WEST",9,"E2L112C17",757,"CM per Industry Switch, FLAT - MULTILEVEL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L112C18","WEST",9,"E2L112C18",758,"CM per Interchange Switch, FLAT - MULTILEVEL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L112C19","WEST",9,"E2L112C19",759,"CM per Intraterminal Switch, FLAT - MULTILEVEL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L112C20","WEST",9,"E2L112C20",760,"CM per Interterminal Switch, FLAT - MULTILEVEL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L112C21","WEST",9,"E2L112C21",761,"CM per I&I Switch, FLAT - MULTILEVEL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L112C22","WEST",9,"E2L112C22",762,"Average CM per CD, Railroad-Owned, FLAT - MULTILEVEL",507.32376098632801,537.49188232421898,546.41351318359398,622.74298095703102,574.45928955078102,533.28076171875,579.11700439453102,533.37860107421898,460.41842651367199,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L112C23","WEST",9,"E2L112C23",763,"Average Miles between I&I Switches, FLAT - MULTILEVEL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L112C24","WEST",9,"E2L112C24",764,"Average Miles between Interchange Switches, FLAT - MULTILEVEL",5584.5556640625,5456.90478515625,5016.99560546875,4154.3984375,3505.26000976563,3960.43603515625,4509.560546875,4679.64111328125,4123.70166015625,3793.3965546945701,3033.3300237671801,2796.5157631023899,3290.7414753926,2669.97661428424,3006.7664527901402,2640.6795349488202]
["WEST-E2L112C25","WEST",9,"E2L112C25",765,"SEMs per Industry Switch, FLAT - MULTILEVEL",5.8928484916687003,5.9121565818786603,5.5734066963195801,5.2377877235412598,5.0537457466125497,5.0996813774108896,5.0501842498779297,5.0666599273681596,4.8895092010498002,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L112C26","WEST",9,"E2L112C26",766,"SEMs per Interchange Switch, FLAT - MULTILEVEL",3.24106669425964,3.2516860961914098,3.0653741359710698,2.8807833194732702,2.7795603275299099,2.8048245906829798,2.7776012420654301,2.7866628170013401,2.68923020362854,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L112C27","WEST",9,"E2L112C27",767,"SEMs per Intraterminal Switch, FLAT - MULTILEVEL",8.8392734527587908,8.8682346343994105,8.3601112365722692,7.8566813468933097,7.5806174278259304,7.6495208740234402,7.5752763748168901,7.5999903678893999,7.3342633247375497,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.5047952272936502]
["WEST-E2L112C28","WEST",9,"E2L112C28",768,"SEMs per Interterminal Switch, FLAT - MULTILEVEL",7.0714192390441903,7.0945878028869602,6.68808841705322,6.2853460311889604,6.0644941329956099,6.1196165084838903,6.06022071838379,6.0799922943115199,5.8674111366271999,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L112C29","WEST",9,"E2L112C29",769,"SEMs per I&I Switch, FLAT - MULTILEVEL",1.47321212291718,1.47803914546967,1.3933516740798999,1.3094469308853101,1.2634361982345601,1.27492010593414,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L113C1","WEST",9,"E2L113C1",770,"Average Tare Weight, FLAT - GENERAL",33.599998474121101,34.099998474121101,34,32.900001525878899,32.200000762939503,33,32.200000762939503,32.799999237060497,32.799999237060497,32.5,32.4,32.200000000000003,32.1,32.200000000000003,32.299999999999997,32.299999999999997]
["WEST-E2L113C2","WEST",9,"E2L113C2",771,"E/L Ratio, Railroad-Owned, FLAT - GENERAL",2.37917923927307,2.3682487010955802,2.4566724300384499,3.14333891868591,2.6306428909301798,2.8487739562988299,2.89248895645142,2.57250952720642,2.4540944099426301,2.0561370123691698,2.5910987482614698,2.63917525773196,2.3356643356643398,2.4675834970530501,2.3322147651006699,2.2784810126582302]
["WEST-E2L113C3","WEST",9,"E2L113C3",772,"E/L Ratio, Privately-Owned, FLAT - GENERAL",2.3860182762146001,1.97187495231628,2.2860412597656299,2.3851590156555198,1.9634146690368699,2.1126761436462398,2.6314606666564901,2.5768024921417201,2.24091768264771,2.4714285714285702,2.0754716981132102,2.2665799739921999,2.2814371257485,2.4734411085450301,1.8738738738738701,1.9911504424778801]
["WEST-E2L113C4","WEST",9,"E2L113C4",773,"E/L Ratio, All Freight Cars, FLAT - GENERAL",2.3805470466613801,2.2859921455383301,2.4098050594329798,2.8984017372131299,2.5633456707000701,2.6434185504913299,2.78914594650269,2.57374095916748,2.3702032566070601,2.17471108089735,2.8166939443535202,2.4106858054226499,2.30645161290323,2.4702760084925699,2.1365384615384602,2.23489932885906]
["WEST-E2L113C5","WEST",9,"E2L113C5",774,"Local circuity, FLAT - GENERAL",1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0859999656677199,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001,1.0860000000000001]
["WEST-E2L113C6","WEST",9,"E2L113C6",775,"Interline circuity, FLAT - GENERAL",1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.1770000457763701,1.177,1.177,1.177,1.177,1.177,1.177,1.177]
["WEST-E2L113C7","WEST",9,"E2L113C7",776,"Average circuity, FLAT - GENERAL",1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.1529999971389799,1.153,1.153,1.153,1.153,1.153,1.153,1.153]
["WEST-E2L113C8","WEST",9,"E2L113C8",777,"Spotted-to-Pulled Ratio, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L113C9","WEST",9,"E2L113C9",778,"CD per Industry Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L113C10","WEST",9,"E2L113C10",779,"CD per Interchange Switch, FLAT - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L113C11","WEST",9,"E2L113C11",780,"CD per Intraterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L113C12","WEST",9,"E2L113C12",781,"CD per Interterminal Switch, FLAT - GENERAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L113C13","WEST",9,"E2L113C13",782,"CD per I&I Switch, FLAT - GENERAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L113C14","WEST",9,"E2L113C14",783,"CD per Load & Unload Industry Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L113C15","WEST",9,"E2L113C15",784,"CD per Load & Unload Intraterminal Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L113C16","WEST",9,"E2L113C16",785,"CD per Load & Unload Interterminal Switch, FLAT - GENERAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L113C17","WEST",9,"E2L113C17",786,"CM per Industry Switch, FLAT - GENERAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L113C18","WEST",9,"E2L113C18",787,"CM per Interchange Switch, FLAT - GENERAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L113C19","WEST",9,"E2L113C19",788,"CM per Intraterminal Switch, FLAT - GENERAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L113C20","WEST",9,"E2L113C20",789,"CM per Interterminal Switch, FLAT - GENERAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L113C21","WEST",9,"E2L113C21",790,"CM per I&I Switch, FLAT - GENERAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L113C22","WEST",9,"E2L113C22",791,"Average CM per CD, Railroad-Owned, FLAT - GENERAL",507.32379150390602,537.49188232421898,546.41357421875,622.742919921875,574.45928955078102,533.28076171875,579.11700439453102,533.37860107421898,460.41845703125,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L113C23","WEST",9,"E2L113C23",792,"Average Miles between I&I Switches, FLAT - GENERAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
[{"$f":"B8578&\"-\"&D8578","v":"WEST-E2L113C24"},"WEST",9,"E2L113C24",793,"Average Miles between Interchange Switches, FLAT - GENERAL",739.13684082031295,605.07568359375,974.71563720703102,446.19836425781301,376.21469116210898,468.04595947265602,402.14666748046898,444.23599243164102,616.66192626953102,805.50973775193597,727.72814467249702,1088.3014426480199,892.97502310452796,973.63206117548305,1024.88162585602,552.736634259982]
["WEST-E2L113C25","WEST",9,"E2L113C25",794,"SEMs per Industry Switch, FLAT - GENERAL",5.8928489685058603,5.9121565818786603,5.5734071731567401,5.2377877235412598,5.0537457466125497,5.0996809005737296,5.0501842498779297,5.0666599273681596,4.88950872421265,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L113C26","WEST",9,"E2L113C26",795,"SEMs per Interchange Switch, FLAT - GENERAL",3.24106669425964,3.2516863346099898,3.0653741359710698,2.8807830810546902,2.7795603275299099,2.8048243522643999,2.7776012420654301,2.7866625785827601,2.6892297267913801,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L113C27","WEST",9,"E2L113C27",796,"SEMs per Intraterminal Switch, FLAT - GENERAL",8.8392744064331108,8.8682355880737305,8.3601112365722692,7.8566808700561497,7.5806179046630904,7.6495208740234402,7.5752758979797399,7.5999898910522496,7.3342628479003897,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L113C28","WEST",9,"E2L113C28",797,"SEMs per Interterminal Switch, FLAT - GENERAL",7.0714197158813503,7.0945878028869602,6.68808889389038,6.2853455543518102,6.0644941329956099,6.1196169853210396,6.06022071838379,6.0799922943115199,5.86741065979004,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L113C29","WEST",9,"E2L113C29",798,"SEMs per I&I Switch, FLAT - GENERAL",1.47321212291718,1.47803914546967,1.3933516740798999,1.3094469308853101,1.2634361982345601,1.27491998672485,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L114C1","WEST",9,"E2L114C1",799,"Average Tare Weight, FLAT - OTHER",34.599998474121101,34.599998474121101,34.700000762939503,34.700000762939503,34.700000762939503,34.700000762939503,35.099998474121101,35.200000762939503,35.200000762939503,35.299999999999997,35.299999999999997,35.299999999999997,35.4,35.299999999999997,35.4,35.4]
["WEST-E2L114C2","WEST",9,"E2L114C2",800,"E/L Ratio, Railroad-Owned, FLAT - OTHER",2.00496578216553,2.00922751426697,2.0045289993286102,1.9951980113983201,1.95815718173981,1.93915832042694,1.9422347545623799,1.96155869960785,1.96120274066925,1.95640433188523,1.9459578231218699,1.9625518817329699,1.94820523623936,1.9630940663869401,1.97305332560056,1.9689474521569199]
["WEST-E2L114C3","WEST",9,"E2L114C3",801,"E/L Ratio, Privately-Owned, FLAT - OTHER",1.92259073257446,1.94982349872589,1.97609043121338,1.9225429296493499,1.8919826745986901,1.8930304050445601,1.9275261163711499,1.91547083854675,1.8678063154220601,1.9267051797132599,1.90477414680604,1.88970813974907,1.9243861462910301,1.93933704898797,1.9407329673150799,1.9168743046808201]
["WEST-E2L114C4","WEST",9,"E2L114C4",802,"E/L Ratio, All Freight Cars, FLAT - OTHER",1.9693752527236901,1.9829949140548699,1.9916901588439899,1.9662036895752,1.9268282651901201,1.91477847099304,1.9338862895965601,1.9354448318481401,1.90719854831696,1.9408598676381099,1.9261287872394299,1.9237587879448499,1.9344856163126001,1.94977790369418,1.9544545063421099,1.9401628388028]
["WEST-E2L114C5","WEST",9,"E2L114C5",803,"Local circuity, FLAT - OTHER",1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000591278101,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001,1.0880000000000001]
["WEST-E2L114C6","WEST",9,"E2L114C6",804,"Interline circuity, FLAT - OTHER",1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.16999995708466,1.17,1.17,1.17,1.17,1.17,1.17,1.17]
["WEST-E2L114C7","WEST",9,"E2L114C7",805,"Average circuity, FLAT - OTHER",1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.1549999713897701,1.155,1.155,1.155,1.155,1.155,1.155,1.155]
["WEST-E2L114C8","WEST",9,"E2L114C8",806,"Spotted-to-Pulled Ratio, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L114C9","WEST",9,"E2L114C9",807,"CD per Industry Switch, FLAT - OTHER",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L114C10","WEST",9,"E2L114C10",808,"CD per Interchange Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L114C11","WEST",9,"E2L114C11",809,"CD per Intraterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L114C12","WEST",9,"E2L114C12",810,"CD per Interterminal Switch, FLAT - OTHER",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L114C13","WEST",9,"E2L114C13",811,"CD per I&I Switch, FLAT - OTHER",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L114C14","WEST",9,"E2L114C14",812,"CD per Load & Unload Industry Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L114C15","WEST",9,"E2L114C15",813,"CD per Load & Unload Intraterminal Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L114C16","WEST",9,"E2L114C16",814,"CD per Load & Unload Interterminal Switch, FLAT - OTHER",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L114C17","WEST",9,"E2L114C17",815,"CM per Industry Switch, FLAT - OTHER",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L114C18","WEST",9,"E2L114C18",816,"CM per Interchange Switch, FLAT - OTHER",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L114C19","WEST",9,"E2L114C19",817,"CM per Intraterminal Switch, FLAT - OTHER",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L114C20","WEST",9,"E2L114C20",818,"CM per Interterminal Switch, FLAT - OTHER",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L114C21","WEST",9,"E2L114C21",819,"CM per I&I Switch, FLAT - OTHER",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L114C22","WEST",9,"E2L114C22",820,"Average CM per CD, Railroad-Owned, FLAT - OTHER",507.32376098632801,537.49188232421898,546.41357421875,622.74298095703102,574.45928955078102,533.28082275390602,579.11700439453102,533.37854003906295,460.41848754882801,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L114C23","WEST",9,"E2L114C23",821,"Average Miles between I&I Switches, FLAT - OTHER",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L114C24","WEST",9,"E2L114C24",822,"Average Miles between Interchange Switches, FLAT - OTHER",1587.68701171875,1172.41076660156,1334.77868652344,8213.90625,1581.22607421875,1481.34265136719,1485.58471679688,1514.171875,1646.74401855469,1428.03819580965,1743.84987562078,1632.2832637075301,1682.8815682965101,1618.28287404815,1958.7466109946399,1946.1679206891999]
["WEST-E2L114C25","WEST",9,"E2L114C25",823,"SEMs per Industry Switch, FLAT - OTHER",5.8928484916687003,5.9121565818786603,5.5734071731567401,5.2377877235412598,5.0537452697753897,5.0996809005737296,5.0501842498779297,5.0666604042053196,4.8895092010498002,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L114C26","WEST",9,"E2L114C26",824,"SEMs per Interchange Switch, FLAT - OTHER",3.24106669425964,3.2516863346099898,3.0653738975524898,2.8807828426361102,2.7795600891113299,2.8048243522643999,2.7776012420654301,2.7866628170013401,2.68922996520996,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L114C27","WEST",9,"E2L114C27",825,"SEMs per Intraterminal Switch, FLAT - OTHER",8.8392734527587908,8.8682346343994105,8.3601112365722692,7.8566813468933097,7.5806183815002397,7.6495213508606001,7.5752758979797399,7.5999903678893999,7.3342633247375497,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L114C28","WEST",9,"E2L114C28",826,"SEMs per Interterminal Switch, FLAT - OTHER",7.0714192390441903,7.0945873260498002,6.68808794021606,6.2853455543518102,6.0644946098327601,6.1196169853210396,6.06022071838379,6.0799922943115199,5.8674111366271999,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L114C29","WEST",9,"E2L114C29",827,"SEMs per I&I Switch, FLAT - OTHER",1.47321224212646,1.47803914546967,1.3933517932891799,1.3094469308853101,1.2634361982345601,1.27492010593414,1.26254594326019,1.2666651010513299,1.2223771810531601,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L115C1","WEST",9,"E2L115C1",828,"Average Tare Weight, TANK <22,000 GAL",32.700000000000003,32.700000000000003,32.6,32.6,32.6,32.6,32.6,32.6,32.6,32.700000000000003,32.700000000000003,32.799999999999997,32.799999999999997,32.9,32.9,32.9]
["WEST-E2L115C2","WEST",9,"E2L115C2",829,"E/L Ratio, Railroad-Owned, TANK <22,000 GAL",2.1786434650421098,2.1863048076629599,2.2478885650634801,1.6600825786590601,1.5641393661498999,1.6894899606704701,1.77481400966644,2.3789808750152601,2.4542617797851598,2.3557632398753898,2.4612176814011701,2.2287581699346402,2.1945080091533198,1.7898782831518301,1.8898370830100899,2.0337078651685401]
["WEST-E2L115C3","WEST",9,"E2L115C3",830,"E/L Ratio, Privately-Owned, TANK <22,000 GAL",2.0398490428924601,2.0386283397674601,2.0678505897521999,2.0455868244171098,2.0231819152832,2.0537905693054199,2.04492235183716,2.0268528461456299,2.0197348594665501,2.03083342281673,2.0339760525104502,2.0289202844311398,2.0248219716920501,2.0348559433575502,2.04817336980773,2.0207516314420499]
["WEST-E2L115C4","WEST",9,"E2L115C4",831,"E/L Ratio, All Freight Cars, TANK <22,000 GAL",2.0398490428924601,2.0386283397674601,2.0678505897521999,2.0455868244171098,2.0231819152832,2.0537905693054199,2.04492235183716,2.0268528461456299,2.0197348594665501,2.03083342281673,2.0339760525104502,2.0289202844311398,2.0248219716920501,2.0348559433575502,2.04817336980773,2.0207516314420499]
["WEST-E2L115C5","WEST",9,"E2L115C5",832,"Local circuity, TANK <22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["WEST-E2L115C6","WEST",9,"E2L115C6",833,"Interline circuity, TANK <22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["WEST-E2L115C7","WEST",9,"E2L115C7",834,"Average circuity, TANK <22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["WEST-E2L115C8","WEST",9,"E2L115C8",835,"Spotted-to-Pulled Ratio, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L115C9","WEST",9,"E2L115C9",836,"CD per Industry Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L115C10","WEST",9,"E2L115C10",837,"CD per Interchange Switch, TANK <22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L115C11","WEST",9,"E2L115C11",838,"CD per Intraterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L115C12","WEST",9,"E2L115C12",839,"CD per Interterminal Switch, TANK <22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L115C13","WEST",9,"E2L115C13",840,"CD per I&I Switch, TANK <22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L115C14","WEST",9,"E2L115C14",841,"CD per Load & Unload Industry Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L115C15","WEST",9,"E2L115C15",842,"CD per Load & Unload Intraterminal Switch, TANK <22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L115C16","WEST",9,"E2L115C16",843,"CD per Load & Unload Interterminal Switch, TANK <22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L115C17","WEST",9,"E2L115C17",844,"CM per Industry Switch, TANK <22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L115C18","WEST",9,"E2L115C18",845,"CM per Interchange Switch, TANK <22,000 GAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L115C19","WEST",9,"E2L115C19",846,"CM per Intraterminal Switch, TANK <22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L115C20","WEST",9,"E2L115C20",847,"CM per Interterminal Switch, TANK <22,000 GAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L115C21","WEST",9,"E2L115C21",848,"CM per I&I Switch, TANK <22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L115C22","WEST",9,"E2L115C22",849,"Average CM per CD, Railroad-Owned, TANK <22,000 GAL",507.32379150390602,537.49188232421898,546.41357421875,622.742919921875,574.459228515625,533.28076171875,579.11700439453102,533.37860107421898,460.41845703125,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L115C23","WEST",9,"E2L115C23",850,"Average Miles between I&I Switches, TANK <22,000 GAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L115C24","WEST",9,"E2L115C24",851,"Average Miles between Interchange Switches, TANK <22,000 GAL",882.26849365234398,932.08892822265602,1018.28155517578,1104.09582519531,1041.70764160156,956.75811767578102,914.664306640625,915.01641845703102,922.90155029296898,1481.24674626722,950.65699180517902,951.39732962896505,1083.98676743807,1419.25448652963,1583.37159831542,1680.42389813462]
["WEST-E2L115C25","WEST",9,"E2L115C25",852,"SEMs per Industry Switch, TANK <22,000 GAL",5.8928489685058603,5.9121565818786603,5.5734071731567401,5.2377877235412598,5.0537457466125497,5.0996813774108896,5.0501842498779297,5.0666604042053196,4.8895092010498002,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L115C26","WEST",9,"E2L115C26",853,"SEMs per Interchange Switch, TANK <22,000 GAL",3.24106669425964,3.2516858577728298,3.0653741359710698,2.8807833194732702,2.7795603275299099,2.8048245906829798,2.7776012420654301,2.7866630554199201,2.68923020362854,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L115C27","WEST",9,"E2L115C27",854,"SEMs per Intraterminal Switch, TANK <22,000 GAL",8.8392744064331108,8.8682355880737305,8.3601112365722692,7.8566818237304696,7.5806183815002397,7.6495203971862802,7.5752754211425799,7.5999898910522496,7.3342628479003897,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L115C28","WEST",9,"E2L115C28",855,"SEMs per Interterminal Switch, TANK <22,000 GAL",7.0714197158813503,7.0945873260498002,6.68808889389038,6.2853455543518102,6.0644941329956099,6.1196169853210396,6.06022071838379,6.0799922943115199,5.86741065979004,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L115C29","WEST",9,"E2L115C29",856,"SEMs per I&I Switch, TANK <22,000 GAL",1.47321212291718,1.47803914546967,1.3933517932891799,1.3094469308853101,1.2634361982345601,1.27492010593414,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
[{"$f":"B8642&\"-\"&D8642","v":"WEST-E2L116C1"},"WEST",9,"E2L116C1",857,"Average Tare Weight, TANK >=22,000 GAL",39.799999999999997,39.200000000000003,38.9,38.9,39,38.9,38.9,39.1,39.5,40.1,40.4,40.700000000000003,41,41.4,41.7,41.9]
["WEST-E2L116C2","WEST",9,"E2L116C2",858,"E/L Ratio, Railroad-Owned, TANK >=22,000 GAL",2.1786434650421098,2.1863048076629599,2.2478885650634801,1.6600825786590601,1.5641393661498999,1.6894899606704701,1.77481400966644,2.3789808750152601,2.4542617797851598,2.3557632398753898,2.4612176814011701,2.2287581699346402,2.1945080091533198,1.7898782831518301,1.8898370830100899,2.0337078651685401]
["WEST-E2L116C3","WEST",9,"E2L116C3",859,"E/L Ratio, Privately-Owned, TANK >=22,000 GAL",2.0472397804260298,2.0505642890930198,2.0903384685516402,2.0837280750274698,2.0655438899993901,2.0732233524322501,2.0353300571441699,2.0426058769226101,2.0391647815704301,2.0420860470364799,2.0420030484286298,2.0428924346984401,2.0271643064953002,2.0386153797608202,2.0510823002419301,2.0321591267536099]
["WEST-E2L116C4","WEST",9,"E2L116C4",860,"E/L Ratio, All Freight Cars, TANK >=22,000 GAL",2.0472397804260298,2.0505642890930198,2.0903384685516402,2.0837280750274698,2.0655438899993901,2.0732233524322501,2.0353300571441699,2.0426058769226101,2.0391647815704301,2.0420860470364799,2.0420030484286298,2.0428924346984401,2.0271643064953002,2.0386153797608202,2.0510823002419301,2.0321591267536099]
["WEST-E2L116C5","WEST",9,"E2L116C5",861,"Local circuity, TANK >=22,000 GAL",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["WEST-E2L116C6","WEST",9,"E2L116C6",862,"Interline circuity, TANK >=22,000 GAL",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["WEST-E2L116C7","WEST",9,"E2L116C7",863,"Average circuity, TANK >=22,000 GAL",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["WEST-E2L116C8","WEST",9,"E2L116C8",864,"Spotted-to-Pulled Ratio, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L116C9","WEST",9,"E2L116C9",865,"CD per Industry Switch, TANK >=22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L116C10","WEST",9,"E2L116C10",866,"CD per Interchange Switch, TANK >=22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L116C11","WEST",9,"E2L116C11",867,"CD per Intraterminal Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L116C12","WEST",9,"E2L116C12",868,"CD per Interterminal Switch, TANK >=22,000 GAL",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L116C13","WEST",9,"E2L116C13",869,"CD per I&I Switch, TANK >=22,000 GAL",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L116C14","WEST",9,"E2L116C14",870,"CD per Load & Unload Industry Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L116C15","WEST",9,"E2L116C15",871,"CD per Load & Unload Intraterminal Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L116C16","WEST",9,"E2L116C16",872,"CD per Load & Unload Interterminal Switch, TANK >=22,000 GAL",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L116C17","WEST",9,"E2L116C17",873,"CM per Industry Switch, TANK >=22,000 GAL",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L116C18","WEST",9,"E2L116C18",874,"CM per Interchange Switch, TANK >=22,000 GAL",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L116C19","WEST",9,"E2L116C19",875,"CM per Intraterminal Switch, TANK >=22,000 GAL",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L116C20","WEST",9,"E2L116C20",876,"CM per Interterminal Switch, TANK >=22,000 GAL",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L116C21","WEST",9,"E2L116C21",877,"CM per I&I Switch, TANK >=22,000 GAL",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L116C22","WEST",9,"E2L116C22",878,"Average CM per CD, Railroad-Owned, TANK >=22,000 GAL",507.32379150390602,537.49188232421898,546.41357421875,622.742919921875,574.459228515625,533.28076171875,579.11700439453102,533.37860107421898,460.41845703125,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L116C23","WEST",9,"E2L116C23",879,"Average Miles between I&I Switches, TANK >=22,000 GAL",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L116C24","WEST",9,"E2L116C24",880,"Average Miles between Interchange Switches, TANK >=22,000 GAL",882.26849365234398,932.08892822265602,1018.28155517578,1104.09582519531,1041.70764160156,956.75811767578102,914.664306640625,915.01641845703102,922.90155029296898,1481.24674626722,950.65699180517902,951.39732962896505,1083.98676743807,1419.25448652963,1583.37159831542,1680.42389813462]
["WEST-E2L116C25","WEST",9,"E2L116C25",881,"SEMs per Industry Switch, TANK >=22,000 GAL",5.8928489685058603,5.9121565818786603,5.5734071731567401,5.2377877235412598,5.0537457466125497,5.0996813774108896,5.0501842498779297,5.0666604042053196,4.8895092010498002,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L116C26","WEST",9,"E2L116C26",882,"SEMs per Interchange Switch, TANK >=22,000 GAL",3.24106669425964,3.2516858577728298,3.0653741359710698,2.8807833194732702,2.7795603275299099,2.8048245906829798,2.7776012420654301,2.7866630554199201,2.68923020362854,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L116C27","WEST",9,"E2L116C27",883,"SEMs per Intraterminal Switch, TANK >=22,000 GAL",8.8392744064331108,8.8682355880737305,8.3601112365722692,7.8566818237304696,7.5806183815002397,7.6495203971862802,7.5752754211425799,7.5999898910522496,7.3342628479003897,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L116C28","WEST",9,"E2L116C28",884,"SEMs per Interterminal Switch, TANK >=22,000 GAL",7.0714197158813503,7.0945873260498002,6.68808889389038,6.2853455543518102,6.0644941329956099,6.1196169853210396,6.06022071838379,6.0799922943115199,5.86741065979004,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L116C29","WEST",9,"E2L116C29",885,"SEMs per I&I Switch, TANK >=22,000 GAL",1.47321212291718,1.47803914546967,1.3933517932891799,1.3094469308853101,1.2634361982345601,1.27492010593414,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L117C1","WEST",9,"E2L117C1",886,"Average Tare Weight, ALL OTHER FREIGHT CARS",36.799999237060497,39.200000762939503,36.5,36.599998474121101,36.700000762939503,36.599998474121101,36.799999237060497,37.099998474121101,37.5,38.1,38.4,38.6,38.9,39.299999999999997,39.6,39.799999999999997]
["WEST-E2L117C2","WEST",9,"E2L117C2",887,"E/L Ratio, Railroad-Owned, ALL OTHER FREIGHT CARS",2.1786434650421098,2.1863048076629599,2.2478885650634801,1.6600825786590601,1.5641393661498999,1.6894899606704701,1.77481400966644,2.3789808750152601,2.4542617797851598,2.3557632398753898,2.4612176814011701,2.2287581699346402,2.1945080091533198,1.7898782831518301,1.8898370830100899,2.0337078651685401]
["WEST-E2L117C3","WEST",9,"E2L117C3",888,"E/L Ratio, Privately-Owned, ALL OTHER FREIGHT CARS",1.5562998056411701,1.60818791389465,1.5276030302047701,1.90880739688873,2.0095734596252401,2.8486747741699201,1.24125993251801,1.4703516960144001,1.5498248338699301,1.2710285714285701,1.52852153667055,1.49609535552815,1.3893921923900501,1.42821285140562,1.4228525980911999,1.38812671489149]
["WEST-E2L117C4","WEST",9,"E2L117C4",889,"E/L Ratio, All Freight Cars, ALL OTHER FREIGHT CAR",2.03223752975464,2.0349888801574698,2.0664968490600599,2.0561759471893302,2.0377893447875999,2.0629248619079599,2.03598833084106,2.0346419811248802,2.0327317714691202,2.0258773806631099,2.0390345913621601,2.0383504295797401,2.0246692336512702,2.03650530995824,2.0489327451397399,2.0284146836691299]
["WEST-E2L117C5","WEST",9,"E2L117C5",890,"Local circuity, ALL OTHER FREIGHT CARS",1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1460000276565601,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999,1.1459999999999999]
["WEST-E2L117C6","WEST",9,"E2L117C6",891,"Interline circuity, ALL OTHER FREIGHT CARS",1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.1900000572204601,1.19,1.19,1.19,1.19,1.19,1.19,1.19]
["WEST-E2L117C7","WEST",9,"E2L117C7",892,"Average circuity, ALL OTHER FREIGHT CARS",1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.17900002002716,1.179,1.179,1.179,1.179,1.179,1.179,1.179]
["WEST-E2L117C8","WEST",9,"E2L117C8",893,"Spotted-to-Pulled Ratio, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L117C9","WEST",9,"E2L117C9",894,"CD per Industry Switch, ALL OTHER FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L117C10","WEST",9,"E2L117C10",895,"CD per Interchange Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L117C11","WEST",9,"E2L117C11",896,"CD per Intraterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L117C12","WEST",9,"E2L117C12",897,"CD per Interterminal Switch, ALL OTHER FREIGHT CARS",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L117C13","WEST",9,"E2L117C13",898,"CD per I&I Switch, ALL OTHER FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L117C14","WEST",9,"E2L117C14",899,"CD per Load & Unload Industry Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L117C15","WEST",9,"E2L117C15",900,"CD per Load & Unload Intraterminal Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L117C16","WEST",9,"E2L117C16",901,"CD per Load & Unload Interterminal Switch, ALL OTHER FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L117C17","WEST",9,"E2L117C17",902,"CM per Industry Switch, ALL OTHER FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L117C18","WEST",9,"E2L117C18",903,"CM per Interchange Switch, ALL OTHER FREIGHT CARS",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L117C19","WEST",9,"E2L117C19",904,"CM per Intraterminal Switch, ALL OTHER FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L117C20","WEST",9,"E2L117C20",905,"CM per Interterminal Switch, ALL OTHER FREIGHT CARS",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L117C21","WEST",9,"E2L117C21",906,"CM per I&I Switch, ALL OTHER FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L117C22","WEST",9,"E2L117C22",907,"Average CM per CD, Railroad-Owned, ALL OTHER FREIGHT CARS",507.32379150390602,537.49188232421898,546.41357421875,622.742919921875,574.459228515625,533.28076171875,579.11700439453102,533.37860107421898,460.41845703125,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L117C23","WEST",9,"E2L117C23",908,"Average Miles between I&I Switches, ALL OTHER FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L117C24","WEST",9,"E2L117C24",909,"Average Miles between Interchange Switches, ALL OTHER FREIGHT CARS",882.26849365234398,932.08892822265602,1018.28155517578,1104.09582519531,1041.70764160156,956.75811767578102,914.664306640625,915.01641845703102,922.90155029296898,1481.24674626722,950.65699180517902,951.39732962896505,1083.98676743807,1419.25448652963,1583.37159831542,1680.42389813462]
["WEST-E2L117C25","WEST",9,"E2L117C25",910,"SEMs per Industry Switch, ALL OTHER FREIGHT CARS",5.8928489685058603,5.9121565818786603,5.5734071731567401,5.2377877235412598,5.0537457466125497,5.0996813774108896,5.0501842498779297,5.0666604042053196,4.8895092010498002,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L117C26","WEST",9,"E2L117C26",911,"SEMs per Interchange Switch, ALL OTHER FREIGHT CARS",3.24106669425964,3.2516858577728298,3.0653741359710698,2.8807833194732702,2.7795603275299099,2.8048245906829798,2.7776012420654301,2.7866630554199201,2.68923020362854,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L117C27","WEST",9,"E2L117C27",912,"SEMs per Intraterminal Switch, ALL OTHER FREIGHT CARS",8.8392744064331108,8.8682355880737305,8.3601112365722692,7.8566818237304696,7.5806183815002397,7.6495203971862802,7.5752754211425799,7.5999898910522496,7.3342628479003897,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L117C28","WEST",9,"E2L117C28",913,"SEMs per Interterminal Switch, ALL OTHER FREIGHT CARS",7.0714197158813503,7.0945873260498002,6.68808889389038,6.2853455543518102,6.0644941329956099,6.1196169853210396,6.06022071838379,6.0799922943115199,5.86741065979004,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L117C29","WEST",9,"E2L117C29",914,"SEMs per I&I Switch, ALL OTHER FREIGHT CARS",1.47321212291718,1.47803914546967,1.3933517932891799,1.3094469308853101,1.2634361982345601,1.27492010593414,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L118C1","WEST",9,"E2L118C1",915,"Average Tare Weight, AVERAGE ALL FREIGHT CARS",34.400001525878899,34.400001525878899,34.299999237060497,34.299999237060497,34.299999237060497,34.299999237060497,34.200000762939503,34.299999237060497,34.400001525878899,34.6,34.799999999999997,34.799999999999997,34.9,35.200000000000003,35.299999999999997,35.4]
["WEST-E2L118C2","WEST",9,"E2L118C2",916,"E/L Ratio, Railroad-Owned, AVERAGE ALL FREIGHT CARS",1.7118117809295701,1.71254765987396,1.70487916469574,1.6954808235168499,1.6703418493270901,1.66139793395996,1.65631568431854,1.7295227050781301,1.73257219791412,1.7492965318053499,1.72153068933576,1.7425521538025901,1.74197285413488,1.7330243362589399,1.7190561743785699,1.74133126335053]
["WEST-E2L118C3","WEST",9,"E2L118C3",917,"E/L Ratio, Privately-Owned, AVERAGE ALL FREIGHT CARS",1.84026420116425,1.8564465045928999,1.8752081394195601,1.8953914642334,1.86263871192932,1.85486376285553,1.84106469154358,1.74926257133484,1.7398309707641599,1.7292798756701799,1.6947448298068599,1.7032002705920499,1.70199273451151,1.71502775103234,1.6909617299145601,1.6834331636047399]
["WEST-E2L118C4","WEST",9,"E2L118C4",918,"E/L Ratio, All Freight Cars, AVERAGE ALL FREIGHT CARS",1.7907294034957899,1.7989199161529501,1.80665230751038,1.8181722164154099,1.7870107889175399,1.7810649871826201,1.7732794284820601,1.74338603019714,1.7377748489379901,1.73483464452142,1.70264355106048,1.71430563024186,1.7131693506240999,1.7200112904882401,1.6993361489038901,1.69969970184774]
["WEST-E2L118C5","WEST",9,"E2L118C5",919,"Local circuity, AVERAGE ALL FREIGHT CARS",1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.0970000028610201,1.097,1.097,1.097,1.097,1.097,1.097,1.097]
["WEST-E2L118C6","WEST",9,"E2L118C6",920,"Interline circuity, AVERAGE ALL FREIGHT CARS",1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.15699994564056,1.157,1.157,1.157,1.157,1.157,1.157,1.157]
[{"$f":"B8706&\"-\"&D8706","v":"WEST-E2L118C7"},"WEST",9,"E2L118C7",921,"Average circuity, AVERAGE ALL FREIGHT CARS",1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.1349999904632599,1.135,1.135,1.135,1.135,1.135,1.135,1.135]
["WEST-E2L118C8","WEST",9,"E2L118C8",922,"Spotted-to-Pulled Ratio, AVERAGE ALL FREIGHT CARS",1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.8999999761581401,1.9,1.9,1.9,1.9,1.9,1.9,1.9]
["WEST-E2L118C9","WEST",9,"E2L118C9",923,"CD per Industry Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L118C10","WEST",9,"E2L118C10",924,"CD per Interchange Switch, AVERAGE ALL FREIGHT CAR",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L118C11","WEST",9,"E2L118C11",925,"CD per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L118C12","WEST",9,"E2L118C12",926,"CD per Interterminal Switch, AVERAGE ALL FREIGHT CARS",1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5,1.5]
["WEST-E2L118C13","WEST",9,"E2L118C13",927,"CD per I&I Switch, AVERAGE ALL FREIGHT CARS",0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5,0.5]
["WEST-E2L118C14","WEST",9,"E2L118C14",928,"CD per Load & Unload Industry Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L118C15","WEST",9,"E2L118C15",929,"CD per Load & Unload Intraterminal Switch, AVERAGE ALL FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L118C16","WEST",9,"E2L118C16",930,"CD per Load & Unload Interterminal Switch, AVERAGE ALL FREIGHT CARS",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
["WEST-E2L118C17","WEST",9,"E2L118C17",931,"CM per Industry Switch, AVERAGE ALL FREIGHT CARS",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
["WEST-E2L118C18","WEST",9,"E2L118C18",932,"CM per Interchange Switch, AVERAGE ALL FREIGHT CAR",2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75,2.75]
["WEST-E2L118C19","WEST",9,"E2L118C19",933,"CM per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",6,6,6,6,6,6,6,6,6,6,6,6,6,6,6,6]
["WEST-E2L118C20","WEST",9,"E2L118C20",934,"CM per Interterminal Switch, AVERAGE ALL FREIGHT CARS",5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25,5.25]
["WEST-E2L118C21","WEST",9,"E2L118C21",935,"CM per I&I Switch, AVERAGE ALL FREIGHT CARS",1,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
["WEST-E2L118C22","WEST",9,"E2L118C22",936,"Average CM per CD, Railroad-Owned, AVERAGE ALL FREIGHT CARS",507.32379150390602,537.49188232421898,546.41351318359398,622.742919921875,574.459228515625,533.28076171875,579.11700439453102,533.37860107421898,460.41842651367199,517.68365917384403,559.03350128456202,512.82685240226294,483.99801596395599,461.61799058003601,523.51897449649596,473.48660392642898]
["WEST-E2L118C23","WEST",9,"E2L118C23",937,"Average Miles between I&I Switches, AVERAGE ALL FREIGHT CARS",200,200,200,200,200,200,200,200,200,200,200,200,200,200,200,200]
["WEST-E2L118C24","WEST",9,"E2L118C24",938,"Average Miles between Interchange Switches, AVERAGE ALL FREIGHT CARS",1514.87927246094,1479.38549804688,1506.14038085938,1650.65808105469,1625.89953613281,1581.5947265625,1547.72302246094,1590.78747558594,1643.52514648438,1782.33617251599,1694.91326310503,1732.0798398407101,1793.29697953357,1866.8698342673699,1937.9119092097601,1963.21017375735]
["WEST-E2L118C25","WEST",9,"E2L118C25",939,"SEMs per Industry Switch, AVERAGE ALL FREIGHT CARS",5.8928484916687003,5.9121565818786603,5.5734071731567401,5.2377877235412598,5.0537452697753897,5.0996809005737296,5.0501842498779297,5.0666599273681596,4.88950872421265,4.7165669901756804,4.7260398607246303,4.5933868999883103,4.66044129068566,4.7136636094607596,4.5485186041330001,4.3365301515291002]
["WEST-E2L118C26","WEST",9,"E2L118C26",940,"SEMs per Interchange Switch, AVERAGE ALL FREIGHT CARS",3.24106693267822,3.2516863346099898,3.0653738975524898,2.8807833194732702,2.7795608043670699,2.8048243522643999,2.7776014804840101,2.7866630554199201,2.68923020362854,2.5941118445966298,2.5993219233985401,2.5263627949935699,2.5632427098771098,2.5925149852034202,2.5016852322731502,2.3850915833410098]
["WEST-E2L118C27","WEST",9,"E2L118C27",941,"SEMs per Intraterminal Switch, AVERAGE ALL FREIGHT CARS",8.8392753601074201,8.8682346343994105,8.3601102828979492,7.8566813468933097,7.5806174278259304,7.6495208740234402,7.5752754211425799,7.5999898910522496,7.3342638015747097,7.0748504852635303,7.0890597910869397,6.8900803499824601,6.9906619360284896,7.0704954141911402,6.8227779061994998,6.50479522729366]
["WEST-E2L118C28","WEST",9,"E2L118C28",942,"SEMs per Interterminal Switch, AVERAGE ALL FREIGHT CARS",7.0714187622070304,7.0945854187011701,6.68808841705322,6.2853460311889604,6.0644946098327601,6.1196174621581996,6.06022071838379,6.0799922943115199,5.86741018295288,5.6598803882108202,5.6712478328695504,5.51206427998597,5.5925295488227897,5.6563963313529104,5.4582223249595998,5.2038361818349204]
["WEST-E2L118C29","WEST",9,"E2L118C29",943,"SEMs per I&I Switch, AVERAGE ALL FREIGHT CARS",1.47321224212646,1.47803914546967,1.3933517932891799,1.3094470500946001,1.2634361982345601,1.27492010593414,1.26254594326019,1.2666649818420399,1.2223773002624501,1.1791417475439201,1.18150996518116,1.14834672499708,1.1651103226714099,1.1784159023651899,1.13712965103325,1.0841325378822799]
["WEST-E2L201C1","WEST",9,"E2L201C1",944,"Average Distance Per Car In Way Trains",14.8998565673828,13.342384338378899,14.237708091735801,13.751813888549799,13.192066192626999,12.7213439941406,12.292202949523899,12.0123863220215,11.1265048980713,11.1860013491929,13.0665703645316,12.633448450818101,12.686083721739699,13.6333652574788,13.6651521465435,13.622462709699301]
["WEST-E2L202C1","WEST",9,"E2L202C1",945,"Average TCUs Per Flat Car",5.9,5.71,5.76,5.51,5.36,5.28,5,5,4.92,4.9686139999999996,4.9201220000000001,4.8690160000000002,4.8877009999999999,5.0627110000000002,4.8583869999999996,4.7877619999999999]
["WEST-E2L203C1","WEST",9,"E2L203C1",946,"Average Tare Weight - Refrigerated TCU",7.3000001907348597,7.3000001907348597,7.1999998092651403,7.0999999046325701,7,7.0999999046325701,6.9000000953674299,6.9000000953674299,6.9000000953674299,6.9,6.9,6.8,6.9,6.9,7.1,7.1]
["WEST-E2L204C1","WEST",9,"E2L204C1",947,"Average Tare Weight - Non-Refrigerated TCU",5,5,5,4.9000000953674299,4.9000000953674299,4.9000000953674299,4.9000000953674299,5,5,5,4.9000000000000004,4.7,4.9000000000000004,4.9000000000000004,4.8,4.8]
["WEST-E2L205C1","WEST",9,"E2L205C1",948,"Linehaul Miles Per TCU Day",478,478,478,478,478,478,478,478,478,478,478,478,478,478,478,478]
["WEST-E2L206C1","WEST",9,"E2L206C1",949,"TCU Days Per Orig Or Term Event",3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.6449999809265101,3.645,3.645,3.645,3.645,3.645,3.645,3.645]
["WEST-E2L207C1","WEST",9,"E2L207C1",950,"L/E Ratio - Refrigerated/Non-Refrigerated - TCU",1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.4800000190734901,1.48,1.48,1.48,1.48,1.48,1.48,1.48]
["WEST-E2L208C1","WEST",9,"E2L208C1",951,"Average Locomotive Units - Unit Train",2.8928663730621298,3.0402691364288299,3.0985324382782,3.1813867092132599,3.1519355773925799,3.1411767005920401,3.1267213821411102,3.1028676033020002,3.0998432636261,3.2678630791440502,3.30645393797304,3.3034886899670002,3.3000664359298901,3.3025833473967299,3.3220208015681498,3.3800302893865402]
["WEST-E2L209C1","WEST",9,"E2L209C1",952,"Average Locomotive Units - Way Train",2.2184743881225599,2.31257152557373,2.23852467536926,2.1813049316406299,2.1666455268859899,2.1773242950439502,2.1517410278320299,2.1632752418518102,2.17909908294678,2.1818580271578298,2.1768750656743898,2.1915692297031502,2.2145316336557901,2.1286222637522401,2.0401538717816301,2.0571275181762698]
["WEST-E2L210C1","WEST",9,"E2L210C1",953,"Average Locomotive Units - Through Train",3.0518279075622599,2.9757504463195801,2.9967846870422399,3.0945143699646001,3.0540702342987101,3.0420908927917498,3.0245161056518599,3.027676820755,2.9442253112793,3.0892703913545798,3.3041310408386599,3.2480027528340201,3.2183888001065299,3.1666254470189199,3.23574018923662,3.31597647188162]
["WEST-E2L211C1","WEST",9,"E2L211C1",954,"Average Gross Tons - Unit Train",9147.8876953125,9350.025390625,9334.1171875,9512.8955078125,9477.4638671875,9379.28515625,9572.1904296875,9535.9658203125,9554.15234375,9693.8502238913807,9567.2957823180004,9621.5944186785491,9640.8069750284103,9705.27125824016,9982.0540635070101,10171.943648190399]
["WEST-E2L212C1","WEST",9,"E2L212C1",955,"Average Gross Tons - Way Train",2154.63842773438,2181.72412109375,2172.8486328125,2029.10815429688,2183.251953125,2212.73974609375,2034.52575683594,2121.08544921875,2255.02514648438,2221.7136118255198,2127.4623313574998,2281.38592972161,2395.3188645538698,2346.7932750169798,2370.2479750968701,2645.3415374414699]
["WEST-E2L213C1","WEST",9,"E2L213C1",956,"Average Gross Tons - Through Train",5277.1357421875,5349.00390625,5452.50830078125,5643.9951171875,5699.17333984375,5733.87060546875,5684.05908203125,5752.42724609375,5846.8662109375,5952.6451047111505,6030.4662961392596,6094.0279963077901,6103.8213241550602,6451.3142368707804,6968.5911684052498,7455.0192443078204]
["WEST-E2L214C1","WEST",9,"E2L214C1",957,"Engine Crews (Excl Train Switching)",1369188.625,1343848.5,1336816.75,1031863.375,1189190.75,1313480.625,1380093.875,1470660.25,1669962.75,1573301.506446,1320801.6515225801,1414849.2784377399,1593961.2189960999,1498233.4662210799,1202288.6506028899,1242881.0157049701]
["WEST-E2L215C1","WEST",9,"E2L215C1",958,"Train Crews (Excl Train Switching)",1112925.75,1110585.625,1072138.875,859539.125,964785.1875,1064823.125,1095222.625,1190766.25,1320461.75,1258344.3129183401,1079003.75282436,1144917.6489977699,1263834.5983583501,1221996.88726598,986386.77647425304,1008714.95858122]
["WEST-E2L216C1","WEST",9,"E2L216C1",959,"Total Crew Wages (Excl Train Switching)",2482114.5,2454434,2408955.5,1891402.5,2153976,2378303.75,2475316.5,2661426.5,2990424.5,2831645.8193643298,2399805.4043469401,2559766.9274355099,2857795.81735445,2720230.3534870599,2188675.4270771402,2251595.9742861898]
["WEST-E2L217C1","WEST",9,"E2L217C1",960,"Train Miles - Running",364542.96875,352692.78125,339074.4375,281756.9375,310161.625,320184.0625,324940.78125,328579.28125,339759.8125,321897.92099999997,297618.30200000003,308631.12300000002,321195.80499999999,294466.34700000001,253949.65299999999,253672.342]
["WEST-E2L218C1","WEST",9,"E2L218C1",961,"Average Crew Wages (Assigned To TM-Crew)",6.8088393211364702,6.95912742614746,7.1045036315918004,6.7128872871398899,6.9446887969970703,7.4279265403747603,7.6177463531494096,8.0998001098632795,8.8015842437744105,8.7967198128140005,8.0633663595961895,8.2939364719724296,8.8973634551498808,9.23783101600762,8.6185407273509504,8.8760010513333292]
["WEST-E2L219C1","WEST",9,"E2L219C1",962,"General Overhead Ratio",1.0758906602859499,1.0648760795593299,1.0654491186142001,1.07285869121552,1.0796365737914999,1.0673466920852701,1.0655990839004501,1.0632406473159799,1.06222355365753,1.0681340652456801,1.0801598360873701,1.07042658872554,1.06661580821685,1.0619464754347501,1.0769144463385301,1.07001626723413]
["WEST-E2L220C1","WEST",9,"E2L220C1",963,"Constant Cost Markup Ratio",1.30225253105164,1.31183874607086,1.3020552396774301,1.3659965991973899,1.35603356361389,1.3405908346176101,1.3391766548156701,1.3481236696243299,1.3443789482116699,1.3771152031479501,1.4055507185904901,1.40396347549175,1.4051042392379001,1.4091141172358701,1.44848190066866,1.4522094029375101]
["WEST-E2L301C1","WEST",9,"E2L301C1",964,"Residual Factor, Industry Switching, Railroad-Owned",34.5777717486475,39.011429823562601,36.731815938454702,47.749378052243998,43.796826221747601,39.781695419483803,41.236868603649597,27.770954756676222,47.487293107066598,45.239097552724303,43.915261095197003,46.205894258723603,49.6926133095617,52.089005571089999,57.619950460233341,63.484170813081398]
["WEST-E2L301C2","WEST",9,"E2L301C2",965,"Residual Factor, Industry Switching, Privately-Owned",26.9986004119128,30.674515693895898,28.556423001702498,33.957463189456497,33.174649790482903,31.6793642180746,29.720042400013099,18.612191770355494,35.923422321542297,30.8253531062871,30.143100193518698,32.623926082739203,36.192150186907398,37.548792005943397,39.970368873142256,45.616124989298399]
["WEST-E2L302C1","WEST",9,"E2L302C1",966,"Residual Factor, Station Clerical, Railroad-Owned",17.5922850140708,19.7615504786855,19.326219491569599,30.933156217532598,24.5725879912066,18.987015033010099,25.3477367121579,19.858019732615631,26.082617002709299,31.277187103983501,29.4008208507096,28.648990030762299,28.225195122674702,30.045636702060001,35.952444794981822,36.997398464518703]
["WEST-E2L302C2","WEST",9,"E2L302C2",967,"Residual Factor, Station Clerical, Privately-Owned",3.0169201167850002,3.7157309256991402,3.6053758988544602,4.3159331621816204,3.8907203613418302,3.1439718919602702,2.9177392422063901,1.675618192360109,3.57060993956101,3.47616817901562,2.9657512898223102,2.6061785452231501,2.0134555959240799,1.9236665535244499,1.7563914786932175,2.1144855151160198]
["WEST-E2L303C1","WEST",9,"E2L303C1",968,"Residual Factor, Interchange Switching, Railroad-Owned",5.4361003087385802,6.4088021034229401,5.9152833675915399,9.8583955454994499,10.4544967821989,11.833997868061701,11.6606599252443,6.5945968209802759,11.117754159204599,14.2907446884164,12.4469845436379,12.294082677603701,13.5086959397673,10.672923421265301,9.7739716084276544,12.490785127130099]
["WEST-E2L303C2","WEST",9,"E2L303C2",969,"Residual Factor, Interchange Switching, Privately-Owned",4.6180534656285097,5.3672519739199203,4.9175556783494399,7.7873863019912299,8.2972662032995004,9.8748191410370207,9.1838186422621497,4.914153237144137,9.0567824044705194,12.411940769424101,10.239128020819299,10.1556644117125,11.4271399311249,8.6993411661869509,7.692921809009051,10.1750004685712]
["WEST-E2L304C1","WEST",9,"E2L304C1",970,"Residual Factor, I&I Switching, Railroad-Owned",11.005887407575599,10.391101092498401,20.334400803502,37.327113906119699,48.400021710787101,46.141737484780002,48.928223445635602,46.362358481735306,50.207921927603202,55.121175413553502,58.7208171624385,63.930999676499503,68.910049168857,59.099024469130498,63.943428367345035,69.741114160925804]
["WEST-E2L304C2","WEST",9,"E2L304C2",971,"Residual Factor, I&I Switching, Privately-Owned",6.9672728616588504,6.8641931130557303,11.109410486261501,17.284107214996499,21.3659682764366,21.373872413410702,20.8759914693578,18.448126744987988,22.7554542007523,24.169102913631502,27.311449929495499,28.278391149741498,32.561856143246203,28.0499288036577,30.086035214017816,34.367026790428703]
["WEST-E2L305C1","WEST",9,"E2L305C1",972,"Residual Factor, Mileage, Railroad-Owned",0.38535211863231,0.48443788992204101,0.346288440350209,0.64895956942567901,0.36754397209909401,0.100731119514417,0.56012960574991,1.0600743388976892,-1.58074798478289,0.50293653663334603,7.6992467347909405E-2,1.86077566065101,0.97490427278577696,1.85109434503826,-9.6793160830105252E-2,-1.48193672253884]
["WEST-E2L305C2","WEST",9,"E2L305C2",973,"Residual Factor, Mileage, Privately-Owned",0.39582407327399199,0.48867596493605903,0.39699870887366101,0.58594727442844696,0.41704153352971501,0.29630449532543801,0.404289715165636,0.43709402282331888,-0.795403959881264,0.50539285305259796,0.25719169981840201,1.0567349531005601,0.71927190753185299,1.2425797266968801,0.57484984330913158,-0.44119083007100401]
["*** End of Data ***"]

{"sheet":"Railroads","index":7,"n_rows":318,"n_cols":8,"rows_kept":318,"cut":false,"hidden":false,"merged":[]}
["Class I Railroads"]
["RR_Num","URCS_RR","RR_Alpha","Region"]
[103,114900,"CN","EAST"]
[105,137700,"CP","WEST"]
[400,134500,"KCS","WEST"]
[555,117000,"NS","EAST"]
[712,125600,"CSXT","EAST"]
[777,130500,"BNSF","WEST"]
[802,139300,"UP","WEST"]
[900004,900004,"EAST","EAST"]
[900007,900007,"WEST","WEST"]
[]
["Railroad to URCS Railroad"]
["RR_Num","RRICC","RR_Region","RR_Alpha","RR_Name","Year","URCS_RR","URCS_Alpha"]
[5,0,7,"ARR","Alaska Railroad",2009,{"$f":"IF($B15<>0,VLOOKUP($A15,ClassIRailroads,2,FALSE),900000+$C15)","v":900007},{"$f":"VLOOKUP($G15,URCSClassIRailroads,2,FALSE)","v":"WEST"}]
[6,0,4,"AA","Ann Arbor Railroad Co.",2003,900004,"EAST"]
[8,0,7,"AC","Algoma Central Ry",2003,900007,"WEST"]
[9,0,4,"AR","Aberdeen & Rockfish Railroad",2003,900004,"EAST"]
[10,0,4,"PR","South Carolina Division of Public Railways dba Palmetto Railway",2018,900004,"EAST"]
[11,0,7,"APA","Apache Railway",2003,900007,"WEST"]
[12,0,4,"AN","Apalachicola Northern Railroad",2003,900004,"EAST"]
[16,0,7,"ALM","Arkansas, Louisiana & Mississippi RR",2003,900007,"WEST"]
[25,0,4,"ATW","Atlantic & Western Railway, L.P.",2003,900004,"EAST"]
[28,0,4,"AVR","Allegheny Valley Railroad Company",2007,900004,"EAST"]
[32,0,7,"ALS","Alton & Southern Railway",2006,900007,"WEST"]
[35,0,7,"ANR","Angelina & Neches River Railroad",2003,900007,"WEST"]
[53,0,4,"CALA","Carolina Southern Railroad",2010,900004,"EAST"]
[56,0,4,"BAR","Bangor & Aroostook Railroad",2003,900004,"EAST"]
[61,0,4,"BLE","Bessemer & Lake Erie Railroad",2003,900004,"EAST"]
[62,0,4,"DREI","Decatur and Eastern Illinois Railroad LLC",2018,900004,"EAST"]
[65,0,4,"BS","Birmingham Southern Railroad",2003,900004,"EAST"]
[67,0,4,"BVRY","Brandywine Valley Railroad Company",2008,900004,"EAST"]
[72,0,7,"ALAB","Alabama Railroad Co.",2003,900007,"WEST"]
[80,0,4,"WNYP","Western New York & Pennsylvania Railroad, L.L.C.",2007,900004,"EAST"]
[83,0,7,"BRC","Belt Railway Company of Chicago",2003,900007,"WEST"]
[84,0,4,"BXN","Bauxite & Northern Railway",2003,900004,"EAST"]
[88,0,4,"BAYL","Bay Line Railroad L.L.C.",2003,900004,"EAST"]
[93,0,4,"FRVT","Fore River Transportation Corporation",2008,900004,"EAST"]
[94,0,4,"CSO","Connecticut Southern Railroad",2009,900004,"EAST"]
[95,0,4,"CCRR","Claremont Concord Railroad Corp.",2003,900004,"EAST"]
[96,0,4,"CDAC","Canadian American Railroad Co.",2003,900004,"EAST"]
[99,0,4,"CF","Cape Fear Railways",2017,900004,"EAST"]
[103,1,4,"CN","Canadian National RY",2003,114900,"CN"]
[105,6,7,"CP","Canadian Pacific, LTD",2003,137700,"CP"]
[108,0,4,"BB","Buckingham Branch Railroad Company",2003,900004,"EAST"]
[111,0,7,"CIC","Cedar Rapids & Iowa City Railway",2003,900007,"WEST"]
[124,0,7,"CSCD","Cascade & Columbia River Railroad",2004,900007,"WEST"]
[127,0,4,"AGR","Alabama & Gulf Coast Railway LLC",2006,900004,"EAST"]
[131,0,7,"SSS","Stewart Southern Railway",2017,900007,"WEST"]
[132,0,7,"CZRY","Carrizo Gorge Railway",2010,900007,"WEST"]
[134,0,4,"GOGR","Geaux Geaux Railroad",2017,900004,"EAST"]
[142,0,4,"CPDR","Carolina Piedmont Railroad",2011,900004,"EAST"]
[144,0,4,"CMPA","Madison Railroad",2012,900004,"EAST"]
[149,0,4,"KTR","Kendallville Terminal Railway Co.",2003,900004,"EAST"]
[151,0,4,"CHAT","Chattahoochee Bay Railroad, Inc.",2007,900004,"EAST"]
[154,0,4,"BPRR","Buffalo & Pittsburgh Railroad, Inc.",2003,900004,"EAST"]
[155,0,4,"EVWR","Evansville Western Railway",2007,900004,"EAST"]
[156,0,4,"CUOH","Columbus & Ohio Railroad Co.",2003,900004,"EAST"]
[160,0,7,"LBWR","Lubbock and Western Railway",2015,900007,"WEST"]
[162,0,4,"MERR","Maine Eastern Railroad",2006,900004,"EAST"]
[163,0,7,"CLC","Columbia & Cowlitz Railway",2003,900007,"WEST"]
[168,0,4,"CSS","Chicago, SouthShore, & South Bend RR",2003,900004,"EAST"]
[169,0,4,"CLP","Clarendon & Pittsford Railroad",2003,900004,"EAST"]
[171,0,4,"PDRR","Pee Dee River Railroad Corp",2007,900004,"EAST"]
[173,0,7,"CGR","C G Railway Inc.",2003,900007,"WEST"]
[177,0,4,"CAGY","Columbus & Greenville Railway",2003,900004,"EAST"]
[182,0,4,"DLWR","Depew, Lancaster & Western Railroad",2014,900004,"EAST"]
[185,0,4,"FGA","Florida, Gulf & Atlantic Railroad",2019,900004,"EAST"]
[188,0,4,"CIND","Central Railroad Co. of Indiana",2003,900004,"EAST"]
[200,0,7,"DQE","De Queen & Eastern Railroad",2003,900007,"WEST"]
[204,0,4,"GET","Gettysburg & Northern Railroad Co.",2003,900004,"EAST"]
[205,0,7,"WTLC","West Texas and Lubbock Railway",2009,900007,"WEST"]
[210,0,7,"DKS","Doniphan, Kennsett & Searcy Railway",2003,900007,"WEST"]
[211,0,7,"DAIR","D&I Railroad",2003,900007,"WEST"]
[213,0,7,"DMIR","Duluth, Missabe & Iron Range Railway",2003,900007,"WEST"]
[218,0,4,"CBNS","Cape Breton & Central Nova Scotia Railway",2011,900004,"EAST"]
[222,0,4,"CIRR","Chattahoochee Industrial Railroad",2003,900004,"EAST"]
[229,0,4,"ECBR","East Cooper & Berkeley Railroad Co.",2003,900004,"EAST"]
[238,0,4,"EJE","Elgin, Joliet & Eastern Railway",2003,900004,"EAST"]
[241,0,4,"ELS","Escanaba & Lake Superior Railroad",2003,900004,"EAST"]
[245,0,4,"EJR","East Jersey Railroad And Terminal Company",2008,900004,"EAST"]
[246,0,4,"GLC","Great Lakes Central Railroad",2008,900004,"EAST"]
[247,0,7,"EDW","El Dorado and Wesson Railway Co.",2003,900007,"WEST"]
[249,0,4,"NBER","Nittany & Bald Eagle Railroad Co.",2003,900004,"EAST"]
[250,0,7,"WC","Historical Wisconsin Central Ltd.",2003,900007,"WEST"]
[252,0,4,"EIRC","Eastern Illinois Railroad Company",2010,900004,"EAST"]
[258,0,4,"WTNN","West Tennessee Railroad",2003,900004,"EAST"]
[260,0,4,"CKIN","Chesapeake and Indiana Railroad",2013,900004,"EAST"]
[263,0,4,"FEC","Florida East Coast Railway",2003,900004,"EAST"]
[264,0,7,"FVW","Fox Valley & Western",2003,900007,"WEST"]
[268,0,4,"FGLK","Finger Lakes Railway Corp",2008,900004,"EAST"]
[283,0,4,"GEXR","Goderich-Exeter Railway Company",2019,900004,"EAST"]
[284,0,7,"DGNO","Dallas Garland & Northeastern Railroad Inc",2008,900007,"WEST"]
[287,0,4,"GCW","Garden City Western Railway, Inc",2009,900004,"EAST"]
[288,0,7,"EFRR","Effingham Railroad Co.",2003,900007,"WEST"]
[289,0,4,"COEH","Conecuh Valley Railroad",2010,900004,"EAST"]
[291,0,7,"FXE","Ferrocarril Mexicano SA DE CV",2005,900007,"WEST"]
[295,0,4,"GTRA","Golden Triangle Railroad",2003,900004,"EAST"]
[296,0,4,"GMRY","Great Miami & Scioto Railway Co.",2003,900004,"EAST"]
[300,0,4,"GFRR","Georgia and Florida Railroad",2009,900004,"EAST"]
[302,0,7,"GRR","Georgetown Railroad",2003,900007,"WEST"]
[303,0,4,"ISRR","Indiana Southern Railroad Co., Inc.",2003,900004,"EAST"]
[306,0,4,"GRW","Gary Railway",2009,900004,"EAST"]
[307,0,4,"FRR","Falls Road Railroad",2010,900004,"EAST"]
[308,0,4,"GTW","Historical Grand Trunk Western, Inc.",2003,900004,"EAST"]
[311,0,7,"GWR","Great Western Railroad of Colorado",2016,900007,"WEST"]
[314,0,4,"GMRC","Green Mountain Railroad Corp.",2003,900004,"EAST"]
[315,0,7,"SDIY","San Diego And Imperial Valley Railroad",2011,900007,"WEST"]
[316,0,7,"IAIS","Iowa Interstate Railroad, Ltd.",2003,900007,"WEST"]
[319,0,4,"FNOR","Florida Northern Railroad Company Inc",2008,900004,"EAST"]
[321,0,7,"RRVW","Rad River Valley & Western RR Co.",2003,900007,"WEST"]
[323,0,4,"GU","Grafton and Upton Railroad",2012,900004,"EAST"]
[328,0,7,"HE","Hollis & Eastern RR, Co.",2007,900007,"WEST"]
[333,0,7,"FSRR","Ferrosur S A DE C V",2006,900007,"WEST"]
[335,0,4,"GDLK","Grand Elk Railroad",2009,900004,"EAST"]
[337,0,4,"GSWR","Georgia Southwestern Railroad, Inc.",2003,900004,"EAST"]
[341,0,7,"IANR","Iowa Northern Railway Co.",2003,900007,"WEST"]
[342,0,4,"ICE","Iowa, Chicago and Eastern Railroad",2009,900004,"EAST"]
[343,0,4,"EARY","Eastern Alabama Railway",2003,900004,"EAST"]
[344,0,4,"MMA","Montreal, Maine & Atlantic",2009,900004,"EAST"]
[345,0,7,"HCRY","Huron Central Railway Inc.",2006,900007,"WEST"]
[351,0,4,"BH","B&H Rail Corp.",2003,900004,"EAST"]
[357,0,4,"IHB","Indiana Harbor Belt Railroad",2003,900004,"EAST"]
[358,0,7,"IBT","International Bridge & Terminal",2003,900007,"WEST"]
[361,0,7,"IMRR","Illinois & Midland Railroad, Inc.",2003,900007,"WEST"]
[362,0,7,"GWWR","Gateway Western Railroad",2003,900007,"WEST"]
[365,0,7,"KJRY","Keokuk Junction Railway",2003,900007,"WEST"]
[367,0,4,"IR","Indiana Railroad",2010,900004,"EAST"]
[377,0,7,"KYLE","Kyle Railroad",2003,900007,"WEST"]
[378,0,7,"FCCM","Compania De Ferrocarriles SA DE CV",2006,900007,"WEST"]
[379,0,7,"IMRL","I&M Rail Link, LLC",2003,900007,"WEST"]
[380,0,7,"KO","Kansas & Oklahoma Railroad Inc.",2003,900007,"WEST"]
[386,0,7,"CMR","Central Midland Railway Company",2003,900007,"WEST"]
[388,0,4,"MGRI","MG Rail Inc",2008,900004,"EAST"]
[393,0,7,"BRR","Battle River Railway NGC Inc.",2021,900007,"WEST"]
[395,0,4,"GC","Georgia Central Railway, L.P.",2003,900004,"EAST"]
[398,0,4,"LAL","Livonia, Avon & Lakeville Railroad Corp.",2003,900004,"EAST"]
[399,0,4,"KBSR","Kankakee, Beaverville & Southern Railroad",2014,900004,"EAST"]
[400,5,7,"KCS","Kansas City Southern Railway Co.",2003,134500,"KCS"]
[404,0,4,"LT","Lake Terminal Railroad Company",2003,900004,"EAST"]
[408,0,4,"LSRC","Lake State Railway Co.",2003,900004,"EAST"]
[410,0,4,"ACWR","Aberdeen Carolina & Western Railway Co.",2003,900004,"EAST"]
[411,0,4,"LMIC","Lake Michigan And Indiana Railroad Company",2008,900004,"EAST"]
[420,0,7,"CRL","Chicago Rail Link",2003,900007,"WEST"]
[424,0,7,"KRR","Kiamichi Railroad Company",2003,900007,"WEST"]
[425,0,4,"LSI","Lake Superior & Ishpeming Railroad",2003,900004,"EAST"]
[426,0,4,"LC","Lancaster And Chester Railway Company",2008,900004,"EAST"]
[427,0,4,"LRS","Laurinburg and Southern Railroad Co.",2003,900004,"EAST"]
[433,0,4,"LXVR","Luxapalila Valley Railroad, Inc.",2003,900004,"EAST"]
[434,0,4,"LIRC","Louisville & Indiana Railroad Co.",2003,900004,"EAST"]
[442,0,7,"LNW","Louisiana & North West Railroad Co.",2003,900007,"WEST"]
[443,0,7,"GNBC","Grainbelt Corporation",2008,900007,"WEST"]
[448,0,7,"GSR","Great Sandhills Railway",2015,900007,"WEST"]
[452,0,4,"LVRC","Lamoille Valley Railroad Company",2003,900004,"EAST"]
[455,0,4,"MHWA","Mohawk, Adirondack and Northern Railroad",2015,900004,"EAST"]
[460,0,4,"UCT","Indiana Business Railroad dba Union City Terminal Railroad",2018,900004,"EAST"]
[461,0,4,"MCER","Massachusetts Central Railroad Corp.",2003,900004,"EAST"]
[462,0,4,"NTZR","Natchez Railway",2010,900004,"EAST"]
[464,0,4,"MC","Michigan Central Railroad",2013,900004,"EAST"]
[466,0,7,"MCR","McCloud Railway Co.",2003,900007,"WEST"]
[469,0,4,"HOG","Heart of Georgia Railroad",2010,900004,"EAST"]
[472,0,4,"CMGN","Central Michigan Railway Co.",2003,900004,"EAST"]
[478,0,7,"LMR","Last Mountain Railway",2013,900007,"WEST"]
[480,0,4,"MNBR","M & B Railroad, L.L.C.",2003,900004,"EAST"]
[485,0,7,"LRWN","Little Rock & Western Railway, L.P.",2003,900007,"WEST"]
[490,0,4,"PAS","Pan Am Southern, LLC",2009,900004,"EAST"]
[495,0,4,"MMID","Maryland Midland Railway",2003,900004,"EAST"]
[496,0,4,"NECR","New England Central Railroad, Inc.",2003,900004,"EAST"]
[501,0,4,"NYA","New York & Atlantic Railway",2003,900004,"EAST"]
[502,0,4,"CWRO","Cleveland Works Railway Company",2007,900004,"EAST"]
[503,0,4,"MSV","Mississippi & Skuna Valley Railway",2003,900004,"EAST"]
[506,0,4,"MSE","Mississippi Export Railroad",2003,900004,"EAST"]
[507,0,4,"FMID","Florida Midland Railroad Co. Inc.",2007,900004,"EAST"]
[508,0,7,"MNA","Missouri & Northern Arkansas RR Co.",2003,900007,"WEST"]
[509,0,7,"MSO","Michigan Southern Railroad Co., Inc.",2003,900007,"WEST"]
[510,0,7,"MDW","Minnesota, Dakota & Western Railway",2003,900007,"WEST"]
[514,0,7,"ATLT","AT&L Railroad",2003,900007,"WEST"]
[518,0,7,"RARW","Rarus Railway Company",2018,900007,"WEST"]
[531,0,4,"NCVA","North Carolina & Virginia Railroad Co. Inc.",2007,900004,"EAST"]
[541,0,4,"NAUG","Naugatuck Railroad Company LLC",2018,900004,"EAST"]
[546,0,4,"NYSW","New York, Susquehanna & Western Rwy.",2003,900004,"EAST"]
[547,0,4,"MS","Michigan Shore Railroad Incorporated",2010,900004,"EAST"]
[555,2,4,"NS","Norfolk Southern Corp.",2003,117000,"NS"]
[556,0,4,"CFS","Sartigan Railway/Chemin De Fer Sartigan",2018,900004,"EAST"]
[557,0,4,"SCIH","South Chicago & Indiana Harbor Railway Company",2008,900004,"EAST"]
[564,0,7,"MSCI","Mississippi Central Railroad Co.",2003,900007,"WEST"]
[570,0,4,"NWR","Nashville & Western Railroad Corp.",2007,900004,"EAST"]
[572,0,4,"NHRR","New Hope and Ivyland Railroad",2020,900004,"EAST"]
[576,0,4,"ASRY","Ashland Railway Co.",2007,900004,"EAST"]
[577,0,4,"KRL","Kasgro Railway",2003,900004,"EAST"]
[578,0,7,"OAR","Old Augusta Railroad",2003,900007,"WEST"]
[582,0,4,"SCRF","South Carolina Central Railroad",2003,900004,"EAST"]
[585,0,4,"NYOG","New York & Ogdensburg Railway Co.",2003,900004,"EAST"]
[588,0,4,"OMID","Ontario Midland Railroad Corporation",2021,900004,"EAST"]
[594,0,7,"OUCH","Ouachita Railroad",2009,900007,"WEST"]
[601,0,4,"OHCR","Ohio Central Railroad Co.",2003,900004,"EAST"]
[609,0,4,"PBR","Patapsco & Back Rivers Railroad Co.",2003,900004,"EAST"]
[610,0,4,"RJCS","RJ Corman Carolina Lines",2016,900004,"EAST"]
[611,0,4,"PVRR","Pioneer Valley Railroad",2012,900004,"EAST"]
[612,0,4,"CFE","Chicago, Ft. Wayne & Eastern",2003,900004,"EAST"]
[622,0,4,"CMQ","Central Maine & Quebec Railway",2014,900004,"EAST"]
[624,0,4,"RSOR","Riceboro Southern Railway",2010,900004,"EAST"]
[631,0,4,"PW","Providence and Worcester Railroad Co",2003,900004,"EAST"]
[635,0,4,"QGRY","Quebec Gatineau Railway",2013,900004,"EAST"]
[639,0,4,"RJCL","RJ Corman Cleveland Line",2014,900004,"EAST"]
[641,0,4,"RBMN","Reading Blue Mountain & Northern Railroad",2017,900004,"EAST"]
[651,0,4,"PCN","Point Comfort & Northern Railway",2003,900004,"EAST"]
[655,0,7,"NNW","Nebraska Northwestern Railroad",2015,900007,"WEST"]
[670,0,7,"SSAM","Sault Ste. Marie Bridge Co.",2003,900007,"WEST"]
[675,0,4,"RSS","Rockdale, Sandow & Southern Railroad",2003,900004,"EAST"]
[676,0,4,"SMW","St Marys Railway West Llc",2008,900004,"EAST"]
[677,0,4,"PBVR","Port Bienville Railroad",2007,900004,"EAST"]
[679,0,7,"SAV","Sacramento Valley Railroad",2017,900007,"WEST"]
[681,0,4,"GNRR","Georgia Northeastern Railroad Co",2008,900004,"EAST"]
[682,0,4,"SM","St. Marys Railroad",2003,900004,"EAST"]
[689,0,7,"SRY","Southern Railway of British Columbia LTD",2003,900007,"WEST"]
[691,0,4,"SAN","Sandersville Railroad",2003,900004,"EAST"]
[695,0,4,"SFR","Southern Freight Railroad",2003,900004,"EAST"]
[696,0,7,"SLC","San Luis Central Railroad",2003,900007,"WEST"]
[697,0,4,"RLK","Ottawa Valley Railway",2015,900004,"EAST"]
[698,0,7,"STMA","St. Maries River Railroad",2003,900007,"WEST"]
[700,0,4,"SLR","St. Lawrence & Atlantic Railroad Co.",2003,900004,"EAST"]
[701,0,7,"SKOL","South Kansas & Oklahoma Railroad, Inc.",2007,900007,"WEST"]
[706,0,7,"BGS","Big Sky Rail",2013,900007,"WEST"]
[707,0,7,"SS","Sand Springs Railway Company",2003,900007,"WEST"]
[712,3,4,"CSXT","CSX Transportation",2003,125600,"CSXT"]
[719,0,4,"SB","South Buffalo Railway Company",2007,900004,"EAST"]
[720,0,4,"SIND","Southern Indiana Railway",2003,900004,"EAST"]
[723,0,4,"SLQ","St. Lawrence and Atlantic Railroad (Quebec) Incorporated (GWI)",2010,900004,"EAST"]
[727,0,7,"SCXY","St Croix Valley Railroad Company",2008,900007,"WEST"]
[728,0,4,"SLRS","SMS Rail Service, Inc.",2004,900004,"EAST"]
[739,0,7,"STE","Stockton Terminal & Eastern Railroad",2003,900007,"WEST"]
[745,0,4,"TKEN","Tennken Railroad",2003,900004,"EAST"]
[746,0,4,"ST","Guilford Rail System",2003,900004,"EAST"]
[753,0,4,"TZPR","Tazewell & Peoria Railroad, Inc.",2003,900004,"EAST"]
[754,0,7,"ONT","Ontario Northland RY",2003,900007,"WEST"]
[755,0,4,"TTR","Talleyrand Terminal Railroad Co.",2004,900004,"EAST"]
[756,0,7,"TIBR","Timberrock Railroad Company Inc",2008,900007,"WEST"]
[757,0,7,"TRRA","Terminal Railroad Assc. of St Louis",2003,900007,"WEST"]
[758,0,4,"TASD","Terminal Railway Alabama State Docks",2008,900004,"EAST"]
[761,0,7,"TCT","Texas City Terminal Railway Co.",2003,900007,"WEST"]
[762,0,7,"TM","Texas Mexican Railway",2003,900007,"WEST"]
[763,0,4,"WGCR","Wiregrass Centrail Railway",2020,900004,"EAST"]
[768,0,7,"TCWR","Twin Cities & Western Railroad Co.",2003,900007,"WEST"]
[769,0,7,"TPW","Toledo, Peoria & Western Railway Corp.",2003,900007,"WEST"]
[770,0,4,"TSBY","Tuscola & Saginaw Bay Railway",2003,900004,"EAST"]
[772,0,7,"TR","Tomahawk Railway, L.P.",2003,900007,"WEST"]
[773,0,4,"TTIS","Transkentucky Transportation Railroad",2003,900004,"EAST"]
[776,0,4,"NCYR","Nash County Railroad Corp",2008,900004,"EAST"]
[777,4,7,"BNSF","BNSF Railway Company.",2003,130500,"BNSF"]
[779,0,7,"TRC","Trona Railway Co.",2003,900007,"WEST"]
[780,0,4,"INRD","Indiana Rail Road, The",2003,900004,"EAST"]
[785,0,4,"MMRR","Mid-Michigan Railroad, Inc.",2003,900004,"EAST"]
[787,0,4,"NHN","New Hampshire Northcoast Corp",2021,900004,"EAST"]
[792,0,4,"RJCM","R J Corman Railroad Company/Memphis Line",2007,900004,"EAST"]
[794,0,7,"SMA","San Manuel Arizona Railroad",2004,900007,"WEST"]
[798,0,4,"TSRR","Tennessee Southern Railroad Co. Inc.",2007,900004,"EAST"]
[799,0,4,"SH","Steelton & Highspire Railroad Company",2008,900004,"EAST"]
[802,7,7,"UP","Union Pacific Railroad Co.",2003,139300,"UP"]
[803,0,7,"URR","Union Railroad Company",2003,900007,"WEST"]
[805,0,4,"SCXF","South Central Florida Express Inc.",2003,900004,"EAST"]
[808,0,4,"UMP","Upper Merion And Plymouth Railroad Company",2008,900004,"EAST"]
[811,0,7,"UTAH","Utah Railway Co.",2003,900007,"WEST"]
[812,0,4,"WACR","Washington County Railroad Company",2004,900004,"EAST"]
[817,0,4,"VTR","Vermont Railway",2003,900004,"EAST"]
[848,0,4,"IERR","Indiana Eastern Railroad",2010,900004,"EAST"]
[849,0,4,"BHRR","Birmingham Terminal Railway",2012,900004,"EAST"]
[850,0,4,"WW","Winchester and Western Railroad",2011,900004,"EAST"]
[853,0,4,"ATN","Alabama & Tennessee River Railway, L.L.C.",2007,900004,"EAST"]
[856,0,4,"WE","Wheeling & Lake Erie Railway Co.",2003,900004,"EAST"]
[857,0,7,"TFM","Transportation Ferroviaria Mexicana",2003,900007,"WEST"]
[858,0,4,"SRP","Safe Handling Rail, Inc.",2003,900004,"EAST"]
[859,0,4,"CNYK","Central New York Railroad Corporation",2007,900004,"EAST"]
[861,0,4,"VR","Valdosta Railway, L.P.",2003,900004,"EAST"]
[864,0,4,"USRP","US Rail Partners, Ltd",2011,900004,"EAST"]
[866,0,7,"WMI","West Michigan Railroad Co.",2006,900007,"WEST"]
[871,0,7,"MRL","Montana Rail Link",2003,900007,"WEST"]
[875,0,7,"VCRR","Ventura County Railroad Company",2003,900007,"WEST"]
[876,0,4,"YB","Youngstown Belt Railroad Company, The",2008,900004,"EAST"]
[877,0,4,"GRYR","Grenada Railway",2009,900004,"EAST"]
[879,0,7,"WSOR","Wisconsin & Southern Railroad",2003,900007,"WEST"]
[880,0,4,"WBCR","Wabash Central Railroad Corp.",2004,900004,"EAST"]
[883,0,4,"WCLR","Waccamaw Coastline Railroad Co Inc",2008,900004,"EAST"]
[888,0,4,"JAIL","Jackson & Lansing Railroad",2014,900004,"EAST"]
[890,0,4,"HESR","Huron & Eastern Railway",2003,900004,"EAST"]
[893,0,4,"AO","Appalachian & Ohio Railroad Inc.",2003,900004,"EAST"]
[894,0,7,"RCPE","Rapid City, Pierre & Eastern Railroad",2014,900007,"WEST"]
[896,0,4,"FCRD","First Coast Railroad Inc",2008,900004,"EAST"]
[906,0,7,"AM","Arkansas & Missouri Railroad",2003,900007,"WEST"]
[907,0,4,"PAL","Paducah & Louisville Railway",2003,900004,"EAST"]
[908,0,4,"YRC","York Railway Company",2007,900004,"EAST"]
[912,0,7,"DME","Dakota, Minnesota & Eastern Railroad",2003,900007,"WEST"]
[916,0,7,"GLSR","Gloster Southern Railroad Co.",2003,900007,"WEST"]
[919,0,4,"MQT","Marquette Rail, L.L.C.",2007,900004,"EAST"]
[920,0,4,"SBS","Saginaw Bay Southern Railway Company",2008,900004,"EAST"]
[926,0,4,"SGVY","Saginaw Valley Railway Co., Inc.",2003,900004,"EAST"]
[932,0,4,"SGLR","Seminole Gulf Railway",2010,900004,"EAST"]
[938,0,4,"WTRM","Warren and Trumbull Railroad",2013,900004,"EAST"]
[941,0,4,"RSR","Rochester & Southern Railroad, Inc.",2003,900004,"EAST"]
[945,0,4,"OCTL","Oil Creek & Titusville Lines, Inc.",2004,900004,"EAST"]
[951,0,4,"HAL","Hilton & Albany Railroad, Inc",2012,900004,"EAST"]
[960,0,7,"PTRA","Port Terminal Railroad Association",2003,900007,"WEST"]
[967,0,4,"RJCC","R J Corman Railroad Company",2006,900004,"EAST"]
[968,0,7,"UPCS","Union Pacific Carrier Services",2010,900007,"WEST"]
[969,0,4,"IORY","Indiana & Ohio Railway, The",2003,900004,"EAST"]
[974,0,4,"BCR","Bay Coast Railroad",2007,900004,"EAST"]
[976,0,7,"KCTL","Kansas City Transportation Co., L.L.C.",2007,900007,"WEST"]
[978,0,7,"KCSM","Kansas City Southern De Mexico S A De C V",2008,900007,"WEST"]
[981,0,4,"WTRY","Wilmington Terminal Railroad",2010,900004,"EAST"]
[984,0,7,"MPLI","Minnesota Prairie Line",2004,900007,"WEST"]
[986,0,4,"FCEN","Florida Central Railroad",2010,900004,"EAST"]
[994,0,7,"IATR","Iowa Traction Railroad Company",2003,900007,"WEST"]
[996,0,4,"KWT","KWT Railway, Inc.",2007,900004,"EAST"]
[997,0,7,"BCOL","BC Rail LTD",2003,900007,"WEST"]
[999,0,7,"AMTK","Amtrak Freight",2006,900007,"WEST"]
[900004,0,4,"EAST","Eastern Region",2003,900004,"EAST"]
[900007,0,7,"WEST","Western Region",2003,900007,"WEST"]
["End of Data"]

{"sheet":"STCCs","index":8,"n_rows":39002,"n_cols":3,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["STCC5 to URCS STCC Types"]
["STCC5","URCS\nSTCC","STCC-Description"]
["01000",{"$f":"IF(NOT(ISNA(VLOOKUP(LEFT($A3,5),URCSSTCCCodes,1,FALSE))),VLOOKUP(LEFT($A3,5),URCSSTCCCodes,1,FALSE),IF(NOT(ISNA(VLOOKUP(LEFT($A3,4),URCSSTCCCodes,1,FALSE))),VLOOKUP(LEFT($A3,4),URCSSTCCCodes,1,FALSE),IF(NOT(ISNA(VLOOKUP(LEFT($A3,3),URCSSTCCCodes,1,FALSE))),VLOOKUP(LEFT($A3,3),URCSSTCCCodes,1,FALSE),IF(NOT(ISNA(VLOOKUP(LEFT($A3,2),URCSSTCCCodes,1,FALSE))),VLOOKUP(LEFT($A3,2),URCSSTCCCodes,1,FALSE),URCSInputs!$O$84))))","v":"01000"},{"$f":"VLOOKUP($B3,URCSSTCCCodes,3,FALSE)","v":"01 All Farm Products"}]
["01001","01","01 Other Farm Products"]
["01002","01","01 Other Farm Products"]
["01003","01","01 Other Farm Products"]
["01004","01","01 Other Farm Products"]
["01005","01","01 Other Farm Products"]
["01006","01","01 Other Farm Products"]
["01007","01","01 Other Farm Products"]
["01008","01","01 Other Farm Products"]
["01009","01","01 Other Farm Products"]
["01010","01","01 Other Farm Products"]
["01011","01","01 Other Farm Products"]
["01012","01","01 Other Farm Products"]
["01013","01","01 Other Farm Products"]
["01014","01","01 Other Farm Products"]
["01015","01","01 Other Farm Products"]
["01016","01","01 Other Farm Products"]
["01017","01","01 Other Farm Products"]
["01018","01","01 Other Farm Products"]
["01019","01","01 Other Farm Products"]
["01020","01","01 Other Farm Products"]
["01021","01","01 Other Farm Products"]
["01022","01","01 Other Farm Products"]
["01023","01","01 Other Farm Products"]
["01024","01","01 Other Farm Products"]
["01025","01","01 Other Farm Products"]
["01026","01","01 Other Farm Products"]
["01027","01","01 Other Farm Products"]
["01028","01","01 Other Farm Products"]
["01029","01","01 Other Farm Products"]
["01030","01","01 Other Farm Products"]
["01031","01","01 Other Farm Products"]
["01032","01","01 Other Farm Products"]
["01033","01","01 Other Farm Products"]
["01034","01","01 Other Farm Products"]
["01035","01","01 Other Farm Products"]
["01036","01","01 Other Farm Products"]
["01037","01","01 Other Farm Products"]
["01038","01","01 Other Farm Products"]
["01039","01","01 Other Farm Products"]
["01040","01","01 Other Farm Products"]
["01041","01","01 Other Farm Products"]
["01042","01","01 Other Farm Products"]
["01043","01","01 Other Farm Products"]
["01044","01","01 Other Farm Products"]
["01045","01","01 Other Farm Products"]
["01046","01","01 Other Farm Products"]
["01047","01","01 Other Farm Products"]
["01048","01","01 Other Farm Products"]
["01049","01","01 Other Farm Products"]
["01050","01","01 Other Farm Products"]
["01051","01","01 Other Farm Products"]
["01052","01","01 Other Farm Products"]
["01053","01","01 Other Farm Products"]
["01054","01","01 Other Farm Products"]
["01055","01","01 Other Farm Products"]
["01056","01","01 Other Farm Products"]
["01057","01","01 Other Farm Products"]
["01058","01","01 Other Farm Products"]
["01059","01","01 Other Farm Products"]
["01060","01","01 Other Farm Products"]
["01061","01","01 Other Farm Products"]
["01062","01","01 Other Farm Products"]
["01063","01","01 Other Farm Products"]
["01064","01","01 Other Farm Products"]
["01065","01","01 Other Farm Products"]
["01066","01","01 Other Farm Products"]
["01067","01","01 Other Farm Products"]
["01068","01","01 Other Farm Products"]
["01069","01","01 Other Farm Products"]
["01070","01","01 Other Farm Products"]
["01071","01","01 Other Farm Products"]
["01072","01","01 Other Farm Products"]
["01073","01","01 Other Farm Products"]
["01074","01","01 Other Farm Products"]
["01075","01","01 Other Farm Products"]
["01076","01","01 Other Farm Products"]
["01077","01","01 Other Farm Products"]
["01078","01","01 Other Farm Products"]
["01079","01","01 Other Farm Products"]
["01080","01","01 Other Farm Products"]
["01081","01","01 Other Farm Products"]
["01082","01","01 Other Farm Products"]
["01083","01","01 Other Farm Products"]
["01084","01","01 Other Farm Products"]
["01085","01","01 Other Farm Products"]
["01086","01","01 Other Farm Products"]
["01087","01","01 Other Farm Products"]
["01088","01","01 Other Farm Products"]
["01089","01","01 Other Farm Products"]
["01090","01","01 Other Farm Products"]
["01091","01","01 Other Farm Products"]
["01092","01","01 Other Farm Products"]
["01093","01","01 Other Farm Products"]
["01094","01","01 Other Farm Products"]
["01095","01","01 Other Farm Products"]
["01096","01","01 Other Farm Products"]
["01097","01","01 Other Farm Products"]
["01098","01","01 Other Farm Products"]
["01099","01","01 Other Farm Products"]
["01100","01","01 Other Farm Products"]
["01101","01","01 Other Farm Products"]
["01102","01","01 Other Farm Products"]
["01103","01","01 Other Farm Products"]
["01104","01","01 Other Farm Products"]
["01105","01","01 Other Farm Products"]
["01106","01","01 Other Farm Products"]
["01107","01","01 Other Farm Products"]
["01108","01","01 Other Farm Products"]
["01109","01","01 Other Farm Products"]
["01110","01","01 Other Farm Products"]
["01111","01","01 Other Farm Products"]
["01112","01","01 Other Farm Products"]
["01113","01","01 Other Farm Products"]
["01114","01","01 Other Farm Products"]
["01115","01","01 Other Farm Products"]
["01116","01","01 Other Farm Products"]
["01117","01","01 Other Farm Products"]
["01118","01","01 Other Farm Products"]
["01119","01","01 Other Farm Products"]
["01120","01","01 Other Farm Products"]
["01121","01","01 Other Farm Products"]
["01122","01","01 Other Farm Products"]
["01123","01","01 Other Farm Products"]
["01124","01","01 Other Farm Products"]
["01125","01","01 Other Farm Products"]
["01126","01","01 Other Farm Products"]
["01127","01","01 Other Farm Products"]
["01128","01","01 Other Farm Products"]
["01129","01","01 Other Farm Products"]
["01130","0113","0113 Grains"]
["01131","0113","0113 Grains"]
["01132","0113","0113 Grains"]
["01133","0113","0113 Grains"]
["01134","0113","0113 Grains"]
["01135","0113","0113 Grains"]
["01136","0113","0113 Grains"]
["01137","0113","0113 Grains"]
["01138","0113","0113 Grains"]
["01139","0113","0113 Grains"]
["01140","01","01 Other Farm Products"]
["01141","01","01 Other Farm Products"]
["01142","01","01 Other Farm Products"]
["01143","01","01 Other Farm Products"]
["01144","01","01 Other Farm Products"]
["01145","01","01 Other Farm Products"]
["01146","01","01 Other Farm Products"]
["01147","01","01 Other Farm Products"]
["01148","01","01 Other Farm Products"]
["01149","01","01 Other Farm Products"]
["01150","01","01 Other Farm Products"]
["01151","01","01 Other Farm Products"]
["01152","01","01 Other Farm Products"]
["01153","01","01 Other Farm Products"]
["01154","01","01 Other Farm Products"]
["01155","01","01 Other Farm Products"]
["01156","01","01 Other Farm Products"]
["01157","01","01 Other Farm Products"]
["01158","01","01 Other Farm Products"]
["01159","01","01 Other Farm Products"]
["01160","01","01 Other Farm Products"]
["01161","01","01 Other Farm Products"]
["01162","01","01 Other Farm Products"]
["01163","01","01 Other Farm Products"]
["01164","01","01 Other Farm Products"]
["01165","01","01 Other Farm Products"]
["01166","01","01 Other Farm Products"]
["01167","01","01 Other Farm Products"]
["01168","01","01 Other Farm Products"]
["01169","01","01 Other Farm Products"]
["01170","01","01 Other Farm Products"]
["01171","01","01 Other Farm Products"]
["01172","01","01 Other Farm Products"]
["01173","01","01 Other Farm Products"]
["01174","01","01 Other Farm Products"]
["01175","01","01 Other Farm Products"]
["01176","01","01 Other Farm Products"]
["01177","01","01 Other Farm Products"]
["01178","01","01 Other Farm Products"]
["01179","01","01 Other Farm Products"]
["01180","01","01 Other Farm Products"]
["01181","01","01 Other Farm Products"]
["01182","01","01 Other Farm Products"]
["01183","01","01 Other Farm Products"]
["01184","01","01 Other Farm Products"]
["01185","01","01 Other Farm Products"]
["01186","01","01 Other Farm Products"]
["01187","01","01 Other Farm Products"]
["01188","01","01 Other Farm Products"]
["01189","01","01 Other Farm Products"]
["01190","01","01 Other Farm Products"]
["01191","01","01 Other Farm Products"]
["01192","01","01 Other Farm Products"]
["01193","01","01 Other Farm Products"]
["01194","01","01 Other Farm Products"]
["01195","01195","01195 Potatoes; Other than Sweet"]
["01196","01","01 Other Farm Products"]
["01197","01","01 Other Farm Products"]
["01198","01","01 Other Farm Products"]
["01199","01","01 Other Farm Products"]
["01200","012","012 Fresh Fruits/Tree Nuts"]
["01201","012","012 Fresh Fruits/Tree Nuts"]
["01202","012","012 Fresh Fruits/Tree Nuts"]
["01203","012","012 Fresh Fruits/Tree Nuts"]
["01204","012","012 Fresh Fruits/Tree Nuts"]
["01205","012","012 Fresh Fruits/Tree Nuts"]
["01206","012","012 Fresh Fruits/Tree Nuts"]
["01207","012","012 Fresh Fruits/Tree Nuts"]
["01208","012","012 Fresh Fruits/Tree Nuts"]
["01209","012","012 Fresh Fruits/Tree Nuts"]
["01210","012","012 Fresh Fruits/Tree Nuts"]
["01211","012","012 Fresh Fruits/Tree Nuts"]
["01212","012","012 Fresh Fruits/Tree Nuts"]
["01213","012","012 Fresh Fruits/Tree Nuts"]
["01214","012","012 Fresh Fruits/Tree Nuts"]
["01215","012","012 Fresh Fruits/Tree Nuts"]
["01216","012","012 Fresh Fruits/Tree Nuts"]
["01217","012","012 Fresh Fruits/Tree Nuts"]
["01218","012","012 Fresh Fruits/Tree Nuts"]
["01219","012","012 Fresh Fruits/Tree Nuts"]
["01220","012","012 Fresh Fruits/Tree Nuts"]
["01221","012","012 Fresh Fruits/Tree Nuts"]
["01222","012","012 Fresh Fruits/Tree Nuts"]
["01223","012","012 Fresh Fruits/Tree Nuts"]
["01224","012","012 Fresh Fruits/Tree Nuts"]
["01225","012","012 Fresh Fruits/Tree Nuts"]
["01226","012","012 Fresh Fruits/Tree Nuts"]
["01227","012","012 Fresh Fruits/Tree Nuts"]
["01228","012","012 Fresh Fruits/Tree Nuts"]
["01229","012","012 Fresh Fruits/Tree Nuts"]
["01230","012","012 Fresh Fruits/Tree Nuts"]
["01231","012","012 Fresh Fruits/Tree Nuts"]
["01232","012","012 Fresh Fruits/Tree Nuts"]
["01233","012","012 Fresh Fruits/Tree Nuts"]
["01234","012","012 Fresh Fruits/Tree Nuts"]
["01235","012","012 Fresh Fruits/Tree Nuts"]
["01236","012","012 Fresh Fruits/Tree Nuts"]
["01237","012","012 Fresh Fruits/Tree Nuts"]
["01238","012","012 Fresh Fruits/Tree Nuts"]
["01239","012","012 Fresh Fruits/Tree Nuts"]
["01240","012","012 Fresh Fruits/Tree Nuts"]
["01241","012","012 Fresh Fruits/Tree Nuts"]
["01242","012","012 Fresh Fruits/Tree Nuts"]
["01243","012","012 Fresh Fruits/Tree Nuts"]
["01244","012","012 Fresh Fruits/Tree Nuts"]
["01245","012","012 Fresh Fruits/Tree Nuts"]
["01246","012","012 Fresh Fruits/Tree Nuts"]
["01247","012","012 Fresh Fruits/Tree Nuts"]
["01248","012","012 Fresh Fruits/Tree Nuts"]
["01249","012","012 Fresh Fruits/Tree Nuts"]
["01250","012","012 Fresh Fruits/Tree Nuts"]
["01251","012","012 Fresh Fruits/Tree Nuts"]
["01252","012","012 Fresh Fruits/Tree Nuts"]
["01253","012","012 Fresh Fruits/Tree Nuts"]
["01254","012","012 Fresh Fruits/Tree Nuts"]
["01255","012","012 Fresh Fruits/Tree Nuts"]
["01256","012","012 Fresh Fruits/Tree Nuts"]
["01257","012","012 Fresh Fruits/Tree Nuts"]
["01258","012","012 Fresh Fruits/Tree Nuts"]
["01259","012","012 Fresh Fruits/Tree Nuts"]
["01260","012","012 Fresh Fruits/Tree Nuts"]
["01261","012","012 Fresh Fruits/Tree Nuts"]
["01262","012","012 Fresh Fruits/Tree Nuts"]
["01263","012","012 Fresh Fruits/Tree Nuts"]
["01264","012","012 Fresh Fruits/Tree Nuts"]
["01265","012","012 Fresh Fruits/Tree Nuts"]
["01266","012","012 Fresh Fruits/Tree Nuts"]
["01267","012","012 Fresh Fruits/Tree Nuts"]
["01268","012","012 Fresh Fruits/Tree Nuts"]
["01269","012","012 Fresh Fruits/Tree Nuts"]
["01270","012","012 Fresh Fruits/Tree Nuts"]
["01271","012","012 Fresh Fruits/Tree Nuts"]
["01272","012","012 Fresh Fruits/Tree Nuts"]
["01273","012","012 Fresh Fruits/Tree Nuts"]
["01274","012","012 Fresh Fruits/Tree Nuts"]
["01275","012","012 Fresh Fruits/Tree Nuts"]
["01276","012","012 Fresh Fruits/Tree Nuts"]
["01277","012","012 Fresh Fruits/Tree Nuts"]
["01278","012","012 Fresh Fruits/Tree Nuts"]
["01279","012","012 Fresh Fruits/Tree Nuts"]
["01280","012","012 Fresh Fruits/Tree Nuts"]
["01281","012","012 Fresh Fruits/Tree Nuts"]
["01282","012","012 Fresh Fruits/Tree Nuts"]
["01283","012","012 Fresh Fruits/Tree Nuts"]
["01284","012","012 Fresh Fruits/Tree Nuts"]
["01285","012","012 Fresh Fruits/Tree Nuts"]
["01286","012","012 Fresh Fruits/Tree Nuts"]
["01287","012","012 Fresh Fruits/Tree Nuts"]
["01288","012","012 Fresh Fruits/Tree Nuts"]
["01289","012","012 Fresh Fruits/Tree Nuts"]
["01290","012","012 Fresh Fruits/Tree Nuts"]
["01291","012","012 Fresh Fruits/Tree Nuts"]
["01292","012","012 Fresh Fruits/Tree Nuts"]
["01293","012","012 Fresh Fruits/Tree Nuts"]
["01294","012","012 Fresh Fruits/Tree Nuts"]
["01295","012","012 Fresh Fruits/Tree Nuts"]
["01296","012","012 Fresh Fruits/Tree Nuts"]
["01297","012","012 Fresh Fruits/Tree Nuts"]
["01298","012","012 Fresh Fruits/Tree Nuts"]
["01299","012","012 Fresh Fruits/Tree Nuts"]
["01300","013","013 Fresh Vegetables"]
["01301","013","013 Fresh Vegetables"]
["01302","013","013 Fresh Vegetables"]
["01303","013","013 Fresh Vegetables"]
["01304","013","013 Fresh Vegetables"]
["01305","013","013 Fresh Vegetables"]
["01306","013","013 Fresh Vegetables"]
["01307","013","013 Fresh Vegetables"]
["01308","013","013 Fresh Vegetables"]
["01309","013","013 Fresh Vegetables"]
["01310","013","013 Fresh Vegetables"]
["01311","013","013 Fresh Vegetables"]
["01312","013","013 Fresh Vegetables"]
["01313","013","013 Fresh Vegetables"]
["01314","013","013 Fresh Vegetables"]
["01315","013","013 Fresh Vegetables"]
["01316","013","013 Fresh Vegetables"]
["01317","013","013 Fresh Vegetables"]
["01318","013","013 Fresh Vegetables"]
["01319","013","013 Fresh Vegetables"]
["01320","013","013 Fresh Vegetables"]
["01321","013","013 Fresh Vegetables"]
["01322","013","013 Fresh Vegetables"]
["01323","013","013 Fresh Vegetables"]
["01324","013","013 Fresh Vegetables"]
["01325","013","013 Fresh Vegetables"]
["01326","013","013 Fresh Vegetables"]
["01327","013","013 Fresh Vegetables"]
["01328","013","013 Fresh Vegetables"]
["01329","013","013 Fresh Vegetables"]
["01330","013","013 Fresh Vegetables"]
["01331","013","013 Fresh Vegetables"]
["01332","013","013 Fresh Vegetables"]
["01333","013","013 Fresh Vegetables"]
["01334","013","013 Fresh Vegetables"]
["01335","013","013 Fresh Vegetables"]
["01336","013","013 Fresh Vegetables"]
["01337","013","013 Fresh Vegetables"]
["01338","013","013 Fresh Vegetables"]
["01339","013","013 Fresh Vegetables"]
["01340","013","013 Fresh Vegetables"]
["01341","013","013 Fresh Vegetables"]
["01342","013","013 Fresh Vegetables"]
["01343","013","013 Fresh Vegetables"]
["01344","013","013 Fresh Vegetables"]
["01345","013","013 Fresh Vegetables"]
["01346","013","013 Fresh Vegetables"]
["01347","013","013 Fresh Vegetables"]
["01348","013","013 Fresh Vegetables"]
["01349","013","013 Fresh Vegetables"]
["01350","013","013 Fresh Vegetables"]
["01351","013","013 Fresh Vegetables"]
["01352","013","013 Fresh Vegetables"]
["01353","013","013 Fresh Vegetables"]
["01354","013","013 Fresh Vegetables"]
["01355","013","013 Fresh Vegetables"]
["01356","013","013 Fresh Vegetables"]
["01357","013","013 Fresh Vegetables"]
["01358","013","013 Fresh Vegetables"]
["01359","013","013 Fresh Vegetables"]
["01360","013","013 Fresh Vegetables"]
["01361","013","013 Fresh Vegetables"]
["01362","013","013 Fresh Vegetables"]
["01363","013","013 Fresh Vegetables"]
["01364","013","013 Fresh Vegetables"]
["01365","013","013 Fresh Vegetables"]
["01366","013","013 Fresh Vegetables"]
["01367","013","013 Fresh Vegetables"]
["01368","013","013 Fresh Vegetables"]
["01369","013","013 Fresh Vegetables"]
["01370","013","013 Fresh Vegetables"]
["01371","013","013 Fresh Vegetables"]
["01372","013","013 Fresh Vegetables"]
["01373","013","013 Fresh Vegetables"]
["01374","013","013 Fresh Vegetables"]
["01375","013","013 Fresh Vegetables"]
["01376","013","013 Fresh Vegetables"]
["01377","013","013 Fresh Vegetables"]
["01378","013","013 Fresh Vegetables"]
["01379","013","013 Fresh Vegetables"]
["01380","013","013 Fresh Vegetables"]
["01381","013","013 Fresh Vegetables"]
["01382","013","013 Fresh Vegetables"]
["01383","013","013 Fresh Vegetables"]
["01384","013","013 Fresh Vegetables"]
["01385","013","013 Fresh Vegetables"]
["01386","013","013 Fresh Vegetables"]
["01387","013","013 Fresh Vegetables"]
["01388","013","013 Fresh Vegetables"]
["01389","013","013 Fresh Vegetables"]
["01390","013","013 Fresh Vegetables"]
["01391","013","013 Fresh Vegetables"]
["01392","013","013 Fresh Vegetables"]
["01393","013","013 Fresh Vegetables"]
["01394","013","013 Fresh Vegetables"]
["01395","013","013 Fresh Vegetables"]
["01396","013","013 Fresh Vegetables"]
["01397","013","013 Fresh Vegetables"]
["01398","013","013 Fresh Vegetables"]
["01399","013","013 Fresh Vegetables"]
["01400","01","01 Other Farm Products"]
["01401","01","01 Other Farm Products"]
["01402","01","01 Other Farm Products"]
["01403","01","01 Other Farm Products"]
["01404","01","01 Other Farm Products"]
["01405","01","01 Other Farm Products"]
["01406","01","01 Other Farm Products"]
["01407","01","01 Other Farm Products"]
["01408","01","01 Other Farm Products"]
["01409","01","01 Other Farm Products"]
["01410","01","01 Other Farm Products"]
["01411","01","01 Other Farm Products"]
["01412","01","01 Other Farm Products"]
["01413","01","01 Other Farm Products"]
["01414","01","01 Other Farm Products"]
["01415","01","01 Other Farm Products"]
["01416","01","01 Other Farm Products"]
["01417","01","01 Other Farm Products"]
["01418","01","01 Other Farm Products"]
["01419","01","01 Other Farm Products"]
["01420","01","01 Other Farm Products"]
["01421","01","01 Other Farm Products"]
["01422","01","01 Other Farm Products"]
["01423","01","01 Other Farm Products"]
["01424","01","01 Other Farm Products"]
["01425","01","01 Other Farm Products"]
["01426","01","01 Other Farm Products"]
["01427","01","01 Other Farm Products"]
["01428","01","01 Other Farm Products"]
["01429","01","01 Other Farm Products"]
["01430","01","01 Other Farm Products"]
["01431","01","01 Other Farm Products"]
["01432","01","01 Other Farm Products"]
["01433","01","01 Other Farm Products"]
["01434","01","01 Other Farm Products"]
["01435","01","01 Other Farm Products"]
["01436","01","01 Other Farm Products"]
["01437","01","01 Other Farm Products"]
["01438","01","01 Other Farm Products"]
["01439","01","01 Other Farm Products"]
["01440","01","01 Other Farm Products"]
["01441","01","01 Other Farm Products"]
["01442","01","01 Other Farm Products"]
["01443","01","01 Other Farm Products"]
["01444","01","01 Other Farm Products"]
["01445","01","01 Other Farm Products"]
["01446","01","01 Other Farm Products"]
["01447","01","01 Other Farm Products"]
["01448","01","01 Other Farm Products"]
["01449","01","01 Other Farm Products"]
["01450","01","01 Other Farm Products"]
["01451","01","01 Other Farm Products"]
["01452","01","01 Other Farm Products"]
["01453","01","01 Other Farm Products"]
["01454","01","01 Other Farm Products"]
["01455","01","01 Other Farm Products"]
["01456","01","01 Other Farm Products"]
["01457","01","01 Other Farm Products"]
["01458","01","01 Other Farm Products"]
["01459","01","01 Other Farm Products"]
["01460","01","01 Other Farm Products"]
["01461","01","01 Other Farm Products"]
["01462","01","01 Other Farm Products"]
["01463","01","01 Other Farm Products"]
["01464","01","01 Other Farm Products"]
["01465","01","01 Other Farm Products"]
["01466","01","01 Other Farm Products"]
["01467","01","01 Other Farm Products"]
["01468","01","01 Other Farm Products"]
["01469","01","01 Other Farm Products"]
["01470","01","01 Other Farm Products"]
["01471","01","01 Other Farm Products"]
["01472","01","01 Other Farm Products"]
["01473","01","01 Other Farm Products"]
["01474","01","01 Other Farm Products"]
["01475","01","01 Other Farm Products"]
["01476","01","01 Other Farm Products"]
["01477","01","01 Other Farm Products"]
["01478","01","01 Other Farm Products"]
["01479","01","01 Other Farm Products"]
["01480","01","01 Other Farm Products"]
["01481","01","01 Other Farm Products"]
["01482","01","01 Other Farm Products"]
["01483","01","01 Other Farm Products"]
["01484","01","01 Other Farm Products"]
["01485","01","01 Other Farm Products"]
["01486","01","01 Other Farm Products"]
["01487","01","01 Other Farm Products"]
["01488","01","01 Other Farm Products"]
["01489","01","01 Other Farm Products"]
["01490","01","01 Other Farm Products"]
["01491","01","01 Other Farm Products"]
["01492","01","01 Other Farm Products"]
["01493","01","01 Other Farm Products"]
["01494","01","01 Other Farm Products"]
["01495","01","01 Other Farm Products"]
["01496","01","01 Other Farm Products"]
["01497","01","01 Other Farm Products"]
["01498","01","01 Other Farm Products"]
["01499","01","01 Other Farm Products"]
["01500","01","01 Other Farm Products"]
["01501","01","01 Other Farm Products"]
["01502","01","01 Other Farm Products"]
["01503","01","01 Other Farm Products"]
["01504","01","01 Other Farm Products"]
["01505","01","01 Other Farm Products"]
["01506","01","01 Other Farm Products"]
["01507","01","01 Other Farm Products"]
["01508","01","01 Other Farm Products"]
["01509","01","01 Other Farm Products"]
["01510","01","01 Other Farm Products"]
["01511","01","01 Other Farm Products"]
["01512","01","01 Other Farm Products"]
["01513","01","01 Other Farm Products"]
["01514","01","01 Other Farm Products"]
["01515","01","01 Other Farm Products"]
["01516","01","01 Other Farm Products"]
["01517","01","01 Other Farm Products"]
["01518","01","01 Other Farm Products"]
["01519","01","01 Other Farm Products"]
["01520","01","01 Other Farm Products"]
["01521","01","01 Other Farm Products"]
["01522","01","01 Other Farm Products"]
["01523","01","01 Other Farm Products"]
["01524","01","01 Other Farm Products"]
["01525","01","01 Other Farm Products"]
["01526","01","01 Other Farm Products"]
["01527","01","01 Other Farm Products"]
["01528","01","01 Other Farm Products"]
["01529","01","01 Other Farm Products"]
["01530","01","01 Other Farm Products"]
["01531","01","01 Other Farm Products"]
["01532","01","01 Other Farm Products"]
["01533","01","01 Other Farm Products"]
["01534","01","01 Other Farm Products"]
["01535","01","01 Other Farm Products"]
["01536","01","01 Other Farm Products"]
["01537","01","01 Other Farm Products"]
["01538","01","01 Other Farm Products"]
["01539","01","01 Other Farm Products"]
["01540","01","01 Other Farm Products"]
["01541","01","01 Other Farm Products"]
["01542","01","01 Other Farm Products"]
["01543","01","01 Other Farm Products"]
["01544","01","01 Other Farm Products"]
["01545","01","01 Other Farm Products"]
["01546","01","01 Other Farm Products"]
["01547","01","01 Other Farm Products"]
["01548","01","01 Other Farm Products"]
["01549","01","01 Other Farm Products"]
["01550","01","01 Other Farm Products"]
["01551","01","01 Other Farm Products"]
["01552","01","01 Other Farm Products"]
["01553","01","01 Other Farm Products"]
["01554","01","01 Other Farm Products"]
["01555","01","01 Other Farm Products"]
["01556","01","01 Other Farm Products"]
["01557","01","01 Other Farm Products"]
["01558","01","01 Other Farm Products"]
["01559","01","01 Other Farm Products"]
["01560","01","01 Other Farm Products"]
["01561","01","01 Other Farm Products"]
["01562","01","01 Other Farm Products"]
["01563","01","01 Other Farm Products"]
["01564","01","01 Other Farm Products"]
["01565","01","01 Other Farm Products"]
["01566","01","01 Other Farm Products"]
["01567","01","01 Other Farm Products"]
["01568","01","01 Other Farm Products"]
["01569","01","01 Other Farm Products"]
["01570","01","01 Other Farm Products"]
["01571","01","01 Other Farm Products"]
["01572","01","01 Other Farm Products"]
["01573","01","01 Other Farm Products"]
["01574","01","01 Other Farm Products"]
["01575","01","01 Other Farm Products"]
["01576","01","01 Other Farm Products"]
["01577","01","01 Other Farm Products"]
["01578","01","01 Other Farm Products"]
["01579","01","01 Other Farm Products"]
["01580","01","01 Other Farm Products"]
["01581","01","01 Other Farm Products"]
["01582","01","01 Other Farm Products"]
["01583","01","01 Other Farm Products"]
["01584","01","01 Other Farm Products"]
["01585","01","01 Other Farm Products"]
["01586","01","01 Other Farm Products"]
["01587","01","01 Other Farm Products"]
["01588","01","01 Other Farm Products"]
["01589","01","01 Other Farm Products"]
["01590","01","01 Other Farm Products"]
["01591","01","01 Other Farm Products"]
["01592","01","01 Other Farm Products"]
["01593","01","01 Other Farm Products"]
["01594","01","01 Other Farm Products"]
["01595","01","01 Other Farm Products"]
["01596","01","01 Other Farm Products"]
["01597","01","01 Other Farm Products"]
["01598","01","01 Other Farm Products"]
["01599","01","01 Other Farm Products"]
["01600","01","01 Other Farm Products"]
["01601","01","01 Other Farm Products"]
["01602","01","01 Other Farm Products"]
["01603","01","01 Other Farm Products"]
["01604","01","01 Other Farm Products"]
["01605","01","01 Other Farm Products"]
["01606","01","01 Other Farm Products"]
["01607","01","01 Other Farm Products"]
["01608","01","01 Other Farm Products"]
["01609","01","01 Other Farm Products"]
["01610","01","01 Other Farm Products"]
["01611","01","01 Other Farm Products"]
["01612","01","01 Other Farm Products"]
["01613","01","01 Other Farm Products"]
["01614","01","01 Other Farm Products"]
["01615","01","01 Other Farm Products"]
["01616","01","01 Other Farm Products"]
["01617","01","01 Other Farm Products"]
["01618","01","01 Other Farm Products"]
["01619","01","01 Other Farm Products"]
["01620","01","01 Other Farm Products"]
["01621","01","01 Other Farm Products"]
["01622","01","01 Other Farm Products"]
["01623","01","01 Other Farm Products"]
["01624","01","01 Other Farm Products"]
["01625","01","01 Other Farm Products"]
["01626","01","01 Other Farm Products"]
["01627","01","01 Other Farm Products"]
["01628","01","01 Other Farm Products"]
["01629","01","01 Other Farm Products"]
["01630","01","01 Other Farm Products"]
["01631","01","01 Other Farm Products"]
["01632","01","01 Other Farm Products"]
["01633","01","01 Other Farm Products"]
["01634","01","01 Other Farm Products"]
["01635","01","01 Other Farm Products"]
["01636","01","01 Other Farm Products"]
["01637","01","01 Other Farm Products"]
["01638","01","01 Other Farm Products"]
["01639","01","01 Other Farm Products"]
["01640","01","01 Other Farm Products"]
["01641","01","01 Other Farm Products"]
["01642","01","01 Other Farm Products"]
["01643","01","01 Other Farm Products"]
["01644","01","01 Other Farm Products"]
["01645","01","01 Other Farm Products"]
["01646","01","01 Other Farm Products"]
["01647","01","01 Other Farm Products"]
["01648","01","01 Other Farm Products"]
["01649","01","01 Other Farm Products"]
["01650","01","01 Other Farm Products"]
["01651","01","01 Other Farm Products"]
["01652","01","01 Other Farm Products"]
["01653","01","01 Other Farm Products"]
["01654","01","01 Other Farm Products"]
["01655","01","01 Other Farm Products"]
["01656","01","01 Other Farm Products"]
["01657","01","01 Other Farm Products"]
["01658","01","01 Other Farm Products"]
["01659","01","01 Other Farm Products"]
["01660","01","01 Other Farm Products"]
["01661","01","01 Other Farm Products"]
["01662","01","01 Other Farm Products"]
["01663","01","01 Other Farm Products"]
["01664","01","01 Other Farm Products"]
["01665","01","01 Other Farm Products"]
["01666","01","01 Other Farm Products"]
["01667","01","01 Other Farm Products"]
["01668","01","01 Other Farm Products"]
["01669","01","01 Other Farm Products"]
["01670","01","01 Other Farm Products"]
["01671","01","01 Other Farm Products"]
["01672","01","01 Other Farm Products"]
["01673","01","01 Other Farm Products"]
["01674","01","01 Other Farm Products"]
["01675","01","01 Other Farm Products"]
["01676","01","01 Other Farm Products"]
["01677","01","01 Other Farm Products"]
["01678","01","01 Other Farm Products"]
["01679","01","01 Other Farm Products"]
["01680","01","01 Other Farm Products"]
["01681","01","01 Other Farm Products"]
["01682","01","01 Other Farm Products"]
["01683","01","01 Other Farm Products"]
["01684","01","01 Other Farm Products"]
["01685","01","01 Other Farm Products"]
["01686","01","01 Other Farm Products"]
["01687","01","01 Other Farm Products"]
["01688","01","01 Other Farm Products"]
["01689","01","01 Other Farm Products"]
["01690","01","01 Other Farm Products"]
["01691","01","01 Other Farm Products"]
["01692","01","01 Other Farm Products"]
["01693","01","01 Other Farm Products"]
["01694","01","01 Other Farm Products"]
["01695","01","01 Other Farm Products"]
["01696","01","01 Other Farm Products"]
["01697","01","01 Other Farm Products"]
["01698","01","01 Other Farm Products"]
["01699","01","01 Other Farm Products"]
["01700","01","01 Other Farm Products"]
["01701","01","01 Other Farm Products"]
["01702","01","01 Other Farm Products"]
["01703","01","01 Other Farm Products"]
["01704","01","01 Other Farm Products"]
["01705","01","01 Other Farm Products"]
["01706","01","01 Other Farm Products"]
["01707","01","01 Other Farm Products"]
["01708","01","01 Other Farm Products"]
["01709","01","01 Other Farm Products"]
["01710","01","01 Other Farm Products"]
["01711","01","01 Other Farm Products"]
["01712","01","01 Other Farm Products"]
["01713","01","01 Other Farm Products"]
["01714","01","01 Other Farm Products"]
["01715","01","01 Other Farm Products"]
["01716","01","01 Other Farm Products"]
["01717","01","01 Other Farm Products"]
["01718","01","01 Other Farm Products"]
["01719","01","01 Other Farm Products"]
["01720","01","01 Other Farm Products"]
["01721","01","01 Other Farm Products"]
["01722","01","01 Other Farm Products"]
["01723","01","01 Other Farm Products"]
["01724","01","01 Other Farm Products"]
["01725","01","01 Other Farm Products"]
["01726","01","01 Other Farm Products"]
["01727","01","01 Other Farm Products"]
["01728","01","01 Other Farm Products"]
["01729","01","01 Other Farm Products"]
["01730","01","01 Other Farm Products"]
["01731","01","01 Other Farm Products"]
["01732","01","01 Other Farm Products"]
["01733","01","01 Other Farm Products"]
["01734","01","01 Other Farm Products"]
["01735","01","01 Other Farm Products"]
["01736","01","01 Other Farm Products"]
["01737","01","01 Other Farm Products"]
["01738","01","01 Other Farm Products"]
["01739","01","01 Other Farm Products"]
["01740","01","01 Other Farm Products"]
["01741","01","01 Other Farm Products"]
["01742","01","01 Other Farm Products"]
["01743","01","01 Other Farm Products"]
["01744","01","01 Other Farm Products"]
["01745","01","01 Other Farm Products"]
["01746","01","01 Other Farm Products"]
["01747","01","01 Other Farm Products"]
["01748","01","01 Other Farm Products"]
["01749","01","01 Other Farm Products"]
["01750","01","01 Other Farm Products"]
["01751","01","01 Other Farm Products"]
["01752","01","01 Other Farm Products"]
["01753","01","01 Other Farm Products"]
["01754","01","01 Other Farm Products"]
["01755","01","01 Other Farm Products"]
["01756","01","01 Other Farm Products"]
["01757","01","01 Other Farm Products"]
["01758","01","01 Other Farm Products"]
["01759","01","01 Other Farm Products"]
["01760","01","01 Other Farm Products"]
["01761","01","01 Other Farm Products"]
["01762","01","01 Other Farm Products"]
["01763","01","01 Other Farm Products"]
["01764","01","01 Other Farm Products"]
["01765","01","01 Other Farm Products"]
["01766","01","01 Other Farm Products"]
["01767","01","01 Other Farm Products"]
["01768","01","01 Other Farm Products"]
["01769","01","01 Other Farm Products"]
["01770","01","01 Other Farm Products"]
["01771","01","01 Other Farm Products"]
["01772","01","01 Other Farm Products"]
["01773","01","01 Other Farm Products"]
["01774","01","01 Other Farm Products"]
["01775","01","01 Other Farm Products"]
["01776","01","01 Other Farm Products"]
["01777","01","01 Other Farm Products"]
["01778","01","01 Other Farm Products"]
["01779","01","01 Other Farm Products"]
["01780","01","01 Other Farm Products"]
["01781","01","01 Other Farm Products"]
["01782","01","01 Other Farm Products"]
["01783","01","01 Other Farm Products"]
["01784","01","01 Other Farm Products"]
["01785","01","01 Other Farm Products"]
["01786","01","01 Other Farm Products"]
["01787","01","01 Other Farm Products"]
["01788","01","01 Other Farm Products"]
["01789","01","01 Other Farm Products"]
["01790","01","01 Other Farm Products"]
["01791","01","01 Other Farm Products"]
["01792","01","01 Other Farm Products"]
["01793","01","01 Other Farm Products"]
["01794","01","01 Other Farm Products"]
["01795","01","01 Other Farm Products"]
["01796","01","01 Other Farm Products"]
["01797","01","01 Other Farm Products"]
["01798","01","01 Other Farm Products"]
["01799","01","01 Other Farm Products"]
["01800","01","01 Other Farm Products"]
["01801","01","01 Other Farm Products"]
["01802","01","01 Other Farm Products"]
["01803","01","01 Other Farm Products"]
["01804","01","01 Other Farm Products"]
["01805","01","01 Other Farm Products"]
["01806","01","01 Other Farm Products"]
["01807","01","01 Other Farm Products"]
["01808","01","01 Other Farm Products"]
["01809","01","01 Other Farm Products"]
["01810","01","01 Other Farm Products"]
["01811","01","01 Other Farm Products"]
["01812","01","01 Other Farm Products"]
["01813","01","01 Other Farm Products"]
["01814","01","01 Other Farm Products"]
["01815","01","01 Other Farm Products"]
["01816","01","01 Other Farm Products"]
["01817","01","01 Other Farm Products"]
["01818","01","01 Other Farm Products"]
["01819","01","01 Other Farm Products"]
["01820","01","01 Other Farm Products"]
["01821","01","01 Other Farm Products"]
["01822","01","01 Other Farm Products"]
["01823","01","01 Other Farm Products"]
["01824","01","01 Other Farm Products"]
["01825","01","01 Other Farm Products"]
["01826","01","01 Other Farm Products"]
["01827","01","01 Other Farm Products"]
["01828","01","01 Other Farm Products"]
["01829","01","01 Other Farm Products"]
["01830","01","01 Other Farm Products"]
["01831","01","01 Other Farm Products"]
["01832","01","01 Other Farm Products"]
["01833","01","01 Other Farm Products"]
["01834","01","01 Other Farm Products"]
["01835","01","01 Other Farm Products"]
["01836","01","01 Other Farm Products"]
["01837","01","01 Other Farm Products"]
["01838","01","01 Other Farm Products"]
["01839","01","01 Other Farm Products"]
["01840","01","01 Other Farm Products"]
["01841","01","01 Other Farm Products"]
["01842","01","01 Other Farm Products"]
["01843","01","01 Other Farm Products"]
["01844","01","01 Other Farm Products"]
["01845","01","01 Other Farm Products"]
["01846","01","01 Other Farm Products"]
["01847","01","01 Other Farm Products"]
["01848","01","01 Other Farm Products"]
["01849","01","01 Other Farm Products"]
["01850","01","01 Other Farm Products"]
["01851","01","01 Other Farm Products"]
["01852","01","01 Other Farm Products"]
["01853","01","01 Other Farm Products"]
["01854","01","01 Other Farm Products"]
["01855","01","01 Other Farm Products"]
["01856","01","01 Other Farm Products"]
["01857","01","01 Other Farm Products"]
["01858","01","01 Other Farm Products"]
["01859","01","01 Other Farm Products"]
["01860","01","01 Other Farm Products"]
["01861","01","01 Other Farm Products"]
["01862","01","01 Other Farm Products"]
["01863","01","01 Other Farm Products"]
["01864","01","01 Other Farm Products"]
["01865","01","01 Other Farm Products"]
["01866","01","01 Other Farm Products"]
["01867","01","01 Other Farm Products"]
["01868","01","01 Other Farm Products"]
["01869","01","01 Other Farm Products"]
["01870","01","01 Other Farm Products"]
["01871","01","01 Other Farm Products"]
["01872","01","01 Other Farm Products"]
["01873","01","01 Other Farm Products"]
["01874","01","01 Other Farm Products"]
["01875","01","01 Other Farm Products"]
["01876","01","01 Other Farm Products"]
["01877","01","01 Other Farm Products"]
["01878","01","01 Other Farm Products"]
["01879","01","01 Other Farm Products"]
["01880","01","01 Other Farm Products"]
["01881","01","01 Other Farm Products"]
["01882","01","01 Other Farm Products"]
["01883","01","01 Other Farm Products"]
["01884","01","01 Other Farm Products"]
["01885","01","01 Other Farm Products"]
["01886","01","01 Other Farm Products"]
["01887","01","01 Other Farm Products"]
["01888","01","01 Other Farm Products"]
["01889","01","01 Other Farm Products"]
["01890","01","01 Other Farm Products"]
["01891","01","01 Other Farm Products"]
["01892","01","01 Other Farm Products"]
["01893","01","01 Other Farm Products"]
["01894","01","01 Other Farm Products"]
["01895","01","01 Other Farm Products"]
["01896","01","01 Other Farm Products"]
["01897","01","01 Other Farm Products"]
["01898","01","01 Other Farm Products"]
["01899","01","01 Other Farm Products"]
["01900","01","01 Other Farm Products"]
["01901","01","01 Other Farm Products"]
["01902","01","01 Other Farm Products"]
["01903","01","01 Other Farm Products"]
["01904","01","01 Other Farm Products"]
["01905","01","01 Other Farm Products"]
["01906","01","01 Other Farm Products"]
["01907","01","01 Other Farm Products"]
["01908","01","01 Other Farm Products"]
["01909","01","01 Other Farm Products"]
["01910","01","01 Other Farm Products"]
["01911","01","01 Other Farm Products"]
["01912","01","01 Other Farm Products"]
["01913","01","01 Other Farm Products"]
["01914","01","01 Other Farm Products"]
["01915","01","01 Other Farm Products"]
["01916","01","01 Other Farm Products"]
["01917","01","01 Other Farm Products"]
["01918","01","01 Other Farm Products"]
["01919","01","01 Other Farm Products"]
["01920","01","01 Other Farm Products"]
["01921","01","01 Other Farm Products"]
["01922","01","01 Other Farm Products"]
["01923","01","01 Other Farm Products"]
["01924","01","01 Other Farm Products"]
["01925","01","01 Other Farm Products"]
["01926","01","01 Other Farm Products"]
["01927","01","01 Other Farm Products"]
["01928","01","01 Other Farm Products"]
["01929","01","01 Other Farm Products"]
["01930","01","01 Other Farm Products"]
["01931","01","01 Other Farm Products"]
["01932","01","01 Other Farm Products"]
["01933","01","01 Other Farm Products"]
["01934","01","01 Other Farm Products"]
["01935","01","01 Other Farm Products"]
["01936","01","01 Other Farm Products"]
["01937","01","01 Other Farm Products"]
["01938","01","01 Other Farm Products"]
["01939","01","01 Other Farm Products"]
["01940","01","01 Other Farm Products"]
["01941","01","01 Other Farm Products"]
["01942","01","01 Other Farm Products"]
["01943","01","01 Other Farm Products"]
["01944","01","01 Other Farm Products"]
["01945","01","01 Other Farm Products"]
["01946","01","01 Other Farm Products"]
["01947","01","01 Other Farm Products"]
["01948","01","01 Other Farm Products"]
["01949","01","01 Other Farm Products"]
["01950","01","01 Other Farm Products"]
["01951","01","01 Other Farm Products"]
["01952","01","01 Other Farm Products"]
["01953","01","01 Other Farm Products"]
["01954","01","01 Other Farm Products"]
["01955","01","01 Other Farm Products"]
["01956","01","01 Other Farm Products"]
["01957","01","01 Other Farm Products"]
["01958","01","01 Other Farm Products"]
["01959","01","01 Other Farm Products"]
["01960","01","01 Other Farm Products"]
["01961","01","01 Other Farm Products"]
["01962","01","01 Other Farm Products"]
["01963","01","01 Other Farm Products"]
["01964","01","01 Other Farm Products"]
["01965","01","01 Other Farm Products"]
["01966","01","01 Other Farm Products"]
["01967","01","01 Other Farm Products"]
["01968","01","01 Other Farm Products"]
["01969","01","01 Other Farm Products"]
["01970","01","01 Other Farm Products"]
["01971","01","01 Other Farm Products"]
["01972","01","01 Other Farm Products"]
["01973","01","01 Other Farm Products"]
["01974","01","01 Other Farm Products"]
["01975","01","01 Other Farm Products"]
["01976","01","01 Other Farm Products"]
["01977","01","01 Other Farm Products"]
["01978","01","01 Other Farm Products"]
["01979","01","01 Other Farm Products"]
["01980","01","01 Other Farm Products"]
["01981","01","01 Other Farm Products"]
["01982","01","01 Other Farm Products"]
["01983","01","01 Other Farm Products"]
["01984","01","01 Other Farm Products"]
["01985","01","01 Other Farm Products"]
["01986","01","01 Other Farm Products"]
["01987","01","01 Other Farm Products"]
["01988","01","01 Other Farm Products"]
["01989","01","01 Other Farm Products"]
["01990","01","01 Other Farm Products"]
["01991","01","01 Other Farm Products"]
["01992","01","01 Other Farm Products"]
["01993","01","01 Other Farm Products"]
["01994","01","01 Other Farm Products"]
["01995","01","01 Other Farm Products"]
["01996","01","01 Other Farm Products"]
["01997","01","01 Other Farm Products"]
["01998","01","01 Other Farm Products"]
["01999","01","01 Other Farm Products"]
["08000","Other","Other Commodities"]
["08001","Other","Other Commodities"]
["08002","Other","Other Commodities"]
["08003","Other","Other Commodities"]
["08004","Other","Other Commodities"]
["08005","Other","Other Commodities"]
["08006","Other","Other Commodities"]
["08007","Other","Other Commodities"]
["08008","Other","Other Commodities"]
["08009","Other","Other Commodities"]
["08010","Other","Other Commodities"]
["08011","Other","Other Commodities"]
["08012","Other","Other Commodities"]
["08013","Other","Other Commodities"]
["08014","Other","Other Commodities"]
["08015","Other","Other Commodities"]
["08016","Other","Other Commodities"]
["08017","Other","Other Commodities"]
["08018","Other","Other Commodities"]
["08019","Other","Other Commodities"]
["08020","Other","Other Commodities"]
["08021","Other","Other Commodities"]
["08022","Other","Other Commodities"]
["08023","Other","Other Commodities"]
["08024","Other","Other Commodities"]
["08025","Other","Other Commodities"]
["08026","Other","Other Commodities"]
["08027","Other","Other Commodities"]
["08028","Other","Other Commodities"]
["08029","Other","Other Commodities"]
["08030","Other","Other Commodities"]
["08031","Other","Other Commodities"]
["08032","Other","Other Commodities"]
["08033","Other","Other Commodities"]
["08034","Other","Other Commodities"]
["08035","Other","Other Commodities"]
["08036","Other","Other Commodities"]
["08037","Other","Other Commodities"]
["08038","Other","Other Commodities"]
["08039","Other","Other Commodities"]
["08040","Other","Other Commodities"]
["08041","Other","Other Commodities"]
["08042","Other","Other Commodities"]
["08043","Other","Other Commodities"]
["08044","Other","Other Commodities"]
["08045","Other","Other Commodities"]
["08046","Other","Other Commodities"]
["08047","Other","Other Commodities"]
["08048","Other","Other Commodities"]
["08049","Other","Other Commodities"]
["08050","Other","Other Commodities"]
["08051","Other","Other Commodities"]
["08052","Other","Other Commodities"]
["08053","Other","Other Commodities"]
["08054","Other","Other Commodities"]
["08055","Other","Other Commodities"]
["08056","Other","Other Commodities"]
["08057","Other","Other Commodities"]
["08058","Other","Other Commodities"]
["08059","Other","Other Commodities"]
["08060","Other","Other Commodities"]
["08061","Other","Other Commodities"]
["08062","Other","Other Commodities"]
["08063","Other","Other Commodities"]
["08064","Other","Other Commodities"]
["08065","Other","Other Commodities"]
["08066","Other","Other Commodities"]
["08067","Other","Other Commodities"]
["08068","Other","Other Commodities"]
["08069","Other","Other Commodities"]
["08070","Other","Other Commodities"]
["08071","Other","Other Commodities"]
["08072","Other","Other Commodities"]
["08073","Other","Other Commodities"]
["08074","Other","Other Commodities"]
["08075","Other","Other Commodities"]
["08076","Other","Other Commodities"]
["08077","Other","Other Commodities"]
["08078","Other","Other Commodities"]
["08079","Other","Other Commodities"]
["08080","Other","Other Commodities"]
["08081","Other","Other Commodities"]
["08082","Other","Other Commodities"]
["08083","Other","Other Commodities"]
["08084","Other","Other Commodities"]
["08085","Other","Other Commodities"]
["08086","Other","Other Commodities"]
["08087","Other","Other Commodities"]
["08088","Other","Other Commodities"]
["08089","Other","Other Commodities"]
["08090","Other","Other Commodities"]
["08091","Other","Other Commodities"]
["08092","Other","Other Commodities"]
["08093","Other","Other Commodities"]
["08094","Other","Other Commodities"]
["08095","Other","Other Commodities"]
["08096","Other","Other Commodities"]
["08097","Other","Other Commodities"]
["08098","Other","Other Commodities"]
["08099","Other","Other Commodities"]
["08100","Other","Other Commodities"]
["08101","Other","Other Commodities"]
["08102","Other","Other Commodities"]
["08103","Other","Other Commodities"]
["08104","Other","Other Commodities"]
["08105","Other","Other Commodities"]
["08106","Other","Other Commodities"]
["08107","Other","Other Commodities"]
["08108","Other","Other Commodities"]
["08109","Other","Other Commodities"]
["08110","Other","Other Commodities"]
["08111","Other","Other Commodities"]
["08112","Other","Other Commodities"]
["08113","Other","Other Commodities"]
["08114","Other","Other Commodities"]
["08115","Other","Other Commodities"]
["08116","Other","Other Commodities"]
["08117","Other","Other Commodities"]
["08118","Other","Other Commodities"]
["08119","Other","Other Commodities"]
["08120","Other","Other Commodities"]
["08121","Other","Other Commodities"]
["08122","Other","Other Commodities"]
["08123","Other","Other Commodities"]
["08124","Other","Other Commodities"]
["08125","Other","Other Commodities"]
["08126","Other","Other Commodities"]
["08127","Other","Other Commodities"]
["08128","Other","Other Commodities"]
["08129","Other","Other Commodities"]
["08130","Other","Other Commodities"]
["08131","Other","Other Commodities"]
["08132","Other","Other Commodities"]
["08133","Other","Other Commodities"]
["08134","Other","Other Commodities"]
["08135","Other","Other Commodities"]
["08136","Other","Other Commodities"]
["08137","Other","Other Commodities"]
["08138","Other","Other Commodities"]
["08139","Other","Other Commodities"]
["08140","Other","Other Commodities"]
["08141","Other","Other Commodities"]
["08142","Other","Other Commodities"]
["08143","Other","Other Commodities"]
["08144","Other","Other Commodities"]
["08145","Other","Other Commodities"]
["08146","Other","Other Commodities"]
["08147","Other","Other Commodities"]
["08148","Other","Other Commodities"]
["08149","Other","Other Commodities"]
["08150","Other","Other Commodities"]
["08151","Other","Other Commodities"]
["08152","Other","Other Commodities"]
["08153","Other","Other Commodities"]
["08154","Other","Other Commodities"]
["08155","Other","Other Commodities"]
["08156","Other","Other Commodities"]
["08157","Other","Other Commodities"]
["08158","Other","Other Commodities"]
["08159","Other","Other Commodities"]
["08160","Other","Other Commodities"]
["08161","Other","Other Commodities"]
["08162","Other","Other Commodities"]
["08163","Other","Other Commodities"]
["08164","Other","Other Commodities"]
["08165","Other","Other Commodities"]
["08166","Other","Other Commodities"]
["08167","Other","Other Commodities"]
["08168","Other","Other Commodities"]
["08169","Other","Other Commodities"]
["08170","Other","Other Commodities"]
["08171","Other","Other Commodities"]
["08172","Other","Other Commodities"]
["08173","Other","Other Commodities"]
["08174","Other","Other Commodities"]
["08175","Other","Other Commodities"]
["08176","Other","Other Commodities"]
["08177","Other","Other Commodities"]
["08178","Other","Other Commodities"]
["08179","Other","Other Commodities"]
["08180","Other","Other Commodities"]
["08181","Other","Other Commodities"]
["08182","Other","Other Commodities"]
["08183","Other","Other Commodities"]
["08184","Other","Other Commodities"]
["08185","Other","Other Commodities"]
["08186","Other","Other Commodities"]
["08187","Other","Other Commodities"]
["08188","Other","Other Commodities"]
["08189","Other","Other Commodities"]
["08190","Other","Other Commodities"]
["08191","Other","Other Commodities"]
["08192","Other","Other Commodities"]
["08193","Other","Other Commodities"]
["08194","Other","Other Commodities"]
["08195","Other","Other Commodities"]
["08196","Other","Other Commodities"]
["08197","Other","Other Commodities"]
["08198","Other","Other Commodities"]
["08199","Other","Other Commodities"]
["08200","Other","Other Commodities"]
["08201","Other","Other Commodities"]
["08202","Other","Other Commodities"]
["08203","Other","Other Commodities"]
["08204","Other","Other Commodities"]
["08205","Other","Other Commodities"]
["08206","Other","Other Commodities"]
["08207","Other","Other Commodities"]
["08208","Other","Other Commodities"]
["08209","Other","Other Commodities"]
["08210","Other","Other Commodities"]
["08211","Other","Other Commodities"]
["08212","Other","Other Commodities"]
["08213","Other","Other Commodities"]
["08214","Other","Other Commodities"]
["08215","Other","Other Commodities"]
["08216","Other","Other Commodities"]
["08217","Other","Other Commodities"]
["08218","Other","Other Commodities"]
["08219","Other","Other Commodities"]
["08220","Other","Other Commodities"]
["08221","Other","Other Commodities"]
["08222","Other","Other Commodities"]
["08223","Other","Other Commodities"]
["08224","Other","Other Commodities"]
["08225","Other","Other Commodities"]
["08226","Other","Other Commodities"]
["08227","Other","Other Commodities"]
["08228","Other","Other Commodities"]
["08229","Other","Other Commodities"]
["08230","Other","Other Commodities"]
["08231","Other","Other Commodities"]
["08232","Other","Other Commodities"]
["08233","Other","Other Commodities"]
["08234","Other","Other Commodities"]
["08235","Other","Other Commodities"]
["08236","Other","Other Commodities"]
["08237","Other","Other Commodities"]
["08238","Other","Other Commodities"]
["08239","Other","Other Commodities"]
["08240","Other","Other Commodities"]
["08241","Other","Other Commodities"]
["08242","Other","Other Commodities"]
["08243","Other","Other Commodities"]
["08244","Other","Other Commodities"]
["08245","Other","Other Commodities"]
["08246","Other","Other Commodities"]
["08247","Other","Other Commodities"]
["08248","Other","Other Commodities"]
["08249","Other","Other Commodities"]
["08250","Other","Other Commodities"]
["08251","Other","Other Commodities"]
["08252","Other","Other Commodities"]
["08253","Other","Other Commodities"]
["08254","Other","Other Commodities"]
["08255","Other","Other Commodities"]
["08256","Other","Other Commodities"]
["08257","Other","Other Commodities"]
["08258","Other","Other Commodities"]
["08259","Other","Other Commodities"]
["08260","Other","Other Commodities"]
["08261","Other","Other Commodities"]
["08262","Other","Other Commodities"]
["08263","Other","Other Commodities"]
["08264","Other","Other Commodities"]
["08265","Other","Other Commodities"]
["08266","Other","Other Commodities"]
["08267","Other","Other Commodities"]
["08268","Other","Other Commodities"]
["08269","Other","Other Commodities"]
["08270","Other","Other Commodities"]
["08271","Other","Other Commodities"]
["08272","Other","Other Commodities"]
["08273","Other","Other Commodities"]
["08274","Other","Other Commodities"]
["08275","Other","Other Commodities"]
["08276","Other","Other Commodities"]
["08277","Other","Other Commodities"]
["08278","Other","Other Commodities"]
["08279","Other","Other Commodities"]
["08280","Other","Other Commodities"]
["08281","Other","Other Commodities"]
["08282","Other","Other Commodities"]
["08283","Other","Other Commodities"]
["08284","Other","Other Commodities"]
["08285","Other","Other Commodities"]
["08286","Other","Other Commodities"]
["08287","Other","Other Commodities"]
["08288","Other","Other Commodities"]
["08289","Other","Other Commodities"]
["08290","Other","Other Commodities"]
["08291","Other","Other Commodities"]
["08292","Other","Other Commodities"]
["08293","Other","Other Commodities"]
["08294","Other","Other Commodities"]
["08295","Other","Other Commodities"]
["08296","Other","Other Commodities"]
["08297","Other","Other Commodities"]
["08298","Other","Other Commodities"]
["08299","Other","Other Commodities"]
["08300","Other","Other Commodities"]
["08301","Other","Other Commodities"]
["08302","Other","Other Commodities"]
["08303","Other","Other Commodities"]
["08304","Other","Other Commodities"]
["08305","Other","Other Commodities"]
["08306","Other","Other Commodities"]
["08307","Other","Other Commodities"]
["08308","Other","Other Commodities"]
["08309","Other","Other Commodities"]
["08310","Other","Other Commodities"]
["08311","Other","Other Commodities"]
["08312","Other","Other Commodities"]
["08313","Other","Other Commodities"]
["08314","Other","Other Commodities"]
["08315","Other","Other Commodities"]
["08316","Other","Other Commodities"]
["08317","Other","Other Commodities"]
["08318","Other","Other Commodities"]
["08319","Other","Other Commodities"]
["08320","Other","Other Commodities"]
["08321","Other","Other Commodities"]
["08322","Other","Other Commodities"]
["08323","Other","Other Commodities"]
["08324","Other","Other Commodities"]
["08325","Other","Other Commodities"]
["08326","Other","Other Commodities"]
["08327","Other","Other Commodities"]
["08328","Other","Other Commodities"]
["08329","Other","Other Commodities"]
["08330","Other","Other Commodities"]
["08331","Other","Other Commodities"]
["08332","Other","Other Commodities"]
["08333","Other","Other Commodities"]
["08334","Other","Other Commodities"]
["08335","Other","Other Commodities"]
["08336","Other","Other Commodities"]
["08337","Other","Other Commodities"]
["08338","Other","Other Commodities"]
["08339","Other","Other Commodities"]
["08340","Other","Other Commodities"]
["08341","Other","Other Commodities"]
["08342","Other","Other Commodities"]
["08343","Other","Other Commodities"]
["08344","Other","Other Commodities"]
["08345","Other","Other Commodities"]
["08346","Other","Other Commodities"]
["08347","Other","Other Commodities"]
["08348","Other","Other Commodities"]
["08349","Other","Other Commodities"]
["08350","Other","Other Commodities"]
["08351","Other","Other Commodities"]
["08352","Other","Other Commodities"]
["08353","Other","Other Commodities"]
["08354","Other","Other Commodities"]
["08355","Other","Other Commodities"]
["08356","Other","Other Commodities"]
["08357","Other","Other Commodities"]
["08358","Other","Other Commodities"]
["08359","Other","Other Commodities"]
["08360","Other","Other Commodities"]
["08361","Other","Other Commodities"]
["08362","Other","Other Commodities"]
["08363","Other","Other Commodities"]
["08364","Other","Other Commodities"]
["08365","Other","Other Commodities"]
["08366","Other","Other Commodities"]
["08367","Other","Other Commodities"]
["08368","Other","Other Commodities"]
["08369","Other","Other Commodities"]
["08370","Other","Other Commodities"]
["08371","Other","Other Commodities"]
["08372","Other","Other Commodities"]
["08373","Other","Other Commodities"]
["08374","Other","Other Commodities"]
["08375","Other","Other Commodities"]
["08376","Other","Other Commodities"]
["08377","Other","Other Commodities"]
["08378","Other","Other Commodities"]
["08379","Other","Other Commodities"]
["08380","Other","Other Commodities"]
["08381","Other","Other Commodities"]
["08382","Other","Other Commodities"]
["08383","Other","Other Commodities"]
["08384","Other","Other Commodities"]
["08385","Other","Other Commodities"]
["08386","Other","Other Commodities"]
["08387","Other","Other Commodities"]
["08388","Other","Other Commodities"]
["08389","Other","Other Commodities"]
["08390","Other","Other Commodities"]
["08391","Other","Other Commodities"]
["08392","Other","Other Commodities"]
["08393","Other","Other Commodities"]
["08394","Other","Other Commodities"]
["08395","Other","Other Commodities"]
["08396","Other","Other Commodities"]
["08397","Other","Other Commodities"]
["08398","Other","Other Commodities"]
["08399","Other","Other Commodities"]
["08400","Other","Other Commodities"]
["08401","Other","Other Commodities"]
["08402","Other","Other Commodities"]
["08403","Other","Other Commodities"]
["08404","Other","Other Commodities"]
["08405","Other","Other Commodities"]
["08406","Other","Other Commodities"]
["08407","Other","Other Commodities"]
["08408","Other","Other Commodities"]
["08409","Other","Other Commodities"]
["08410","Other","Other Commodities"]
["08411","Other","Other Commodities"]
["08412","Other","Other Commodities"]
["08413","Other","Other Commodities"]
["08414","Other","Other Commodities"]
["08415","Other","Other Commodities"]
["08416","Other","Other Commodities"]
["08417","Other","Other Commodities"]
["08418","Other","Other Commodities"]
["08419","Other","Other Commodities"]
["08420","Other","Other Commodities"]
["08421","Other","Other Commodities"]
["08422","Other","Other Commodities"]
["08423","Other","Other Commodities"]
["08424","Other","Other Commodities"]
["08425","Other","Other Commodities"]
["08426","Other","Other Commodities"]
["08427","Other","Other Commodities"]
["08428","Other","Other Commodities"]
["08429","Other","Other Commodities"]
["08430","Other","Other Commodities"]
["08431","Other","Other Commodities"]
["08432","Other","Other Commodities"]
["08433","Other","Other Commodities"]
["08434","Other","Other Commodities"]
["08435","Other","Other Commodities"]
["08436","Other","Other Commodities"]
["08437","Other","Other Commodities"]
["08438","Other","Other Commodities"]
["08439","Other","Other Commodities"]
["08440","Other","Other Commodities"]
["08441","Other","Other Commodities"]
["08442","Other","Other Commodities"]
["08443","Other","Other Commodities"]
["08444","Other","Other Commodities"]
["08445","Other","Other Commodities"]
["08446","Other","Other Commodities"]
["08447","Other","Other Commodities"]
["08448","Other","Other Commodities"]
["08449","Other","Other Commodities"]
["08450","Other","Other Commodities"]
["08451","Other","Other Commodities"]
["08452","Other","Other Commodities"]
["08453","Other","Other Commodities"]
["08454","Other","Other Commodities"]
["08455","Other","Other Commodities"]
["08456","Other","Other Commodities"]
["08457","Other","Other Commodities"]
["08458","Other","Other Commodities"]
["08459","Other","Other Commodities"]
["08460","Other","Other Commodities"]
["08461","Other","Other Commodities"]
["08462","Other","Other Commodities"]
["08463","Other","Other Commodities"]
["08464","Other","Other Commodities"]
["08465","Other","Other Commodities"]
["08466","Other","Other Commodities"]
["08467","Other","Other Commodities"]
["08468","Other","Other Commodities"]
["08469","Other","Other Commodities"]
["08470","Other","Other Commodities"]
["08471","Other","Other Commodities"]
["08472","Other","Other Commodities"]
["08473","Other","Other Commodities"]
["08474","Other","Other Commodities"]
["08475","Other","Other Commodities"]
["08476","Other","Other Commodities"]
["08477","Other","Other Commodities"]
["08478","Other","Other Commodities"]
["08479","Other","Other Commodities"]
["08480","Other","Other Commodities"]
["08481","Other","Other Commodities"]
["08482","Other","Other Commodities"]
["08483","Other","Other Commodities"]
["08484","Other","Other Commodities"]
["08485","Other","Other Commodities"]
["08486","Other","Other Commodities"]
["08487","Other","Other Commodities"]
["08488","Other","Other Commodities"]
["08489","Other","Other Commodities"]
["08490","Other","Other Commodities"]
["08491","Other","Other Commodities"]
["08492","Other","Other Commodities"]
["08493","Other","Other Commodities"]
["08494","Other","Other Commodities"]
["08495","Other","Other Commodities"]
["08496","Other","Other Commodities"]
["08497","Other","Other Commodities"]
["08498","Other","Other Commodities"]
["08499","Other","Other Commodities"]
["08500","Other","Other Commodities"]
["08501","Other","Other Commodities"]
["08502","Other","Other Commodities"]
["08503","Other","Other Commodities"]
["08504","Other","Other Commodities"]
["08505","Other","Other Commodities"]
["08506","Other","Other Commodities"]
["08507","Other","Other Commodities"]
["08508","Other","Other Commodities"]
["08509","Other","Other Commodities"]
["08510","Other","Other Commodities"]
["08511","Other","Other Commodities"]
["08512","Other","Other Commodities"]
["08513","Other","Other Commodities"]
["08514","Other","Other Commodities"]
["08515","Other","Other Commodities"]
["08516","Other","Other Commodities"]
["08517","Other","Other Commodities"]
["08518","Other","Other Commodities"]
["08519","Other","Other Commodities"]
["08520","Other","Other Commodities"]
["08521","Other","Other Commodities"]
["08522","Other","Other Commodities"]
["08523","Other","Other Commodities"]
["08524","Other","Other Commodities"]
["08525","Other","Other Commodities"]
["08526","Other","Other Commodities"]
["08527","Other","Other Commodities"]
["08528","Other","Other Commodities"]
["08529","Other","Other Commodities"]
["08530","Other","Other Commodities"]
["08531","Other","Other Commodities"]
["08532","Other","Other Commodities"]
["08533","Other","Other Commodities"]
["08534","Other","Other Commodities"]
["08535","Other","Other Commodities"]
["08536","Other","Other Commodities"]
["08537","Other","Other Commodities"]
["08538","Other","Other Commodities"]
["08539","Other","Other Commodities"]
["08540","Other","Other Commodities"]
["08541","Other","Other Commodities"]
["08542","Other","Other Commodities"]
["08543","Other","Other Commodities"]
["08544","Other","Other Commodities"]
["08545","Other","Other Commodities"]
["08546","Other","Other Commodities"]
["08547","Other","Other Commodities"]
["08548","Other","Other Commodities"]
["08549","Other","Other Commodities"]
["08550","Other","Other Commodities"]
["08551","Other","Other Commodities"]
["08552","Other","Other Commodities"]
["08553","Other","Other Commodities"]
["08554","Other","Other Commodities"]
["08555","Other","Other Commodities"]
["08556","Other","Other Commodities"]
["08557","Other","Other Commodities"]
["08558","Other","Other Commodities"]
["08559","Other","Other Commodities"]
["08560","Other","Other Commodities"]
["08561","Other","Other Commodities"]
["08562","Other","Other Commodities"]
["08563","Other","Other Commodities"]
["08564","Other","Other Commodities"]
["08565","Other","Other Commodities"]
["08566","Other","Other Commodities"]
["08567","Other","Other Commodities"]
["08568","Other","Other Commodities"]
["08569","Other","Other Commodities"]
["08570","Other","Other Commodities"]
["08571","Other","Other Commodities"]
["08572","Other","Other Commodities"]
["08573","Other","Other Commodities"]
["08574","Other","Other Commodities"]
["08575","Other","Other Commodities"]
["08576","Other","Other Commodities"]
["08577","Other","Other Commodities"]
["08578","Other","Other Commodities"]
["08579","Other","Other Commodities"]
["08580","Other","Other Commodities"]
["08581","Other","Other Commodities"]
["08582","Other","Other Commodities"]
["08583","Other","Other Commodities"]
["08584","Other","Other Commodities"]
["08585","Other","Other Commodities"]
["08586","Other","Other Commodities"]
["08587","Other","Other Commodities"]
["08588","Other","Other Commodities"]
["08589","Other","Other Commodities"]
["08590","Other","Other Commodities"]
["08591","Other","Other Commodities"]
["08592","Other","Other Commodities"]
["08593","Other","Other Commodities"]
["08594","Other","Other Commodities"]
["08595","Other","Other Commodities"]
["08596","Other","Other Commodities"]
["08597","Other","Other Commodities"]
["08598","Other","Other Commodities"]
["08599","Other","Other Commodities"]
["08600","Other","Other Commodities"]
["08601","Other","Other Commodities"]
["08602","Other","Other Commodities"]
["08603","Other","Other Commodities"]
["08604","Other","Other Commodities"]
["08605","Other","Other Commodities"]
["08606","Other","Other Commodities"]
["08607","Other","Other Commodities"]
["08608","Other","Other Commodities"]
["08609","Other","Other Commodities"]
["08610","Other","Other Commodities"]
["08611","Other","Other Commodities"]
["08612","Other","Other Commodities"]
["08613","Other","Other Commodities"]
["08614","Other","Other Commodities"]
["08615","Other","Other Commodities"]
["08616","Other","Other Commodities"]
["08617","Other","Other Commodities"]
["08618","Other","Other Commodities"]
["08619","Other","Other Commodities"]
["08620","Other","Other Commodities"]
["08621","Other","Other Commodities"]
["08622","Other","Other Commodities"]
["08623","Other","Other Commodities"]
["08624","Other","Other Commodities"]
["08625","Other","Other Commodities"]
["08626","Other","Other Commodities"]
["08627","Other","Other Commodities"]
["08628","Other","Other Commodities"]
["08629","Other","Other Commodities"]
["08630","Other","Other Commodities"]
["08631","Other","Other Commodities"]
["08632","Other","Other Commodities"]
["08633","Other","Other Commodities"]
["08634","Other","Other Commodities"]
["08635","Other","Other Commodities"]
["08636","Other","Other Commodities"]
["08637","Other","Other Commodities"]
["08638","Other","Other Commodities"]
["08639","Other","Other Commodities"]
["08640","Other","Other Commodities"]
["08641","Other","Other Commodities"]
["08642","Other","Other Commodities"]
["08643","Other","Other Commodities"]
["08644","Other","Other Commodities"]
["08645","Other","Other Commodities"]
["08646","Other","Other Commodities"]
["08647","Other","Other Commodities"]
["08648","Other","Other Commodities"]
["08649","Other","Other Commodities"]
["08650","Other","Other Commodities"]
["08651","Other","Other Commodities"]
["08652","Other","Other Commodities"]
["08653","Other","Other Commodities"]
["08654","Other","Other Commodities"]
["08655","Other","Other Commodities"]
["08656","Other","Other Commodities"]
["08657","Other","Other Commodities"]
["08658","Other","Other Commodities"]
["08659","Other","Other Commodities"]
["08660","Other","Other Commodities"]
["08661","Other","Other Commodities"]
["08662","Other","Other Commodities"]
["08663","Other","Other Commodities"]
["08664","Other","Other Commodities"]
["08665","Other","Other Commodities"]
["08666","Other","Other Commodities"]
["08667","Other","Other Commodities"]
["08668","Other","Other Commodities"]
["08669","Other","Other Commodities"]
["08670","Other","Other Commodities"]
["08671","Other","Other Commodities"]
["08672","Other","Other Commodities"]
["08673","Other","Other Commodities"]
["08674","Other","Other Commodities"]
["08675","Other","Other Commodities"]
["08676","Other","Other Commodities"]
["08677","Other","Other Commodities"]
["08678","Other","Other Commodities"]
["08679","Other","Other Commodities"]
["08680","Other","Other Commodities"]
["08681","Other","Other Commodities"]
["08682","Other","Other Commodities"]
["08683","Other","Other Commodities"]
["08684","Other","Other Commodities"]
["08685","Other","Other Commodities"]
["08686","Other","Other Commodities"]
["08687","Other","Other Commodities"]
["08688","Other","Other Commodities"]
["08689","Other","Other Commodities"]
["08690","Other","Other Commodities"]
["08691","Other","Other Commodities"]
["08692","Other","Other Commodities"]
["08693","Other","Other Commodities"]
["08694","Other","Other Commodities"]
["08695","Other","Other Commodities"]
["08696","Other","Other Commodities"]
["08697","Other","Other Commodities"]
["08698","Other","Other Commodities"]
["08699","Other","Other Commodities"]
["08700","Other","Other Commodities"]
["08701","Other","Other Commodities"]
["08702","Other","Other Commodities"]
["08703","Other","Other Commodities"]
["08704","Other","Other Commodities"]
["08705","Other","Other Commodities"]
["08706","Other","Other Commodities"]
["08707","Other","Other Commodities"]
["08708","Other","Other Commodities"]
["08709","Other","Other Commodities"]
["08710","Other","Other Commodities"]
["08711","Other","Other Commodities"]
["08712","Other","Other Commodities"]
["08713","Other","Other Commodities"]
["08714","Other","Other Commodities"]
["08715","Other","Other Commodities"]
["08716","Other","Other Commodities"]
["08717","Other","Other Commodities"]
["08718","Other","Other Commodities"]
["08719","Other","Other Commodities"]
["08720","Other","Other Commodities"]
["08721","Other","Other Commodities"]
["08722","Other","Other Commodities"]
["08723","Other","Other Commodities"]
["08724","Other","Other Commodities"]
["08725","Other","Other Commodities"]
["08726","Other","Other Commodities"]
["08727","Other","Other Commodities"]
["08728","Other","Other Commodities"]
["08729","Other","Other Commodities"]
["08730","Other","Other Commodities"]
["08731","Other","Other Commodities"]
["08732","Other","Other Commodities"]
["08733","Other","Other Commodities"]
["08734","Other","Other Commodities"]
["08735","Other","Other Commodities"]
["08736","Other","Other Commodities"]
["08737","Other","Other Commodities"]
["08738","Other","Other Commodities"]
["08739","Other","Other Commodities"]
["08740","Other","Other Commodities"]
["08741","Other","Other Commodities"]
["08742","Other","Other Commodities"]
["08743","Other","Other Commodities"]
["08744","Other","Other Commodities"]
["08745","Other","Other Commodities"]
["08746","Other","Other Commodities"]
["08747","Other","Other Commodities"]
["08748","Other","Other Commodities"]
["08749","Other","Other Commodities"]
["08750","Other","Other Commodities"]
["08751","Other","Other Commodities"]
["08752","Other","Other Commodities"]
["08753","Other","Other Commodities"]
["08754","Other","Other Commodities"]
["08755","Other","Other Commodities"]
["08756","Other","Other Commodities"]
["08757","Other","Other Commodities"]
["08758","Other","Other Commodities"]
["08759","Other","Other Commodities"]
["08760","Other","Other Commodities"]
["08761","Other","Other Commodities"]
["08762","Other","Other Commodities"]
["08763","Other","Other Commodities"]
["08764","Other","Other Commodities"]
["08765","Other","Other Commodities"]
["08766","Other","Other Commodities"]
["08767","Other","Other Commodities"]
["08768","Other","Other Commodities"]
["08769","Other","Other Commodities"]
["08770","Other","Other Commodities"]
["08771","Other","Other Commodities"]
["08772","Other","Other Commodities"]
["08773","Other","Other Commodities"]
["08774","Other","Other Commodities"]
["08775","Other","Other Commodities"]
["08776","Other","Other Commodities"]
["08777","Other","Other Commodities"]
["08778","Other","Other Commodities"]
["08779","Other","Other Commodities"]
["08780","Other","Other Commodities"]
["08781","Other","Other Commodities"]
["08782","Other","Other Commodities"]
["08783","Other","Other Commodities"]
["08784","Other","Other Commodities"]
["08785","Other","Other Commodities"]
["08786","Other","Other Commodities"]
["08787","Other","Other Commodities"]
["08788","Other","Other Commodities"]
["08789","Other","Other Commodities"]
["08790","Other","Other Commodities"]
["08791","Other","Other Commodities"]
["08792","Other","Other Commodities"]
["08793","Other","Other Commodities"]
["08794","Other","Other Commodities"]
["08795","Other","Other Commodities"]
["08796","Other","Other Commodities"]
["08797","Other","Other Commodities"]
["08798","Other","Other Commodities"]
["08799","Other","Other Commodities"]
["08800","Other","Other Commodities"]
["08801","Other","Other Commodities"]
["08802","Other","Other Commodities"]
["08803","Other","Other Commodities"]
["08804","Other","Other Commodities"]
["08805","Other","Other Commodities"]
["08806","Other","Other Commodities"]
["08807","Other","Other Commodities"]
["08808","Other","Other Commodities"]
["08809","Other","Other Commodities"]
["08810","Other","Other Commodities"]
["08811","Other","Other Commodities"]
["08812","Other","Other Commodities"]
["08813","Other","Other Commodities"]
["08814","Other","Other Commodities"]
["08815","Other","Other Commodities"]
["08816","Other","Other Commodities"]
["08817","Other","Other Commodities"]
["08818","Other","Other Commodities"]
["08819","Other","Other Commodities"]
["08820","Other","Other Commodities"]
["08821","Other","Other Commodities"]
["08822","Other","Other Commodities"]
["08823","Other","Other Commodities"]
["08824","Other","Other Commodities"]
["08825","Other","Other Commodities"]
["08826","Other","Other Commodities"]
["08827","Other","Other Commodities"]
["08828","Other","Other Commodities"]
["08829","Other","Other Commodities"]
["08830","Other","Other Commodities"]
["08831","Other","Other Commodities"]
["08832","Other","Other Commodities"]
["08833","Other","Other Commodities"]
["08834","Other","Other Commodities"]
["08835","Other","Other Commodities"]
["08836","Other","Other Commodities"]
["08837","Other","Other Commodities"]
["08838","Other","Other Commodities"]
["08839","Other","Other Commodities"]
["08840","Other","Other Commodities"]
["08841","Other","Other Commodities"]
["08842","Other","Other Commodities"]
["08843","Other","Other Commodities"]
["08844","Other","Other Commodities"]
["08845","Other","Other Commodities"]
["08846","Other","Other Commodities"]
["08847","Other","Other Commodities"]
["08848","Other","Other Commodities"]
["08849","Other","Other Commodities"]
["08850","Other","Other Commodities"]
["08851","Other","Other Commodities"]
["08852","Other","Other Commodities"]
["08853","Other","Other Commodities"]
["08854","Other","Other Commodities"]
["08855","Other","Other Commodities"]
["08856","Other","Other Commodities"]
["08857","Other","Other Commodities"]
["08858","Other","Other Commodities"]
["08859","Other","Other Commodities"]
["08860","Other","Other Commodities"]
["08861","Other","Other Commodities"]
["08862","Other","Other Commodities"]
["08863","Other","Other Commodities"]
["08864","Other","Other Commodities"]
["08865","Other","Other Commodities"]
["08866","Other","Other Commodities"]
["08867","Other","Other Commodities"]
["08868","Other","Other Commodities"]
["08869","Other","Other Commodities"]
["08870","Other","Other Commodities"]
["08871","Other","Other Commodities"]
["08872","Other","Other Commodities"]
["08873","Other","Other Commodities"]
["08874","Other","Other Commodities"]
["08875","Other","Other Commodities"]
["08876","Other","Other Commodities"]
["08877","Other","Other Commodities"]
["08878","Other","Other Commodities"]
["08879","Other","Other Commodities"]
["08880","Other","Other Commodities"]
["08881","Other","Other Commodities"]
["08882","Other","Other Commodities"]
["08883","Other","Other Commodities"]
["08884","Other","Other Commodities"]
["08885","Other","Other Commodities"]
["08886","Other","Other Commodities"]
["08887","Other","Other Commodities"]
["08888","Other","Other Commodities"]
["08889","Other","Other Commodities"]
["08890","Other","Other Commodities"]
["08891","Other","Other Commodities"]
["08892","Other","Other Commodities"]
["08893","Other","Other Commodities"]
["08894","Other","Other Commodities"]
["08895","Other","Other Commodities"]
["08896","Other","Other Commodities"]
["08897","Other","Other Commodities"]
["08898","Other","Other Commodities"]
["08899","Other","Other Commodities"]
["08900","Other","Other Commodities"]
["08901","Other","Other Commodities"]
["08902","Other","Other Commodities"]
["08903","Other","Other Commodities"]
["08904","Other","Other Commodities"]
["08905","Other","Other Commodities"]
["08906","Other","Other Commodities"]
["08907","Other","Other Commodities"]
["08908","Other","Other Commodities"]
["08909","Other","Other Commodities"]
["08910","Other","Other Commodities"]
["08911","Other","Other Commodities"]
["08912","Other","Other Commodities"]
["08913","Other","Other Commodities"]
["08914","Other","Other Commodities"]
["08915","Other","Other Commodities"]
["08916","Other","Other Commodities"]
["08917","Other","Other Commodities"]
["08918","Other","Other Commodities"]
["08919","Other","Other Commodities"]
["08920","Other","Other Commodities"]
["08921","Other","Other Commodities"]
["08922","Other","Other Commodities"]
["08923","Other","Other Commodities"]
["08924","Other","Other Commodities"]
["08925","Other","Other Commodities"]
["08926","Other","Other Commodities"]
["08927","Other","Other Commodities"]
["08928","Other","Other Commodities"]
["08929","Other","Other Commodities"]
["08930","Other","Other Commodities"]
["08931","Other","Other Commodities"]
["08932","Other","Other Commodities"]
["08933","Other","Other Commodities"]
["08934","Other","Other Commodities"]
["08935","Other","Other Commodities"]
["08936","Other","Other Commodities"]
["08937","Other","Other Commodities"]
["08938","Other","Other Commodities"]
["08939","Other","Other Commodities"]
["08940","Other","Other Commodities"]
["08941","Other","Other Commodities"]
["08942","Other","Other Commodities"]
["08943","Other","Other Commodities"]
["08944","Other","Other Commodities"]
["08945","Other","Other Commodities"]
["08946","Other","Other Commodities"]
["08947","Other","Other Commodities"]
["08948","Other","Other Commodities"]
["08949","Other","Other Commodities"]
["08950","Other","Other Commodities"]
["08951","Other","Other Commodities"]
["08952","Other","Other Commodities"]
["08953","Other","Other Commodities"]
["08954","Other","Other Commodities"]
["08955","Other","Other Commodities"]
["08956","Other","Other Commodities"]
["08957","Other","Other Commodities"]
["08958","Other","Other Commodities"]
["08959","Other","Other Commodities"]
["08960","Other","Other Commodities"]
["08961","Other","Other Commodities"]
["08962","Other","Other Commodities"]
["08963","Other","Other Commodities"]
["08964","Other","Other Commodities"]
["08965","Other","Other Commodities"]
["08966","Other","Other Commodities"]
["08967","Other","Other Commodities"]
["08968","Other","Other Commodities"]
["08969","Other","Other Commodities"]
["08970","Other","Other Commodities"]
["08971","Other","Other Commodities"]
["08972","Other","Other Commodities"]
["08973","Other","Other Commodities"]
["08974","Other","Other Commodities"]
["08975","Other","Other Commodities"]
["08976","Other","Other Commodities"]
["08977","Other","Other Commodities"]
["08978","Other","Other Commodities"]
["08979","Other","Other Commodities"]
["08980","Other","Other Commodities"]
["08981","Other","Other Commodities"]
["08982","Other","Other Commodities"]
["08983","Other","Other Commodities"]
["08984","Other","Other Commodities"]
["08985","Other","Other Commodities"]
["08986","Other","Other Commodities"]
["08987","Other","Other Commodities"]
["08988","Other","Other Commodities"]
["08989","Other","Other Commodities"]
["08990","Other","Other Commodities"]
["08991","Other","Other Commodities"]
["08992","Other","Other Commodities"]
["08993","Other","Other Commodities"]
["08994","Other","Other Commodities"]
["08995","Other","Other Commodities"]
["08996","Other","Other Commodities"]
["08997","Other","Other Commodities"]
["09013","Other","Other Commodities"]
["09020","Other","Other Commodities"]
["09041","Other","Other Commodities"]
["09059","Other","Other Commodities"]
["09088","Other","Other Commodities"]
["09091","Other","Other Commodities"]
["09116","Other","Other Commodities"]
["09138","Other","Other Commodities"]
["09145","Other","Other Commodities"]
["09166","Other","Other Commodities"]
["09187","Other","Other Commodities"]
["09204","Other","Other Commodities"]
["09234","Other","Other Commodities"]
["09237","Other","Other Commodities"]
["09262","Other","Other Commodities"]
["09283","Other","Other Commodities"]
["09291","Other","Other Commodities"]
["09312","Other","Other Commodities"]
["09333","Other","Other Commodities"]
["09349","Other","Other Commodities"]
["09380","Other","Other Commodities"]
["09387","Other","Other Commodities"]
["09408","Other","Other Commodities"]
["09428","Other","Other Commodities"]
["09437","Other","Other Commodities"]
["09458","Other","Other Commodities"]
["09479","Other","Other Commodities"]
["09494","Other","Other Commodities"]
["09526","Other","Other Commodities"]
["09533","Other","Other Commodities"]
["09554","Other","Other Commodities"]
["09573","Other","Other Commodities"]
["09583","Other","Other Commodities"]
["09604","Other","Other Commodities"]
["09625","Other","Other Commodities"]
["09639","Other","Other Commodities"]
["09672","Other","Other Commodities"]
["09679","Other","Other Commodities"]
["09700","Other","Other Commodities"]
["09718","Other","Other Commodities"]
["09729","Other","Other Commodities"]
["09750","Other","Other Commodities"]
["09775","Other","Other Commodities"]
["09784","Other","Other Commodities"]
["09818","Other","Other Commodities"]
["09825","Other","Other Commodities"]
["09846","Other","Other Commodities"]
["09863","Other","Other Commodities"]
["09875","Other","Other Commodities"]
["09896","Other","Other Commodities"]
["09921","Other","Other Commodities"]
["09929","Other","Other Commodities"]
["09964","Other","Other Commodities"]
["09971","Other","Other Commodities"]
["09992","Other","Other Commodities"]
["10014","10","10 Metallic Ores"]
["10021","10","10 Metallic Ores"]
["10042","10","10 Metallic Ores"]
["10067","10","10 Metallic Ores"]
["10074","10","10 Metallic Ores"]
["10110","10","10 Metallic Ores"]
["10117","10","10 Metallic Ores"]
["10138","10","10 Metallic Ores"]
["10159","10","10 Metallic Ores"]
["10167","10","10 Metallic Ores"]
["10188","10","10 Metallic Ores"]
["10213","10","10 Metallic Ores"]
["10238","10","10 Metallic Ores"]
["10256","10","10 Metallic Ores"]
["10263","10","10 Metallic Ores"]
["10284","10","10 Metallic Ores"]
["10304","10","10 Metallic Ores"]
["10313","10","10 Metallic Ores"]
["10334","10","10 Metallic Ores"]
["10359","10","10 Metallic Ores"]
["10383","10","10 Metallic Ores"]
["10388","10","10 Metallic Ores"]
["10409","10","10 Metallic Ores"]
["10430","10","10 Metallic Ores"]
["10449","10","10 Metallic Ores"]
["10459","10","10 Metallic Ores"]
["10480","10","10 Metallic Ores"]
["10505","10","10 Metallic Ores"]
["10528","10","10 Metallic Ores"]
["10534","10","10 Metallic Ores"]
["10555","10","10 Metallic Ores"]
["10576","10","10 Metallic Ores"]
["10594","10","10 Metallic Ores"]
["10605","10","10 Metallic Ores"]
["10626","10","10 Metallic Ores"]
["10651","10","10 Metallic Ores"]
["10673","10","10 Metallic Ores"]
["10680","10","10 Metallic Ores"]
["10701","10","10 Metallic Ores"]
["10722","10","10 Metallic Ores"]
["10739","10","10 Metallic Ores"]
["10751","10","10 Metallic Ores"]
["10776","10","10 Metallic Ores"]
["10797","10","10 Metallic Ores"]
["10818","10","10 Metallic Ores"]
["10826","10","10 Metallic Ores"]
["10847","10","10 Metallic Ores"]
["10868","10","10 Metallic Ores"]
["10884","10","10 Metallic Ores"]
["10897","10","10 Metallic Ores"]
["10922","10","10 Metallic Ores"]
["10943","10","10 Metallic Ores"]
["10963","10","10 Metallic Ores"]
["10972","10","10 Metallic Ores"]
["10993","10","10 Metallic Ores"]
["11018","11","11 Coal"]
["11029","11","11 Coal"]
["11043","11","11 Coal"]
["11068","11","11 Coal"]
["11089","11","11 Coal"]
["11108","11","11 Coal"]
["11118","11","11 Coal"]
["11139","11","11 Coal"]
["11164","11","11 Coal"]
["11174","11","11 Coal"]
["11189","11","11 Coal"]
["11214","11","11 Coal"]
["11235","11","11 Coal"]
["11253","11","11 Coal"]
["11264","11","11 Coal"]
["11285","11","11 Coal"]
["11310","11","11 Coal"]
["11319","11","11 Coal"]
["11335","11","11 Coal"]
["11360","11","11 Coal"]
["11381","11","11 Coal"]
["11404","11","11 Coal"]
["11410","11","11 Coal"]
["11431","11","11 Coal"]
["11456","11","11 Coal"]
["11464","11","11 Coal"]
["11481","11","11 Coal"]
["11506","11","11 Coal"]
["11527","11","11 Coal"]
["11549","11","11 Coal"]
["11556","11","11 Coal"]
["11577","11","11 Coal"]
["11602","11","11 Coal"]
["11609","11","11 Coal"]
["11631","11","11 Coal"]
["11652","11","11 Coal"]
["11673","11","11 Coal"]
["11694","11","11 Coal"]
["11702","11","11 Coal"]
["11723","11","11 Coal"]
["11748","11","11 Coal"]
["11754","11","11 Coal"]
["11777","11","11 Coal"]
["11798","11","11 Coal"]
["11819","11","11 Coal"]
["11839","11","11 Coal"]
["11848","11","11 Coal"]
["11869","11","11 Coal"]
["11894","11","11 Coal"]
["11899","11","11 Coal"]
["11923","11","11 Coal"]
["11944","11","11 Coal"]
["11965","11","11 Coal"]
["11984","11","11 Coal"]
["11994","11","11 Coal"]
["13019","Other","Other Commodities"]
["13040","Other","Other Commodities"]
["13063","Other","Other Commodities"]
["13069","Other","Other Commodities"]
["13090","Other","Other Commodities"]
["13111","Other","Other Commodities"]
["13129","Other","Other Commodities"]
["13140","Other","Other Commodities"]
["13165","Other","Other Commodities"]
["13186","Other","Other Commodities"]
["13208","Other","Other Commodities"]
["13215","Other","Other Commodities"]
["13236","Other","Other Commodities"]
["13257","Other","Other Commodities"]
["13274","Other","Other Commodities"]
["13286","Other","Other Commodities"]
["13311","Other","Other Commodities"]
["13332","Other","Other Commodities"]
["13353","Other","Other Commodities"]
["13361","Other","Other Commodities"]
["13382","Other","Other Commodities"]
["13407","Other","Other Commodities"]
["13419","Other","Other Commodities"]
["13432","Other","Other Commodities"]
["13457","Other","Other Commodities"]
["13478","Other","Other Commodities"]
["13498","Other","Other Commodities"]
["13507","Other","Other Commodities"]
["13528","Other","Other Commodities"]
["13553","Other","Other Commodities"]
["13564","Other","Other Commodities"]
["13578","Other","Other Commodities"]
["13603","Other","Other Commodities"]
["13624","Other","Other Commodities"]
["13630","Other","Other Commodities"]
["13653","Other","Other Commodities"]
["13674","Other","Other Commodities"]
["13699","Other","Other Commodities"]
["13709","Other","Other Commodities"]
["13724","Other","Other Commodities"]
["13749","Other","Other Commodities"]
["13770","Other","Other Commodities"]
["13775","Other","Other Commodities"]
["13799","Other","Other Commodities"]
["13820","Other","Other Commodities"]
["13845","Other","Other Commodities"]
["13854","Other","Other Commodities"]
["13870","Other","Other Commodities"]
["13895","Other","Other Commodities"]
["13916","Other","Other Commodities"]
["13939","Other","Other Commodities"]
["13945","Other","Other Commodities"]
["13966","Other","Other Commodities"]
["13991","Other","Other Commodities"]
["13999","Other","Other Commodities"]
["14020","14","14 Non-Metallic Minerals"]
["14041","14","14 Non-Metallic Minerals"]
["14062","14","14 Non-Metallic Minerals"]
["14084","14","14 Non-Metallic Minerals"]
["14091","14","14 Non-Metallic Minerals"]
["14112","14","14 Non-Metallic Minerals"]
["14137","14","14 Non-Metallic Minerals"]
["14144","14","14 Non-Metallic Minerals"]
["14166","14","14 Non-Metallic Minerals"]
["14187","14","14 Non-Metallic Minerals"]
["14208","14","14 Non-Metallic Minerals"]
["14229","14","14 Non-Metallic Minerals"]
["14237","14","14 Non-Metallic Minerals"]
["14258","14","14 Non-Metallic Minerals"]
["14283","14","14 Non-Metallic Minerals"]
["14289","14","14 Non-Metallic Minerals"]
["14312","14","14 Non-Metallic Minerals"]
["14333","14","14 Non-Metallic Minerals"]
["14354","14","14 Non-Metallic Minerals"]
["14374","14","14 Non-Metallic Minerals"]
["14383","14","14 Non-Metallic Minerals"]
["14408","14","14 Non-Metallic Minerals"]
["14429","14","14 Non-Metallic Minerals"]
["14434","14","14 Non-Metallic Minerals"]
["14458","14","14 Non-Metallic Minerals"]
["14479","14","14 Non-Metallic Minerals"]
["14500","14","14 Non-Metallic Minerals"]
["14519","14","14 Non-Metallic Minerals"]
["14529","14","14 Non-Metallic Minerals"]
["14554","14","14 Non-Metallic Minerals"]
["14561","14","14 Non-Metallic Minerals"]
["14579","14","14 Non-Metallic Minerals"]
["14604","14","14 Non-Metallic Minerals"]
["14625","14","14 Non-Metallic Minerals"]
["14646","14","14 Non-Metallic Minerals"]
["14654","14","14 Non-Metallic Minerals"]
["14675","14","14 Non-Metallic Minerals"]
["14700","14","14 Non-Metallic Minerals"]
["14706","14","14 Non-Metallic Minerals"]
["14725","14","14 Non-Metallic Minerals"]
["14750","14","14 Non-Metallic Minerals"]
["14771","14","14 Non-Metallic Minerals"]
["14791","14","14 Non-Metallic Minerals"]
["14800","14","14 Non-Metallic Minerals"]
["14821","14","14 Non-Metallic Minerals"]
["14846","14","14 Non-Metallic Minerals"]
["14870","14","14 Non-Metallic Minerals"]
["14871","14","14 Non-Metallic Minerals"]
["14896","14","14 Non-Metallic Minerals"]
["14917","14","14 Non-Metallic Minerals"]
["14936","14","14 Non-Metallic Minerals"]
["14946","14","14 Non-Metallic Minerals"]
["14967","14","14 Non-Metallic Minerals"]
["14992","14","14 Non-Metallic Minerals"]
["19015","Other","Other Commodities"]
["19021","Other","Other Commodities"]
["19042","Other","Other Commodities"]
["19063","Other","Other Commodities"]
["19081","Other","Other Commodities"]
["19092","Other","Other Commodities"]
["19113","Other","Other Commodities"]
["19138","Other","Other Commodities"]
["19160","Other","Other Commodities"]
["19167","Other","Other Commodities"]
["19188","Other","Other Commodities"]
["19209","Other","Other Commodities"]
["19226","Other","Other Commodities"]
["19238","Other","Other Commodities"]
["19263","Other","Other Commodities"]
["19284","Other","Other Commodities"]
["19305","Other","Other Commodities"]
["19313","Other","Other Commodities"]
["19334","Other","Other Commodities"]
["19355","Other","Other Commodities"]
["19371","Other","Other Commodities"]
["19384","Other","Other Commodities"]
["19409","Other","Other Commodities"]
["19430","Other","Other Commodities"]
["19450","Other","Other Commodities"]
["19459","Other","Other Commodities"]
["19480","Other","Other Commodities"]
["19501","Other","Other Commodities"]
["19516","Other","Other Commodities"]
["19530","Other","Other Commodities"]
["19555","Other","Other Commodities"]
["19576","Other","Other Commodities"]
["19595","Other","Other Commodities"]
["19605","Other","Other Commodities"]
["19626","Other","Other Commodities"]
["19651","Other","Other Commodities"]
["19661","Other","Other Commodities"]
["19676","Other","Other Commodities"]
["19701","Other","Other Commodities"]
["19722","Other","Other Commodities"]
["19740","Other","Other Commodities"]
["19751","Other","Other Commodities"]
["19772","Other","Other Commodities"]
["19797","Other","Other Commodities"]
["19806","Other","Other Commodities"]
["19822","Other","Other Commodities"]
["19847","Other","Other Commodities"]
["19868","Other","Other Commodities"]
["19885","Other","Other Commodities"]
["19897","Other","Other Commodities"]
["19918","Other","Other Commodities"]
["19943","Other","Other Commodities"]
["19951","Other","Other Commodities"]
["19968","Other","Other Commodities"]
["19993","Other","Other Commodities"]
["20014","20","20 Other Food & Kindred Products"]
["20036","20","20 Other Food & Kindred Products"]
["20043","20","20 Other Food & Kindred Products"]
["20064","20","20 Other Food & Kindred Products"]
["20089","20","20 Other Food & Kindred Products"]
["20096","20","20 Other Food & Kindred Products"]
["20114","2011","2011 Fresh Meats"]
["20139","20","20 Other Food & Kindred Products"]
["20160","20","20 Other Food & Kindred Products"]
["20181","20","20 Other Food & Kindred Products"]
["20189","20","20 Other Food & Kindred Products"]
["20210","202","202 Dairy Products"]
["20235","202","202 Dairy Products"]
["20241","202","202 Dairy Products"]
["20264","202","202 Dairy Products"]
["20285","202","202 Dairy Products"]
["20306","203","203 Canned Fruits/Vegetables"]
["20326","203","203 Canned Fruits/Vegetables"]
["20335","203","203 Canned Fruits/Vegetables"]
["20356","203","203 Canned Fruits/Vegetables"]
["20381","203","203 Canned Fruits/Vegetables"]
["20386","203","203 Canned Fruits/Vegetables"]
["20410","2041","2041 Flour"]
["20431","2043","2043 Cereal Preparations"]
["20452","2045","2045 Prepared Flour"]
["20471","204","204 Grain Mill Products"]
["20481","204","204 Grain Mill Products"]
["20502","20","20 Other Food & Kindred Products"]
["20527","20","20 Other Food & Kindred Products"]
["20531","20","20 Other Food & Kindred Products"]
["20556","20","20 Other Food & Kindred Products"]
["20577","20","20 Other Food & Kindred Products"]
["20598","20","20 Other Food & Kindred Products"]
["20616","20","20 Other Food & Kindred Products"]
["20627","2062","2062 Refined Sugar"]
["20652","20","20 Other Food & Kindred Products"]
["20673","20","20 Other Food & Kindred Products"]
["20695","20","20 Other Food & Kindred Products"]
["20702","20","20 Other Food & Kindred Products"]
["20723","20","20 Other Food & Kindred Products"]
["20744","20","20 Other Food & Kindred Products"]
["20761","20","20 Other Food & Kindred Products"]
["20773","20","20 Other Food & Kindred Products"]
["20798","20","20 Other Food & Kindred Products"]
["20819","20","20 Other Food & Kindred Products"]
["20840","2084","2084 Wines/Brandy Spirits"]
["20848","2084","2084 Wines/Brandy Spirits"]
["20869","20","20 Other Food & Kindred Products"]
["20894","20","20 Other Food & Kindred Products"]
["20906","209","209 Misc. Food Preparations"]
["20919","209","209 Misc. Food Preparations"]
["20944","209","209 Misc. Food Preparations"]
["20965","209","209 Misc. Food Preparations"]
["20985","209","209 Misc. Food Preparations"]
["20994","209","209 Misc. Food Preparations"]
["21015","21","21 Tobacco Products"]
["21040","21","21 Tobacco Products"]
["21051","21","21 Tobacco Products"]
["21065","21","21 Tobacco Products"]
["21090","21","21 Tobacco Products"]
["21111","21","21 Tobacco Products"]
["21130","21","21 Tobacco Products"]
["21140","21","21 Tobacco Products"]
["21161","21","21 Tobacco Products"]
["21186","21","21 Tobacco Products"]
["21196","21","21 Tobacco Products"]
["21211","21","21 Tobacco Products"]
["21236","21","21 Tobacco Products"]
["21257","21","21 Tobacco Products"]
["21262","21","21 Tobacco Products"]
["21286","21","21 Tobacco Products"]
["21307","21","21 Tobacco Products"]
["21332","21","21 Tobacco Products"]
["21341","21","21 Tobacco Products"]
["21357","21","21 Tobacco Products"]
["21382","21","21 Tobacco Products"]
["21403","21","21 Tobacco Products"]
["21407","21","21 Tobacco Products"]
["21432","21","21 Tobacco Products"]
["21453","21","21 Tobacco Products"]
["21478","21","21 Tobacco Products"]
["21486","21","21 Tobacco Products"]
["21503","21","21 Tobacco Products"]
["21528","21","21 Tobacco Products"]
["21549","21","21 Tobacco Products"]
["21571","21","21 Tobacco Products"]
["21578","21","21 Tobacco Products"]
["21599","21","21 Tobacco Products"]
["21624","21","21 Tobacco Products"]
["21631","21","21 Tobacco Products"]
["21653","21","21 Tobacco Products"]
["21674","21","21 Tobacco Products"]
["21695","21","21 Tobacco Products"]
["21716","21","21 Tobacco Products"]
["21724","21","21 Tobacco Products"]
["21745","21","21 Tobacco Products"]
["21770","21","21 Tobacco Products"]
["21776","21","21 Tobacco Products"]
["21799","21","21 Tobacco Products"]
["21820","21","21 Tobacco Products"]
["21841","21","21 Tobacco Products"]
["21861","21","21 Tobacco Products"]
["21870","21","21 Tobacco Products"]
["21895","21","21 Tobacco Products"]
["21916","21","21 Tobacco Products"]
["21921","21","21 Tobacco Products"]
["21945","21","21 Tobacco Products"]
["21966","21","21 Tobacco Products"]
["21987","21","21 Tobacco Products"]
["22006","Other","Other Commodities"]
["22016","Other","Other Commodities"]
["22041","Other","Other Commodities"]
["22062","Other","Other Commodities"]
["22066","Other","Other Commodities"]
["22091","Other","Other Commodities"]
["22112","Other","Other Commodities"]
["22133","Other","Other Commodities"]
["22151","Other","Other Commodities"]
["22162","Other","Other Commodities"]
["22187","Other","Other Commodities"]
["22208","Other","Other Commodities"]
["22211","Other","Other Commodities"]
["22237","Other","Other Commodities"]
["22258","Other","Other Commodities"]
["22265","Other","Other Commodities"]
["22296","Other","Other Commodities"]
["22308","Other","Other Commodities"]
["22333","Other","Other Commodities"]
["22354","Other","Other Commodities"]
["22356","Other","Other Commodities"]
["22383","Other","Other Commodities"]
["22404","Other","Other Commodities"]
["22411","Other","Other Commodities"]
["22441","Other","Other Commodities"]
["22454","Other","Other Commodities"]
["22479","Other","Other Commodities"]
["22500","Other","Other Commodities"]
["22520","Other","Other Commodities"]
["22529","Other","Other Commodities"]
["22550","Other","Other Commodities"]
["22557","Other","Other Commodities"]
["22586","Other","Other Commodities"]
["22600","Other","Other Commodities"]
["22625","Other","Other Commodities"]
["22646","Other","Other Commodities"]
["22652","Other","Other Commodities"]
["22675","Other","Other Commodities"]
["22696","Other","Other Commodities"]
["22703","Other","Other Commodities"]
["22731","Other","Other Commodities"]
["22746","Other","Other Commodities"]
["22771","Other","Other Commodities"]
["22792","Other","Other Commodities"]
["22797","Other","Other Commodities"]
["22821","Other","Other Commodities"]
["22842","Other","Other Commodities"]
["22849","Other","Other Commodities"]
["22876","Other","Other Commodities"]
["22896","Other","Other Commodities"]
["22917","Other","Other Commodities"]
["22938","Other","Other Commodities"]
["22942","Other","Other Commodities"]
["22967","Other","Other Commodities"]
["22988","Other","Other Commodities"]
["22995","Other","Other Commodities"]
["23021","Other","Other Commodities"]
["23042","Other","Other Commodities"]
["23063","Other","Other Commodities"]
["23084","Other","Other Commodities"]
["23087","Other","Other Commodities"]
["23113","Other","Other Commodities"]
["23134","Other","Other Commodities"]
["23148","Other","Other Commodities"]
["23163","Other","Other Commodities"]
["23188","Other","Other Commodities"]
["23209","Other","Other Commodities"]
["23227","Other","Other Commodities"]
["23238","Other","Other Commodities"]
["23259","Other","Other Commodities"]
["23284","Other","Other Commodities"]
["23293","Other","Other Commodities"]
["23309","Other","Other Commodities"]
["23334","Other","Other Commodities"]
["23355","Other","Other Commodities"]
["23372","Other","Other Commodities"]
["23384","Other","Other Commodities"]
["23405","Other","Other Commodities"]
["23430","Other","Other Commodities"]
["23438","Other","Other Commodities"]
["23455","Other","Other Commodities"]
["23480","Other","Other Commodities"]
["23501","Other","Other Commodities"]
["23523","Other","Other Commodities"]
["23530","Other","Other Commodities"]
["23551","Other","Other Commodities"]
["23576","Other","Other Commodities"]
["23583","Other","Other Commodities"]
["23601","Other","Other Commodities"]
["23626","Other","Other Commodities"]
["23647","Other","Other Commodities"]
["23668","Other","Other Commodities"]
["23676","Other","Other Commodities"]
["23697","Other","Other Commodities"]
["23722","Other","Other Commodities"]
["23728","Other","Other Commodities"]
["23747","Other","Other Commodities"]
["23772","Other","Other Commodities"]
["23793","Other","Other Commodities"]
["23813","Other","Other Commodities"]
["23822","Other","Other Commodities"]
["23843","Other","Other Commodities"]
["23868","Other","Other Commodities"]
["23873","Other","Other Commodities"]
["23897","Other","Other Commodities"]
["23918","Other","Other Commodities"]
["23939","Other","Other Commodities"]
["23958","Other","Other Commodities"]
["23968","Other","Other Commodities"]
["23989","Other","Other Commodities"]
["24014","24","24 Other Lumber & Wood Products"]
["24018","24","24 Other Lumber & Wood Products"]
["24043","24","24 Other Lumber & Wood Products"]
["24064","24","24 Other Lumber & Wood Products"]
["24085","24","24 Other Lumber & Wood Products"]
["24103","24","24 Other Lumber & Wood Products"]
["24114","24","24 Other Lumber & Wood Products"]
["24135","24","24 Other Lumber & Wood Products"]
["24160","24","24 Other Lumber & Wood Products"]
["24163","24","24 Other Lumber & Wood Products"]
["24189","24","24 Other Lumber & Wood Products"]
["24210","2421","2421 Lumber/Dimension Stock"]
["24231","24","24 Other Lumber & Wood Products"]
["24248","24","24 Other Lumber & Wood Products"]
["24260","24","24 Other Lumber & Wood Products"]
["24285","24","24 Other Lumber & Wood Products"]
["24306","24","24 Other Lumber & Wood Products"]
["24327","2432","2432 Plywood or Veneer"]
["24335","24","24 Other Lumber & Wood Products"]
["24356","24","24 Other Lumber & Wood Products"]
["24377","24","24 Other Lumber & Wood Products"]
["24393","24","24 Other Lumber & Wood Products"]
["24406","24","24 Other Lumber & Wood Products"]
["24431","24","24 Other Lumber & Wood Products"]
["24452","24","24 Other Lumber & Wood Products"]
["24472","24","24 Other Lumber & Wood Products"]
["24481","24","24 Other Lumber & Wood Products"]
["24502","24","24 Other Lumber & Wood Products"]
["24527","24","24 Other Lumber & Wood Products"]
["24538","24","24 Other Lumber & Wood Products"]
["24552","24","24 Other Lumber & Wood Products"]
["24577","24","24 Other Lumber & Wood Products"]
["24598","24","24 Other Lumber & Wood Products"]
["24617","24","24 Other Lumber & Wood Products"]
["24627","24","24 Other Lumber & Wood Products"]
["24648","24","24 Other Lumber & Wood Products"]
["24673","24","24 Other Lumber & Wood Products"]
["24683","24","24 Other Lumber & Wood Products"]
["24698","24","24 Other Lumber & Wood Products"]
["24723","24","24 Other Lumber & Wood Products"]
["24744","24","24 Other Lumber & Wood Products"]
["24762","24","24 Other Lumber & Wood Products"]
["24773","24","24 Other Lumber & Wood Products"]
["24794","24","24 Other Lumber & Wood Products"]
["24819","24","24 Other Lumber & Wood Products"]
["24828","24","24 Other Lumber & Wood Products"]
["24844","24","24 Other Lumber & Wood Products"]
["24869","24","24 Other Lumber & Wood Products"]
["24890","24","24 Other Lumber & Wood Products"]
["24894","24","24 Other Lumber & Wood Products"]
["24919","24","24 Other Lumber & Wood Products"]
["24940","24","24 Other Lumber & Wood Products"]
["24965","24","24 Other Lumber & Wood Products"]
["24973","24","24 Other Lumber & Wood Products"]
["24990","24","24 Other Lumber & Wood Products"]
["25015","25","25 Furniture & Fixtures"]
["25036","25","25 Furniture & Fixtures"]
["25039","25","25 Furniture & Fixtures"]
["25065","25","25 Furniture & Fixtures"]
["25086","25","25 Furniture & Fixtures"]
["25111","25","25 Furniture & Fixtures"]
["25118","25","25 Furniture & Fixtures"]
["25136","25","25 Furniture & Fixtures"]
["25161","25","25 Furniture & Fixtures"]
["25182","25","25 Furniture & Fixtures"]
["25203","25","25 Furniture & Fixtures"]
["25211","25","25 Furniture & Fixtures"]
["25232","25","25 Furniture & Fixtures"]
["25257","25","25 Furniture & Fixtures"]
["25263","25","25 Furniture & Fixtures"]
["25286","25","25 Furniture & Fixtures"]
["25307","25","25 Furniture & Fixtures"]
["25328","25","25 Furniture & Fixtures"]
["25348","25","25 Furniture & Fixtures"]
["25357","25","25 Furniture & Fixtures"]
["25378","25","25 Furniture & Fixtures"]
["25403","25","25 Furniture & Fixtures"]
["25408","25","25 Furniture & Fixtures"]
["25432","25","25 Furniture & Fixtures"]
["25453","25","25 Furniture & Fixtures"]
["25474","25","25 Furniture & Fixtures"]
["25493","25","25 Furniture & Fixtures"]
["25503","25","25 Furniture & Fixtures"]
["25528","25","25 Furniture & Fixtures"]
["25549","25","25 Furniture & Fixtures"]
["25553","25","25 Furniture & Fixtures"]
["25578","25","25 Furniture & Fixtures"]
["25599","25","25 Furniture & Fixtures"]
["25620","25","25 Furniture & Fixtures"]
["25638","25","25 Furniture & Fixtures"]
["25649","25","25 Furniture & Fixtures"]
["25674","25","25 Furniture & Fixtures"]
["25695","25","25 Furniture & Fixtures"]
["25698","25","25 Furniture & Fixtures"]
["25724","25","25 Furniture & Fixtures"]
["25745","25","25 Furniture & Fixtures"]
["25766","25","25 Furniture & Fixtures"]
["25783","25","25 Furniture & Fixtures"]
["25795","25","25 Furniture & Fixtures"]
["25820","25","25 Furniture & Fixtures"]
["25841","25","25 Furniture & Fixtures"]
["25843","25","25 Furniture & Fixtures"]
["25870","25","25 Furniture & Fixtures"]
["25891","25","25 Furniture & Fixtures"]
["25898","25","25 Furniture & Fixtures"]
["25928","25","25 Furniture & Fixtures"]
["25941","25","25 Furniture & Fixtures"]
["25966","25","25 Furniture & Fixtures"]
["25987","25","25 Furniture & Fixtures"]
["25988","25","25 Furniture & Fixtures"]
["26016","26","26 Other Paper Products"]
["26037","26","26 Other Paper Products"]
["26044","26","26 Other Paper Products"]
["26073","26","26 Other Paper Products"]
["26087","26","26 Other Paper Products"]
["26112","26","26 Other Paper Products"]
["26133","26","26 Other Paper Products"]
["26139","26","26 Other Paper Products"]
["26162","26","26 Other Paper Products"]
["26183","26","26 Other Paper Products"]
["26190","26","26 Other Paper Products"]
["26218","26","26 Other Paper Products"]
["26233","26","26 Other Paper Products"]
["26258","26","26 Other Paper Products"]
["26279","26","26 Other Paper Products"]
["26284","26","26 Other Paper Products"]
["26308","263","263 Paperboard/Fibreboard"]
["26329","263","263 Paperboard/Fibreboard"]
["26336","263","263 Paperboard/Fibreboard"]
["26363","263","263 Paperboard/Fibreboard"]
["26379","263","263 Paperboard/Fibreboard"]
["26404","264","264 Conv Paper/Paperboard"]
["26425","264","264 Conv Paper/Paperboard"]
["26429","264","264 Conv Paper/Paperboard"]
["26454","264","264 Conv Paper/Paperboard"]
["26475","264","264 Conv Paper/Paperboard"]
["26482","264","264 Conv Paper/Paperboard"]
["26508","26","26 Other Paper Products"]
["26529","26","26 Other Paper Products"]
["26550","26","26 Other Paper Products"]
["26571","26","26 Other Paper Products"]
["26574","26","26 Other Paper Products"]
["26600","26","26 Other Paper Products"]
["26621","26","26 Other Paper Products"]
["26628","26","26 Other Paper Products"]
["26653","26","26 Other Paper Products"]
["26675","26","26 Other Paper Products"]
["26696","26","26 Other Paper Products"]
["26717","26","26 Other Paper Products"]
["26719","26","26 Other Paper Products"]
["26746","26","26 Other Paper Products"]
["26767","26","26 Other Paper Products"]
["26774","26","26 Other Paper Products"]
["26798","26","26 Other Paper Products"]
["26821","26","26 Other Paper Products"]
["26842","26","26 Other Paper Products"]
["26863","26","26 Other Paper Products"]
["26864","26","26 Other Paper Products"]
["26892","26","26 Other Paper Products"]
["26917","26","26 Other Paper Products"]
["26920","26","26 Other Paper Products"]
["26943","26","26 Other Paper Products"]
["26967","26","26 Other Paper Products"]
["26988","26","26 Other Paper Products"]
["27009","Other","Other Commodities"]
["27028","Other","Other Commodities"]
["27038","Other","Other Commodities"]
["27063","Other","Other Commodities"]
["27066","Other","Other Commodities"]
["27088","Other","Other Commodities"]
["27113","Other","Other Commodities"]
["27134","Other","Other Commodities"]
["27141","Other","Other Commodities"]
["27173","Other","Other Commodities"]
["27184","Other","Other Commodities"]
["27209","Other","Other Commodities"]
["27212","Other","Other Commodities"]
["27233","Other","Other Commodities"]
["27259","Other","Other Commodities"]
["27280","Other","Other Commodities"]
["27287","Other","Other Commodities"]
["27318","Other","Other Commodities"]
["27330","Other","Other Commodities"]
["27355","Other","Other Commodities"]
["27358","Other","Other Commodities"]
["27378","Other","Other Commodities"]
["27405","Other","Other Commodities"]
["27426","Other","Other Commodities"]
["27433","Other","Other Commodities"]
["27463","Other","Other Commodities"]
["27476","Other","Other Commodities"]
["27501","Other","Other Commodities"]
["27504","Other","Other Commodities"]
["27529","Other","Other Commodities"]
["27551","Other","Other Commodities"]
["27572","Other","Other Commodities"]
["27579","Other","Other Commodities"]
["27608","Other","Other Commodities"]
["27622","Other","Other Commodities"]
["27647","Other","Other Commodities"]
["27650","Other","Other Commodities"]
["27674","Other","Other Commodities"]
["27697","Other","Other Commodities"]
["27718","Other","Other Commodities"]
["27735","Other","Other Commodities"]
["27747","Other","Other Commodities"]
["27772","Other","Other Commodities"]
["27793","Other","Other Commodities"]
["27795","Other","Other Commodities"]
["27822","Other","Other Commodities"]
["27843","Other","Other Commodities"]
["27864","Other","Other Commodities"]
["27880","Other","Other Commodities"]
["27893","Other","Other Commodities"]
["27918","Other","Other Commodities"]
["27939","Other","Other Commodities"]
["27959","Other","Other Commodities"]
["27968","Other","Other Commodities"]
["27989","Other","Other Commodities"]
["28010","28","28 Other Chemicals"]
["28025","28","28 Other Chemicals"]
["28039","28","28 Other Chemicals"]
["28064","28","28 Other Chemicals"]
["28085","28","28 Other Chemicals"]
["28104","281","281 Industrial Chemicals"]
["28114","281","281 Industrial Chemicals"]
["28135","281","281 Industrial Chemicals"]
["28142","281","281 Industrial Chemicals"]
["28170","281","281 Industrial Chemicals"]
["28185","281","281 Industrial Chemicals"]
["28210","282","282 Syn Fibers/Resins/Rubber"]
["28231","282","282 Syn Fibers/Resins/Rubber"]
["28249","282","282 Syn Fibers/Resins/Rubber"]
["28260","282","282 Syn Fibers/Resins/Rubber"]
["28281","282","282 Syn Fibers/Resins/Rubber"]
["28288","282","282 Syn Fibers/Resins/Rubber"]
["28315","28","28 Other Chemicals"]
["28331","28","28 Other Chemicals"]
["28356","28","28 Other Chemicals"]
["28377","28","28 Other Chemicals"]
["28394","28","28 Other Chemicals"]
["28406","28","28 Other Chemicals"]
["28427","28","28 Other Chemicals"]
["28434","28","28 Other Chemicals"]
["28460","28","28 Other Chemicals"]
["28477","28","28 Other Chemicals"]
["28502","28","28 Other Chemicals"]
["28523","28","28 Other Chemicals"]
["28526","28","28 Other Chemicals"]
["28552","28","28 Other Chemicals"]
["28573","28","28 Other Chemicals"]
["28580","28","28 Other Chemicals"]
["28605","28","28 Other Chemicals"]
["28623","28","28 Other Chemicals"]
["28648","28","28 Other Chemicals"]
["28669","28","28 Other Chemicals"]
["28671","28","28 Other Chemicals"]
["28698","28","28 Other Chemicals"]
["28719","28","28 Other Chemicals"]
["28726","28","28 Other Chemicals"]
["28750","28","28 Other Chemicals"]
["28773","28","28 Other Chemicals"]
["28794","28","28 Other Chemicals"]
["28815","28","28 Other Chemicals"]
["28835","28","28 Other Chemicals"]
["28844","28","28 Other Chemicals"]
["28865","28","28 Other Chemicals"]
["28872","28","28 Other Chemicals"]
["28895","28","28 Other Chemicals"]
["28919","289","289 Misc Chemical Products"]
["28940","289","289 Misc Chemical Products"]
["28961","289","289 Misc Chemical Products"]
["28980","289","289 Misc Chemical Products"]
["28990","289","289 Misc Chemical Products"]
["29011","29","29 Petroleum or Coal Products"]
["29018","29","29 Petroleum or Coal Products"]
["29040","29","29 Petroleum or Coal Products"]
["29065","29","29 Petroleum or Coal Products"]
["29086","29","29 Petroleum or Coal Products"]
["29107","29","29 Petroleum or Coal Products"]
["29125","29","29 Petroleum or Coal Products"]
["29136","29","29 Petroleum or Coal Products"]
["29161","29","29 Petroleum or Coal Products"]
["29164","29","29 Petroleum or Coal Products"]
["29185","29","29 Petroleum or Coal Products"]
["29211","29","29 Petroleum or Coal Products"]
["29232","29","29 Petroleum or Coal Products"]
["29253","29","29 Petroleum or Coal Products"]
["29270","29","29 Petroleum or Coal Products"]
["29282","29","29 Petroleum or Coal Products"]
["29307","29","29 Petroleum or Coal Products"]
["29310","29","29 Petroleum or Coal Products"]
["29330","29","29 Petroleum or Coal Products"]
["29357","29","29 Petroleum or Coal Products"]
["29378","29","29 Petroleum or Coal Products"]
["29399","29","29 Petroleum or Coal Products"]
["29415","29","29 Petroleum or Coal Products"]
["29428","29","29 Petroleum or Coal Products"]
["29453","29","29 Petroleum or Coal Products"]
["29456","29","29 Petroleum or Coal Products"]
["29475","29","29 Petroleum or Coal Products"]
["29503","29","29 Petroleum or Coal Products"]
["29524","29","29 Petroleum or Coal Products"]
["29531","29","29 Petroleum or Coal Products"]
["29560","29","29 Petroleum or Coal Products"]
["29574","29","29 Petroleum or Coal Products"]
["29599","29","29 Petroleum or Coal Products"]
["29602","29","29 Petroleum or Coal Products"]
["29620","29","29 Petroleum or Coal Products"]
["29649","29","29 Petroleum or Coal Products"]
["29670","29","29 Petroleum or Coal Products"]
["29677","29","29 Petroleum or Coal Products"]
["29705","29","29 Petroleum or Coal Products"]
["29720","29","29 Petroleum or Coal Products"]
["29745","29","29 Petroleum or Coal Products"]
["29748","29","29 Petroleum or Coal Products"]
["29771","29","29 Petroleum or Coal Products"]
["29795","29","29 Petroleum or Coal Products"]
["29816","29","29 Petroleum or Coal Products"]
["29823","29","29 Petroleum or Coal Products"]
["29850","29","29 Petroleum or Coal Products"]
["29866","29","29 Petroleum or Coal Products"]
["29891","29","29 Petroleum or Coal Products"]
["29894","29","29 Petroleum or Coal Products"]
["29916","29","29 Petroleum or Coal Products"]
["29941","29","29 Petroleum or Coal Products"]
["29962","29","29 Petroleum or Coal Products"]
["29969","29","29 Petroleum or Coal Products"]
["29995","29","29 Petroleum or Coal Products"]
["30012","30","30 Other Rubber Products"]
["30037","30","30 Other Rubber Products"]
["30040","30","30 Other Rubber Products"]
["30061","30","30 Other Rubber Products"]
["30087","30","30 Other Rubber Products"]
["30108","301","301 Rubber Tires/Innertubes"]
["30115","301","301 Rubber Tires/Innertubes"]
["30140","301","301 Rubber Tires/Innertubes"]
["30162","301","301 Rubber Tires/Innertubes"]
["30183","301","301 Rubber Tires/Innertubes"]
["30186","301","301 Rubber Tires/Innertubes"]
["30206","30","30 Other Rubber Products"]
["30233","30","30 Other Rubber Products"]
["30254","30","30 Other Rubber Products"]
["30261","30","30 Other Rubber Products"]
["30285","30","30 Other Rubber Products"]
["30308","30","30 Other Rubber Products"]
["30329","30","30 Other Rubber Products"]
["30332","30","30 Other Rubber Products"]
["30351","30","30 Other Rubber Products"]
["30379","30","30 Other Rubber Products"]
["30404","30","30 Other Rubber Products"]
["30407","30","30 Other Rubber Products"]
["30430","30","30 Other Rubber Products"]
["30454","30","30 Other Rubber Products"]
["30475","30","30 Other Rubber Products"]
["30478","30","30 Other Rubber Products"]
["30496","30","30 Other Rubber Products"]
["30525","30","30 Other Rubber Products"]
["30550","30","30 Other Rubber Products"]
["30553","30","30 Other Rubber Products"]
["30575","30","30 Other Rubber Products"]
["30600","30","30 Other Rubber Products"]
["30621","30","30 Other Rubber Products"]
["30624","30","30 Other Rubber Products"]
["30660","30","30 Other Rubber Products"]
["30671","30","30 Other Rubber Products"]
["30696","30","30 Other Rubber Products"]
["30699","30","30 Other Rubber Products"]
["30720","30","30 Other Rubber Products"]
["30746","30","30 Other Rubber Products"]
["30767","30","30 Other Rubber Products"]
["30774","30","30 Other Rubber Products"]
["30805","30","30 Other Rubber Products"]
["30817","30","30 Other Rubber Products"]
["30842","30","30 Other Rubber Products"]
["30845","30","30 Other Rubber Products"]
["30865","30","30 Other Rubber Products"]
["30892","30","30 Other Rubber Products"]
["30913","30","30 Other Rubber Products"]
["30920","30","30 Other Rubber Products"]
["30950","30","30 Other Rubber Products"]
["30963","30","30 Other Rubber Products"]
["30988","30","30 Other Rubber Products"]
["30991","30","30 Other Rubber Products"]
["31010","Other","Other Commodities"]
["31038","Other","Other Commodities"]
["31059","Other","Other Commodities"]
["31066","Other","Other Commodities"]
["31095","Other","Other Commodities"]
["31109","Other","Other Commodities"]
["31134","Other","Other Commodities"]
["31137","Other","Other Commodities"]
["31161","Other","Other Commodities"]
["31184","Other","Other Commodities"]
["31205","Other","Other Commodities"]
["31212","Other","Other Commodities"]
["31240","Other","Other Commodities"]
["31255","Other","Other Commodities"]
["31280","Other","Other Commodities"]
["31283","Other","Other Commodities"]
["31306","Other","Other Commodities"]
["31330","Other","Other Commodities"]
["31351","Other","Other Commodities"]
["31358","Other","Other Commodities"]
["31385","Other","Other Commodities"]
["31405","Other","Other Commodities"]
["31426","Other","Other Commodities"]
["31429","Other","Other Commodities"]
["31451","Other","Other Commodities"]
["31476","Other","Other Commodities"]
["31497","Other","Other Commodities"]
["31504","Other","Other Commodities"]
["31530","Other","Other Commodities"]
["31551","Other","Other Commodities"]
["31572","Other","Other Commodities"]
["31575","Other","Other Commodities"]
["31596","Other","Other Commodities"]
["31622","Other","Other Commodities"]
["31643","Other","Other Commodities"]
["31650","Other","Other Commodities"]
["31675","Other","Other Commodities"]
["31697","Other","Other Commodities"]
["31718","Other","Other Commodities"]
["31721","Other","Other Commodities"]
["31741","Other","Other Commodities"]
["31768","Other","Other Commodities"]
["31775","Other","Other Commodities"]
["31796","Other","Other Commodities"]
["31820","Other","Other Commodities"]
["31843","Other","Other Commodities"]
["31864","Other","Other Commodities"]
["31867","Other","Other Commodities"]
["31886","Other","Other Commodities"]
["31914","Other","Other Commodities"]
["31921","Other","Other Commodities"]
["31942","Other","Other Commodities"]
["31965","Other","Other Commodities"]
["31989","Other","Other Commodities"]
["32010","32","32 Other Stone Products"]
["32017","32","32 Other Stone Products"]
["32031","32","32 Other Stone Products"]
["32060","32","32 Other Stone Products"]
["32067","32","32 Other Stone Products"]
["32088","32","32 Other Stone Products"]
["32110","321","321 Flat Glass"]
["32135","321","321 Flat Glass"]
["32156","321","321 Flat Glass"]
["32163","321","321 Flat Glass"]
["32176","321","321 Flat Glass"]
["32206","32","32 Other Stone Products"]
["32213","32","32 Other Stone Products"]
["32237","32","32 Other Stone Products"]
["32256","32","32 Other Stone Products"]
["32281","32","32 Other Stone Products"]
["32302","32","32 Other Stone Products"]
["32303","32","32 Other Stone Products"]
["32331","32","32 Other Stone Products"]
["32352","32","32 Other Stone Products"]
["32359","32","32 Other Stone Products"]
["32382","32","32 Other Stone Products"]
["32406","32","32 Other Stone Products"]
["32427","32","32 Other Stone Products"]
["32448","32","32 Other Stone Products"]
["32467","32","32 Other Stone Products"]
["32477","32","32 Other Stone Products"]
["32498","32","32 Other Stone Products"]
["32505","32","32 Other Stone Products"]
["32527","32","32 Other Stone Products"]
["32552","32","32 Other Stone Products"]
["32573","32","32 Other Stone Products"]
["32594","32","32 Other Stone Products"]
["32612","32","32 Other Stone Products"]
["32623","32","32 Other Stone Products"]
["32644","32","32 Other Stone Products"]
["32651","32","32 Other Stone Products"]
["32672","32","32 Other Stone Products"]
["32698","32","32 Other Stone Products"]
["32719","32","32 Other Stone Products"]
["32740","32","32 Other Stone Products"]
["32757","32","32 Other Stone Products"]
["32769","32","32 Other Stone Products"]
["32794","32","32 Other Stone Products"]
["32797","32","32 Other Stone Products"]
["32817","32","32 Other Stone Products"]
["32844","32","32 Other Stone Products"]
["32865","32","32 Other Stone Products"]
["32886","32","32 Other Stone Products"]
["32902","32","32 Other Stone Products"]
["32915","32","32 Other Stone Products"]
["32940","32","32 Other Stone Products"]
["32943","32","32 Other Stone Products"]
["32962","32","32 Other Stone Products"]
["32990","32","32 Other Stone Products"]
["33011","33","33 Other Primary Metal Products"]
["33018","33","33 Other Primary Metal Products"]
["33047","33","33 Other Primary Metal Products"]
["33061","33","33 Other Primary Metal Products"]
["33086","33","33 Other Primary Metal Products"]
["33089","33","33 Other Primary Metal Products"]
["33107","33","33 Other Primary Metal Products"]
["33136","33","33 Other Primary Metal Products"]
["33157","33","33 Other Primary Metal Products"]
["33164","33","33 Other Primary Metal Products"]
["33192","33","33 Other Primary Metal Products"]
["33207","33","33 Other Primary Metal Products"]
["33232","33","33 Other Primary Metal Products"]
["33235","33","33 Other Primary Metal Products"]
["33252","33","33 Other Primary Metal Products"]
["33282","33","33 Other Primary Metal Products"]
["33303","33","33 Other Primary Metal Products"]
["33310","33","33 Other Primary Metal Products"]
["33337","33","33 Other Primary Metal Products"]
["33353","33","33 Other Primary Metal Products"]
["33378","33","33 Other Primary Metal Products"]
["33381","33","33 Other Primary Metal Products"]
["33403","33","33 Other Primary Metal Products"]
["33428","33","33 Other Primary Metal Products"]
["33449","33","33 Other Primary Metal Products"]
["33456","33","33 Other Primary Metal Products"]
["33482","33","33 Other Primary Metal Products"]
["33499","33","33 Other Primary Metal Products"]
["33524","3352","3352 Aluminum Shapes"]
["33527","3352","3352 Aluminum Shapes"]
["33548","33","33 Other Primary Metal Products"]
["33574","33","33 Other Primary Metal Products"]
["33595","33","33 Other Primary Metal Products"]
["33602","33","33 Other Primary Metal Products"]
["33627","33","33 Other Primary Metal Products"]
["33645","33","33 Other Primary Metal Products"]
["33670","33","33 Other Primary Metal Products"]
["33673","33","33 Other Primary Metal Products"]
["33693","33","33 Other Primary Metal Products"]
["33720","33","33 Other Primary Metal Products"]
["33741","33","33 Other Primary Metal Products"]
["33748","33","33 Other Primary Metal Products"]
["33772","33","33 Other Primary Metal Products"]
["33795","33","33 Other Primary Metal Products"]
["33816","33","33 Other Primary Metal Products"]
["33819","33","33 Other Primary Metal Products"]
["33838","33","33 Other Primary Metal Products"]
["33866","33","33 Other Primary Metal Products"]
["33887","33","33 Other Primary Metal Products"]
["33894","33","33 Other Primary Metal Products"]
["33917","33","33 Other Primary Metal Products"]
["33941","33","33 Other Primary Metal Products"]
["33962","33","33 Other Primary Metal Products"]
["33965","33","33 Other Primary Metal Products"]
["33983","33","33 Other Primary Metal Products"]
["34012","34","34 Other Fab. Metal Products"]
["34019","34","34 Other Fab. Metal Products"]
["34040","34","34 Other Fab. Metal Products"]
["34062","34","34 Other Fab. Metal Products"]
["34087","34","34 Other Fab. Metal Products"]
["34108","34","34 Other Fab. Metal Products"]
["34111","34","34 Other Fab. Metal Products"]
["34128","34","34 Other Fab. Metal Products"]
["34158","34","34 Other Fab. Metal Products"]
["34165","34","34 Other Fab. Metal Products"]
["34186","34","34 Other Fab. Metal Products"]
["34207","34","34 Other Fab. Metal Products"]
["34233","34","34 Other Fab. Metal Products"]
["34254","34","34 Other Fab. Metal Products"]
["34257","34","34 Other Fab. Metal Products"]
["34292","34","34 Other Fab. Metal Products"]
["34304","34","34 Other Fab. Metal Products"]
["34311","34","34 Other Fab. Metal Products"]
["34332","34","34 Other Fab. Metal Products"]
["34352","34","34 Other Fab. Metal Products"]
["34379","34","34 Other Fab. Metal Products"]
["34400","344","344 Fabric. Structural Metal"]
["34407","344","344 Fabric. Structural Metal"]
["34437","344","344 Fabric. Structural Metal"]
["34450","344","344 Fabric. Structural Metal"]
["34457","344","344 Fabric. Structural Metal"]
["34478","344","344 Fabric. Structural Metal"]
["34497","344","344 Fabric. Structural Metal"]
["34525","34","34 Other Fab. Metal Products"]
["34546","34","34 Other Fab. Metal Products"]
["34553","34","34 Other Fab. Metal Products"]
["34582","34","34 Other Fab. Metal Products"]
["34596","34","34 Other Fab. Metal Products"]
["34603","34","34 Other Fab. Metal Products"]
["34624","34","34 Other Fab. Metal Products"]
["34648","34","34 Other Fab. Metal Products"]
["34671","34","34 Other Fab. Metal Products"]
["34692","34","34 Other Fab. Metal Products"]
["34699","34","34 Other Fab. Metal Products"]
["34727","34","34 Other Fab. Metal Products"]
["34742","34","34 Other Fab. Metal Products"]
["34749","34","34 Other Fab. Metal Products"]
["34770","34","34 Other Fab. Metal Products"]
["34793","34","34 Other Fab. Metal Products"]
["34817","34","34 Other Fab. Metal Products"]
["34838","34","34 Other Fab. Metal Products"]
["34845","34","34 Other Fab. Metal Products"]
["34872","34","34 Other Fab. Metal Products"]
["34888","34","34 Other Fab. Metal Products"]
["34895","34","34 Other Fab. Metal Products"]
["34916","34","34 Other Fab. Metal Products"]
["34938","34","34 Other Fab. Metal Products"]
["34963","34","34 Other Fab. Metal Products"]
["34984","34","34 Other Fab. Metal Products"]
["34991","34","34 Other Fab. Metal Products"]
["35017","35","35 Other Non-Elec. Machinery"]
["35038","35","35 Other Non-Elec. Machinery"]
["35041","35","35 Other Non-Elec. Machinery"]
["35062","35","35 Other Non-Elec. Machinery"]
["35083","35","35 Other Non-Elec. Machinery"]
["35109","351","351 Engines/Turbines"]
["35130","351","351 Engines/Turbines"]
["35137","351","351 Engines/Turbines"]
["35162","351","351 Engines/Turbines"]
["35184","351","351 Engines/Turbines"]
["35187","351","351 Engines/Turbines"]
["35208","352","352 Farm Machinery"]
["35228","352","352 Farm Machinery"]
["35255","352","352 Farm Machinery"]
["35276","352","352 Farm Machinery"]
["35283","352","352 Farm Machinery"]
["35307","353","353 Constr./Mining/Hand Machinery"]
["35330","353","353 Constr./Mining/Hand Machinery"]
["35333","353","353 Constr./Mining/Hand Machinery"]
["35354","353","353 Constr./Mining/Hand Machinery"]
["35373","353","353 Constr./Mining/Hand Machinery"]
["35401","35","35 Other Non-Elec. Machinery"]
["35408","35","35 Other Non-Elec. Machinery"]
["35429","35","35 Other Non-Elec. Machinery"]
["35452","35","35 Other Non-Elec. Machinery"]
["35476","35","35 Other Non-Elec. Machinery"]
["35479","35","35 Other Non-Elec. Machinery"]
["35500","35","35 Other Non-Elec. Machinery"]
["35518","35","35 Other Non-Elec. Machinery"]
["35547","35","35 Other Non-Elec. Machinery"]
["35554","35","35 Other Non-Elec. Machinery"]
["35575","35","35 Other Non-Elec. Machinery"]
["35597","35","35 Other Non-Elec. Machinery"]
["35622","35","35 Other Non-Elec. Machinery"]
["35625","35","35 Other Non-Elec. Machinery"]
["35650","35","35 Other Non-Elec. Machinery"]
["35663","35","35 Other Non-Elec. Machinery"]
["35693","35","35 Other Non-Elec. Machinery"]
["35700","35","35 Other Non-Elec. Machinery"]
["35721","35","35 Other Non-Elec. Machinery"]
["35742","35","35 Other Non-Elec. Machinery"]
["35768","35","35 Other Non-Elec. Machinery"]
["35771","35","35 Other Non-Elec. Machinery"]
["35796","35","35 Other Non-Elec. Machinery"]
["35808","35","35 Other Non-Elec. Machinery"]
["35839","35","35 Other Non-Elec. Machinery"]
["35846","35","35 Other Non-Elec. Machinery"]
["35867","35","35 Other Non-Elec. Machinery"]
["35887","35","35 Other Non-Elec. Machinery"]
["35914","35","35 Other Non-Elec. Machinery"]
["35917","35","35 Other Non-Elec. Machinery"]
["35942","35","35 Other Non-Elec. Machinery"]
["35953","35","35 Other Non-Elec. Machinery"]
["35985","35","35 Other Non-Elec. Machinery"]
["35992","35","35 Other Non-Elec. Machinery"]
["36013","36","36 Other Electrical Machinery"]
["36038","36","36 Other Electrical Machinery"]
["36060","36","36 Other Electrical Machinery"]
["36063","36","36 Other Electrical Machinery"]
["36088","36","36 Other Electrical Machinery"]
["36117","361","361 Electrical Trans Equipment"]
["36131","361","361 Electrical Trans Equipment"]
["36138","361","361 Electrical Trans Equipment"]
["36159","361","361 Electrical Trans Equipment"]
["36183","361","361 Electrical Trans Equipment"]
["36206","36","36 Other Electrical Machinery"]
["36209","36","36 Other Electrical Machinery"]
["36234","36","36 Other Electrical Machinery"]
["36262","36","36 Other Electrical Machinery"]
["36277","36","36 Other Electrical Machinery"]
["36284","36","36 Other Electrical Machinery"]
["36305","363","363 Household Appliances"]
["36328","363","363 Household Appliances"]
["36352","363","363 Household Appliances"]
["36355","363","363 Household Appliances"]
["36380","363","363 Household Appliances"]
["36407","36","36 Other Electrical Machinery"]
["36427","36","36 Other Electrical Machinery"]
["36430","36","36 Other Electrical Machinery"]
["36451","36","36 Other Electrical Machinery"]
["36473","36","36 Other Electrical Machinery"]
["36498","36","36 Other Electrical Machinery"]
["36501","365","365 Radio or TV Sets"]
["36526","365","365 Radio or TV Sets"]
["36552","365","365 Radio or TV Sets"]
["36573","365","365 Radio or TV Sets"]
["36576","365","365 Radio or TV Sets"]
["36597","365","365 Radio or TV Sets"]
["36618","36","36 Other Electrical Machinery"]
["36644","36","36 Other Electrical Machinery"]
["36651","36","36 Other Electrical Machinery"]
["36672","36","36 Other Electrical Machinery"]
["36697","36","36 Other Electrical Machinery"]
["36719","36","36 Other Electrical Machinery"]
["36722","36","36 Other Electrical Machinery"]
["36743","36","36 Other Electrical Machinery"]
["36763","36","36 Other Electrical Machinery"]
["36790","36","36 Other Electrical Machinery"]
["36797","36","36 Other Electrical Machinery"]
["36824","36","36 Other Electrical Machinery"]
["36840","36","36 Other Electrical Machinery"]
["36865","36","36 Other Electrical Machinery"]
["36868","36","36 Other Electrical Machinery"]
["36884","36","36 Other Electrical Machinery"]
["36915","36","36 Other Electrical Machinery"]
["36936","36","36 Other Electrical Machinery"]
["36943","36","36 Other Electrical Machinery"]
["36969","36","36 Other Electrical Machinery"]
["36986","36","36 Other Electrical Machinery"]
["37011","37","37 Other Trans. Equipment"]
["37014","37","37 Other Trans. Equipment"]
["37035","37","37 Other Trans. Equipment"]
["37061","37","37 Other Trans. Equipment"]
["37082","37","37 Other Trans. Equipment"]
["37089","37","37 Other Trans. Equipment"]
["37114","37","37 Other Trans. Equipment"]
["37132","37","37 Other Trans. Equipment"]
["37157","37","37 Other Trans. Equipment"]
["37160","37","37 Other Trans. Equipment"]
["37180","37","37 Other Trans. Equipment"]
["37207","37","37 Other Trans. Equipment"]
["37228","37","37 Other Trans. Equipment"]
["37235","37","37 Other Trans. Equipment"]
["37259","37","37 Other Trans. Equipment"]
["37282","37","37 Other Trans. Equipment"]
["37303","37","37 Other Trans. Equipment"]
["37306","37","37 Other Trans. Equipment"]
["37325","37","37 Other Trans. Equipment"]
["37353","37","37 Other Trans. Equipment"]
["37374","37","37 Other Trans. Equipment"]
["37381","37","37 Other Trans. Equipment"]
["37404","37","37 Other Trans. Equipment"]
["37428","37","37 Other Trans. Equipment"]
["37449","37","37 Other Trans. Equipment"]
["37452","37","37 Other Trans. Equipment"]
["37470","37","37 Other Trans. Equipment"]
["37499","37","37 Other Trans. Equipment"]
["37520","37","37 Other Trans. Equipment"]
["37527","37","37 Other Trans. Equipment"]
["37549","37","37 Other Trans. Equipment"]
["37574","37","37 Other Trans. Equipment"]
["37595","37","37 Other Trans. Equipment"]
["37598","37","37 Other Trans. Equipment"]
["37615","37","37 Other Trans. Equipment"]
["37645","37","37 Other Trans. Equipment"]
["37652","37","37 Other Trans. Equipment"]
["37673","37","37 Other Trans. Equipment"]
["37694","37","37 Other Trans. Equipment"]
["37720","37","37 Other Trans. Equipment"]
["37741","37","37 Other Trans. Equipment"]
["37744","37","37 Other Trans. Equipment"]
["37760","37","37 Other Trans. Equipment"]
["37791","37","37 Other Trans. Equipment"]
["37798","37","37 Other Trans. Equipment"]
["37819","37","37 Other Trans. Equipment"]
["37839","37","37 Other Trans. Equipment"]
["37866","37","37 Other Trans. Equipment"]
["37887","37","37 Other Trans. Equipment"]
["37890","37","37 Other Trans. Equipment"]
["37924","37","37 Other Trans. Equipment"]
["37937","37","37 Other Trans. Equipment"]
["37944","37","37 Other Trans. Equipment"]
["37965","37","37 Other Trans. Equipment"]
["37984","37","37 Other Trans. Equipment"]
["38012","Other","Other Commodities"]
["38033","Other","Other Commodities"]
["38040","Other","Other Commodities"]
["38069","Other","Other Commodities"]
["38083","Other","Other Commodities"]
["38090","Other","Other Commodities"]
["38111","Other","Other Commodities"]
["38129","Other","Other Commodities"]
["38158","Other","Other Commodities"]
["38179","Other","Other Commodities"]
["38186","Other","Other Commodities"]
["38214","Other","Other Commodities"]
["38229","Other","Other Commodities"]
["38236","Other","Other Commodities"]
["38257","Other","Other Commodities"]
["38280","Other","Other Commodities"]
["38304","Other","Other Commodities"]
["38325","Other","Other Commodities"]
["38332","Other","Other Commodities"]
["38359","Other","Other Commodities"]
["38375","Other","Other Commodities"]
["38382","Other","Other Commodities"]
["38403","Other","Other Commodities"]
["38425","Other","Other Commodities"]
["38450","Other","Other Commodities"]
["38471","Other","Other Commodities"]
["38478","Other","Other Commodities"]
["38504","Other","Other Commodities"]
["38521","Other","Other Commodities"]
["38528","Other","Other Commodities"]
["38549","Other","Other Commodities"]
["38570","Other","Other Commodities"]
["38596","Other","Other Commodities"]
["38617","Other","Other Commodities"]
["38624","Other","Other Commodities"]
["38649","Other","Other Commodities"]
["38671","Other","Other Commodities"]
["38674","Other","Other Commodities"]
["38695","Other","Other Commodities"]
["38715","Other","Other Commodities"]
["38742","Other","Other Commodities"]
["38763","Other","Other Commodities"]
["38770","Other","Other Commodities"]
["38794","Other","Other Commodities"]
["38817","Other","Other Commodities"]
["38820","Other","Other Commodities"]
["38841","Other","Other Commodities"]
["38860","Other","Other Commodities"]
["38888","Other","Other Commodities"]
["38895","Other","Other Commodities"]
["38916","Other","Other Commodities"]
["38939","Other","Other Commodities"]
["38963","Other","Other Commodities"]
["38966","Other","Other Commodities"]
["38987","Other","Other Commodities"]
["39005","Other","Other Commodities"]
["39034","Other","Other Commodities"]
["39041","Other","Other Commodities"]
["39062","Other","Other Commodities"]
["39084","Other","Other Commodities"]
["39109","Other","Other Commodities"]
["39112","Other","Other Commodities"]
["39133","Other","Other Commodities"]
["39150","Other","Other Commodities"]
["39180","Other","Other Commodities"]
["39187","Other","Other Commodities"]
["39208","Other","Other Commodities"]
["39229","Other","Other Commodities"]
["39255","Other","Other Commodities"]
["39258","Other","Other Commodities"]
["39283","Other","Other Commodities"]
["39295","Other","Other Commodities"]
["39326","Other","Other Commodities"]
["39333","Other","Other Commodities"]
["39354","Other","Other Commodities"]
["39374","Other","Other Commodities"]
["39401","Other","Other Commodities"]
["39404","Other","Other Commodities"]
["39429","Other","Other Commodities"]
["39440","Other","Other Commodities"]
["39472","Other","Other Commodities"]
["39479","Other","Other Commodities"]
["39500","Other","Other Commodities"]
["39519","Other","Other Commodities"]
["39547","Other","Other Commodities"]
["39550","Other","Other Commodities"]
["39575","Other","Other Commodities"]
["39585","Other","Other Commodities"]
["39618","Other","Other Commodities"]
["39625","Other","Other Commodities"]
["39646","Other","Other Commodities"]
["39670","Other","Other Commodities"]
["39693","Other","Other Commodities"]
["39696","Other","Other Commodities"]
["39721","Other","Other Commodities"]
["39749","Other","Other Commodities"]
["39764","Other","Other Commodities"]
["39771","Other","Other Commodities"]
["39792","Other","Other Commodities"]
["39815","Other","Other Commodities"]
["39839","Other","Other Commodities"]
["39842","Other","Other Commodities"]
["39867","Other","Other Commodities"]
["39894","Other","Other Commodities"]
["39896","Other","Other Commodities"]
["39917","Other","Other Commodities"]
["39938","Other","Other Commodities"]
["39960","Other","Other Commodities"]
["39985","Other","Other Commodities"]
["39988","Other","Other Commodities"]
["40013","Other","Other Commodities"]
["40039","Other","Other Commodities"]
["40042","Other","Other Commodities"]
["40063","Other","Other Commodities"]
["40084","Other","Other Commodities"]
["40105","Other","Other Commodities"]
["40131","Other","Other Commodities"]
["40134","Other","Other Commodities"]
["40159","Other","Other Commodities"]
["40184","Other","Other Commodities"]
["40188","Other","Other Commodities"]
["40209","Other","Other Commodities"]
["40230","Other","Other Commodities"]
["40250","Other","Other Commodities"]
["40277","Other","Other Commodities"]
["40284","Other","Other Commodities"]
["40305","Other","Other Commodities"]
["40329","Other","Other Commodities"]
["40334","Other","Other Commodities"]
["40355","Other","Other Commodities"]
["40376","Other","Other Commodities"]
["40395","Other","Other Commodities"]
["40423","Other","Other Commodities"]
["40430","Other","Other Commodities"]
["40451","Other","Other Commodities"]
["40474","Other","Other Commodities"]
["40480","Other","Other Commodities"]
["40501","Other","Other Commodities"]
["40522","Other","Other Commodities"]
["40540","Other","Other Commodities"]
["40569","Other","Other Commodities"]
["40576","Other","Other Commodities"]
["40597","Other","Other Commodities"]
["40619","Other","Other Commodities"]
["40626","Other","Other Commodities"]
["40647","Other","Other Commodities"]
["40672","Other","Other Commodities"]
["40685","Other","Other Commodities"]
["40715","Other","Other Commodities"]
["40722","Other","Other Commodities"]
["40743","Other","Other Commodities"]
["40764","Other","Other Commodities"]
["40772","Other","Other Commodities"]
["40793","Other","Other Commodities"]
["40818","Other","Other Commodities"]
["40830","Other","Other Commodities"]
["40861","Other","Other Commodities"]
["40868","Other","Other Commodities"]
["40889","Other","Other Commodities"]
["40915","Other","Other Commodities"]
["40918","Other","Other Commodities"]
["40939","Other","Other Commodities"]
["40964","Other","Other Commodities"]
["40975","Other","Other Commodities"]
["41007","Other","Other Commodities"]
["41014","Other","Other Commodities"]
["41035","Other","Other Commodities"]
["41060","Other","Other Commodities"]
["41064","Other","Other Commodities"]
["41085","Other","Other Commodities"]
["41110","Other","Other Commodities"]
["41120","Other","Other Commodities"]
["41153","Other","Other Commodities"]
["41160","Other","Other Commodities"]
["41181","Other","Other Commodities"]
["41205","Other","Other Commodities"]
["41210","Other","Other Commodities"]
["41231","Other","Other Commodities"]
["41256","Other","Other Commodities"]
["41265","Other","Other Commodities"]
["41285","Other","Other Commodities"]
["41306","Other","Other Commodities"]
["41327","Other","Other Commodities"]
["41350","Other","Other Commodities"]
["41356","Other","Other Commodities"]
["41377","Other","Other Commodities"]
["41392","Other","Other Commodities"]
["41424","Other","Other Commodities"]
["41431","Other","Other Commodities"]
["41452","Other","Other Commodities"]
["41471","Other","Other Commodities"]
["41499","Other","Other Commodities"]
["41502","Other","Other Commodities"]
["41527","Other","Other Commodities"]
["41556","Other","Other Commodities"]
["41570","Other","Other Commodities"]
["41577","Other","Other Commodities"]
["41598","Other","Other Commodities"]
["41616","Other","Other Commodities"]
["41645","Other","Other Commodities"]
["41648","Other","Other Commodities"]
["41673","Other","Other Commodities"]
["41701","Other","Other Commodities"]
["41716","Other","Other Commodities"]
["41723","Other","Other Commodities"]
["41744","Other","Other Commodities"]
["41761","Other","Other Commodities"]
["41791","Other","Other Commodities"]
["41794","Other","Other Commodities"]
["41819","Other","Other Commodities"]
["41846","Other","Other Commodities"]
["41862","Other","Other Commodities"]
["41869","Other","Other Commodities"]
["41890","Other","Other Commodities"]
["41912","Other","Other Commodities"]
["41937","Other","Other Commodities"]
["41940","Other","Other Commodities"]
["41965","Other","Other Commodities"]
["41991","Other","Other Commodities"]
["42008","Other","Other Commodities"]
["42015","Other","Other Commodities"]
["42036","Other","Other Commodities"]
["42057","Other","Other Commodities"]
["42083","Other","Other Commodities"]
["42086","Other","Other Commodities"]
["42111","Other","Other Commodities"]
["42136","Other","Other Commodities"]
["42154","Other","Other Commodities"]
["42161","Other","Other Commodities"]
["42182","Other","Other Commodities"]
["42202","Other","Other Commodities"]
["42229","Other","Other Commodities"]
["42232","Other","Other Commodities"]
["42257","Other","Other Commodities"]
["42281","Other","Other Commodities"]
["42304","Other","Other Commodities"]
["42307","Other","Other Commodities"]
["42328","Other","Other Commodities"]
["42347","Other","Other Commodities"]
["42375","Other","Other Commodities"]
["42378","Other","Other Commodities"]
["42403","Other","Other Commodities"]
["42426","Other","Other Commodities"]
["42450","Other","Other Commodities"]
["42453","Other","Other Commodities"]
["42474","Other","Other Commodities"]
["42492","Other","Other Commodities"]
["42521","Other","Other Commodities"]
["42528","Other","Other Commodities"]
["42549","Other","Other Commodities"]
["42571","Other","Other Commodities"]
["42596","Other","Other Commodities"]
["42599","Other","Other Commodities"]
["42620","Other","Other Commodities"]
["42637","Other","Other Commodities"]
["42667","Other","Other Commodities"]
["42674","Other","Other Commodities"]
["42695","Other","Other Commodities"]
["42716","Other","Other Commodities"]
["42742","Other","Other Commodities"]
["42745","Other","Other Commodities"]
["42766","Other","Other Commodities"]
["42782","Other","Other Commodities"]
["42813","Other","Other Commodities"]
["42820","Other","Other Commodities"]
["42841","Other","Other Commodities"]
["42861","Other","Other Commodities"]
["42888","Other","Other Commodities"]
["42891","Other","Other Commodities"]
["42916","Other","Other Commodities"]
["42927","Other","Other Commodities"]
["42959","Other","Other Commodities"]
["42966","Other","Other Commodities"]
["42987","Other","Other Commodities"]
["43006","Other","Other Commodities"]
["43034","Other","Other Commodities"]
["43037","Other","Other Commodities"]
["43062","Other","Other Commodities"]
["43072","Other","Other Commodities"]
["43105","Other","Other Commodities"]
["43112","Other","Other Commodities"]
["43133","Other","Other Commodities"]
["43151","Other","Other Commodities"]
["43180","Other","Other Commodities"]
["43183","Other","Other Commodities"]
["43208","Other","Other Commodities"]
["43217","Other","Other Commodities"]
["43251","Other","Other Commodities"]
["43258","Other","Other Commodities"]
["43279","Other","Other Commodities"]
["43302","Other","Other Commodities"]
["43326","Other","Other Commodities"]
["43329","Other","Other Commodities"]
["43354","Other","Other Commodities"]
["43381","Other","Other Commodities"]
["43397","Other","Other Commodities"]
["43404","Other","Other Commodities"]
["43425","Other","Other Commodities"]
["43447","Other","Other Commodities"]
["43472","Other","Other Commodities"]
["43475","Other","Other Commodities"]
["43500","Other","Other Commodities"]
["43526","Other","Other Commodities"]
["43529","Other","Other Commodities"]
["43550","Other","Other Commodities"]
["43571","Other","Other Commodities"]
["43592","Other","Other Commodities"]
["43618","Other","Other Commodities"]
["43621","Other","Other Commodities"]
["43646","Other","Other Commodities"]
["43671","Other","Other Commodities"]
["43675","Other","Other Commodities"]
["43696","Other","Other Commodities"]
["43717","Other","Other Commodities"]
["43737","Other","Other Commodities"]
["43764","Other","Other Commodities"]
["43767","Other","Other Commodities"]
["43792","Other","Other Commodities"]
["43816","Other","Other Commodities"]
["43821","Other","Other Commodities"]
["43842","Other","Other Commodities"]
["43863","Other","Other Commodities"]
["43882","Other","Other Commodities"]
["43910","Other","Other Commodities"]
["43917","Other","Other Commodities"]
["43938","Other","Other Commodities"]
["43961","Other","Other Commodities"]
["43967","Other","Other Commodities"]
["43988","Other","Other Commodities"]
["44009","44","44 Freight Forwarder Traffic"]
["44027","44","44 Freight Forwarder Traffic"]
["44056","44","44 Freight Forwarder Traffic"]
["44063","44","44 Freight Forwarder Traffic"]
["44084","44","44 Freight Forwarder Traffic"]
["44106","44","44 Freight Forwarder Traffic"]
["44113","44","44 Freight Forwarder Traffic"]
["44134","44","44 Freight Forwarder Traffic"]
["44159","44","44 Freight Forwarder Traffic"]
["44172","44","44 Freight Forwarder Traffic"]
["44202","44","44 Freight Forwarder Traffic"]
["44209","44","44 Freight Forwarder Traffic"]
["44230","44","44 Freight Forwarder Traffic"]
["44251","44","44 Freight Forwarder Traffic"]
["44259","44","44 Freight Forwarder Traffic"]
["44280","44","44 Freight Forwarder Traffic"]
["44305","44","44 Freight Forwarder Traffic"]
["44317","44","44 Freight Forwarder Traffic"]
["44348","44","44 Freight Forwarder Traffic"]
["44355","44","44 Freight Forwarder Traffic"]
["44376","44","44 Freight Forwarder Traffic"]
["44396","44","44 Freight Forwarder Traffic"]
["44405","44","44 Freight Forwarder Traffic"]
["44426","44","44 Freight Forwarder Traffic"]
["44451","44","44 Freight Forwarder Traffic"]
["44462","44","44 Freight Forwarder Traffic"]
["44494","44","44 Freight Forwarder Traffic"]
["44501","44","44 Freight Forwarder Traffic"]
["44522","44","44 Freight Forwarder Traffic"]
["44547","44","44 Freight Forwarder Traffic"]
["44551","44","44 Freight Forwarder Traffic"]
["44572","44","44 Freight Forwarder Traffic"]
["44597","44","44 Freight Forwarder Traffic"]
["44607","44","44 Freight Forwarder Traffic"]
["44640","44","44 Freight Forwarder Traffic"]
["44647","44","44 Freight Forwarder Traffic"]
["44668","44","44 Freight Forwarder Traffic"]
["44692","44","44 Freight Forwarder Traffic"]
["44697","44","44 Freight Forwarder Traffic"]
["44718","44","44 Freight Forwarder Traffic"]
["44743","44","44 Freight Forwarder Traffic"]
["44752","44","44 Freight Forwarder Traffic"]
["44786","44","44 Freight Forwarder Traffic"]
["44793","44","44 Freight Forwarder Traffic"]
["44814","44","44 Freight Forwarder Traffic"]
["44837","44","44 Freight Forwarder Traffic"]
["44843","44","44 Freight Forwarder Traffic"]
["44864","44","44 Freight Forwarder Traffic"]
["44889","44","44 Freight Forwarder Traffic"]
["44897","44","44 Freight Forwarder Traffic"]
["44918","44","44 Freight Forwarder Traffic"]
["44939","44","44 Freight Forwarder Traffic"]
["44960","44","44 Freight Forwarder Traffic"]
["44982","44","44 Freight Forwarder Traffic"]
["44989","44","44 Freight Forwarder Traffic"]
["45010","45","45 Shipper Assocation Traffic"]
["45035","45","45 Shipper Assocation Traffic"]
["45042","45","45 Shipper Assocation Traffic"]
["45064","45","45 Shipper Assocation Traffic"]
["45085","45","45 Shipper Assocation Traffic"]
["45106","45","45 Shipper Assocation Traffic"]
["45127","45","45 Shipper Assocation Traffic"]
["45135","45","45 Shipper Assocation Traffic"]
["45160","45","45 Shipper Assocation Traffic"]
["45181","45","45 Shipper Assocation Traffic"]
["45206","45","45 Shipper Assocation Traffic"]
["45210","45","45 Shipper Assocation Traffic"]
["45231","45","45 Shipper Assocation Traffic"]
["45252","45","45 Shipper Assocation Traffic"]
["45272","45","45 Shipper Assocation Traffic"]
["45281","45","45 Shipper Assocation Traffic"]
["45306","45","45 Shipper Assocation Traffic"]
["45327","45","45 Shipper Assocation Traffic"]
["45351","45","45 Shipper Assocation Traffic"]
["45356","45","45 Shipper Assocation Traffic"]
["45377","45","45 Shipper Assocation Traffic"]
["45398","45","45 Shipper Assocation Traffic"]
["45417","45","45 Shipper Assocation Traffic"]
["45427","45","45 Shipper Assocation Traffic"]
["45452","45","45 Shipper Assocation Traffic"]
["45473","45","45 Shipper Assocation Traffic"]
["45496","45","45 Shipper Assocation Traffic"]
["45502","45","45 Shipper Assocation Traffic"]
["45523","45","45 Shipper Assocation Traffic"]
["45548","45","45 Shipper Assocation Traffic"]
["45562","45","45 Shipper Assocation Traffic"]
["45573","45","45 Shipper Assocation Traffic"]
["45598","45","45 Shipper Assocation Traffic"]
["45619","45","45 Shipper Assocation Traffic"]
["45641","45","45 Shipper Assocation Traffic"]
["45648","45","45 Shipper Assocation Traffic"]
["45669","45","45 Shipper Assocation Traffic"]
["45694","45","45 Shipper Assocation Traffic"]
["45707","45","45 Shipper Assocation Traffic"]
["45719","45","45 Shipper Assocation Traffic"]
["45744","45","45 Shipper Assocation Traffic"]
["45765","45","45 Shipper Assocation Traffic"]
["45773","45","45 Shipper Assocation Traffic"]
["45794","45","45 Shipper Assocation Traffic"]
["45815","45","45 Shipper Assocation Traffic"]
["45840","45","45 Shipper Assocation Traffic"]
["45852","45","45 Shipper Assocation Traffic"]
["45865","45","45 Shipper Assocation Traffic"]
["45890","45","45 Shipper Assocation Traffic"]
["45911","45","45 Shipper Assocation Traffic"]
["45918","45","45 Shipper Assocation Traffic"]
["45940","45","45 Shipper Assocation Traffic"]
["45961","45","45 Shipper Assocation Traffic"]
["45979","45","45 Shipper Assocation Traffic"]
["46008","46","46 Other Misc. Mixed Shipments"]
["46011","46","46 Other Misc. Mixed Shipments"]
["46036","46","46 Other Misc. Mixed Shipments"]
["46058","46","46 Other Misc. Mixed Shipments"]
["46065","46","46 Other Misc. Mixed Shipments"]
["46086","46","46 Other Misc. Mixed Shipments"]
["46107","461","461 Misc. Mixed Shipments not TOFC"]
["46124","461","461 Misc. Mixed Shipments not TOFC"]
["46154","461","461 Misc. Mixed Shipments not TOFC"]
["46161","461","461 Misc. Mixed Shipments not TOFC"]
["46182","461","461 Misc. Mixed Shipments not TOFC"]
["46203","46","46 Other Misc. Mixed Shipments"]
["46211","46","46 Other Misc. Mixed Shipments"]
["46232","46","46 Other Misc. Mixed Shipments"]
["46253","46","46 Other Misc. Mixed Shipments"]
["46269","46","46 Other Misc. Mixed Shipments"]
["46300","46","46 Other Misc. Mixed Shipments"]
["46307","46","46 Other Misc. Mixed Shipments"]
["46328","46","46 Other Misc. Mixed Shipments"]
["46348","46","46 Other Misc. Mixed Shipments"]
["46357","46","46 Other Misc. Mixed Shipments"]
["46378","46","46 Other Misc. Mixed Shipments"]
["46399","46","46 Other Misc. Mixed Shipments"]
["46414","46","46 Other Misc. Mixed Shipments"]
["46446","46","46 Other Misc. Mixed Shipments"]
["46453","46","46 Other Misc. Mixed Shipments"]
["46474","46","46 Other Misc. Mixed Shipments"]
["46493","46","46 Other Misc. Mixed Shipments"]
["46503","46","46 Other Misc. Mixed Shipments"]
["46524","46","46 Other Misc. Mixed Shipments"]
["46549","46","46 Other Misc. Mixed Shipments"]
["46559","46","46 Other Misc. Mixed Shipments"]
["46592","46","46 Other Misc. Mixed Shipments"]
["46599","46","46 Other Misc. Mixed Shipments"]
["46620","46","46 Other Misc. Mixed Shipments"]
["46638","46","46 Other Misc. Mixed Shipments"]
["46649","46","46 Other Misc. Mixed Shipments"]
["46670","46","46 Other Misc. Mixed Shipments"]
["46695","46","46 Other Misc. Mixed Shipments"]
["46704","46","46 Other Misc. Mixed Shipments"]
["46738","46","46 Other Misc. Mixed Shipments"]
["46745","46","46 Other Misc. Mixed Shipments"]
["46766","46","46 Other Misc. Mixed Shipments"]
["46789","46","46 Other Misc. Mixed Shipments"]
["46795","46","46 Other Misc. Mixed Shipments"]
["46816","46","46 Other Misc. Mixed Shipments"]
["46841","46","46 Other Misc. Mixed Shipments"]
["46849","46","46 Other Misc. Mixed Shipments"]
["46884","46","46 Other Misc. Mixed Shipments"]
["46891","46","46 Other Misc. Mixed Shipments"]
["46912","46","46 Other Misc. Mixed Shipments"]
["46934","46","46 Other Misc. Mixed Shipments"]
["46941","46","46 Other Misc. Mixed Shipments"]
["46962","46","46 Other Misc. Mixed Shipments"]
["46987","46","46 Other Misc. Mixed Shipments"]
["47013","Other","Other Commodities"]
["47030","Other","Other Commodities"]
["47037","Other","Other Commodities"]
["47058","Other","Other Commodities"]
["47079","Other","Other Commodities"]
["47087","Other","Other Commodities"]
["47108","Other","Other Commodities"]
["47133","Other","Other Commodities"]
["47158","Other","Other Commodities"]
["47162","Other","Other Commodities"]
["47183","Other","Other Commodities"]
["47204","Other","Other Commodities"]
["47224","Other","Other Commodities"]
["47233","Other","Other Commodities"]
["47254","Other","Other Commodities"]
["47279","Other","Other Commodities"]
["47303","Other","Other Commodities"]
["47308","Other","Other Commodities"]
["47329","Other","Other Commodities"]
["47350","Other","Other Commodities"]
["47369","Other","Other Commodities"]
["47379","Other","Other Commodities"]
["47400","Other","Other Commodities"]
["47425","Other","Other Commodities"]
["47448","Other","Other Commodities"]
["47454","Other","Other Commodities"]
["47475","Other","Other Commodities"]
["47496","Other","Other Commodities"]
["47514","Other","Other Commodities"]
["47525","Other","Other Commodities"]
["47550","Other","Other Commodities"]
["47571","Other","Other Commodities"]
["47593","Other","Other Commodities"]
["47600","Other","Other Commodities"]
["47621","Other","Other Commodities"]
["47642","Other","Other Commodities"]
["47659","Other","Other Commodities"]
["47671","Other","Other Commodities"]
["47696","Other","Other Commodities"]
["47717","Other","Other Commodities"]
["47738","Other","Other Commodities"]
["47746","Other","Other Commodities"]
["47767","Other","Other Commodities"]
["47792","Other","Other Commodities"]
["47804","Other","Other Commodities"]
["47817","Other","Other Commodities"]
["47842","Other","Other Commodities"]
["47863","Other","Other Commodities"]
["47883","Other","Other Commodities"]
["47892","Other","Other Commodities"]
["47913","Other","Other Commodities"]
["47938","Other","Other Commodities"]
["47949","Other","Other Commodities"]
["47963","Other","Other Commodities"]
["47988","Other","Other Commodities"]
["48009","48","48 Hazardous Materials"]
["48028","48","48 Hazardous Materials"]
["48038","48","48 Hazardous Materials"]
["48059","48","48 Hazardous Materials"]
["48084","48","48 Hazardous Materials"]
["48094","48","48 Hazardous Materials"]
["48109","48","48 Hazardous Materials"]
["48134","48","48 Hazardous Materials"]
["48155","48","48 Hazardous Materials"]
["48179","48","48 Hazardous Materials"]
["48184","48","48 Hazardous Materials"]
["48205","48","48 Hazardous Materials"]
["48230","48","48 Hazardous Materials"]
["48239","48","48 Hazardous Materials"]
["48255","48","48 Hazardous Materials"]
["48280","48","48 Hazardous Materials"]
["48301","48","48 Hazardous Materials"]
["48324","48","48 Hazardous Materials"]
["48330","48","48 Hazardous Materials"]
["48351","48","48 Hazardous Materials"]
["48376","48","48 Hazardous Materials"]
["48384","48","48 Hazardous Materials"]
["48405","48","48 Hazardous Materials"]
["48426","48","48 Hazardous Materials"]
["48447","48","48 Hazardous Materials"]
["48469","48","48 Hazardous Materials"]
["48476","48","48 Hazardous Materials"]
["48497","48","48 Hazardous Materials"]
["48522","48","48 Hazardous Materials"]
["48529","48","48 Hazardous Materials"]
["48551","48","48 Hazardous Materials"]
["48572","48","48 Hazardous Materials"]
["48593","48","48 Hazardous Materials"]
["48614","48","48 Hazardous Materials"]
["48622","48","48 Hazardous Materials"]
["48643","48","48 Hazardous Materials"]
["48668","48","48 Hazardous Materials"]
["48674","48","48 Hazardous Materials"]
["48697","48","48 Hazardous Materials"]
["48718","48","48 Hazardous Materials"]
["48739","48","48 Hazardous Materials"]
["48759","48","48 Hazardous Materials"]
["48768","48","48 Hazardous Materials"]
["48793","48","48 Hazardous Materials"]
["48814","48","48 Hazardous Materials"]
["48838","48","48 Hazardous Materials"]
["48843","48","48 Hazardous Materials"]
["48864","48","48 Hazardous Materials"]
["48885","48","48 Hazardous Materials"]
["48904","48","48 Hazardous Materials"]
["48914","48","48 Hazardous Materials"]
["48939","48","48 Hazardous Materials"]
["48960","48","48 Hazardous Materials"]
["48983","48","48 Hazardous Materials"]
["48989","48","48 Hazardous Materials"]
["49010","Other","Other Commodities"]
["49031","Other","Other Commodities"]
["49049","Other","Other Commodities"]
["49060","Other","Other Commodities"]
["49085","Other","Other Commodities"]
["49106","Other","Other Commodities"]
["49128","Other","Other Commodities"]
["49135","Other","Other Commodities"]
["49156","Other","Other Commodities"]
["49181","Other","Other Commodities"]
["49194","Other","Other Commodities"]
["49206","Other","Other Commodities"]
["49231","Other","Other Commodities"]
["49252","Other","Other Commodities"]
["49273","Other","Other Commodities"]
["49281","Other","Other Commodities"]
["49302","Other","Other Commodities"]
["49327","Other","Other Commodities"]
["49339","Other","Other Commodities"]
["49352","Other","Other Commodities"]
["49377","Other","Other Commodities"]
["49398","Other","Other Commodities"]
["49405","Other","Other Commodities"]
["49427","Other","Other Commodities"]
["49448","Other","Other Commodities"]
["49473","Other","Other Commodities"]
["49484","Other","Other Commodities"]
["49498","Other","Other Commodities"]
["49523","Other","Other Commodities"]
["49544","Other","Other Commodities"]
["49550","Other","Other Commodities"]
["49573","Other","Other Commodities"]
["49594","Other","Other Commodities"]
["49619","Other","Other Commodities"]
["49629","Other","Other Commodities"]
["49644","Other","Other Commodities"]
["49669","Other","Other Commodities"]
["49690","Other","Other Commodities"]
["49714","Other","Other Commodities"]
["49719","Other","Other Commodities"]
["49740","Other","Other Commodities"]
["49765","Other","Other Commodities"]
["49774","Other","Other Commodities"]
["49794","Other","Other Commodities"]
["49815","Other","Other Commodities"]
["49836","Other","Other Commodities"]
["49859","Other","Other Commodities"]
["49865","Other","Other Commodities"]
["49886","Other","Other Commodities"]
["49911","Other","Other Commodities"]
["49919","Other","Other Commodities"]
["49940","Other","Other Commodities"]
["49961","Other","Other Commodities"]
["49982","Other","Other Commodities"]
["50004","Other","Other Commodities"]
["50011","Other","Other Commodities"]
["50036","Other","Other Commodities"]
["50057","Other","Other Commodities"]
["50064","Other","Other Commodities"]
["50086","Other","Other Commodities"]
["50107","Other","Other Commodities"]
["50128","Other","Other Commodities"]
["50149","Other","Other Commodities"]
["50157","Other","Other Commodities"]
["50182","Other","Other Commodities"]
["50203","Other","Other Commodities"]
["50209","Other","Other Commodities"]
["50232","Other","Other Commodities"]
["50253","Other","Other Commodities"]
["50274","Other","Other Commodities"]
["50294","Other","Other Commodities"]
["50303","Other","Other Commodities"]
["50328","Other","Other Commodities"]
["50349","Other","Other Commodities"]
["50354","Other","Other Commodities"]
["50378","Other","Other Commodities"]
["50399","Other","Other Commodities"]
["50424","Other","Other Commodities"]
["50439","Other","Other Commodities"]
["50449","Other","Other Commodities"]
["50474","Other","Other Commodities"]
["50481","Other","Other Commodities"]
["50500","Other","Other Commodities"]
["50501","Other","Other Commodities"]
["50502","Other","Other Commodities"]
["50503","Other","Other Commodities"]
["50504","Other","Other Commodities"]
["50505","Other","Other Commodities"]
["50506","Other","Other Commodities"]
["50507","Other","Other Commodities"]
["50508","Other","Other Commodities"]
["50509","Other","Other Commodities"]
["50510","Other","Other Commodities"]
["50511","Other","Other Commodities"]
["50512","Other","Other Commodities"]
["50513","Other","Other Commodities"]
["50514","Other","Other Commodities"]
["50515","Other","Other Commodities"]
["50516","Other","Other Commodities"]
["50517","Other","Other Commodities"]
["50518","Other","Other Commodities"]
["50519","Other","Other Commodities"]
["50520","Other","Other Commodities"]
["50521","Other","Other Commodities"]
["50522","Other","Other Commodities"]
["50523","Other","Other Commodities"]
["50524","Other","Other Commodities"]
["50525","Other","Other Commodities"]
["50526","Other","Other Commodities"]
["50527","Other","Other Commodities"]
["50528","Other","Other Commodities"]
["50529","Other","Other Commodities"]
["50530","Other","Other Commodities"]
["50531","Other","Other Commodities"]
["50532","Other","Other Commodities"]
["50533","Other","Other Commodities"]
["50534","Other","Other Commodities"]
["50535","Other","Other Commodities"]
["50536","Other","Other Commodities"]
["50537","Other","Other Commodities"]
["50538","Other","Other Commodities"]
["50539","Other","Other Commodities"]
["50540","Other","Other Commodities"]
["50541","Other","Other Commodities"]
["50542","Other","Other Commodities"]
["50543","Other","Other Commodities"]
["50544","Other","Other Commodities"]
["50545","Other","Other Commodities"]
["50546","Other","Other Commodities"]
["50547","Other","Other Commodities"]
["50548","Other","Other Commodities"]
["50549","Other","Other Commodities"]
["50550","Other","Other Commodities"]
["50551","Other","Other Commodities"]
["50552","Other","Other Commodities"]
["50553","Other","Other Commodities"]
["50554","Other","Other Commodities"]
["50555","Other","Other Commodities"]
["50556","Other","Other Commodities"]
["50557","Other","Other Commodities"]
["50558","Other","Other Commodities"]
["50559","Other","Other Commodities"]
["50560","Other","Other Commodities"]
["50561","Other","Other Commodities"]
["50562","Other","Other Commodities"]
["50563","Other","Other Commodities"]
["50564","Other","Other Commodities"]
["50565","Other","Other Commodities"]
["50566","Other","Other Commodities"]
["50567","Other","Other Commodities"]
["50568","Other","Other Commodities"]
["50569","Other","Other Commodities"]
["50570","Other","Other Commodities"]
["50571","Other","Other Commodities"]
["50572","Other","Other Commodities"]
["50573","Other","Other Commodities"]
["50574","Other","Other Commodities"]
["50575","Other","Other Commodities"]
["50576","Other","Other Commodities"]
["50577","Other","Other Commodities"]
["50578","Other","Other Commodities"]
["50579","Other","Other Commodities"]
["50580","Other","Other Commodities"]
["50581","Other","Other Commodities"]
["50582","Other","Other Commodities"]
["50583","Other","Other Commodities"]
["50584","Other","Other Commodities"]
["50585","Other","Other Commodities"]
["50586","Other","Other Commodities"]
["50587","Other","Other Commodities"]
["50588","Other","Other Commodities"]
["50589","Other","Other Commodities"]
["50590","Other","Other Commodities"]
["50591","Other","Other Commodities"]
["50592","Other","Other Commodities"]
["50593","Other","Other Commodities"]
["50594","Other","Other Commodities"]
["50595","Other","Other Commodities"]
["50596","Other","Other Commodities"]
["50597","Other","Other Commodities"]
["50598","Other","Other Commodities"]
["50599","Other","Other Commodities"]
["50600","Other","Other Commodities"]
["50601","Other","Other Commodities"]
["50602","Other","Other Commodities"]
["50603","Other","Other Commodities"]
["50604","Other","Other Commodities"]
["50605","Other","Other Commodities"]
["50606","Other","Other Commodities"]
["50607","Other","Other Commodities"]
["50608","Other","Other Commodities"]
["50609","Other","Other Commodities"]
["50610","Other","Other Commodities"]
["50611","Other","Other Commodities"]
["50612","Other","Other Commodities"]
["50613","Other","Other Commodities"]
["50614","Other","Other Commodities"]
["50615","Other","Other Commodities"]
["50616","Other","Other Commodities"]
["50617","Other","Other Commodities"]
["50618","Other","Other Commodities"]
["50619","Other","Other Commodities"]
["50620","Other","Other Commodities"]
["50621","Other","Other Commodities"]
["50622","Other","Other Commodities"]
["50623","Other","Other Commodities"]
["50624","Other","Other Commodities"]
["50625","Other","Other Commodities"]
["50626","Other","Other Commodities"]
["50627","Other","Other Commodities"]
["50628","Other","Other Commodities"]
["50629","Other","Other Commodities"]
["50630","Other","Other Commodities"]
["50631","Other","Other Commodities"]
["50632","Other","Other Commodities"]
["50633","Other","Other Commodities"]
["50634","Other","Other Commodities"]
["50635","Other","Other Commodities"]
["50636","Other","Other Commodities"]
["50637","Other","Other Commodities"]
["50638","Other","Other Commodities"]
["50639","Other","Other Commodities"]
["50640","Other","Other Commodities"]
["50641","Other","Other Commodities"]
["50642","Other","Other Commodities"]
["50643","Other","Other Commodities"]
["50644","Other","Other Commodities"]
["50645","Other","Other Commodities"]
["50646","Other","Other Commodities"]
["50647","Other","Other Commodities"]
["50648","Other","Other Commodities"]
["50649","Other","Other Commodities"]
["50650","Other","Other Commodities"]
["50651","Other","Other Commodities"]
["50652","Other","Other Commodities"]
["50653","Other","Other Commodities"]
["50654","Other","Other Commodities"]
["50655","Other","Other Commodities"]
["50656","Other","Other Commodities"]
["50657","Other","Other Commodities"]
["50658","Other","Other Commodities"]
["50659","Other","Other Commodities"]
["50660","Other","Other Commodities"]
["50661","Other","Other Commodities"]
["50662","Other","Other Commodities"]
["50663","Other","Other Commodities"]
["50664","Other","Other Commodities"]
["50665","Other","Other Commodities"]
["50666","Other","Other Commodities"]
["50667","Other","Other Commodities"]
["50668","Other","Other Commodities"]
["50669","Other","Other Commodities"]
["50670","Other","Other Commodities"]
["50671","Other","Other Commodities"]
["50672","Other","Other Commodities"]
["50673","Other","Other Commodities"]
["50674","Other","Other Commodities"]
["50675","Other","Other Commodities"]
["50676","Other","Other Commodities"]
["50677","Other","Other Commodities"]
["50678","Other","Other Commodities"]
["50679","Other","Other Commodities"]
["50680","Other","Other Commodities"]
["50681","Other","Other Commodities"]
["50682","Other","Other Commodities"]
["50683","Other","Other Commodities"]
["50684","Other","Other Commodities"]
["50685","Other","Other Commodities"]
["50686","Other","Other Commodities"]
["50687","Other","Other Commodities"]
["50688","Other","Other Commodities"]
["50689","Other","Other Commodities"]
["50690","Other","Other Commodities"]
["50691","Other","Other Commodities"]
["50692","Other","Other Commodities"]
["50693","Other","Other Commodities"]
["50694","Other","Other Commodities"]
["50695","Other","Other Commodities"]
["50696","Other","Other Commodities"]
["50697","Other","Other Commodities"]
["50698","Other","Other Commodities"]
["50699","Other","Other Commodities"]
["50700","Other","Other Commodities"]
["50701","Other","Other Commodities"]
["50702","Other","Other Commodities"]
["50703","Other","Other Commodities"]
["50704","Other","Other Commodities"]
["50705","Other","Other Commodities"]
["50706","Other","Other Commodities"]
["50707","Other","Other Commodities"]
["50708","Other","Other Commodities"]
["50709","Other","Other Commodities"]
["50710","Other","Other Commodities"]
["50711","Other","Other Commodities"]
["50712","Other","Other Commodities"]
["50713","Other","Other Commodities"]
["50714","Other","Other Commodities"]
["50715","Other","Other Commodities"]
["50716","Other","Other Commodities"]
["50717","Other","Other Commodities"]
["50718","Other","Other Commodities"]
["50719","Other","Other Commodities"]
["50720","Other","Other Commodities"]
["50721","Other","Other Commodities"]
["50722","Other","Other Commodities"]
["50723","Other","Other Commodities"]
["50724","Other","Other Commodities"]
["50725","Other","Other Commodities"]
["50726","Other","Other Commodities"]
["50727","Other","Other Commodities"]
["50728","Other","Other Commodities"]
["50729","Other","Other Commodities"]
["50730","Other","Other Commodities"]
["50731","Other","Other Commodities"]
["50732","Other","Other Commodities"]
["50733","Other","Other Commodities"]
["50734","Other","Other Commodities"]
["50735","Other","Other Commodities"]
["50736","Other","Other Commodities"]
["50737","Other","Other Commodities"]
["50738","Other","Other Commodities"]
["50739","Other","Other Commodities"]
["50740","Other","Other Commodities"]
["50741","Other","Other Commodities"]
["50742","Other","Other Commodities"]
["50743","Other","Other Commodities"]
["50744","Other","Other Commodities"]
["50745","Other","Other Commodities"]
["50746","Other","Other Commodities"]
["50747","Other","Other Commodities"]
["50748","Other","Other Commodities"]
["50749","Other","Other Commodities"]
["50750","Other","Other Commodities"]
["50751","Other","Other Commodities"]
["50752","Other","Other Commodities"]
["50753","Other","Other Commodities"]
["50754","Other","Other Commodities"]
["50755","Other","Other Commodities"]
["50756","Other","Other Commodities"]
["50757","Other","Other Commodities"]
["50758","Other","Other Commodities"]
["50759","Other","Other Commodities"]
["50760","Other","Other Commodities"]
["50761","Other","Other Commodities"]
["50762","Other","Other Commodities"]
["50763","Other","Other Commodities"]
["50764","Other","Other Commodities"]
["50765","Other","Other Commodities"]
["50766","Other","Other Commodities"]
["50767","Other","Other Commodities"]
["50768","Other","Other Commodities"]
["50769","Other","Other Commodities"]
["50770","Other","Other Commodities"]
["50771","Other","Other Commodities"]
["50772","Other","Other Commodities"]
["50773","Other","Other Commodities"]
["50774","Other","Other Commodities"]
["50775","Other","Other Commodities"]
["50776","Other","Other Commodities"]
["50777","Other","Other Commodities"]
["50778","Other","Other Commodities"]
["50779","Other","Other Commodities"]
["50780","Other","Other Commodities"]
["50781","Other","Other Commodities"]
["50782","Other","Other Commodities"]
["50783","Other","Other Commodities"]
["50784","Other","Other Commodities"]
["50785","Other","Other Commodities"]
["50786","Other","Other Commodities"]
["50787","Other","Other Commodities"]
["50788","Other","Other Commodities"]
["50789","Other","Other Commodities"]
["50790","Other","Other Commodities"]
["50791","Other","Other Commodities"]
["50792","Other","Other Commodities"]
["50793","Other","Other Commodities"]
["50794","Other","Other Commodities"]
["50795","Other","Other Commodities"]
["50796","Other","Other Commodities"]
["50797","Other","Other Commodities"]
["50798","Other","Other Commodities"]
["50799","Other","Other Commodities"]
["50800","Other","Other Commodities"]
["50801","Other","Other Commodities"]
["50802","Other","Other Commodities"]
["50803","Other","Other Commodities"]
["50804","Other","Other Commodities"]
["50805","Other","Other Commodities"]
["50806","Other","Other Commodities"]
["50807","Other","Other Commodities"]
["50808","Other","Other Commodities"]
["50809","Other","Other Commodities"]
["50810","Other","Other Commodities"]
["50811","Other","Other Commodities"]
["50812","Other","Other Commodities"]
["50813","Other","Other Commodities"]
["50814","Other","Other Commodities"]
["50815","Other","Other Commodities"]
["50816","Other","Other Commodities"]
["50817","Other","Other Commodities"]
["50818","Other","Other Commodities"]
["50819","Other","Other Commodities"]
["50820","Other","Other Commodities"]
["50821","Other","Other Commodities"]
["50822","Other","Other Commodities"]
["50823","Other","Other Commodities"]
["50824","Other","Other Commodities"]
["50825","Other","Other Commodities"]
["50826","Other","Other Commodities"]
["50827","Other","Other Commodities"]
["50828","Other","Other Commodities"]
["50829","Other","Other Commodities"]
["50830","Other","Other Commodities"]
["50831","Other","Other Commodities"]
["50832","Other","Other Commodities"]
["50833","Other","Other Commodities"]
["50834","Other","Other Commodities"]
["50835","Other","Other Commodities"]
["50836","Other","Other Commodities"]
["50837","Other","Other Commodities"]
["50838","Other","Other Commodities"]
["50839","Other","Other Commodities"]
["50840","Other","Other Commodities"]
["50841","Other","Other Commodities"]
["50842","Other","Other Commodities"]
["50843","Other","Other Commodities"]
["50844","Other","Other Commodities"]
["50845","Other","Other Commodities"]
["50846","Other","Other Commodities"]
["50847","Other","Other Commodities"]
["50848","Other","Other Commodities"]
["50849","Other","Other Commodities"]
["50850","Other","Other Commodities"]
["50851","Other","Other Commodities"]
["50852","Other","Other Commodities"]
["50853","Other","Other Commodities"]
["50854","Other","Other Commodities"]
["50855","Other","Other Commodities"]
["50856","Other","Other Commodities"]
["50857","Other","Other Commodities"]
["50858","Other","Other Commodities"]
["50859","Other","Other Commodities"]
["50860","Other","Other Commodities"]
["50861","Other","Other Commodities"]
["50862","Other","Other Commodities"]
["50863","Other","Other Commodities"]
["50864","Other","Other Commodities"]
["50865","Other","Other Commodities"]
["50866","Other","Other Commodities"]
["50867","Other","Other Commodities"]
["50868","Other","Other Commodities"]
["50869","Other","Other Commodities"]
["50870","Other","Other Commodities"]
["50871","Other","Other Commodities"]
["50872","Other","Other Commodities"]
["50873","Other","Other Commodities"]
["50874","Other","Other Commodities"]
["50875","Other","Other Commodities"]
["50876","Other","Other Commodities"]
["50877","Other","Other Commodities"]
["50878","Other","Other Commodities"]
["50879","Other","Other Commodities"]
["50880","Other","Other Commodities"]
["50881","Other","Other Commodities"]
["50882","Other","Other Commodities"]
["50883","Other","Other Commodities"]
["50884","Other","Other Commodities"]
["50885","Other","Other Commodities"]
["50886","Other","Other Commodities"]
["50887","Other","Other Commodities"]
["50888","Other","Other Commodities"]
["50889","Other","Other Commodities"]
["50890","Other","Other Commodities"]
["50891","Other","Other Commodities"]
["50892","Other","Other Commodities"]
["50893","Other","Other Commodities"]
["50894","Other","Other Commodities"]
["50895","Other","Other Commodities"]
["50896","Other","Other Commodities"]
["50897","Other","Other Commodities"]
["50898","Other","Other Commodities"]
["50899","Other","Other Commodities"]
["50900","Other","Other Commodities"]
["50901","Other","Other Commodities"]
["50902","Other","Other Commodities"]
["50903","Other","Other Commodities"]
["50904","Other","Other Commodities"]
["50905","Other","Other Commodities"]
["50906","Other","Other Commodities"]
["50907","Other","Other Commodities"]
["50908","Other","Other Commodities"]
["50909","Other","Other Commodities"]
["50910","Other","Other Commodities"]
["50911","Other","Other Commodities"]
["50912","Other","Other Commodities"]
["50913","Other","Other Commodities"]
["50914","Other","Other Commodities"]
["50915","Other","Other Commodities"]
["50916","Other","Other Commodities"]
["50917","Other","Other Commodities"]
["50918","Other","Other Commodities"]
["50919","Other","Other Commodities"]
["50920","Other","Other Commodities"]
["50921","Other","Other Commodities"]
["50922","Other","Other Commodities"]
["50923","Other","Other Commodities"]
["50924","Other","Other Commodities"]
["50925","Other","Other Commodities"]
["50926","Other","Other Commodities"]
["50927","Other","Other Commodities"]
["50928","Other","Other Commodities"]
["50929","Other","Other Commodities"]
["50930","Other","Other Commodities"]
["50931","Other","Other Commodities"]
["50932","Other","Other Commodities"]
["50933","Other","Other Commodities"]
["50934","Other","Other Commodities"]
["50935","Other","Other Commodities"]
["50936","Other","Other Commodities"]
["50937","Other","Other Commodities"]
["50938","Other","Other Commodities"]
["50939","Other","Other Commodities"]
["50940","Other","Other Commodities"]
["50941","Other","Other Commodities"]
["50942","Other","Other Commodities"]
["50943","Other","Other Commodities"]
["50944","Other","Other Commodities"]
["50945","Other","Other Commodities"]
["50946","Other","Other Commodities"]
["50947","Other","Other Commodities"]
["50948","Other","Other Commodities"]
["50949","Other","Other Commodities"]
["50950","Other","Other Commodities"]
["50951","Other","Other Commodities"]
["50952","Other","Other Commodities"]
["50953","Other","Other Commodities"]
["50954","Other","Other Commodities"]
["50955","Other","Other Commodities"]
["50956","Other","Other Commodities"]
["50957","Other","Other Commodities"]
["50958","Other","Other Commodities"]
["50959","Other","Other Commodities"]
["50960","Other","Other Commodities"]
["50961","Other","Other Commodities"]
["50962","Other","Other Commodities"]
["50963","Other","Other Commodities"]
["50964","Other","Other Commodities"]
["50965","Other","Other Commodities"]
["50966","Other","Other Commodities"]
["50967","Other","Other Commodities"]
["50968","Other","Other Commodities"]
["50969","Other","Other Commodities"]
["50970","Other","Other Commodities"]
["50971","Other","Other Commodities"]
["50972","Other","Other Commodities"]
["50973","Other","Other Commodities"]
["50974","Other","Other Commodities"]
["50975","Other","Other Commodities"]
["50976","Other","Other Commodities"]
["50977","Other","Other Commodities"]
["50978","Other","Other Commodities"]
["50979","Other","Other Commodities"]
["50980","Other","Other Commodities"]
["50981","Other","Other Commodities"]
["50982","Other","Other Commodities"]
["50983","Other","Other Commodities"]
["50984","Other","Other Commodities"]
["50985","Other","Other Commodities"]
["50986","Other","Other Commodities"]
["50987","Other","Other Commodities"]
["50988","Other","Other Commodities"]
["50989","Other","Other Commodities"]
["50990","Other","Other Commodities"]
["50991","Other","Other Commodities"]
["50992","Other","Other Commodities"]
["50993","Other","Other Commodities"]
["50994","Other","Other Commodities"]
["50995","Other","Other Commodities"]
["50996","Other","Other Commodities"]
["50997","Other","Other Commodities"]
["50998","Other","Other Commodities"]
["50999","Other","Other Commodities"]

{"sheet":"ECodeTable","index":9,"n_rows":975,"n_cols":3,"rows_kept":975,"cut":false,"hidden":false,"merged":[]}
["eCode_id","eCode","eTitle_and_Desc"]
[1,"E1L101C1","Gross Ton Mile (GTM), OPR Expense"]
[2,"E1L101C2","Gross Ton Mile (GTM), DRL Expense"]
[3,"E1L101C3","Gross Ton Mile (GTM), ROI Expense"]
[4,"E1L102C1","Car Mile (CM) - Other Than Clerical, OPR Expense"]
[5,"E1L102C2","Car Mile (CM) - Other Than Clerical, DRL Expense"]
[6,"E1L102C3","Car Mile (CM) - Other Than Clerical, ROI Expense"]
[7,"E1L103C1","Train Mile (TM) - Other Than Crew, OPR Expense"]
[8,"E1L103C2","Train Mile (TM) - Other Than Crew, DRL Expense"]
[9,"E1L103C3","Train Mile (TM) - Other Than Crew, ROI Expense"]
[10,"E1L104C1","Train Mile (TM) - Crew, OPR Expense"]
[11,"E1L104C2","Train Mile (TM) - Crew, DRL Expense"]
[12,"E1L104C3","Train Mile (TM) - Crew, ROI Expense"]
[13,"E1L105C1","Locomotive Unit Mile (LUM), OPR Expense"]
[14,"E1L105C2","Locomotive Unit Mile (LUM), DRL Expense"]
[15,"E1L105C3","Locomotive Unit Mile (LUM), ROI Expense"]
[16,"E1L106C1","CLOR (Carloads Handled) - Other, OPR Expense"]
[17,"E1L106C2","CLOR (Carloads Handled) - Other, DRL Expense"]
[18,"E1L106C3","CLOR (Carloads Handled) - Other, ROI Expense"]
[19,"E1L107C1","CLOR (Carloads Handled) - Clerical, OPR Expense"]
[20,"E1L107C2","CLOR (Carloads Handled) - Clerical, DRL Expense"]
[21,"E1L107C3","CLOR (Carloads Handled) - Clerical, ROI Expense"]
[22,"E1L108C1","CLOT (Carloads Orig Or Term) - Other, OPR Expense"]
[23,"E1L108C2","CLOT (Carloads Orig Or Term) - Other, DRL Expense"]
[24,"E1L108C3","CLOT (Carloads Orig Or Term) - Other, ROI Expense"]
[25,"E1L109C1","CLOT (Carloads Orig Or Term) - Clerical, OPR Expense"]
[26,"E1L109C2","CLOT (Carloads Orig Or Term) - Clerical, DRL Expense"]
[27,"E1L109C3","CLOT (Carloads Orig Or Term) - Clerical, ROI Expense"]
[28,"E1L110C1","Car Mile (CM) - Clerical, OPR Expense"]
[29,"E1L110C2","Car Mile (CM) - Clerical, DRL Expense"]
[30,"E1L110C3","Car Mile (CM) - Clerical, ROI Expense"]
[31,"E1L111C1","Switch Engine Minutes (SEM), OPR Expense"]
[32,"E1L111C2","Switch Engine Minutes (SEM), DRL Expense"]
[33,"E1L111C3","Switch Engine Minutes (SEM), ROI Expense"]
[34,"E1L112C1","Ton Miles In Lake Transfer Service, OPR Expense"]
[35,"E1L112C2","Ton Miles In Lake Transfer Service, DRL Expense"]
[36,"E1L112C3","Ton Miles In Lake Transfer Service, ROI Expense"]
[37,"E1L113C1","Tons Handled at Coal Terminals, OPR Expense"]
[38,"E1L113C2","Tons Handled at Coal Terminals, DRL Expense"]
[39,"E1L113C3","Tons Handled at Coal Terminals, ROI Expense"]
[40,"E1L114C1","Tons Handled at Ore Terminals, OPR Expense"]
[41,"E1L114C2","Tons Handled at Ore Terminals, DRL Expense"]
[42,"E1L114C3","Tons Handled at Ore Terminals, ROI Expense"]
[43,"E1L115C1","Tons Handled at Other Marine Terminals, OPR Expense"]
[44,"E1L115C2","Tons Handled at Other Marine Terminals, DRL Expense"]
[45,"E1L115C3","Tons Handled at Other Marine Terminals, ROI Expense"]
[46,"E1L116C1","Refrigerated Car Miles, OPR Expense"]
[47,"E1L116C2","Refrigerated Car Miles, DRL Expense"]
[48,"E1L116C3","Refrigerated Car Miles, ROI Expense"]
[49,"E1L117C1","Protective Service Reefer TCU Days, OPR Expense"]
[50,"E1L117C2","Protective Service Reefer TCU Days, DRL Expense"]
[51,"E1L117C3","Protective Service Reefer TCU Days, ROI Expense"]
[52,"E1L118C1","Refrigerated TCU Days, OPR Expense"]
[53,"E1L118C2","Refrigerated TCU Days, DRL Expense"]
[54,"E1L118C3","Refrigerated TCU Days, ROI Expense"]
[55,"E1L119C1","Other (Non-Refrigerated) TCU Days, OPR Expense"]
[56,"E1L119C2","Other (Non-Refrigerated) TCU Days, DRL Expense"]
[57,"E1L119C3","Other (Non-Refrigerated) TCU Days, ROI Expense"]
[58,"E1L120C1","TCUs Loaded And Unloaded (L&UL), OPR Expense"]
[59,"E1L120C2","TCUs Loaded And Unloaded (L&UL), DRL Expense"]
[60,"E1L120C3","TCUs Loaded And Unloaded (L&UL), ROI Expense"]
[61,"E1L121C1","MVUs Loaded And Unloaded (L&UL), OPR Expense"]
[62,"E1L121C2","MVUs Loaded And Unloaded (L&UL), DRL Expense"]
[63,"E1L121C3","MVUs Loaded And Unloaded (L&UL), ROI Expense"]
[64,"E1L122C1","TCUs Picked Up and Delivered (PU&D), OPR Expense"]
[65,"E1L122C2","TCUs Picked Up and Delivered (PU&D), DRL Expense"]
[66,"E1L122C3","TCUs Picked Up and Delivered (PU&D), ROI Expense"]
[67,"E1L201C1","CM(R), OPR Expense, Railroad-Owned, BOX - 40 FT"]
[68,"E1L201C2","CM(R), DRL Expense, Railroad-Owned, BOX - 40 FT"]
[69,"E1L201C3","CM(R), ROI Expense, Railroad-Owned, BOX - 40 FT"]
[70,"E1L201C4","CM(Y), OPR Expense, Railroad-Owned, BOX - 40 FT"]
[71,"E1L201C5","CM(Y), DRL Expense, Railroad-Owned, BOX - 40 FT"]
[72,"E1L201C6","CM(Y), ROI Expense, Railroad-Owned, BOX - 40 FT"]
[73,"E1L201C7","CD(R), OPR Expense, Railroad-Owned, BOX - 40 FT"]
[74,"E1L201C8","CD(R), DRL Expense, Railroad-Owned, BOX - 40 FT"]
[75,"E1L201C9","CD(R), ROI Expense, Railroad-Owned, BOX - 40 FT"]
[76,"E1L201C10","CD(Y), OPR Expense, Railroad-Owned, BOX - 40 FT"]
[77,"E1L201C11","CD(Y), DRL Expense, Railroad-Owned, BOX - 40 FT"]
[78,"E1L201C12","CD(Y), ROI Expense, Railroad-Owned, BOX - 40 FT"]
[79,"E1L201C13","CM(R), DRL Expense, Privately-Owned, BOX - 40 FT"]
[80,"E1L202C1","CM(R), OPR Expense, Railroad-Owned, BOX - 50 FT"]
[81,"E1L202C2","CM(R), DRL Expense, Railroad-Owned, BOX - 50 FT"]
[82,"E1L202C3","CM(R), ROI Expense, Railroad-Owned, BOX - 50 FT"]
[83,"E1L202C4","CM(Y), OPR Expense, Railroad-Owned, BOX - 50 FT"]
[84,"E1L202C5","CM(Y), DRL Expense, Railroad-Owned, BOX - 50 FT"]
[85,"E1L202C6","CM(Y), ROI Expense, Railroad-Owned, BOX - 50 FT"]
[86,"E1L202C7","CD(R), OPR Expense, Railroad-Owned, BOX - 50 FT"]
[87,"E1L202C8","CD(R), DRL Expense, Railroad-Owned, BOX - 50 FT"]
[88,"E1L202C9","CD(R), ROI Expense, Railroad-Owned, BOX - 50 FT"]
[89,"E1L202C10","CD(Y), OPR Expense, Railroad-Owned, BOX - 50 FT"]
[90,"E1L202C11","CD(Y), DRL Expense, Railroad-Owned, BOX - 50 FT"]
[91,"E1L202C12","CD(Y), ROI Expense, Railroad-Owned, BOX - 50 FT"]
[92,"E1L202C13","CM(R), DRL Expense, Privately-Owned, BOX - 50 FT"]
[93,"E1L203C1","CM(R), OPR Expense, Railroad-Owned, BOX - EQUIPPED"]
[94,"E1L203C2","CM(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED"]
[95,"E1L203C3","CM(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED"]
[96,"E1L203C4","CM(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED"]
[97,"E1L203C5","CM(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED"]
[98,"E1L203C6","CM(Y), ROI Expense, Railroad-Owned, BOX - EQUIPPED"]
[99,"E1L203C7","CD(R), OPR Expense, Railroad-Owned, BOX - EQUIPPED"]
[100,"E1L203C8","CD(R), DRL Expense, Railroad-Owned, BOX - EQUIPPED"]
[101,"E1L203C9","CD(R), ROI Expense, Railroad-Owned, BOX - EQUIPPED"]
[102,"E1L203C10","CD(Y), OPR Expense, Railroad-Owned, BOX - EQUIPPED"]
[103,"E1L203C11","CD(Y), DRL Expense, Railroad-Owned, BOX - EQUIPPED"]
[104,"E1L203C12","CD(Y), ROI Expense, Railroad-Owned, BOX - EQUIPPED"]
[105,"E1L203C13","CM(R), DRL Expense, Privately-Owned, BOX - EQUIPPED"]
[106,"E1L204C1","CM(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN"]
[107,"E1L204C2","CM(R), DRL Expense, Railroad-Owned, GONDOLA - PLAIN"]
[108,"E1L204C3","CM(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN"]
[109,"E1L204C4","CM(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN"]
[110,"E1L204C5","CM(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN"]
[111,"E1L204C6","CM(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN"]
[112,"E1L204C7","CD(R), OPR Expense, Railroad-Owned, GONDOLA - PLAIN"]
[113,"E1L204C8","CD(R), DRL Expense, Railroad-Owned, GONDOLA - PLAIN"]
[114,"E1L204C9","CD(R), ROI Expense, Railroad-Owned, GONDOLA - PLAIN"]
[115,"E1L204C10","CD(Y), OPR Expense, Railroad-Owned, GONDOLA - PLAIN"]
[116,"E1L204C11","CD(Y), DRL Expense, Railroad-Owned, GONDOLA - PLAIN"]
[117,"E1L204C12","CD(Y), ROI Expense, Railroad-Owned, GONDOLA - PLAIN"]
[118,"E1L204C13","CM(R), DRL Expense, Privately-Owned, GONDOLA - PLAIN"]
[119,"E1L205C1","CM(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[120,"E1L205C2","CM(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[121,"E1L205C3","CM(R), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[122,"E1L205C4","CM(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[123,"E1L205C5","CM(Y), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[124,"E1L205C6","CM(Y), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[125,"E1L205C7","CD(R), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[126,"E1L205C8","CD(R), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[127,"E1L205C9","CD(R), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[128,"E1L205C10","CD(Y), OPR Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[129,"E1L205C11","CD(Y), DRL Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[130,"E1L205C12","CD(Y), ROI Expense, Railroad-Owned, GONDOLA - EQUIPPED"]
[131,"E1L205C13","CM(R), DRL Expense, Privately-Owned, GONDOLA - EQUIPPED"]
[132,"E1L206C1","CM(R), OPR Expense, Railroad-Owned, HOPPER - COVERED"]
[133,"E1L206C2","CM(R), DRL Expense, Railroad-Owned, HOPPER - COVERED"]
[134,"E1L206C3","CM(R), ROI Expense, Railroad-Owned, HOPPER - COVERED"]
[135,"E1L206C4","CM(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED"]
[136,"E1L206C5","CM(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED"]
[137,"E1L206C6","CM(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED"]
[138,"E1L206C7","CD(R), OPR Expense, Railroad-Owned, HOPPER - COVERED"]
[139,"E1L206C8","CD(R), DRL Expense, Railroad-Owned, HOPPER - COVERED"]
[140,"E1L206C9","CD(R), ROI Expense, Railroad-Owned, HOPPER - COVERED"]
[141,"E1L206C10","CD(Y), OPR Expense, Railroad-Owned, HOPPER - COVERED"]
[142,"E1L206C11","CD(Y), DRL Expense, Railroad-Owned, HOPPER - COVERED"]
[143,"E1L206C12","CD(Y), ROI Expense, Railroad-Owned, HOPPER - COVERED"]
[144,"E1L206C13","CM(R), DRL Expense, Privately-Owned, HOPPER - COVERED"]
[145,"E1L207C1","CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[146,"E1L207C2","CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[147,"E1L207C3","CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[148,"E1L207C4","CM(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[149,"E1L207C5","CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[150,"E1L207C6","CM(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[151,"E1L207C7","CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[152,"E1L207C8","CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[153,"E1L207C9","CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[154,"E1L207C10","CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[155,"E1L207C11","CD(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[156,"E1L207C12","CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[157,"E1L207C13","CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - GENERAL"]
[158,"E1L208C1","CM(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[159,"E1L208C2","CM(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[160,"E1L208C3","CM(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[161,"E1L208C4","CM(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[162,"E1L208C5","CM(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[163,"E1L208C6","CM(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[164,"E1L208C7","CD(R), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[165,"E1L208C8","CD(R), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[166,"E1L208C9","CD(R), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[167,"E1L208C10","CD(Y), OPR Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[168,"E1L208C11","CD(Y), DRL Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[169,"E1L208C12","CD(Y), ROI Expense, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[170,"E1L208C13","CM(R), DRL Expense, Privately-Owned, HOPPER - OPEN TOP - SPECIAL"]
[171,"E1L209C1","CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH"]
[172,"E1L209C2","CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH"]
[173,"E1L209C3","CM(R), ROI Expense, Railroad-Owned, REFRIGERATED - MECH"]
[174,"E1L209C4","CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH"]
[175,"E1L209C5","CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH"]
[176,"E1L209C6","CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH"]
[177,"E1L209C7","CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - MECH"]
[178,"E1L209C8","CD(R), DRL Expense, Railroad-Owned, REFRIGERATED - MECH"]
[179,"E1L209C9","CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - MECH"]
[180,"E1L209C10","CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - MECH"]
[181,"E1L209C11","CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - MECH"]
[182,"E1L209C12","CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - MECH"]
[183,"E1L209C13","CM(R), DRL Expense, Privately-Owned, REFRIGERATED - MECH"]
[184,"E1L210C1","CM(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[185,"E1L210C2","CM(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[186,"E1L210C3","CM(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[187,"E1L210C4","CM(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[188,"E1L210C5","CM(Y), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[189,"E1L210C6","CM(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[190,"E1L210C7","CD(R), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[191,"E1L210C8","CD(R), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[192,"E1L210C9","CD(R), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[193,"E1L210C10","CD(Y), OPR Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[194,"E1L210C11","CD(Y), DRL Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[195,"E1L210C12","CD(Y), ROI Expense, Railroad-Owned, REFRIGERATED - NON-MECH"]
[196,"E1L210C13","CM(R), DRL Expense, Privately-Owned, REFRIGERATED - NON-MECH"]
[197,"E1L211C1","CM(R), OPR Expense, Railroad-Owned, FLAT - TOFC"]
[198,"E1L211C2","CM(R), DRL Expense, Railroad-Owned, FLAT - TOFC"]
[199,"E1L211C3","CM(R), ROI Expense, Railroad-Owned, FLAT - TOFC"]
[200,"E1L211C4","CM(Y), OPR Expense, Railroad-Owned, FLAT - TOFC"]
[201,"E1L211C5","CM(Y), DRL Expense, Railroad-Owned, FLAT - TOFC"]
[202,"E1L211C6","CM(Y), ROI Expense, Railroad-Owned, FLAT - TOFC"]
[203,"E1L211C7","CD(R), OPR Expense, Railroad-Owned, FLAT - TOFC"]
[204,"E1L211C8","CD(R), DRL Expense, Railroad-Owned, FLAT - TOFC"]
[205,"E1L211C9","CD(R), ROI Expense, Railroad-Owned, FLAT - TOFC"]
[206,"E1L211C10","CD(Y), OPR Expense, Railroad-Owned, FLAT - TOFC"]
[207,"E1L211C11","CD(Y), DRL Expense, Railroad-Owned, FLAT - TOFC"]
[208,"E1L211C12","CD(Y), ROI Expense, Railroad-Owned, FLAT - TOFC"]
[209,"E1L211C13","CM(R), DRL Expense, Privately-Owned, FLAT - TOFC"]
[210,"E1L212C1","CM(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[211,"E1L212C2","CM(R), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[212,"E1L212C3","CM(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[213,"E1L212C4","CM(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[214,"E1L212C5","CM(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[215,"E1L212C6","CM(Y), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[216,"E1L212C7","CD(R), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[217,"E1L212C8","CD(R), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[218,"E1L212C9","CD(R), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[219,"E1L212C10","CD(Y), OPR Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[220,"E1L212C11","CD(Y), DRL Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[221,"E1L212C12","CD(Y), ROI Expense, Railroad-Owned, FLAT - MULTILEVEL"]
[222,"E1L212C13","CM(R), DRL Expense, Privately-Owned, FLAT - MULTILEVEL"]
[223,"E1L213C1","CM(R), OPR Expense, Railroad-Owned, FLAT - GENERAL"]
[224,"E1L213C2","CM(R), DRL Expense, Railroad-Owned, FLAT - GENERAL"]
[225,"E1L213C3","CM(R), ROI Expense, Railroad-Owned, FLAT - GENERAL"]
[226,"E1L213C4","CM(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL"]
[227,"E1L213C5","CM(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL"]
[228,"E1L213C6","CM(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL"]
[229,"E1L213C7","CD(R), OPR Expense, Railroad-Owned, FLAT - GENERAL"]
[230,"E1L213C8","CD(R), DRL Expense, Railroad-Owned, FLAT - GENERAL"]
[231,"E1L213C9","CD(R), ROI Expense, Railroad-Owned, FLAT - GENERAL"]
[232,"E1L213C10","CD(Y), OPR Expense, Railroad-Owned, FLAT - GENERAL"]
[233,"E1L213C11","CD(Y), DRL Expense, Railroad-Owned, FLAT - GENERAL"]
[234,"E1L213C12","CD(Y), ROI Expense, Railroad-Owned, FLAT - GENERAL"]
[235,"E1L213C13","CM(R), DRL Expense, Privately-Owned, FLAT - GENERAL"]
[236,"E1L214C1","CM(R), OPR Expense, Railroad-Owned, FLAT - OTHER"]
[237,"E1L214C2","CM(R), DRL Expense, Railroad-Owned, FLAT - OTHER"]
[238,"E1L214C3","CM(R), ROI Expense, Railroad-Owned, FLAT - OTHER"]
[239,"E1L214C4","CM(Y), OPR Expense, Railroad-Owned, FLAT - OTHER"]
[240,"E1L214C5","CM(Y), DRL Expense, Railroad-Owned, FLAT - OTHER"]
[241,"E1L214C6","CM(Y), ROI Expense, Railroad-Owned, FLAT - OTHER"]
[242,"E1L214C7","CD(R), OPR Expense, Railroad-Owned, FLAT - OTHER"]
[243,"E1L214C8","CD(R), DRL Expense, Railroad-Owned, FLAT - OTHER"]
[244,"E1L214C9","CD(R), ROI Expense, Railroad-Owned, FLAT - OTHER"]
[245,"E1L214C10","CD(Y), OPR Expense, Railroad-Owned, FLAT - OTHER"]
[246,"E1L214C11","CD(Y), DRL Expense, Railroad-Owned, FLAT - OTHER"]
[247,"E1L214C12","CD(Y), ROI Expense, Railroad-Owned, FLAT - OTHER"]
[248,"E1L214C13","CM(R), DRL Expense, Privately-Owned, FLAT - OTHER"]
[249,"E1L215C1","CM(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL"]
[250,"E1L215C2","CM(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL"]
[251,"E1L215C3","CM(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL"]
[252,"E1L215C4","CM(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL"]
[253,"E1L215C5","CM(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL"]
[254,"E1L215C6","CM(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL"]
[255,"E1L215C7","CD(R), OPR Expense, Railroad-Owned, TANK <22,000 GAL"]
[256,"E1L215C8","CD(R), DRL Expense, Railroad-Owned, TANK <22,000 GAL"]
[257,"E1L215C9","CD(R), ROI Expense, Railroad-Owned, TANK <22,000 GAL"]
[258,"E1L215C10","CD(Y), OPR Expense, Railroad-Owned, TANK <22,000 GAL"]
[259,"E1L215C11","CD(Y), DRL Expense, Railroad-Owned, TANK <22,000 GAL"]
[260,"E1L215C12","CD(Y), ROI Expense, Railroad-Owned, TANK <22,000 GAL"]
[261,"E1L215C13","CM(R), DRL Expense, Privately-Owned, TANK <22,000 GAL"]
[262,"E1L216C1","CM(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL"]
[263,"E1L216C2","CM(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL"]
[264,"E1L216C3","CM(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL"]
[265,"E1L216C4","CM(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL"]
[266,"E1L216C5","CM(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL"]
[267,"E1L216C6","CM(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL"]
[268,"E1L216C7","CD(R), OPR Expense, Railroad-Owned, TANK >=22,000 GAL"]
[269,"E1L216C8","CD(R), DRL Expense, Railroad-Owned, TANK >=22,000 GAL"]
[270,"E1L216C9","CD(R), ROI Expense, Railroad-Owned, TANK >=22,000 GAL"]
[271,"E1L216C10","CD(Y), OPR Expense, Railroad-Owned, TANK >=22,000 GAL"]
[272,"E1L216C11","CD(Y), DRL Expense, Railroad-Owned, TANK >=22,000 GAL"]
[273,"E1L216C12","CD(Y), ROI Expense, Railroad-Owned, TANK >=22,000 GAL"]
[274,"E1L216C13","CM(R), DRL Expense, Privately-Owned, TANK >=22,000 GAL"]
[275,"E1L217C1","CM(R), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[276,"E1L217C2","CM(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[277,"E1L217C3","CM(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[278,"E1L217C4","CM(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[279,"E1L217C5","CM(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[280,"E1L217C6","CM(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[281,"E1L217C7","CD(R), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[282,"E1L217C8","CD(R), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[283,"E1L217C9","CD(R), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[284,"E1L217C10","CD(Y), OPR Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[285,"E1L217C11","CD(Y), DRL Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[286,"E1L217C12","CD(Y), ROI Expense, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[287,"E1L217C13","CM(R), DRL Expense, Privately-Owned, ALL OTHER FREIGHT CARS"]
[288,"E1L218C1","CM(R), OPR Expense, Railroad-Owned, AUTO RACKS"]
[289,"E1L218C2","CM(R), DRL Expense, Railroad-Owned, AUTO RACKS"]
[290,"E1L218C3","CM(R), ROI Expense, Railroad-Owned, AUTO RACKS"]
[291,"E1L218C4","CM(Y), OPR Expense, Railroad-Owned, AUTO RACKS"]
[292,"E1L218C5","CM(Y), DRL Expense, Railroad-Owned, AUTO RACKS"]
[293,"E1L218C6","CM(Y), ROI Expense, Railroad-Owned, AUTO RACKS"]
[294,"E1L218C7","CD(R), OPR Expense, Railroad-Owned, AUTO RACKS"]
[295,"E1L218C8","CD(R), DRL Expense, Railroad-Owned, AUTO RACKS"]
[296,"E1L218C9","CD(R), ROI Expense, Railroad-Owned, AUTO RACKS"]
[297,"E1L218C10","CD(Y), OPR Expense, Railroad-Owned, AUTO RACKS"]
[298,"E1L218C11","CD(Y), DRL Expense, Railroad-Owned, AUTO RACKS"]
[299,"E1L218C12","CD(Y), ROI Expense, Railroad-Owned, AUTO RACKS"]
[300,"E1L218C13","CM(R), DRL Expense, Privately-Owned, AUTO RACKS"]
[301,"E1L219C1","CM(R), OPR Expense, Railroad-Owned, ACCESSORIAL"]
[302,"E1L219C2","CM(R), DRL Expense, Railroad-Owned, ACCESSORIAL"]
[303,"E1L219C3","CM(R), ROI Expense, Railroad-Owned, ACCESSORIAL"]
[304,"E1L219C4","CM(Y), OPR Expense, Railroad-Owned, ACCESSORIAL"]
[305,"E1L219C5","CM(Y), DRL Expense, Railroad-Owned, ACCESSORIAL"]
[306,"E1L219C6","CM(Y), ROI Expense, Railroad-Owned, ACCESSORIAL"]
[307,"E1L219C7","CD(R), OPR Expense, Railroad-Owned, ACCESSORIAL"]
[308,"E1L219C8","CD(R), DRL Expense, Railroad-Owned, ACCESSORIAL"]
[309,"E1L219C9","CD(R), ROI Expense, Railroad-Owned, ACCESSORIAL"]
[310,"E1L219C10","CD(Y), OPR Expense, Railroad-Owned, ACCESSORIAL"]
[311,"E1L219C11","CD(Y), DRL Expense, Railroad-Owned, ACCESSORIAL"]
[312,"E1L219C12","CD(Y), ROI Expense, Railroad-Owned, ACCESSORIAL"]
[313,"E1L219C13","CM(R), DRL Expense, Privately-Owned, ACCESSORIAL"]
[314,"E1L220C1","CM(R), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[315,"E1L220C2","CM(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[316,"E1L220C3","CM(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[317,"E1L220C4","CM(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[318,"E1L220C5","CM(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[319,"E1L220C6","CM(Y), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[320,"E1L220C7","CD(R), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[321,"E1L220C8","CD(R), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[322,"E1L220C9","CD(R), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[323,"E1L220C10","CD(Y), OPR Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[324,"E1L220C11","CD(Y), DRL Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[325,"E1L220C12","CD(Y), ROI Expense, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[326,"E1L220C13","CM(R), DRL Expense, Privately-Owned, AVERAGE ALL FREIGHT CARS"]
[327,"E1L221C1","CM(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[328,"E1L221C2","CM(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[329,"E1L221C3","CM(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[330,"E1L221C4","CM(Y), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[331,"E1L221C5","CM(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[332,"E1L221C6","CM(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[333,"E1L221C7","CD(R), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[334,"E1L221C8","CD(R), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[335,"E1L221C9","CD(R), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[336,"E1L221C10","CD(Y), OPR Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[337,"E1L221C11","CD(Y), DRL Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[338,"E1L221C12","CD(Y), ROI Expense, Railroad-Owned, TOTAL FLAT, MULTILEVEL"]
[339,"E1L221C13","CM(R), DRL Expense, Privately-Owned, TOTAL FLAT, MULTILEVEL"]
[340,"E1L301C1","L&D Expense, FARM PRODUCTS"]
[341,"E1L302C1","L&D Expense, GRAIN"]
[342,"E1L303C1","L&D Expense, POTATOES OTHER THAN SWEET"]
[343,"E1L304C1","L&D Expense, FRESH FRUITS"]
[344,"E1L305C1","L&D Expense, FRESH VEGETABLES"]
[345,"E1L306C1","L&D Expense, ALL OTHER FARM PRODUCTS"]
[346,"E1L307C1","L&D Expense, METALLIC ORES"]
[347,"E1L308C1","L&D Expense, COAL"]
[348,"E1L309C1","L&D Expense, NONMETALLIC MINERALS"]
[349,"E1L310C1","L&D Expense, FOOD AND KINDRED PRODUCTS"]
[350,"E1L311C1","L&D Expense, FRESH MEATS"]
[351,"E1L312C1","L&D Expense, DAIRY PRODUCTS"]
[352,"E1L313C1","L&D Expense, CANNED FRUITS/VEG"]
[353,"E1L314C1","L&D Expense, GRAIN MILL PRODUCTS"]
[354,"E1L315C1","L&D Expense, FLOUR"]
[355,"E1L316C1","L&D Expense, PREPARED FEEDS"]
[356,"E1L317C1","L&D Expense, CEREALS"]
[357,"E1L318C1","L&D Expense, RICE"]
[358,"E1L319C1","L&D Expense, PREPARED FLOUR"]
[359,"E1L320C1","L&D Expense, CORN PRODUCTS"]
[360,"E1L321C1","L&D Expense, REFINED SUGAR"]
[361,"E1L322C1","L&D Expense, BEER"]
[362,"E1L323C1","L&D Expense, WINES"]
[363,"E1L324C1","L&D Expense, WHISKEY"]
[364,"E1L325C1","L&D Expense, MISC FOOD PREPARATIONS"]
[365,"E1L326C1","L&D Expense, ALL OTHER FOOD PRODUCTS"]
[366,"E1L327C1","L&D Expense, TOBACCO PRODUCTS"]
[367,"E1L328C1","L&D Expense, LUMBER AND WOOD EX FURNITURE"]
[368,"E1L329C1","L&D Expense, LUMBER/DIMENSION STOCK"]
[369,"E1L330C1","L&D Expense, PLYWOOD OR VENEER"]
[370,"E1L331C1","L&D Expense, ALL OTHER LUMBER AND WOOD PRODUCTS"]
[371,"E1L332C1","L&D Expense, FURNITURE AND FIXTURES"]
[372,"E1L333C1","L&D Expense, PULP, PAPER AND ALLIED PRODUCTS"]
[373,"E1L334C1","L&D Expense, NEWSPRINT"]
[374,"E1L335C1","L&D Expense, PRINTING PAPER"]
[375,"E1L336C1","L&D Expense, FIBREBD/PAPERDB/PULPDB"]
[376,"E1L337C1","L&D Expense, COV PAPER/PAPERBOARD"]
[377,"E1L338C1","L&D Expense, SANITARY TISSUES"]
[378,"E1L339C1","L&D Expense, ALL OTHER PULP, PAPER & ALLIED PRODUCTS"]
[379,"E1L340C1","L&D Expense, CHEMICALS"]
[380,"E1L341C1","L&D Expense, INDUSTRIAL CHEMICALS"]
[381,"E1L342C1","L&D Expense, POTASSIUM OR SODIUM"]
[382,"E1L343C1","L&D Expense, SYN FIBRES/RESINS/RUBBER"]
[383,"E1L344C1","L&D Expense, MISC CHEMICALS PRODUCTS"]
[384,"E1L345C1","L&D Expense, ALL OTHER CHEMICALS"]
[385,"E1L346C1","L&D Expense, PETROLEUM OR COAL PRODUCTS"]
[386,"E1L347C1","L&D Expense, RUBBER AND MISC PLASTICS"]
[387,"E1L348C1","L&D Expense, RUBBER TIRES/INNER TUBES"]
[388,"E1L349C1","L&D Expense, ALL OTHER RUBBER PRODUCTS"]
[389,"E1L350C1","L&D Expense, STONE, CLAY AND GLASS PRODUCTS"]
[390,"E1L351C1","L&D Expense, FLAT GLASS"]
[391,"E1L352C1","L&D Expense, NONMETALLIC EARTH/MIN"]
[392,"E1L353C1","L&D Expense, ALL OTHER STONE & CLAY, GLASS PRODUCTS"]
[393,"E1L354C1","L&D Expense, PRIMARY METAL PRODUCTS"]
[394,"E1L355C1","L&D Expense, PRIMARY IRON/STEEL PRODUCTS"]
[395,"E1L356C1","L&D Expense, ALUMINUM BASIC SHAPES"]
[396,"E1L357C1","L&D Expense, ALL OTHER PRIMARY METAL PRODUCTS"]
[397,"E1L358C1","L&D Expense, FABRICATED METAL PRODUCTS"]
[398,"E1L359C1","L&D Expense, FAB STRUC METAL PRODUCTS"]
[399,"E1L360C1","L&D Expense, ALL OTHER FAB METAL PRODUCTS"]
[400,"E1L361C1","L&D Expense, MACHINERY EXCEPT ELECTRICAL"]
[401,"E1L362C1","L&D Expense, ENGINES/TURBINES"]
[402,"E1L363C1","L&D Expense, FARM MACHINERY"]
[403,"E1L364C1","L&D Expense, CONST MIN/MAT HAND MACHINERY"]
[404,"E1L365C1","L&D Expense, ALL OTHER MACHINERY EXCEPT ELECTRICAL"]
[405,"E1L366C1","L&D Expense, ELECTRICAL MACHINERY"]
[406,"E1L367C1","L&D Expense, ELECTRICAL TRANS/DIST EQUIPMENT"]
[407,"E1L368C1","L&D Expense, HOUSEHOLD APPLIANCES"]
[408,"E1L369C1","L&D Expense, RADIO OR TV SETS"]
[409,"E1L370C1","L&D Expense, ALL OTHER ELECTRICAL MACHINERY"]
[410,"E1L371C1","L&D Expense, TRANSPORTAION EQUIPMENT"]
[411,"E1L372C1","L&D Expense, MOTOR PASSENGER CARS"]
[412,"E1L373C1","L&D Expense, MOTOR TRUCKS"]
[413,"E1L374C1","L&D Expense, MOTOR VECHICLE PARTS"]
[414,"E1L375C1","L&D Expense, ALL OTHER TRANSPORTATION EQUIPMENT"]
[415,"E1L376C1","L&D Expense, FREIGHT FORWARDER TRAFFIC"]
[416,"E1L377C1","L&D Expense, SHIPPER ASSOCIATION TRAFFIC"]
[417,"E1L378C1","L&D Expense, MISC MIXED SHIPMENTS"]
[418,"E1L379C1","L&D Expense, MISC MIXED SHIPMENTS NEC INC TOFC"]
[419,"E1L380C1","L&D Expense, ALL OTHER MIXED SHIPMENTS"]
[420,"E1L381C1","L&D Expense, HAZARDOUS MATERIALS"]
[421,"E1L382C1","L&D Expense, ALL OTHER COMMODITIES"]
[422,"E2L101C1","Average Tare Weight, BOX - 40 FT"]
[423,"E2L101C2","E/L Ratio, Railroad-Owned, BOX - 40 FT"]
[424,"E2L101C3","E/L Ratio, Privately-Owned, BOX - 40 FT"]
[425,"E2L101C4","E/L Ratio, All Freight Cars, BOX - 40 FT"]
[426,"E2L101C5","Local circuity, BOX - 40 FT"]
[427,"E2L101C6","Interline circuity, BOX - 40 FT"]
[428,"E2L101C7","Average circuity, BOX - 40 FT"]
[429,"E2L101C8","Spotted-to-Pulled Ratio, BOX - 40 FT"]
[430,"E2L101C9","CD per Industry Switch, BOX - 40 FT"]
[431,"E2L101C10","CD per Interchange Switch, BOX - 40 FT"]
[432,"E2L101C11","CD per Intraterminal Switch, BOX - 40 FT"]
[433,"E2L101C12","CD per Interterminal Switch, BOX - 40 FT"]
[434,"E2L101C13","CD per I&I Switch, BOX - 40 FT"]
[435,"E2L101C14","CD per Load & Unload Industry Switch, BOX - 40 FT"]
[436,"E2L101C15","CD per Load & Unload Intraterminal Switch, BOX - 40 FT"]
[437,"E2L101C16","CD per Load & Unload Interterminal Switch, BOX - 40 FT"]
[438,"E2L101C17","CM per Industry Switch, BOX - 40 FT"]
[439,"E2L101C18","CM per Interchange Switch, BOX - 40 FT"]
[440,"E2L101C19","CM per Intraterminal Switch, BOX - 40 FT"]
[441,"E2L101C20","CM per Interterminal Switch, BOX - 40 FT"]
[442,"E2L101C21","CM per I&I Switch, BOX - 40 FT"]
[443,"E2L101C22","Average CM per CD, Railroad-Owned, BOX - 40 FT"]
[444,"E2L101C23","Average Miles between I&I Switches, BOX - 40 FT"]
[445,"E2L101C24","Average Miles between Interchange Switches, BOX - 40 FT"]
[446,"E2L101C25","SEMs per Industry Switch, BOX - 40 FT"]
[447,"E2L101C26","SEMs per Interchange Switch, BOX - 40 FT"]
[448,"E2L101C27","SEMs per Intraterminal Switch, BOX - 40 FT"]
[449,"E2L101C28","SEMs per Interterminal Switch, BOX - 40 FT"]
[450,"E2L101C29","SEMs per I&I Switch, BOX - 40 FT"]
[451,"E2L102C1","Average Tare Weight, BOX - 50 FT"]
[452,"E2L102C2","E/L Ratio, Railroad-Owned, BOX - 50 FT"]
[453,"E2L102C3","E/L Ratio, Privately-Owned, BOX - 50 FT"]
[454,"E2L102C4","E/L Ratio, All Freight Cars, BOX - 50 FT"]
[455,"E2L102C5","Local circuity, BOX - 50 FT"]
[456,"E2L102C6","Interline circuity, BOX - 50 FT"]
[457,"E2L102C7","Average circuity, BOX - 50 FT"]
[458,"E2L102C8","Spotted-to-Pulled Ratio, BOX - 50 FT"]
[459,"E2L102C9","CD per Industry Switch, BOX - 50 FT"]
[460,"E2L102C10","CD per Interchange Switch, BOX - 50 FT"]
[461,"E2L102C11","CD per Intraterminal Switch, BOX - 50 FT"]
[462,"E2L102C12","CD per Interterminal Switch, BOX - 50 FT"]
[463,"E2L102C13","CD per I&I Switch, BOX - 50 FT"]
[464,"E2L102C14","CD per Load & Unload Industry Switch, BOX - 50 FT"]
[465,"E2L102C15","CD per Load & Unload Intraterminal Switch, BOX - 50 FT"]
[466,"E2L102C16","CD per Load & Unload Interterminal Switch, BOX - 50 FT"]
[467,"E2L102C17","CM per Industry Switch, BOX - 50 FT"]
[468,"E2L102C18","CM per Interchange Switch, BOX - 50 FT"]
[469,"E2L102C19","CM per Intraterminal Switch, BOX - 50 FT"]
[470,"E2L102C20","CM per Interterminal Switch, BOX - 50 FT"]
[471,"E2L102C21","CM per I&I Switch, BOX - 50 FT"]
[472,"E2L102C22","Average CM per CD, Railroad-Owned, BOX - 50 FT"]
[473,"E2L102C23","Average Miles between I&I Switches, BOX - 50 FT"]
[474,"E2L102C24","Average Miles between Interchange Switches, BOX - 50 FT"]
[475,"E2L102C25","SEMs per Industry Switch, BOX - 50 FT"]
[476,"E2L102C26","SEMs per Interchange Switch, BOX - 50 FT"]
[477,"E2L102C27","SEMs per Intraterminal Switch, BOX - 50 FT"]
[478,"E2L102C28","SEMs per Interterminal Switch, BOX - 50 FT"]
[479,"E2L102C29","SEMs per I&I Switch, BOX - 50 FT"]
[480,"E2L103C1","Average Tare Weight, BOX - EQUIPPED"]
[481,"E2L103C2","E/L Ratio, Railroad-Owned, BOX - EQUIPPED"]
[482,"E2L103C3","E/L Ratio, Privately-Owned, BOX - EQUIPPED"]
[483,"E2L103C4","E/L Ratio, All Freight Cars, BOX - EQUIPPED"]
[484,"E2L103C5","Local circuity, BOX - EQUIPPED"]
[485,"E2L103C6","Interline circuity, BOX - EQUIPPED"]
[486,"E2L103C7","Average circuity, BOX - EQUIPPED"]
[487,"E2L103C8","Spotted-to-Pulled Ratio, BOX - EQUIPPED"]
[488,"E2L103C9","CD per Industry Switch, BOX - EQUIPPED"]
[489,"E2L103C10","CD per Interchange Switch, BOX - EQUIPPED"]
[490,"E2L103C11","CD per Intraterminal Switch, BOX - EQUIPPED"]
[491,"E2L103C12","CD per Interterminal Switch, BOX - EQUIPPED"]
[492,"E2L103C13","CD per I&I Switch, BOX - EQUIPPED"]
[493,"E2L103C14","CD per Load & Unload Industry Switch, BOX - EQUIPP"]
[494,"E2L103C15","CD per Load & Unload Intraterminal Switch, BOX - EQUIPPED"]
[495,"E2L103C16","CD per Load & Unload Interterminal Switch, BOX - EQUIPPED"]
[496,"E2L103C17","CM per Industry Switch, BOX - EQUIPPED"]
[497,"E2L103C18","CM per Interchange Switch, BOX - EQUIPPED"]
[498,"E2L103C19","CM per Intraterminal Switch, BOX - EQUIPPED"]
[499,"E2L103C20","CM per Interterminal Switch, BOX - EQUIPPED"]
[500,"E2L103C21","CM per I&I Switch, BOX - EQUIPPED"]
[501,"E2L103C22","Average CM per CD, Railroad-Owned, BOX - EQUIPPED"]
[502,"E2L103C23","Average Miles between I&I Switches, BOX - EQUIPPED"]
[503,"E2L103C24","Average Miles between Interchange Switches, BOX - EQUIPPED"]
[504,"E2L103C25","SEMs per Industry Switch, BOX - EQUIPPED"]
[505,"E2L103C26","SEMs per Interchange Switch, BOX - EQUIPPED"]
[506,"E2L103C27","SEMs per Intraterminal Switch, BOX - EQUIPPED"]
[507,"E2L103C28","SEMs per Interterminal Switch, BOX - EQUIPPED"]
[508,"E2L103C29","SEMs per I&I Switch, BOX - EQUIPPED"]
[509,"E2L104C1","Average Tare Weight, GONDOLA - PLAIN"]
[510,"E2L104C2","E/L Ratio, Railroad-Owned, GONDOLA - PLAIN"]
[511,"E2L104C3","E/L Ratio, Privately-Owned, GONDOLA - PLAIN"]
[512,"E2L104C4","E/L Ratio, All Freight Cars, GONDOLA - PLAIN"]
[513,"E2L104C5","Local circuity, GONDOLA - PLAIN"]
[514,"E2L104C6","Interline circuity, GONDOLA - PLAIN"]
[515,"E2L104C7","Average circuity, GONDOLA - PLAIN"]
[516,"E2L104C8","Spotted-to-Pulled Ratio, GONDOLA - PLAIN"]
[517,"E2L104C9","CD per Industry Switch, GONDOLA - PLAIN"]
[518,"E2L104C10","CD per Interchange Switch, GONDOLA - PLAIN"]
[519,"E2L104C11","CD per Intraterminal Switch, GONDOLA - PLAIN"]
[520,"E2L104C12","CD per Interterminal Switch, GONDOLA - PLAIN"]
[521,"E2L104C13","CD per I&I Switch, GONDOLA - PLAIN"]
[522,"E2L104C14","CD per Load & Unload Industry Switch, GONDOLA - PLAIN"]
[523,"E2L104C15","CD per Load & Unload Intraterminal Switch, GONDOLA - PLAIN"]
[524,"E2L104C16","CD per Load & Unload Interterminal Switch, GONDOLA - PLAIN"]
[525,"E2L104C17","CM per Industry Switch, GONDOLA - PLAIN"]
[526,"E2L104C18","CM per Interchange Switch, GONDOLA - PLAIN"]
[527,"E2L104C19","CM per Intraterminal Switch, GONDOLA - PLAIN"]
[528,"E2L104C20","CM per Interterminal Switch, GONDOLA - PLAIN"]
[529,"E2L104C21","CM per I&I Switch, GONDOLA - PLAIN"]
[530,"E2L104C22","Average CM per CD, Railroad-Owned, GONDOLA - PLAIN"]
[531,"E2L104C23","Average Miles between I&I Switches, GONDOLA - PLAIN"]
[532,"E2L104C24","Average Miles between Interchange Switches, GONDOLA - PLAIN"]
[533,"E2L104C25","SEMs per Industry Switch, GONDOLA - PLAIN"]
[534,"E2L104C26","SEMs per Interchange Switch, GONDOLA - PLAIN"]
[535,"E2L104C27","SEMs per Intraterminal Switch, GONDOLA - PLAIN"]
[536,"E2L104C28","SEMs per Interterminal Switch, GONDOLA - PLAIN"]
[537,"E2L104C29","SEMs per I&I Switch, GONDOLA - PLAIN"]
[538,"E2L105C1","Average Tare Weight, GONDOLA - EQUIPPED"]
[539,"E2L105C2","E/L Ratio, Railroad-Owned, GONDOLA - EQUIPPED"]
[540,"E2L105C3","E/L Ratio, Privately-Owned, GONDOLA - EQUIPPED"]
[541,"E2L105C4","E/L Ratio, All Freight Cars, GONDOLA - EQUIPPED"]
[542,"E2L105C5","Local circuity, GONDOLA - EQUIPPED"]
[543,"E2L105C6","Interline circuity, GONDOLA - EQUIPPED"]
[544,"E2L105C7","Average circuity, GONDOLA - EQUIPPED"]
[545,"E2L105C8","Spotted-to-Pulled Ratio, GONDOLA - EQUIPPED"]
[546,"E2L105C9","CD per Industry Switch, GONDOLA - EQUIPPED"]
[547,"E2L105C10","CD per Interchange Switch, GONDOLA - EQUIPPED"]
[548,"E2L105C11","CD per Intraterminal Switch, GONDOLA - EQUIPPED"]
[549,"E2L105C12","CD per Interterminal Switch, GONDOLA - EQUIPPED"]
[550,"E2L105C13","CD per I&I Switch, GONDOLA - EQUIPPED"]
[551,"E2L105C14","CD per Load & Unload Industry Switch, GONDOLA - EQUIPPED"]
[552,"E2L105C15","CD per Load & Unload Intraterminal Switch, GONDOLA - EQUIPPED"]
[553,"E2L105C16","CD per Load & Unload Interterminal Switch, GONDOLA - EQUIPPED"]
[554,"E2L105C17","CM per Industry Switch, GONDOLA - EQUIPPED"]
[555,"E2L105C18","CM per Interchange Switch, GONDOLA - EQUIPPED"]
[556,"E2L105C19","CM per Intraterminal Switch, GONDOLA - EQUIPPED"]
[557,"E2L105C20","CM per Interterminal Switch, GONDOLA - EQUIPPED"]
[558,"E2L105C21","CM per I&I Switch, GONDOLA - EQUIPPED"]
[559,"E2L105C22","Average CM per CD, Railroad-Owned, GONDOLA - EQUIPPED"]
[560,"E2L105C23","Average Miles between I&I Switches, GONDOLA - EQUIPPED"]
[561,"E2L105C24","Average Miles between Interchange Switches, GONDOLA - EQUIPPED"]
[562,"E2L105C25","SEMs per Industry Switch, GONDOLA - EQUIPPED"]
[563,"E2L105C26","SEMs per Interchange Switch, GONDOLA - EQUIPPED"]
[564,"E2L105C27","SEMs per Intraterminal Switch, GONDOLA - EQUIPPED"]
[565,"E2L105C28","SEMs per Interterminal Switch, GONDOLA - EQUIPPED"]
[566,"E2L105C29","SEMs per I&I Switch, GONDOLA - EQUIPPED"]
[567,"E2L106C1","Average Tare Weight, HOPPER - COVERED"]
[568,"E2L106C2","E/L Ratio, Railroad-Owned, HOPPER - COVERED"]
[569,"E2L106C3","E/L Ratio, Privately-Owned, HOPPER - COVERED"]
[570,"E2L106C4","E/L Ratio, All Freight Cars, HOPPER - COVERED"]
[571,"E2L106C5","Local circuity, HOPPER - COVERED"]
[572,"E2L106C6","Interline circuity, HOPPER - COVERED"]
[573,"E2L106C7","Average circuity, HOPPER - COVERED"]
[574,"E2L106C8","Spotted-to-Pulled Ratio, HOPPER - COVERED"]
[575,"E2L106C9","CD per Industry Switch, HOPPER - COVERED"]
[576,"E2L106C10","CD per Interchange Switch, HOPPER - COVERED"]
[577,"E2L106C11","CD per Intraterminal Switch, HOPPER - COVERED"]
[578,"E2L106C12","CD per Interterminal Switch, HOPPER - COVERED"]
[579,"E2L106C13","CD per I&I Switch, HOPPER - COVERED"]
[580,"E2L106C14","CD per Load & Unload Industry Switch, HOPPER - COVERED"]
[581,"E2L106C15","CD per Load & Unload Intraterminal Switch, HOPPER - COVERED"]
[582,"E2L106C16","CD per Load & Unload Interterminal Switch, HOPPER - COVERED"]
[583,"E2L106C17","CM per Industry Switch, HOPPER - COVERED"]
[584,"E2L106C18","CM per Interchange Switch, HOPPER - COVERED"]
[585,"E2L106C19","CM per Intraterminal Switch, HOPPER - COVERED"]
[586,"E2L106C20","CM per Interterminal Switch, HOPPER - COVERED"]
[587,"E2L106C21","CM per I&I Switch, HOPPER - COVERED"]
[588,"E2L106C22","Average CM per CD, Railroad-Owned, HOPPER - COVERED"]
[589,"E2L106C23","Average Miles between I&I Switches, HOPPER - COVERED"]
[590,"E2L106C24","Average Miles between Interchange Switches, HOPPER - COVERED"]
[591,"E2L106C25","SEMs per Industry Switch, HOPPER - COVERED"]
[592,"E2L106C26","SEMs per Interchange Switch, HOPPER - COVERED"]
[593,"E2L106C27","SEMs per Intraterminal Switch, HOPPER - COVERED"]
[594,"E2L106C28","SEMs per Interterminal Switch, HOPPER - COVERED"]
[595,"E2L106C29","SEMs per I&I Switch, HOPPER - COVERED"]
[596,"E2L107C1","Average Tare Weight, HOPPER - OPEN TOP - GENERAL"]
[597,"E2L107C2","E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[598,"E2L107C3","E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - GENERAL"]
[599,"E2L107C4","E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - GENERAL"]
[600,"E2L107C5","Local circuity, HOPPER - OPEN TOP - GENERAL"]
[601,"E2L107C6","Interline circuity, HOPPER - OPEN TOP - GENERAL"]
[602,"E2L107C7","Average circuity, HOPPER - OPEN TOP - GENERAL"]
[603,"E2L107C8","Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - GENERAL"]
[604,"E2L107C9","CD per Industry Switch, HOPPER - OPEN TOP - GENERAL"]
[605,"E2L107C10","CD per Interchange Switch, HOPPER - OPEN TOP - GENERAL"]
[606,"E2L107C11","CD per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL"]
[607,"E2L107C12","CD per Interterminal Switch, HOPPER - OPEN TOP - GENERAL"]
[608,"E2L107C13","CD per I&I Switch, HOPPER - OPEN TOP - GENERAL"]
[609,"E2L107C14","CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - GENERAL"]
[610,"E2L107C15","CD per Load & Unload Intraterminal Switch, HOPPER - OPEN TOP - GENERAL"]
[611,"E2L107C16","CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - GENERAL"]
[612,"E2L107C17","CM per Industry Switch, HOPPER - OPEN TOP - GENERAL"]
[613,"E2L107C18","CM per Interchange Switch, HOPPER - OPEN TOP - GENERAL"]
[614,"E2L107C19","CM per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL"]
[615,"E2L107C20","CM per Interterminal Switch, HOPPER - OPEN TOP - GENERAL"]
[616,"E2L107C21","CM per I&I Switch, HOPPER - OPEN TOP - GENERAL"]
[617,"E2L107C22","Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - GENERAL"]
[618,"E2L107C23","Average Miles between I&I Switches, HOPPER - OPEN TOP - GENERAL"]
[619,"E2L107C24","Average Miles between Interchange Switches, HOPPER - OPEN TOP - GENERAL"]
[620,"E2L107C25","SEMs per Industry Switch, HOPPER - OPEN TOP - GENERAL"]
[621,"E2L107C26","SEMs per Interchange Switch, HOPPER - OPEN TOP - GENERAL"]
[622,"E2L107C27","SEMs per Intraterminal Switch, HOPPER - OPEN TOP - GENERAL"]
[623,"E2L107C28","SEMs per Interterminal Switch, HOPPER - OPEN TOP - GENERAL"]
[624,"E2L107C29","SEMs per I&I Switch, HOPPER - OPEN TOP - GENERAL"]
[625,"E2L108C1","Average Tare Weight, HOPPER - OPEN TOP - SPECIAL"]
[626,"E2L108C2","E/L Ratio, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[627,"E2L108C3","E/L Ratio, Privately-Owned, HOPPER - OPEN TOP - SPECIAL"]
[628,"E2L108C4","E/L Ratio, All Freight Cars, HOPPER - OPEN TOP - SPECIAL"]
[629,"E2L108C5","Local circuity, HOPPER - OPEN TOP - SPECIAL"]
[630,"E2L108C6","Interline circuity, HOPPER - OPEN TOP - SPECIAL"]
[631,"E2L108C7","Average circuity, HOPPER - OPEN TOP - SPECIAL"]
[632,"E2L108C8","Spotted-to-Pulled Ratio, HOPPER - OPEN TOP - SPECIAL"]
[633,"E2L108C9","CD per Industry Switch, HOPPER - OPEN TOP - SPECIAL"]
[634,"E2L108C10","CD per Interchange Switch, HOPPER - OPEN TOP - SPECIAL"]
[635,"E2L108C11","CD per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL"]
[636,"E2L108C12","CD per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL"]
[637,"E2L108C13","CD per I&I Switch, HOPPER - OPEN TOP - SPECIAL"]
[638,"E2L108C14","CD per Load & Unload Industry Switch, HOPPER - OPEN TOP - SPECIAL"]
[639,"E2L108C15","CD per Load & Unload Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL"]
[640,"E2L108C16","CD per Load & Unload Interterminal Switch, HOPPER - OPEN TOP - SPECIAL"]
[641,"E2L108C17","CM per Industry Switch, HOPPER - OPEN TOP - SPECIAL"]
[642,"E2L108C18","CM per Interchange Switch, HOPPER - OPEN TOP - SPECIAL"]
[643,"E2L108C19","CM per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL"]
[644,"E2L108C20","CM per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL"]
[645,"E2L108C21","CM per I&I Switch, HOPPER - OPEN TOP - SPECIAL"]
[646,"E2L108C22","Average CM per CD, Railroad-Owned, HOPPER - OPEN TOP - SPECIAL"]
[647,"E2L108C23","Average Miles between I&I Switches, HOPPER - OPEN TOP - SPECIAL"]
[648,"E2L108C24","Average Miles between Interchange Switches, HOPPER - OPEN TOP - SPECIAL"]
[649,"E2L108C25","SEMs per Industry Switch, HOPPER - OPEN TOP - SPECIAL"]
[650,"E2L108C26","SEMs per Interchange Switch, HOPPER - OPEN TOP - SPECIAL"]
[651,"E2L108C27","SEMs per Intraterminal Switch, HOPPER - OPEN TOP - SPECIAL"]
[652,"E2L108C28","SEMs per Interterminal Switch, HOPPER - OPEN TOP - SPECIAL"]
[653,"E2L108C29","SEMs per I&I Switch, HOPPER - OPEN TOP - SPECIAL"]
[654,"E2L109C1","Average Tare Weight, REFRIGERATED - MECH"]
[655,"E2L109C2","E/L Ratio, Railroad-Owned, REFRIGERATED - MECH"]
[656,"E2L109C3","E/L Ratio, Privately-Owned, REFRIGERATED - MECH"]
[657,"E2L109C4","E/L Ratio, All Freight Cars, REFRIGERATED - MECH"]
[658,"E2L109C5","Local circuity, REFRIGERATED - MECH"]
[659,"E2L109C6","Interline circuity, REFRIGERATED - MECH"]
[660,"E2L109C7","Average circuity, REFRIGERATED - MECH"]
[661,"E2L109C8","Spotted-to-Pulled Ratio, REFRIGERATED - MECH"]
[662,"E2L109C9","CD per Industry Switch, REFRIGERATED - MECH"]
[663,"E2L109C10","CD per Interchange Switch, REFRIGERATED - MECH"]
[664,"E2L109C11","CD per Intraterminal Switch, REFRIGERATED - MECH"]
[665,"E2L109C12","CD per Interterminal Switch, REFRIGERATED - MECH"]
[666,"E2L109C13","CD per I&I Switch, REFRIGERATED - MECH"]
[667,"E2L109C14","CD per Load & Unload Industry Switch, REFRIGERATED - MECH"]
[668,"E2L109C15","CD per Load & Unload Intraterminal Switch, REFRIGERATED - MECH"]
[669,"E2L109C16","CD per Load & Unload Interterminal Switch, REFRIGERATED - MECH"]
[670,"E2L109C17","CM per Industry Switch, REFRIGERATED - MECH"]
[671,"E2L109C18","CM per Interchange Switch, REFRIGERATED - MECH"]
[672,"E2L109C19","CM per Intraterminal Switch, REFRIGERATED - MECH"]
[673,"E2L109C20","CM per Interterminal Switch, REFRIGERATED - MECH"]
[674,"E2L109C21","CM per I&I Switch, REFRIGERATED - MECH"]
[675,"E2L109C22","Average CM per CD, Railroad-Owned, REFRIGERATED - MECH"]
[676,"E2L109C23","Average Miles between I&I Switches, REFRIGERATED - MECH"]
[677,"E2L109C24","Average Miles between Interchange Switches, REFRIGERATED - MECH"]
[678,"E2L109C25","SEMs per Industry Switch, REFRIGERATED - MECH"]
[679,"E2L109C26","SEMs per Interchange Switch, REFRIGERATED - MECH"]
[680,"E2L109C27","SEMs per Intraterminal Switch, REFRIGERATED - MECH"]
[681,"E2L109C28","SEMs per Interterminal Switch, REFRIGERATED - MECH"]
[682,"E2L109C29","SEMs per I&I Switch, REFRIGERATED - MECH"]
[683,"E2L110C1","Average Tare Weight, REFRIGERATED - NON-MECH"]
[684,"E2L110C2","E/L Ratio, Railroad-Owned, REFRIGERATED - NON-MECH"]
[685,"E2L110C3","E/L Ratio, Privately-Owned, REFRIGERATED - NON-MECH"]
[686,"E2L110C4","E/L Ratio, All Freight Cars, REFRIGERATED - NON-MECH"]
[687,"E2L110C5","Local circuity, REFRIGERATED - NON-MECH"]
[688,"E2L110C6","Interline circuity, REFRIGERATED - NON-MECH"]
[689,"E2L110C7","Average circuity, REFRIGERATED - NON-MECH"]
[690,"E2L110C8","Spotted-to-Pulled Ratio, REFRIGERATED - NON-MECH"]
[691,"E2L110C9","CD per Industry Switch, REFRIGERATED - NON-MECH"]
[692,"E2L110C10","CD per Interchange Switch, REFRIGERATED - NON-MECH"]
[693,"E2L110C11","CD per Intraterminal Switch, REFRIGERATED - NON-MECH"]
[694,"E2L110C12","CD per Interterminal Switch, REFRIGERATED - NON-MECH"]
[695,"E2L110C13","CD per I&I Switch, REFRIGERATED - NON-MECH"]
[696,"E2L110C14","CD per Load & Unload Industry Switch, REFRIGERATED - NON-MECH"]
[697,"E2L110C15","CD per Load & Unload Intraterminal Switch, REFRIGERATED - NON-MECH"]
[698,"E2L110C16","CD per Load & Unload Interterminal Switch, REFRIGERATED - NON-MECH"]
[699,"E2L110C17","CM per Industry Switch, REFRIGERATED - NON-MECH"]
[700,"E2L110C18","CM per Interchange Switch, REFRIGERATED - NON-MECH"]
[701,"E2L110C19","CM per Intraterminal Switch, REFRIGERATED - NON-MECH"]
[702,"E2L110C20","CM per Interterminal Switch, REFRIGERATED - NON-MECH"]
[703,"E2L110C21","CM per I&I Switch, REFRIGERATED - NON-MECH"]
[704,"E2L110C22","Average CM per CD, Railroad-Owned, REFRIGERATED - NON-MECH"]
[705,"E2L110C23","Average Miles between I&I Switches, REFRIGERATED - NON-MECH"]
[706,"E2L110C24","Average Miles between Interchange Switches, REFRIGERATED - NON-MECH"]
[707,"E2L110C25","SEMs per Industry Switch, REFRIGERATED - NON-MECH"]
[708,"E2L110C26","SEMs per Interchange Switch, REFRIGERATED - NON-MECH"]
[709,"E2L110C27","SEMs per Intraterminal Switch, REFRIGERATED - NON-MECH"]
[710,"E2L110C28","SEMs per Interterminal Switch, REFRIGERATED - NON-MECH"]
[711,"E2L110C29","SEMs per I&I Switch, REFRIGERATED - NON-MECH"]
[712,"E2L111C1","Average Tare Weight, FLAT - TOFC"]
[713,"E2L111C2","E/L Ratio, Railroad-Owned, FLAT - TOFC"]
[714,"E2L111C3","E/L Ratio, Privately-Owned, FLAT - TOFC"]
[715,"E2L111C4","E/L Ratio, All Freight Cars, FLAT - TOFC"]
[716,"E2L111C5","Local circuity, FLAT - TOFC"]
[717,"E2L111C6","Interline circuity, FLAT - TOFC"]
[718,"E2L111C7","Average circuity, FLAT - TOFC"]
[719,"E2L111C8","Spotted-to-Pulled Ratio, FLAT - TOFC"]
[720,"E2L111C9","CD per Industry Switch, FLAT - TOFC"]
[721,"E2L111C10","CD per Interchange Switch, FLAT - TOFC"]
[722,"E2L111C11","CD per Intraterminal Switch, FLAT - TOFC"]
[723,"E2L111C12","CD per Interterminal Switch, FLAT - TOFC"]
[724,"E2L111C13","CD per I&I Switch, FLAT - TOFC"]
[725,"E2L111C14","CD per Load & Unload Industry Switch, FLAT - TOFC"]
[726,"E2L111C15","CD per Load & Unload Intraterminal Switch, FLAT - TOFC"]
[727,"E2L111C16","CD per Load & Unload Interterminal Switch, FLAT - TOFC"]
[728,"E2L111C17","CM per Industry Switch, FLAT - TOFC"]
[729,"E2L111C18","CM per Interchange Switch, FLAT - TOFC"]
[730,"E2L111C19","CM per Intraterminal Switch, FLAT - TOFC"]
[731,"E2L111C20","CM per Interterminal Switch, FLAT - TOFC"]
[732,"E2L111C21","CM per I&I Switch, FLAT - TOFC"]
[733,"E2L111C22","Average CM per CD, Railroad-Owned, FLAT - TOFC"]
[734,"E2L111C23","Average Miles between I&I Switches, FLAT - TOFC"]
[735,"E2L111C24","Average Miles between Interchange Switches, FLAT - TOFC"]
[736,"E2L111C25","SEMs per Industry Switch, FLAT - TOFC"]
[737,"E2L111C26","SEMs per Interchange Switch, FLAT - TOFC"]
[738,"E2L111C27","SEMs per Intraterminal Switch, FLAT - TOFC"]
[739,"E2L111C28","SEMs per Interterminal Switch, FLAT - TOFC"]
[740,"E2L111C29","SEMs per I&I Switch, FLAT - TOFC"]
[741,"E2L112C1","Average Tare Weight, FLAT - MULTILEVEL"]
[742,"E2L112C2","E/L Ratio, Railroad-Owned, FLAT - MULTILEVEL"]
[743,"E2L112C3","E/L Ratio, Privately-Owned, FLAT - MULTILEVEL"]
[744,"E2L112C4","E/L Ratio, All Freight Cars, FLAT - MULTILEVEL"]
[745,"E2L112C5","Local circuity, FLAT - MULTILEVEL"]
[746,"E2L112C6","Interline circuity, FLAT - MULTILEVEL"]
[747,"E2L112C7","Average circuity, FLAT - MULTILEVEL"]
[748,"E2L112C8","Spotted-to-Pulled Ratio, FLAT - MULTILEVEL"]
[749,"E2L112C9","CD per Industry Switch, FLAT - MULTILEVEL"]
[750,"E2L112C10","CD per Interchange Switch, FLAT - MULTILEVEL"]
[751,"E2L112C11","CD per Intraterminal Switch, FLAT - MULTILEVEL"]
[752,"E2L112C12","CD per Interterminal Switch, FLAT - MULTILEVEL"]
[753,"E2L112C13","CD per I&I Switch, FLAT - MULTILEVEL"]
[754,"E2L112C14","CD per Load & Unload Industry Switch, FLAT - MULTILEVEL"]
[755,"E2L112C15","CD per Load & Unload Intraterminal Switch, FLAT - MULTILEVEL"]
[756,"E2L112C16","CD per Load & Unload Interterminal Switch, FLAT - MULTILEVEL"]
[757,"E2L112C17","CM per Industry Switch, FLAT - MULTILEVEL"]
[758,"E2L112C18","CM per Interchange Switch, FLAT - MULTILEVEL"]
[759,"E2L112C19","CM per Intraterminal Switch, FLAT - MULTILEVEL"]
[760,"E2L112C20","CM per Interterminal Switch, FLAT - MULTILEVEL"]
[761,"E2L112C21","CM per I&I Switch, FLAT - MULTILEVEL"]
[762,"E2L112C22","Average CM per CD, Railroad-Owned, FLAT - MULTILEVEL"]
[763,"E2L112C23","Average Miles between I&I Switches, FLAT - MULTILEVEL"]
[764,"E2L112C24","Average Miles between Interchange Switches, FLAT - MULTILEVEL"]
[765,"E2L112C25","SEMs per Industry Switch, FLAT - MULTILEVEL"]
[766,"E2L112C26","SEMs per Interchange Switch, FLAT - MULTILEVEL"]
[767,"E2L112C27","SEMs per Intraterminal Switch, FLAT - MULTILEVEL"]
[768,"E2L112C28","SEMs per Interterminal Switch, FLAT - MULTILEVEL"]
[769,"E2L112C29","SEMs per I&I Switch, FLAT - MULTILEVEL"]
[770,"E2L113C1","Average Tare Weight, FLAT - GENERAL"]
[771,"E2L113C2","E/L Ratio, Railroad-Owned, FLAT - GENERAL"]
[772,"E2L113C3","E/L Ratio, Privately-Owned, FLAT - GENERAL"]
[773,"E2L113C4","E/L Ratio, All Freight Cars, FLAT - GENERAL"]
[774,"E2L113C5","Local circuity, FLAT - GENERAL"]
[775,"E2L113C6","Interline circuity, FLAT - GENERAL"]
[776,"E2L113C7","Average circuity, FLAT - GENERAL"]
[777,"E2L113C8","Spotted-to-Pulled Ratio, FLAT - GENERAL"]
[778,"E2L113C9","CD per Industry Switch, FLAT - GENERAL"]
[779,"E2L113C10","CD per Interchange Switch, FLAT - GENERAL"]
[780,"E2L113C11","CD per Intraterminal Switch, FLAT - GENERAL"]
[781,"E2L113C12","CD per Interterminal Switch, FLAT - GENERAL"]
[782,"E2L113C13","CD per I&I Switch, FLAT - GENERAL"]
[783,"E2L113C14","CD per Load & Unload Industry Switch, FLAT - GENERAL"]
[784,"E2L113C15","CD per Load & Unload Intraterminal Switch, FLAT - GENERAL"]
[785,"E2L113C16","CD per Load & Unload Interterminal Switch, FLAT - GENERAL"]
[786,"E2L113C17","CM per Industry Switch, FLAT - GENERAL"]
[787,"E2L113C18","CM per Interchange Switch, FLAT - GENERAL"]
[788,"E2L113C19","CM per Intraterminal Switch, FLAT - GENERAL"]
[789,"E2L113C20","CM per Interterminal Switch, FLAT - GENERAL"]
[790,"E2L113C21","CM per I&I Switch, FLAT - GENERAL"]
[791,"E2L113C22","Average CM per CD, Railroad-Owned, FLAT - GENERAL"]
[792,"E2L113C23","Average Miles between I&I Switches, FLAT - GENERAL"]
[793,"E2L113C24","Average Miles between Interchange Switches, FLAT - GENERAL"]
[794,"E2L113C25","SEMs per Industry Switch, FLAT - GENERAL"]
[795,"E2L113C26","SEMs per Interchange Switch, FLAT - GENERAL"]
[796,"E2L113C27","SEMs per Intraterminal Switch, FLAT - GENERAL"]
[797,"E2L113C28","SEMs per Interterminal Switch, FLAT - GENERAL"]
[798,"E2L113C29","SEMs per I&I Switch, FLAT - GENERAL"]
[799,"E2L114C1","Average Tare Weight, FLAT - OTHER"]
[800,"E2L114C2","E/L Ratio, Railroad-Owned, FLAT - OTHER"]
[801,"E2L114C3","E/L Ratio, Privately-Owned, FLAT - OTHER"]
[802,"E2L114C4","E/L Ratio, All Freight Cars, FLAT - OTHER"]
[803,"E2L114C5","Local circuity, FLAT - OTHER"]
[804,"E2L114C6","Interline circuity, FLAT - OTHER"]
[805,"E2L114C7","Average circuity, FLAT - OTHER"]
[806,"E2L114C8","Spotted-to-Pulled Ratio, FLAT - OTHER"]
[807,"E2L114C9","CD per Industry Switch, FLAT - OTHER"]
[808,"E2L114C10","CD per Interchange Switch, FLAT - OTHER"]
[809,"E2L114C11","CD per Intraterminal Switch, FLAT - OTHER"]
[810,"E2L114C12","CD per Interterminal Switch, FLAT - OTHER"]
[811,"E2L114C13","CD per I&I Switch, FLAT - OTHER"]
[812,"E2L114C14","CD per Load & Unload Industry Switch, FLAT - OTHER"]
[813,"E2L114C15","CD per Load & Unload Intraterminal Switch, FLAT - OTHER"]
[814,"E2L114C16","CD per Load & Unload Interterminal Switch, FLAT - OTHER"]
[815,"E2L114C17","CM per Industry Switch, FLAT - OTHER"]
[816,"E2L114C18","CM per Interchange Switch, FLAT - OTHER"]
[817,"E2L114C19","CM per Intraterminal Switch, FLAT - OTHER"]
[818,"E2L114C20","CM per Interterminal Switch, FLAT - OTHER"]
[819,"E2L114C21","CM per I&I Switch, FLAT - OTHER"]
[820,"E2L114C22","Average CM per CD, Railroad-Owned, FLAT - OTHER"]
[821,"E2L114C23","Average Miles between I&I Switches, FLAT - OTHER"]
[822,"E2L114C24","Average Miles between Interchange Switches, FLAT - OTHER"]
[823,"E2L114C25","SEMs per Industry Switch, FLAT - OTHER"]
[824,"E2L114C26","SEMs per Interchange Switch, FLAT - OTHER"]
[825,"E2L114C27","SEMs per Intraterminal Switch, FLAT - OTHER"]
[826,"E2L114C28","SEMs per Interterminal Switch, FLAT - OTHER"]
[827,"E2L114C29","SEMs per I&I Switch, FLAT - OTHER"]
[828,"E2L115C1","Average Tare Weight, TANK <22,000 GAL"]
[829,"E2L115C2","E/L Ratio, Railroad-Owned, TANK <22,000 GAL"]
[830,"E2L115C3","E/L Ratio, Privately-Owned, TANK <22,000 GAL"]
[831,"E2L115C4","E/L Ratio, All Freight Cars, TANK <22,000 GAL"]
[832,"E2L115C5","Local circuity, TANK <22,000 GAL"]
[833,"E2L115C6","Interline circuity, TANK <22,000 GAL"]
[834,"E2L115C7","Average circuity, TANK <22,000 GAL"]
[835,"E2L115C8","Spotted-to-Pulled Ratio, TANK <22,000 GAL"]
[836,"E2L115C9","CD per Industry Switch, TANK <22,000 GAL"]
[837,"E2L115C10","CD per Interchange Switch, TANK <22,000 GAL"]
[838,"E2L115C11","CD per Intraterminal Switch, TANK <22,000 GAL"]
[839,"E2L115C12","CD per Interterminal Switch, TANK <22,000 GAL"]
[840,"E2L115C13","CD per I&I Switch, TANK <22,000 GAL"]
[841,"E2L115C14","CD per Load & Unload Industry Switch, TANK <22,000 GAL"]
[842,"E2L115C15","CD per Load & Unload Intraterminal Switch, TANK <22,000 GAL"]
[843,"E2L115C16","CD per Load & Unload Interterminal Switch, TANK <22,000 GAL"]
[844,"E2L115C17","CM per Industry Switch, TANK <22,000 GAL"]
[845,"E2L115C18","CM per Interchange Switch, TANK <22,000 GAL"]
[846,"E2L115C19","CM per Intraterminal Switch, TANK <22,000 GAL"]
[847,"E2L115C20","CM per Interterminal Switch, TANK <22,000 GAL"]
[848,"E2L115C21","CM per I&I Switch, TANK <22,000 GAL"]
[849,"E2L115C22","Average CM per CD, Railroad-Owned, TANK <22,000 GAL"]
[850,"E2L115C23","Average Miles between I&I Switches, TANK <22,000 GAL"]
[851,"E2L115C24","Average Miles between Interchange Switches, TANK <22,000 GAL"]
[852,"E2L115C25","SEMs per Industry Switch, TANK <22,000 GAL"]
[853,"E2L115C26","SEMs per Interchange Switch, TANK <22,000 GAL"]
[854,"E2L115C27","SEMs per Intraterminal Switch, TANK <22,000 GAL"]
[855,"E2L115C28","SEMs per Interterminal Switch, TANK <22,000 GAL"]
[856,"E2L115C29","SEMs per I&I Switch, TANK <22,000 GAL"]
[857,"E2L116C1","Average Tare Weight, TANK >=22,000 GAL"]
[858,"E2L116C2","E/L Ratio, Railroad-Owned, TANK >=22,000 GAL"]
[859,"E2L116C3","E/L Ratio, Privately-Owned, TANK >=22,000 GAL"]
[860,"E2L116C4","E/L Ratio, All Freight Cars, TANK >=22,000 GAL"]
[861,"E2L116C5","Local circuity, TANK >=22,000 GAL"]
[862,"E2L116C6","Interline circuity, TANK >=22,000 GAL"]
[863,"E2L116C7","Average circuity, TANK >=22,000 GAL"]
[864,"E2L116C8","Spotted-to-Pulled Ratio, TANK >=22,000 GAL"]
[865,"E2L116C9","CD per Industry Switch, TANK >=22,000 GAL"]
[866,"E2L116C10","CD per Interchange Switch, TANK >=22,000 GAL"]
[867,"E2L116C11","CD per Intraterminal Switch, TANK >=22,000 GAL"]
[868,"E2L116C12","CD per Interterminal Switch, TANK >=22,000 GAL"]
[869,"E2L116C13","CD per I&I Switch, TANK >=22,000 GAL"]
[870,"E2L116C14","CD per Load & Unload Industry Switch, TANK >=22,000 GAL"]
[871,"E2L116C15","CD per Load & Unload Intraterminal Switch, TANK >=22,000 GAL"]
[872,"E2L116C16","CD per Load & Unload Interterminal Switch, TANK >=22,000 GAL"]
[873,"E2L116C17","CM per Industry Switch, TANK >=22,000 GAL"]
[874,"E2L116C18","CM per Interchange Switch, TANK >=22,000 GAL"]
[875,"E2L116C19","CM per Intraterminal Switch, TANK >=22,000 GAL"]
[876,"E2L116C20","CM per Interterminal Switch, TANK >=22,000 GAL"]
[877,"E2L116C21","CM per I&I Switch, TANK >=22,000 GAL"]
[878,"E2L116C22","Average CM per CD, Railroad-Owned, TANK >=22,000 GAL"]
[879,"E2L116C23","Average Miles between I&I Switches, TANK >=22,000 GAL"]
[880,"E2L116C24","Average Miles between Interchange Switches, TANK >=22,000 GAL"]
[881,"E2L116C25","SEMs per Industry Switch, TANK >=22,000 GAL"]
[882,"E2L116C26","SEMs per Interchange Switch, TANK >=22,000 GAL"]
[883,"E2L116C27","SEMs per Intraterminal Switch, TANK >=22,000 GAL"]
[884,"E2L116C28","SEMs per Interterminal Switch, TANK >=22,000 GAL"]
[885,"E2L116C29","SEMs per I&I Switch, TANK >=22,000 GAL"]
[886,"E2L117C1","Average Tare Weight, ALL OTHER FREIGHT CARS"]
[887,"E2L117C2","E/L Ratio, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[888,"E2L117C3","E/L Ratio, Privately-Owned, ALL OTHER FREIGHT CARS"]
[889,"E2L117C4","E/L Ratio, All Freight Cars, ALL OTHER FREIGHT CAR"]
[890,"E2L117C5","Local circuity, ALL OTHER FREIGHT CARS"]
[891,"E2L117C6","Interline circuity, ALL OTHER FREIGHT CARS"]
[892,"E2L117C7","Average circuity, ALL OTHER FREIGHT CARS"]
[893,"E2L117C8","Spotted-to-Pulled Ratio, ALL OTHER FREIGHT CARS"]
[894,"E2L117C9","CD per Industry Switch, ALL OTHER FREIGHT CARS"]
[895,"E2L117C10","CD per Interchange Switch, ALL OTHER FREIGHT CARS"]
[896,"E2L117C11","CD per Intraterminal Switch, ALL OTHER FREIGHT CARS"]
[897,"E2L117C12","CD per Interterminal Switch, ALL OTHER FREIGHT CARS"]
[898,"E2L117C13","CD per I&I Switch, ALL OTHER FREIGHT CARS"]
[899,"E2L117C14","CD per Load & Unload Industry Switch, ALL OTHER FREIGHT CARS"]
[900,"E2L117C15","CD per Load & Unload Intraterminal Switch, ALL OTHER FREIGHT CARS"]
[901,"E2L117C16","CD per Load & Unload Interterminal Switch, ALL OTHER FREIGHT CARS"]
[902,"E2L117C17","CM per Industry Switch, ALL OTHER FREIGHT CARS"]
[903,"E2L117C18","CM per Interchange Switch, ALL OTHER FREIGHT CARS"]
[904,"E2L117C19","CM per Intraterminal Switch, ALL OTHER FREIGHT CARS"]
[905,"E2L117C20","CM per Interterminal Switch, ALL OTHER FREIGHT CARS"]
[906,"E2L117C21","CM per I&I Switch, ALL OTHER FREIGHT CARS"]
[907,"E2L117C22","Average CM per CD, Railroad-Owned, ALL OTHER FREIGHT CARS"]
[908,"E2L117C23","Average Miles between I&I Switches, ALL OTHER FREIGHT CARS"]
[909,"E2L117C24","Average Miles between Interchange Switches, ALL OTHER FREIGHT CARS"]
[910,"E2L117C25","SEMs per Industry Switch, ALL OTHER FREIGHT CARS"]
[911,"E2L117C26","SEMs per Interchange Switch, ALL OTHER FREIGHT CARS"]
[912,"E2L117C27","SEMs per Intraterminal Switch, ALL OTHER FREIGHT CARS"]
[913,"E2L117C28","SEMs per Interterminal Switch, ALL OTHER FREIGHT CARS"]
[914,"E2L117C29","SEMs per I&I Switch, ALL OTHER FREIGHT CARS"]
[915,"E2L118C1","Average Tare Weight, AVERAGE ALL FREIGHT CARS"]
[916,"E2L118C2","E/L Ratio, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[917,"E2L118C3","E/L Ratio, Privately-Owned, AVERAGE ALL FREIGHT CARS"]
[918,"E2L118C4","E/L Ratio, All Freight Cars, AVERAGE ALL FREIGHT CARS"]
[919,"E2L118C5","Local circuity, AVERAGE ALL FREIGHT CARS"]
[920,"E2L118C6","Interline circuity, AVERAGE ALL FREIGHT CARS"]
[921,"E2L118C7","Average circuity, AVERAGE ALL FREIGHT CARS"]
[922,"E2L118C8","Spotted-to-Pulled Ratio, AVERAGE ALL FREIGHT CARS"]
[923,"E2L118C9","CD per Industry Switch, AVERAGE ALL FREIGHT CARS"]
[924,"E2L118C10","CD per Interchange Switch, AVERAGE ALL FREIGHT CAR"]
[925,"E2L118C11","CD per Intraterminal Switch, AVERAGE ALL FREIGHT CARS"]
[926,"E2L118C12","CD per Interterminal Switch, AVERAGE ALL FREIGHT CARS"]
[927,"E2L118C13","CD per I&I Switch, AVERAGE ALL FREIGHT CARS"]
[928,"E2L118C14","CD per Load & Unload Industry Switch, AVERAGE ALL FREIGHT CARS"]
[929,"E2L118C15","CD per Load & Unload Intraterminal Switch, AVERAGE ALL FREIGHT CARS"]
[930,"E2L118C16","CD per Load & Unload Interterminal Switch, AVERAGE ALL FREIGHT CARS"]
[931,"E2L118C17","CM per Industry Switch, AVERAGE ALL FREIGHT CARS"]
[932,"E2L118C18","CM per Interchange Switch, AVERAGE ALL FREIGHT CAR"]
[933,"E2L118C19","CM per Intraterminal Switch, AVERAGE ALL FREIGHT CARS"]
[934,"E2L118C20","CM per Interterminal Switch, AVERAGE ALL FREIGHT CARS"]
[935,"E2L118C21","CM per I&I Switch, AVERAGE ALL FREIGHT CARS"]
[936,"E2L118C22","Average CM per CD, Railroad-Owned, AVERAGE ALL FREIGHT CARS"]
[937,"E2L118C23","Average Miles between I&I Switches, AVERAGE ALL FREIGHT CARS"]
[938,"E2L118C24","Average Miles between Interchange Switches, AVERAGE ALL FREIGHT CARS"]
[939,"E2L118C25","SEMs per Industry Switch, AVERAGE ALL FREIGHT CARS"]
[940,"E2L118C26","SEMs per Interchange Switch, AVERAGE ALL FREIGHT CARS"]
[941,"E2L118C27","SEMs per Intraterminal Switch, AVERAGE ALL FREIGHT CARS"]
[942,"E2L118C28","SEMs per Interterminal Switch, AVERAGE ALL FREIGHT CARS"]
[943,"E2L118C29","SEMs per I&I Switch, AVERAGE ALL FREIGHT CARS"]
[944,"E2L201C1","Average Distance Per Car In Way Trains"]
[945,"E2L202C1","Average TCUs Per Flat Car"]
[946,"E2L203C1","Average Tare Weight - Refrigerated TCU"]
[947,"E2L204C1","Average Tare Weight - Non-Refrigerated TCU"]
[948,"E2L205C1","Linehaul Miles Per TCU Day"]
[949,"E2L206C1","TCU Days Per Orig Or Term Event"]
[950,"E2L207C1","L/E Ratio - Refrigerated/Non-Refrigerated - TCU"]
[951,"E2L208C1","Average Locomotive Units - Unit Train"]
[952,"E2L209C1","Average Locomotive Units - Way Train"]
[953,"E2L210C1","Average Locomotive Units - Through Train"]
[954,"E2L211C1","Average Gross Tons - Unit Train"]
[955,"E2L212C1","Average Gross Tons - Way Train"]
[956,"E2L213C1","Average Gross Tons - Through Train"]
[957,"E2L214C1","Engine Crews (Excl Train Switching)"]
[958,"E2L215C1","Train Crews (Excl Train Switching)"]
[959,"E2L216C1","Total Crew Wages (Excl Train Switching)"]
[960,"E2L217C1","Train Miles - Running"]
[961,"E2L218C1","Average Crew Wages (Assigned To TM-Crew)"]
[962,"E2L219C1","General Overhead Ratio"]
[963,"E2L220C1","Constant Cost Markup Ratio"]
[964,"E2L301C1","Residual Factor, Industry Switching, Operating and Equipment"]
[965,"E2L301C2","Residual Factor, Industry Switching, Operating"]
[966,"E2L302C1","Residual Factor, Station Clerical, Operating and Equipment"]
[967,"E2L302C2","Residual Factor, Station Clerical, Operating"]
[968,"E2L303C1","Residual Factor, Interchange Switching, Operating and Equipment"]
[969,"E2L303C2","Residual Factor, Interchange Switching, Operating"]
[970,"E2L304C1","Residual Factor, I&I Switching, Operating and Equipment"]
[971,"E2L304C2","Residual Factor, I&I Switching, Operating"]
[972,"E2L305C1","Residual Factor, Mileage, Operating and Equipment"]
[973,"E2L305C2","Residual Factor, Mileage, Operating"]
["*** End of Data ***"]